{"text_format":"1","workbook":"xlsx","n_sheets":26,"sheets":["Summary","Snapshot","Graphs","IP_Manager","Clock","Logic","IO","BRAM","DSP","PLL","CLKMGR","PHASER","PCIE","GTP","GTX","GTH","PS","GTZ","GTY","HardIP","Data","Test","Template","Other","User","Release"],"not_rendered":{"charts":7,"images":67,"macros":1,"external_links":0,"defined_names":365,"comments":19,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Summary","index":0,"n_rows":82,"n_cols":65,"rows_kept":82,"cut":false,"hidden":false,"merged":[[36,5,36,10],[35,12,35,15],[36,12,36,15],[27,12,27,13],[18,12,18,13],[20,12,20,13],[27,6,28,6],[19,12,19,13],[35,5,35,8],[33,12,33,13],[30,12,30,13],[28,12,28,13],[22,12,22,13],[29,12,29,13],[24,12,24,13],[31,12,31,13],[1,4,1,11],[4,2,4,15],[13,12,13,13],[14,12,14,13],[13,2,13,4],[6,9,7,10],[8,9,8,10],[10,6,10,8],[8,6,8,8],[6,6,7,8],[9,2,9,4],[5,6,5,15],[7,2,7,4],[10,2,10,4],[11,2,11,4],[8,2,8,4],[35,1,35,4],[28,1,28,4],[31,1,33,1],[29,2,29,4],[31,2,31,10],[32,2,32,10],[33,2,33,10],[25,6,26,6],[32,12,32,13],[29,7,29,8],[25,12,25,13],[24,2,24,4],[20,2,20,4],[21,2,21,4],[25,2,25,4],[26,12,26,13],[26,2,26,4],[15,6,23,6],[16,1,16,4],[17,12,17,13],[15,12,15,13],[17,2,17,3],[23,12,23,13],[21,12,21,13],[23,2,23,4],[22,2,22,4],[18,2,18,4],[19,2,19,3],[6,1,6,4],[10,9,10,10],[16,12,16,13],[9,6,9,8],[12,2,12,4],[13,9,13,10],[14,2,14,4],[13,6,13,8]]}
[null,null,null,null,{"$f":"\"           Xilinx Power Estimator (XPE) - \" & VERSION","v":"           Xilinx Power Estimator (XPE) - 2015,4"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VCCINT/0.95","v":1},null,"Pkgs",{"$f":"IF(PROCESS<>\"Maximum\",1,IF(OR(ISOLY,GRADE=\"Extended\",GRADE=\"Commercial\",NUM_DICE>2),16,IF(OR(LEFT(GRADE,1)=\"Q\",LEFT(GRADE,1)=\"M\",RIGHT(SPEEDGRADE,3)=\"L\"),46,31)))","v":1},"CLKROW","CLKCOL","LUT","FF","BRAM","MMCM","PLL","DSP","GT","PCIE / MAC",null,"3.3 Pins","Pins","Banks","ThetaJA","ThetaJB","ThetaJC","JA250","JA500","JA750","Pkgs"]
[null,null,null,null," Kintex® UltraScaleTM,  Virtex® UltraScale",null,null,null,null,null,null,null,null,null,{"$f":"\"Release: \" & TEXT(RELEASE_DATE,\"d-mmm-yyyy\")","v":"Release: d-00-yyyy"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FFVA1760",{"$f":"MATCH(RIGHT(PART,LEN(PART)-2),PVT_LIST,FALSE)","v":14},15,6,1074240,2148480,3780,30,60,1800,0,6,0,0,448,17,5.9,1.4,0.06,3.4,2.8,2.7,"FLGB2104"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"FFVB1517",{"$f":"IF(GRADE=\"Commercial\",1,IF(OR(GRADE=\"Q-Grade\",LEFT(SPEEDGRADE,3)=\"-2L\"),3,2))","v":2},3,null,406080,null,null,null,null,null,60,9,null,null,null,null,null,null,null,null,null,null,"FLGC2104"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FFVC1517",null,{"$f":"IF(AND(LEFT(FAMILY,4)=\"Zynq\",OPTIMIZATION=\"Powered Off\"),0,1)","v":1},null,null,null,null,null,null,null,null,9,null,null,null,null,null,null,null,null,null,null,"FLGA2577"]
[null,"Project",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FFVD1924",null,13,null,null,null,null,null,null,null,0]
[null,"    Settings",null,null,null,null,"Summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FFVE1924",null,null,null,null,null,null,null,null,null,60]
[null,"   Device",null,null,null,null,"Total On-Chip Power",null,null,{"$f":"SUM(J12:J30)","v":83.87946480050806},null,null,{"$f":"P7/TOTAL_POWER","v":0.54296229126097639},"Transceiver……",null,{"$f":"SUM(J26:J27)","v":45.543386397828279},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FFVJ1924"]
[null,"Family","Virtex UltraScale",null,null,null,null,null,null,null,null,null,{"$f":"P8/TOTAL_POWER","v":3.9338514969516833E-2},"I/O………………",null,{"$f":"J25","v":3.2996935816898465}]
[null,"Device","XCVU190",null,null,null,"Junction Temperature",null,null,{"$f":"IF(ISBLANK(USER_TJ),IF(TJA*TOTAL_POWER+AMBIENT_TEMP > 125, \"125+\",TJA*TOTAL_POWER+AMBIENT_TEMP),USER_TJ)","v":85.325771389040298},null,null,{"$f":"P9/TOTAL_POWER","v":0.32949587066033315},{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",\"PS+FPGA Dyn..\",\"Core Dynamic..\")","v":"Core Dynamic.."},null,{"$f":"SUM(J16:J24,J28)","v":27.637937284966171}]
[null,"Package","FLGA2577",null,null,null,"   Thermal Margin              ",null,null,{"$f":"IF(ISBLANK(USER_TJ),TJ_MAX - (TJA*TOTAL_POWER + AMBIENT_TEMP),TJ_MAX-USER_TJ)","v":14.674228610959702},{"$f":"IF(ISBLANK(USER_TJ),IF(THERMAL_MARGIN_C/TJA+TOTAL_POWER>=0,(MAX_AMBIENT - AMBIENT_TEMP)/TJA,\"\"),(TJ_MAX-USER_TJ)/TJA)","v":16.17093554791197},null,{"$f":"P10/TOTAL_POWER","v":8.8203323109173434E-2},"Device Static…..",null,{"$f":"J29+J30","v":7.3984475360237525},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,70.112496241786957,2.1156936293560058]
[null,"Speed Grade",-2,null,null,null,"   Effective ΘJA",null,null,{"$f":"IF(USER_THETAJA>0,USER_THETAJA,$V54)","v":0.77880529572292434},null,"       Power supplied to off-chip devices…",null,null,null,{"$f":"VCCO_OFFCHIP+PS_OFFCHIP","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,70.490885500489355,2.4940828880583972]
[null,"Temp Grade","Industrial",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40,71.06910219484682,3.0722995824158712]
[null,"Process","Typical",null,null,null,"    On-Chip Power",null,null,null,null,null,"  Power Supply",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,71.978214929706681,3.9814123172757201,null,null,null,null,null,null,{"$f":"IF(GRADE=\"Industrial\",153,139)","v":153}]
[null,"Voltage ID Used","No",null,null,null,"Resource",null,null,"Power",null,null,"Source",null,"Voltage","Total (A)","Static","Active",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70,73.398822351347732,5.4020197389167812,null,null,null,null,null,"Static",{"$f":"IF(AND(PROCESS=\"Maximum\",NOT(EXACT($Z$1,\"nomtpf\"))),1,0)","v":0}]
[null,"Characterization",{"$f":"Production_Status&\" (± \"&IF(LEFT(Production_Status,3)=\"Pro\",20,25)&\"% accuracy)\"","v":"Production (± 20% accuracy)"},null,null,null,null,null,"(Jump to sheet)","(W)","(%)",null,"VCCINT",null,0.95,{"$f":"MAX(ICCINT_POWERUP,Q15+R15)*PL_POWERED","v":37.564070086258027},{"$f":"AX15*ICCQ_TEMP","v":4.1850035275084165},{"$f":"(CLOCK_POWER+LOGIC_POWER+Other_INTPOWER+BRAM_INTPOWER+DSP_POWER+MMCMINT_POWER+PLLINT_POWER+GTH_INTPOWER+GTY_INTPOWER+IO!AH18) / VCCINT","v":33.379066558749614},{"$f":"O15*P15","v":35.685866581945128},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,85,75.561972948832519,7.5651703364015672,null,null,null,null,null,null,{"$f":"IF(AND($AX$14>0,OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13)>0),OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13),1)","v":1}]
[null,null,null,null,null,null,"Core Dynamic",null,null,{"$f":"CLOCK_POWER","v":2.2318180018399989},{"$f":"IF(AND(ISNUMBER(J16),J16>0),J16/TOTAL_POWER,0)*100","v":2.6607442085473112},null,"VCCINT_IO",null,0.95,{"$f":"MAX(OFFSET(ICCINT_POWERUP,0,1),Q16+R16)","v":0.91909657589002802},{"$f":"AX16*J58","v":0.2589972017529561},{"$f":"IOINT_POWER/VCCINT_IO","v":0.66009937413707198},{"$f":"O16*P16","v":0.87314174709552661},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100,78.750650939409297,10.753848326978341,null,null,null,null,null,null,{"$f":"IF(AND($AX$14>0,OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+1)>0),OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+1),1)","v":1}]
[null,"     Environment",null,null,null,null,null,null,null,{"$f":"LOGIC_POWER","v":13.462057892934997},16.049289209167029,null,"VCCBRAM",null,0.95,{"$f":"MAX(ICCBRAM_POWERUP,Q17+R17)*PL_POWERED","v":0.52474105850230968},{"$f":"AX17*ICCBRAM_TEMP","v":0.36579772850230963},{"$f":"BRAM_BRAMPOWER/VCCBRAM","v":0.15894333000000002},0.49850400557719415,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND($AX$14>0,OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+2)>0),OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+2),1)","v":1}]
[null,"Junction Temperature",null,null,{"$f":"JUNCTION_TEMP","v":85.325771389040298},null,null,null,null,{"$f":"BRAM_POWER","v":5.7806426049106845},6.8916064482038406,null,"VCCAUX",null,1.8,{"$f":"MAX(ICCAUX_POWERUP,Q18+R18)*PL_POWERED","v":0.89912576732929073},{"$f":"AX18*ICCAUXQ_TEMP","v":0.55150221873536498},{"$f":"(MMCMAUX_POWER+PLLAUX_POWER+Other_AUXPOWER) / VCCAUX","v":0.34762354859392575},1.6184263811927233,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VCC_MIN","v":0.92},70.254254637843886,null,null,null,null,null,null,null,{"$f":"IF(AND($AX$14>0,OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+3)>0),OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+3),1)","v":1}]
[null,"Ambient Temp",20,null,null,null,null,null,null,{"$f":"DSP_POWER","v":5.5196240740114275},6.5804235722519717,null,"VCCAUX_IO",null,1.8,{"$f":"MAX(ICCAUXIO_POWERUP,Q19+R19)*PL_POWERED","v":0.56038230001102307},{"$f":"AX19*H58","v":0.222451260011023},{"$f":"IO!E6","v":0.33793104000000007},1.0086881400198415,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(AO18+AO20)/2","v":0.93500000000000005},71.17980482967684,null,null,null,null,null,null,null,{"$f":"IF(AND($AX$14>0,OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+4)>0),OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+4),1)","v":1}]
[null,"Effective ΘJA",null,null,{"$f":"TJA","v":0.77880529572292434},null,null,null,null,{"$f":"PLL_POWER","v":0.10789043426906636},0.12862556351028706,null,"VCCO 3.3V",null,3.3,{"$f":"IF(Q20>0,MAX(ICCO_POWERUP,IO!G7+Q20),0)*PL_POWERED","v":0},{"$f":"AW20*AX20","v":0},{"$f":"IO!G7","v":0},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SPEEDGRADE=\"-1L (0.9V)\",0.9,IF(SPEEDGRADE=\"-3\",1,0.95))","v":0.95},72.124198044875698,null,null,null,null,null,null,{"$f":"IF(OR(IO!BA501>0,LEFT(CFG_BANK,1)=\"3\"),ICCOQ_D,0)*PL_POWERED","v":0},{"$f":"IF(AND($AX$14>0,OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+6)>0),OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+6),1)","v":1}]
[null,"Airflow",500,null,null,null,null,null,null,{"$f":"MMCM_POWER","v":0.51026587700000003},0.60833229946515988,null,"VCCO 2.5V",null,2.5,{"$f":"IF(Q21>0,MAX(ICCO_POWERUP,IO!G8+Q21),0)*PL_POWERED","v":0},{"$f":"AW21*AX21","v":0},{"$f":"IO!G8","v":0},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(AO20+AO22)/2","v":0.96449999999999991},73.087791495136713,null,null,null,null,null,null,{"$f":"IF(OR(IO!BB501>0,LEFT(CFG_BANK,1)=\"2\"),ICCOQ_D,0)*PL_POWERED","v":0},{"$f":"IF(AND($AX$14>0,OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+6)>0),OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+6),1)","v":1}]
[null,"Heat Sink","Low Profile",null,null,null,null,null,null,{"$f":"Other_INTPOWER+Other_AUXPOWER+Other_XADCPOWER","v":2.5638400000000002E-2},3.0565764887718633E-2,null,"VCCO 1.8V",null,1.8,{"$f":"IF(Q22>0,MAX(ICCO_POWERUP,IO!G9+Q22),0)*PL_POWERED","v":1.0762907166350126},8.1486430670325003E-5,{"$f":"IO!G9","v":1.0762092302043422},1.9373232899430228,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VCC_MAX","v":0.97899999999999998},74.070968007883721,null,null,null,null,null,null,{"$f":"IF(OR(IO!BC501>0,LEFT(CFG_BANK,1)=\"1\"),ICCOQ_D,0)*PL_POWERED","v":8.1486430670325003E-5},{"$f":"IF(AND($AX$14>0,OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+5)>0),OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+5),1)","v":1}]
[null,"   ΘSA",0.9,null,null,null,null,null,null,{"$f":"IF(OR(NUM_CMACS>0,NUM_ILMACS>0),CMAC_POWER+ILMAC_POWER,0)+IF(NUM_PCIES>0,PCIE_POWER,0)","v":0},0,null,"VCCO 1.5V",null,1.5,{"$f":"IF(Q23>0,MAX(ICCO_POWERUP,IO!G10+Q23),0)*PL_POWERED","v":0},0,{"$f":"IO!G10","v":0},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(IO!BD501>0,ICCOQ_D,0)*PL_POWERED","v":0},{"$f":"IF(AND($AX$14>0,OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+5)>0),OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+5),1)","v":1}]
[null,"Board Selection","Small (4\"x4\")",null,null,null,null,null,null,0,{"$f":"IF(AND(ISNUMBER(J24),J24>0),J24/TOTAL_POWER,0)*100","v":0},null,"VCCO 1.35V",null,1.35,{"$f":"IF(Q24>0,MAX(ICCO_POWERUP,IO!G11+Q24),0)*PL_POWERED","v":0},0,{"$f":"IO!G11","v":0},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(IO!BE501>0,ICCOQ_D,0)*PL_POWERED","v":0},{"$f":"IF(AND($AX$14>0,OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+5)>0),OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+5),1)","v":1}]
[null,"   # of Board Layers","16 or more",null,null,null,"I/O",null,null,{"$f":"IO_POWER","v":3.2996935816898465},{"$f":"IF(AND(ISNUMBER(J25),J25>0),J25/TOTAL_POWER,0)*100","v":3.9338514969516831},null,"VCCO 1.2V",null,1.2,{"$f":"IF(Q25>0,MAX(ICCO_POWERUP,IO!G12+Q25),0)*PL_POWERED","v":0},0,{"$f":"IO!G12","v":0},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(IO!BF501>0,ICCOQ_D,0)*PL_POWERED","v":0},{"$f":"IF(AND($AX$14>0,OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+5)>0),OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+5),1)","v":1}]
[null,"   ΘJB",1.4,null,null,null,"Transceiver",null,null,{"$f":"IF(NUM_GTS>0,GTX_POWER,IF(NUM_GTHS>0,GTH_POWER,IF(NUM_GTPS>0,GTP_POWER,0)))","v":17.663842814539279},21.058602193694835,null,"Vcco 1.0V",null,1,{"$f":"IF(Q26>0,MAX(ICCO_POWERUP,IO!G13+Q26),0)*PL_POWERED","v":0},0,{"$f":"IO!G13","v":0},0,null,"0.95V","1.0V","1.2V","1.8V","total","checksum",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(IO!BG501>0,ICCOQ_D,0)*PL_POWERED","v":0},{"$f":"IF(AND($AX$14>0,OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+5)>0),OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+5),1)","v":1}]
[null,"   Board Temperature",25,null,null,null,null,null,null,{"$f":"IF(NUM_GTZS>0,GTZ_POWER,IF(NUM_GTYS>0,GTY_POWER,0))","v":27.879543583288999},33.237626932402812,null,"MGTVCCAUX",null,1.8,{"$f":"MAX(IGTVCCAUX_POWERUP,Q27+R27)*PL_POWERED","v":0.21704544182369145},{"$f":"IF(AND(O27>0,NUM_GTS>0),GTXAUXQ,IF(AND(O27>0,NUM_GTHS>0),GTHAUXQ,0))*PL_POWERED*AX27","v":2.6131185913682684E-3},{"$f":"IF(AND(O27>0,NUM_GTS>0),GTX_AUXPOWER/GTVCCAUX,IF(AND(O27>0,NUM_GTHS>0),GTH_AUXPOWER/GTVCCAUX,0))","v":0.2144323232323232},0.39068179528264463,null,{"$f":"P15+P16+P17","v":39.007907720650365},{"$f":"P28+P31","v":15.248209162743732},{"$f":"P25+P29+P32","v":21.657382736036492},{"$f":"P18+P19+P22+P27+P30+P34","v":3.102713344390386},{"$f":"U27+V27+W27+X27","v":79.016212963820976},{"$f":"SUM(P15:P34)","v":79.016212963820976},"(A)",null,null,null,null,null,null,null,null,null,null,null,null,null,"Temp",50,85,100,null,null,null,null,null,{"$f":"IF(AND($AX$14>0,OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+7)>0),OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+7),1)","v":1}]
[null,null,null,null,null,null,{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",\"PS Dynamic Static\",\"\")","v":""},null,null,{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",PS_POWER,0)","v":0},0,null,"MGTAVCC",null,1,{"$f":"MAX(IAVCC_POWERUP,Q28+R28)*PL_POWERED","v":11.027680806701404},{"$f":"IF(AND(O28>0,NUM_GTS>0),AVCCQ,IF(AND(O28>0,NUM_GTHS>0),GTHAVCCQ,IF(AND(O28>0,NUM_GTPS>0),GTPAVCCQ,0)))*PL_POWERED*AX28","v":0.3308571672145097},{"$f":"IF(AND(O28>0,NUM_GTS>0),GTAVCC_POWER/O28,IF(AND(O28>0,NUM_GTHS>0),GTH_AVDD/O28,IF(AND(O28>0,NUM_GTPS>0),GTP_AVCCPOWER/O28,0)))","v":10.696823639486896},11.027680806701404,null,{"$f":"U27*0.95","v":37.057512334617847},{"$f":"V27","v":15.248209162743732},{"$f":"1.2*W27","v":25.988859283243791},{"$f":"1.8*X27","v":5.5848840199026952},{"$f":"U28+V28+W28+X28","v":83.87946480050806},{"$f":"SUM(S15:S34)","v":83.87946480050806},"(W)",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"Typical (\" & IF(SPEEDGRADE=\"-1L (0.9V)\",\"0.9\",IF(SPEEDGRADE=\"-3\",\"1.0\",0.95))&\"V)\"","v":"Typical (0,95V)"},71.6282904089488,75.561972948832519,78.750650939409297,null,null,null,null,null,{"$f":"IF(AND($AX$14>0,OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+8)>0),OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+8),1)","v":1}]
[null,{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",\"PL\",\"\")&\" Implementation\"","v":" Implementation"},null,null,null,null,null,null,null,{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",PS_STATIC+IF(PL_POWERED=0,#REF!*VCCADC,0),0)","v":0},0,null,"MGTAVTT",null,1.2,{"$f":"MAX(IAVTT_POWERUP,Q29+R29)*PL_POWERED","v":4.0362035924677171},{"$f":"IF(AND(O29>0,NUM_GTS>0),AVTTQ,IF(AND(O29>0,NUM_GTHS>0),GTHVTTXQ,IF(AND(O29>0,NUM_GTPS>0),GTPVTTXQ,0)))*PL_POWERED*AX29","v":0.16370899246771675},{"$f":"IF(AND(O29>0,NUM_GTS>0),GTAVTT_POWER/AVTT,IF(AND(O29>0,NUM_GTHS>0),GTH_VTTX/O29,IF(AND(O29>0,NUM_GTPS>0),GTP_AVTTPOWER/O29,0)))","v":3.8724946},4.8434443109612602,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"Maximum (\" & VCC_MAX &\"V)\"","v":"Maximum (0,979V)"},76.70149605225825,83.888078746922773,89.184163987263048,null,null,null,null,null,{"$f":"IF(AND($AX$14>0,OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+9)>0),OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+9),1)","v":1}]
[null,{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",\"Usage/\",\"\")&\"Optimization\"","v":"Optimization"},"Default",null,null,{"$f":"IF(C30=\"Power Optimization\",2,IF(C30=\"Default\",1,3))","v":1},{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",\"PL Static \",\"Device Static\")","v":"Device Static"},{"$f":"J29+J30","v":7.3984475360237525},null,{"$f":"PL_STATIC","v":7.3984475360237525},8.8203323109173439,null,"MGTYVCCAUX",null,1.8,{"$f":"MAX(OFFSET(IGTVCCAUX_POWERUP,0,3),Q30+R30)","v":0.30837311859136829},{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",$G50,IF(NUM_GTZS>1,MGTZVCCHQ,IF(NUM_GTYS>0,GTYAUXQ,0)))*AX30","v":2.6131185913682684E-3},{"$f":"IF(AND(O30>0,LEFT(FAMILY,4)=\"Zynq\"),PS!D5,IF(NUM_GTZS>0,GTZ!D6,IF(NUM_GTYS>0,GTY!D6,0)))","v":0.30576000000000003},0.55507161346446299,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND($AX$14>0,OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+10)>0),OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+10),1)","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,null,"MGTYAVCC",null,1,{"$f":"MAX(OFFSET(IAVCC_POWERUP,0,3),Q31+R31)","v":4.2205283560423279},{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",PS!S3/1000,IF(NUM_GTZS>1,MGTZAVCCQ,IF(NUM_GTYS>0,GTYAVCCQ,0)))*AX31","v":0.53855255604232821},{"$f":"IF(AND(O31>0,LEFT(FAMILY,4)=\"Zynq\"),PS!D6,IF(NUM_GTZS>0,GTZ!D7,IF(NUM_GTYS>0,GTY!D7,0)))","v":3.6819757999999996},4.2205283560423279,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND($AX$14>0,OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+11)>0),OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+11),1)","v":1}]
[null,"Messages",{"$f":"IF(LEN(OVERMAP)>3,\"Number of \" & OVERMAP & \" exceeds part size.\",\"\")","v":""},null,null,null,null,null,null,null,null,null,"MGTYAVTT",null,1.2,{"$f":"MAX(OFFSET(IAVTT_POWERUP,0,3),Q32+R32)","v":17.621179143568774},{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",PS!S4/1000,IF(NUM_GTZS>1,MGTZVCCLQ,IF(NUM_GTYS>0,GTYVTTXQ,0)))*AX32","v":0.23840693556877182},{"$f":"IF(AND(O32>0,LEFT(FAMILY,4)=\"Zynq\"),PS!D7,IF(NUM_GTZS>0,GTZ!D8,IF(NUM_GTYS>0,GTY!D8,0)))","v":17.382772208000002},21.145414972282527,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND($AX$14>0,OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+12)>0),OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+12),1)","v":1}]
[null,null,{"$f":"IF(IOERRORS>0,\"WARNING: Unsupported I/O standard(s) for current selections, ignored for power calculations\",\"\")","v":""},null,null,null,null,null,null,null,null,null,"        -"]
[null,null,null,null,null,null,null,null,null,null,null,null,"VCCADC",null,1.8,{"$f":"Q34+R34","v":4.1496000000000005E-2},{"$f":"AW34*AX34","v":4.1400000000000006E-2},{"$f":"Other_XADCPOWER/VCCADC","v":9.6000000000000409E-5},7.4692800000000018E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VCCADCQ","v":4.1400000000000006E-2},{"$f":"IF(AND($AX$14>0,OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+13)>0),OFFSET(QUIESCENT_DATA,FACTOROW,$AX$13+13),1)","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,null,"        -"]
[null,"XILINX Power Advantage (check for updates)",null,null,null,"File Support Request (WebCase)",null,null,null,null,null,null,"Xilinx Power Estimator User Guide"]
[null,{"$f":"COPYRIGHT","v":"© Copyright 1994-2015 Xilinx, Inc. All Rights Reserved "},null,null,null,"Whitepaper - 7 Steps for Worst Case Power Estimation",null,null,null,null,null,null,"Introduction to XPE (video)"]
[]
[null,"Legend",null,"User Entry",null,null,"Calculated Value",null,"Summary Value",null,null,"User Override",null,"Warning",null,"Error"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEDEC",{"$f":"IF(AIRFLOW=250,THETAJA250,IF(AIRFLOW=500,THETAJA500,IF(AIRFLOW=750,THETAJA750,THETAJA)))","v":2.8}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Opt"]
[null,null,null,null,null,null,"Piccq","Iccauxq","Tj","Iccq",null,null,null,null,null,null,null,null,null,null,"BoardType",{"$f":"IF(EXACT(\"Small (4\"\"x4\"\")\",BOARD),1,IF(EXACT(\"Medium (10\"\"x10\"\")\",BOARD),2,IF(EXACT(\"Large (20\"\"x20\"\")\",BOARD),3,0)))","v":1},null,"Airflow","None",null,"Leakage",{"$f":"PL_POWERED*(ICCQ_TEMP*VCCINT+ICCBRAM_TEMP*VCCBRAM+ICCAUXQ_TEMP*VCCAUX+J58*O16+H58*O19+AW20*VCCO33+AW21*VCCO25+AW22*VCCO18+AW23*VCCO15+AW24*VCCO135+AW25*VCCO12+AW26*VCCO10+GTX_LEAKAGE+GTH_LEAKAGE+AW34*VCCADC+GTY_LEAKAGE)","v":7.3984475360237525},null,{"$f":"Q15*1000","v":4185.0035275084165},null,null,null,null,null,null,null,null,"Utilization",{"$f":"AM44&AM45&AM46&AM47&AM48&AM49","v":""}]
[null,null,null,null,null,{"$f":"PL_POWERED*OFFSET(VccScale,2,0)*((P53*F46^4+Q53*F46^3+R53*F46^2+S53*F46+T53)+(Iccbramq*1000/OFFSET(BLOCK_LEAKAGE,2,3)*EXP(F46/OFFSET(BLOCK_LEAKAGE,2,4))))/1000","v":0.36579772850230963},{"$f":"PS!S$2/OFFSET(PS_DATA,PSFACTOROW,IF(PROCESS<>\"Maximum\",6,9))*EXP(MIN(155,$I44)/OFFSET(PS_DATA,PSFACTOROW,IF(PROCESS<>\"Maximum\",7,10)))/1000","v":0},{"$f":"PL_POWERED*VccAuxScale*($P$52*$I44^4+$Q$52*$I44^3+$R$52*$I44^2+$S$52*$I44+$T$52)/1000","v":0.54926117298511057},{"$f":"TemperatureEstimate","v":83.634328072469927},{"$f":"PL_POWERED*VccScale*($P$51*$I44^4+$Q$51*$I44^3+$R$51*$I44^2+$S$51*$I44+$T$51+OFFSET(Iccbramq,0,2))/1000","v":4.1462443833545395},"Non-int Leakage",{"$f":"PL_POWERED*(Iccauxq_d*VCCAUX+IF(IO!AT504>0,ICCOQ_D, 0)*VCCO33+IF(IO!AT508>0,ICCOQ_D, 0)*VCCO25+IF(IO!AT509>0,ICCOQ_D, 0)*VCCO18+IF(IO!AT510>0,ICCOQ_D, 0)*VCCO15+IF(IO!AT511>0,ICCOQ_D, 0)*VCCO135+IF(IO!AT512>0,ICCOQ_D, 0)*VCCO12+GTX_LEAKAGE+GTH_LEAKAGE+GTP_LEAKAGE)","v":1.1622523037741721},null,null,null,null,null,null,null,null,"BoardLyr",{"$f":"IF(EXACT(\"8 to 11\",LAYERS),1,IF(EXACT(\"12 to 15\",LAYERS),2,IF(EXACT(\"16 or more\",LAYERS),3,0)))","v":3},null,"N/A","Default",null,"CLOCK",{"$f":"CLOCK_POWER","v":2.2318180018399989},null,{"$f":"Q16*1000","v":258.99720175295607},null,null,null,null,null,null,null,null,{"$f":"IF(IO!L11>1,\"I/O, \",\"\")","v":""}]
[null,null,null,null,"Temp",{"$f":"MIN(125,IF(ISBLANK(USER_TJ),TJA*(SUM(J12:J28,AW34)+PL_POWERED*((P52*F46^4+Q52*F46^3+R52*F46^2+S52*F46+T52)/1000*VccAuxScale*VCCAUX+(P51*F46^4+Q51*F46^3+R51*F46^2+S51*F46+T51)/1000*VccScale*VCCINT+(P55*F46^4+Q55*F46^3+R55*F46^2+S55*F46+T55)/1000*VccAuxScale*VCCAUX_IO+(P54*F46^4+Q54*F46^3+R54*F46^2+S54*F46+T54)/1000*VccioScale*VCCINT_IO))+AMBIENT_TEMP,USER_TJ))","v":83.634328072469927},{"$f":"PS!S$2/OFFSET(PS_DATA,PSFACTOROW,IF(PROCESS<>\"Maximum\",6,9))*EXP(MIN(155,$I45)/OFFSET(PS_DATA,PSFACTOROW,IF(PROCESS<>\"Maximum\",7,10)))/1000","v":0},0.55125383191240163,{"$f":"MIN(125,IF(ISBLANK(USER_TJ),TJA*(SUM(J$12:J$28)+$G44+$H44*VCCAUX+$J44*VCCINT+$H52*VCCAUX_IO+$J52*VCCINT_IO)+AMBIENT_TEMP,USER_TJ))","v":83.90335750196823},4.1807082584868498,"Scaled ICCQ_D",{"$f":"PL_POWERED*ICCQ_DES*PROCESS_FACTOR*VccScale","v":0.64118098977605842},null,null,null,"Max Adj","Typ Adj",null,null,null,"Airflow",{"$f":"IF(AIRFLOW=250,1,IF(AIRFLOW=500,2,IF(AIRFLOW=750,3,0)))","v":2},null,0,"Power Optimization",null,"LOGIC",{"$f":"LOGIC_POWER","v":13.462057892934997},null,365.79772850230961,null,null,null,null,null,null,null,null,{"$f":"IF(Logic!I4>1,\"Registers, \",\"\")","v":""}]
[null,null,null,null,"Initial",{"$f":"MIN(125,IF(ISBLANK(USER_TJ),TJA*(SUM(J12:J28)+(Iccauxq_d*VccAuxScale*VCCAUX+ICCQ_DES*VccScale*VCCINT+VccAuxScale*L81*VCCAUX_IO+VccioScale*L80*VCCINT_IO))+AMBIENT_TEMP,USER_TJ))","v":80.870245149869874},{"$f":"PS!S$2/OFFSET(PS_DATA,PSFACTOROW,IF(PROCESS<>\"Maximum\",6,9))*EXP(MIN(155,$I46)/OFFSET(PS_DATA,PSFACTOROW,IF(PROCESS<>\"Maximum\",7,10)))/1000","v":0},0.55147468473992145,83.933048037637917,4.1845273989382505,"Non-aux Leakage",{"$f":"L45+IF(IO!AT504>0,ICCOQ_D, 0)*VCCO33+IF(IO!AT508>0,ICCOQ_D, 0)*VCCO25+IF(IO!AT509>0,ICCOQ_D, 0)*VCCO18+IF(IO!AS510>0,ICCOQ_D, 0)*VCCO15+IF(IO!AT511>0,ICCOQ_D, 0)*VCCO135+IF(IO!AT512>0,ICCOQ_D, 0)*VCCO12+GTP_LEAKAGE+GTX_LEAKAGE+GTH_LEAKAGE","v":1.1734614666375032},null,null,"MMF Factor",{"$f":"IF(PROCESS<>\"Maximum\",1,OFFSET(QUIESCENT_DATA,FACTOROW,IF(OR(GRADE=\"Extended\",GRADE=\"Commercial\"),64,IF(OR(LEFT(GRADE,1)=\"Q\",LEFT(GRADE,1)=\"M\",LEFT(SPEEDGRADE,3)=\"-1L\"),66,65)))*OFFSET(POWER_SCALE,10,OFFSET(POWER_SCALE,1,1)))","v":1},1,{"$f":"IF(PROCESS<>\"Maximum\",1,OFFSET(QUIESCENT_DATA,FACTOROW,IF(OR(GRADE=\"Extended\",GRADE=\"Commercial\"),133,IF(OR(LEFT(GRADE,1)=\"Q\",LEFT(GRADE,1)=\"M\",LEFT(SPEEDGRADE,3)=\"-1L\"),135,134)))*OFFSET(POWER_SCALE,10,OFFSET(POWER_SCALE,1,1)))","v":1},1,null,"Heatsink",{"$f":"IF(EXACT(\"Custom\",HEATSINK),1,IF(EXACT(\"Low Profile\",HEATSINK),0,IF(EXACT(\"Medium Profile\",HEATSINK),2,IF(EXACT(\"High Profile\",HEATSINK),4,3))))","v":0},null,250,"Power Off",null,"BRAM",{"$f":"BRAM_POWER","v":5.7806426049106845},null,551.50221873536498,null,null,null,null,null,null,null,null,{"$f":"IF(Logic!I5>1,\"LUTs, \",\"\")","v":""}]
[null,null,null,null,null,null,{"$f":"PS!S$2/OFFSET(PS_DATA,PSFACTOROW,IF(PROCESS<>\"Maximum\",6,9))*EXP(MIN(155,$I47)/OFFSET(PS_DATA,PSFACTOROW,IF(PROCESS<>\"Maximum\",7,10)))/1000","v":0},0.55149916975686297,83.936338152530709,4.1849508034766174,"Scaled ICCAUXQ_D",{"$f":"Iccauxq_d*IF(PROCESS=\"Typical\",1,2)/0.121","v":2.8929938317664505},null,null,"MMF Aux",{"$f":"IF(PROCESS<>\"Maximum\",1,OFFSET(QUIESCENT_DATA,FACTOROW,IF(OR(GRADE=\"Extended\",GRADE=\"Commercial\"),67,IF(OR(LEFT(GRADE,1)=\"Q\",LEFT(GRADE,1)=\"M\",LEFT(SPEEDGRADE,3)=\"-1L\"),69,68)))*OFFSET(POWER_SCALE,10,OFFSET(POWER_SCALE,1,1)))","v":1},1,{"$f":"IF(PROCESS<>\"Maximum\",1,OFFSET(QUIESCENT_DATA,FACTOROW,IF(OR(GRADE=\"Extended\",GRADE=\"Commercial\"),136,IF(OR(LEFT(GRADE,1)=\"Q\",LEFT(GRADE,1)=\"M\",LEFT(SPEEDGRADE,3)=\"-1L\"),138,137)))*OFFSET(POWER_SCALE,10,OFFSET(POWER_SCALE,1,1)))","v":1},1,null,"Pkg size",{"$f":"OFFSET(Data!$A$718,MATCH(PACKAGE,BOARD_PKG_LIST,FALSE),3)","v":2756.25},null,500,{"$f":"\"Y43:Y45\"","v":"Y43:Y45"},null,"DSP",{"$f":"DSP_POWER","v":5.5196240740114275},null,222.45126001102301,null,null,null,null,null,null,null,null,{"$f":"IF(BRAM!H4>1,\"BRAMs, \",\"\")","v":""}]
[null,null,null,null,null,null,{"$f":"PS!S$2/OFFSET(PS_DATA,PSFACTOROW,IF(PROCESS<>\"Maximum\",6,9))*EXP(MIN(155,$I48)/OFFSET(PS_DATA,PSFACTOROW,IF(PROCESS<>\"Maximum\",7,10)))/1000","v":0},0.55150188439536585,83.936702906483745,4.1849977459821321,"Iccint_c1",{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+1)","v":8.8637783099584423E-4},null,null,"MMF Bram",{"$f":"IF(PROCESS<>\"Maximum\",1,OFFSET(QUIESCENT_DATA,FACTOROW,IF(OR(GRADE=\"Extended\",GRADE=\"Commercial\"),70,IF(OR(LEFT(GRADE,1)=\"Q\",LEFT(GRADE,1)=\"M\",LEFT(SPEEDGRADE,3)=\"-1L\"),72,71)))*OFFSET(POWER_SCALE,10,OFFSET(POWER_SCALE,1,1)))","v":1},1,null,null,null,"Air",{"$f":"1/(6*$V47*0.000001)","v":60.468631897203323},null,750,null,null,"PLL",{"$f":"PLL_POWER","v":0.10789043426906636},null,0,null,null,null,null,null,null,null,null,{"$f":"IF(DSP!H4>1,\"DSPs, \",\"\")","v":""}]
[null,null,null,null,null,null,{"$f":"PS!S$2/OFFSET(PS_DATA,PSFACTOROW,IF(PROCESS<>\"Maximum\",6,9))*EXP(MIN(155,$I49)/OFFSET(PS_DATA,PSFACTOROW,IF(PROCESS<>\"Maximum\",7,10)))/1000","v":0},0.55150218536672491,83.936743346438476,4.1850029504860258,"Iccint_c2",{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+2)","v":0.11990560983505652},null,null,"VID Factor",{"$f":"IF(AND(VID_Allowed=1,PROCESS=\"Maximum\",Voltage_Scaling=\"Yes\"),0.7,1)","v":1},null,null,null,null,"ThetaSA",{"$f":"IF((HEATSINK=\"Custom\")*(CUSTOMTSA>0),CUSTOMTSA,IF(HEATSINK=\"None\",0,OFFSET(Data!$A$953,OFFSET(Data!$A$718,MATCH(PACKAGE,BOARD_PKG_LIST,FALSE),2)+IF($V45<=1,0,1)+$V46,3)))","v":0.9},null,{"$f":"IF(OR($C22=\"None\",$C22=\"Custom\"),\"X45:X48\",\"X46:X47\")","v":"X46:X47"},null,null,"MMCM",{"$f":"MMCM_POWER","v":0.51026587700000003},null,0]
[null,null,null,null,null,null,{"$f":"PS!S$2/OFFSET(PS_DATA,PSFACTOROW,IF(PROCESS<>\"Maximum\",6,9))*EXP(MIN(155,$I50)/OFFSET(PS_DATA,PSFACTOROW,IF(PROCESS<>\"Maximum\",7,10)))/1000","v":0},0.55150221873536498,83.936747830006055,4.1850035275084165,"Iccintq_d",{"$f":"(P51*390625+Q51*15625+R51*625+S51*25+T51)/1000*OFFSET(POWER_SCALE,9,1)","v":0.63952900616079367},null,null,"Bali Factor",{"$f":"IF(AND(NUM_DICE>1,PROCESS=\"Maximum\",LEFT(SPEEDGRADE,3)<>\"-1L\"),IF(RIGHT(PART,5)=\"VU440\",1,1),1)","v":1},null,null,null,null,"ThetaCS",0.1,null,null,null,null,"Hard IP",{"$f":"PCIE_POWER+IF(OR(NUM_CMACS>0,NUM_ILMACS>0),CMAC_POWER+ILMAC_POWER,0)","v":0},null,8.1486430670325002E-2]
[null,null,null,null,null,null,null,"auxioq",null,"iccioq","Iccintq_des",{"$f":"ICCINTQ_D+OFFSET(BLOCK_LEAKAGE,1,1)*BRAM!I4/1000","v":0.64148687948937155},null,null,"Vccint",{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL)","v":3.3743240444207193E-5},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+1)","v":8.8637783099584423E-4},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+2)","v":0.11990560983505652},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+3)","v":10.076554775760851},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+4)","v":285.64352371203353},"ThetaJB",{"$f":"IF((BOARD=\"Custom\")*(CUSTOMTJB>0),CUSTOMTJB,THETAJB)","v":1.4},null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,{"$f":"PL_POWERED*$L$82*($P$55*$I44^4+$Q$55*$I44^3+$R$55*$I44^2+$S$55*$I44+$T$55)/1000","v":0.22240296709252494},null,{"$f":"PL_POWERED*VccioScale*($P$54*$I44^4+$Q$54*$I44^3+$R$54*$I44^2+$S$54*$I44+$T$54)/1000","v":0.25696307209871405},"Iccaux_c1",{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+6)","v":1.3169424834856415E-5},null,null,"Vccaux",{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+5)","v":2.2773392491199095E-6},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+6)","v":1.3169424834856415E-5},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+7)","v":6.6275639733392637E-3},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+8)","v":0.66452312605831276},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+9)","v":328.20159010171352},"ThetaJA",{"$f":"IF(BOARD=\"JEDEC (2S2P)\",V41,MIN(V41,OFFSET(Data!$A$815,OFFSET(Data!$A$718,MATCH(PACKAGE,BOARD_PKG_LIST,FALSE),1)+(4*$V45)+$V44,3+$V43)))","v":2.8},null,null,null,null,"IO",{"$f":"IO_POWER","v":3.2996935816898465},null,0]
[null,null,null,null,null,null,null,0.2224459014956735,null,0.25877194806191628,"Iccaux_c2",{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+7)","v":6.6275639733392637E-3},null,null,"Vccbram",{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+10)","v":1.2902428174797283E-6},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+11)","v":1.3796494125804877E-5},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+12)","v":7.1350554812356862E-3},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+13)","v":0.92615663124331837},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+14)","v":37.075943367494304},"ThetaJX",{"$f":"$V52*(THETAJC+$V48)/(THETAJC+$V48-$V52)","v":2.9358078260707887},null,null,null,null,{"$f":"IF(NUM_GTS>0,\"GTX\",IF(NUM_GTHS>0,\"GTH\",IF(NUM_GTPS>0,\"GTP\",\"\")))","v":"GTH"},{"$f":"IF(NUM_GTS>0,GTX_POWER,IF(NUM_GTHS>0,GTH_POWER,IF(NUM_GTPS>0,GTP_POWER,0)))","v":17.663842814539279},null,0]
[null,null,null,null,null,null,null,0.22245066593990509,null,0.25897223453507429,"Iccauxq_d",{"$f":"(P52*390625+Q52*15625+R52*625+S52*25+T52)/1000*OFFSET(POWER_SCALE,10,1)","v":0.35005225364374049},null,null,"Vccint_io",{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+72)","v":9.4026040376562139E-7},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+72+1)","v":9.3083239533747874E-5},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+72+2)","v":1.0958233301091337E-2},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+72+3)","v":0.72209462803770252},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+72+4)","v":19.644655760179944},"eThetaJA",{"$f":"IF((BOARD=\"Custom\"),$V57,IF($V46=3,$V52,$V53*(THETAJC+$V49+$V50)/($V53+THETAJC+$V49+$V50)))","v":0.77880529572292434},null,null,null,null,{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",\"PS\",IF(NUM_GTYS>0,\"GTY\",\"\"))","v":"GTY"},{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",PS_POWER,IF(NUM_GTYS>0,GTY_POWER,0))","v":27.879543583288999},null,0]
[null,null,null,null,null,null,null,0.22245119422563087,null,0.25899443703665442,"Iccoq",{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,IF(PROCESS=\"Typical\",61,IF(TJ_MAX=85,62,63)))/1000","v":8.1486430670325003E-5},null,null,"Vccaux_io",{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+72+5)","v":8.2165693508678828E-8},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+72+6)","v":-2.0770031921271607E-6},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+72+7)","v":4.727356642507581E-6},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+72+8)","v":9.3259042364777864E-3},{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+72+9)","v":218.78495021333421},"TJA-Top",{"$f":"$V49+THETAJC","v":0.96},null,null,null,null,null,null,null,2.6131185913682682]
[null,null,null,null,null,null,null,0.22245125279722303,null,0.25899689858448982,"Iccbram_c1",{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+11)","v":1.3796494125804877E-5},null,null,null,null,null,null,null,null,"TJ",{"$f":"(TOTAL_POWER*$V55*$V51+$V51*AMBIENT_TEMP+$V55*BOARD_TEMP)/($V55+$V51)","v":69.802542666052048},null,null,null,null,null,null,null,330.85716721450967]
[null,null,null,null,null,null,null,0.22245125929105311,null,0.25899717149537965,"Iccbram_c2",{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+12)","v":7.1350554812356862E-3},null,null,null,null,null,null,null,null,"eThetaJA",{"$f":"($V61 - AMBIENT_TEMP) /$V58","v":0.59396211898416174},null,null,null,null,null,null,null,163.70899246771674]
[null,null,null,null,null,null,null,0.222451260011023,null,0.2589972017529561,"Iccbramq",{"$f":"(IF(PROCESS=\"Typical\",1,OFFSET(BLOCK_LEAKAGE,2,IF(FACTORCOL=16,10,IF(FACTORCOL=31,9,8))))*(OFFSET(BLOCK_LEAKAGE,2,1)*BRAM!I4))/1000*OFFSET(POWER_SCALE,9,1)","v":2.4272000000000002E-2},{"$f":"(IF(PROCESS=\"Typical\",1,OFFSET(BLOCK_LEAKAGE,2,IF(FACTORCOL=16,10,IF(FACTORCOL=31,9,8))))*(OFFSET(BLOCK_LEAKAGE,1,1)*BRAM!I4))/1000*OFFSET(POWER_SCALE,9,1)","v":1.957873328577925E-3},{"$f":"OFFSET(Iccbramq,0,1)*1000/OFFSET(BLOCK_LEAKAGE,2,3)*EXP(F46/OFFSET(BLOCK_LEAKAGE,2,4))","v":11.684322987038966},null,null,null,null,null,null,"Power",{"$f":"SUM(J12:J28)+((P52*V62^4+Q52*V62^3+R52*V62^2+S52*V62+T52)/1000*VCCAUX+(P51*V62^4+Q51*V62^3+R51*V62^2+S51*V62+T51)/1000*VccScale*VCCINT)","v":83.116018418670251},null,null,null,null,null,null,null,2.6131185913682682]
[null,null,null,null,null,null,null,null,null,null,"Process",{"$f":"IF(PROCESS=\"Typical\",1,OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL))","v":1},null,null,null,null,null,null,null,null,"Power2",null,null,null,null,null,null,null,null,538.55255604232821]
[null,null,null,null,null,null,null,null,null,null,"I-Grade",{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+3)","v":10.076554775760851},null,null,null,null,null,null,null,null,"Temp",{"$f":"MIN(125,$V55*$V58+AMBIENT_TEMP)","v":99.791377681923436},null,null,null,null,null,null,null,238.40693556877181]
[null,null,null,null,null,null,null,null,null,null,"Q-Grade",{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+4)","v":285.64352371203353},null,null,null,null,null,null,null,null,"Temp",{"$f":"($V58 * $V55 * $V51 + $V51 * AMBIENT_TEMP + $V55 * BOARD_TEMP) / ($V55 + $V51)","v":69.367766421479999},null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,"I-Grade",{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+8)","v":0.66452312605831276},null,null,null,null,null,null,null,null,"Temp",{"$f":"MIN(125,IF(ISBLANK(USER_TJ),$V55*(SUM(J12:J28)+(Iccauxq_d*VccAuxScale*VCCAUX+ICCQ_DES*VccScale*VCCINT))+AMBIENT_TEMP,USER_TJ))","v":94.611423930877081},null,null,null,null,null,null,null,41.400000000000006]
[null,null,null,null,null,null,null,null,null,null,"Q-Grade",{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+9)","v":328.20159010171352}]
[null,null,null,null,null,null,null,null,null,null,"I-Grade",{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+13)","v":0.92615663124331837},null,null,"PowerUp","Int","Int_io","Aux","I/O","Aux_io","Bram","Avcc","Avtt","GTVccaux","Avcc","Avtt","GTVccaux"]
[null,null,null,null,null,null,null,null,null,null,"Q-Grade",{"$f":"OFFSET(QUIESCENT_DATA,FACTOROW,FACTORCOL+14)","v":37.075943367494304},null,null,"Adder",6.5949999999999998,0,0.8,0.08,0,0.3,9.4999999999999998E-3,4.4999999999999997E-3,2E-3,2.0833333333333332E-2,0.11666666666666667,1.6666666666666668E-3]
[null,null,null,null,null,null,null,null,null,null,"Vcc_c1",{"$f":"OFFSET(VOLTAGE_DATA,1,1)","v":0.16438900000000001},null,null,"Min",{"$f":"IF(AND(LEFT(PROCESS,3)=\"Max\",P65>0),ICCINTQ_D*VccScale+P65,0)","v":0},{"$f":"IF(AND(LEFT(PROCESS,3)=\"Max\",Q65>0),L80*L79+Q65,0)","v":0},{"$f":"IF(AND(LEFT(PROCESS,3)=\"Max\",R65>0),Iccauxq_d*VccAuxScale + R65,0)","v":0},{"$f":"IF(AND(LEFT(PROCESS,3)=\"Max\",S65>0),ICCOQ_D+S65,0)","v":0},{"$f":"IF(AND(LEFT(PROCESS,3)=\"Max\",T65>0),L81*L82+T65,0)","v":0},{"$f":"IF(AND(LEFT(PROCESS,3)=\"Max\",U65>0),(P53*390625+Q53*15625+R53*625+S53*25+T53)/1000*OFFSET(VccScale,2,0)+U65,0)","v":0},{"$f":"IF(AND(LEFT(PROCESS,3)=\"Max\",V65>0),OFFSET(GTHAVCCQ,0,-1)+IF(Q28>0,V65*MAX(NUM_GTHS,OFFSET(GTH_PLANES,-1,0)),0),0)","v":0},{"$f":"IF(AND(LEFT(PROCESS,3)=\"Max\",W65>0),OFFSET(GTHVTTXQ,0,-1)+IF(Q29>0,W65*MAX(NUM_GTHS,OFFSET(GTH_PLANES,-1,0)),0),0)","v":0},{"$f":"IF(AND(LEFT(PROCESS,3)=\"Max\",X65>0),OFFSET(GTHAUXQ,0,-1)+IF(Q27>0,X65*MAX(NUM_GTHS,OFFSET(GTH_PLANES,-1,0)),0),0)","v":0},{"$f":"IF(AND(LEFT(PROCESS,3)=\"Max\",Y65>0),OFFSET(GTYAVCCQ,0,-1)+IF(Q31>0,Y65*NUM_GTYS,0),0)","v":0},{"$f":"IF(AND(LEFT(PROCESS,3)=\"Max\",Z65>0),OFFSET(GTYVTTXQ,0,-1)+IF(Q32>0,Z65*NUM_GTYS,0),0)","v":0},{"$f":"IF(AND(LEFT(PROCESS,3)=\"Max\",AA65>0),OFFSET(GTYAUXQ,0,-1)+IF(Q30>0,AA65*NUM_GTYS,0),0)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"Vcc_c2",{"$f":"OFFSET(VOLTAGE_DATA,2,1)","v":1.900045}]
[null,null,null,null,null,null,null,null,null,null,"VccScale",{"$f":"Vcc_c1*EXP(Vcc_c2*VCCINT)*Bali_Factor*VID_Factor*MMF_Factor*OFFSET(MMF_Factor,0,1)*SCD_FACTOR","v":0.99952315515236012}]
[null,null,null,null,null,null,null,null,null,null,"VccAuxScale",{"$f":"Bali_Factor*OFFSET(MMF_Factor,1,0)*OFFSET(MMF_Factor,1,1)*SCD_FACTOR","v":1}]
[null,null,null,null,null,null,null,null,null,null,"VccBramScale",{"$f":"Vcc_c1*EXP(Vcc_c2*VCCBRAM)*VID_Factor*OFFSET(MMF_Factor,2,0)*OFFSET(MMF_Factor,2,1)","v":0.99952315515236012}]
[null,null,null,null,null,null,null,null,null,null,"AVccScale",{"$f":"Vcc_c1*EXP(Vcc_c2*AVCC)","v":1.0991369615222559}]
[null,null,null,null,null,null,null,null,null,null,"Max bram",{"$f":"Iccbramq/OFFSET(BLOCK_LEAKAGE,2,3)*EXP(TJ_MAX/OFFSET(BLOCK_LEAKAGE,2,4))*VCCBRAM","v":0.25367959207525348}]
[null,null,null,null,null,null,null,null,null,null,"Max PS",{"$f":"PS!S$2/OFFSET(PS_DATA,PSFACTOROW,IF(PROCESS_FACTOR=1,6,9))*EXP(TJ_MAX/OFFSET(PS_DATA,PSFACTOROW,IF(PROCESS_FACTOR=1,7,10)))/1000*VCCPINT","v":0}]
[null,null,null,null,null,null,null,null,null,null,"Max Aux",{"$f":"(($P$52*TJ_MAX^4+$Q$52*TJ_MAX^3+$R$52*TJ_MAX^2+$S$52*TJ_MAX+$T$52)+($P$55*TJ_MAX^4+$Q$55*TJ_MAX^3+$R$55*TJ_MAX^2+$S$55*TJ_MAX+$T$55))/1000*VCCAUX","v":1.6699270905898789}]
[null,null,null,null,null,null,null,null,null,null,"Max Int",{"$f":"(($P$51*TJ_MAX^4+$Q$51*TJ_MAX^3+$R$51*TJ_MAX^2+$S$51*TJ_MAX+$T$51)+($P$54*TJ_MAX^4+$Q$54*TJ_MAX^3+$R$54*TJ_MAX^2+$S$54*TJ_MAX+$T$54))/1000*VCCINT","v":6.7845225712134001}]
[null,null,null,null,null,null,null,null,null,null,"Max Ambient",{"$f":"IF(ISBLANK(USER_TJ),TJ_MAX-(TJA*(SUM(L72:L75)+SUM(J12:J28)+GTX_LEAKAGE+GTH_LEAKAGE+GTP_LEAKAGE+GTY_LEAKAGE)),AMBIENT_TEMP)","v":32.594010241507931}]
[]
[null,null,null,null,null,null,null,null,null,null,"Oly",{"$f":"IF(MID(PART,4,1) = \"U\",1,0)","v":1}]
[null,null,null,null,null,null,null,null,null,null,"VccioScale",{"$f":"OFFSET(VOLTAGE_DATA,1,2)*EXP(OFFSET(VOLTAGE_DATA,2,2)*VCCINT_IO)*VID_Factor*OFFSET(MMF_Factor,0,2)*OFFSET(MMF_Factor,0,3)*SCD_FACTOR","v":0.99930193719829807}]
[null,null,null,null,null,null,null,null,null,null,"vccio_d",{"$f":"(P54*390625+Q54*15625+R54*625+S54*25+T54)/1000*OFFSET(POWER_SCALE,9,1)","v":4.6367632112240348E-2}]
[null,null,null,null,null,null,null,null,null,null,"vccauxio_d",{"$f":"(P55*390625+Q55*15625+R55*625+S55*25+T55)/1000*OFFSET(POWER_SCALE,10,1)","v":0.21902069521629755}]
[null,null,null,null,null,null,null,null,null,null,"vccauxioScale",{"$f":"OFFSET(MMF_Factor,1,3)*OFFSET(MMF_Factor,1,2)*SCD_FACTOR","v":1}]

{"sheet":"Snapshot","index":1,"n_rows":45,"n_cols":11,"rows_kept":45,"cut":false,"hidden":false,"merged":[[2,1,5,1],[2,2,2,3],[2,4,2,5],[2,6,2,7],[2,8,2,9],[3,2,3,3],[3,4,3,5],[3,6,3,7],[3,8,3,9],[4,2,4,3],[4,4,4,5],[4,6,4,7],[4,8,4,9],[5,2,5,3],[5,4,5,5],[5,6,5,7],[2,20,2,21],[2,22,2,23],[2,24,2,25],[2,26,2,27],[2,28,2,29],[2,10,2,11],[2,12,2,13],[2,14,2,15],[2,16,2,17],[2,18,2,19],[2,40,2,41],[2,42,2,43],[2,44,2,45],[2,46,2,47],[2,48,2,49],[2,30,2,31],[2,32,2,33],[2,34,2,35],[2,36,2,37],[2,38,2,39],[3,20,3,21],[3,22,3,23],[3,24,3,25],[3,26,3,27],[3,28,3,29],[3,10,3,11],[3,12,3,13],[3,14,3,15],[3,16,3,17],[3,18,3,19],[3,40,3,41],[3,42,3,43],[3,44,3,45],[3,46,3,47],[3,48,3,49],[3,30,3,31],[3,32,3,33],[3,34,3,35],[3,36,3,37],[3,38,3,39],[4,20,4,21],[4,22,4,23],[4,24,4,25],[4,26,4,27],[4,28,4,29],[4,10,4,11],[4,12,4,13],[4,14,4,15],[4,16,4,17],[4,18,4,19],[4,40,4,41],[4,42,4,43],[4,44,4,45],[4,46,4,47],[4,48,4,49],[4,30,4,31],[4,32,4,33],[4,34,4,35],[4,36,4,37],[4,38,4,39],[5,34,5,35],[5,36,5,37],[5,18,5,19],[5,20,5,21],[5,22,5,23],[5,24,5,25],[5,26,5,27],[5,8,5,9],[5,10,5,11],[5,12,5,13],[5,14,5,15],[5,16,5,17],[5,48,5,49],[6,2,6,3],[6,4,6,5],[6,6,6,7],[6,8,6,9],[6,10,6,11],[6,12,6,13],[6,14,6,15],[6,16,6,17],[6,18,6,19],[6,20,6,21],[6,22,6,23],[6,24,6,25],[6,26,6,27],[6,28,6,29],[6,30,6,31],[5,38,5,39],[5,40,5,41],[5,42,5,43],[5,44,5,45],[5,46,5,47],[5,28,5,29],[5,30,5,31],[5,32,5,33],[7,2,7,3],[7,4,7,5],[7,6,7,7],[7,8,7,9],[7,10,7,11],[7,12,7,13],[7,14,7,15],[7,16,7,17],[7,18,7,19],[6,42,6,43],[6,44,6,45],[8,48,8,49],[8,30,8,31],[8,32,8,33],[8,34,8,35],[8,36,8,37],[8,38,8,39],[7,46,7,47],[7,48,7,49],[8,40,8,41],[8,42,8,43],[8,44,8,45],[8,46,8,47],[6,46,6,47],[6,48,6,49],[6,32,6,33],[6,34,6,35],[6,36,6,37],[6,38,6,39],[6,40,6,41],[7,40,7,41],[7,42,7,43],[7,44,7,45],[8,18,8,19],[7,30,7,31],[7,32,7,33],[7,34,7,35],[7,20,7,21],[7,22,7,23],[7,24,7,25],[7,26,7,27],[7,28,7,29],[8,20,8,21],[8,22,8,23],[8,24,8,25],[8,26,8,27],[8,28,8,29],[7,36,7,37],[7,38,7,39],[9,2,9,3],[9,4,9,5],[9,6,9,7],[9,8,9,9],[9,10,9,11],[9,24,9,25],[9,26,9,27],[9,28,9,29],[9,30,9,31],[9,12,9,13],[9,14,9,15],[9,16,9,17],[9,18,9,19],[9,20,9,21],[8,2,8,3],[8,4,8,5],[8,6,8,7],[8,8,8,9],[8,10,8,11],[8,12,8,13],[8,14,8,15],[8,16,8,17],[12,32,12,33],[12,34,12,35],[9,42,9,43],[9,44,9,45],[9,46,9,47],[9,48,9,49],[12,2,12,3],[12,4,12,5],[12,6,12,7],[12,8,12,9],[12,10,12,11],[12,12,12,13],[12,14,12,15],[12,16,12,17],[12,18,12,19],[12,20,12,21],[12,22,12,23],[12,24,12,25],[9,32,9,33],[9,34,9,35],[9,36,9,37],[9,38,9,39],[9,40,9,41],[9,22,9,23],[12,46,12,47],[12,48,12,49],[13,2,13,3],[13,4,13,5],[13,6,13,7],[13,8,13,9],[13,10,13,11],[13,12,13,13],[13,14,13,15],[13,16,13,17],[13,18,13,19],[13,20,13,21],[13,22,13,23],[13,24,13,25],[13,26,13,27],[13,28,13,29],[12,36,12,37],[12,38,12,39],[12,40,12,41],[12,42,12,43],[12,44,12,45],[12,26,12,27],[12,28,12,29],[12,30,12,31],[13,40,13,41],[13,42,13,43],[13,44,13,45],[13,46,13,47],[13,48,13,49],[13,30,13,31],[13,32,13,33],[13,34,13,35],[13,36,13,37],[13,38,13,39],[14,12,14,13],[14,14,14,15],[14,16,14,17],[14,18,14,19],[14,20,14,21],[14,2,14,3],[14,4,14,5],[14,6,14,7],[14,8,14,9],[14,10,14,11],[14,46,14,47],[14,48,14,49],[17,2,17,3],[17,4,17,5],[17,6,17,7],[17,8,17,9],[17,10,17,11],[17,12,17,13],[17,14,17,15],[17,16,17,17],[17,18,17,19],[17,20,17,21],[17,22,17,23],[17,24,17,25],[14,32,14,33],[14,34,14,35],[14,36,14,37],[14,38,14,39],[14,40,14,41],[14,22,14,23],[14,24,14,25],[14,26,14,27],[14,28,14,29],[14,30,14,31],[17,40,17,41],[17,42,17,43],[17,44,17,45],[17,26,17,27],[17,28,17,29],[17,30,17,31],[17,32,17,33],[17,34,17,35],[14,42,14,43],[14,44,14,45],[18,48,18,49],[18,30,18,31],[18,32,18,33],[18,34,18,35],[18,36,18,37],[18,38,18,39],[17,46,17,47],[17,48,17,49],[18,2,18,3],[18,4,18,5],[18,6,18,7],[18,8,18,9],[18,10,18,11],[18,12,18,13],[18,14,18,15],[18,16,18,17],[18,18,18,19],[18,20,18,21],[18,22,18,23],[18,24,18,25],[18,26,18,27],[18,28,18,29],[17,36,17,37],[17,38,17,39],[19,2,19,3],[19,4,19,5],[19,6,19,7],[19,8,19,9],[19,10,19,11],[18,40,18,41],[18,42,18,43],[18,44,18,45],[18,46,18,47],[19,24,19,25],[19,26,19,27],[19,28,19,29],[19,30,19,31],[19,12,19,13],[19,14,19,15],[19,16,19,17],[19,18,19,19],[19,20,19,21],[20,32,20,33],[20,34,20,35],[19,42,19,43],[19,44,19,45],[19,46,19,47],[19,48,19,49],[20,2,20,3],[20,4,20,5],[20,6,20,7],[20,8,20,9],[20,10,20,11],[20,12,20,13],[20,14,20,15],[20,16,20,17],[20,18,20,19],[20,20,20,21],[20,22,20,23],[20,24,20,25],[19,32,19,33],[19,34,19,35],[19,36,19,37],[19,38,19,39],[19,40,19,41],[19,22,19,23],[20,46,20,47],[20,48,20,49],[21,2,21,3],[21,4,21,5],[21,6,21,7],[21,8,21,9],[21,10,21,11],[21,12,21,13],[21,14,21,15],[21,16,21,17],[21,18,21,19],[21,20,21,21],[21,22,21,23],[21,24,21,25],[21,26,21,27],[21,28,21,29],[20,36,20,37],[20,38,20,39],[20,40,20,41],[20,42,20,43],[20,44,20,45],[20,26,20,27],[20,28,20,29],[20,30,20,31],[21,40,21,41],[21,42,21,43],[21,44,21,45],[21,46,21,47],[21,48,21,49],[21,30,21,31],[21,32,21,33],[21,34,21,35],[21,36,21,37],[21,38,21,39],[22,28,22,29],[22,30,22,31],[22,12,22,13],[22,14,22,15],[22,16,22,17],[22,18,22,19],[22,20,22,21],[22,2,22,3],[22,4,22,5],[22,6,22,7],[22,8,22,9],[22,10,22,11],[22,42,22,43],[22,44,22,45],[22,46,22,47],[22,48,22,49],[23,2,23,3],[23,4,23,5],[23,6,23,7],[23,8,23,9],[23,10,23,11],[23,12,23,13],[23,14,23,15],[23,16,23,17],[23,18,23,19],[23,20,23,21],[23,22,23,23],[23,24,23,25],[22,32,22,33],[22,34,22,35],[22,36,22,37],[22,38,22,39],[22,40,22,41],[22,22,22,23],[22,24,22,25],[22,26,22,27],[23,46,23,47],[23,48,23,49],[23,36,23,37],[23,38,23,39],[23,40,23,41],[23,42,23,43],[23,44,23,45],[23,26,23,27],[23,28,23,29],[23,30,23,31],[23,32,23,33],[23,34,23,35]]}
[null,"                                                                                                        ",null,null,null,null,null,null,null,null,"Power Comparison Snapshots"]
[]
[null,"Settings"]
[]
[]
[]
[null,"Part"]
[null,"Ambient Temperature"]
[null,"Process"]
[null,"Implementation"]
[]
[null,"Summary"]
[null,"Total On-Chip Power"]
[null,"Junction Temperature"]
[null,"Effective ΘJA"]
[]
[null,"On-Chip Power"]
[null,"Clocking"]
[null,"Logic"]
[null,"I/O"]
[null,"BRAM"]
[null,"DSP"]
[null,"Transceiver"]
[null,"Device Static"]
[]
[null,"Supply Summary"]
[null,"VCCINT"]
[null,"VCCINT_IO"]
[null,"VCCBRAM"]
[null,"VCCAUX"]
[null,"VCCAUX_IO"]
[null,"VCCO 3.3V"]
[null,"VCCO 2.5V"]
[null,"VCCO 1.8V"]
[null,"VCCO 1.5V"]
[null,"VCCO 1.35V"]
[null,"VCCO 1.2V"]
[null,"VCCO 1.0V"]
[null,"MGTVCCAUX"]
[null,"MGTAVCC"]
[null,"MGTAVTT"]
[null,"MGTYVCCAUX"]
[null,"MGTYAVCC"]
[null,"MGTYAVTT"]
[null,"VCCADC"]

{"sheet":"Graphs","index":2,"n_rows":43,"n_cols":2,"rows_kept":43,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"\"On-Chip Power over Vccint - (\" & PROCESS & \", \" & IF(JUNCTION_TEMP=\"125+\",JUNCTION_TEMP,INT(JUNCTION_TEMP))& \"C)\"","v":"On-Chip Power over Vccint - (Typical, 85C)"}]
[null,{"$f":"\"On-Chip Power - (\" & PROCESS & \", \" & VCCINT & \"V)\"","v":"On-Chip Power - (Typical, 0,95V)"}]
[null,{"$f":"\"On-Chip Power by Function - (\" & PROCESS & \", \" & VCCINT & \"V, \" & IF(JUNCTION_TEMP=\"125+\",JUNCTION_TEMP,INT(JUNCTION_TEMP)) & \"C)\"","v":"On-Chip Power by Function - (Typical, 0,95V, 85C)"}]

{"sheet":"IP_Manager","index":3,"n_rows":43,"n_cols":37,"rows_kept":43,"cut":false,"hidden":false,"merged":[[13,1,13,3],[5,7,5,8],[3,2,3,3],[4,2,4,3],[5,2,5,3],[12,1,12,3],[14,1,14,3],[15,1,15,3],[19,1,19,3],[20,1,20,3],[16,1,16,3],[17,1,17,3],[18,1,18,3],[32,1,32,3],[37,1,37,3],[38,1,38,3],[39,1,39,3],[21,1,21,3],[22,1,22,3],[23,1,23,3],[24,1,24,3],[0,1,0,11],[2,5,2,8],[3,5,3,6],[4,5,4,6],[2,1,2,3],[3,7,3,8],[41,1,41,3],[4,7,4,8],[5,5,5,6],[6,2,6,3],[35,1,35,3],[25,1,25,3],[26,1,26,3],[27,1,27,3],[28,1,28,3],[36,1,36,3],[33,1,33,3],[34,1,34,3],[40,1,40,3],[29,1,29,3],[30,1,30,3],[31,1,31,3]]}
[null,"IP Manager",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IP Catalog"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Block Memory"]
[null,"Device",null,null,null,"On-Chip Summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Distributed Memory"]
[null,"Part","XCVU095FFVD1924-2I",null,null,"Junction Temp",null,{"$f":"JUNCTION_TEMP","v":85.325771389040298},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Memory Interface"]
[null,"Process",{"$f":"PROCESS","v":"Typical"},null,null,"Static Power",null,{"$f":"SUM(Summary!J29:J30)","v":7.3984475360237525},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(NUM_GTHS>1, \"Transceiver Interface\",\"\")","v":"Transceiver Interface"}]
[null,"Effective ΘJA",{"$f":"TJA","v":0.77880529572292434},null,null,"Total Power",null,{"$f":"TOTAL_POWER","v":83.87946480050806},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(NUM_GTYS>1,\"GTY Transceiver Interface\",\"\")","v":"GTY Transceiver Interface"}]
[null,"Implementation",{"$f":"OPTIMIZATION","v":"Default"}]
[]
[]
[]
[]
[]
[null,"IP Modules",null,null,"Power (W)","Clocking*","Logic","I/O*","BRAM","DSP","Transceiver*","Source",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Clock","PLL","MMCM","Logic","I/O","Phaser","BRAM","DSP","PCIE","GTP/X/H","GTZ"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"ROW(IPROWS)-14","v":29}]

{"sheet":"Clock","index":4,"n_rows":201,"n_cols":23,"rows_kept":201,"cut":false,"hidden":false,"merged":[[6,9,6,11],[0,1,0,11],[47,1,47,3],[48,1,48,3],[2,9,2,11],[2,5,2,7],[20,1,20,3],[22,1,22,3],[31,1,31,3],[26,1,26,3],[33,1,33,3],[42,1,42,3],[43,1,43,3],[4,9,4,11],[9,1,9,3],[15,1,15,3],[16,1,16,3],[10,1,10,3],[34,1,34,3],[35,1,35,3],[29,1,29,3],[27,1,27,3],[2,1,2,3],[4,1,4,3],[82,1,82,3],[80,1,80,3],[81,1,81,3],[83,1,83,3],[73,1,73,3],[66,1,66,3],[36,1,36,3],[40,1,40,3],[45,1,45,3],[39,1,39,3],[38,1,38,3],[53,1,53,3],[44,1,44,3],[46,1,46,3],[41,1,41,3],[52,1,52,3],[76,1,76,3],[69,1,69,3],[60,1,60,3],[58,1,58,3],[71,1,71,3],[72,1,72,3],[51,1,51,3],[77,1,77,3],[79,1,79,3],[25,1,25,3],[17,1,17,3],[18,1,18,3],[28,1,28,3],[49,1,49,3],[50,1,50,3],[32,1,32,3],[55,1,55,3],[56,1,56,3],[57,1,57,3],[59,1,59,3],[65,1,65,3],[74,1,74,3],[78,1,78,3],[75,1,75,3],[61,1,61,3],[64,1,64,3],[62,1,62,3],[70,1,70,3],[67,1,67,3],[68,1,68,3],[37,1,37,3],[13,1,13,3],[11,1,11,3],[14,1,14,3],[12,1,12,3],[30,1,30,3],[19,1,19,3],[21,1,21,3],[24,1,24,3],[23,1,23,3],[8,1,8,3],[63,1,63,3],[54,1,54,3],[147,1,147,3],[145,1,145,3],[91,1,91,3],[84,1,84,3],[139,1,139,3],[144,1,144,3],[135,1,135,3],[137,1,137,3],[130,1,130,3],[140,1,140,3],[86,1,86,3],[88,1,88,3],[116,1,116,3],[117,1,117,3],[98,1,98,3],[102,1,102,3],[105,1,105,3],[143,1,143,3],[122,1,122,3],[123,1,123,3],[87,1,87,3],[92,1,92,3],[146,1,146,3],[85,1,85,3],[150,1,150,3],[99,1,99,3],[89,1,89,3],[90,1,90,3],[94,1,94,3],[124,1,124,3],[128,1,128,3],[126,1,126,3],[127,1,127,3],[121,1,121,3],[113,1,113,3],[95,1,95,3],[108,1,108,3],[109,1,109,3],[93,1,93,3],[97,1,97,3],[96,1,96,3],[104,1,104,3],[110,1,110,3],[120,1,120,3],[119,1,119,3],[111,1,111,3],[115,1,115,3],[118,1,118,3],[154,1,154,3],[151,1,151,3],[152,1,152,3],[156,1,156,3],[100,1,100,3],[101,1,101,3],[112,1,112,3],[103,1,103,3],[106,1,106,3],[107,1,107,3],[149,1,149,3],[153,1,153,3],[134,1,134,3],[125,1,125,3],[141,1,141,3],[138,1,138,3],[129,1,129,3],[148,1,148,3],[142,1,142,3],[136,1,136,3],[114,1,114,3],[131,1,131,3],[133,1,133,3],[132,1,132,3],[176,1,176,3],[175,1,175,3],[171,1,171,3],[173,1,173,3],[155,1,155,3],[162,1,162,3],[163,1,163,3],[159,1,159,3],[168,1,168,3],[160,1,160,3],[170,1,170,3],[158,1,158,3],[167,1,167,3],[166,1,166,3],[164,1,164,3],[165,1,165,3],[169,1,169,3],[174,1,174,3],[172,1,172,3],[161,1,161,3],[157,1,157,3],[177,1,177,3],[178,1,178,3],[185,1,185,3],[184,1,184,3],[180,1,180,3],[183,1,183,3],[199,1,199,3],[198,1,198,3],[194,1,194,3],[196,1,196,3],[197,1,197,3],[182,1,182,3],[192,1,192,3],[187,1,187,3],[193,1,193,3],[195,1,195,3],[190,1,190,3],[188,1,188,3],[189,1,189,3],[191,1,191,3],[186,1,186,3],[179,1,179,3],[181,1,181,3]]}
[null,"Clock Tree Power",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(FALSE,1,OFFSET(POWER_SCALE,2,OFFSET(POWER_SCALE,1,1))*PL_POWERED/0.95)*0.95","v":0.99999999999999989},{"$f":"CLOCK_ROWS*CLOCK_COLS*34","v":3060},720,30,20]
[]
[null,"Power",null,null,null,"Utilization",null,null,null,"Clocking Resources User Guide"]
[null,"VCCINT",{"$f":"TEXT(VCCINT,\"0.000\")&\"V\"","v":"0.001V"},{"$f":"SUM(J10:J200)","v":2.2318180018399989},null,"  Global",{"$f":"SUM(IF((F10:F199=\"Global\")*(E10:E199>0),1))","v":1},{"$f":"IF(AND(G4/NUM_BUFG>=0.995, G4/NUM_BUFG<0.9999),0.99,G4/NUM_BUFG)","v":1.3888888888888889E-3}]
[null,{"$f":"TEXT(CLOCK_POWER/TOTAL_POWER,\"0%\")&\" of total on-chip power \"&TEXT(TOTAL_POWER,\"0.000\")&\"W\"","v":"3% of total on-chip power 0.084W"},null,null,null,"  I/O",{"$f":"SUM(IF((F9:F198=\"I/O\")*(E9:E198>0),1))","v":0},"-",null,"XPE User Guide"]
[null,null,null,null,null,"  Other",{"$f":"SUM(IF((F9:F199=\"Other\")*(E9:E199>0),1))","v":0},"-"]
[null,null,null,null,null,null,null,null,null,"Introduction to XPE (video)"]
[]
[null,"Name",null,null,"Frequency (MHz)","Type","Fanout","Clock Buffer Enable","Slice Clock Enable","Power (W)",null,null,"Buffer","HROW","LEAF","Local","HROW Utilization","LEAF Utilization","Slices",null,"RP","Total Slice Clock Enable","Number of Bels in Logic sheet "]
[null,"ck1",null,null,640,"Global",150000,1,0.5,{"$f":"IF($G10>0,SUM($M10:$P10)*(VCCINT/1000)*VCCINT_N,0)*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),1)*$P$1","v":2.2318180018399989},null,null,{"$f":"IF($F10=\"Other\",0.0004,IF($F10=\"CMT\",OFFSET(CLOCK_DATA,5,7),OFFSET(CLOCK_DATA,5,1)))*$E10","v":2.3705919999999998},{"$f":"(OFFSET(CLOCK_DATA,5,2)+OFFSET(CLOCK_DATA,5,10)*0.25)*$E10*$H10*$Q10","v":51.520551999999988},{"$f":"OFFSET(CLOCK_DATA,5,3)*$E10*$H10*$R10","v":287.14380800000004},{"$f":"((OFFSET(CLOCK_DATA,5,4)*1.5)+OFFSET(CLOCK_DATA,5,5)*2.25*MIN($H10,$I10))*$E10*$S10","v":2008.2471551999993},{"$f":"IF(AND($G10>0,OR($F10=\"Global\",$F10=\"Regional\")), INT(0.99+MAX(CLOCK_COLS/2000/NUM_DICE,MIN(CLOCK_ROWS*(CLOCK_COLS), 0.5*$G10^0.32))), 0)","v":23},{"$f":"IF(AND($G10>0,OR($F10=\"Global\",$F10=\"Regional\")),INT(0.99+MIN(NUM_LEAFS, 0.0845*(NUM_FFS^0.08)*$G10^0.6551)), 0)","v":668},{"$f":"INT(0.9 + MIN(NUM_LUTS/8,INT(0.99+0.3589*$G10^0.9323)))","v":24024}]
[null,"ck2",null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,{"$f":"IF($G42>0,SUM($M42:$P42)*(VCCINT/1000)*VCCINT_N,0)*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),1)*$P$1","v":0},null,null,0,{"$f":"(OFFSET(CLOCK_DATA,5,2)+OFFSET(CLOCK_DATA,5,10)*0.25)*$E42*$H42*$Q42","v":0},{"$f":"OFFSET(CLOCK_DATA,5,3)*$E42*$H42*$R42","v":0},{"$f":"((OFFSET(CLOCK_DATA,5,4)*1.5)+OFFSET(CLOCK_DATA,5,5)*2.25*MIN($H42,$I42))*$E42*$S42","v":0},{"$f":"IF(AND($G42>0,OR($F42=\"Global\",$F42=\"Regional\")), INT(0.99+MAX(CLOCK_COLS/2000/NUM_DICE,MIN(CLOCK_ROWS*(CLOCK_COLS), 0.5*$G42^0.32))), 0)","v":0},{"$f":"IF(AND($G42>0,OR($F42=\"Global\",$F42=\"Regional\")),INT(0.99+MIN(NUM_LEAFS, 0.0845*(NUM_FFS^0.08)*$G42^0.6551)), 0)","v":0},{"$f":"INT(0.9 + MIN(NUM_LUTS/8,INT(0.99+0.3589*$G42^0.9323)))","v":0}]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,{"$f":"IF($G74>0,SUM($M74:$P74)*(VCCINT/1000)*VCCINT_N,0)*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),1)*$P$1","v":0},null,null,{"$f":"IF($F74=\"Other\",0.0004,IF($F74=\"CMT\",OFFSET(CLOCK_DATA,5,7),OFFSET(CLOCK_DATA,5,1)))*$E74","v":0},{"$f":"(OFFSET(CLOCK_DATA,5,2)+OFFSET(CLOCK_DATA,5,10)*0.25)*$E74*$H74*$Q74","v":0},{"$f":"OFFSET(CLOCK_DATA,5,3)*$E74*$H74*$R74","v":0},{"$f":"((OFFSET(CLOCK_DATA,5,4)*1.5)+OFFSET(CLOCK_DATA,5,5)*2.25*MIN($H74,$I74))*$E74*$S74","v":0},{"$f":"IF(AND($G74>0,OR($F74=\"Global\",$F74=\"Regional\")), INT(0.99+MAX(CLOCK_COLS/2000/NUM_DICE,MIN(CLOCK_ROWS*(CLOCK_COLS), 0.5*$G74^0.32))), 0)","v":0},{"$f":"IF(AND($G74>0,OR($F74=\"Global\",$F74=\"Regional\")),INT(0.99+MIN(NUM_LEAFS, 0.0845*(NUM_FFS^0.08)*$G74^0.6551)), 0)","v":0},{"$f":"INT(0.9 + MIN(NUM_LUTS/8,INT(0.99+0.3589*$G74^0.9323)))","v":0}]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,{"$f":"IF($G106>0,SUM($M106:$P106)*(VCCINT/1000)*VCCINT_N,0)*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),1)*$P$1","v":0},null,null,0,{"$f":"(OFFSET(CLOCK_DATA,5,2)+OFFSET(CLOCK_DATA,5,10)*0.25)*$E106*$H106*$Q106","v":0},{"$f":"OFFSET(CLOCK_DATA,5,3)*$E106*$H106*$R106","v":0},{"$f":"((OFFSET(CLOCK_DATA,5,4)*1.5)+OFFSET(CLOCK_DATA,5,5)*2.25*MIN($H106,$I106))*$E106*$S106","v":0},{"$f":"IF(AND($G106>0,OR($F106=\"Global\",$F106=\"Regional\")), INT(0.99+MAX(CLOCK_COLS/2000/NUM_DICE,MIN(CLOCK_ROWS*(CLOCK_COLS), 0.5*$G106^0.32))), 0)","v":0},{"$f":"IF(AND($G106>0,OR($F106=\"Global\",$F106=\"Regional\")),INT(0.99+MIN(NUM_LEAFS, 0.0845*(NUM_FFS^0.08)*$G106^0.6551)), 0)","v":0},{"$f":"INT(0.9 + MIN(NUM_LUTS/8,INT(0.99+0.3589*$G106^0.9323)))","v":0}]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,{"$f":"IF($G138>0,SUM($M138:$P138)*(VCCINT/1000)*VCCINT_N,0)*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),1)*$P$1","v":0},null,null,{"$f":"IF($F138=\"Other\",0.0004,IF($F138=\"CMT\",OFFSET(CLOCK_DATA,5,7),OFFSET(CLOCK_DATA,5,1)))*$E138","v":0},{"$f":"(OFFSET(CLOCK_DATA,5,2)+OFFSET(CLOCK_DATA,5,10)*0.25)*$E138*$H138*$Q138","v":0},{"$f":"OFFSET(CLOCK_DATA,5,3)*$E138*$H138*$R138","v":0},{"$f":"((OFFSET(CLOCK_DATA,5,4)*1.5)+OFFSET(CLOCK_DATA,5,5)*2.25*MIN($H138,$I138))*$E138*$S138","v":0},{"$f":"IF(AND($G138>0,OR($F138=\"Global\",$F138=\"Regional\")), INT(0.99+MAX(CLOCK_COLS/2000/NUM_DICE,MIN(CLOCK_ROWS*(CLOCK_COLS), 0.5*$G138^0.32))), 0)","v":0},{"$f":"IF(AND($G138>0,OR($F138=\"Global\",$F138=\"Regional\")),INT(0.99+MIN(NUM_LEAFS, 0.0845*(NUM_FFS^0.08)*$G138^0.6551)), 0)","v":0},{"$f":"INT(0.9 + MIN(NUM_LUTS/8,INT(0.99+0.3589*$G138^0.9323)))","v":0}]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,{"$f":"IF($G170>0,SUM($M170:$P170)*(VCCINT/1000)*VCCINT_N,0)*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),1)*$P$1","v":0},null,null,0,{"$f":"(OFFSET(CLOCK_DATA,5,2)+OFFSET(CLOCK_DATA,5,10)*0.25)*$E170*$H170*$Q170","v":0},{"$f":"OFFSET(CLOCK_DATA,5,3)*$E170*$H170*$R170","v":0},{"$f":"((OFFSET(CLOCK_DATA,5,4)*1.5)+OFFSET(CLOCK_DATA,5,5)*2.25*MIN($H170,$I170))*$E170*$S170","v":0},{"$f":"IF(AND($G170>0,OR($F170=\"Global\",$F170=\"Regional\")), INT(0.99+MAX(CLOCK_COLS/2000/NUM_DICE,MIN(CLOCK_ROWS*(CLOCK_COLS), 0.5*$G170^0.32))), 0)","v":0},{"$f":"IF(AND($G170>0,OR($F170=\"Global\",$F170=\"Regional\")),INT(0.99+MIN(NUM_LEAFS, 0.0845*(NUM_FFS^0.08)*$G170^0.6551)), 0)","v":0},{"$f":"INT(0.9 + MIN(NUM_LUTS/8,INT(0.99+0.3589*$G170^0.9323)))","v":0}]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,"Global",null,1,0.5,0,null,null,0,0,0,0,0,0,0]
[null,{"$f":"ROW(CLOCKROWS)-10","v":191}]

{"sheet":"Logic","index":5,"n_rows":501,"n_cols":32,"rows_kept":501,"cut":false,"hidden":false,"merged":[[416,1,416,3],[417,1,417,3],[418,1,418,3],[419,1,419,3],[420,1,420,3],[421,1,421,3],[422,1,422,3],[423,1,423,3],[424,1,424,3],[407,1,407,3],[408,1,408,3],[409,1,409,3],[410,1,410,3],[411,1,411,3],[412,1,412,3],[413,1,413,3],[414,1,414,3],[415,1,415,3],[398,1,398,3],[399,1,399,3],[400,1,400,3],[401,1,401,3],[402,1,402,3],[403,1,403,3],[404,1,404,3],[405,1,405,3],[406,1,406,3],[389,1,389,3],[390,1,390,3],[391,1,391,3],[392,1,392,3],[393,1,393,3],[394,1,394,3],[395,1,395,3],[396,1,396,3],[397,1,397,3],[380,1,380,3],[381,1,381,3],[382,1,382,3],[383,1,383,3],[384,1,384,3],[385,1,385,3],[386,1,386,3],[387,1,387,3],[388,1,388,3],[371,1,371,3],[372,1,372,3],[373,1,373,3],[374,1,374,3],[375,1,375,3],[376,1,376,3],[377,1,377,3],[378,1,378,3],[379,1,379,3],[362,1,362,3],[363,1,363,3],[364,1,364,3],[365,1,365,3],[366,1,366,3],[367,1,367,3],[368,1,368,3],[369,1,369,3],[370,1,370,3],[353,1,353,3],[354,1,354,3],[355,1,355,3],[356,1,356,3],[357,1,357,3],[358,1,358,3],[359,1,359,3],[360,1,360,3],[361,1,361,3],[344,1,344,3],[345,1,345,3],[346,1,346,3],[347,1,347,3],[348,1,348,3],[349,1,349,3],[350,1,350,3],[351,1,351,3],[352,1,352,3],[335,1,335,3],[336,1,336,3],[337,1,337,3],[338,1,338,3],[339,1,339,3],[340,1,340,3],[341,1,341,3],[342,1,342,3],[343,1,343,3],[326,1,326,3],[327,1,327,3],[328,1,328,3],[329,1,329,3],[330,1,330,3],[331,1,331,3],[332,1,332,3],[333,1,333,3],[334,1,334,3],[317,1,317,3],[318,1,318,3],[319,1,319,3],[320,1,320,3],[321,1,321,3],[322,1,322,3],[323,1,323,3],[324,1,324,3],[325,1,325,3],[195,1,195,3],[196,1,196,3],[197,1,197,3],[198,1,198,3],[312,1,312,3],[313,1,313,3],[314,1,314,3],[315,1,315,3],[316,1,316,3],[263,1,263,3],[258,1,258,3],[257,1,257,3],[254,1,254,3],[244,1,244,3],[245,1,245,3],[239,1,239,3],[242,1,242,3],[243,1,243,3],[304,1,304,3],[252,1,252,3],[260,1,260,3],[269,1,269,3],[261,1,261,3],[294,1,294,3],[186,1,186,3],[187,1,187,3],[188,1,188,3],[189,1,189,3],[190,1,190,3],[191,1,191,3],[192,1,192,3],[193,1,193,3],[194,1,194,3],[177,1,177,3],[178,1,178,3],[179,1,179,3],[180,1,180,3],[181,1,181,3],[182,1,182,3],[183,1,183,3],[184,1,184,3],[185,1,185,3],[168,1,168,3],[169,1,169,3],[170,1,170,3],[171,1,171,3],[172,1,172,3],[173,1,173,3],[174,1,174,3],[175,1,175,3],[176,1,176,3],[159,1,159,3],[160,1,160,3],[161,1,161,3],[162,1,162,3],[163,1,163,3],[164,1,164,3],[165,1,165,3],[166,1,166,3],[167,1,167,3],[150,1,150,3],[151,1,151,3],[152,1,152,3],[153,1,153,3],[154,1,154,3],[155,1,155,3],[156,1,156,3],[157,1,157,3],[158,1,158,3],[141,1,141,3],[142,1,142,3],[143,1,143,3],[144,1,144,3],[145,1,145,3],[146,1,146,3],[147,1,147,3],[148,1,148,3],[149,1,149,3],[132,1,132,3],[133,1,133,3],[134,1,134,3],[135,1,135,3],[136,1,136,3],[137,1,137,3],[138,1,138,3],[139,1,139,3],[140,1,140,3],[123,1,123,3],[124,1,124,3],[125,1,125,3],[126,1,126,3],[127,1,127,3],[128,1,128,3],[129,1,129,3],[130,1,130,3],[131,1,131,3],[114,1,114,3],[115,1,115,3],[116,1,116,3],[117,1,117,3],[118,1,118,3],[119,1,119,3],[120,1,120,3],[121,1,121,3],[122,1,122,3],[105,1,105,3],[106,1,106,3],[107,1,107,3],[108,1,108,3],[109,1,109,3],[110,1,110,3],[111,1,111,3],[112,1,112,3],[113,1,113,3],[96,1,96,3],[97,1,97,3],[98,1,98,3],[99,1,99,3],[100,1,100,3],[101,1,101,3],[102,1,102,3],[103,1,103,3],[104,1,104,3],[87,1,87,3],[88,1,88,3],[89,1,89,3],[90,1,90,3],[91,1,91,3],[92,1,92,3],[93,1,93,3],[94,1,94,3],[95,1,95,3],[78,1,78,3],[79,1,79,3],[80,1,80,3],[81,1,81,3],[82,1,82,3],[83,1,83,3],[84,1,84,3],[85,1,85,3],[86,1,86,3],[69,1,69,3],[70,1,70,3],[71,1,71,3],[72,1,72,3],[73,1,73,3],[74,1,74,3],[75,1,75,3],[76,1,76,3],[77,1,77,3],[60,1,60,3],[61,1,61,3],[62,1,62,3],[63,1,63,3],[64,1,64,3],[65,1,65,3],[66,1,66,3],[67,1,67,3],[68,1,68,3],[51,1,51,3],[52,1,52,3],[53,1,53,3],[54,1,54,3],[55,1,55,3],[56,1,56,3],[57,1,57,3],[58,1,58,3],[59,1,59,3],[42,1,42,3],[43,1,43,3],[44,1,44,3],[45,1,45,3],[46,1,46,3],[47,1,47,3],[48,1,48,3],[49,1,49,3],[50,1,50,3],[33,1,33,3],[34,1,34,3],[35,1,35,3],[36,1,36,3],[37,1,37,3],[38,1,38,3],[39,1,39,3],[40,1,40,3],[41,1,41,3],[24,1,24,3],[25,1,25,3],[26,1,26,3],[27,1,27,3],[28,1,28,3],[29,1,29,3],[30,1,30,3],[31,1,31,3],[32,1,32,3],[15,1,15,3],[16,1,16,3],[17,1,17,3],[18,1,18,3],[19,1,19,3],[20,1,20,3],[21,1,21,3],[22,1,22,3],[23,1,23,3],[299,1,299,3],[292,1,292,3],[293,1,293,3],[284,1,284,3],[287,1,287,3],[290,1,290,3],[266,1,266,3],[265,1,265,3],[255,1,255,3],[285,1,285,3],[286,1,286,3],[288,1,288,3],[281,1,281,3],[279,1,279,3],[282,1,282,3],[251,1,251,3],[247,1,247,3],[248,1,248,3],[249,1,249,3],[250,1,250,3],[236,1,236,3],[291,1,291,3],[253,1,253,3],[278,1,278,3],[274,1,274,3],[276,1,276,3],[275,1,275,3],[272,1,272,3],[277,1,277,3],[256,1,256,3],[259,1,259,3],[271,1,271,3],[216,1,216,3],[221,1,221,3],[224,1,224,3],[223,1,223,3],[219,1,219,3],[220,1,220,3],[226,1,226,3],[246,1,246,3],[238,1,238,3],[240,1,240,3],[211,1,211,3],[9,8,10,8],[9,4,10,4],[225,1,225,3],[230,1,230,3],[2,10,2,12],[227,1,227,3],[228,1,228,3],[229,1,229,3],[217,1,217,3],[4,5,4,6],[5,5,5,6],[4,1,4,3],[9,1,10,3],[199,1,199,3],[11,1,11,3],[201,1,201,3],[202,1,202,3],[200,1,200,3],[203,1,203,3],[6,10,6,12],[12,1,12,3],[13,1,13,3],[14,1,14,3],[0,1,0,12],[9,10,10,10],[9,12,10,12],[9,5,9,7],[6,5,6,6],[7,5,7,6],[6,8,7,8],[2,1,2,2],[2,5,2,8],[3,5,3,6],[9,9,10,9],[9,11,10,11],[493,1,493,3],[492,1,492,3],[491,1,491,3],[487,1,487,3],[489,1,489,3],[490,1,490,3],[205,1,205,3],[204,1,204,3],[206,1,206,3],[308,1,308,3],[311,1,311,3],[425,1,425,3],[426,1,426,3],[273,1,273,3],[262,1,262,3],[237,1,237,3],[241,1,241,3],[305,1,305,3],[309,1,309,3],[307,1,307,3],[306,1,306,3],[280,1,280,3],[464,1,464,3],[232,1,232,3],[499,1,499,3],[498,1,498,3],[497,1,497,3],[496,1,496,3],[486,1,486,3],[427,1,427,3],[428,1,428,3],[481,1,481,3],[495,1,495,3],[494,1,494,3],[479,1,479,3],[483,1,483,3],[480,1,480,3],[482,1,482,3],[488,1,488,3],[484,1,484,3],[485,1,485,3],[459,1,459,3],[430,1,430,3],[431,1,431,3],[434,1,434,3],[442,1,442,3],[440,1,440,3],[429,1,429,3],[435,1,435,3],[268,1,268,3],[213,1,213,3],[214,1,214,3],[449,1,449,3],[453,1,453,3],[439,1,439,3],[264,1,264,3],[233,1,233,3],[234,1,234,3],[231,1,231,3],[222,1,222,3],[301,1,301,3],[302,1,302,3],[295,1,295,3],[296,1,296,3],[297,1,297,3],[298,1,298,3],[300,1,300,3],[267,1,267,3],[289,1,289,3],[283,1,283,3],[215,1,215,3],[303,1,303,3],[478,1,478,3],[443,1,443,3],[474,1,474,3],[476,1,476,3],[451,1,451,3],[470,1,470,3],[472,1,472,3],[447,1,447,3],[448,1,448,3],[457,1,457,3],[477,1,477,3],[461,1,461,3],[462,1,462,3],[465,1,465,3],[473,1,473,3],[466,1,466,3],[467,1,467,3],[471,1,471,3],[468,1,468,3],[463,1,463,3],[446,1,446,3],[445,1,445,3],[444,1,444,3],[460,1,460,3],[454,1,454,3],[4,10,4,12],[469,1,469,3],[475,1,475,3],[270,1,270,3],[455,1,455,3],[456,1,456,3],[437,1,437,3],[441,1,441,3],[450,1,450,3],[438,1,438,3],[218,1,218,3],[436,1,436,3],[310,1,310,3],[235,1,235,3],[432,1,432,3],[433,1,433,3],[452,1,452,3],[207,1,207,3],[209,1,209,3],[208,1,208,3],[212,1,212,3],[210,1,210,3],[458,1,458,3]]}
[null,"Logic Power",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(TRUE,1,OFFSET(POWER_SCALE,3,OFFSET(POWER_SCALE,1,1))*PL_POWERED)","v":1}]
[]
[null,"Power",null,null,null,"Utilization",null,null,null,null,"CLB User Guide",null,null,null,null,null,"Logic","Signals"]
[null,"VCCINT",{"$f":"TEXT(VCCINT,\"0.000\")&\"V\"","v":"0.001V"},{"$f":"SUM(M12:M500)","v":13.462057892934997},null," Registers",null,{"$f":"SUM(I12:I500)","v":0},{"$f":"H4/NUM_FFS","v":0},null,null,null,null,null,null,null,{"$f":"SUM(Z12:Z500)","v":0},{"$f":"SUM(AD12:AD500)","v":0}]
[null,{"$f":"TEXT(LOGIC_POWER/TOTAL_POWER,\"0%\")&\" of total on-chip power \"&TEXT(TOTAL_POWER,\"0.000\")&\"W\"","v":"16% of total on-chip power 0.084W"},null,null,null," LUTs",null,{"$f":"SUM(H6:H8)","v":650000},{"$f":"H5/NUM_LUTS","v":0.60507893952934166},null,"XPE User Guide",null,null,null,null,null,{"$f":"SUM(Q6:Q8)","v":9.4873326999999996},{"$f":"SUM(R6:R8)","v":3.9747251929349967}]
[null,null,null,null,null,"      Combinatorial",null,{"$f":"SUM(F12:F500)","v":500000},{"$f":"H6/NUM_LUTS","v":0.46544533809949362},null,null,null,null,null,null,null,{"$f":"SUM(W12:W500)","v":6.3643758500000001},{"$f":"SUM(AA12:AA500)","v":2.9789263584952521}]
[null,null,null,null,null,"      Shift Registers",null,{"$f":"SUM(G12:G500)","v":100000},{"$f":"SUM(H7:H8)/NUM_LUTRAM","v":0.36938534278959811},null,"Introduction to XPE (video)",null,null,null,null,null,{"$f":"SUM(X12:X500)","v":1.9023039400000001},{"$f":"SUM(AB12:AB500)","v":0.67024740931435389}]
[null,null,null,null,null,"      Distributed RAMs",null,{"$f":"SUM(H12:H500)","v":50000},null,null,null,null,null,null,null,null,{"$f":"SUM(Y12:Y500)","v":1.2206529099999999},{"$f":"SUM(AC12:AC500)","v":0.32555142512539081}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(Q4:Q5)","v":9.4873326999999996},{"$f":"SUM(R4:R5)","v":3.9747251929349967}]
[null,"Name",null,null,"Clock (MHz)","LUTs as",null,null,"Registers","Toggle Rate","Routing Complexity","Signal Rate (Mtr/s)","Power (W)",null,{"$f":"SUM(O12:O500)","v":0},{"$f":"SUM(P12:P500)","v":0},null,null,null,null,"Routing",null,"LUTs as",null,null,"Registers","LUTs as",null,null,"Registers"]
[null,null,null,null,null,"Logic","Shift Registers","Distributed RAMs",null,null,null,null,null,null,"RP_power","RP_spower","RF",null,null,null,null,null,"Logic","Shift Registers","Distributed RAMs",null,"Logic","Shift Registers","Distributed RAMs",null,"Logic","Routing"]
[null,null,null,null,160,500000,100000,50000,0,0.5,8,{"$f":"E12*J12","v":80},{"$f":"IF(TRUE,SUM(AE12:AF12),(VCCINT/1000)*VCCINT_N*IF($R12>0,$R12,($L12/2*(($F12+$I12)*0.45*$U12+($F12*(OFFSET(FANOUT,8,2))+$G12*(OFFSET(FANOUT,8,4)+$U12)+$H12*(OFFSET(FANOUT,8,5)+$U12)+$I12*(OFFSET(FANOUT,8,3)))))*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1)","v":13.462057892934997},null,0,0,{"$f":"10^(K12/10)-1","v":5.3095734448019343},null,null,null,{"$f":"OFFSET(FANOUT,8,1)+OFFSET(FANOUT,9,1)*($K12-3)","v":8.1363158974999991E-4},null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T12>0,$T12,($L12/2*(($F12*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":6.3643758500000001},{"$f":"(VCCINT/1000)*VCCINT*(IF($T12>0,$T12,($L12/2*($G12*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":1.9023039400000001},{"$f":"(VCCINT/1000)*VCCINT*(IF($T12>0,$T12,($L12/2*($H12*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":1.2206529099999999},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T12 > 0, $T12, ( $L12 / 2 * ( ( $I12 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T12 > 0, $T12,($L12/2*(($F12)*(Q12*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":2.9789263584952521},{"$f":"(VCCINT/1000)*VCCINT*(IF($T12 > 0, $T12,($L12/2*($G12*(Q12*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0.67024740931435389},{"$f":"(VCCINT/1000)*VCCINT*(IF($T12 > 0, $T12,($L12/2*($H12*(Q12*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0.32555142512539081},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T12 > 0, $T12, ( $L12 / 2 * ( ( $I12 ) * (Q12*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"SUM(W12:Z12)","v":9.4873326999999996},{"$f":"SUM(AA12:AD12)","v":3.9747251929349967}]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,{"$f":"10^(K13/10)-1","v":5.3095734448019343},null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T13>0,$T13,($L13/2*(($F13*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T13>0,$T13,($L13/2*($G13*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T13>0,$T13,($L13/2*($H13*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T13 > 0, $T13, ( $L13 / 2 * ( ( $I13 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T13 > 0, $T13,($L13/2*(($F13)*(Q13*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T13 > 0, $T13,($L13/2*($G13*(Q13*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T13 > 0, $T13,($L13/2*($H13*(Q13*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T13 > 0, $T13, ( $L13 / 2 * ( ( $I13 ) * (Q13*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"SUM(W13:Z13)","v":0},{"$f":"SUM(AA13:AD13)","v":0}]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T14>0,$T14,($L14/2*(($F14*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T14>0,$T14,($L14/2*($G14*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T14>0,$T14,($L14/2*($H14*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T14 > 0, $T14, ( $L14 / 2 * ( ( $I14 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T14 > 0, $T14,($L14/2*(($F14)*(Q14*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T14 > 0, $T14,($L14/2*($G14*(Q14*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T14 > 0, $T14,($L14/2*($H14*(Q14*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T14 > 0, $T14, ( $L14 / 2 * ( ( $I14 ) * (Q14*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T15>0,$T15,($L15/2*(($F15*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T15>0,$T15,($L15/2*($G15*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T15>0,$T15,($L15/2*($H15*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T15 > 0, $T15, ( $L15 / 2 * ( ( $I15 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T15 > 0, $T15,($L15/2*(($F15)*(Q15*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T15 > 0, $T15,($L15/2*($G15*(Q15*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T15 > 0, $T15,($L15/2*($H15*(Q15*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T15 > 0, $T15, ( $L15 / 2 * ( ( $I15 ) * (Q15*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T16>0,$T16,($L16/2*(($F16*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T16>0,$T16,($L16/2*($G16*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T16>0,$T16,($L16/2*($H16*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T16 > 0, $T16, ( $L16 / 2 * ( ( $I16 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T16 > 0, $T16,($L16/2*(($F16)*(Q16*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T16 > 0, $T16,($L16/2*($G16*(Q16*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T16 > 0, $T16,($L16/2*($H16*(Q16*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T16 > 0, $T16, ( $L16 / 2 * ( ( $I16 ) * (Q16*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T17>0,$T17,($L17/2*(($F17*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T17>0,$T17,($L17/2*($G17*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T17>0,$T17,($L17/2*($H17*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T17 > 0, $T17, ( $L17 / 2 * ( ( $I17 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T17 > 0, $T17,($L17/2*(($F17)*(Q17*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T17 > 0, $T17,($L17/2*($G17*(Q17*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T17 > 0, $T17,($L17/2*($H17*(Q17*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T17 > 0, $T17, ( $L17 / 2 * ( ( $I17 ) * (Q17*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T18>0,$T18,($L18/2*(($F18*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T18>0,$T18,($L18/2*($G18*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T18>0,$T18,($L18/2*($H18*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T18 > 0, $T18, ( $L18 / 2 * ( ( $I18 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T18 > 0, $T18,($L18/2*(($F18)*(Q18*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T18 > 0, $T18,($L18/2*($G18*(Q18*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T18 > 0, $T18,($L18/2*($H18*(Q18*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T18 > 0, $T18, ( $L18 / 2 * ( ( $I18 ) * (Q18*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T19>0,$T19,($L19/2*(($F19*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T19>0,$T19,($L19/2*($G19*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T19>0,$T19,($L19/2*($H19*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T19 > 0, $T19, ( $L19 / 2 * ( ( $I19 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T19 > 0, $T19,($L19/2*(($F19)*(Q19*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T19 > 0, $T19,($L19/2*($G19*(Q19*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T19 > 0, $T19,($L19/2*($H19*(Q19*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T19 > 0, $T19, ( $L19 / 2 * ( ( $I19 ) * (Q19*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T20>0,$T20,($L20/2*(($F20*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T20>0,$T20,($L20/2*($G20*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T20>0,$T20,($L20/2*($H20*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T20 > 0, $T20, ( $L20 / 2 * ( ( $I20 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T20 > 0, $T20,($L20/2*(($F20)*(Q20*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T20 > 0, $T20,($L20/2*($G20*(Q20*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T20 > 0, $T20,($L20/2*($H20*(Q20*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T20 > 0, $T20, ( $L20 / 2 * ( ( $I20 ) * (Q20*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T21>0,$T21,($L21/2*(($F21*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T21>0,$T21,($L21/2*($G21*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T21>0,$T21,($L21/2*($H21*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T21 > 0, $T21, ( $L21 / 2 * ( ( $I21 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T21 > 0, $T21,($L21/2*(($F21)*(Q21*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T21 > 0, $T21,($L21/2*($G21*(Q21*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T21 > 0, $T21,($L21/2*($H21*(Q21*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T21 > 0, $T21, ( $L21 / 2 * ( ( $I21 ) * (Q21*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T22>0,$T22,($L22/2*(($F22*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T22>0,$T22,($L22/2*($G22*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T22>0,$T22,($L22/2*($H22*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T22 > 0, $T22, ( $L22 / 2 * ( ( $I22 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T22 > 0, $T22,($L22/2*(($F22)*(Q22*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T22 > 0, $T22,($L22/2*($G22*(Q22*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T22 > 0, $T22,($L22/2*($H22*(Q22*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T22 > 0, $T22, ( $L22 / 2 * ( ( $I22 ) * (Q22*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T23>0,$T23,($L23/2*(($F23*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T23>0,$T23,($L23/2*($G23*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T23>0,$T23,($L23/2*($H23*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T23 > 0, $T23, ( $L23 / 2 * ( ( $I23 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T23 > 0, $T23,($L23/2*(($F23)*(Q23*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T23 > 0, $T23,($L23/2*($G23*(Q23*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T23 > 0, $T23,($L23/2*($H23*(Q23*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T23 > 0, $T23, ( $L23 / 2 * ( ( $I23 ) * (Q23*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T24>0,$T24,($L24/2*(($F24*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T24>0,$T24,($L24/2*($G24*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T24>0,$T24,($L24/2*($H24*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T24 > 0, $T24, ( $L24 / 2 * ( ( $I24 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T24 > 0, $T24,($L24/2*(($F24)*(Q24*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T24 > 0, $T24,($L24/2*($G24*(Q24*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T24 > 0, $T24,($L24/2*($H24*(Q24*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T24 > 0, $T24, ( $L24 / 2 * ( ( $I24 ) * (Q24*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T25>0,$T25,($L25/2*(($F25*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T25>0,$T25,($L25/2*($G25*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T25>0,$T25,($L25/2*($H25*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T25 > 0, $T25, ( $L25 / 2 * ( ( $I25 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T25 > 0, $T25,($L25/2*(($F25)*(Q25*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T25 > 0, $T25,($L25/2*($G25*(Q25*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T25 > 0, $T25,($L25/2*($H25*(Q25*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T25 > 0, $T25, ( $L25 / 2 * ( ( $I25 ) * (Q25*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T26>0,$T26,($L26/2*(($F26*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T26>0,$T26,($L26/2*($G26*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T26>0,$T26,($L26/2*($H26*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T26 > 0, $T26, ( $L26 / 2 * ( ( $I26 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T26 > 0, $T26,($L26/2*(($F26)*(Q26*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T26 > 0, $T26,($L26/2*($G26*(Q26*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T26 > 0, $T26,($L26/2*($H26*(Q26*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T26 > 0, $T26, ( $L26 / 2 * ( ( $I26 ) * (Q26*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T27>0,$T27,($L27/2*(($F27*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T27>0,$T27,($L27/2*($G27*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T27>0,$T27,($L27/2*($H27*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T27 > 0, $T27, ( $L27 / 2 * ( ( $I27 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T27 > 0, $T27,($L27/2*(($F27)*(Q27*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T27 > 0, $T27,($L27/2*($G27*(Q27*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T27 > 0, $T27,($L27/2*($H27*(Q27*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T27 > 0, $T27, ( $L27 / 2 * ( ( $I27 ) * (Q27*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T28>0,$T28,($L28/2*(($F28*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T28>0,$T28,($L28/2*($G28*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T28>0,$T28,($L28/2*($H28*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T28 > 0, $T28, ( $L28 / 2 * ( ( $I28 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T28 > 0, $T28,($L28/2*(($F28)*(Q28*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T28 > 0, $T28,($L28/2*($G28*(Q28*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T28 > 0, $T28,($L28/2*($H28*(Q28*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T28 > 0, $T28, ( $L28 / 2 * ( ( $I28 ) * (Q28*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T29>0,$T29,($L29/2*(($F29*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T29>0,$T29,($L29/2*($G29*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T29>0,$T29,($L29/2*($H29*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T29 > 0, $T29, ( $L29 / 2 * ( ( $I29 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T29 > 0, $T29,($L29/2*(($F29)*(Q29*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T29 > 0, $T29,($L29/2*($G29*(Q29*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T29 > 0, $T29,($L29/2*($H29*(Q29*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T29 > 0, $T29, ( $L29 / 2 * ( ( $I29 ) * (Q29*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T30>0,$T30,($L30/2*(($F30*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T30>0,$T30,($L30/2*($G30*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T30>0,$T30,($L30/2*($H30*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T30 > 0, $T30, ( $L30 / 2 * ( ( $I30 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T30 > 0, $T30,($L30/2*(($F30)*(Q30*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T30 > 0, $T30,($L30/2*($G30*(Q30*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T30 > 0, $T30,($L30/2*($H30*(Q30*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T30 > 0, $T30, ( $L30 / 2 * ( ( $I30 ) * (Q30*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T31>0,$T31,($L31/2*(($F31*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T31>0,$T31,($L31/2*($G31*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T31>0,$T31,($L31/2*($H31*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T31 > 0, $T31, ( $L31 / 2 * ( ( $I31 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T31 > 0, $T31,($L31/2*(($F31)*(Q31*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T31 > 0, $T31,($L31/2*($G31*(Q31*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T31 > 0, $T31,($L31/2*($H31*(Q31*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T31 > 0, $T31, ( $L31 / 2 * ( ( $I31 ) * (Q31*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T32>0,$T32,($L32/2*(($F32*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T32>0,$T32,($L32/2*($G32*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T32>0,$T32,($L32/2*($H32*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T32 > 0, $T32, ( $L32 / 2 * ( ( $I32 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T32 > 0, $T32,($L32/2*(($F32)*(Q32*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T32 > 0, $T32,($L32/2*($G32*(Q32*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T32 > 0, $T32,($L32/2*($H32*(Q32*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T32 > 0, $T32, ( $L32 / 2 * ( ( $I32 ) * (Q32*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T33>0,$T33,($L33/2*(($F33*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T33>0,$T33,($L33/2*($G33*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T33>0,$T33,($L33/2*($H33*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T33 > 0, $T33, ( $L33 / 2 * ( ( $I33 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T33 > 0, $T33,($L33/2*(($F33)*(Q33*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T33 > 0, $T33,($L33/2*($G33*(Q33*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T33 > 0, $T33,($L33/2*($H33*(Q33*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T33 > 0, $T33, ( $L33 / 2 * ( ( $I33 ) * (Q33*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T34>0,$T34,($L34/2*(($F34*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T34>0,$T34,($L34/2*($G34*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T34>0,$T34,($L34/2*($H34*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T34 > 0, $T34, ( $L34 / 2 * ( ( $I34 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T34 > 0, $T34,($L34/2*(($F34)*(Q34*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T34 > 0, $T34,($L34/2*($G34*(Q34*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T34 > 0, $T34,($L34/2*($H34*(Q34*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T34 > 0, $T34, ( $L34 / 2 * ( ( $I34 ) * (Q34*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T35>0,$T35,($L35/2*(($F35*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T35>0,$T35,($L35/2*($G35*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T35>0,$T35,($L35/2*($H35*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T35 > 0, $T35, ( $L35 / 2 * ( ( $I35 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T35 > 0, $T35,($L35/2*(($F35)*(Q35*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T35 > 0, $T35,($L35/2*($G35*(Q35*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T35 > 0, $T35,($L35/2*($H35*(Q35*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T35 > 0, $T35, ( $L35 / 2 * ( ( $I35 ) * (Q35*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T36>0,$T36,($L36/2*(($F36*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T36>0,$T36,($L36/2*($G36*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T36>0,$T36,($L36/2*($H36*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T36 > 0, $T36, ( $L36 / 2 * ( ( $I36 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T36 > 0, $T36,($L36/2*(($F36)*(Q36*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T36 > 0, $T36,($L36/2*($G36*(Q36*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T36 > 0, $T36,($L36/2*($H36*(Q36*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T36 > 0, $T36, ( $L36 / 2 * ( ( $I36 ) * (Q36*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T37>0,$T37,($L37/2*(($F37*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T37>0,$T37,($L37/2*($G37*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T37>0,$T37,($L37/2*($H37*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T37 > 0, $T37, ( $L37 / 2 * ( ( $I37 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T37 > 0, $T37,($L37/2*(($F37)*(Q37*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T37 > 0, $T37,($L37/2*($G37*(Q37*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T37 > 0, $T37,($L37/2*($H37*(Q37*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T37 > 0, $T37, ( $L37 / 2 * ( ( $I37 ) * (Q37*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T38>0,$T38,($L38/2*(($F38*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T38>0,$T38,($L38/2*($G38*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T38>0,$T38,($L38/2*($H38*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T38 > 0, $T38, ( $L38 / 2 * ( ( $I38 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T38 > 0, $T38,($L38/2*(($F38)*(Q38*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T38 > 0, $T38,($L38/2*($G38*(Q38*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T38 > 0, $T38,($L38/2*($H38*(Q38*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T38 > 0, $T38, ( $L38 / 2 * ( ( $I38 ) * (Q38*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T39>0,$T39,($L39/2*(($F39*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T39>0,$T39,($L39/2*($G39*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T39>0,$T39,($L39/2*($H39*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T39 > 0, $T39, ( $L39 / 2 * ( ( $I39 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T39 > 0, $T39,($L39/2*(($F39)*(Q39*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T39 > 0, $T39,($L39/2*($G39*(Q39*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T39 > 0, $T39,($L39/2*($H39*(Q39*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T39 > 0, $T39, ( $L39 / 2 * ( ( $I39 ) * (Q39*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T40>0,$T40,($L40/2*(($F40*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T40>0,$T40,($L40/2*($G40*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T40>0,$T40,($L40/2*($H40*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T40 > 0, $T40, ( $L40 / 2 * ( ( $I40 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T40 > 0, $T40,($L40/2*(($F40)*(Q40*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T40 > 0, $T40,($L40/2*($G40*(Q40*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T40 > 0, $T40,($L40/2*($H40*(Q40*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T40 > 0, $T40, ( $L40 / 2 * ( ( $I40 ) * (Q40*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T41>0,$T41,($L41/2*(($F41*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T41>0,$T41,($L41/2*($G41*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T41>0,$T41,($L41/2*($H41*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T41 > 0, $T41, ( $L41 / 2 * ( ( $I41 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T41 > 0, $T41,($L41/2*(($F41)*(Q41*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T41 > 0, $T41,($L41/2*($G41*(Q41*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T41 > 0, $T41,($L41/2*($H41*(Q41*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T41 > 0, $T41, ( $L41 / 2 * ( ( $I41 ) * (Q41*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T42>0,$T42,($L42/2*(($F42*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T42>0,$T42,($L42/2*($G42*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T42>0,$T42,($L42/2*($H42*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T42 > 0, $T42, ( $L42 / 2 * ( ( $I42 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T42 > 0, $T42,($L42/2*(($F42)*(Q42*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T42 > 0, $T42,($L42/2*($G42*(Q42*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T42 > 0, $T42,($L42/2*($H42*(Q42*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T42 > 0, $T42, ( $L42 / 2 * ( ( $I42 ) * (Q42*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T43>0,$T43,($L43/2*(($F43*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T43>0,$T43,($L43/2*($G43*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T43>0,$T43,($L43/2*($H43*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T43 > 0, $T43, ( $L43 / 2 * ( ( $I43 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T43 > 0, $T43,($L43/2*(($F43)*(Q43*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T43 > 0, $T43,($L43/2*($G43*(Q43*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T43 > 0, $T43,($L43/2*($H43*(Q43*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T43 > 0, $T43, ( $L43 / 2 * ( ( $I43 ) * (Q43*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T44>0,$T44,($L44/2*(($F44*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T44>0,$T44,($L44/2*($G44*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T44>0,$T44,($L44/2*($H44*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T44 > 0, $T44, ( $L44 / 2 * ( ( $I44 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T44 > 0, $T44,($L44/2*(($F44)*(Q44*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T44 > 0, $T44,($L44/2*($G44*(Q44*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T44 > 0, $T44,($L44/2*($H44*(Q44*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T44 > 0, $T44, ( $L44 / 2 * ( ( $I44 ) * (Q44*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T45>0,$T45,($L45/2*(($F45*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T45>0,$T45,($L45/2*($G45*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T45>0,$T45,($L45/2*($H45*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T45 > 0, $T45, ( $L45 / 2 * ( ( $I45 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T45 > 0, $T45,($L45/2*(($F45)*(Q45*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T45 > 0, $T45,($L45/2*($G45*(Q45*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T45 > 0, $T45,($L45/2*($H45*(Q45*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T45 > 0, $T45, ( $L45 / 2 * ( ( $I45 ) * (Q45*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T46>0,$T46,($L46/2*(($F46*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T46>0,$T46,($L46/2*($G46*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T46>0,$T46,($L46/2*($H46*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T46 > 0, $T46, ( $L46 / 2 * ( ( $I46 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T46 > 0, $T46,($L46/2*(($F46)*(Q46*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T46 > 0, $T46,($L46/2*($G46*(Q46*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T46 > 0, $T46,($L46/2*($H46*(Q46*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T46 > 0, $T46, ( $L46 / 2 * ( ( $I46 ) * (Q46*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T47>0,$T47,($L47/2*(($F47*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T47>0,$T47,($L47/2*($G47*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T47>0,$T47,($L47/2*($H47*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T47 > 0, $T47, ( $L47 / 2 * ( ( $I47 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T47 > 0, $T47,($L47/2*(($F47)*(Q47*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T47 > 0, $T47,($L47/2*($G47*(Q47*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T47 > 0, $T47,($L47/2*($H47*(Q47*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T47 > 0, $T47, ( $L47 / 2 * ( ( $I47 ) * (Q47*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T48>0,$T48,($L48/2*(($F48*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T48>0,$T48,($L48/2*($G48*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T48>0,$T48,($L48/2*($H48*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T48 > 0, $T48, ( $L48 / 2 * ( ( $I48 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T48 > 0, $T48,($L48/2*(($F48)*(Q48*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T48 > 0, $T48,($L48/2*($G48*(Q48*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T48 > 0, $T48,($L48/2*($H48*(Q48*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T48 > 0, $T48, ( $L48 / 2 * ( ( $I48 ) * (Q48*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T49>0,$T49,($L49/2*(($F49*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T49>0,$T49,($L49/2*($G49*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T49>0,$T49,($L49/2*($H49*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T49 > 0, $T49, ( $L49 / 2 * ( ( $I49 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T49 > 0, $T49,($L49/2*(($F49)*(Q49*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T49 > 0, $T49,($L49/2*($G49*(Q49*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T49 > 0, $T49,($L49/2*($H49*(Q49*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T49 > 0, $T49, ( $L49 / 2 * ( ( $I49 ) * (Q49*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T50>0,$T50,($L50/2*(($F50*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T50>0,$T50,($L50/2*($G50*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T50>0,$T50,($L50/2*($H50*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T50 > 0, $T50, ( $L50 / 2 * ( ( $I50 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T50 > 0, $T50,($L50/2*(($F50)*(Q50*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T50 > 0, $T50,($L50/2*($G50*(Q50*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T50 > 0, $T50,($L50/2*($H50*(Q50*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T50 > 0, $T50, ( $L50 / 2 * ( ( $I50 ) * (Q50*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T51>0,$T51,($L51/2*(($F51*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T51>0,$T51,($L51/2*($G51*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T51>0,$T51,($L51/2*($H51*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T51 > 0, $T51, ( $L51 / 2 * ( ( $I51 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T51 > 0, $T51,($L51/2*(($F51)*(Q51*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T51 > 0, $T51,($L51/2*($G51*(Q51*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T51 > 0, $T51,($L51/2*($H51*(Q51*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T51 > 0, $T51, ( $L51 / 2 * ( ( $I51 ) * (Q51*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T52>0,$T52,($L52/2*(($F52*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T52>0,$T52,($L52/2*($G52*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T52>0,$T52,($L52/2*($H52*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T52 > 0, $T52, ( $L52 / 2 * ( ( $I52 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T52 > 0, $T52,($L52/2*(($F52)*(Q52*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T52 > 0, $T52,($L52/2*($G52*(Q52*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T52 > 0, $T52,($L52/2*($H52*(Q52*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T52 > 0, $T52, ( $L52 / 2 * ( ( $I52 ) * (Q52*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T53>0,$T53,($L53/2*(($F53*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T53>0,$T53,($L53/2*($G53*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T53>0,$T53,($L53/2*($H53*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T53 > 0, $T53, ( $L53 / 2 * ( ( $I53 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T53 > 0, $T53,($L53/2*(($F53)*(Q53*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T53 > 0, $T53,($L53/2*($G53*(Q53*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T53 > 0, $T53,($L53/2*($H53*(Q53*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T53 > 0, $T53, ( $L53 / 2 * ( ( $I53 ) * (Q53*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T54>0,$T54,($L54/2*(($F54*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T54>0,$T54,($L54/2*($G54*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T54>0,$T54,($L54/2*($H54*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T54 > 0, $T54, ( $L54 / 2 * ( ( $I54 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T54 > 0, $T54,($L54/2*(($F54)*(Q54*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T54 > 0, $T54,($L54/2*($G54*(Q54*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T54 > 0, $T54,($L54/2*($H54*(Q54*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T54 > 0, $T54, ( $L54 / 2 * ( ( $I54 ) * (Q54*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T55>0,$T55,($L55/2*(($F55*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T55>0,$T55,($L55/2*($G55*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T55>0,$T55,($L55/2*($H55*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T55 > 0, $T55, ( $L55 / 2 * ( ( $I55 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T55 > 0, $T55,($L55/2*(($F55)*(Q55*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T55 > 0, $T55,($L55/2*($G55*(Q55*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T55 > 0, $T55,($L55/2*($H55*(Q55*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T55 > 0, $T55, ( $L55 / 2 * ( ( $I55 ) * (Q55*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T56>0,$T56,($L56/2*(($F56*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T56>0,$T56,($L56/2*($G56*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T56>0,$T56,($L56/2*($H56*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T56 > 0, $T56, ( $L56 / 2 * ( ( $I56 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T56 > 0, $T56,($L56/2*(($F56)*(Q56*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T56 > 0, $T56,($L56/2*($G56*(Q56*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T56 > 0, $T56,($L56/2*($H56*(Q56*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T56 > 0, $T56, ( $L56 / 2 * ( ( $I56 ) * (Q56*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T57>0,$T57,($L57/2*(($F57*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T57>0,$T57,($L57/2*($G57*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T57>0,$T57,($L57/2*($H57*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T57 > 0, $T57, ( $L57 / 2 * ( ( $I57 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T57 > 0, $T57,($L57/2*(($F57)*(Q57*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T57 > 0, $T57,($L57/2*($G57*(Q57*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T57 > 0, $T57,($L57/2*($H57*(Q57*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T57 > 0, $T57, ( $L57 / 2 * ( ( $I57 ) * (Q57*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T58>0,$T58,($L58/2*(($F58*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T58>0,$T58,($L58/2*($G58*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T58>0,$T58,($L58/2*($H58*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T58 > 0, $T58, ( $L58 / 2 * ( ( $I58 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T58 > 0, $T58,($L58/2*(($F58)*(Q58*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T58 > 0, $T58,($L58/2*($G58*(Q58*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T58 > 0, $T58,($L58/2*($H58*(Q58*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T58 > 0, $T58, ( $L58 / 2 * ( ( $I58 ) * (Q58*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T59>0,$T59,($L59/2*(($F59*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T59>0,$T59,($L59/2*($G59*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T59>0,$T59,($L59/2*($H59*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T59 > 0, $T59, ( $L59 / 2 * ( ( $I59 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T59 > 0, $T59,($L59/2*(($F59)*(Q59*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T59 > 0, $T59,($L59/2*($G59*(Q59*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T59 > 0, $T59,($L59/2*($H59*(Q59*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T59 > 0, $T59, ( $L59 / 2 * ( ( $I59 ) * (Q59*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T60>0,$T60,($L60/2*(($F60*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T60>0,$T60,($L60/2*($G60*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T60>0,$T60,($L60/2*($H60*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T60 > 0, $T60, ( $L60 / 2 * ( ( $I60 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T60 > 0, $T60,($L60/2*(($F60)*(Q60*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T60 > 0, $T60,($L60/2*($G60*(Q60*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T60 > 0, $T60,($L60/2*($H60*(Q60*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T60 > 0, $T60, ( $L60 / 2 * ( ( $I60 ) * (Q60*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T61>0,$T61,($L61/2*(($F61*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T61>0,$T61,($L61/2*($G61*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T61>0,$T61,($L61/2*($H61*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T61 > 0, $T61, ( $L61 / 2 * ( ( $I61 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T61 > 0, $T61,($L61/2*(($F61)*(Q61*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T61 > 0, $T61,($L61/2*($G61*(Q61*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T61 > 0, $T61,($L61/2*($H61*(Q61*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T61 > 0, $T61, ( $L61 / 2 * ( ( $I61 ) * (Q61*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T62>0,$T62,($L62/2*(($F62*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T62>0,$T62,($L62/2*($G62*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T62>0,$T62,($L62/2*($H62*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T62 > 0, $T62, ( $L62 / 2 * ( ( $I62 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T62 > 0, $T62,($L62/2*(($F62)*(Q62*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T62 > 0, $T62,($L62/2*($G62*(Q62*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T62 > 0, $T62,($L62/2*($H62*(Q62*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T62 > 0, $T62, ( $L62 / 2 * ( ( $I62 ) * (Q62*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T63>0,$T63,($L63/2*(($F63*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T63>0,$T63,($L63/2*($G63*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T63>0,$T63,($L63/2*($H63*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T63 > 0, $T63, ( $L63 / 2 * ( ( $I63 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T63 > 0, $T63,($L63/2*(($F63)*(Q63*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T63 > 0, $T63,($L63/2*($G63*(Q63*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T63 > 0, $T63,($L63/2*($H63*(Q63*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T63 > 0, $T63, ( $L63 / 2 * ( ( $I63 ) * (Q63*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T64>0,$T64,($L64/2*(($F64*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T64>0,$T64,($L64/2*($G64*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T64>0,$T64,($L64/2*($H64*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T64 > 0, $T64, ( $L64 / 2 * ( ( $I64 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T64 > 0, $T64,($L64/2*(($F64)*(Q64*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T64 > 0, $T64,($L64/2*($G64*(Q64*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T64 > 0, $T64,($L64/2*($H64*(Q64*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T64 > 0, $T64, ( $L64 / 2 * ( ( $I64 ) * (Q64*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T65>0,$T65,($L65/2*(($F65*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T65>0,$T65,($L65/2*($G65*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T65>0,$T65,($L65/2*($H65*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T65 > 0, $T65, ( $L65 / 2 * ( ( $I65 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T65 > 0, $T65,($L65/2*(($F65)*(Q65*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T65 > 0, $T65,($L65/2*($G65*(Q65*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T65 > 0, $T65,($L65/2*($H65*(Q65*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T65 > 0, $T65, ( $L65 / 2 * ( ( $I65 ) * (Q65*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T66>0,$T66,($L66/2*(($F66*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T66>0,$T66,($L66/2*($G66*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T66>0,$T66,($L66/2*($H66*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T66 > 0, $T66, ( $L66 / 2 * ( ( $I66 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T66 > 0, $T66,($L66/2*(($F66)*(Q66*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T66 > 0, $T66,($L66/2*($G66*(Q66*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T66 > 0, $T66,($L66/2*($H66*(Q66*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T66 > 0, $T66, ( $L66 / 2 * ( ( $I66 ) * (Q66*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T67>0,$T67,($L67/2*(($F67*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T67>0,$T67,($L67/2*($G67*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T67>0,$T67,($L67/2*($H67*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T67 > 0, $T67, ( $L67 / 2 * ( ( $I67 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T67 > 0, $T67,($L67/2*(($F67)*(Q67*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T67 > 0, $T67,($L67/2*($G67*(Q67*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T67 > 0, $T67,($L67/2*($H67*(Q67*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T67 > 0, $T67, ( $L67 / 2 * ( ( $I67 ) * (Q67*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T68>0,$T68,($L68/2*(($F68*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T68>0,$T68,($L68/2*($G68*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T68>0,$T68,($L68/2*($H68*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T68 > 0, $T68, ( $L68 / 2 * ( ( $I68 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T68 > 0, $T68,($L68/2*(($F68)*(Q68*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T68 > 0, $T68,($L68/2*($G68*(Q68*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T68 > 0, $T68,($L68/2*($H68*(Q68*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T68 > 0, $T68, ( $L68 / 2 * ( ( $I68 ) * (Q68*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T69>0,$T69,($L69/2*(($F69*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T69>0,$T69,($L69/2*($G69*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T69>0,$T69,($L69/2*($H69*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T69 > 0, $T69, ( $L69 / 2 * ( ( $I69 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T69 > 0, $T69,($L69/2*(($F69)*(Q69*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T69 > 0, $T69,($L69/2*($G69*(Q69*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T69 > 0, $T69,($L69/2*($H69*(Q69*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T69 > 0, $T69, ( $L69 / 2 * ( ( $I69 ) * (Q69*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T70>0,$T70,($L70/2*(($F70*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T70>0,$T70,($L70/2*($G70*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T70>0,$T70,($L70/2*($H70*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T70 > 0, $T70, ( $L70 / 2 * ( ( $I70 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T70 > 0, $T70,($L70/2*(($F70)*(Q70*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T70 > 0, $T70,($L70/2*($G70*(Q70*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T70 > 0, $T70,($L70/2*($H70*(Q70*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T70 > 0, $T70, ( $L70 / 2 * ( ( $I70 ) * (Q70*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T71>0,$T71,($L71/2*(($F71*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T71>0,$T71,($L71/2*($G71*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T71>0,$T71,($L71/2*($H71*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T71 > 0, $T71, ( $L71 / 2 * ( ( $I71 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T71 > 0, $T71,($L71/2*(($F71)*(Q71*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T71 > 0, $T71,($L71/2*($G71*(Q71*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T71 > 0, $T71,($L71/2*($H71*(Q71*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T71 > 0, $T71, ( $L71 / 2 * ( ( $I71 ) * (Q71*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T72>0,$T72,($L72/2*(($F72*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T72>0,$T72,($L72/2*($G72*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T72>0,$T72,($L72/2*($H72*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T72 > 0, $T72, ( $L72 / 2 * ( ( $I72 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T72 > 0, $T72,($L72/2*(($F72)*(Q72*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T72 > 0, $T72,($L72/2*($G72*(Q72*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T72 > 0, $T72,($L72/2*($H72*(Q72*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T72 > 0, $T72, ( $L72 / 2 * ( ( $I72 ) * (Q72*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T73>0,$T73,($L73/2*(($F73*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T73>0,$T73,($L73/2*($G73*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T73>0,$T73,($L73/2*($H73*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T73 > 0, $T73, ( $L73 / 2 * ( ( $I73 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T73 > 0, $T73,($L73/2*(($F73)*(Q73*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T73 > 0, $T73,($L73/2*($G73*(Q73*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T73 > 0, $T73,($L73/2*($H73*(Q73*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T73 > 0, $T73, ( $L73 / 2 * ( ( $I73 ) * (Q73*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T74>0,$T74,($L74/2*(($F74*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T74>0,$T74,($L74/2*($G74*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T74>0,$T74,($L74/2*($H74*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T74 > 0, $T74, ( $L74 / 2 * ( ( $I74 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T74 > 0, $T74,($L74/2*(($F74)*(Q74*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T74 > 0, $T74,($L74/2*($G74*(Q74*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T74 > 0, $T74,($L74/2*($H74*(Q74*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T74 > 0, $T74, ( $L74 / 2 * ( ( $I74 ) * (Q74*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T75>0,$T75,($L75/2*(($F75*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T75>0,$T75,($L75/2*($G75*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T75>0,$T75,($L75/2*($H75*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T75 > 0, $T75, ( $L75 / 2 * ( ( $I75 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T75 > 0, $T75,($L75/2*(($F75)*(Q75*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T75 > 0, $T75,($L75/2*($G75*(Q75*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T75 > 0, $T75,($L75/2*($H75*(Q75*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T75 > 0, $T75, ( $L75 / 2 * ( ( $I75 ) * (Q75*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,{"$f":"E76*J76","v":0},{"$f":"IF(TRUE,SUM(AE76:AF76),(VCCINT/1000)*VCCINT_N*IF($R76>0,$R76,($L76/2*(($F76+$I76)*0.45*$U76+($F76*(OFFSET(FANOUT,8,2))+$G76*(OFFSET(FANOUT,8,4)+$U76)+$H76*(OFFSET(FANOUT,8,5)+$U76)+$I76*(OFFSET(FANOUT,8,3)))))*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1)","v":0},null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T76>0,$T76,($L76/2*(($F76*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T76>0,$T76,($L76/2*($G76*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T76>0,$T76,($L76/2*($H76*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T76 > 0, $T76, ( $L76 / 2 * ( ( $I76 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T76 > 0, $T76,($L76/2*(($F76)*(Q76*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T76 > 0, $T76,($L76/2*($G76*(Q76*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T76 > 0, $T76,($L76/2*($H76*(Q76*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T76 > 0, $T76, ( $L76 / 2 * ( ( $I76 ) * (Q76*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,{"$f":"10^(K77/10)-1","v":5.3095734448019343},null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T77>0,$T77,($L77/2*(($F77*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T77>0,$T77,($L77/2*($G77*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T77>0,$T77,($L77/2*($H77*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T77 > 0, $T77, ( $L77 / 2 * ( ( $I77 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T77 > 0, $T77,($L77/2*(($F77)*(Q77*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T77 > 0, $T77,($L77/2*($G77*(Q77*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T77 > 0, $T77,($L77/2*($H77*(Q77*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T77 > 0, $T77, ( $L77 / 2 * ( ( $I77 ) * (Q77*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"SUM(W77:Z77)","v":0},{"$f":"SUM(AA77:AD77)","v":0}]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T78>0,$T78,($L78/2*(($F78*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T78>0,$T78,($L78/2*($G78*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T78>0,$T78,($L78/2*($H78*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T78 > 0, $T78, ( $L78 / 2 * ( ( $I78 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T78 > 0, $T78,($L78/2*(($F78)*(Q78*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T78 > 0, $T78,($L78/2*($G78*(Q78*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T78 > 0, $T78,($L78/2*($H78*(Q78*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T78 > 0, $T78, ( $L78 / 2 * ( ( $I78 ) * (Q78*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T79>0,$T79,($L79/2*(($F79*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T79>0,$T79,($L79/2*($G79*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T79>0,$T79,($L79/2*($H79*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T79 > 0, $T79, ( $L79 / 2 * ( ( $I79 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T79 > 0, $T79,($L79/2*(($F79)*(Q79*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T79 > 0, $T79,($L79/2*($G79*(Q79*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T79 > 0, $T79,($L79/2*($H79*(Q79*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T79 > 0, $T79, ( $L79 / 2 * ( ( $I79 ) * (Q79*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T80>0,$T80,($L80/2*(($F80*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T80>0,$T80,($L80/2*($G80*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T80>0,$T80,($L80/2*($H80*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T80 > 0, $T80, ( $L80 / 2 * ( ( $I80 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T80 > 0, $T80,($L80/2*(($F80)*(Q80*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T80 > 0, $T80,($L80/2*($G80*(Q80*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T80 > 0, $T80,($L80/2*($H80*(Q80*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T80 > 0, $T80, ( $L80 / 2 * ( ( $I80 ) * (Q80*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T81>0,$T81,($L81/2*(($F81*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T81>0,$T81,($L81/2*($G81*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T81>0,$T81,($L81/2*($H81*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T81 > 0, $T81, ( $L81 / 2 * ( ( $I81 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T81 > 0, $T81,($L81/2*(($F81)*(Q81*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T81 > 0, $T81,($L81/2*($G81*(Q81*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T81 > 0, $T81,($L81/2*($H81*(Q81*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T81 > 0, $T81, ( $L81 / 2 * ( ( $I81 ) * (Q81*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T82>0,$T82,($L82/2*(($F82*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T82>0,$T82,($L82/2*($G82*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T82>0,$T82,($L82/2*($H82*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T82 > 0, $T82, ( $L82 / 2 * ( ( $I82 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T82 > 0, $T82,($L82/2*(($F82)*(Q82*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T82 > 0, $T82,($L82/2*($G82*(Q82*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T82 > 0, $T82,($L82/2*($H82*(Q82*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T82 > 0, $T82, ( $L82 / 2 * ( ( $I82 ) * (Q82*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T83>0,$T83,($L83/2*(($F83*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T83>0,$T83,($L83/2*($G83*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T83>0,$T83,($L83/2*($H83*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T83 > 0, $T83, ( $L83 / 2 * ( ( $I83 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T83 > 0, $T83,($L83/2*(($F83)*(Q83*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T83 > 0, $T83,($L83/2*($G83*(Q83*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T83 > 0, $T83,($L83/2*($H83*(Q83*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T83 > 0, $T83, ( $L83 / 2 * ( ( $I83 ) * (Q83*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T84>0,$T84,($L84/2*(($F84*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T84>0,$T84,($L84/2*($G84*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T84>0,$T84,($L84/2*($H84*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T84 > 0, $T84, ( $L84 / 2 * ( ( $I84 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T84 > 0, $T84,($L84/2*(($F84)*(Q84*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T84 > 0, $T84,($L84/2*($G84*(Q84*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T84 > 0, $T84,($L84/2*($H84*(Q84*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T84 > 0, $T84, ( $L84 / 2 * ( ( $I84 ) * (Q84*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T85>0,$T85,($L85/2*(($F85*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T85>0,$T85,($L85/2*($G85*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T85>0,$T85,($L85/2*($H85*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T85 > 0, $T85, ( $L85 / 2 * ( ( $I85 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T85 > 0, $T85,($L85/2*(($F85)*(Q85*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T85 > 0, $T85,($L85/2*($G85*(Q85*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T85 > 0, $T85,($L85/2*($H85*(Q85*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T85 > 0, $T85, ( $L85 / 2 * ( ( $I85 ) * (Q85*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T86>0,$T86,($L86/2*(($F86*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T86>0,$T86,($L86/2*($G86*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T86>0,$T86,($L86/2*($H86*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T86 > 0, $T86, ( $L86 / 2 * ( ( $I86 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T86 > 0, $T86,($L86/2*(($F86)*(Q86*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T86 > 0, $T86,($L86/2*($G86*(Q86*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T86 > 0, $T86,($L86/2*($H86*(Q86*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T86 > 0, $T86, ( $L86 / 2 * ( ( $I86 ) * (Q86*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T87>0,$T87,($L87/2*(($F87*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T87>0,$T87,($L87/2*($G87*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T87>0,$T87,($L87/2*($H87*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T87 > 0, $T87, ( $L87 / 2 * ( ( $I87 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T87 > 0, $T87,($L87/2*(($F87)*(Q87*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T87 > 0, $T87,($L87/2*($G87*(Q87*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T87 > 0, $T87,($L87/2*($H87*(Q87*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T87 > 0, $T87, ( $L87 / 2 * ( ( $I87 ) * (Q87*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T88>0,$T88,($L88/2*(($F88*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T88>0,$T88,($L88/2*($G88*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T88>0,$T88,($L88/2*($H88*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T88 > 0, $T88, ( $L88 / 2 * ( ( $I88 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T88 > 0, $T88,($L88/2*(($F88)*(Q88*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T88 > 0, $T88,($L88/2*($G88*(Q88*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T88 > 0, $T88,($L88/2*($H88*(Q88*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T88 > 0, $T88, ( $L88 / 2 * ( ( $I88 ) * (Q88*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T89>0,$T89,($L89/2*(($F89*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T89>0,$T89,($L89/2*($G89*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T89>0,$T89,($L89/2*($H89*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T89 > 0, $T89, ( $L89 / 2 * ( ( $I89 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T89 > 0, $T89,($L89/2*(($F89)*(Q89*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T89 > 0, $T89,($L89/2*($G89*(Q89*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T89 > 0, $T89,($L89/2*($H89*(Q89*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T89 > 0, $T89, ( $L89 / 2 * ( ( $I89 ) * (Q89*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T90>0,$T90,($L90/2*(($F90*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T90>0,$T90,($L90/2*($G90*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T90>0,$T90,($L90/2*($H90*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T90 > 0, $T90, ( $L90 / 2 * ( ( $I90 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T90 > 0, $T90,($L90/2*(($F90)*(Q90*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T90 > 0, $T90,($L90/2*($G90*(Q90*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T90 > 0, $T90,($L90/2*($H90*(Q90*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T90 > 0, $T90, ( $L90 / 2 * ( ( $I90 ) * (Q90*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T91>0,$T91,($L91/2*(($F91*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T91>0,$T91,($L91/2*($G91*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T91>0,$T91,($L91/2*($H91*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T91 > 0, $T91, ( $L91 / 2 * ( ( $I91 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T91 > 0, $T91,($L91/2*(($F91)*(Q91*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T91 > 0, $T91,($L91/2*($G91*(Q91*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T91 > 0, $T91,($L91/2*($H91*(Q91*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T91 > 0, $T91, ( $L91 / 2 * ( ( $I91 ) * (Q91*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T92>0,$T92,($L92/2*(($F92*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T92>0,$T92,($L92/2*($G92*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T92>0,$T92,($L92/2*($H92*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T92 > 0, $T92, ( $L92 / 2 * ( ( $I92 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T92 > 0, $T92,($L92/2*(($F92)*(Q92*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T92 > 0, $T92,($L92/2*($G92*(Q92*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T92 > 0, $T92,($L92/2*($H92*(Q92*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T92 > 0, $T92, ( $L92 / 2 * ( ( $I92 ) * (Q92*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T93>0,$T93,($L93/2*(($F93*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T93>0,$T93,($L93/2*($G93*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T93>0,$T93,($L93/2*($H93*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T93 > 0, $T93, ( $L93 / 2 * ( ( $I93 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T93 > 0, $T93,($L93/2*(($F93)*(Q93*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T93 > 0, $T93,($L93/2*($G93*(Q93*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T93 > 0, $T93,($L93/2*($H93*(Q93*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T93 > 0, $T93, ( $L93 / 2 * ( ( $I93 ) * (Q93*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T94>0,$T94,($L94/2*(($F94*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T94>0,$T94,($L94/2*($G94*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T94>0,$T94,($L94/2*($H94*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T94 > 0, $T94, ( $L94 / 2 * ( ( $I94 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T94 > 0, $T94,($L94/2*(($F94)*(Q94*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T94 > 0, $T94,($L94/2*($G94*(Q94*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T94 > 0, $T94,($L94/2*($H94*(Q94*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T94 > 0, $T94, ( $L94 / 2 * ( ( $I94 ) * (Q94*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T95>0,$T95,($L95/2*(($F95*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T95>0,$T95,($L95/2*($G95*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T95>0,$T95,($L95/2*($H95*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T95 > 0, $T95, ( $L95 / 2 * ( ( $I95 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T95 > 0, $T95,($L95/2*(($F95)*(Q95*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T95 > 0, $T95,($L95/2*($G95*(Q95*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T95 > 0, $T95,($L95/2*($H95*(Q95*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T95 > 0, $T95, ( $L95 / 2 * ( ( $I95 ) * (Q95*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T96>0,$T96,($L96/2*(($F96*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T96>0,$T96,($L96/2*($G96*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T96>0,$T96,($L96/2*($H96*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T96 > 0, $T96, ( $L96 / 2 * ( ( $I96 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T96 > 0, $T96,($L96/2*(($F96)*(Q96*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T96 > 0, $T96,($L96/2*($G96*(Q96*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T96 > 0, $T96,($L96/2*($H96*(Q96*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T96 > 0, $T96, ( $L96 / 2 * ( ( $I96 ) * (Q96*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T97>0,$T97,($L97/2*(($F97*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T97>0,$T97,($L97/2*($G97*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T97>0,$T97,($L97/2*($H97*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T97 > 0, $T97, ( $L97 / 2 * ( ( $I97 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T97 > 0, $T97,($L97/2*(($F97)*(Q97*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T97 > 0, $T97,($L97/2*($G97*(Q97*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T97 > 0, $T97,($L97/2*($H97*(Q97*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T97 > 0, $T97, ( $L97 / 2 * ( ( $I97 ) * (Q97*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T98>0,$T98,($L98/2*(($F98*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T98>0,$T98,($L98/2*($G98*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T98>0,$T98,($L98/2*($H98*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T98 > 0, $T98, ( $L98 / 2 * ( ( $I98 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T98 > 0, $T98,($L98/2*(($F98)*(Q98*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T98 > 0, $T98,($L98/2*($G98*(Q98*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T98 > 0, $T98,($L98/2*($H98*(Q98*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T98 > 0, $T98, ( $L98 / 2 * ( ( $I98 ) * (Q98*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T99>0,$T99,($L99/2*(($F99*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T99>0,$T99,($L99/2*($G99*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T99>0,$T99,($L99/2*($H99*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T99 > 0, $T99, ( $L99 / 2 * ( ( $I99 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T99 > 0, $T99,($L99/2*(($F99)*(Q99*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T99 > 0, $T99,($L99/2*($G99*(Q99*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T99 > 0, $T99,($L99/2*($H99*(Q99*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T99 > 0, $T99, ( $L99 / 2 * ( ( $I99 ) * (Q99*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T100>0,$T100,($L100/2*(($F100*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T100>0,$T100,($L100/2*($G100*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T100>0,$T100,($L100/2*($H100*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T100 > 0, $T100, ( $L100 / 2 * ( ( $I100 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T100 > 0, $T100,($L100/2*(($F100)*(Q100*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T100 > 0, $T100,($L100/2*($G100*(Q100*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T100 > 0, $T100,($L100/2*($H100*(Q100*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T100 > 0, $T100, ( $L100 / 2 * ( ( $I100 ) * (Q100*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T101>0,$T101,($L101/2*(($F101*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T101>0,$T101,($L101/2*($G101*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T101>0,$T101,($L101/2*($H101*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T101 > 0, $T101, ( $L101 / 2 * ( ( $I101 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T101 > 0, $T101,($L101/2*(($F101)*(Q101*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T101 > 0, $T101,($L101/2*($G101*(Q101*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T101 > 0, $T101,($L101/2*($H101*(Q101*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T101 > 0, $T101, ( $L101 / 2 * ( ( $I101 ) * (Q101*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T102>0,$T102,($L102/2*(($F102*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T102>0,$T102,($L102/2*($G102*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T102>0,$T102,($L102/2*($H102*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T102 > 0, $T102, ( $L102 / 2 * ( ( $I102 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T102 > 0, $T102,($L102/2*(($F102)*(Q102*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T102 > 0, $T102,($L102/2*($G102*(Q102*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T102 > 0, $T102,($L102/2*($H102*(Q102*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T102 > 0, $T102, ( $L102 / 2 * ( ( $I102 ) * (Q102*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T103>0,$T103,($L103/2*(($F103*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T103>0,$T103,($L103/2*($G103*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T103>0,$T103,($L103/2*($H103*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T103 > 0, $T103, ( $L103 / 2 * ( ( $I103 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T103 > 0, $T103,($L103/2*(($F103)*(Q103*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T103 > 0, $T103,($L103/2*($G103*(Q103*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T103 > 0, $T103,($L103/2*($H103*(Q103*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T103 > 0, $T103, ( $L103 / 2 * ( ( $I103 ) * (Q103*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T104>0,$T104,($L104/2*(($F104*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T104>0,$T104,($L104/2*($G104*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T104>0,$T104,($L104/2*($H104*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T104 > 0, $T104, ( $L104 / 2 * ( ( $I104 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T104 > 0, $T104,($L104/2*(($F104)*(Q104*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T104 > 0, $T104,($L104/2*($G104*(Q104*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T104 > 0, $T104,($L104/2*($H104*(Q104*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T104 > 0, $T104, ( $L104 / 2 * ( ( $I104 ) * (Q104*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T105>0,$T105,($L105/2*(($F105*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T105>0,$T105,($L105/2*($G105*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T105>0,$T105,($L105/2*($H105*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T105 > 0, $T105, ( $L105 / 2 * ( ( $I105 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T105 > 0, $T105,($L105/2*(($F105)*(Q105*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T105 > 0, $T105,($L105/2*($G105*(Q105*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T105 > 0, $T105,($L105/2*($H105*(Q105*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T105 > 0, $T105, ( $L105 / 2 * ( ( $I105 ) * (Q105*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T106>0,$T106,($L106/2*(($F106*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T106>0,$T106,($L106/2*($G106*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T106>0,$T106,($L106/2*($H106*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T106 > 0, $T106, ( $L106 / 2 * ( ( $I106 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T106 > 0, $T106,($L106/2*(($F106)*(Q106*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T106 > 0, $T106,($L106/2*($G106*(Q106*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T106 > 0, $T106,($L106/2*($H106*(Q106*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T106 > 0, $T106, ( $L106 / 2 * ( ( $I106 ) * (Q106*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T107>0,$T107,($L107/2*(($F107*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T107>0,$T107,($L107/2*($G107*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T107>0,$T107,($L107/2*($H107*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T107 > 0, $T107, ( $L107 / 2 * ( ( $I107 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T107 > 0, $T107,($L107/2*(($F107)*(Q107*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T107 > 0, $T107,($L107/2*($G107*(Q107*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T107 > 0, $T107,($L107/2*($H107*(Q107*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T107 > 0, $T107, ( $L107 / 2 * ( ( $I107 ) * (Q107*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T108>0,$T108,($L108/2*(($F108*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T108>0,$T108,($L108/2*($G108*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T108>0,$T108,($L108/2*($H108*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T108 > 0, $T108, ( $L108 / 2 * ( ( $I108 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T108 > 0, $T108,($L108/2*(($F108)*(Q108*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T108 > 0, $T108,($L108/2*($G108*(Q108*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T108 > 0, $T108,($L108/2*($H108*(Q108*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T108 > 0, $T108, ( $L108 / 2 * ( ( $I108 ) * (Q108*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T109>0,$T109,($L109/2*(($F109*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T109>0,$T109,($L109/2*($G109*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T109>0,$T109,($L109/2*($H109*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T109 > 0, $T109, ( $L109 / 2 * ( ( $I109 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T109 > 0, $T109,($L109/2*(($F109)*(Q109*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T109 > 0, $T109,($L109/2*($G109*(Q109*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T109 > 0, $T109,($L109/2*($H109*(Q109*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T109 > 0, $T109, ( $L109 / 2 * ( ( $I109 ) * (Q109*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T110>0,$T110,($L110/2*(($F110*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T110>0,$T110,($L110/2*($G110*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T110>0,$T110,($L110/2*($H110*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T110 > 0, $T110, ( $L110 / 2 * ( ( $I110 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T110 > 0, $T110,($L110/2*(($F110)*(Q110*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T110 > 0, $T110,($L110/2*($G110*(Q110*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T110 > 0, $T110,($L110/2*($H110*(Q110*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T110 > 0, $T110, ( $L110 / 2 * ( ( $I110 ) * (Q110*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T111>0,$T111,($L111/2*(($F111*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T111>0,$T111,($L111/2*($G111*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T111>0,$T111,($L111/2*($H111*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T111 > 0, $T111, ( $L111 / 2 * ( ( $I111 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T111 > 0, $T111,($L111/2*(($F111)*(Q111*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T111 > 0, $T111,($L111/2*($G111*(Q111*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T111 > 0, $T111,($L111/2*($H111*(Q111*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T111 > 0, $T111, ( $L111 / 2 * ( ( $I111 ) * (Q111*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T112>0,$T112,($L112/2*(($F112*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T112>0,$T112,($L112/2*($G112*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T112>0,$T112,($L112/2*($H112*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T112 > 0, $T112, ( $L112 / 2 * ( ( $I112 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T112 > 0, $T112,($L112/2*(($F112)*(Q112*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T112 > 0, $T112,($L112/2*($G112*(Q112*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T112 > 0, $T112,($L112/2*($H112*(Q112*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T112 > 0, $T112, ( $L112 / 2 * ( ( $I112 ) * (Q112*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T113>0,$T113,($L113/2*(($F113*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T113>0,$T113,($L113/2*($G113*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T113>0,$T113,($L113/2*($H113*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T113 > 0, $T113, ( $L113 / 2 * ( ( $I113 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T113 > 0, $T113,($L113/2*(($F113)*(Q113*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T113 > 0, $T113,($L113/2*($G113*(Q113*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T113 > 0, $T113,($L113/2*($H113*(Q113*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T113 > 0, $T113, ( $L113 / 2 * ( ( $I113 ) * (Q113*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T114>0,$T114,($L114/2*(($F114*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T114>0,$T114,($L114/2*($G114*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T114>0,$T114,($L114/2*($H114*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T114 > 0, $T114, ( $L114 / 2 * ( ( $I114 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T114 > 0, $T114,($L114/2*(($F114)*(Q114*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T114 > 0, $T114,($L114/2*($G114*(Q114*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T114 > 0, $T114,($L114/2*($H114*(Q114*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T114 > 0, $T114, ( $L114 / 2 * ( ( $I114 ) * (Q114*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T115>0,$T115,($L115/2*(($F115*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T115>0,$T115,($L115/2*($G115*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T115>0,$T115,($L115/2*($H115*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T115 > 0, $T115, ( $L115 / 2 * ( ( $I115 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T115 > 0, $T115,($L115/2*(($F115)*(Q115*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T115 > 0, $T115,($L115/2*($G115*(Q115*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T115 > 0, $T115,($L115/2*($H115*(Q115*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T115 > 0, $T115, ( $L115 / 2 * ( ( $I115 ) * (Q115*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T116>0,$T116,($L116/2*(($F116*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T116>0,$T116,($L116/2*($G116*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T116>0,$T116,($L116/2*($H116*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T116 > 0, $T116, ( $L116 / 2 * ( ( $I116 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T116 > 0, $T116,($L116/2*(($F116)*(Q116*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T116 > 0, $T116,($L116/2*($G116*(Q116*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T116 > 0, $T116,($L116/2*($H116*(Q116*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T116 > 0, $T116, ( $L116 / 2 * ( ( $I116 ) * (Q116*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T117>0,$T117,($L117/2*(($F117*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T117>0,$T117,($L117/2*($G117*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T117>0,$T117,($L117/2*($H117*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T117 > 0, $T117, ( $L117 / 2 * ( ( $I117 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T117 > 0, $T117,($L117/2*(($F117)*(Q117*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T117 > 0, $T117,($L117/2*($G117*(Q117*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T117 > 0, $T117,($L117/2*($H117*(Q117*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T117 > 0, $T117, ( $L117 / 2 * ( ( $I117 ) * (Q117*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T118>0,$T118,($L118/2*(($F118*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T118>0,$T118,($L118/2*($G118*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T118>0,$T118,($L118/2*($H118*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T118 > 0, $T118, ( $L118 / 2 * ( ( $I118 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T118 > 0, $T118,($L118/2*(($F118)*(Q118*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T118 > 0, $T118,($L118/2*($G118*(Q118*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T118 > 0, $T118,($L118/2*($H118*(Q118*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T118 > 0, $T118, ( $L118 / 2 * ( ( $I118 ) * (Q118*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T119>0,$T119,($L119/2*(($F119*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T119>0,$T119,($L119/2*($G119*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T119>0,$T119,($L119/2*($H119*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T119 > 0, $T119, ( $L119 / 2 * ( ( $I119 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T119 > 0, $T119,($L119/2*(($F119)*(Q119*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T119 > 0, $T119,($L119/2*($G119*(Q119*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T119 > 0, $T119,($L119/2*($H119*(Q119*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T119 > 0, $T119, ( $L119 / 2 * ( ( $I119 ) * (Q119*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T120>0,$T120,($L120/2*(($F120*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T120>0,$T120,($L120/2*($G120*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T120>0,$T120,($L120/2*($H120*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T120 > 0, $T120, ( $L120 / 2 * ( ( $I120 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T120 > 0, $T120,($L120/2*(($F120)*(Q120*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T120 > 0, $T120,($L120/2*($G120*(Q120*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T120 > 0, $T120,($L120/2*($H120*(Q120*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T120 > 0, $T120, ( $L120 / 2 * ( ( $I120 ) * (Q120*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T121>0,$T121,($L121/2*(($F121*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T121>0,$T121,($L121/2*($G121*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T121>0,$T121,($L121/2*($H121*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T121 > 0, $T121, ( $L121 / 2 * ( ( $I121 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T121 > 0, $T121,($L121/2*(($F121)*(Q121*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T121 > 0, $T121,($L121/2*($G121*(Q121*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T121 > 0, $T121,($L121/2*($H121*(Q121*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T121 > 0, $T121, ( $L121 / 2 * ( ( $I121 ) * (Q121*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T122>0,$T122,($L122/2*(($F122*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T122>0,$T122,($L122/2*($G122*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T122>0,$T122,($L122/2*($H122*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T122 > 0, $T122, ( $L122 / 2 * ( ( $I122 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T122 > 0, $T122,($L122/2*(($F122)*(Q122*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T122 > 0, $T122,($L122/2*($G122*(Q122*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T122 > 0, $T122,($L122/2*($H122*(Q122*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T122 > 0, $T122, ( $L122 / 2 * ( ( $I122 ) * (Q122*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T123>0,$T123,($L123/2*(($F123*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T123>0,$T123,($L123/2*($G123*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T123>0,$T123,($L123/2*($H123*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T123 > 0, $T123, ( $L123 / 2 * ( ( $I123 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T123 > 0, $T123,($L123/2*(($F123)*(Q123*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T123 > 0, $T123,($L123/2*($G123*(Q123*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T123 > 0, $T123,($L123/2*($H123*(Q123*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T123 > 0, $T123, ( $L123 / 2 * ( ( $I123 ) * (Q123*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T124>0,$T124,($L124/2*(($F124*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T124>0,$T124,($L124/2*($G124*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T124>0,$T124,($L124/2*($H124*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T124 > 0, $T124, ( $L124 / 2 * ( ( $I124 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T124 > 0, $T124,($L124/2*(($F124)*(Q124*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T124 > 0, $T124,($L124/2*($G124*(Q124*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T124 > 0, $T124,($L124/2*($H124*(Q124*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T124 > 0, $T124, ( $L124 / 2 * ( ( $I124 ) * (Q124*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T125>0,$T125,($L125/2*(($F125*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T125>0,$T125,($L125/2*($G125*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T125>0,$T125,($L125/2*($H125*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T125 > 0, $T125, ( $L125 / 2 * ( ( $I125 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T125 > 0, $T125,($L125/2*(($F125)*(Q125*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T125 > 0, $T125,($L125/2*($G125*(Q125*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T125 > 0, $T125,($L125/2*($H125*(Q125*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T125 > 0, $T125, ( $L125 / 2 * ( ( $I125 ) * (Q125*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T126>0,$T126,($L126/2*(($F126*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T126>0,$T126,($L126/2*($G126*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T126>0,$T126,($L126/2*($H126*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T126 > 0, $T126, ( $L126 / 2 * ( ( $I126 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T126 > 0, $T126,($L126/2*(($F126)*(Q126*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T126 > 0, $T126,($L126/2*($G126*(Q126*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T126 > 0, $T126,($L126/2*($H126*(Q126*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T126 > 0, $T126, ( $L126 / 2 * ( ( $I126 ) * (Q126*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T127>0,$T127,($L127/2*(($F127*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T127>0,$T127,($L127/2*($G127*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T127>0,$T127,($L127/2*($H127*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T127 > 0, $T127, ( $L127 / 2 * ( ( $I127 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T127 > 0, $T127,($L127/2*(($F127)*(Q127*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T127 > 0, $T127,($L127/2*($G127*(Q127*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T127 > 0, $T127,($L127/2*($H127*(Q127*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T127 > 0, $T127, ( $L127 / 2 * ( ( $I127 ) * (Q127*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T128>0,$T128,($L128/2*(($F128*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T128>0,$T128,($L128/2*($G128*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T128>0,$T128,($L128/2*($H128*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T128 > 0, $T128, ( $L128 / 2 * ( ( $I128 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T128 > 0, $T128,($L128/2*(($F128)*(Q128*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T128 > 0, $T128,($L128/2*($G128*(Q128*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T128 > 0, $T128,($L128/2*($H128*(Q128*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T128 > 0, $T128, ( $L128 / 2 * ( ( $I128 ) * (Q128*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T129>0,$T129,($L129/2*(($F129*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T129>0,$T129,($L129/2*($G129*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T129>0,$T129,($L129/2*($H129*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T129 > 0, $T129, ( $L129 / 2 * ( ( $I129 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T129 > 0, $T129,($L129/2*(($F129)*(Q129*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T129 > 0, $T129,($L129/2*($G129*(Q129*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T129 > 0, $T129,($L129/2*($H129*(Q129*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T129 > 0, $T129, ( $L129 / 2 * ( ( $I129 ) * (Q129*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T130>0,$T130,($L130/2*(($F130*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T130>0,$T130,($L130/2*($G130*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T130>0,$T130,($L130/2*($H130*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T130 > 0, $T130, ( $L130 / 2 * ( ( $I130 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T130 > 0, $T130,($L130/2*(($F130)*(Q130*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T130 > 0, $T130,($L130/2*($G130*(Q130*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T130 > 0, $T130,($L130/2*($H130*(Q130*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T130 > 0, $T130, ( $L130 / 2 * ( ( $I130 ) * (Q130*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T131>0,$T131,($L131/2*(($F131*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T131>0,$T131,($L131/2*($G131*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T131>0,$T131,($L131/2*($H131*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T131 > 0, $T131, ( $L131 / 2 * ( ( $I131 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T131 > 0, $T131,($L131/2*(($F131)*(Q131*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T131 > 0, $T131,($L131/2*($G131*(Q131*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T131 > 0, $T131,($L131/2*($H131*(Q131*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T131 > 0, $T131, ( $L131 / 2 * ( ( $I131 ) * (Q131*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T132>0,$T132,($L132/2*(($F132*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T132>0,$T132,($L132/2*($G132*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T132>0,$T132,($L132/2*($H132*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T132 > 0, $T132, ( $L132 / 2 * ( ( $I132 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T132 > 0, $T132,($L132/2*(($F132)*(Q132*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T132 > 0, $T132,($L132/2*($G132*(Q132*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T132 > 0, $T132,($L132/2*($H132*(Q132*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T132 > 0, $T132, ( $L132 / 2 * ( ( $I132 ) * (Q132*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T133>0,$T133,($L133/2*(($F133*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T133>0,$T133,($L133/2*($G133*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T133>0,$T133,($L133/2*($H133*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T133 > 0, $T133, ( $L133 / 2 * ( ( $I133 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T133 > 0, $T133,($L133/2*(($F133)*(Q133*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T133 > 0, $T133,($L133/2*($G133*(Q133*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T133 > 0, $T133,($L133/2*($H133*(Q133*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T133 > 0, $T133, ( $L133 / 2 * ( ( $I133 ) * (Q133*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T134>0,$T134,($L134/2*(($F134*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T134>0,$T134,($L134/2*($G134*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T134>0,$T134,($L134/2*($H134*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T134 > 0, $T134, ( $L134 / 2 * ( ( $I134 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T134 > 0, $T134,($L134/2*(($F134)*(Q134*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T134 > 0, $T134,($L134/2*($G134*(Q134*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T134 > 0, $T134,($L134/2*($H134*(Q134*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T134 > 0, $T134, ( $L134 / 2 * ( ( $I134 ) * (Q134*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T135>0,$T135,($L135/2*(($F135*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T135>0,$T135,($L135/2*($G135*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T135>0,$T135,($L135/2*($H135*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T135 > 0, $T135, ( $L135 / 2 * ( ( $I135 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T135 > 0, $T135,($L135/2*(($F135)*(Q135*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T135 > 0, $T135,($L135/2*($G135*(Q135*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T135 > 0, $T135,($L135/2*($H135*(Q135*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T135 > 0, $T135, ( $L135 / 2 * ( ( $I135 ) * (Q135*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T136>0,$T136,($L136/2*(($F136*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T136>0,$T136,($L136/2*($G136*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T136>0,$T136,($L136/2*($H136*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T136 > 0, $T136, ( $L136 / 2 * ( ( $I136 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T136 > 0, $T136,($L136/2*(($F136)*(Q136*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T136 > 0, $T136,($L136/2*($G136*(Q136*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T136 > 0, $T136,($L136/2*($H136*(Q136*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T136 > 0, $T136, ( $L136 / 2 * ( ( $I136 ) * (Q136*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T137>0,$T137,($L137/2*(($F137*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T137>0,$T137,($L137/2*($G137*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T137>0,$T137,($L137/2*($H137*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T137 > 0, $T137, ( $L137 / 2 * ( ( $I137 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T137 > 0, $T137,($L137/2*(($F137)*(Q137*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T137 > 0, $T137,($L137/2*($G137*(Q137*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T137 > 0, $T137,($L137/2*($H137*(Q137*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T137 > 0, $T137, ( $L137 / 2 * ( ( $I137 ) * (Q137*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T138>0,$T138,($L138/2*(($F138*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T138>0,$T138,($L138/2*($G138*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T138>0,$T138,($L138/2*($H138*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T138 > 0, $T138, ( $L138 / 2 * ( ( $I138 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T138 > 0, $T138,($L138/2*(($F138)*(Q138*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T138 > 0, $T138,($L138/2*($G138*(Q138*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T138 > 0, $T138,($L138/2*($H138*(Q138*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T138 > 0, $T138, ( $L138 / 2 * ( ( $I138 ) * (Q138*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T139>0,$T139,($L139/2*(($F139*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T139>0,$T139,($L139/2*($G139*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T139>0,$T139,($L139/2*($H139*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T139 > 0, $T139, ( $L139 / 2 * ( ( $I139 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T139 > 0, $T139,($L139/2*(($F139)*(Q139*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T139 > 0, $T139,($L139/2*($G139*(Q139*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T139 > 0, $T139,($L139/2*($H139*(Q139*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T139 > 0, $T139, ( $L139 / 2 * ( ( $I139 ) * (Q139*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,{"$f":"E140*J140","v":0},{"$f":"IF(TRUE,SUM(AE140:AF140),(VCCINT/1000)*VCCINT_N*IF($R140>0,$R140,($L140/2*(($F140+$I140)*0.45*$U140+($F140*(OFFSET(FANOUT,8,2))+$G140*(OFFSET(FANOUT,8,4)+$U140)+$H140*(OFFSET(FANOUT,8,5)+$U140)+$I140*(OFFSET(FANOUT,8,3)))))*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1)","v":0},null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T140>0,$T140,($L140/2*(($F140*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T140>0,$T140,($L140/2*($G140*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T140>0,$T140,($L140/2*($H140*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T140 > 0, $T140, ( $L140 / 2 * ( ( $I140 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T140 > 0, $T140,($L140/2*(($F140)*(Q140*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T140 > 0, $T140,($L140/2*($G140*(Q140*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T140 > 0, $T140,($L140/2*($H140*(Q140*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T140 > 0, $T140, ( $L140 / 2 * ( ( $I140 ) * (Q140*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,{"$f":"10^(K141/10)-1","v":5.3095734448019343},null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T141>0,$T141,($L141/2*(($F141*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T141>0,$T141,($L141/2*($G141*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T141>0,$T141,($L141/2*($H141*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T141 > 0, $T141, ( $L141 / 2 * ( ( $I141 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T141 > 0, $T141,($L141/2*(($F141)*(Q141*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T141 > 0, $T141,($L141/2*($G141*(Q141*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T141 > 0, $T141,($L141/2*($H141*(Q141*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T141 > 0, $T141, ( $L141 / 2 * ( ( $I141 ) * (Q141*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"SUM(W141:Z141)","v":0},{"$f":"SUM(AA141:AD141)","v":0}]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T142>0,$T142,($L142/2*(($F142*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T142>0,$T142,($L142/2*($G142*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T142>0,$T142,($L142/2*($H142*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T142 > 0, $T142, ( $L142 / 2 * ( ( $I142 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T142 > 0, $T142,($L142/2*(($F142)*(Q142*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T142 > 0, $T142,($L142/2*($G142*(Q142*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T142 > 0, $T142,($L142/2*($H142*(Q142*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T142 > 0, $T142, ( $L142 / 2 * ( ( $I142 ) * (Q142*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T143>0,$T143,($L143/2*(($F143*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T143>0,$T143,($L143/2*($G143*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T143>0,$T143,($L143/2*($H143*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T143 > 0, $T143, ( $L143 / 2 * ( ( $I143 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T143 > 0, $T143,($L143/2*(($F143)*(Q143*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T143 > 0, $T143,($L143/2*($G143*(Q143*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T143 > 0, $T143,($L143/2*($H143*(Q143*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T143 > 0, $T143, ( $L143 / 2 * ( ( $I143 ) * (Q143*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T144>0,$T144,($L144/2*(($F144*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T144>0,$T144,($L144/2*($G144*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T144>0,$T144,($L144/2*($H144*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T144 > 0, $T144, ( $L144 / 2 * ( ( $I144 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T144 > 0, $T144,($L144/2*(($F144)*(Q144*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T144 > 0, $T144,($L144/2*($G144*(Q144*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T144 > 0, $T144,($L144/2*($H144*(Q144*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T144 > 0, $T144, ( $L144 / 2 * ( ( $I144 ) * (Q144*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T145>0,$T145,($L145/2*(($F145*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T145>0,$T145,($L145/2*($G145*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T145>0,$T145,($L145/2*($H145*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T145 > 0, $T145, ( $L145 / 2 * ( ( $I145 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T145 > 0, $T145,($L145/2*(($F145)*(Q145*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T145 > 0, $T145,($L145/2*($G145*(Q145*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T145 > 0, $T145,($L145/2*($H145*(Q145*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T145 > 0, $T145, ( $L145 / 2 * ( ( $I145 ) * (Q145*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T146>0,$T146,($L146/2*(($F146*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T146>0,$T146,($L146/2*($G146*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T146>0,$T146,($L146/2*($H146*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T146 > 0, $T146, ( $L146 / 2 * ( ( $I146 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T146 > 0, $T146,($L146/2*(($F146)*(Q146*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T146 > 0, $T146,($L146/2*($G146*(Q146*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T146 > 0, $T146,($L146/2*($H146*(Q146*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T146 > 0, $T146, ( $L146 / 2 * ( ( $I146 ) * (Q146*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T147>0,$T147,($L147/2*(($F147*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T147>0,$T147,($L147/2*($G147*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T147>0,$T147,($L147/2*($H147*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T147 > 0, $T147, ( $L147 / 2 * ( ( $I147 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T147 > 0, $T147,($L147/2*(($F147)*(Q147*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T147 > 0, $T147,($L147/2*($G147*(Q147*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T147 > 0, $T147,($L147/2*($H147*(Q147*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T147 > 0, $T147, ( $L147 / 2 * ( ( $I147 ) * (Q147*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T148>0,$T148,($L148/2*(($F148*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T148>0,$T148,($L148/2*($G148*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T148>0,$T148,($L148/2*($H148*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T148 > 0, $T148, ( $L148 / 2 * ( ( $I148 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T148 > 0, $T148,($L148/2*(($F148)*(Q148*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T148 > 0, $T148,($L148/2*($G148*(Q148*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T148 > 0, $T148,($L148/2*($H148*(Q148*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T148 > 0, $T148, ( $L148 / 2 * ( ( $I148 ) * (Q148*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T149>0,$T149,($L149/2*(($F149*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T149>0,$T149,($L149/2*($G149*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T149>0,$T149,($L149/2*($H149*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T149 > 0, $T149, ( $L149 / 2 * ( ( $I149 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T149 > 0, $T149,($L149/2*(($F149)*(Q149*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T149 > 0, $T149,($L149/2*($G149*(Q149*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T149 > 0, $T149,($L149/2*($H149*(Q149*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T149 > 0, $T149, ( $L149 / 2 * ( ( $I149 ) * (Q149*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T150>0,$T150,($L150/2*(($F150*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T150>0,$T150,($L150/2*($G150*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T150>0,$T150,($L150/2*($H150*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T150 > 0, $T150, ( $L150 / 2 * ( ( $I150 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T150 > 0, $T150,($L150/2*(($F150)*(Q150*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T150 > 0, $T150,($L150/2*($G150*(Q150*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T150 > 0, $T150,($L150/2*($H150*(Q150*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T150 > 0, $T150, ( $L150 / 2 * ( ( $I150 ) * (Q150*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T151>0,$T151,($L151/2*(($F151*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T151>0,$T151,($L151/2*($G151*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T151>0,$T151,($L151/2*($H151*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T151 > 0, $T151, ( $L151 / 2 * ( ( $I151 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T151 > 0, $T151,($L151/2*(($F151)*(Q151*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T151 > 0, $T151,($L151/2*($G151*(Q151*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T151 > 0, $T151,($L151/2*($H151*(Q151*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T151 > 0, $T151, ( $L151 / 2 * ( ( $I151 ) * (Q151*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T152>0,$T152,($L152/2*(($F152*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T152>0,$T152,($L152/2*($G152*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T152>0,$T152,($L152/2*($H152*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T152 > 0, $T152, ( $L152 / 2 * ( ( $I152 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T152 > 0, $T152,($L152/2*(($F152)*(Q152*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T152 > 0, $T152,($L152/2*($G152*(Q152*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T152 > 0, $T152,($L152/2*($H152*(Q152*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T152 > 0, $T152, ( $L152 / 2 * ( ( $I152 ) * (Q152*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T153>0,$T153,($L153/2*(($F153*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T153>0,$T153,($L153/2*($G153*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T153>0,$T153,($L153/2*($H153*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T153 > 0, $T153, ( $L153 / 2 * ( ( $I153 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T153 > 0, $T153,($L153/2*(($F153)*(Q153*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T153 > 0, $T153,($L153/2*($G153*(Q153*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T153 > 0, $T153,($L153/2*($H153*(Q153*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T153 > 0, $T153, ( $L153 / 2 * ( ( $I153 ) * (Q153*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T154>0,$T154,($L154/2*(($F154*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T154>0,$T154,($L154/2*($G154*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T154>0,$T154,($L154/2*($H154*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T154 > 0, $T154, ( $L154 / 2 * ( ( $I154 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T154 > 0, $T154,($L154/2*(($F154)*(Q154*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T154 > 0, $T154,($L154/2*($G154*(Q154*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T154 > 0, $T154,($L154/2*($H154*(Q154*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T154 > 0, $T154, ( $L154 / 2 * ( ( $I154 ) * (Q154*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T155>0,$T155,($L155/2*(($F155*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T155>0,$T155,($L155/2*($G155*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T155>0,$T155,($L155/2*($H155*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T155 > 0, $T155, ( $L155 / 2 * ( ( $I155 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T155 > 0, $T155,($L155/2*(($F155)*(Q155*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T155 > 0, $T155,($L155/2*($G155*(Q155*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T155 > 0, $T155,($L155/2*($H155*(Q155*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T155 > 0, $T155, ( $L155 / 2 * ( ( $I155 ) * (Q155*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T156>0,$T156,($L156/2*(($F156*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T156>0,$T156,($L156/2*($G156*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T156>0,$T156,($L156/2*($H156*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T156 > 0, $T156, ( $L156 / 2 * ( ( $I156 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T156 > 0, $T156,($L156/2*(($F156)*(Q156*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T156 > 0, $T156,($L156/2*($G156*(Q156*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T156 > 0, $T156,($L156/2*($H156*(Q156*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T156 > 0, $T156, ( $L156 / 2 * ( ( $I156 ) * (Q156*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T157>0,$T157,($L157/2*(($F157*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T157>0,$T157,($L157/2*($G157*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T157>0,$T157,($L157/2*($H157*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T157 > 0, $T157, ( $L157 / 2 * ( ( $I157 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T157 > 0, $T157,($L157/2*(($F157)*(Q157*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T157 > 0, $T157,($L157/2*($G157*(Q157*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T157 > 0, $T157,($L157/2*($H157*(Q157*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T157 > 0, $T157, ( $L157 / 2 * ( ( $I157 ) * (Q157*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T158>0,$T158,($L158/2*(($F158*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T158>0,$T158,($L158/2*($G158*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T158>0,$T158,($L158/2*($H158*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T158 > 0, $T158, ( $L158 / 2 * ( ( $I158 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T158 > 0, $T158,($L158/2*(($F158)*(Q158*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T158 > 0, $T158,($L158/2*($G158*(Q158*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T158 > 0, $T158,($L158/2*($H158*(Q158*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T158 > 0, $T158, ( $L158 / 2 * ( ( $I158 ) * (Q158*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T159>0,$T159,($L159/2*(($F159*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T159>0,$T159,($L159/2*($G159*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T159>0,$T159,($L159/2*($H159*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T159 > 0, $T159, ( $L159 / 2 * ( ( $I159 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T159 > 0, $T159,($L159/2*(($F159)*(Q159*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T159 > 0, $T159,($L159/2*($G159*(Q159*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T159 > 0, $T159,($L159/2*($H159*(Q159*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T159 > 0, $T159, ( $L159 / 2 * ( ( $I159 ) * (Q159*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T160>0,$T160,($L160/2*(($F160*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T160>0,$T160,($L160/2*($G160*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T160>0,$T160,($L160/2*($H160*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T160 > 0, $T160, ( $L160 / 2 * ( ( $I160 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T160 > 0, $T160,($L160/2*(($F160)*(Q160*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T160 > 0, $T160,($L160/2*($G160*(Q160*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T160 > 0, $T160,($L160/2*($H160*(Q160*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T160 > 0, $T160, ( $L160 / 2 * ( ( $I160 ) * (Q160*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T161>0,$T161,($L161/2*(($F161*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T161>0,$T161,($L161/2*($G161*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T161>0,$T161,($L161/2*($H161*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T161 > 0, $T161, ( $L161 / 2 * ( ( $I161 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T161 > 0, $T161,($L161/2*(($F161)*(Q161*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T161 > 0, $T161,($L161/2*($G161*(Q161*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T161 > 0, $T161,($L161/2*($H161*(Q161*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T161 > 0, $T161, ( $L161 / 2 * ( ( $I161 ) * (Q161*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T162>0,$T162,($L162/2*(($F162*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T162>0,$T162,($L162/2*($G162*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T162>0,$T162,($L162/2*($H162*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T162 > 0, $T162, ( $L162 / 2 * ( ( $I162 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T162 > 0, $T162,($L162/2*(($F162)*(Q162*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T162 > 0, $T162,($L162/2*($G162*(Q162*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T162 > 0, $T162,($L162/2*($H162*(Q162*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T162 > 0, $T162, ( $L162 / 2 * ( ( $I162 ) * (Q162*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T163>0,$T163,($L163/2*(($F163*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T163>0,$T163,($L163/2*($G163*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T163>0,$T163,($L163/2*($H163*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T163 > 0, $T163, ( $L163 / 2 * ( ( $I163 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T163 > 0, $T163,($L163/2*(($F163)*(Q163*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T163 > 0, $T163,($L163/2*($G163*(Q163*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T163 > 0, $T163,($L163/2*($H163*(Q163*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T163 > 0, $T163, ( $L163 / 2 * ( ( $I163 ) * (Q163*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T164>0,$T164,($L164/2*(($F164*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T164>0,$T164,($L164/2*($G164*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T164>0,$T164,($L164/2*($H164*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T164 > 0, $T164, ( $L164 / 2 * ( ( $I164 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T164 > 0, $T164,($L164/2*(($F164)*(Q164*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T164 > 0, $T164,($L164/2*($G164*(Q164*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T164 > 0, $T164,($L164/2*($H164*(Q164*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T164 > 0, $T164, ( $L164 / 2 * ( ( $I164 ) * (Q164*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T165>0,$T165,($L165/2*(($F165*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T165>0,$T165,($L165/2*($G165*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T165>0,$T165,($L165/2*($H165*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T165 > 0, $T165, ( $L165 / 2 * ( ( $I165 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T165 > 0, $T165,($L165/2*(($F165)*(Q165*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T165 > 0, $T165,($L165/2*($G165*(Q165*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T165 > 0, $T165,($L165/2*($H165*(Q165*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T165 > 0, $T165, ( $L165 / 2 * ( ( $I165 ) * (Q165*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T166>0,$T166,($L166/2*(($F166*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T166>0,$T166,($L166/2*($G166*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T166>0,$T166,($L166/2*($H166*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T166 > 0, $T166, ( $L166 / 2 * ( ( $I166 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T166 > 0, $T166,($L166/2*(($F166)*(Q166*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T166 > 0, $T166,($L166/2*($G166*(Q166*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T166 > 0, $T166,($L166/2*($H166*(Q166*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T166 > 0, $T166, ( $L166 / 2 * ( ( $I166 ) * (Q166*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T167>0,$T167,($L167/2*(($F167*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T167>0,$T167,($L167/2*($G167*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T167>0,$T167,($L167/2*($H167*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T167 > 0, $T167, ( $L167 / 2 * ( ( $I167 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T167 > 0, $T167,($L167/2*(($F167)*(Q167*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T167 > 0, $T167,($L167/2*($G167*(Q167*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T167 > 0, $T167,($L167/2*($H167*(Q167*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T167 > 0, $T167, ( $L167 / 2 * ( ( $I167 ) * (Q167*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T168>0,$T168,($L168/2*(($F168*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T168>0,$T168,($L168/2*($G168*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T168>0,$T168,($L168/2*($H168*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T168 > 0, $T168, ( $L168 / 2 * ( ( $I168 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T168 > 0, $T168,($L168/2*(($F168)*(Q168*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T168 > 0, $T168,($L168/2*($G168*(Q168*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T168 > 0, $T168,($L168/2*($H168*(Q168*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T168 > 0, $T168, ( $L168 / 2 * ( ( $I168 ) * (Q168*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T169>0,$T169,($L169/2*(($F169*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T169>0,$T169,($L169/2*($G169*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T169>0,$T169,($L169/2*($H169*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T169 > 0, $T169, ( $L169 / 2 * ( ( $I169 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T169 > 0, $T169,($L169/2*(($F169)*(Q169*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T169 > 0, $T169,($L169/2*($G169*(Q169*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T169 > 0, $T169,($L169/2*($H169*(Q169*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T169 > 0, $T169, ( $L169 / 2 * ( ( $I169 ) * (Q169*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T170>0,$T170,($L170/2*(($F170*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T170>0,$T170,($L170/2*($G170*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T170>0,$T170,($L170/2*($H170*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T170 > 0, $T170, ( $L170 / 2 * ( ( $I170 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T170 > 0, $T170,($L170/2*(($F170)*(Q170*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T170 > 0, $T170,($L170/2*($G170*(Q170*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T170 > 0, $T170,($L170/2*($H170*(Q170*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T170 > 0, $T170, ( $L170 / 2 * ( ( $I170 ) * (Q170*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T171>0,$T171,($L171/2*(($F171*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T171>0,$T171,($L171/2*($G171*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T171>0,$T171,($L171/2*($H171*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T171 > 0, $T171, ( $L171 / 2 * ( ( $I171 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T171 > 0, $T171,($L171/2*(($F171)*(Q171*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T171 > 0, $T171,($L171/2*($G171*(Q171*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T171 > 0, $T171,($L171/2*($H171*(Q171*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T171 > 0, $T171, ( $L171 / 2 * ( ( $I171 ) * (Q171*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T172>0,$T172,($L172/2*(($F172*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T172>0,$T172,($L172/2*($G172*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T172>0,$T172,($L172/2*($H172*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T172 > 0, $T172, ( $L172 / 2 * ( ( $I172 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T172 > 0, $T172,($L172/2*(($F172)*(Q172*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T172 > 0, $T172,($L172/2*($G172*(Q172*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T172 > 0, $T172,($L172/2*($H172*(Q172*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T172 > 0, $T172, ( $L172 / 2 * ( ( $I172 ) * (Q172*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T173>0,$T173,($L173/2*(($F173*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T173>0,$T173,($L173/2*($G173*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T173>0,$T173,($L173/2*($H173*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T173 > 0, $T173, ( $L173 / 2 * ( ( $I173 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T173 > 0, $T173,($L173/2*(($F173)*(Q173*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T173 > 0, $T173,($L173/2*($G173*(Q173*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T173 > 0, $T173,($L173/2*($H173*(Q173*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T173 > 0, $T173, ( $L173 / 2 * ( ( $I173 ) * (Q173*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T174>0,$T174,($L174/2*(($F174*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T174>0,$T174,($L174/2*($G174*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T174>0,$T174,($L174/2*($H174*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T174 > 0, $T174, ( $L174 / 2 * ( ( $I174 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T174 > 0, $T174,($L174/2*(($F174)*(Q174*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T174 > 0, $T174,($L174/2*($G174*(Q174*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T174 > 0, $T174,($L174/2*($H174*(Q174*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T174 > 0, $T174, ( $L174 / 2 * ( ( $I174 ) * (Q174*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T175>0,$T175,($L175/2*(($F175*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T175>0,$T175,($L175/2*($G175*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T175>0,$T175,($L175/2*($H175*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T175 > 0, $T175, ( $L175 / 2 * ( ( $I175 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T175 > 0, $T175,($L175/2*(($F175)*(Q175*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T175 > 0, $T175,($L175/2*($G175*(Q175*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T175 > 0, $T175,($L175/2*($H175*(Q175*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T175 > 0, $T175, ( $L175 / 2 * ( ( $I175 ) * (Q175*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T176>0,$T176,($L176/2*(($F176*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T176>0,$T176,($L176/2*($G176*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T176>0,$T176,($L176/2*($H176*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T176 > 0, $T176, ( $L176 / 2 * ( ( $I176 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T176 > 0, $T176,($L176/2*(($F176)*(Q176*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T176 > 0, $T176,($L176/2*($G176*(Q176*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T176 > 0, $T176,($L176/2*($H176*(Q176*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T176 > 0, $T176, ( $L176 / 2 * ( ( $I176 ) * (Q176*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T177>0,$T177,($L177/2*(($F177*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T177>0,$T177,($L177/2*($G177*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T177>0,$T177,($L177/2*($H177*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T177 > 0, $T177, ( $L177 / 2 * ( ( $I177 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T177 > 0, $T177,($L177/2*(($F177)*(Q177*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T177 > 0, $T177,($L177/2*($G177*(Q177*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T177 > 0, $T177,($L177/2*($H177*(Q177*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T177 > 0, $T177, ( $L177 / 2 * ( ( $I177 ) * (Q177*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T178>0,$T178,($L178/2*(($F178*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T178>0,$T178,($L178/2*($G178*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T178>0,$T178,($L178/2*($H178*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T178 > 0, $T178, ( $L178 / 2 * ( ( $I178 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T178 > 0, $T178,($L178/2*(($F178)*(Q178*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T178 > 0, $T178,($L178/2*($G178*(Q178*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T178 > 0, $T178,($L178/2*($H178*(Q178*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T178 > 0, $T178, ( $L178 / 2 * ( ( $I178 ) * (Q178*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T179>0,$T179,($L179/2*(($F179*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T179>0,$T179,($L179/2*($G179*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T179>0,$T179,($L179/2*($H179*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T179 > 0, $T179, ( $L179 / 2 * ( ( $I179 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T179 > 0, $T179,($L179/2*(($F179)*(Q179*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T179 > 0, $T179,($L179/2*($G179*(Q179*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T179 > 0, $T179,($L179/2*($H179*(Q179*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T179 > 0, $T179, ( $L179 / 2 * ( ( $I179 ) * (Q179*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T180>0,$T180,($L180/2*(($F180*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T180>0,$T180,($L180/2*($G180*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T180>0,$T180,($L180/2*($H180*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T180 > 0, $T180, ( $L180 / 2 * ( ( $I180 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T180 > 0, $T180,($L180/2*(($F180)*(Q180*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T180 > 0, $T180,($L180/2*($G180*(Q180*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T180 > 0, $T180,($L180/2*($H180*(Q180*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T180 > 0, $T180, ( $L180 / 2 * ( ( $I180 ) * (Q180*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T181>0,$T181,($L181/2*(($F181*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T181>0,$T181,($L181/2*($G181*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T181>0,$T181,($L181/2*($H181*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T181 > 0, $T181, ( $L181 / 2 * ( ( $I181 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T181 > 0, $T181,($L181/2*(($F181)*(Q181*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T181 > 0, $T181,($L181/2*($G181*(Q181*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T181 > 0, $T181,($L181/2*($H181*(Q181*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T181 > 0, $T181, ( $L181 / 2 * ( ( $I181 ) * (Q181*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T182>0,$T182,($L182/2*(($F182*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T182>0,$T182,($L182/2*($G182*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T182>0,$T182,($L182/2*($H182*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T182 > 0, $T182, ( $L182 / 2 * ( ( $I182 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T182 > 0, $T182,($L182/2*(($F182)*(Q182*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T182 > 0, $T182,($L182/2*($G182*(Q182*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T182 > 0, $T182,($L182/2*($H182*(Q182*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T182 > 0, $T182, ( $L182 / 2 * ( ( $I182 ) * (Q182*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T183>0,$T183,($L183/2*(($F183*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T183>0,$T183,($L183/2*($G183*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T183>0,$T183,($L183/2*($H183*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T183 > 0, $T183, ( $L183 / 2 * ( ( $I183 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T183 > 0, $T183,($L183/2*(($F183)*(Q183*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T183 > 0, $T183,($L183/2*($G183*(Q183*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T183 > 0, $T183,($L183/2*($H183*(Q183*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T183 > 0, $T183, ( $L183 / 2 * ( ( $I183 ) * (Q183*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T184>0,$T184,($L184/2*(($F184*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T184>0,$T184,($L184/2*($G184*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T184>0,$T184,($L184/2*($H184*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T184 > 0, $T184, ( $L184 / 2 * ( ( $I184 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T184 > 0, $T184,($L184/2*(($F184)*(Q184*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T184 > 0, $T184,($L184/2*($G184*(Q184*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T184 > 0, $T184,($L184/2*($H184*(Q184*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T184 > 0, $T184, ( $L184 / 2 * ( ( $I184 ) * (Q184*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T185>0,$T185,($L185/2*(($F185*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T185>0,$T185,($L185/2*($G185*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T185>0,$T185,($L185/2*($H185*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T185 > 0, $T185, ( $L185 / 2 * ( ( $I185 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T185 > 0, $T185,($L185/2*(($F185)*(Q185*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T185 > 0, $T185,($L185/2*($G185*(Q185*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T185 > 0, $T185,($L185/2*($H185*(Q185*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T185 > 0, $T185, ( $L185 / 2 * ( ( $I185 ) * (Q185*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T186>0,$T186,($L186/2*(($F186*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T186>0,$T186,($L186/2*($G186*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T186>0,$T186,($L186/2*($H186*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T186 > 0, $T186, ( $L186 / 2 * ( ( $I186 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T186 > 0, $T186,($L186/2*(($F186)*(Q186*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T186 > 0, $T186,($L186/2*($G186*(Q186*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T186 > 0, $T186,($L186/2*($H186*(Q186*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T186 > 0, $T186, ( $L186 / 2 * ( ( $I186 ) * (Q186*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T187>0,$T187,($L187/2*(($F187*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T187>0,$T187,($L187/2*($G187*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T187>0,$T187,($L187/2*($H187*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T187 > 0, $T187, ( $L187 / 2 * ( ( $I187 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T187 > 0, $T187,($L187/2*(($F187)*(Q187*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T187 > 0, $T187,($L187/2*($G187*(Q187*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T187 > 0, $T187,($L187/2*($H187*(Q187*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T187 > 0, $T187, ( $L187 / 2 * ( ( $I187 ) * (Q187*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T188>0,$T188,($L188/2*(($F188*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T188>0,$T188,($L188/2*($G188*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T188>0,$T188,($L188/2*($H188*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T188 > 0, $T188, ( $L188 / 2 * ( ( $I188 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T188 > 0, $T188,($L188/2*(($F188)*(Q188*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T188 > 0, $T188,($L188/2*($G188*(Q188*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T188 > 0, $T188,($L188/2*($H188*(Q188*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T188 > 0, $T188, ( $L188 / 2 * ( ( $I188 ) * (Q188*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T189>0,$T189,($L189/2*(($F189*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T189>0,$T189,($L189/2*($G189*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T189>0,$T189,($L189/2*($H189*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T189 > 0, $T189, ( $L189 / 2 * ( ( $I189 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T189 > 0, $T189,($L189/2*(($F189)*(Q189*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T189 > 0, $T189,($L189/2*($G189*(Q189*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T189 > 0, $T189,($L189/2*($H189*(Q189*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T189 > 0, $T189, ( $L189 / 2 * ( ( $I189 ) * (Q189*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T190>0,$T190,($L190/2*(($F190*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T190>0,$T190,($L190/2*($G190*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T190>0,$T190,($L190/2*($H190*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T190 > 0, $T190, ( $L190 / 2 * ( ( $I190 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T190 > 0, $T190,($L190/2*(($F190)*(Q190*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T190 > 0, $T190,($L190/2*($G190*(Q190*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T190 > 0, $T190,($L190/2*($H190*(Q190*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T190 > 0, $T190, ( $L190 / 2 * ( ( $I190 ) * (Q190*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T191>0,$T191,($L191/2*(($F191*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T191>0,$T191,($L191/2*($G191*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T191>0,$T191,($L191/2*($H191*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T191 > 0, $T191, ( $L191 / 2 * ( ( $I191 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T191 > 0, $T191,($L191/2*(($F191)*(Q191*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T191 > 0, $T191,($L191/2*($G191*(Q191*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T191 > 0, $T191,($L191/2*($H191*(Q191*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T191 > 0, $T191, ( $L191 / 2 * ( ( $I191 ) * (Q191*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T192>0,$T192,($L192/2*(($F192*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T192>0,$T192,($L192/2*($G192*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T192>0,$T192,($L192/2*($H192*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T192 > 0, $T192, ( $L192 / 2 * ( ( $I192 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T192 > 0, $T192,($L192/2*(($F192)*(Q192*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T192 > 0, $T192,($L192/2*($G192*(Q192*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T192 > 0, $T192,($L192/2*($H192*(Q192*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T192 > 0, $T192, ( $L192 / 2 * ( ( $I192 ) * (Q192*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T193>0,$T193,($L193/2*(($F193*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T193>0,$T193,($L193/2*($G193*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T193>0,$T193,($L193/2*($H193*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T193 > 0, $T193, ( $L193 / 2 * ( ( $I193 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T193 > 0, $T193,($L193/2*(($F193)*(Q193*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T193 > 0, $T193,($L193/2*($G193*(Q193*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T193 > 0, $T193,($L193/2*($H193*(Q193*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T193 > 0, $T193, ( $L193 / 2 * ( ( $I193 ) * (Q193*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T194>0,$T194,($L194/2*(($F194*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T194>0,$T194,($L194/2*($G194*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T194>0,$T194,($L194/2*($H194*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T194 > 0, $T194, ( $L194 / 2 * ( ( $I194 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T194 > 0, $T194,($L194/2*(($F194)*(Q194*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T194 > 0, $T194,($L194/2*($G194*(Q194*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T194 > 0, $T194,($L194/2*($H194*(Q194*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T194 > 0, $T194, ( $L194 / 2 * ( ( $I194 ) * (Q194*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T195>0,$T195,($L195/2*(($F195*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T195>0,$T195,($L195/2*($G195*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T195>0,$T195,($L195/2*($H195*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T195 > 0, $T195, ( $L195 / 2 * ( ( $I195 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T195 > 0, $T195,($L195/2*(($F195)*(Q195*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T195 > 0, $T195,($L195/2*($G195*(Q195*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T195 > 0, $T195,($L195/2*($H195*(Q195*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T195 > 0, $T195, ( $L195 / 2 * ( ( $I195 ) * (Q195*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T196>0,$T196,($L196/2*(($F196*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T196>0,$T196,($L196/2*($G196*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T196>0,$T196,($L196/2*($H196*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T196 > 0, $T196, ( $L196 / 2 * ( ( $I196 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T196 > 0, $T196,($L196/2*(($F196)*(Q196*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T196 > 0, $T196,($L196/2*($G196*(Q196*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T196 > 0, $T196,($L196/2*($H196*(Q196*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T196 > 0, $T196, ( $L196 / 2 * ( ( $I196 ) * (Q196*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T197>0,$T197,($L197/2*(($F197*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T197>0,$T197,($L197/2*($G197*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T197>0,$T197,($L197/2*($H197*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T197 > 0, $T197, ( $L197 / 2 * ( ( $I197 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T197 > 0, $T197,($L197/2*(($F197)*(Q197*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T197 > 0, $T197,($L197/2*($G197*(Q197*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T197 > 0, $T197,($L197/2*($H197*(Q197*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T197 > 0, $T197, ( $L197 / 2 * ( ( $I197 ) * (Q197*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T198>0,$T198,($L198/2*(($F198*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T198>0,$T198,($L198/2*($G198*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T198>0,$T198,($L198/2*($H198*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T198 > 0, $T198, ( $L198 / 2 * ( ( $I198 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T198 > 0, $T198,($L198/2*(($F198)*(Q198*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T198 > 0, $T198,($L198/2*($G198*(Q198*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T198 > 0, $T198,($L198/2*($H198*(Q198*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T198 > 0, $T198, ( $L198 / 2 * ( ( $I198 ) * (Q198*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T199>0,$T199,($L199/2*(($F199*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T199>0,$T199,($L199/2*($G199*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T199>0,$T199,($L199/2*($H199*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T199 > 0, $T199, ( $L199 / 2 * ( ( $I199 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T199 > 0, $T199,($L199/2*(($F199)*(Q199*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T199 > 0, $T199,($L199/2*($G199*(Q199*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T199 > 0, $T199,($L199/2*($H199*(Q199*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T199 > 0, $T199, ( $L199 / 2 * ( ( $I199 ) * (Q199*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,{"$f":"E200*J200","v":0},0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T200>0,$T200,($L200/2*(($F200*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T200>0,$T200,($L200/2*($G200*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T200>0,$T200,($L200/2*($H200*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T200 > 0, $T200, ( $L200 / 2 * ( ( $I200 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T200 > 0, $T200,($L200/2*(($F200)*(Q200*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T200 > 0, $T200,($L200/2*($G200*(Q200*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T200 > 0, $T200,($L200/2*($H200*(Q200*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T200 > 0, $T200, ( $L200 / 2 * ( ( $I200 ) * (Q200*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T201>0,$T201,($L201/2*(($F201*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T201>0,$T201,($L201/2*($G201*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T201>0,$T201,($L201/2*($H201*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T201 > 0, $T201, ( $L201 / 2 * ( ( $I201 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T201 > 0, $T201,($L201/2*(($F201)*(Q201*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T201 > 0, $T201,($L201/2*($G201*(Q201*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T201 > 0, $T201,($L201/2*($H201*(Q201*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T201 > 0, $T201, ( $L201 / 2 * ( ( $I201 ) * (Q201*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T202>0,$T202,($L202/2*(($F202*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T202>0,$T202,($L202/2*($G202*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T202>0,$T202,($L202/2*($H202*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T202 > 0, $T202, ( $L202 / 2 * ( ( $I202 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T202 > 0, $T202,($L202/2*(($F202)*(Q202*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T202 > 0, $T202,($L202/2*($G202*(Q202*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T202 > 0, $T202,($L202/2*($H202*(Q202*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T202 > 0, $T202, ( $L202 / 2 * ( ( $I202 ) * (Q202*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T203>0,$T203,($L203/2*(($F203*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T203>0,$T203,($L203/2*($G203*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T203>0,$T203,($L203/2*($H203*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T203 > 0, $T203, ( $L203 / 2 * ( ( $I203 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T203 > 0, $T203,($L203/2*(($F203)*(Q203*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T203 > 0, $T203,($L203/2*($G203*(Q203*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T203 > 0, $T203,($L203/2*($H203*(Q203*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T203 > 0, $T203, ( $L203 / 2 * ( ( $I203 ) * (Q203*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,{"$f":"IF(TRUE,SUM(AE204:AF204),(VCCINT/1000)*VCCINT_N*IF($R204>0,$R204,($L204/2*(($F204+$I204)*0.45*$U204+($F204*(OFFSET(FANOUT,8,2))+$G204*(OFFSET(FANOUT,8,4)+$U204)+$H204*(OFFSET(FANOUT,8,5)+$U204)+$I204*(OFFSET(FANOUT,8,3)))))*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1)","v":0},null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T204>0,$T204,($L204/2*(($F204*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T204>0,$T204,($L204/2*($G204*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T204>0,$T204,($L204/2*($H204*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T204 > 0, $T204, ( $L204 / 2 * ( ( $I204 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T204 > 0, $T204,($L204/2*(($F204)*(Q204*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T204 > 0, $T204,($L204/2*($G204*(Q204*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T204 > 0, $T204,($L204/2*($H204*(Q204*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T204 > 0, $T204, ( $L204 / 2 * ( ( $I204 ) * (Q204*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,{"$f":"10^(K205/10)-1","v":5.3095734448019343},null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T205>0,$T205,($L205/2*(($F205*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T205>0,$T205,($L205/2*($G205*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T205>0,$T205,($L205/2*($H205*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T205 > 0, $T205, ( $L205 / 2 * ( ( $I205 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T205 > 0, $T205,($L205/2*(($F205)*(Q205*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T205 > 0, $T205,($L205/2*($G205*(Q205*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T205 > 0, $T205,($L205/2*($H205*(Q205*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T205 > 0, $T205, ( $L205 / 2 * ( ( $I205 ) * (Q205*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"SUM(W205:Z205)","v":0},{"$f":"SUM(AA205:AD205)","v":0}]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T206>0,$T206,($L206/2*(($F206*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T206>0,$T206,($L206/2*($G206*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T206>0,$T206,($L206/2*($H206*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T206 > 0, $T206, ( $L206 / 2 * ( ( $I206 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T206 > 0, $T206,($L206/2*(($F206)*(Q206*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T206 > 0, $T206,($L206/2*($G206*(Q206*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T206 > 0, $T206,($L206/2*($H206*(Q206*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T206 > 0, $T206, ( $L206 / 2 * ( ( $I206 ) * (Q206*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T207>0,$T207,($L207/2*(($F207*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T207>0,$T207,($L207/2*($G207*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T207>0,$T207,($L207/2*($H207*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T207 > 0, $T207, ( $L207 / 2 * ( ( $I207 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T207 > 0, $T207,($L207/2*(($F207)*(Q207*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T207 > 0, $T207,($L207/2*($G207*(Q207*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T207 > 0, $T207,($L207/2*($H207*(Q207*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T207 > 0, $T207, ( $L207 / 2 * ( ( $I207 ) * (Q207*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T208>0,$T208,($L208/2*(($F208*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T208>0,$T208,($L208/2*($G208*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T208>0,$T208,($L208/2*($H208*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T208 > 0, $T208, ( $L208 / 2 * ( ( $I208 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T208 > 0, $T208,($L208/2*(($F208)*(Q208*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T208 > 0, $T208,($L208/2*($G208*(Q208*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T208 > 0, $T208,($L208/2*($H208*(Q208*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T208 > 0, $T208, ( $L208 / 2 * ( ( $I208 ) * (Q208*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T209>0,$T209,($L209/2*(($F209*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T209>0,$T209,($L209/2*($G209*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T209>0,$T209,($L209/2*($H209*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T209 > 0, $T209, ( $L209 / 2 * ( ( $I209 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T209 > 0, $T209,($L209/2*(($F209)*(Q209*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T209 > 0, $T209,($L209/2*($G209*(Q209*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T209 > 0, $T209,($L209/2*($H209*(Q209*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T209 > 0, $T209, ( $L209 / 2 * ( ( $I209 ) * (Q209*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T210>0,$T210,($L210/2*(($F210*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T210>0,$T210,($L210/2*($G210*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T210>0,$T210,($L210/2*($H210*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T210 > 0, $T210, ( $L210 / 2 * ( ( $I210 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T210 > 0, $T210,($L210/2*(($F210)*(Q210*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T210 > 0, $T210,($L210/2*($G210*(Q210*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T210 > 0, $T210,($L210/2*($H210*(Q210*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T210 > 0, $T210, ( $L210 / 2 * ( ( $I210 ) * (Q210*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T211>0,$T211,($L211/2*(($F211*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T211>0,$T211,($L211/2*($G211*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T211>0,$T211,($L211/2*($H211*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T211 > 0, $T211, ( $L211 / 2 * ( ( $I211 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T211 > 0, $T211,($L211/2*(($F211)*(Q211*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T211 > 0, $T211,($L211/2*($G211*(Q211*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T211 > 0, $T211,($L211/2*($H211*(Q211*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T211 > 0, $T211, ( $L211 / 2 * ( ( $I211 ) * (Q211*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T212>0,$T212,($L212/2*(($F212*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T212>0,$T212,($L212/2*($G212*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T212>0,$T212,($L212/2*($H212*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T212 > 0, $T212, ( $L212 / 2 * ( ( $I212 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T212 > 0, $T212,($L212/2*(($F212)*(Q212*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T212 > 0, $T212,($L212/2*($G212*(Q212*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T212 > 0, $T212,($L212/2*($H212*(Q212*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T212 > 0, $T212, ( $L212 / 2 * ( ( $I212 ) * (Q212*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T213>0,$T213,($L213/2*(($F213*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T213>0,$T213,($L213/2*($G213*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T213>0,$T213,($L213/2*($H213*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T213 > 0, $T213, ( $L213 / 2 * ( ( $I213 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T213 > 0, $T213,($L213/2*(($F213)*(Q213*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T213 > 0, $T213,($L213/2*($G213*(Q213*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T213 > 0, $T213,($L213/2*($H213*(Q213*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T213 > 0, $T213, ( $L213 / 2 * ( ( $I213 ) * (Q213*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T214>0,$T214,($L214/2*(($F214*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T214>0,$T214,($L214/2*($G214*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T214>0,$T214,($L214/2*($H214*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T214 > 0, $T214, ( $L214 / 2 * ( ( $I214 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T214 > 0, $T214,($L214/2*(($F214)*(Q214*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T214 > 0, $T214,($L214/2*($G214*(Q214*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T214 > 0, $T214,($L214/2*($H214*(Q214*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T214 > 0, $T214, ( $L214 / 2 * ( ( $I214 ) * (Q214*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T215>0,$T215,($L215/2*(($F215*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T215>0,$T215,($L215/2*($G215*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T215>0,$T215,($L215/2*($H215*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T215 > 0, $T215, ( $L215 / 2 * ( ( $I215 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T215 > 0, $T215,($L215/2*(($F215)*(Q215*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T215 > 0, $T215,($L215/2*($G215*(Q215*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T215 > 0, $T215,($L215/2*($H215*(Q215*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T215 > 0, $T215, ( $L215 / 2 * ( ( $I215 ) * (Q215*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T216>0,$T216,($L216/2*(($F216*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T216>0,$T216,($L216/2*($G216*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T216>0,$T216,($L216/2*($H216*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T216 > 0, $T216, ( $L216 / 2 * ( ( $I216 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T216 > 0, $T216,($L216/2*(($F216)*(Q216*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T216 > 0, $T216,($L216/2*($G216*(Q216*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T216 > 0, $T216,($L216/2*($H216*(Q216*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T216 > 0, $T216, ( $L216 / 2 * ( ( $I216 ) * (Q216*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T217>0,$T217,($L217/2*(($F217*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T217>0,$T217,($L217/2*($G217*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T217>0,$T217,($L217/2*($H217*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T217 > 0, $T217, ( $L217 / 2 * ( ( $I217 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T217 > 0, $T217,($L217/2*(($F217)*(Q217*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T217 > 0, $T217,($L217/2*($G217*(Q217*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T217 > 0, $T217,($L217/2*($H217*(Q217*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T217 > 0, $T217, ( $L217 / 2 * ( ( $I217 ) * (Q217*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T218>0,$T218,($L218/2*(($F218*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T218>0,$T218,($L218/2*($G218*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T218>0,$T218,($L218/2*($H218*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T218 > 0, $T218, ( $L218 / 2 * ( ( $I218 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T218 > 0, $T218,($L218/2*(($F218)*(Q218*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T218 > 0, $T218,($L218/2*($G218*(Q218*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T218 > 0, $T218,($L218/2*($H218*(Q218*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T218 > 0, $T218, ( $L218 / 2 * ( ( $I218 ) * (Q218*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T219>0,$T219,($L219/2*(($F219*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T219>0,$T219,($L219/2*($G219*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T219>0,$T219,($L219/2*($H219*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T219 > 0, $T219, ( $L219 / 2 * ( ( $I219 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T219 > 0, $T219,($L219/2*(($F219)*(Q219*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T219 > 0, $T219,($L219/2*($G219*(Q219*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T219 > 0, $T219,($L219/2*($H219*(Q219*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T219 > 0, $T219, ( $L219 / 2 * ( ( $I219 ) * (Q219*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T220>0,$T220,($L220/2*(($F220*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T220>0,$T220,($L220/2*($G220*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T220>0,$T220,($L220/2*($H220*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T220 > 0, $T220, ( $L220 / 2 * ( ( $I220 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T220 > 0, $T220,($L220/2*(($F220)*(Q220*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T220 > 0, $T220,($L220/2*($G220*(Q220*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T220 > 0, $T220,($L220/2*($H220*(Q220*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T220 > 0, $T220, ( $L220 / 2 * ( ( $I220 ) * (Q220*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T221>0,$T221,($L221/2*(($F221*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T221>0,$T221,($L221/2*($G221*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T221>0,$T221,($L221/2*($H221*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T221 > 0, $T221, ( $L221 / 2 * ( ( $I221 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T221 > 0, $T221,($L221/2*(($F221)*(Q221*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T221 > 0, $T221,($L221/2*($G221*(Q221*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T221 > 0, $T221,($L221/2*($H221*(Q221*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T221 > 0, $T221, ( $L221 / 2 * ( ( $I221 ) * (Q221*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T222>0,$T222,($L222/2*(($F222*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T222>0,$T222,($L222/2*($G222*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T222>0,$T222,($L222/2*($H222*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T222 > 0, $T222, ( $L222 / 2 * ( ( $I222 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T222 > 0, $T222,($L222/2*(($F222)*(Q222*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T222 > 0, $T222,($L222/2*($G222*(Q222*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T222 > 0, $T222,($L222/2*($H222*(Q222*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T222 > 0, $T222, ( $L222 / 2 * ( ( $I222 ) * (Q222*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T223>0,$T223,($L223/2*(($F223*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T223>0,$T223,($L223/2*($G223*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T223>0,$T223,($L223/2*($H223*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T223 > 0, $T223, ( $L223 / 2 * ( ( $I223 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T223 > 0, $T223,($L223/2*(($F223)*(Q223*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T223 > 0, $T223,($L223/2*($G223*(Q223*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T223 > 0, $T223,($L223/2*($H223*(Q223*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T223 > 0, $T223, ( $L223 / 2 * ( ( $I223 ) * (Q223*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T224>0,$T224,($L224/2*(($F224*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T224>0,$T224,($L224/2*($G224*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T224>0,$T224,($L224/2*($H224*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T224 > 0, $T224, ( $L224 / 2 * ( ( $I224 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T224 > 0, $T224,($L224/2*(($F224)*(Q224*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T224 > 0, $T224,($L224/2*($G224*(Q224*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T224 > 0, $T224,($L224/2*($H224*(Q224*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T224 > 0, $T224, ( $L224 / 2 * ( ( $I224 ) * (Q224*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T225>0,$T225,($L225/2*(($F225*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T225>0,$T225,($L225/2*($G225*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T225>0,$T225,($L225/2*($H225*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T225 > 0, $T225, ( $L225 / 2 * ( ( $I225 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T225 > 0, $T225,($L225/2*(($F225)*(Q225*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T225 > 0, $T225,($L225/2*($G225*(Q225*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T225 > 0, $T225,($L225/2*($H225*(Q225*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T225 > 0, $T225, ( $L225 / 2 * ( ( $I225 ) * (Q225*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T226>0,$T226,($L226/2*(($F226*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T226>0,$T226,($L226/2*($G226*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T226>0,$T226,($L226/2*($H226*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T226 > 0, $T226, ( $L226 / 2 * ( ( $I226 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T226 > 0, $T226,($L226/2*(($F226)*(Q226*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T226 > 0, $T226,($L226/2*($G226*(Q226*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T226 > 0, $T226,($L226/2*($H226*(Q226*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T226 > 0, $T226, ( $L226 / 2 * ( ( $I226 ) * (Q226*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T227>0,$T227,($L227/2*(($F227*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T227>0,$T227,($L227/2*($G227*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T227>0,$T227,($L227/2*($H227*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T227 > 0, $T227, ( $L227 / 2 * ( ( $I227 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T227 > 0, $T227,($L227/2*(($F227)*(Q227*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T227 > 0, $T227,($L227/2*($G227*(Q227*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T227 > 0, $T227,($L227/2*($H227*(Q227*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T227 > 0, $T227, ( $L227 / 2 * ( ( $I227 ) * (Q227*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T228>0,$T228,($L228/2*(($F228*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T228>0,$T228,($L228/2*($G228*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T228>0,$T228,($L228/2*($H228*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T228 > 0, $T228, ( $L228 / 2 * ( ( $I228 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T228 > 0, $T228,($L228/2*(($F228)*(Q228*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T228 > 0, $T228,($L228/2*($G228*(Q228*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T228 > 0, $T228,($L228/2*($H228*(Q228*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T228 > 0, $T228, ( $L228 / 2 * ( ( $I228 ) * (Q228*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T229>0,$T229,($L229/2*(($F229*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T229>0,$T229,($L229/2*($G229*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T229>0,$T229,($L229/2*($H229*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T229 > 0, $T229, ( $L229 / 2 * ( ( $I229 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T229 > 0, $T229,($L229/2*(($F229)*(Q229*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T229 > 0, $T229,($L229/2*($G229*(Q229*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T229 > 0, $T229,($L229/2*($H229*(Q229*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T229 > 0, $T229, ( $L229 / 2 * ( ( $I229 ) * (Q229*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T230>0,$T230,($L230/2*(($F230*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T230>0,$T230,($L230/2*($G230*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T230>0,$T230,($L230/2*($H230*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T230 > 0, $T230, ( $L230 / 2 * ( ( $I230 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T230 > 0, $T230,($L230/2*(($F230)*(Q230*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T230 > 0, $T230,($L230/2*($G230*(Q230*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T230 > 0, $T230,($L230/2*($H230*(Q230*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T230 > 0, $T230, ( $L230 / 2 * ( ( $I230 ) * (Q230*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,{"$f":"OFFSET(FANOUT,8,1)+OFFSET(FANOUT,9,1)*($K231-3)","v":8.1363158974999991E-4},null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T231>0,$T231,($L231/2*(($F231*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T231>0,$T231,($L231/2*($G231*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T231>0,$T231,($L231/2*($H231*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T231 > 0, $T231, ( $L231 / 2 * ( ( $I231 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T231 > 0, $T231,($L231/2*(($F231)*(Q231*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T231 > 0, $T231,($L231/2*($G231*(Q231*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T231 > 0, $T231,($L231/2*($H231*(Q231*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T231 > 0, $T231, ( $L231 / 2 * ( ( $I231 ) * (Q231*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T232>0,$T232,($L232/2*(($F232*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T232>0,$T232,($L232/2*($G232*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T232>0,$T232,($L232/2*($H232*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T232 > 0, $T232, ( $L232 / 2 * ( ( $I232 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T232 > 0, $T232,($L232/2*(($F232)*(Q232*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T232 > 0, $T232,($L232/2*($G232*(Q232*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T232 > 0, $T232,($L232/2*($H232*(Q232*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T232 > 0, $T232, ( $L232 / 2 * ( ( $I232 ) * (Q232*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T233>0,$T233,($L233/2*(($F233*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T233>0,$T233,($L233/2*($G233*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T233>0,$T233,($L233/2*($H233*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T233 > 0, $T233, ( $L233 / 2 * ( ( $I233 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T233 > 0, $T233,($L233/2*(($F233)*(Q233*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T233 > 0, $T233,($L233/2*($G233*(Q233*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T233 > 0, $T233,($L233/2*($H233*(Q233*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T233 > 0, $T233, ( $L233 / 2 * ( ( $I233 ) * (Q233*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T234>0,$T234,($L234/2*(($F234*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T234>0,$T234,($L234/2*($G234*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T234>0,$T234,($L234/2*($H234*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T234 > 0, $T234, ( $L234 / 2 * ( ( $I234 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T234 > 0, $T234,($L234/2*(($F234)*(Q234*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T234 > 0, $T234,($L234/2*($G234*(Q234*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T234 > 0, $T234,($L234/2*($H234*(Q234*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T234 > 0, $T234, ( $L234 / 2 * ( ( $I234 ) * (Q234*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T235>0,$T235,($L235/2*(($F235*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T235>0,$T235,($L235/2*($G235*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T235>0,$T235,($L235/2*($H235*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T235 > 0, $T235, ( $L235 / 2 * ( ( $I235 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T235 > 0, $T235,($L235/2*(($F235)*(Q235*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T235 > 0, $T235,($L235/2*($G235*(Q235*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T235 > 0, $T235,($L235/2*($H235*(Q235*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T235 > 0, $T235, ( $L235 / 2 * ( ( $I235 ) * (Q235*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T236>0,$T236,($L236/2*(($F236*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T236>0,$T236,($L236/2*($G236*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T236>0,$T236,($L236/2*($H236*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T236 > 0, $T236, ( $L236 / 2 * ( ( $I236 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T236 > 0, $T236,($L236/2*(($F236)*(Q236*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T236 > 0, $T236,($L236/2*($G236*(Q236*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T236 > 0, $T236,($L236/2*($H236*(Q236*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T236 > 0, $T236, ( $L236 / 2 * ( ( $I236 ) * (Q236*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T237>0,$T237,($L237/2*(($F237*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T237>0,$T237,($L237/2*($G237*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T237>0,$T237,($L237/2*($H237*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T237 > 0, $T237, ( $L237 / 2 * ( ( $I237 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T237 > 0, $T237,($L237/2*(($F237)*(Q237*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T237 > 0, $T237,($L237/2*($G237*(Q237*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T237 > 0, $T237,($L237/2*($H237*(Q237*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T237 > 0, $T237, ( $L237 / 2 * ( ( $I237 ) * (Q237*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T238>0,$T238,($L238/2*(($F238*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T238>0,$T238,($L238/2*($G238*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T238>0,$T238,($L238/2*($H238*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T238 > 0, $T238, ( $L238 / 2 * ( ( $I238 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T238 > 0, $T238,($L238/2*(($F238)*(Q238*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T238 > 0, $T238,($L238/2*($G238*(Q238*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T238 > 0, $T238,($L238/2*($H238*(Q238*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T238 > 0, $T238, ( $L238 / 2 * ( ( $I238 ) * (Q238*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T239>0,$T239,($L239/2*(($F239*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T239>0,$T239,($L239/2*($G239*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T239>0,$T239,($L239/2*($H239*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T239 > 0, $T239, ( $L239 / 2 * ( ( $I239 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T239 > 0, $T239,($L239/2*(($F239)*(Q239*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T239 > 0, $T239,($L239/2*($G239*(Q239*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T239 > 0, $T239,($L239/2*($H239*(Q239*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T239 > 0, $T239, ( $L239 / 2 * ( ( $I239 ) * (Q239*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T240>0,$T240,($L240/2*(($F240*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T240>0,$T240,($L240/2*($G240*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T240>0,$T240,($L240/2*($H240*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T240 > 0, $T240, ( $L240 / 2 * ( ( $I240 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T240 > 0, $T240,($L240/2*(($F240)*(Q240*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T240 > 0, $T240,($L240/2*($G240*(Q240*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T240 > 0, $T240,($L240/2*($H240*(Q240*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T240 > 0, $T240, ( $L240 / 2 * ( ( $I240 ) * (Q240*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T241>0,$T241,($L241/2*(($F241*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T241>0,$T241,($L241/2*($G241*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T241>0,$T241,($L241/2*($H241*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T241 > 0, $T241, ( $L241 / 2 * ( ( $I241 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T241 > 0, $T241,($L241/2*(($F241)*(Q241*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T241 > 0, $T241,($L241/2*($G241*(Q241*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T241 > 0, $T241,($L241/2*($H241*(Q241*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T241 > 0, $T241, ( $L241 / 2 * ( ( $I241 ) * (Q241*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T242>0,$T242,($L242/2*(($F242*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T242>0,$T242,($L242/2*($G242*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T242>0,$T242,($L242/2*($H242*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T242 > 0, $T242, ( $L242 / 2 * ( ( $I242 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T242 > 0, $T242,($L242/2*(($F242)*(Q242*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T242 > 0, $T242,($L242/2*($G242*(Q242*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T242 > 0, $T242,($L242/2*($H242*(Q242*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T242 > 0, $T242, ( $L242 / 2 * ( ( $I242 ) * (Q242*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T243>0,$T243,($L243/2*(($F243*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T243>0,$T243,($L243/2*($G243*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T243>0,$T243,($L243/2*($H243*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T243 > 0, $T243, ( $L243 / 2 * ( ( $I243 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T243 > 0, $T243,($L243/2*(($F243)*(Q243*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T243 > 0, $T243,($L243/2*($G243*(Q243*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T243 > 0, $T243,($L243/2*($H243*(Q243*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T243 > 0, $T243, ( $L243 / 2 * ( ( $I243 ) * (Q243*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T244>0,$T244,($L244/2*(($F244*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T244>0,$T244,($L244/2*($G244*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T244>0,$T244,($L244/2*($H244*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T244 > 0, $T244, ( $L244 / 2 * ( ( $I244 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T244 > 0, $T244,($L244/2*(($F244)*(Q244*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T244 > 0, $T244,($L244/2*($G244*(Q244*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T244 > 0, $T244,($L244/2*($H244*(Q244*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T244 > 0, $T244, ( $L244 / 2 * ( ( $I244 ) * (Q244*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T245>0,$T245,($L245/2*(($F245*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T245>0,$T245,($L245/2*($G245*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T245>0,$T245,($L245/2*($H245*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T245 > 0, $T245, ( $L245 / 2 * ( ( $I245 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T245 > 0, $T245,($L245/2*(($F245)*(Q245*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T245 > 0, $T245,($L245/2*($G245*(Q245*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T245 > 0, $T245,($L245/2*($H245*(Q245*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T245 > 0, $T245, ( $L245 / 2 * ( ( $I245 ) * (Q245*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T246>0,$T246,($L246/2*(($F246*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T246>0,$T246,($L246/2*($G246*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T246>0,$T246,($L246/2*($H246*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T246 > 0, $T246, ( $L246 / 2 * ( ( $I246 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T246 > 0, $T246,($L246/2*(($F246)*(Q246*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T246 > 0, $T246,($L246/2*($G246*(Q246*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T246 > 0, $T246,($L246/2*($H246*(Q246*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T246 > 0, $T246, ( $L246 / 2 * ( ( $I246 ) * (Q246*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T247>0,$T247,($L247/2*(($F247*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T247>0,$T247,($L247/2*($G247*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T247>0,$T247,($L247/2*($H247*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T247 > 0, $T247, ( $L247 / 2 * ( ( $I247 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T247 > 0, $T247,($L247/2*(($F247)*(Q247*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T247 > 0, $T247,($L247/2*($G247*(Q247*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T247 > 0, $T247,($L247/2*($H247*(Q247*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T247 > 0, $T247, ( $L247 / 2 * ( ( $I247 ) * (Q247*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T248>0,$T248,($L248/2*(($F248*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T248>0,$T248,($L248/2*($G248*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T248>0,$T248,($L248/2*($H248*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T248 > 0, $T248, ( $L248 / 2 * ( ( $I248 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T248 > 0, $T248,($L248/2*(($F248)*(Q248*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T248 > 0, $T248,($L248/2*($G248*(Q248*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T248 > 0, $T248,($L248/2*($H248*(Q248*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T248 > 0, $T248, ( $L248 / 2 * ( ( $I248 ) * (Q248*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T249>0,$T249,($L249/2*(($F249*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T249>0,$T249,($L249/2*($G249*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T249>0,$T249,($L249/2*($H249*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T249 > 0, $T249, ( $L249 / 2 * ( ( $I249 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T249 > 0, $T249,($L249/2*(($F249)*(Q249*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T249 > 0, $T249,($L249/2*($G249*(Q249*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T249 > 0, $T249,($L249/2*($H249*(Q249*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T249 > 0, $T249, ( $L249 / 2 * ( ( $I249 ) * (Q249*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T250>0,$T250,($L250/2*(($F250*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T250>0,$T250,($L250/2*($G250*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T250>0,$T250,($L250/2*($H250*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T250 > 0, $T250, ( $L250 / 2 * ( ( $I250 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T250 > 0, $T250,($L250/2*(($F250)*(Q250*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T250 > 0, $T250,($L250/2*($G250*(Q250*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T250 > 0, $T250,($L250/2*($H250*(Q250*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T250 > 0, $T250, ( $L250 / 2 * ( ( $I250 ) * (Q250*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T251>0,$T251,($L251/2*(($F251*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T251>0,$T251,($L251/2*($G251*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T251>0,$T251,($L251/2*($H251*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T251 > 0, $T251, ( $L251 / 2 * ( ( $I251 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T251 > 0, $T251,($L251/2*(($F251)*(Q251*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T251 > 0, $T251,($L251/2*($G251*(Q251*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T251 > 0, $T251,($L251/2*($H251*(Q251*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T251 > 0, $T251, ( $L251 / 2 * ( ( $I251 ) * (Q251*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T252>0,$T252,($L252/2*(($F252*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T252>0,$T252,($L252/2*($G252*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T252>0,$T252,($L252/2*($H252*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T252 > 0, $T252, ( $L252 / 2 * ( ( $I252 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T252 > 0, $T252,($L252/2*(($F252)*(Q252*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T252 > 0, $T252,($L252/2*($G252*(Q252*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T252 > 0, $T252,($L252/2*($H252*(Q252*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T252 > 0, $T252, ( $L252 / 2 * ( ( $I252 ) * (Q252*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T253>0,$T253,($L253/2*(($F253*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T253>0,$T253,($L253/2*($G253*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T253>0,$T253,($L253/2*($H253*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T253 > 0, $T253, ( $L253 / 2 * ( ( $I253 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T253 > 0, $T253,($L253/2*(($F253)*(Q253*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T253 > 0, $T253,($L253/2*($G253*(Q253*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T253 > 0, $T253,($L253/2*($H253*(Q253*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T253 > 0, $T253, ( $L253 / 2 * ( ( $I253 ) * (Q253*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T254>0,$T254,($L254/2*(($F254*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T254>0,$T254,($L254/2*($G254*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T254>0,$T254,($L254/2*($H254*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T254 > 0, $T254, ( $L254 / 2 * ( ( $I254 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T254 > 0, $T254,($L254/2*(($F254)*(Q254*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T254 > 0, $T254,($L254/2*($G254*(Q254*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T254 > 0, $T254,($L254/2*($H254*(Q254*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T254 > 0, $T254, ( $L254 / 2 * ( ( $I254 ) * (Q254*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T255>0,$T255,($L255/2*(($F255*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T255>0,$T255,($L255/2*($G255*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T255>0,$T255,($L255/2*($H255*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T255 > 0, $T255, ( $L255 / 2 * ( ( $I255 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T255 > 0, $T255,($L255/2*(($F255)*(Q255*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T255 > 0, $T255,($L255/2*($G255*(Q255*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T255 > 0, $T255,($L255/2*($H255*(Q255*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T255 > 0, $T255, ( $L255 / 2 * ( ( $I255 ) * (Q255*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T256>0,$T256,($L256/2*(($F256*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T256>0,$T256,($L256/2*($G256*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T256>0,$T256,($L256/2*($H256*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T256 > 0, $T256, ( $L256 / 2 * ( ( $I256 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T256 > 0, $T256,($L256/2*(($F256)*(Q256*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T256 > 0, $T256,($L256/2*($G256*(Q256*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T256 > 0, $T256,($L256/2*($H256*(Q256*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T256 > 0, $T256, ( $L256 / 2 * ( ( $I256 ) * (Q256*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T257>0,$T257,($L257/2*(($F257*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T257>0,$T257,($L257/2*($G257*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T257>0,$T257,($L257/2*($H257*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T257 > 0, $T257, ( $L257 / 2 * ( ( $I257 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T257 > 0, $T257,($L257/2*(($F257)*(Q257*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T257 > 0, $T257,($L257/2*($G257*(Q257*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T257 > 0, $T257,($L257/2*($H257*(Q257*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T257 > 0, $T257, ( $L257 / 2 * ( ( $I257 ) * (Q257*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T258>0,$T258,($L258/2*(($F258*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T258>0,$T258,($L258/2*($G258*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T258>0,$T258,($L258/2*($H258*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T258 > 0, $T258, ( $L258 / 2 * ( ( $I258 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T258 > 0, $T258,($L258/2*(($F258)*(Q258*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T258 > 0, $T258,($L258/2*($G258*(Q258*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T258 > 0, $T258,($L258/2*($H258*(Q258*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T258 > 0, $T258, ( $L258 / 2 * ( ( $I258 ) * (Q258*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T259>0,$T259,($L259/2*(($F259*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T259>0,$T259,($L259/2*($G259*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T259>0,$T259,($L259/2*($H259*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T259 > 0, $T259, ( $L259 / 2 * ( ( $I259 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T259 > 0, $T259,($L259/2*(($F259)*(Q259*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T259 > 0, $T259,($L259/2*($G259*(Q259*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T259 > 0, $T259,($L259/2*($H259*(Q259*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T259 > 0, $T259, ( $L259 / 2 * ( ( $I259 ) * (Q259*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T260>0,$T260,($L260/2*(($F260*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T260>0,$T260,($L260/2*($G260*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T260>0,$T260,($L260/2*($H260*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T260 > 0, $T260, ( $L260 / 2 * ( ( $I260 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T260 > 0, $T260,($L260/2*(($F260)*(Q260*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T260 > 0, $T260,($L260/2*($G260*(Q260*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T260 > 0, $T260,($L260/2*($H260*(Q260*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T260 > 0, $T260, ( $L260 / 2 * ( ( $I260 ) * (Q260*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T261>0,$T261,($L261/2*(($F261*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T261>0,$T261,($L261/2*($G261*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T261>0,$T261,($L261/2*($H261*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T261 > 0, $T261, ( $L261 / 2 * ( ( $I261 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T261 > 0, $T261,($L261/2*(($F261)*(Q261*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T261 > 0, $T261,($L261/2*($G261*(Q261*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T261 > 0, $T261,($L261/2*($H261*(Q261*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T261 > 0, $T261, ( $L261 / 2 * ( ( $I261 ) * (Q261*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T262>0,$T262,($L262/2*(($F262*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T262>0,$T262,($L262/2*($G262*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T262>0,$T262,($L262/2*($H262*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T262 > 0, $T262, ( $L262 / 2 * ( ( $I262 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T262 > 0, $T262,($L262/2*(($F262)*(Q262*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T262 > 0, $T262,($L262/2*($G262*(Q262*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T262 > 0, $T262,($L262/2*($H262*(Q262*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T262 > 0, $T262, ( $L262 / 2 * ( ( $I262 ) * (Q262*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,{"$f":"OFFSET(FANOUT,8,1)+OFFSET(FANOUT,9,1)*($K263-3)","v":8.1363158974999991E-4},null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T263>0,$T263,($L263/2*(($F263*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T263>0,$T263,($L263/2*($G263*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T263>0,$T263,($L263/2*($H263*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T263 > 0, $T263, ( $L263 / 2 * ( ( $I263 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T263 > 0, $T263,($L263/2*(($F263)*(Q263*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T263 > 0, $T263,($L263/2*($G263*(Q263*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T263 > 0, $T263,($L263/2*($H263*(Q263*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T263 > 0, $T263, ( $L263 / 2 * ( ( $I263 ) * (Q263*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,{"$f":"E264*J264","v":0},0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T264>0,$T264,($L264/2*(($F264*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T264>0,$T264,($L264/2*($G264*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T264>0,$T264,($L264/2*($H264*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T264 > 0, $T264, ( $L264 / 2 * ( ( $I264 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T264 > 0, $T264,($L264/2*(($F264)*(Q264*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T264 > 0, $T264,($L264/2*($G264*(Q264*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T264 > 0, $T264,($L264/2*($H264*(Q264*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T264 > 0, $T264, ( $L264 / 2 * ( ( $I264 ) * (Q264*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T265>0,$T265,($L265/2*(($F265*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T265>0,$T265,($L265/2*($G265*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T265>0,$T265,($L265/2*($H265*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T265 > 0, $T265, ( $L265 / 2 * ( ( $I265 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T265 > 0, $T265,($L265/2*(($F265)*(Q265*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T265 > 0, $T265,($L265/2*($G265*(Q265*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T265 > 0, $T265,($L265/2*($H265*(Q265*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T265 > 0, $T265, ( $L265 / 2 * ( ( $I265 ) * (Q265*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T266>0,$T266,($L266/2*(($F266*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T266>0,$T266,($L266/2*($G266*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T266>0,$T266,($L266/2*($H266*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T266 > 0, $T266, ( $L266 / 2 * ( ( $I266 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T266 > 0, $T266,($L266/2*(($F266)*(Q266*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T266 > 0, $T266,($L266/2*($G266*(Q266*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T266 > 0, $T266,($L266/2*($H266*(Q266*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T266 > 0, $T266, ( $L266 / 2 * ( ( $I266 ) * (Q266*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T267>0,$T267,($L267/2*(($F267*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T267>0,$T267,($L267/2*($G267*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T267>0,$T267,($L267/2*($H267*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T267 > 0, $T267, ( $L267 / 2 * ( ( $I267 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T267 > 0, $T267,($L267/2*(($F267)*(Q267*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T267 > 0, $T267,($L267/2*($G267*(Q267*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T267 > 0, $T267,($L267/2*($H267*(Q267*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T267 > 0, $T267, ( $L267 / 2 * ( ( $I267 ) * (Q267*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,{"$f":"IF(TRUE,SUM(AE268:AF268),(VCCINT/1000)*VCCINT_N*IF($R268>0,$R268,($L268/2*(($F268+$I268)*0.45*$U268+($F268*(OFFSET(FANOUT,8,2))+$G268*(OFFSET(FANOUT,8,4)+$U268)+$H268*(OFFSET(FANOUT,8,5)+$U268)+$I268*(OFFSET(FANOUT,8,3)))))*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1)","v":0},null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T268>0,$T268,($L268/2*(($F268*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T268>0,$T268,($L268/2*($G268*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T268>0,$T268,($L268/2*($H268*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T268 > 0, $T268, ( $L268 / 2 * ( ( $I268 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T268 > 0, $T268,($L268/2*(($F268)*(Q268*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T268 > 0, $T268,($L268/2*($G268*(Q268*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T268 > 0, $T268,($L268/2*($H268*(Q268*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T268 > 0, $T268, ( $L268 / 2 * ( ( $I268 ) * (Q268*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,{"$f":"10^(K269/10)-1","v":5.3095734448019343},null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T269>0,$T269,($L269/2*(($F269*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T269>0,$T269,($L269/2*($G269*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T269>0,$T269,($L269/2*($H269*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T269 > 0, $T269, ( $L269 / 2 * ( ( $I269 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T269 > 0, $T269,($L269/2*(($F269)*(Q269*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T269 > 0, $T269,($L269/2*($G269*(Q269*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T269 > 0, $T269,($L269/2*($H269*(Q269*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T269 > 0, $T269, ( $L269 / 2 * ( ( $I269 ) * (Q269*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"SUM(W269:Z269)","v":0},{"$f":"SUM(AA269:AD269)","v":0}]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T270>0,$T270,($L270/2*(($F270*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T270>0,$T270,($L270/2*($G270*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T270>0,$T270,($L270/2*($H270*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T270 > 0, $T270, ( $L270 / 2 * ( ( $I270 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T270 > 0, $T270,($L270/2*(($F270)*(Q270*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T270 > 0, $T270,($L270/2*($G270*(Q270*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T270 > 0, $T270,($L270/2*($H270*(Q270*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T270 > 0, $T270, ( $L270 / 2 * ( ( $I270 ) * (Q270*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T271>0,$T271,($L271/2*(($F271*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T271>0,$T271,($L271/2*($G271*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T271>0,$T271,($L271/2*($H271*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T271 > 0, $T271, ( $L271 / 2 * ( ( $I271 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T271 > 0, $T271,($L271/2*(($F271)*(Q271*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T271 > 0, $T271,($L271/2*($G271*(Q271*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T271 > 0, $T271,($L271/2*($H271*(Q271*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T271 > 0, $T271, ( $L271 / 2 * ( ( $I271 ) * (Q271*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T272>0,$T272,($L272/2*(($F272*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T272>0,$T272,($L272/2*($G272*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T272>0,$T272,($L272/2*($H272*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T272 > 0, $T272, ( $L272 / 2 * ( ( $I272 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T272 > 0, $T272,($L272/2*(($F272)*(Q272*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T272 > 0, $T272,($L272/2*($G272*(Q272*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T272 > 0, $T272,($L272/2*($H272*(Q272*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T272 > 0, $T272, ( $L272 / 2 * ( ( $I272 ) * (Q272*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T273>0,$T273,($L273/2*(($F273*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T273>0,$T273,($L273/2*($G273*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T273>0,$T273,($L273/2*($H273*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T273 > 0, $T273, ( $L273 / 2 * ( ( $I273 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T273 > 0, $T273,($L273/2*(($F273)*(Q273*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T273 > 0, $T273,($L273/2*($G273*(Q273*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T273 > 0, $T273,($L273/2*($H273*(Q273*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T273 > 0, $T273, ( $L273 / 2 * ( ( $I273 ) * (Q273*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T274>0,$T274,($L274/2*(($F274*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T274>0,$T274,($L274/2*($G274*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T274>0,$T274,($L274/2*($H274*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T274 > 0, $T274, ( $L274 / 2 * ( ( $I274 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T274 > 0, $T274,($L274/2*(($F274)*(Q274*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T274 > 0, $T274,($L274/2*($G274*(Q274*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T274 > 0, $T274,($L274/2*($H274*(Q274*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T274 > 0, $T274, ( $L274 / 2 * ( ( $I274 ) * (Q274*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T275>0,$T275,($L275/2*(($F275*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T275>0,$T275,($L275/2*($G275*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T275>0,$T275,($L275/2*($H275*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T275 > 0, $T275, ( $L275 / 2 * ( ( $I275 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T275 > 0, $T275,($L275/2*(($F275)*(Q275*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T275 > 0, $T275,($L275/2*($G275*(Q275*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T275 > 0, $T275,($L275/2*($H275*(Q275*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T275 > 0, $T275, ( $L275 / 2 * ( ( $I275 ) * (Q275*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T276>0,$T276,($L276/2*(($F276*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T276>0,$T276,($L276/2*($G276*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T276>0,$T276,($L276/2*($H276*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T276 > 0, $T276, ( $L276 / 2 * ( ( $I276 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T276 > 0, $T276,($L276/2*(($F276)*(Q276*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T276 > 0, $T276,($L276/2*($G276*(Q276*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T276 > 0, $T276,($L276/2*($H276*(Q276*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T276 > 0, $T276, ( $L276 / 2 * ( ( $I276 ) * (Q276*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T277>0,$T277,($L277/2*(($F277*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T277>0,$T277,($L277/2*($G277*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T277>0,$T277,($L277/2*($H277*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T277 > 0, $T277, ( $L277 / 2 * ( ( $I277 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T277 > 0, $T277,($L277/2*(($F277)*(Q277*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T277 > 0, $T277,($L277/2*($G277*(Q277*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T277 > 0, $T277,($L277/2*($H277*(Q277*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T277 > 0, $T277, ( $L277 / 2 * ( ( $I277 ) * (Q277*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T278>0,$T278,($L278/2*(($F278*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T278>0,$T278,($L278/2*($G278*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T278>0,$T278,($L278/2*($H278*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T278 > 0, $T278, ( $L278 / 2 * ( ( $I278 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T278 > 0, $T278,($L278/2*(($F278)*(Q278*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T278 > 0, $T278,($L278/2*($G278*(Q278*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T278 > 0, $T278,($L278/2*($H278*(Q278*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T278 > 0, $T278, ( $L278 / 2 * ( ( $I278 ) * (Q278*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T279>0,$T279,($L279/2*(($F279*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T279>0,$T279,($L279/2*($G279*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T279>0,$T279,($L279/2*($H279*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T279 > 0, $T279, ( $L279 / 2 * ( ( $I279 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T279 > 0, $T279,($L279/2*(($F279)*(Q279*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T279 > 0, $T279,($L279/2*($G279*(Q279*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T279 > 0, $T279,($L279/2*($H279*(Q279*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T279 > 0, $T279, ( $L279 / 2 * ( ( $I279 ) * (Q279*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T280>0,$T280,($L280/2*(($F280*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T280>0,$T280,($L280/2*($G280*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T280>0,$T280,($L280/2*($H280*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T280 > 0, $T280, ( $L280 / 2 * ( ( $I280 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T280 > 0, $T280,($L280/2*(($F280)*(Q280*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T280 > 0, $T280,($L280/2*($G280*(Q280*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T280 > 0, $T280,($L280/2*($H280*(Q280*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T280 > 0, $T280, ( $L280 / 2 * ( ( $I280 ) * (Q280*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T281>0,$T281,($L281/2*(($F281*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T281>0,$T281,($L281/2*($G281*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T281>0,$T281,($L281/2*($H281*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T281 > 0, $T281, ( $L281 / 2 * ( ( $I281 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T281 > 0, $T281,($L281/2*(($F281)*(Q281*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T281 > 0, $T281,($L281/2*($G281*(Q281*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T281 > 0, $T281,($L281/2*($H281*(Q281*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T281 > 0, $T281, ( $L281 / 2 * ( ( $I281 ) * (Q281*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T282>0,$T282,($L282/2*(($F282*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T282>0,$T282,($L282/2*($G282*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T282>0,$T282,($L282/2*($H282*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T282 > 0, $T282, ( $L282 / 2 * ( ( $I282 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T282 > 0, $T282,($L282/2*(($F282)*(Q282*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T282 > 0, $T282,($L282/2*($G282*(Q282*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T282 > 0, $T282,($L282/2*($H282*(Q282*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T282 > 0, $T282, ( $L282 / 2 * ( ( $I282 ) * (Q282*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T283>0,$T283,($L283/2*(($F283*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T283>0,$T283,($L283/2*($G283*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T283>0,$T283,($L283/2*($H283*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T283 > 0, $T283, ( $L283 / 2 * ( ( $I283 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T283 > 0, $T283,($L283/2*(($F283)*(Q283*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T283 > 0, $T283,($L283/2*($G283*(Q283*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T283 > 0, $T283,($L283/2*($H283*(Q283*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T283 > 0, $T283, ( $L283 / 2 * ( ( $I283 ) * (Q283*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T284>0,$T284,($L284/2*(($F284*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T284>0,$T284,($L284/2*($G284*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T284>0,$T284,($L284/2*($H284*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T284 > 0, $T284, ( $L284 / 2 * ( ( $I284 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T284 > 0, $T284,($L284/2*(($F284)*(Q284*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T284 > 0, $T284,($L284/2*($G284*(Q284*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T284 > 0, $T284,($L284/2*($H284*(Q284*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T284 > 0, $T284, ( $L284 / 2 * ( ( $I284 ) * (Q284*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T285>0,$T285,($L285/2*(($F285*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T285>0,$T285,($L285/2*($G285*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T285>0,$T285,($L285/2*($H285*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T285 > 0, $T285, ( $L285 / 2 * ( ( $I285 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T285 > 0, $T285,($L285/2*(($F285)*(Q285*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T285 > 0, $T285,($L285/2*($G285*(Q285*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T285 > 0, $T285,($L285/2*($H285*(Q285*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T285 > 0, $T285, ( $L285 / 2 * ( ( $I285 ) * (Q285*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T286>0,$T286,($L286/2*(($F286*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T286>0,$T286,($L286/2*($G286*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T286>0,$T286,($L286/2*($H286*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T286 > 0, $T286, ( $L286 / 2 * ( ( $I286 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T286 > 0, $T286,($L286/2*(($F286)*(Q286*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T286 > 0, $T286,($L286/2*($G286*(Q286*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T286 > 0, $T286,($L286/2*($H286*(Q286*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T286 > 0, $T286, ( $L286 / 2 * ( ( $I286 ) * (Q286*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T287>0,$T287,($L287/2*(($F287*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T287>0,$T287,($L287/2*($G287*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T287>0,$T287,($L287/2*($H287*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T287 > 0, $T287, ( $L287 / 2 * ( ( $I287 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T287 > 0, $T287,($L287/2*(($F287)*(Q287*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T287 > 0, $T287,($L287/2*($G287*(Q287*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T287 > 0, $T287,($L287/2*($H287*(Q287*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T287 > 0, $T287, ( $L287 / 2 * ( ( $I287 ) * (Q287*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T288>0,$T288,($L288/2*(($F288*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T288>0,$T288,($L288/2*($G288*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T288>0,$T288,($L288/2*($H288*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T288 > 0, $T288, ( $L288 / 2 * ( ( $I288 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T288 > 0, $T288,($L288/2*(($F288)*(Q288*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T288 > 0, $T288,($L288/2*($G288*(Q288*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T288 > 0, $T288,($L288/2*($H288*(Q288*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T288 > 0, $T288, ( $L288 / 2 * ( ( $I288 ) * (Q288*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T289>0,$T289,($L289/2*(($F289*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T289>0,$T289,($L289/2*($G289*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T289>0,$T289,($L289/2*($H289*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T289 > 0, $T289, ( $L289 / 2 * ( ( $I289 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T289 > 0, $T289,($L289/2*(($F289)*(Q289*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T289 > 0, $T289,($L289/2*($G289*(Q289*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T289 > 0, $T289,($L289/2*($H289*(Q289*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T289 > 0, $T289, ( $L289 / 2 * ( ( $I289 ) * (Q289*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T290>0,$T290,($L290/2*(($F290*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T290>0,$T290,($L290/2*($G290*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T290>0,$T290,($L290/2*($H290*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T290 > 0, $T290, ( $L290 / 2 * ( ( $I290 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T290 > 0, $T290,($L290/2*(($F290)*(Q290*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T290 > 0, $T290,($L290/2*($G290*(Q290*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T290 > 0, $T290,($L290/2*($H290*(Q290*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T290 > 0, $T290, ( $L290 / 2 * ( ( $I290 ) * (Q290*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T291>0,$T291,($L291/2*(($F291*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T291>0,$T291,($L291/2*($G291*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T291>0,$T291,($L291/2*($H291*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T291 > 0, $T291, ( $L291 / 2 * ( ( $I291 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T291 > 0, $T291,($L291/2*(($F291)*(Q291*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T291 > 0, $T291,($L291/2*($G291*(Q291*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T291 > 0, $T291,($L291/2*($H291*(Q291*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T291 > 0, $T291, ( $L291 / 2 * ( ( $I291 ) * (Q291*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T292>0,$T292,($L292/2*(($F292*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T292>0,$T292,($L292/2*($G292*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T292>0,$T292,($L292/2*($H292*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T292 > 0, $T292, ( $L292 / 2 * ( ( $I292 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T292 > 0, $T292,($L292/2*(($F292)*(Q292*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T292 > 0, $T292,($L292/2*($G292*(Q292*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T292 > 0, $T292,($L292/2*($H292*(Q292*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T292 > 0, $T292, ( $L292 / 2 * ( ( $I292 ) * (Q292*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T293>0,$T293,($L293/2*(($F293*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T293>0,$T293,($L293/2*($G293*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T293>0,$T293,($L293/2*($H293*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T293 > 0, $T293, ( $L293 / 2 * ( ( $I293 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T293 > 0, $T293,($L293/2*(($F293)*(Q293*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T293 > 0, $T293,($L293/2*($G293*(Q293*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T293 > 0, $T293,($L293/2*($H293*(Q293*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T293 > 0, $T293, ( $L293 / 2 * ( ( $I293 ) * (Q293*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T294>0,$T294,($L294/2*(($F294*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T294>0,$T294,($L294/2*($G294*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T294>0,$T294,($L294/2*($H294*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T294 > 0, $T294, ( $L294 / 2 * ( ( $I294 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T294 > 0, $T294,($L294/2*(($F294)*(Q294*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T294 > 0, $T294,($L294/2*($G294*(Q294*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T294 > 0, $T294,($L294/2*($H294*(Q294*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T294 > 0, $T294, ( $L294 / 2 * ( ( $I294 ) * (Q294*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,{"$f":"OFFSET(FANOUT,8,1)+OFFSET(FANOUT,9,1)*($K295-3)","v":8.1363158974999991E-4},null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T295>0,$T295,($L295/2*(($F295*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T295>0,$T295,($L295/2*($G295*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T295>0,$T295,($L295/2*($H295*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T295 > 0, $T295, ( $L295 / 2 * ( ( $I295 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T295 > 0, $T295,($L295/2*(($F295)*(Q295*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T295 > 0, $T295,($L295/2*($G295*(Q295*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T295 > 0, $T295,($L295/2*($H295*(Q295*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T295 > 0, $T295, ( $L295 / 2 * ( ( $I295 ) * (Q295*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T296>0,$T296,($L296/2*(($F296*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T296>0,$T296,($L296/2*($G296*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T296>0,$T296,($L296/2*($H296*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T296 > 0, $T296, ( $L296 / 2 * ( ( $I296 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T296 > 0, $T296,($L296/2*(($F296)*(Q296*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T296 > 0, $T296,($L296/2*($G296*(Q296*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T296 > 0, $T296,($L296/2*($H296*(Q296*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T296 > 0, $T296, ( $L296 / 2 * ( ( $I296 ) * (Q296*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T297>0,$T297,($L297/2*(($F297*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T297>0,$T297,($L297/2*($G297*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T297>0,$T297,($L297/2*($H297*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T297 > 0, $T297, ( $L297 / 2 * ( ( $I297 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T297 > 0, $T297,($L297/2*(($F297)*(Q297*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T297 > 0, $T297,($L297/2*($G297*(Q297*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T297 > 0, $T297,($L297/2*($H297*(Q297*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T297 > 0, $T297, ( $L297 / 2 * ( ( $I297 ) * (Q297*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T298>0,$T298,($L298/2*(($F298*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T298>0,$T298,($L298/2*($G298*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T298>0,$T298,($L298/2*($H298*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T298 > 0, $T298, ( $L298 / 2 * ( ( $I298 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T298 > 0, $T298,($L298/2*(($F298)*(Q298*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T298 > 0, $T298,($L298/2*($G298*(Q298*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T298 > 0, $T298,($L298/2*($H298*(Q298*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T298 > 0, $T298, ( $L298 / 2 * ( ( $I298 ) * (Q298*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T299>0,$T299,($L299/2*(($F299*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T299>0,$T299,($L299/2*($G299*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T299>0,$T299,($L299/2*($H299*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T299 > 0, $T299, ( $L299 / 2 * ( ( $I299 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T299 > 0, $T299,($L299/2*(($F299)*(Q299*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T299 > 0, $T299,($L299/2*($G299*(Q299*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T299 > 0, $T299,($L299/2*($H299*(Q299*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T299 > 0, $T299, ( $L299 / 2 * ( ( $I299 ) * (Q299*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T300>0,$T300,($L300/2*(($F300*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T300>0,$T300,($L300/2*($G300*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T300>0,$T300,($L300/2*($H300*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T300 > 0, $T300, ( $L300 / 2 * ( ( $I300 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T300 > 0, $T300,($L300/2*(($F300)*(Q300*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T300 > 0, $T300,($L300/2*($G300*(Q300*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T300 > 0, $T300,($L300/2*($H300*(Q300*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T300 > 0, $T300, ( $L300 / 2 * ( ( $I300 ) * (Q300*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T301>0,$T301,($L301/2*(($F301*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T301>0,$T301,($L301/2*($G301*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T301>0,$T301,($L301/2*($H301*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T301 > 0, $T301, ( $L301 / 2 * ( ( $I301 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T301 > 0, $T301,($L301/2*(($F301)*(Q301*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T301 > 0, $T301,($L301/2*($G301*(Q301*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T301 > 0, $T301,($L301/2*($H301*(Q301*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T301 > 0, $T301, ( $L301 / 2 * ( ( $I301 ) * (Q301*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T302>0,$T302,($L302/2*(($F302*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T302>0,$T302,($L302/2*($G302*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T302>0,$T302,($L302/2*($H302*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T302 > 0, $T302, ( $L302 / 2 * ( ( $I302 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T302 > 0, $T302,($L302/2*(($F302)*(Q302*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T302 > 0, $T302,($L302/2*($G302*(Q302*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T302 > 0, $T302,($L302/2*($H302*(Q302*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T302 > 0, $T302, ( $L302 / 2 * ( ( $I302 ) * (Q302*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T303>0,$T303,($L303/2*(($F303*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T303>0,$T303,($L303/2*($G303*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T303>0,$T303,($L303/2*($H303*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T303 > 0, $T303, ( $L303 / 2 * ( ( $I303 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T303 > 0, $T303,($L303/2*(($F303)*(Q303*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T303 > 0, $T303,($L303/2*($G303*(Q303*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T303 > 0, $T303,($L303/2*($H303*(Q303*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T303 > 0, $T303, ( $L303 / 2 * ( ( $I303 ) * (Q303*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T304>0,$T304,($L304/2*(($F304*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T304>0,$T304,($L304/2*($G304*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T304>0,$T304,($L304/2*($H304*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T304 > 0, $T304, ( $L304 / 2 * ( ( $I304 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T304 > 0, $T304,($L304/2*(($F304)*(Q304*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T304 > 0, $T304,($L304/2*($G304*(Q304*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T304 > 0, $T304,($L304/2*($H304*(Q304*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T304 > 0, $T304, ( $L304 / 2 * ( ( $I304 ) * (Q304*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,{"$f":"E305*J305","v":0},0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T305>0,$T305,($L305/2*(($F305*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T305>0,$T305,($L305/2*($G305*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T305>0,$T305,($L305/2*($H305*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T305 > 0, $T305, ( $L305 / 2 * ( ( $I305 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T305 > 0, $T305,($L305/2*(($F305)*(Q305*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T305 > 0, $T305,($L305/2*($G305*(Q305*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T305 > 0, $T305,($L305/2*($H305*(Q305*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T305 > 0, $T305, ( $L305 / 2 * ( ( $I305 ) * (Q305*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T306>0,$T306,($L306/2*(($F306*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T306>0,$T306,($L306/2*($G306*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T306>0,$T306,($L306/2*($H306*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T306 > 0, $T306, ( $L306 / 2 * ( ( $I306 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T306 > 0, $T306,($L306/2*(($F306)*(Q306*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T306 > 0, $T306,($L306/2*($G306*(Q306*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T306 > 0, $T306,($L306/2*($H306*(Q306*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T306 > 0, $T306, ( $L306 / 2 * ( ( $I306 ) * (Q306*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T307>0,$T307,($L307/2*(($F307*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T307>0,$T307,($L307/2*($G307*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T307>0,$T307,($L307/2*($H307*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T307 > 0, $T307, ( $L307 / 2 * ( ( $I307 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T307 > 0, $T307,($L307/2*(($F307)*(Q307*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T307 > 0, $T307,($L307/2*($G307*(Q307*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T307 > 0, $T307,($L307/2*($H307*(Q307*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T307 > 0, $T307, ( $L307 / 2 * ( ( $I307 ) * (Q307*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T308>0,$T308,($L308/2*(($F308*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T308>0,$T308,($L308/2*($G308*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T308>0,$T308,($L308/2*($H308*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T308 > 0, $T308, ( $L308 / 2 * ( ( $I308 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T308 > 0, $T308,($L308/2*(($F308)*(Q308*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T308 > 0, $T308,($L308/2*($G308*(Q308*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T308 > 0, $T308,($L308/2*($H308*(Q308*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T308 > 0, $T308, ( $L308 / 2 * ( ( $I308 ) * (Q308*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T309>0,$T309,($L309/2*(($F309*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T309>0,$T309,($L309/2*($G309*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T309>0,$T309,($L309/2*($H309*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T309 > 0, $T309, ( $L309 / 2 * ( ( $I309 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T309 > 0, $T309,($L309/2*(($F309)*(Q309*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T309 > 0, $T309,($L309/2*($G309*(Q309*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T309 > 0, $T309,($L309/2*($H309*(Q309*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T309 > 0, $T309, ( $L309 / 2 * ( ( $I309 ) * (Q309*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T310>0,$T310,($L310/2*(($F310*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T310>0,$T310,($L310/2*($G310*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T310>0,$T310,($L310/2*($H310*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T310 > 0, $T310, ( $L310 / 2 * ( ( $I310 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T310 > 0, $T310,($L310/2*(($F310)*(Q310*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T310 > 0, $T310,($L310/2*($G310*(Q310*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T310 > 0, $T310,($L310/2*($H310*(Q310*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T310 > 0, $T310, ( $L310 / 2 * ( ( $I310 ) * (Q310*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T311>0,$T311,($L311/2*(($F311*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T311>0,$T311,($L311/2*($G311*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T311>0,$T311,($L311/2*($H311*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T311 > 0, $T311, ( $L311 / 2 * ( ( $I311 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T311 > 0, $T311,($L311/2*(($F311)*(Q311*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T311 > 0, $T311,($L311/2*($G311*(Q311*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T311 > 0, $T311,($L311/2*($H311*(Q311*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T311 > 0, $T311, ( $L311 / 2 * ( ( $I311 ) * (Q311*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T312>0,$T312,($L312/2*(($F312*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T312>0,$T312,($L312/2*($G312*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T312>0,$T312,($L312/2*($H312*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T312 > 0, $T312, ( $L312 / 2 * ( ( $I312 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T312 > 0, $T312,($L312/2*(($F312)*(Q312*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T312 > 0, $T312,($L312/2*($G312*(Q312*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T312 > 0, $T312,($L312/2*($H312*(Q312*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T312 > 0, $T312, ( $L312 / 2 * ( ( $I312 ) * (Q312*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T313>0,$T313,($L313/2*(($F313*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T313>0,$T313,($L313/2*($G313*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T313>0,$T313,($L313/2*($H313*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T313 > 0, $T313, ( $L313 / 2 * ( ( $I313 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T313 > 0, $T313,($L313/2*(($F313)*(Q313*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T313 > 0, $T313,($L313/2*($G313*(Q313*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T313 > 0, $T313,($L313/2*($H313*(Q313*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T313 > 0, $T313, ( $L313 / 2 * ( ( $I313 ) * (Q313*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T314>0,$T314,($L314/2*(($F314*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T314>0,$T314,($L314/2*($G314*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T314>0,$T314,($L314/2*($H314*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T314 > 0, $T314, ( $L314 / 2 * ( ( $I314 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T314 > 0, $T314,($L314/2*(($F314)*(Q314*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T314 > 0, $T314,($L314/2*($G314*(Q314*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T314 > 0, $T314,($L314/2*($H314*(Q314*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T314 > 0, $T314, ( $L314 / 2 * ( ( $I314 ) * (Q314*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T315>0,$T315,($L315/2*(($F315*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T315>0,$T315,($L315/2*($G315*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T315>0,$T315,($L315/2*($H315*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T315 > 0, $T315, ( $L315 / 2 * ( ( $I315 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T315 > 0, $T315,($L315/2*(($F315)*(Q315*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T315 > 0, $T315,($L315/2*($G315*(Q315*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T315 > 0, $T315,($L315/2*($H315*(Q315*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T315 > 0, $T315, ( $L315 / 2 * ( ( $I315 ) * (Q315*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T316>0,$T316,($L316/2*(($F316*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T316>0,$T316,($L316/2*($G316*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T316>0,$T316,($L316/2*($H316*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T316 > 0, $T316, ( $L316 / 2 * ( ( $I316 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T316 > 0, $T316,($L316/2*(($F316)*(Q316*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T316 > 0, $T316,($L316/2*($G316*(Q316*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T316 > 0, $T316,($L316/2*($H316*(Q316*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T316 > 0, $T316, ( $L316 / 2 * ( ( $I316 ) * (Q316*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T317>0,$T317,($L317/2*(($F317*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T317>0,$T317,($L317/2*($G317*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T317>0,$T317,($L317/2*($H317*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T317 > 0, $T317, ( $L317 / 2 * ( ( $I317 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T317 > 0, $T317,($L317/2*(($F317)*(Q317*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T317 > 0, $T317,($L317/2*($G317*(Q317*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T317 > 0, $T317,($L317/2*($H317*(Q317*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T317 > 0, $T317, ( $L317 / 2 * ( ( $I317 ) * (Q317*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T318>0,$T318,($L318/2*(($F318*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T318>0,$T318,($L318/2*($G318*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T318>0,$T318,($L318/2*($H318*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T318 > 0, $T318, ( $L318 / 2 * ( ( $I318 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T318 > 0, $T318,($L318/2*(($F318)*(Q318*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T318 > 0, $T318,($L318/2*($G318*(Q318*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T318 > 0, $T318,($L318/2*($H318*(Q318*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T318 > 0, $T318, ( $L318 / 2 * ( ( $I318 ) * (Q318*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T319>0,$T319,($L319/2*(($F319*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T319>0,$T319,($L319/2*($G319*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T319>0,$T319,($L319/2*($H319*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T319 > 0, $T319, ( $L319 / 2 * ( ( $I319 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T319 > 0, $T319,($L319/2*(($F319)*(Q319*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T319 > 0, $T319,($L319/2*($G319*(Q319*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T319 > 0, $T319,($L319/2*($H319*(Q319*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T319 > 0, $T319, ( $L319 / 2 * ( ( $I319 ) * (Q319*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T320>0,$T320,($L320/2*(($F320*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T320>0,$T320,($L320/2*($G320*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T320>0,$T320,($L320/2*($H320*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T320 > 0, $T320, ( $L320 / 2 * ( ( $I320 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T320 > 0, $T320,($L320/2*(($F320)*(Q320*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T320 > 0, $T320,($L320/2*($G320*(Q320*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T320 > 0, $T320,($L320/2*($H320*(Q320*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T320 > 0, $T320, ( $L320 / 2 * ( ( $I320 ) * (Q320*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T321>0,$T321,($L321/2*(($F321*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T321>0,$T321,($L321/2*($G321*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T321>0,$T321,($L321/2*($H321*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T321 > 0, $T321, ( $L321 / 2 * ( ( $I321 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T321 > 0, $T321,($L321/2*(($F321)*(Q321*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T321 > 0, $T321,($L321/2*($G321*(Q321*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T321 > 0, $T321,($L321/2*($H321*(Q321*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T321 > 0, $T321, ( $L321 / 2 * ( ( $I321 ) * (Q321*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T322>0,$T322,($L322/2*(($F322*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T322>0,$T322,($L322/2*($G322*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T322>0,$T322,($L322/2*($H322*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T322 > 0, $T322, ( $L322 / 2 * ( ( $I322 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T322 > 0, $T322,($L322/2*(($F322)*(Q322*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T322 > 0, $T322,($L322/2*($G322*(Q322*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T322 > 0, $T322,($L322/2*($H322*(Q322*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T322 > 0, $T322, ( $L322 / 2 * ( ( $I322 ) * (Q322*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T323>0,$T323,($L323/2*(($F323*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T323>0,$T323,($L323/2*($G323*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T323>0,$T323,($L323/2*($H323*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T323 > 0, $T323, ( $L323 / 2 * ( ( $I323 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T323 > 0, $T323,($L323/2*(($F323)*(Q323*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T323 > 0, $T323,($L323/2*($G323*(Q323*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T323 > 0, $T323,($L323/2*($H323*(Q323*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T323 > 0, $T323, ( $L323 / 2 * ( ( $I323 ) * (Q323*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T324>0,$T324,($L324/2*(($F324*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T324>0,$T324,($L324/2*($G324*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T324>0,$T324,($L324/2*($H324*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T324 > 0, $T324, ( $L324 / 2 * ( ( $I324 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T324 > 0, $T324,($L324/2*(($F324)*(Q324*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T324 > 0, $T324,($L324/2*($G324*(Q324*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T324 > 0, $T324,($L324/2*($H324*(Q324*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T324 > 0, $T324, ( $L324 / 2 * ( ( $I324 ) * (Q324*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T325>0,$T325,($L325/2*(($F325*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T325>0,$T325,($L325/2*($G325*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T325>0,$T325,($L325/2*($H325*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T325 > 0, $T325, ( $L325 / 2 * ( ( $I325 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T325 > 0, $T325,($L325/2*(($F325)*(Q325*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T325 > 0, $T325,($L325/2*($G325*(Q325*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T325 > 0, $T325,($L325/2*($H325*(Q325*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T325 > 0, $T325, ( $L325 / 2 * ( ( $I325 ) * (Q325*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T326>0,$T326,($L326/2*(($F326*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T326>0,$T326,($L326/2*($G326*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T326>0,$T326,($L326/2*($H326*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T326 > 0, $T326, ( $L326 / 2 * ( ( $I326 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T326 > 0, $T326,($L326/2*(($F326)*(Q326*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T326 > 0, $T326,($L326/2*($G326*(Q326*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T326 > 0, $T326,($L326/2*($H326*(Q326*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T326 > 0, $T326, ( $L326 / 2 * ( ( $I326 ) * (Q326*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T327>0,$T327,($L327/2*(($F327*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T327>0,$T327,($L327/2*($G327*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T327>0,$T327,($L327/2*($H327*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T327 > 0, $T327, ( $L327 / 2 * ( ( $I327 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T327 > 0, $T327,($L327/2*(($F327)*(Q327*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T327 > 0, $T327,($L327/2*($G327*(Q327*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T327 > 0, $T327,($L327/2*($H327*(Q327*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T327 > 0, $T327, ( $L327 / 2 * ( ( $I327 ) * (Q327*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T328>0,$T328,($L328/2*(($F328*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T328>0,$T328,($L328/2*($G328*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T328>0,$T328,($L328/2*($H328*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T328 > 0, $T328, ( $L328 / 2 * ( ( $I328 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T328 > 0, $T328,($L328/2*(($F328)*(Q328*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T328 > 0, $T328,($L328/2*($G328*(Q328*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T328 > 0, $T328,($L328/2*($H328*(Q328*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T328 > 0, $T328, ( $L328 / 2 * ( ( $I328 ) * (Q328*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T329>0,$T329,($L329/2*(($F329*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T329>0,$T329,($L329/2*($G329*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T329>0,$T329,($L329/2*($H329*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T329 > 0, $T329, ( $L329 / 2 * ( ( $I329 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T329 > 0, $T329,($L329/2*(($F329)*(Q329*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T329 > 0, $T329,($L329/2*($G329*(Q329*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T329 > 0, $T329,($L329/2*($H329*(Q329*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T329 > 0, $T329, ( $L329 / 2 * ( ( $I329 ) * (Q329*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T330>0,$T330,($L330/2*(($F330*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T330>0,$T330,($L330/2*($G330*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T330>0,$T330,($L330/2*($H330*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T330 > 0, $T330, ( $L330 / 2 * ( ( $I330 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T330 > 0, $T330,($L330/2*(($F330)*(Q330*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T330 > 0, $T330,($L330/2*($G330*(Q330*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T330 > 0, $T330,($L330/2*($H330*(Q330*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T330 > 0, $T330, ( $L330 / 2 * ( ( $I330 ) * (Q330*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T331>0,$T331,($L331/2*(($F331*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T331>0,$T331,($L331/2*($G331*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T331>0,$T331,($L331/2*($H331*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T331 > 0, $T331, ( $L331 / 2 * ( ( $I331 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T331 > 0, $T331,($L331/2*(($F331)*(Q331*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T331 > 0, $T331,($L331/2*($G331*(Q331*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T331 > 0, $T331,($L331/2*($H331*(Q331*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T331 > 0, $T331, ( $L331 / 2 * ( ( $I331 ) * (Q331*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,{"$f":"IF(TRUE,SUM(AE332:AF332),(VCCINT/1000)*VCCINT_N*IF($R332>0,$R332,($L332/2*(($F332+$I332)*0.45*$U332+($F332*(OFFSET(FANOUT,8,2))+$G332*(OFFSET(FANOUT,8,4)+$U332)+$H332*(OFFSET(FANOUT,8,5)+$U332)+$I332*(OFFSET(FANOUT,8,3)))))*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1)","v":0},null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T332>0,$T332,($L332/2*(($F332*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T332>0,$T332,($L332/2*($G332*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T332>0,$T332,($L332/2*($H332*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T332 > 0, $T332, ( $L332 / 2 * ( ( $I332 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T332 > 0, $T332,($L332/2*(($F332)*(Q332*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T332 > 0, $T332,($L332/2*($G332*(Q332*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T332 > 0, $T332,($L332/2*($H332*(Q332*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T332 > 0, $T332, ( $L332 / 2 * ( ( $I332 ) * (Q332*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,{"$f":"10^(K333/10)-1","v":5.3095734448019343},null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T333>0,$T333,($L333/2*(($F333*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T333>0,$T333,($L333/2*($G333*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T333>0,$T333,($L333/2*($H333*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T333 > 0, $T333, ( $L333 / 2 * ( ( $I333 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T333 > 0, $T333,($L333/2*(($F333)*(Q333*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T333 > 0, $T333,($L333/2*($G333*(Q333*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T333 > 0, $T333,($L333/2*($H333*(Q333*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T333 > 0, $T333, ( $L333 / 2 * ( ( $I333 ) * (Q333*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"SUM(W333:Z333)","v":0},{"$f":"SUM(AA333:AD333)","v":0}]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T334>0,$T334,($L334/2*(($F334*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T334>0,$T334,($L334/2*($G334*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T334>0,$T334,($L334/2*($H334*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T334 > 0, $T334, ( $L334 / 2 * ( ( $I334 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T334 > 0, $T334,($L334/2*(($F334)*(Q334*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T334 > 0, $T334,($L334/2*($G334*(Q334*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T334 > 0, $T334,($L334/2*($H334*(Q334*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T334 > 0, $T334, ( $L334 / 2 * ( ( $I334 ) * (Q334*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T335>0,$T335,($L335/2*(($F335*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T335>0,$T335,($L335/2*($G335*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T335>0,$T335,($L335/2*($H335*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T335 > 0, $T335, ( $L335 / 2 * ( ( $I335 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T335 > 0, $T335,($L335/2*(($F335)*(Q335*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T335 > 0, $T335,($L335/2*($G335*(Q335*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T335 > 0, $T335,($L335/2*($H335*(Q335*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T335 > 0, $T335, ( $L335 / 2 * ( ( $I335 ) * (Q335*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T336>0,$T336,($L336/2*(($F336*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T336>0,$T336,($L336/2*($G336*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T336>0,$T336,($L336/2*($H336*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T336 > 0, $T336, ( $L336 / 2 * ( ( $I336 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T336 > 0, $T336,($L336/2*(($F336)*(Q336*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T336 > 0, $T336,($L336/2*($G336*(Q336*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T336 > 0, $T336,($L336/2*($H336*(Q336*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T336 > 0, $T336, ( $L336 / 2 * ( ( $I336 ) * (Q336*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T337>0,$T337,($L337/2*(($F337*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T337>0,$T337,($L337/2*($G337*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T337>0,$T337,($L337/2*($H337*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T337 > 0, $T337, ( $L337 / 2 * ( ( $I337 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T337 > 0, $T337,($L337/2*(($F337)*(Q337*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T337 > 0, $T337,($L337/2*($G337*(Q337*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T337 > 0, $T337,($L337/2*($H337*(Q337*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T337 > 0, $T337, ( $L337 / 2 * ( ( $I337 ) * (Q337*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T338>0,$T338,($L338/2*(($F338*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T338>0,$T338,($L338/2*($G338*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T338>0,$T338,($L338/2*($H338*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T338 > 0, $T338, ( $L338 / 2 * ( ( $I338 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T338 > 0, $T338,($L338/2*(($F338)*(Q338*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T338 > 0, $T338,($L338/2*($G338*(Q338*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T338 > 0, $T338,($L338/2*($H338*(Q338*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T338 > 0, $T338, ( $L338 / 2 * ( ( $I338 ) * (Q338*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T339>0,$T339,($L339/2*(($F339*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T339>0,$T339,($L339/2*($G339*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T339>0,$T339,($L339/2*($H339*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T339 > 0, $T339, ( $L339 / 2 * ( ( $I339 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T339 > 0, $T339,($L339/2*(($F339)*(Q339*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T339 > 0, $T339,($L339/2*($G339*(Q339*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T339 > 0, $T339,($L339/2*($H339*(Q339*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T339 > 0, $T339, ( $L339 / 2 * ( ( $I339 ) * (Q339*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T340>0,$T340,($L340/2*(($F340*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T340>0,$T340,($L340/2*($G340*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T340>0,$T340,($L340/2*($H340*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T340 > 0, $T340, ( $L340 / 2 * ( ( $I340 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T340 > 0, $T340,($L340/2*(($F340)*(Q340*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T340 > 0, $T340,($L340/2*($G340*(Q340*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T340 > 0, $T340,($L340/2*($H340*(Q340*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T340 > 0, $T340, ( $L340 / 2 * ( ( $I340 ) * (Q340*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T341>0,$T341,($L341/2*(($F341*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T341>0,$T341,($L341/2*($G341*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T341>0,$T341,($L341/2*($H341*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T341 > 0, $T341, ( $L341 / 2 * ( ( $I341 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T341 > 0, $T341,($L341/2*(($F341)*(Q341*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T341 > 0, $T341,($L341/2*($G341*(Q341*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T341 > 0, $T341,($L341/2*($H341*(Q341*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T341 > 0, $T341, ( $L341 / 2 * ( ( $I341 ) * (Q341*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T342>0,$T342,($L342/2*(($F342*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T342>0,$T342,($L342/2*($G342*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T342>0,$T342,($L342/2*($H342*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T342 > 0, $T342, ( $L342 / 2 * ( ( $I342 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T342 > 0, $T342,($L342/2*(($F342)*(Q342*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T342 > 0, $T342,($L342/2*($G342*(Q342*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T342 > 0, $T342,($L342/2*($H342*(Q342*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T342 > 0, $T342, ( $L342 / 2 * ( ( $I342 ) * (Q342*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T343>0,$T343,($L343/2*(($F343*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T343>0,$T343,($L343/2*($G343*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T343>0,$T343,($L343/2*($H343*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T343 > 0, $T343, ( $L343 / 2 * ( ( $I343 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T343 > 0, $T343,($L343/2*(($F343)*(Q343*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T343 > 0, $T343,($L343/2*($G343*(Q343*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T343 > 0, $T343,($L343/2*($H343*(Q343*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T343 > 0, $T343, ( $L343 / 2 * ( ( $I343 ) * (Q343*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T344>0,$T344,($L344/2*(($F344*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T344>0,$T344,($L344/2*($G344*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T344>0,$T344,($L344/2*($H344*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T344 > 0, $T344, ( $L344 / 2 * ( ( $I344 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T344 > 0, $T344,($L344/2*(($F344)*(Q344*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T344 > 0, $T344,($L344/2*($G344*(Q344*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T344 > 0, $T344,($L344/2*($H344*(Q344*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T344 > 0, $T344, ( $L344 / 2 * ( ( $I344 ) * (Q344*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T345>0,$T345,($L345/2*(($F345*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T345>0,$T345,($L345/2*($G345*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T345>0,$T345,($L345/2*($H345*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T345 > 0, $T345, ( $L345 / 2 * ( ( $I345 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T345 > 0, $T345,($L345/2*(($F345)*(Q345*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T345 > 0, $T345,($L345/2*($G345*(Q345*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T345 > 0, $T345,($L345/2*($H345*(Q345*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T345 > 0, $T345, ( $L345 / 2 * ( ( $I345 ) * (Q345*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T346>0,$T346,($L346/2*(($F346*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T346>0,$T346,($L346/2*($G346*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T346>0,$T346,($L346/2*($H346*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T346 > 0, $T346, ( $L346 / 2 * ( ( $I346 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T346 > 0, $T346,($L346/2*(($F346)*(Q346*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T346 > 0, $T346,($L346/2*($G346*(Q346*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T346 > 0, $T346,($L346/2*($H346*(Q346*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T346 > 0, $T346, ( $L346 / 2 * ( ( $I346 ) * (Q346*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T347>0,$T347,($L347/2*(($F347*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T347>0,$T347,($L347/2*($G347*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T347>0,$T347,($L347/2*($H347*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T347 > 0, $T347, ( $L347 / 2 * ( ( $I347 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T347 > 0, $T347,($L347/2*(($F347)*(Q347*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T347 > 0, $T347,($L347/2*($G347*(Q347*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T347 > 0, $T347,($L347/2*($H347*(Q347*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T347 > 0, $T347, ( $L347 / 2 * ( ( $I347 ) * (Q347*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T348>0,$T348,($L348/2*(($F348*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T348>0,$T348,($L348/2*($G348*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T348>0,$T348,($L348/2*($H348*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T348 > 0, $T348, ( $L348 / 2 * ( ( $I348 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T348 > 0, $T348,($L348/2*(($F348)*(Q348*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T348 > 0, $T348,($L348/2*($G348*(Q348*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T348 > 0, $T348,($L348/2*($H348*(Q348*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T348 > 0, $T348, ( $L348 / 2 * ( ( $I348 ) * (Q348*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T349>0,$T349,($L349/2*(($F349*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T349>0,$T349,($L349/2*($G349*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T349>0,$T349,($L349/2*($H349*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T349 > 0, $T349, ( $L349 / 2 * ( ( $I349 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T349 > 0, $T349,($L349/2*(($F349)*(Q349*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T349 > 0, $T349,($L349/2*($G349*(Q349*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T349 > 0, $T349,($L349/2*($H349*(Q349*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T349 > 0, $T349, ( $L349 / 2 * ( ( $I349 ) * (Q349*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T350>0,$T350,($L350/2*(($F350*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T350>0,$T350,($L350/2*($G350*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T350>0,$T350,($L350/2*($H350*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T350 > 0, $T350, ( $L350 / 2 * ( ( $I350 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T350 > 0, $T350,($L350/2*(($F350)*(Q350*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T350 > 0, $T350,($L350/2*($G350*(Q350*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T350 > 0, $T350,($L350/2*($H350*(Q350*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T350 > 0, $T350, ( $L350 / 2 * ( ( $I350 ) * (Q350*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T351>0,$T351,($L351/2*(($F351*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T351>0,$T351,($L351/2*($G351*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T351>0,$T351,($L351/2*($H351*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T351 > 0, $T351, ( $L351 / 2 * ( ( $I351 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T351 > 0, $T351,($L351/2*(($F351)*(Q351*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T351 > 0, $T351,($L351/2*($G351*(Q351*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T351 > 0, $T351,($L351/2*($H351*(Q351*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T351 > 0, $T351, ( $L351 / 2 * ( ( $I351 ) * (Q351*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T352>0,$T352,($L352/2*(($F352*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T352>0,$T352,($L352/2*($G352*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T352>0,$T352,($L352/2*($H352*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T352 > 0, $T352, ( $L352 / 2 * ( ( $I352 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T352 > 0, $T352,($L352/2*(($F352)*(Q352*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T352 > 0, $T352,($L352/2*($G352*(Q352*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T352 > 0, $T352,($L352/2*($H352*(Q352*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T352 > 0, $T352, ( $L352 / 2 * ( ( $I352 ) * (Q352*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T353>0,$T353,($L353/2*(($F353*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T353>0,$T353,($L353/2*($G353*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T353>0,$T353,($L353/2*($H353*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T353 > 0, $T353, ( $L353 / 2 * ( ( $I353 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T353 > 0, $T353,($L353/2*(($F353)*(Q353*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T353 > 0, $T353,($L353/2*($G353*(Q353*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T353 > 0, $T353,($L353/2*($H353*(Q353*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T353 > 0, $T353, ( $L353 / 2 * ( ( $I353 ) * (Q353*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T354>0,$T354,($L354/2*(($F354*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T354>0,$T354,($L354/2*($G354*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T354>0,$T354,($L354/2*($H354*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T354 > 0, $T354, ( $L354 / 2 * ( ( $I354 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T354 > 0, $T354,($L354/2*(($F354)*(Q354*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T354 > 0, $T354,($L354/2*($G354*(Q354*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T354 > 0, $T354,($L354/2*($H354*(Q354*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T354 > 0, $T354, ( $L354 / 2 * ( ( $I354 ) * (Q354*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T355>0,$T355,($L355/2*(($F355*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T355>0,$T355,($L355/2*($G355*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T355>0,$T355,($L355/2*($H355*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T355 > 0, $T355, ( $L355 / 2 * ( ( $I355 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T355 > 0, $T355,($L355/2*(($F355)*(Q355*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T355 > 0, $T355,($L355/2*($G355*(Q355*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T355 > 0, $T355,($L355/2*($H355*(Q355*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T355 > 0, $T355, ( $L355 / 2 * ( ( $I355 ) * (Q355*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T356>0,$T356,($L356/2*(($F356*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T356>0,$T356,($L356/2*($G356*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T356>0,$T356,($L356/2*($H356*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T356 > 0, $T356, ( $L356 / 2 * ( ( $I356 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T356 > 0, $T356,($L356/2*(($F356)*(Q356*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T356 > 0, $T356,($L356/2*($G356*(Q356*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T356 > 0, $T356,($L356/2*($H356*(Q356*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T356 > 0, $T356, ( $L356 / 2 * ( ( $I356 ) * (Q356*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T357>0,$T357,($L357/2*(($F357*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T357>0,$T357,($L357/2*($G357*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T357>0,$T357,($L357/2*($H357*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T357 > 0, $T357, ( $L357 / 2 * ( ( $I357 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T357 > 0, $T357,($L357/2*(($F357)*(Q357*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T357 > 0, $T357,($L357/2*($G357*(Q357*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T357 > 0, $T357,($L357/2*($H357*(Q357*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T357 > 0, $T357, ( $L357 / 2 * ( ( $I357 ) * (Q357*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T358>0,$T358,($L358/2*(($F358*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T358>0,$T358,($L358/2*($G358*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T358>0,$T358,($L358/2*($H358*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T358 > 0, $T358, ( $L358 / 2 * ( ( $I358 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T358 > 0, $T358,($L358/2*(($F358)*(Q358*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T358 > 0, $T358,($L358/2*($G358*(Q358*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T358 > 0, $T358,($L358/2*($H358*(Q358*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T358 > 0, $T358, ( $L358 / 2 * ( ( $I358 ) * (Q358*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T359>0,$T359,($L359/2*(($F359*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T359>0,$T359,($L359/2*($G359*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T359>0,$T359,($L359/2*($H359*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T359 > 0, $T359, ( $L359 / 2 * ( ( $I359 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T359 > 0, $T359,($L359/2*(($F359)*(Q359*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T359 > 0, $T359,($L359/2*($G359*(Q359*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T359 > 0, $T359,($L359/2*($H359*(Q359*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T359 > 0, $T359, ( $L359 / 2 * ( ( $I359 ) * (Q359*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T360>0,$T360,($L360/2*(($F360*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T360>0,$T360,($L360/2*($G360*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T360>0,$T360,($L360/2*($H360*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T360 > 0, $T360, ( $L360 / 2 * ( ( $I360 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T360 > 0, $T360,($L360/2*(($F360)*(Q360*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T360 > 0, $T360,($L360/2*($G360*(Q360*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T360 > 0, $T360,($L360/2*($H360*(Q360*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T360 > 0, $T360, ( $L360 / 2 * ( ( $I360 ) * (Q360*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T361>0,$T361,($L361/2*(($F361*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T361>0,$T361,($L361/2*($G361*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T361>0,$T361,($L361/2*($H361*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T361 > 0, $T361, ( $L361 / 2 * ( ( $I361 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T361 > 0, $T361,($L361/2*(($F361)*(Q361*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T361 > 0, $T361,($L361/2*($G361*(Q361*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T361 > 0, $T361,($L361/2*($H361*(Q361*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T361 > 0, $T361, ( $L361 / 2 * ( ( $I361 ) * (Q361*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T362>0,$T362,($L362/2*(($F362*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T362>0,$T362,($L362/2*($G362*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T362>0,$T362,($L362/2*($H362*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T362 > 0, $T362, ( $L362 / 2 * ( ( $I362 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T362 > 0, $T362,($L362/2*(($F362)*(Q362*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T362 > 0, $T362,($L362/2*($G362*(Q362*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T362 > 0, $T362,($L362/2*($H362*(Q362*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T362 > 0, $T362, ( $L362 / 2 * ( ( $I362 ) * (Q362*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T363>0,$T363,($L363/2*(($F363*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T363>0,$T363,($L363/2*($G363*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T363>0,$T363,($L363/2*($H363*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T363 > 0, $T363, ( $L363 / 2 * ( ( $I363 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T363 > 0, $T363,($L363/2*(($F363)*(Q363*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T363 > 0, $T363,($L363/2*($G363*(Q363*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T363 > 0, $T363,($L363/2*($H363*(Q363*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T363 > 0, $T363, ( $L363 / 2 * ( ( $I363 ) * (Q363*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T364>0,$T364,($L364/2*(($F364*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T364>0,$T364,($L364/2*($G364*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T364>0,$T364,($L364/2*($H364*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T364 > 0, $T364, ( $L364 / 2 * ( ( $I364 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T364 > 0, $T364,($L364/2*(($F364)*(Q364*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T364 > 0, $T364,($L364/2*($G364*(Q364*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T364 > 0, $T364,($L364/2*($H364*(Q364*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T364 > 0, $T364, ( $L364 / 2 * ( ( $I364 ) * (Q364*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T365>0,$T365,($L365/2*(($F365*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T365>0,$T365,($L365/2*($G365*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T365>0,$T365,($L365/2*($H365*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T365 > 0, $T365, ( $L365 / 2 * ( ( $I365 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T365 > 0, $T365,($L365/2*(($F365)*(Q365*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T365 > 0, $T365,($L365/2*($G365*(Q365*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T365 > 0, $T365,($L365/2*($H365*(Q365*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T365 > 0, $T365, ( $L365 / 2 * ( ( $I365 ) * (Q365*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T366>0,$T366,($L366/2*(($F366*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T366>0,$T366,($L366/2*($G366*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T366>0,$T366,($L366/2*($H366*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T366 > 0, $T366, ( $L366 / 2 * ( ( $I366 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T366 > 0, $T366,($L366/2*(($F366)*(Q366*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T366 > 0, $T366,($L366/2*($G366*(Q366*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T366 > 0, $T366,($L366/2*($H366*(Q366*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T366 > 0, $T366, ( $L366 / 2 * ( ( $I366 ) * (Q366*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T367>0,$T367,($L367/2*(($F367*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T367>0,$T367,($L367/2*($G367*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T367>0,$T367,($L367/2*($H367*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T367 > 0, $T367, ( $L367 / 2 * ( ( $I367 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T367 > 0, $T367,($L367/2*(($F367)*(Q367*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T367 > 0, $T367,($L367/2*($G367*(Q367*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T367 > 0, $T367,($L367/2*($H367*(Q367*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T367 > 0, $T367, ( $L367 / 2 * ( ( $I367 ) * (Q367*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T368>0,$T368,($L368/2*(($F368*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T368>0,$T368,($L368/2*($G368*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T368>0,$T368,($L368/2*($H368*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T368 > 0, $T368, ( $L368 / 2 * ( ( $I368 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T368 > 0, $T368,($L368/2*(($F368)*(Q368*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T368 > 0, $T368,($L368/2*($G368*(Q368*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T368 > 0, $T368,($L368/2*($H368*(Q368*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T368 > 0, $T368, ( $L368 / 2 * ( ( $I368 ) * (Q368*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T369>0,$T369,($L369/2*(($F369*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T369>0,$T369,($L369/2*($G369*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T369>0,$T369,($L369/2*($H369*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T369 > 0, $T369, ( $L369 / 2 * ( ( $I369 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T369 > 0, $T369,($L369/2*(($F369)*(Q369*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T369 > 0, $T369,($L369/2*($G369*(Q369*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T369 > 0, $T369,($L369/2*($H369*(Q369*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T369 > 0, $T369, ( $L369 / 2 * ( ( $I369 ) * (Q369*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T370>0,$T370,($L370/2*(($F370*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T370>0,$T370,($L370/2*($G370*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T370>0,$T370,($L370/2*($H370*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T370 > 0, $T370, ( $L370 / 2 * ( ( $I370 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T370 > 0, $T370,($L370/2*(($F370)*(Q370*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T370 > 0, $T370,($L370/2*($G370*(Q370*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T370 > 0, $T370,($L370/2*($H370*(Q370*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T370 > 0, $T370, ( $L370 / 2 * ( ( $I370 ) * (Q370*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T371>0,$T371,($L371/2*(($F371*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T371>0,$T371,($L371/2*($G371*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T371>0,$T371,($L371/2*($H371*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T371 > 0, $T371, ( $L371 / 2 * ( ( $I371 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T371 > 0, $T371,($L371/2*(($F371)*(Q371*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T371 > 0, $T371,($L371/2*($G371*(Q371*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T371 > 0, $T371,($L371/2*($H371*(Q371*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T371 > 0, $T371, ( $L371 / 2 * ( ( $I371 ) * (Q371*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T372>0,$T372,($L372/2*(($F372*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T372>0,$T372,($L372/2*($G372*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T372>0,$T372,($L372/2*($H372*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T372 > 0, $T372, ( $L372 / 2 * ( ( $I372 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T372 > 0, $T372,($L372/2*(($F372)*(Q372*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T372 > 0, $T372,($L372/2*($G372*(Q372*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T372 > 0, $T372,($L372/2*($H372*(Q372*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T372 > 0, $T372, ( $L372 / 2 * ( ( $I372 ) * (Q372*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T373>0,$T373,($L373/2*(($F373*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T373>0,$T373,($L373/2*($G373*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T373>0,$T373,($L373/2*($H373*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T373 > 0, $T373, ( $L373 / 2 * ( ( $I373 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T373 > 0, $T373,($L373/2*(($F373)*(Q373*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T373 > 0, $T373,($L373/2*($G373*(Q373*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T373 > 0, $T373,($L373/2*($H373*(Q373*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T373 > 0, $T373, ( $L373 / 2 * ( ( $I373 ) * (Q373*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T374>0,$T374,($L374/2*(($F374*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T374>0,$T374,($L374/2*($G374*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T374>0,$T374,($L374/2*($H374*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T374 > 0, $T374, ( $L374 / 2 * ( ( $I374 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T374 > 0, $T374,($L374/2*(($F374)*(Q374*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T374 > 0, $T374,($L374/2*($G374*(Q374*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T374 > 0, $T374,($L374/2*($H374*(Q374*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T374 > 0, $T374, ( $L374 / 2 * ( ( $I374 ) * (Q374*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T375>0,$T375,($L375/2*(($F375*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T375>0,$T375,($L375/2*($G375*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T375>0,$T375,($L375/2*($H375*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T375 > 0, $T375, ( $L375 / 2 * ( ( $I375 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T375 > 0, $T375,($L375/2*(($F375)*(Q375*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T375 > 0, $T375,($L375/2*($G375*(Q375*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T375 > 0, $T375,($L375/2*($H375*(Q375*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T375 > 0, $T375, ( $L375 / 2 * ( ( $I375 ) * (Q375*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T376>0,$T376,($L376/2*(($F376*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T376>0,$T376,($L376/2*($G376*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T376>0,$T376,($L376/2*($H376*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T376 > 0, $T376, ( $L376 / 2 * ( ( $I376 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T376 > 0, $T376,($L376/2*(($F376)*(Q376*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T376 > 0, $T376,($L376/2*($G376*(Q376*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T376 > 0, $T376,($L376/2*($H376*(Q376*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T376 > 0, $T376, ( $L376 / 2 * ( ( $I376 ) * (Q376*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T377>0,$T377,($L377/2*(($F377*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T377>0,$T377,($L377/2*($G377*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T377>0,$T377,($L377/2*($H377*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T377 > 0, $T377, ( $L377 / 2 * ( ( $I377 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T377 > 0, $T377,($L377/2*(($F377)*(Q377*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T377 > 0, $T377,($L377/2*($G377*(Q377*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T377 > 0, $T377,($L377/2*($H377*(Q377*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T377 > 0, $T377, ( $L377 / 2 * ( ( $I377 ) * (Q377*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T378>0,$T378,($L378/2*(($F378*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T378>0,$T378,($L378/2*($G378*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T378>0,$T378,($L378/2*($H378*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T378 > 0, $T378, ( $L378 / 2 * ( ( $I378 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T378 > 0, $T378,($L378/2*(($F378)*(Q378*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T378 > 0, $T378,($L378/2*($G378*(Q378*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T378 > 0, $T378,($L378/2*($H378*(Q378*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T378 > 0, $T378, ( $L378 / 2 * ( ( $I378 ) * (Q378*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T379>0,$T379,($L379/2*(($F379*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T379>0,$T379,($L379/2*($G379*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T379>0,$T379,($L379/2*($H379*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T379 > 0, $T379, ( $L379 / 2 * ( ( $I379 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T379 > 0, $T379,($L379/2*(($F379)*(Q379*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T379 > 0, $T379,($L379/2*($G379*(Q379*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T379 > 0, $T379,($L379/2*($H379*(Q379*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T379 > 0, $T379, ( $L379 / 2 * ( ( $I379 ) * (Q379*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T380>0,$T380,($L380/2*(($F380*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T380>0,$T380,($L380/2*($G380*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T380>0,$T380,($L380/2*($H380*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T380 > 0, $T380, ( $L380 / 2 * ( ( $I380 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T380 > 0, $T380,($L380/2*(($F380)*(Q380*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T380 > 0, $T380,($L380/2*($G380*(Q380*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T380 > 0, $T380,($L380/2*($H380*(Q380*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T380 > 0, $T380, ( $L380 / 2 * ( ( $I380 ) * (Q380*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T381>0,$T381,($L381/2*(($F381*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T381>0,$T381,($L381/2*($G381*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T381>0,$T381,($L381/2*($H381*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T381 > 0, $T381, ( $L381 / 2 * ( ( $I381 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T381 > 0, $T381,($L381/2*(($F381)*(Q381*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T381 > 0, $T381,($L381/2*($G381*(Q381*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T381 > 0, $T381,($L381/2*($H381*(Q381*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T381 > 0, $T381, ( $L381 / 2 * ( ( $I381 ) * (Q381*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T382>0,$T382,($L382/2*(($F382*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T382>0,$T382,($L382/2*($G382*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T382>0,$T382,($L382/2*($H382*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T382 > 0, $T382, ( $L382 / 2 * ( ( $I382 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T382 > 0, $T382,($L382/2*(($F382)*(Q382*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T382 > 0, $T382,($L382/2*($G382*(Q382*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T382 > 0, $T382,($L382/2*($H382*(Q382*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T382 > 0, $T382, ( $L382 / 2 * ( ( $I382 ) * (Q382*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T383>0,$T383,($L383/2*(($F383*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T383>0,$T383,($L383/2*($G383*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T383>0,$T383,($L383/2*($H383*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T383 > 0, $T383, ( $L383 / 2 * ( ( $I383 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T383 > 0, $T383,($L383/2*(($F383)*(Q383*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T383 > 0, $T383,($L383/2*($G383*(Q383*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T383 > 0, $T383,($L383/2*($H383*(Q383*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T383 > 0, $T383, ( $L383 / 2 * ( ( $I383 ) * (Q383*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T384>0,$T384,($L384/2*(($F384*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T384>0,$T384,($L384/2*($G384*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T384>0,$T384,($L384/2*($H384*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T384 > 0, $T384, ( $L384 / 2 * ( ( $I384 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T384 > 0, $T384,($L384/2*(($F384)*(Q384*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T384 > 0, $T384,($L384/2*($G384*(Q384*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T384 > 0, $T384,($L384/2*($H384*(Q384*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T384 > 0, $T384, ( $L384 / 2 * ( ( $I384 ) * (Q384*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T385>0,$T385,($L385/2*(($F385*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T385>0,$T385,($L385/2*($G385*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T385>0,$T385,($L385/2*($H385*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T385 > 0, $T385, ( $L385 / 2 * ( ( $I385 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T385 > 0, $T385,($L385/2*(($F385)*(Q385*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T385 > 0, $T385,($L385/2*($G385*(Q385*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T385 > 0, $T385,($L385/2*($H385*(Q385*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T385 > 0, $T385, ( $L385 / 2 * ( ( $I385 ) * (Q385*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T386>0,$T386,($L386/2*(($F386*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T386>0,$T386,($L386/2*($G386*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T386>0,$T386,($L386/2*($H386*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T386 > 0, $T386, ( $L386 / 2 * ( ( $I386 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T386 > 0, $T386,($L386/2*(($F386)*(Q386*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T386 > 0, $T386,($L386/2*($G386*(Q386*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T386 > 0, $T386,($L386/2*($H386*(Q386*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T386 > 0, $T386, ( $L386 / 2 * ( ( $I386 ) * (Q386*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T387>0,$T387,($L387/2*(($F387*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T387>0,$T387,($L387/2*($G387*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T387>0,$T387,($L387/2*($H387*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T387 > 0, $T387, ( $L387 / 2 * ( ( $I387 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T387 > 0, $T387,($L387/2*(($F387)*(Q387*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T387 > 0, $T387,($L387/2*($G387*(Q387*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T387 > 0, $T387,($L387/2*($H387*(Q387*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T387 > 0, $T387, ( $L387 / 2 * ( ( $I387 ) * (Q387*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T388>0,$T388,($L388/2*(($F388*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T388>0,$T388,($L388/2*($G388*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T388>0,$T388,($L388/2*($H388*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T388 > 0, $T388, ( $L388 / 2 * ( ( $I388 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T388 > 0, $T388,($L388/2*(($F388)*(Q388*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T388 > 0, $T388,($L388/2*($G388*(Q388*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T388 > 0, $T388,($L388/2*($H388*(Q388*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T388 > 0, $T388, ( $L388 / 2 * ( ( $I388 ) * (Q388*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T389>0,$T389,($L389/2*(($F389*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T389>0,$T389,($L389/2*($G389*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T389>0,$T389,($L389/2*($H389*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T389 > 0, $T389, ( $L389 / 2 * ( ( $I389 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T389 > 0, $T389,($L389/2*(($F389)*(Q389*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T389 > 0, $T389,($L389/2*($G389*(Q389*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T389 > 0, $T389,($L389/2*($H389*(Q389*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T389 > 0, $T389, ( $L389 / 2 * ( ( $I389 ) * (Q389*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T390>0,$T390,($L390/2*(($F390*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T390>0,$T390,($L390/2*($G390*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T390>0,$T390,($L390/2*($H390*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T390 > 0, $T390, ( $L390 / 2 * ( ( $I390 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T390 > 0, $T390,($L390/2*(($F390)*(Q390*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T390 > 0, $T390,($L390/2*($G390*(Q390*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T390 > 0, $T390,($L390/2*($H390*(Q390*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T390 > 0, $T390, ( $L390 / 2 * ( ( $I390 ) * (Q390*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T391>0,$T391,($L391/2*(($F391*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T391>0,$T391,($L391/2*($G391*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T391>0,$T391,($L391/2*($H391*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T391 > 0, $T391, ( $L391 / 2 * ( ( $I391 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T391 > 0, $T391,($L391/2*(($F391)*(Q391*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T391 > 0, $T391,($L391/2*($G391*(Q391*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T391 > 0, $T391,($L391/2*($H391*(Q391*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T391 > 0, $T391, ( $L391 / 2 * ( ( $I391 ) * (Q391*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T392>0,$T392,($L392/2*(($F392*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T392>0,$T392,($L392/2*($G392*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T392>0,$T392,($L392/2*($H392*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T392 > 0, $T392, ( $L392 / 2 * ( ( $I392 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T392 > 0, $T392,($L392/2*(($F392)*(Q392*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T392 > 0, $T392,($L392/2*($G392*(Q392*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T392 > 0, $T392,($L392/2*($H392*(Q392*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T392 > 0, $T392, ( $L392 / 2 * ( ( $I392 ) * (Q392*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T393>0,$T393,($L393/2*(($F393*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T393>0,$T393,($L393/2*($G393*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T393>0,$T393,($L393/2*($H393*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T393 > 0, $T393, ( $L393 / 2 * ( ( $I393 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T393 > 0, $T393,($L393/2*(($F393)*(Q393*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T393 > 0, $T393,($L393/2*($G393*(Q393*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T393 > 0, $T393,($L393/2*($H393*(Q393*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T393 > 0, $T393, ( $L393 / 2 * ( ( $I393 ) * (Q393*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T394>0,$T394,($L394/2*(($F394*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T394>0,$T394,($L394/2*($G394*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T394>0,$T394,($L394/2*($H394*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T394 > 0, $T394, ( $L394 / 2 * ( ( $I394 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T394 > 0, $T394,($L394/2*(($F394)*(Q394*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T394 > 0, $T394,($L394/2*($G394*(Q394*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T394 > 0, $T394,($L394/2*($H394*(Q394*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T394 > 0, $T394, ( $L394 / 2 * ( ( $I394 ) * (Q394*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T395>0,$T395,($L395/2*(($F395*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T395>0,$T395,($L395/2*($G395*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T395>0,$T395,($L395/2*($H395*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T395 > 0, $T395, ( $L395 / 2 * ( ( $I395 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T395 > 0, $T395,($L395/2*(($F395)*(Q395*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T395 > 0, $T395,($L395/2*($G395*(Q395*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T395 > 0, $T395,($L395/2*($H395*(Q395*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T395 > 0, $T395, ( $L395 / 2 * ( ( $I395 ) * (Q395*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,{"$f":"IF(TRUE,SUM(AE396:AF396),(VCCINT/1000)*VCCINT_N*IF($R396>0,$R396,($L396/2*(($F396+$I396)*0.45*$U396+($F396*(OFFSET(FANOUT,8,2))+$G396*(OFFSET(FANOUT,8,4)+$U396)+$H396*(OFFSET(FANOUT,8,5)+$U396)+$I396*(OFFSET(FANOUT,8,3)))))*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1)","v":0},null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T396>0,$T396,($L396/2*(($F396*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T396>0,$T396,($L396/2*($G396*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T396>0,$T396,($L396/2*($H396*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T396 > 0, $T396, ( $L396 / 2 * ( ( $I396 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T396 > 0, $T396,($L396/2*(($F396)*(Q396*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T396 > 0, $T396,($L396/2*($G396*(Q396*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T396 > 0, $T396,($L396/2*($H396*(Q396*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T396 > 0, $T396, ( $L396 / 2 * ( ( $I396 ) * (Q396*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,{"$f":"10^(K397/10)-1","v":5.3095734448019343},null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T397>0,$T397,($L397/2*(($F397*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T397>0,$T397,($L397/2*($G397*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T397>0,$T397,($L397/2*($H397*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T397 > 0, $T397, ( $L397 / 2 * ( ( $I397 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T397 > 0, $T397,($L397/2*(($F397)*(Q397*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T397 > 0, $T397,($L397/2*($G397*(Q397*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T397 > 0, $T397,($L397/2*($H397*(Q397*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T397 > 0, $T397, ( $L397 / 2 * ( ( $I397 ) * (Q397*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"SUM(W397:Z397)","v":0},{"$f":"SUM(AA397:AD397)","v":0}]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T398>0,$T398,($L398/2*(($F398*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T398>0,$T398,($L398/2*($G398*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T398>0,$T398,($L398/2*($H398*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T398 > 0, $T398, ( $L398 / 2 * ( ( $I398 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T398 > 0, $T398,($L398/2*(($F398)*(Q398*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T398 > 0, $T398,($L398/2*($G398*(Q398*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T398 > 0, $T398,($L398/2*($H398*(Q398*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T398 > 0, $T398, ( $L398 / 2 * ( ( $I398 ) * (Q398*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T399>0,$T399,($L399/2*(($F399*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T399>0,$T399,($L399/2*($G399*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T399>0,$T399,($L399/2*($H399*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T399 > 0, $T399, ( $L399 / 2 * ( ( $I399 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T399 > 0, $T399,($L399/2*(($F399)*(Q399*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T399 > 0, $T399,($L399/2*($G399*(Q399*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T399 > 0, $T399,($L399/2*($H399*(Q399*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T399 > 0, $T399, ( $L399 / 2 * ( ( $I399 ) * (Q399*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T400>0,$T400,($L400/2*(($F400*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T400>0,$T400,($L400/2*($G400*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T400>0,$T400,($L400/2*($H400*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T400 > 0, $T400, ( $L400 / 2 * ( ( $I400 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T400 > 0, $T400,($L400/2*(($F400)*(Q400*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T400 > 0, $T400,($L400/2*($G400*(Q400*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T400 > 0, $T400,($L400/2*($H400*(Q400*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T400 > 0, $T400, ( $L400 / 2 * ( ( $I400 ) * (Q400*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T401>0,$T401,($L401/2*(($F401*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T401>0,$T401,($L401/2*($G401*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T401>0,$T401,($L401/2*($H401*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T401 > 0, $T401, ( $L401 / 2 * ( ( $I401 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T401 > 0, $T401,($L401/2*(($F401)*(Q401*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T401 > 0, $T401,($L401/2*($G401*(Q401*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T401 > 0, $T401,($L401/2*($H401*(Q401*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T401 > 0, $T401, ( $L401 / 2 * ( ( $I401 ) * (Q401*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T402>0,$T402,($L402/2*(($F402*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T402>0,$T402,($L402/2*($G402*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T402>0,$T402,($L402/2*($H402*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T402 > 0, $T402, ( $L402 / 2 * ( ( $I402 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T402 > 0, $T402,($L402/2*(($F402)*(Q402*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T402 > 0, $T402,($L402/2*($G402*(Q402*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T402 > 0, $T402,($L402/2*($H402*(Q402*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T402 > 0, $T402, ( $L402 / 2 * ( ( $I402 ) * (Q402*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T403>0,$T403,($L403/2*(($F403*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T403>0,$T403,($L403/2*($G403*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T403>0,$T403,($L403/2*($H403*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T403 > 0, $T403, ( $L403 / 2 * ( ( $I403 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T403 > 0, $T403,($L403/2*(($F403)*(Q403*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T403 > 0, $T403,($L403/2*($G403*(Q403*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T403 > 0, $T403,($L403/2*($H403*(Q403*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T403 > 0, $T403, ( $L403 / 2 * ( ( $I403 ) * (Q403*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T404>0,$T404,($L404/2*(($F404*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T404>0,$T404,($L404/2*($G404*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T404>0,$T404,($L404/2*($H404*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T404 > 0, $T404, ( $L404 / 2 * ( ( $I404 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T404 > 0, $T404,($L404/2*(($F404)*(Q404*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T404 > 0, $T404,($L404/2*($G404*(Q404*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T404 > 0, $T404,($L404/2*($H404*(Q404*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T404 > 0, $T404, ( $L404 / 2 * ( ( $I404 ) * (Q404*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T405>0,$T405,($L405/2*(($F405*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T405>0,$T405,($L405/2*($G405*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T405>0,$T405,($L405/2*($H405*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T405 > 0, $T405, ( $L405 / 2 * ( ( $I405 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T405 > 0, $T405,($L405/2*(($F405)*(Q405*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T405 > 0, $T405,($L405/2*($G405*(Q405*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T405 > 0, $T405,($L405/2*($H405*(Q405*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T405 > 0, $T405, ( $L405 / 2 * ( ( $I405 ) * (Q405*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T406>0,$T406,($L406/2*(($F406*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T406>0,$T406,($L406/2*($G406*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T406>0,$T406,($L406/2*($H406*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T406 > 0, $T406, ( $L406 / 2 * ( ( $I406 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T406 > 0, $T406,($L406/2*(($F406)*(Q406*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T406 > 0, $T406,($L406/2*($G406*(Q406*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T406 > 0, $T406,($L406/2*($H406*(Q406*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T406 > 0, $T406, ( $L406 / 2 * ( ( $I406 ) * (Q406*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T407>0,$T407,($L407/2*(($F407*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T407>0,$T407,($L407/2*($G407*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T407>0,$T407,($L407/2*($H407*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T407 > 0, $T407, ( $L407 / 2 * ( ( $I407 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T407 > 0, $T407,($L407/2*(($F407)*(Q407*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T407 > 0, $T407,($L407/2*($G407*(Q407*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T407 > 0, $T407,($L407/2*($H407*(Q407*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T407 > 0, $T407, ( $L407 / 2 * ( ( $I407 ) * (Q407*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T408>0,$T408,($L408/2*(($F408*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T408>0,$T408,($L408/2*($G408*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T408>0,$T408,($L408/2*($H408*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T408 > 0, $T408, ( $L408 / 2 * ( ( $I408 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T408 > 0, $T408,($L408/2*(($F408)*(Q408*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T408 > 0, $T408,($L408/2*($G408*(Q408*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T408 > 0, $T408,($L408/2*($H408*(Q408*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T408 > 0, $T408, ( $L408 / 2 * ( ( $I408 ) * (Q408*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T409>0,$T409,($L409/2*(($F409*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T409>0,$T409,($L409/2*($G409*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T409>0,$T409,($L409/2*($H409*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T409 > 0, $T409, ( $L409 / 2 * ( ( $I409 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T409 > 0, $T409,($L409/2*(($F409)*(Q409*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T409 > 0, $T409,($L409/2*($G409*(Q409*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T409 > 0, $T409,($L409/2*($H409*(Q409*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T409 > 0, $T409, ( $L409 / 2 * ( ( $I409 ) * (Q409*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T410>0,$T410,($L410/2*(($F410*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T410>0,$T410,($L410/2*($G410*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T410>0,$T410,($L410/2*($H410*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T410 > 0, $T410, ( $L410 / 2 * ( ( $I410 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T410 > 0, $T410,($L410/2*(($F410)*(Q410*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T410 > 0, $T410,($L410/2*($G410*(Q410*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T410 > 0, $T410,($L410/2*($H410*(Q410*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T410 > 0, $T410, ( $L410 / 2 * ( ( $I410 ) * (Q410*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T411>0,$T411,($L411/2*(($F411*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T411>0,$T411,($L411/2*($G411*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T411>0,$T411,($L411/2*($H411*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T411 > 0, $T411, ( $L411 / 2 * ( ( $I411 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T411 > 0, $T411,($L411/2*(($F411)*(Q411*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T411 > 0, $T411,($L411/2*($G411*(Q411*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T411 > 0, $T411,($L411/2*($H411*(Q411*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T411 > 0, $T411, ( $L411 / 2 * ( ( $I411 ) * (Q411*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T412>0,$T412,($L412/2*(($F412*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T412>0,$T412,($L412/2*($G412*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T412>0,$T412,($L412/2*($H412*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T412 > 0, $T412, ( $L412 / 2 * ( ( $I412 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T412 > 0, $T412,($L412/2*(($F412)*(Q412*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T412 > 0, $T412,($L412/2*($G412*(Q412*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T412 > 0, $T412,($L412/2*($H412*(Q412*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T412 > 0, $T412, ( $L412 / 2 * ( ( $I412 ) * (Q412*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T413>0,$T413,($L413/2*(($F413*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T413>0,$T413,($L413/2*($G413*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T413>0,$T413,($L413/2*($H413*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T413 > 0, $T413, ( $L413 / 2 * ( ( $I413 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T413 > 0, $T413,($L413/2*(($F413)*(Q413*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T413 > 0, $T413,($L413/2*($G413*(Q413*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T413 > 0, $T413,($L413/2*($H413*(Q413*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T413 > 0, $T413, ( $L413 / 2 * ( ( $I413 ) * (Q413*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T414>0,$T414,($L414/2*(($F414*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T414>0,$T414,($L414/2*($G414*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T414>0,$T414,($L414/2*($H414*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T414 > 0, $T414, ( $L414 / 2 * ( ( $I414 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T414 > 0, $T414,($L414/2*(($F414)*(Q414*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T414 > 0, $T414,($L414/2*($G414*(Q414*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T414 > 0, $T414,($L414/2*($H414*(Q414*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T414 > 0, $T414, ( $L414 / 2 * ( ( $I414 ) * (Q414*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T415>0,$T415,($L415/2*(($F415*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T415>0,$T415,($L415/2*($G415*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T415>0,$T415,($L415/2*($H415*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T415 > 0, $T415, ( $L415 / 2 * ( ( $I415 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T415 > 0, $T415,($L415/2*(($F415)*(Q415*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T415 > 0, $T415,($L415/2*($G415*(Q415*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T415 > 0, $T415,($L415/2*($H415*(Q415*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T415 > 0, $T415, ( $L415 / 2 * ( ( $I415 ) * (Q415*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T416>0,$T416,($L416/2*(($F416*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T416>0,$T416,($L416/2*($G416*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T416>0,$T416,($L416/2*($H416*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T416 > 0, $T416, ( $L416 / 2 * ( ( $I416 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T416 > 0, $T416,($L416/2*(($F416)*(Q416*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T416 > 0, $T416,($L416/2*($G416*(Q416*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T416 > 0, $T416,($L416/2*($H416*(Q416*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T416 > 0, $T416, ( $L416 / 2 * ( ( $I416 ) * (Q416*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T417>0,$T417,($L417/2*(($F417*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T417>0,$T417,($L417/2*($G417*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T417>0,$T417,($L417/2*($H417*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T417 > 0, $T417, ( $L417 / 2 * ( ( $I417 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T417 > 0, $T417,($L417/2*(($F417)*(Q417*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T417 > 0, $T417,($L417/2*($G417*(Q417*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T417 > 0, $T417,($L417/2*($H417*(Q417*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T417 > 0, $T417, ( $L417 / 2 * ( ( $I417 ) * (Q417*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,{"$f":"E418*J418","v":0},0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T418>0,$T418,($L418/2*(($F418*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T418>0,$T418,($L418/2*($G418*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T418>0,$T418,($L418/2*($H418*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T418 > 0, $T418, ( $L418 / 2 * ( ( $I418 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T418 > 0, $T418,($L418/2*(($F418)*(Q418*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T418 > 0, $T418,($L418/2*($G418*(Q418*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T418 > 0, $T418,($L418/2*($H418*(Q418*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T418 > 0, $T418, ( $L418 / 2 * ( ( $I418 ) * (Q418*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T419>0,$T419,($L419/2*(($F419*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T419>0,$T419,($L419/2*($G419*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T419>0,$T419,($L419/2*($H419*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T419 > 0, $T419, ( $L419 / 2 * ( ( $I419 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T419 > 0, $T419,($L419/2*(($F419)*(Q419*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T419 > 0, $T419,($L419/2*($G419*(Q419*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T419 > 0, $T419,($L419/2*($H419*(Q419*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T419 > 0, $T419, ( $L419 / 2 * ( ( $I419 ) * (Q419*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T420>0,$T420,($L420/2*(($F420*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T420>0,$T420,($L420/2*($G420*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T420>0,$T420,($L420/2*($H420*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T420 > 0, $T420, ( $L420 / 2 * ( ( $I420 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T420 > 0, $T420,($L420/2*(($F420)*(Q420*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T420 > 0, $T420,($L420/2*($G420*(Q420*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T420 > 0, $T420,($L420/2*($H420*(Q420*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T420 > 0, $T420, ( $L420 / 2 * ( ( $I420 ) * (Q420*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T421>0,$T421,($L421/2*(($F421*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T421>0,$T421,($L421/2*($G421*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T421>0,$T421,($L421/2*($H421*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T421 > 0, $T421, ( $L421 / 2 * ( ( $I421 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T421 > 0, $T421,($L421/2*(($F421)*(Q421*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T421 > 0, $T421,($L421/2*($G421*(Q421*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T421 > 0, $T421,($L421/2*($H421*(Q421*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T421 > 0, $T421, ( $L421 / 2 * ( ( $I421 ) * (Q421*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T422>0,$T422,($L422/2*(($F422*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T422>0,$T422,($L422/2*($G422*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T422>0,$T422,($L422/2*($H422*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T422 > 0, $T422, ( $L422 / 2 * ( ( $I422 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T422 > 0, $T422,($L422/2*(($F422)*(Q422*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T422 > 0, $T422,($L422/2*($G422*(Q422*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T422 > 0, $T422,($L422/2*($H422*(Q422*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T422 > 0, $T422, ( $L422 / 2 * ( ( $I422 ) * (Q422*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T423>0,$T423,($L423/2*(($F423*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T423>0,$T423,($L423/2*($G423*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T423>0,$T423,($L423/2*($H423*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T423 > 0, $T423, ( $L423 / 2 * ( ( $I423 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T423 > 0, $T423,($L423/2*(($F423)*(Q423*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T423 > 0, $T423,($L423/2*($G423*(Q423*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T423 > 0, $T423,($L423/2*($H423*(Q423*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T423 > 0, $T423, ( $L423 / 2 * ( ( $I423 ) * (Q423*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T424>0,$T424,($L424/2*(($F424*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T424>0,$T424,($L424/2*($G424*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T424>0,$T424,($L424/2*($H424*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T424 > 0, $T424, ( $L424 / 2 * ( ( $I424 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T424 > 0, $T424,($L424/2*(($F424)*(Q424*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T424 > 0, $T424,($L424/2*($G424*(Q424*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T424 > 0, $T424,($L424/2*($H424*(Q424*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T424 > 0, $T424, ( $L424 / 2 * ( ( $I424 ) * (Q424*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T425>0,$T425,($L425/2*(($F425*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T425>0,$T425,($L425/2*($G425*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T425>0,$T425,($L425/2*($H425*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T425 > 0, $T425, ( $L425 / 2 * ( ( $I425 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T425 > 0, $T425,($L425/2*(($F425)*(Q425*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T425 > 0, $T425,($L425/2*($G425*(Q425*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T425 > 0, $T425,($L425/2*($H425*(Q425*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T425 > 0, $T425, ( $L425 / 2 * ( ( $I425 ) * (Q425*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T426>0,$T426,($L426/2*(($F426*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T426>0,$T426,($L426/2*($G426*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T426>0,$T426,($L426/2*($H426*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T426 > 0, $T426, ( $L426 / 2 * ( ( $I426 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T426 > 0, $T426,($L426/2*(($F426)*(Q426*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T426 > 0, $T426,($L426/2*($G426*(Q426*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T426 > 0, $T426,($L426/2*($H426*(Q426*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T426 > 0, $T426, ( $L426 / 2 * ( ( $I426 ) * (Q426*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T427>0,$T427,($L427/2*(($F427*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T427>0,$T427,($L427/2*($G427*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T427>0,$T427,($L427/2*($H427*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T427 > 0, $T427, ( $L427 / 2 * ( ( $I427 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T427 > 0, $T427,($L427/2*(($F427)*(Q427*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T427 > 0, $T427,($L427/2*($G427*(Q427*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T427 > 0, $T427,($L427/2*($H427*(Q427*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T427 > 0, $T427, ( $L427 / 2 * ( ( $I427 ) * (Q427*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T428>0,$T428,($L428/2*(($F428*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T428>0,$T428,($L428/2*($G428*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T428>0,$T428,($L428/2*($H428*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T428 > 0, $T428, ( $L428 / 2 * ( ( $I428 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T428 > 0, $T428,($L428/2*(($F428)*(Q428*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T428 > 0, $T428,($L428/2*($G428*(Q428*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T428 > 0, $T428,($L428/2*($H428*(Q428*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T428 > 0, $T428, ( $L428 / 2 * ( ( $I428 ) * (Q428*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T429>0,$T429,($L429/2*(($F429*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T429>0,$T429,($L429/2*($G429*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T429>0,$T429,($L429/2*($H429*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T429 > 0, $T429, ( $L429 / 2 * ( ( $I429 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T429 > 0, $T429,($L429/2*(($F429)*(Q429*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T429 > 0, $T429,($L429/2*($G429*(Q429*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T429 > 0, $T429,($L429/2*($H429*(Q429*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T429 > 0, $T429, ( $L429 / 2 * ( ( $I429 ) * (Q429*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T430>0,$T430,($L430/2*(($F430*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T430>0,$T430,($L430/2*($G430*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T430>0,$T430,($L430/2*($H430*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T430 > 0, $T430, ( $L430 / 2 * ( ( $I430 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T430 > 0, $T430,($L430/2*(($F430)*(Q430*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T430 > 0, $T430,($L430/2*($G430*(Q430*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T430 > 0, $T430,($L430/2*($H430*(Q430*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T430 > 0, $T430, ( $L430 / 2 * ( ( $I430 ) * (Q430*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T431>0,$T431,($L431/2*(($F431*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T431>0,$T431,($L431/2*($G431*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T431>0,$T431,($L431/2*($H431*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T431 > 0, $T431, ( $L431 / 2 * ( ( $I431 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T431 > 0, $T431,($L431/2*(($F431)*(Q431*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T431 > 0, $T431,($L431/2*($G431*(Q431*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T431 > 0, $T431,($L431/2*($H431*(Q431*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T431 > 0, $T431, ( $L431 / 2 * ( ( $I431 ) * (Q431*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T432>0,$T432,($L432/2*(($F432*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T432>0,$T432,($L432/2*($G432*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T432>0,$T432,($L432/2*($H432*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T432 > 0, $T432, ( $L432 / 2 * ( ( $I432 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T432 > 0, $T432,($L432/2*(($F432)*(Q432*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T432 > 0, $T432,($L432/2*($G432*(Q432*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T432 > 0, $T432,($L432/2*($H432*(Q432*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T432 > 0, $T432, ( $L432 / 2 * ( ( $I432 ) * (Q432*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T433>0,$T433,($L433/2*(($F433*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T433>0,$T433,($L433/2*($G433*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T433>0,$T433,($L433/2*($H433*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T433 > 0, $T433, ( $L433 / 2 * ( ( $I433 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T433 > 0, $T433,($L433/2*(($F433)*(Q433*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T433 > 0, $T433,($L433/2*($G433*(Q433*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T433 > 0, $T433,($L433/2*($H433*(Q433*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T433 > 0, $T433, ( $L433 / 2 * ( ( $I433 ) * (Q433*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T434>0,$T434,($L434/2*(($F434*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T434>0,$T434,($L434/2*($G434*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T434>0,$T434,($L434/2*($H434*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T434 > 0, $T434, ( $L434 / 2 * ( ( $I434 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T434 > 0, $T434,($L434/2*(($F434)*(Q434*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T434 > 0, $T434,($L434/2*($G434*(Q434*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T434 > 0, $T434,($L434/2*($H434*(Q434*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T434 > 0, $T434, ( $L434 / 2 * ( ( $I434 ) * (Q434*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T435>0,$T435,($L435/2*(($F435*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T435>0,$T435,($L435/2*($G435*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T435>0,$T435,($L435/2*($H435*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T435 > 0, $T435, ( $L435 / 2 * ( ( $I435 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T435 > 0, $T435,($L435/2*(($F435)*(Q435*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T435 > 0, $T435,($L435/2*($G435*(Q435*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T435 > 0, $T435,($L435/2*($H435*(Q435*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T435 > 0, $T435, ( $L435 / 2 * ( ( $I435 ) * (Q435*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T436>0,$T436,($L436/2*(($F436*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T436>0,$T436,($L436/2*($G436*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T436>0,$T436,($L436/2*($H436*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T436 > 0, $T436, ( $L436 / 2 * ( ( $I436 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T436 > 0, $T436,($L436/2*(($F436)*(Q436*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T436 > 0, $T436,($L436/2*($G436*(Q436*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T436 > 0, $T436,($L436/2*($H436*(Q436*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T436 > 0, $T436, ( $L436 / 2 * ( ( $I436 ) * (Q436*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T437>0,$T437,($L437/2*(($F437*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T437>0,$T437,($L437/2*($G437*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T437>0,$T437,($L437/2*($H437*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T437 > 0, $T437, ( $L437 / 2 * ( ( $I437 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T437 > 0, $T437,($L437/2*(($F437)*(Q437*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T437 > 0, $T437,($L437/2*($G437*(Q437*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T437 > 0, $T437,($L437/2*($H437*(Q437*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T437 > 0, $T437, ( $L437 / 2 * ( ( $I437 ) * (Q437*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T438>0,$T438,($L438/2*(($F438*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T438>0,$T438,($L438/2*($G438*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T438>0,$T438,($L438/2*($H438*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T438 > 0, $T438, ( $L438 / 2 * ( ( $I438 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T438 > 0, $T438,($L438/2*(($F438)*(Q438*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T438 > 0, $T438,($L438/2*($G438*(Q438*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T438 > 0, $T438,($L438/2*($H438*(Q438*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T438 > 0, $T438, ( $L438 / 2 * ( ( $I438 ) * (Q438*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T439>0,$T439,($L439/2*(($F439*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T439>0,$T439,($L439/2*($G439*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T439>0,$T439,($L439/2*($H439*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T439 > 0, $T439, ( $L439 / 2 * ( ( $I439 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T439 > 0, $T439,($L439/2*(($F439)*(Q439*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T439 > 0, $T439,($L439/2*($G439*(Q439*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T439 > 0, $T439,($L439/2*($H439*(Q439*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T439 > 0, $T439, ( $L439 / 2 * ( ( $I439 ) * (Q439*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,{"$f":"OFFSET(FANOUT,8,1)+OFFSET(FANOUT,9,1)*($K440-3)","v":8.1363158974999991E-4},null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T440>0,$T440,($L440/2*(($F440*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T440>0,$T440,($L440/2*($G440*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T440>0,$T440,($L440/2*($H440*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T440 > 0, $T440, ( $L440 / 2 * ( ( $I440 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T440 > 0, $T440,($L440/2*(($F440)*(Q440*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T440 > 0, $T440,($L440/2*($G440*(Q440*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T440 > 0, $T440,($L440/2*($H440*(Q440*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T440 > 0, $T440, ( $L440 / 2 * ( ( $I440 ) * (Q440*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,{"$f":"E441*J441","v":0},0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T441>0,$T441,($L441/2*(($F441*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T441>0,$T441,($L441/2*($G441*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T441>0,$T441,($L441/2*($H441*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T441 > 0, $T441, ( $L441 / 2 * ( ( $I441 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T441 > 0, $T441,($L441/2*(($F441)*(Q441*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T441 > 0, $T441,($L441/2*($G441*(Q441*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T441 > 0, $T441,($L441/2*($H441*(Q441*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T441 > 0, $T441, ( $L441 / 2 * ( ( $I441 ) * (Q441*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T442>0,$T442,($L442/2*(($F442*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T442>0,$T442,($L442/2*($G442*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T442>0,$T442,($L442/2*($H442*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T442 > 0, $T442, ( $L442 / 2 * ( ( $I442 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T442 > 0, $T442,($L442/2*(($F442)*(Q442*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T442 > 0, $T442,($L442/2*($G442*(Q442*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T442 > 0, $T442,($L442/2*($H442*(Q442*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T442 > 0, $T442, ( $L442 / 2 * ( ( $I442 ) * (Q442*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T443>0,$T443,($L443/2*(($F443*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T443>0,$T443,($L443/2*($G443*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T443>0,$T443,($L443/2*($H443*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T443 > 0, $T443, ( $L443 / 2 * ( ( $I443 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T443 > 0, $T443,($L443/2*(($F443)*(Q443*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T443 > 0, $T443,($L443/2*($G443*(Q443*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T443 > 0, $T443,($L443/2*($H443*(Q443*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T443 > 0, $T443, ( $L443 / 2 * ( ( $I443 ) * (Q443*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T444>0,$T444,($L444/2*(($F444*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T444>0,$T444,($L444/2*($G444*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T444>0,$T444,($L444/2*($H444*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T444 > 0, $T444, ( $L444 / 2 * ( ( $I444 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T444 > 0, $T444,($L444/2*(($F444)*(Q444*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T444 > 0, $T444,($L444/2*($G444*(Q444*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T444 > 0, $T444,($L444/2*($H444*(Q444*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T444 > 0, $T444, ( $L444 / 2 * ( ( $I444 ) * (Q444*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T445>0,$T445,($L445/2*(($F445*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T445>0,$T445,($L445/2*($G445*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T445>0,$T445,($L445/2*($H445*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T445 > 0, $T445, ( $L445 / 2 * ( ( $I445 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T445 > 0, $T445,($L445/2*(($F445)*(Q445*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T445 > 0, $T445,($L445/2*($G445*(Q445*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T445 > 0, $T445,($L445/2*($H445*(Q445*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T445 > 0, $T445, ( $L445 / 2 * ( ( $I445 ) * (Q445*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T446>0,$T446,($L446/2*(($F446*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T446>0,$T446,($L446/2*($G446*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T446>0,$T446,($L446/2*($H446*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T446 > 0, $T446, ( $L446 / 2 * ( ( $I446 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T446 > 0, $T446,($L446/2*(($F446)*(Q446*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T446 > 0, $T446,($L446/2*($G446*(Q446*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T446 > 0, $T446,($L446/2*($H446*(Q446*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T446 > 0, $T446, ( $L446 / 2 * ( ( $I446 ) * (Q446*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T447>0,$T447,($L447/2*(($F447*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T447>0,$T447,($L447/2*($G447*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T447>0,$T447,($L447/2*($H447*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T447 > 0, $T447, ( $L447 / 2 * ( ( $I447 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T447 > 0, $T447,($L447/2*(($F447)*(Q447*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T447 > 0, $T447,($L447/2*($G447*(Q447*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T447 > 0, $T447,($L447/2*($H447*(Q447*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T447 > 0, $T447, ( $L447 / 2 * ( ( $I447 ) * (Q447*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T448>0,$T448,($L448/2*(($F448*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T448>0,$T448,($L448/2*($G448*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T448>0,$T448,($L448/2*($H448*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T448 > 0, $T448, ( $L448 / 2 * ( ( $I448 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T448 > 0, $T448,($L448/2*(($F448)*(Q448*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T448 > 0, $T448,($L448/2*($G448*(Q448*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T448 > 0, $T448,($L448/2*($H448*(Q448*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T448 > 0, $T448, ( $L448 / 2 * ( ( $I448 ) * (Q448*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T449>0,$T449,($L449/2*(($F449*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T449>0,$T449,($L449/2*($G449*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T449>0,$T449,($L449/2*($H449*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T449 > 0, $T449, ( $L449 / 2 * ( ( $I449 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T449 > 0, $T449,($L449/2*(($F449)*(Q449*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T449 > 0, $T449,($L449/2*($G449*(Q449*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T449 > 0, $T449,($L449/2*($H449*(Q449*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T449 > 0, $T449, ( $L449 / 2 * ( ( $I449 ) * (Q449*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T450>0,$T450,($L450/2*(($F450*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T450>0,$T450,($L450/2*($G450*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T450>0,$T450,($L450/2*($H450*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T450 > 0, $T450, ( $L450 / 2 * ( ( $I450 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T450 > 0, $T450,($L450/2*(($F450)*(Q450*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T450 > 0, $T450,($L450/2*($G450*(Q450*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T450 > 0, $T450,($L450/2*($H450*(Q450*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T450 > 0, $T450, ( $L450 / 2 * ( ( $I450 ) * (Q450*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T451>0,$T451,($L451/2*(($F451*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T451>0,$T451,($L451/2*($G451*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T451>0,$T451,($L451/2*($H451*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T451 > 0, $T451, ( $L451 / 2 * ( ( $I451 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T451 > 0, $T451,($L451/2*(($F451)*(Q451*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T451 > 0, $T451,($L451/2*($G451*(Q451*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T451 > 0, $T451,($L451/2*($H451*(Q451*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T451 > 0, $T451, ( $L451 / 2 * ( ( $I451 ) * (Q451*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T452>0,$T452,($L452/2*(($F452*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T452>0,$T452,($L452/2*($G452*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T452>0,$T452,($L452/2*($H452*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T452 > 0, $T452, ( $L452 / 2 * ( ( $I452 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T452 > 0, $T452,($L452/2*(($F452)*(Q452*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T452 > 0, $T452,($L452/2*($G452*(Q452*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T452 > 0, $T452,($L452/2*($H452*(Q452*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T452 > 0, $T452, ( $L452 / 2 * ( ( $I452 ) * (Q452*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T453>0,$T453,($L453/2*(($F453*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T453>0,$T453,($L453/2*($G453*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T453>0,$T453,($L453/2*($H453*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T453 > 0, $T453, ( $L453 / 2 * ( ( $I453 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T453 > 0, $T453,($L453/2*(($F453)*(Q453*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T453 > 0, $T453,($L453/2*($G453*(Q453*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T453 > 0, $T453,($L453/2*($H453*(Q453*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T453 > 0, $T453, ( $L453 / 2 * ( ( $I453 ) * (Q453*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T454>0,$T454,($L454/2*(($F454*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T454>0,$T454,($L454/2*($G454*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T454>0,$T454,($L454/2*($H454*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T454 > 0, $T454, ( $L454 / 2 * ( ( $I454 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T454 > 0, $T454,($L454/2*(($F454)*(Q454*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T454 > 0, $T454,($L454/2*($G454*(Q454*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T454 > 0, $T454,($L454/2*($H454*(Q454*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T454 > 0, $T454, ( $L454 / 2 * ( ( $I454 ) * (Q454*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T455>0,$T455,($L455/2*(($F455*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T455>0,$T455,($L455/2*($G455*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T455>0,$T455,($L455/2*($H455*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T455 > 0, $T455, ( $L455 / 2 * ( ( $I455 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T455 > 0, $T455,($L455/2*(($F455)*(Q455*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T455 > 0, $T455,($L455/2*($G455*(Q455*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T455 > 0, $T455,($L455/2*($H455*(Q455*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T455 > 0, $T455, ( $L455 / 2 * ( ( $I455 ) * (Q455*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T456>0,$T456,($L456/2*(($F456*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T456>0,$T456,($L456/2*($G456*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T456>0,$T456,($L456/2*($H456*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T456 > 0, $T456, ( $L456 / 2 * ( ( $I456 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T456 > 0, $T456,($L456/2*(($F456)*(Q456*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T456 > 0, $T456,($L456/2*($G456*(Q456*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T456 > 0, $T456,($L456/2*($H456*(Q456*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T456 > 0, $T456, ( $L456 / 2 * ( ( $I456 ) * (Q456*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T457>0,$T457,($L457/2*(($F457*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T457>0,$T457,($L457/2*($G457*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T457>0,$T457,($L457/2*($H457*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T457 > 0, $T457, ( $L457 / 2 * ( ( $I457 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T457 > 0, $T457,($L457/2*(($F457)*(Q457*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T457 > 0, $T457,($L457/2*($G457*(Q457*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T457 > 0, $T457,($L457/2*($H457*(Q457*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T457 > 0, $T457, ( $L457 / 2 * ( ( $I457 ) * (Q457*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T458>0,$T458,($L458/2*(($F458*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T458>0,$T458,($L458/2*($G458*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T458>0,$T458,($L458/2*($H458*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T458 > 0, $T458, ( $L458 / 2 * ( ( $I458 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T458 > 0, $T458,($L458/2*(($F458)*(Q458*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T458 > 0, $T458,($L458/2*($G458*(Q458*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T458 > 0, $T458,($L458/2*($H458*(Q458*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T458 > 0, $T458, ( $L458 / 2 * ( ( $I458 ) * (Q458*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T459>0,$T459,($L459/2*(($F459*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T459>0,$T459,($L459/2*($G459*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T459>0,$T459,($L459/2*($H459*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T459 > 0, $T459, ( $L459 / 2 * ( ( $I459 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T459 > 0, $T459,($L459/2*(($F459)*(Q459*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T459 > 0, $T459,($L459/2*($G459*(Q459*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T459 > 0, $T459,($L459/2*($H459*(Q459*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T459 > 0, $T459, ( $L459 / 2 * ( ( $I459 ) * (Q459*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,{"$f":"IF(TRUE,SUM(AE460:AF460),(VCCINT/1000)*VCCINT_N*IF($R460>0,$R460,($L460/2*(($F460+$I460)*0.45*$U460+($F460*(OFFSET(FANOUT,8,2))+$G460*(OFFSET(FANOUT,8,4)+$U460)+$H460*(OFFSET(FANOUT,8,5)+$U460)+$I460*(OFFSET(FANOUT,8,3)))))*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1)","v":0},null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T460>0,$T460,($L460/2*(($F460*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T460>0,$T460,($L460/2*($G460*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T460>0,$T460,($L460/2*($H460*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T460 > 0, $T460, ( $L460 / 2 * ( ( $I460 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T460 > 0, $T460,($L460/2*(($F460)*(Q460*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T460 > 0, $T460,($L460/2*($G460*(Q460*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T460 > 0, $T460,($L460/2*($H460*(Q460*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T460 > 0, $T460, ( $L460 / 2 * ( ( $I460 ) * (Q460*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,{"$f":"10^(K461/10)-1","v":5.3095734448019343},null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T461>0,$T461,($L461/2*(($F461*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T461>0,$T461,($L461/2*($G461*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T461>0,$T461,($L461/2*($H461*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T461 > 0, $T461, ( $L461 / 2 * ( ( $I461 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T461 > 0, $T461,($L461/2*(($F461)*(Q461*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T461 > 0, $T461,($L461/2*($G461*(Q461*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T461 > 0, $T461,($L461/2*($H461*(Q461*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T461 > 0, $T461, ( $L461 / 2 * ( ( $I461 ) * (Q461*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"SUM(W461:Z461)","v":0},{"$f":"SUM(AA461:AD461)","v":0}]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T462>0,$T462,($L462/2*(($F462*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T462>0,$T462,($L462/2*($G462*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T462>0,$T462,($L462/2*($H462*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T462 > 0, $T462, ( $L462 / 2 * ( ( $I462 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T462 > 0, $T462,($L462/2*(($F462)*(Q462*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T462 > 0, $T462,($L462/2*($G462*(Q462*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T462 > 0, $T462,($L462/2*($H462*(Q462*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T462 > 0, $T462, ( $L462 / 2 * ( ( $I462 ) * (Q462*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T463>0,$T463,($L463/2*(($F463*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T463>0,$T463,($L463/2*($G463*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T463>0,$T463,($L463/2*($H463*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T463 > 0, $T463, ( $L463 / 2 * ( ( $I463 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T463 > 0, $T463,($L463/2*(($F463)*(Q463*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T463 > 0, $T463,($L463/2*($G463*(Q463*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T463 > 0, $T463,($L463/2*($H463*(Q463*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T463 > 0, $T463, ( $L463 / 2 * ( ( $I463 ) * (Q463*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T464>0,$T464,($L464/2*(($F464*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T464>0,$T464,($L464/2*($G464*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T464>0,$T464,($L464/2*($H464*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T464 > 0, $T464, ( $L464 / 2 * ( ( $I464 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T464 > 0, $T464,($L464/2*(($F464)*(Q464*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T464 > 0, $T464,($L464/2*($G464*(Q464*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T464 > 0, $T464,($L464/2*($H464*(Q464*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T464 > 0, $T464, ( $L464 / 2 * ( ( $I464 ) * (Q464*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T465>0,$T465,($L465/2*(($F465*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T465>0,$T465,($L465/2*($G465*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T465>0,$T465,($L465/2*($H465*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T465 > 0, $T465, ( $L465 / 2 * ( ( $I465 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T465 > 0, $T465,($L465/2*(($F465)*(Q465*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T465 > 0, $T465,($L465/2*($G465*(Q465*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T465 > 0, $T465,($L465/2*($H465*(Q465*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T465 > 0, $T465, ( $L465 / 2 * ( ( $I465 ) * (Q465*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T466>0,$T466,($L466/2*(($F466*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T466>0,$T466,($L466/2*($G466*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T466>0,$T466,($L466/2*($H466*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T466 > 0, $T466, ( $L466 / 2 * ( ( $I466 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T466 > 0, $T466,($L466/2*(($F466)*(Q466*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T466 > 0, $T466,($L466/2*($G466*(Q466*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T466 > 0, $T466,($L466/2*($H466*(Q466*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T466 > 0, $T466, ( $L466 / 2 * ( ( $I466 ) * (Q466*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T467>0,$T467,($L467/2*(($F467*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T467>0,$T467,($L467/2*($G467*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T467>0,$T467,($L467/2*($H467*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T467 > 0, $T467, ( $L467 / 2 * ( ( $I467 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T467 > 0, $T467,($L467/2*(($F467)*(Q467*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T467 > 0, $T467,($L467/2*($G467*(Q467*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T467 > 0, $T467,($L467/2*($H467*(Q467*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T467 > 0, $T467, ( $L467 / 2 * ( ( $I467 ) * (Q467*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T468>0,$T468,($L468/2*(($F468*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T468>0,$T468,($L468/2*($G468*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T468>0,$T468,($L468/2*($H468*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T468 > 0, $T468, ( $L468 / 2 * ( ( $I468 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T468 > 0, $T468,($L468/2*(($F468)*(Q468*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T468 > 0, $T468,($L468/2*($G468*(Q468*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T468 > 0, $T468,($L468/2*($H468*(Q468*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T468 > 0, $T468, ( $L468 / 2 * ( ( $I468 ) * (Q468*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T469>0,$T469,($L469/2*(($F469*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T469>0,$T469,($L469/2*($G469*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T469>0,$T469,($L469/2*($H469*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T469 > 0, $T469, ( $L469 / 2 * ( ( $I469 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T469 > 0, $T469,($L469/2*(($F469)*(Q469*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T469 > 0, $T469,($L469/2*($G469*(Q469*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T469 > 0, $T469,($L469/2*($H469*(Q469*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T469 > 0, $T469, ( $L469 / 2 * ( ( $I469 ) * (Q469*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T470>0,$T470,($L470/2*(($F470*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T470>0,$T470,($L470/2*($G470*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T470>0,$T470,($L470/2*($H470*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T470 > 0, $T470, ( $L470 / 2 * ( ( $I470 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T470 > 0, $T470,($L470/2*(($F470)*(Q470*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T470 > 0, $T470,($L470/2*($G470*(Q470*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T470 > 0, $T470,($L470/2*($H470*(Q470*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T470 > 0, $T470, ( $L470 / 2 * ( ( $I470 ) * (Q470*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T471>0,$T471,($L471/2*(($F471*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T471>0,$T471,($L471/2*($G471*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T471>0,$T471,($L471/2*($H471*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T471 > 0, $T471, ( $L471 / 2 * ( ( $I471 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T471 > 0, $T471,($L471/2*(($F471)*(Q471*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T471 > 0, $T471,($L471/2*($G471*(Q471*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T471 > 0, $T471,($L471/2*($H471*(Q471*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T471 > 0, $T471, ( $L471 / 2 * ( ( $I471 ) * (Q471*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,{"$f":"OFFSET(FANOUT,8,1)+OFFSET(FANOUT,9,1)*($K472-3)","v":8.1363158974999991E-4},null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T472>0,$T472,($L472/2*(($F472*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T472>0,$T472,($L472/2*($G472*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T472>0,$T472,($L472/2*($H472*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T472 > 0, $T472, ( $L472 / 2 * ( ( $I472 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T472 > 0, $T472,($L472/2*(($F472)*(Q472*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T472 > 0, $T472,($L472/2*($G472*(Q472*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T472 > 0, $T472,($L472/2*($H472*(Q472*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T472 > 0, $T472, ( $L472 / 2 * ( ( $I472 ) * (Q472*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T473>0,$T473,($L473/2*(($F473*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T473>0,$T473,($L473/2*($G473*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T473>0,$T473,($L473/2*($H473*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T473 > 0, $T473, ( $L473 / 2 * ( ( $I473 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T473 > 0, $T473,($L473/2*(($F473)*(Q473*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T473 > 0, $T473,($L473/2*($G473*(Q473*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T473 > 0, $T473,($L473/2*($H473*(Q473*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T473 > 0, $T473, ( $L473 / 2 * ( ( $I473 ) * (Q473*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T474>0,$T474,($L474/2*(($F474*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T474>0,$T474,($L474/2*($G474*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T474>0,$T474,($L474/2*($H474*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T474 > 0, $T474, ( $L474 / 2 * ( ( $I474 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T474 > 0, $T474,($L474/2*(($F474)*(Q474*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T474 > 0, $T474,($L474/2*($G474*(Q474*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T474 > 0, $T474,($L474/2*($H474*(Q474*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T474 > 0, $T474, ( $L474 / 2 * ( ( $I474 ) * (Q474*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T475>0,$T475,($L475/2*(($F475*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T475>0,$T475,($L475/2*($G475*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T475>0,$T475,($L475/2*($H475*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T475 > 0, $T475, ( $L475 / 2 * ( ( $I475 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T475 > 0, $T475,($L475/2*(($F475)*(Q475*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T475 > 0, $T475,($L475/2*($G475*(Q475*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T475 > 0, $T475,($L475/2*($H475*(Q475*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T475 > 0, $T475, ( $L475 / 2 * ( ( $I475 ) * (Q475*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T476>0,$T476,($L476/2*(($F476*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T476>0,$T476,($L476/2*($G476*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T476>0,$T476,($L476/2*($H476*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T476 > 0, $T476, ( $L476 / 2 * ( ( $I476 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T476 > 0, $T476,($L476/2*(($F476)*(Q476*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T476 > 0, $T476,($L476/2*($G476*(Q476*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T476 > 0, $T476,($L476/2*($H476*(Q476*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T476 > 0, $T476, ( $L476 / 2 * ( ( $I476 ) * (Q476*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T477>0,$T477,($L477/2*(($F477*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T477>0,$T477,($L477/2*($G477*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T477>0,$T477,($L477/2*($H477*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T477 > 0, $T477, ( $L477 / 2 * ( ( $I477 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T477 > 0, $T477,($L477/2*(($F477)*(Q477*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T477 > 0, $T477,($L477/2*($G477*(Q477*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T477 > 0, $T477,($L477/2*($H477*(Q477*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T477 > 0, $T477, ( $L477 / 2 * ( ( $I477 ) * (Q477*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T478>0,$T478,($L478/2*(($F478*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T478>0,$T478,($L478/2*($G478*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T478>0,$T478,($L478/2*($H478*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T478 > 0, $T478, ( $L478 / 2 * ( ( $I478 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T478 > 0, $T478,($L478/2*(($F478)*(Q478*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T478 > 0, $T478,($L478/2*($G478*(Q478*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T478 > 0, $T478,($L478/2*($H478*(Q478*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T478 > 0, $T478, ( $L478 / 2 * ( ( $I478 ) * (Q478*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T479>0,$T479,($L479/2*(($F479*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T479>0,$T479,($L479/2*($G479*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T479>0,$T479,($L479/2*($H479*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T479 > 0, $T479, ( $L479 / 2 * ( ( $I479 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T479 > 0, $T479,($L479/2*(($F479)*(Q479*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T479 > 0, $T479,($L479/2*($G479*(Q479*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T479 > 0, $T479,($L479/2*($H479*(Q479*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T479 > 0, $T479, ( $L479 / 2 * ( ( $I479 ) * (Q479*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T480>0,$T480,($L480/2*(($F480*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T480>0,$T480,($L480/2*($G480*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T480>0,$T480,($L480/2*($H480*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T480 > 0, $T480, ( $L480 / 2 * ( ( $I480 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T480 > 0, $T480,($L480/2*(($F480)*(Q480*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T480 > 0, $T480,($L480/2*($G480*(Q480*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T480 > 0, $T480,($L480/2*($H480*(Q480*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T480 > 0, $T480, ( $L480 / 2 * ( ( $I480 ) * (Q480*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T481>0,$T481,($L481/2*(($F481*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T481>0,$T481,($L481/2*($G481*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T481>0,$T481,($L481/2*($H481*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T481 > 0, $T481, ( $L481 / 2 * ( ( $I481 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T481 > 0, $T481,($L481/2*(($F481)*(Q481*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T481 > 0, $T481,($L481/2*($G481*(Q481*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T481 > 0, $T481,($L481/2*($H481*(Q481*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T481 > 0, $T481, ( $L481 / 2 * ( ( $I481 ) * (Q481*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T482>0,$T482,($L482/2*(($F482*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T482>0,$T482,($L482/2*($G482*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T482>0,$T482,($L482/2*($H482*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T482 > 0, $T482, ( $L482 / 2 * ( ( $I482 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T482 > 0, $T482,($L482/2*(($F482)*(Q482*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T482 > 0, $T482,($L482/2*($G482*(Q482*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T482 > 0, $T482,($L482/2*($H482*(Q482*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T482 > 0, $T482, ( $L482 / 2 * ( ( $I482 ) * (Q482*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T483>0,$T483,($L483/2*(($F483*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T483>0,$T483,($L483/2*($G483*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T483>0,$T483,($L483/2*($H483*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T483 > 0, $T483, ( $L483 / 2 * ( ( $I483 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T483 > 0, $T483,($L483/2*(($F483)*(Q483*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T483 > 0, $T483,($L483/2*($G483*(Q483*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T483 > 0, $T483,($L483/2*($H483*(Q483*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T483 > 0, $T483, ( $L483 / 2 * ( ( $I483 ) * (Q483*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T484>0,$T484,($L484/2*(($F484*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T484>0,$T484,($L484/2*($G484*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T484>0,$T484,($L484/2*($H484*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T484 > 0, $T484, ( $L484 / 2 * ( ( $I484 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T484 > 0, $T484,($L484/2*(($F484)*(Q484*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T484 > 0, $T484,($L484/2*($G484*(Q484*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T484 > 0, $T484,($L484/2*($H484*(Q484*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T484 > 0, $T484, ( $L484 / 2 * ( ( $I484 ) * (Q484*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T485>0,$T485,($L485/2*(($F485*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T485>0,$T485,($L485/2*($G485*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T485>0,$T485,($L485/2*($H485*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T485 > 0, $T485, ( $L485 / 2 * ( ( $I485 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T485 > 0, $T485,($L485/2*(($F485)*(Q485*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T485 > 0, $T485,($L485/2*($G485*(Q485*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T485 > 0, $T485,($L485/2*($H485*(Q485*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T485 > 0, $T485, ( $L485 / 2 * ( ( $I485 ) * (Q485*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T486>0,$T486,($L486/2*(($F486*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T486>0,$T486,($L486/2*($G486*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T486>0,$T486,($L486/2*($H486*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T486 > 0, $T486, ( $L486 / 2 * ( ( $I486 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T486 > 0, $T486,($L486/2*(($F486)*(Q486*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T486 > 0, $T486,($L486/2*($G486*(Q486*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T486 > 0, $T486,($L486/2*($H486*(Q486*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T486 > 0, $T486, ( $L486 / 2 * ( ( $I486 ) * (Q486*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T487>0,$T487,($L487/2*(($F487*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T487>0,$T487,($L487/2*($G487*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T487>0,$T487,($L487/2*($H487*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T487 > 0, $T487, ( $L487 / 2 * ( ( $I487 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T487 > 0, $T487,($L487/2*(($F487)*(Q487*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T487 > 0, $T487,($L487/2*($G487*(Q487*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T487 > 0, $T487,($L487/2*($H487*(Q487*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T487 > 0, $T487, ( $L487 / 2 * ( ( $I487 ) * (Q487*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T488>0,$T488,($L488/2*(($F488*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T488>0,$T488,($L488/2*($G488*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T488>0,$T488,($L488/2*($H488*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T488 > 0, $T488, ( $L488 / 2 * ( ( $I488 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T488 > 0, $T488,($L488/2*(($F488)*(Q488*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T488 > 0, $T488,($L488/2*($G488*(Q488*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T488 > 0, $T488,($L488/2*($H488*(Q488*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T488 > 0, $T488, ( $L488 / 2 * ( ( $I488 ) * (Q488*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T489>0,$T489,($L489/2*(($F489*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T489>0,$T489,($L489/2*($G489*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T489>0,$T489,($L489/2*($H489*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T489 > 0, $T489, ( $L489 / 2 * ( ( $I489 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T489 > 0, $T489,($L489/2*(($F489)*(Q489*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T489 > 0, $T489,($L489/2*($G489*(Q489*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T489 > 0, $T489,($L489/2*($H489*(Q489*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T489 > 0, $T489, ( $L489 / 2 * ( ( $I489 ) * (Q489*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T490>0,$T490,($L490/2*(($F490*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T490>0,$T490,($L490/2*($G490*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T490>0,$T490,($L490/2*($H490*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T490 > 0, $T490, ( $L490 / 2 * ( ( $I490 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T490 > 0, $T490,($L490/2*(($F490)*(Q490*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T490 > 0, $T490,($L490/2*($G490*(Q490*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T490 > 0, $T490,($L490/2*($H490*(Q490*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T490 > 0, $T490, ( $L490 / 2 * ( ( $I490 ) * (Q490*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T491>0,$T491,($L491/2*(($F491*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T491>0,$T491,($L491/2*($G491*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T491>0,$T491,($L491/2*($H491*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T491 > 0, $T491, ( $L491 / 2 * ( ( $I491 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T491 > 0, $T491,($L491/2*(($F491)*(Q491*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T491 > 0, $T491,($L491/2*($G491*(Q491*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T491 > 0, $T491,($L491/2*($H491*(Q491*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T491 > 0, $T491, ( $L491 / 2 * ( ( $I491 ) * (Q491*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T492>0,$T492,($L492/2*(($F492*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T492>0,$T492,($L492/2*($G492*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T492>0,$T492,($L492/2*($H492*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T492 > 0, $T492, ( $L492 / 2 * ( ( $I492 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T492 > 0, $T492,($L492/2*(($F492)*(Q492*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T492 > 0, $T492,($L492/2*($G492*(Q492*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T492 > 0, $T492,($L492/2*($H492*(Q492*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T492 > 0, $T492, ( $L492 / 2 * ( ( $I492 ) * (Q492*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T493>0,$T493,($L493/2*(($F493*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T493>0,$T493,($L493/2*($G493*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T493>0,$T493,($L493/2*($H493*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T493 > 0, $T493, ( $L493 / 2 * ( ( $I493 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T493 > 0, $T493,($L493/2*(($F493)*(Q493*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T493 > 0, $T493,($L493/2*($G493*(Q493*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T493 > 0, $T493,($L493/2*($H493*(Q493*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T493 > 0, $T493, ( $L493 / 2 * ( ( $I493 ) * (Q493*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T494>0,$T494,($L494/2*(($F494*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T494>0,$T494,($L494/2*($G494*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T494>0,$T494,($L494/2*($H494*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T494 > 0, $T494, ( $L494 / 2 * ( ( $I494 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T494 > 0, $T494,($L494/2*(($F494)*(Q494*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T494 > 0, $T494,($L494/2*($G494*(Q494*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T494 > 0, $T494,($L494/2*($H494*(Q494*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T494 > 0, $T494, ( $L494 / 2 * ( ( $I494 ) * (Q494*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T495>0,$T495,($L495/2*(($F495*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T495>0,$T495,($L495/2*($G495*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T495>0,$T495,($L495/2*($H495*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T495 > 0, $T495, ( $L495 / 2 * ( ( $I495 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T495 > 0, $T495,($L495/2*(($F495)*(Q495*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T495 > 0, $T495,($L495/2*($G495*(Q495*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T495 > 0, $T495,($L495/2*($H495*(Q495*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T495 > 0, $T495, ( $L495 / 2 * ( ( $I495 ) * (Q495*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T496>0,$T496,($L496/2*(($F496*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T496>0,$T496,($L496/2*($G496*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T496>0,$T496,($L496/2*($H496*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T496 > 0, $T496, ( $L496 / 2 * ( ( $I496 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T496 > 0, $T496,($L496/2*(($F496)*(Q496*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T496 > 0, $T496,($L496/2*($G496*(Q496*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T496 > 0, $T496,($L496/2*($H496*(Q496*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T496 > 0, $T496, ( $L496 / 2 * ( ( $I496 ) * (Q496*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T497>0,$T497,($L497/2*(($F497*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T497>0,$T497,($L497/2*($G497*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T497>0,$T497,($L497/2*($H497*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T497 > 0, $T497, ( $L497 / 2 * ( ( $I497 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T497 > 0, $T497,($L497/2*(($F497)*(Q497*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T497 > 0, $T497,($L497/2*($G497*(Q497*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T497 > 0, $T497,($L497/2*($H497*(Q497*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T497 > 0, $T497, ( $L497 / 2 * ( ( $I497 ) * (Q497*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T498>0,$T498,($L498/2*(($F498*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T498>0,$T498,($L498/2*($G498*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T498>0,$T498,($L498/2*($H498*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T498 > 0, $T498, ( $L498 / 2 * ( ( $I498 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T498 > 0, $T498,($L498/2*(($F498)*(Q498*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T498 > 0, $T498,($L498/2*($G498*(Q498*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T498 > 0, $T498,($L498/2*($H498*(Q498*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T498 > 0, $T498, ( $L498 / 2 * ( ( $I498 ) * (Q498*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T499>0,$T499,($L499/2*(($F499*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T499>0,$T499,($L499/2*($G499*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T499>0,$T499,($L499/2*($H499*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T499 > 0, $T499, ( $L499 / 2 * ( ( $I499 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T499 > 0, $T499,($L499/2*(($F499)*(Q499*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T499 > 0, $T499,($L499/2*($G499*(Q499*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T499 > 0, $T499,($L499/2*($H499*(Q499*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T499 > 0, $T499, ( $L499 / 2 * ( ( $I499 ) * (Q499*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,null,null,null,null,null,null,null,null,0.125,8,0,0,null,0,0,5.3095734448019343,null,null,null,8.1363158974999991E-4,null,{"$f":"(VCCINT/1000)*VCCINT*(IF($T500>0,$T500,($L500/2*(($F500*(Data!$N$435)))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1))","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T500>0,$T500,($L500/2*($G500*(Data!$P$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T500>0,$T500,($L500/2*($H500*(Data!$Q$435))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T500 > 0, $T500, ( $L500 / 2 * ( ( $I500 * ( Data!$O$435 ) ) ) ) *OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T500 > 0, $T500,($L500/2*(($F500)*(Q500*Data!$N$436+Data!$N$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T500 > 0, $T500,($L500/2*($G500*(Q500*Data!$P$436+Data!$P$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"(VCCINT/1000)*VCCINT*(IF($T500 > 0, $T500,($L500/2*($H500*(Q500*Data!$Q$436+Data!$Q$437))))*\nOFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),2))*$U$1","v":0},{"$f":"( VCCINT / 1000 ) * VCCINT * ( IF( $T500 > 0, $T500, ( $L500 / 2 * ( ( $I500 ) * (Q500*Data!$O$436+Data!$O$437)  ) ) * OFFSET( POWER_OPT, OFFSET( OPTIMIZATION, 0, 3), 2)) * $U$1 )","v":0},0,0]
[null,{"$f":"ROW(LOGICROWS)-12","v":489}]

{"sheet":"IO","index":6,"n_rows":555,"n_cols":87,"rows_kept":555,"cut":false,"hidden":false,"merged":[[4,18,4,20],[498,1,498,3],[498,5,498,7],[493,1,493,3],[493,5,493,7],[494,1,494,3],[494,5,494,7],[495,1,495,3],[495,5,495,7],[496,1,496,3],[496,5,496,7],[497,1,497,3],[497,5,497,7],[488,1,488,3],[488,5,488,7],[489,1,489,3],[489,5,489,7],[490,1,490,3],[490,5,490,7],[491,1,491,3],[491,5,491,7],[492,1,492,3],[492,5,492,7],[483,1,483,3],[483,5,483,7],[484,1,484,3],[484,5,484,7],[485,1,485,3],[485,5,485,7],[486,1,486,3],[486,5,486,7],[487,1,487,3],[478,1,478,3],[478,5,478,7],[479,1,479,3],[479,5,479,7],[480,1,480,3],[480,5,480,7],[481,1,481,3],[481,5,481,7],[482,1,482,3],[482,5,482,7],[473,1,473,3],[473,5,473,7],[474,1,474,3],[474,5,474,7],[475,1,475,3],[475,5,475,7],[476,1,476,3],[476,5,476,7],[477,1,477,3],[477,5,477,7],[468,1,468,3],[468,5,468,7],[469,1,469,3],[469,5,469,7],[470,1,470,3],[470,5,470,7],[471,1,471,3],[471,5,471,7],[472,1,472,3],[472,5,472,7],[463,1,463,3],[463,5,463,7],[464,1,464,3],[464,5,464,7],[465,1,465,3],[465,5,465,7],[466,1,466,3],[466,5,466,7],[467,1,467,3],[467,5,467,7],[458,1,458,3],[458,5,458,7],[459,1,459,3],[459,5,459,7],[460,1,460,3],[460,5,460,7],[461,1,461,3],[461,5,461,7],[462,1,462,3],[462,5,462,7],[451,1,451,3],[451,5,451,7],[452,1,452,3],[452,5,452,7],[453,1,453,3],[453,5,453,7],[454,1,454,3],[454,5,454,7],[457,1,457,3],[457,5,457,7],[456,1,456,3],[456,5,456,7],[428,1,428,3],[428,5,428,7],[429,1,429,3],[429,5,429,7],[433,1,433,3],[433,5,433,7],[434,1,434,3],[434,5,434,7],[439,1,439,3],[439,5,439,7],[430,1,430,3],[430,5,430,7],[431,1,431,3],[431,5,431,7],[432,1,432,3],[432,5,432,7],[455,1,455,3],[455,5,455,7],[444,1,444,3],[444,5,444,7],[435,1,435,3],[435,5,435,7],[436,1,436,3],[436,5,436,7],[437,1,437,3],[437,5,437,7],[438,1,438,3],[438,5,438,7],[375,1,375,3],[375,5,375,7],[421,1,421,3],[421,5,421,7],[422,1,422,3],[422,5,422,7],[423,1,423,3],[423,5,423,7],[424,1,424,3],[424,5,424,7],[427,1,427,3],[427,5,427,7],[398,1,398,3],[398,5,398,7],[399,1,399,3],[399,5,399,7],[403,1,403,3],[403,5,403,7],[404,1,404,3],[404,5,404,7],[409,1,409,3],[409,5,409,7],[425,1,425,3],[425,5,425,7],[426,1,426,3],[426,5,426,7],[420,1,420,3],[420,5,420,7],[415,1,415,3],[415,5,415,7],[405,1,405,3],[405,5,405,7],[353,1,353,3],[353,5,353,7],[354,1,354,3],[354,5,354,7],[346,1,346,3],[346,5,346,7],[347,1,347,3],[347,5,347,7],[359,1,359,3],[359,5,359,7],[350,1,350,3],[350,5,350,7],[391,1,391,3],[391,5,391,7],[392,1,392,3],[392,5,392,7],[393,1,393,3],[393,5,393,7],[368,1,368,3],[368,5,368,7],[369,1,369,3],[369,5,369,7],[373,1,373,3],[373,5,373,7],[374,1,374,3],[374,5,374,7],[379,1,379,3],[379,5,379,7],[380,1,380,3],[380,5,380,7],[381,1,381,3],[381,5,381,7],[285,1,285,3],[285,5,285,7],[331,1,331,3],[331,5,331,7],[332,1,332,3],[332,5,332,7],[333,1,333,3],[333,5,333,7],[334,1,334,3],[334,5,334,7],[337,1,337,3],[337,5,337,7],[308,1,308,3],[308,5,308,7],[309,1,309,3],[309,5,309,7],[313,1,313,3],[313,5,313,7],[314,1,314,3],[314,5,314,7],[319,1,319,3],[319,5,319,7],[335,1,335,3],[335,5,335,7],[336,1,336,3],[336,5,336,7],[330,1,330,3],[330,5,330,7],[325,1,325,3],[325,5,325,7],[315,1,315,3],[315,5,315,7],[256,1,256,3],[256,5,256,7],[257,1,257,3],[257,5,257,7],[269,1,269,3],[269,5,269,7],[260,1,260,3],[260,5,260,7],[301,1,301,3],[301,5,301,7],[302,1,302,3],[302,5,302,7],[303,1,303,3],[303,5,303,7],[304,1,304,3],[304,5,304,7],[307,1,307,3],[307,5,307,7],[278,1,278,3],[278,5,278,7],[279,1,279,3],[279,5,279,7],[283,1,283,3],[283,5,283,7],[284,1,284,3],[284,5,284,7],[289,1,289,3],[289,5,289,7],[290,1,290,3],[290,5,290,7],[291,1,291,3],[291,5,291,7],[259,1,259,3],[259,5,259,7],[265,1,265,3],[265,5,265,7],[266,1,266,3],[266,5,266,7],[267,1,267,3],[267,5,267,7],[268,1,268,3],[268,5,268,7],[261,1,261,3],[261,5,261,7],[262,1,262,3],[262,5,262,7],[263,1,263,3],[263,5,263,7],[264,1,264,3],[264,5,264,7],[195,1,195,3],[195,5,195,7],[241,1,241,3],[241,5,241,7],[242,1,242,3],[242,5,242,7],[243,1,243,3],[243,5,243,7],[244,1,244,3],[244,5,244,7],[247,1,247,3],[247,5,247,7],[218,1,218,3],[218,5,218,7],[219,1,219,3],[219,5,219,7],[223,1,223,3],[223,5,223,7],[224,1,224,3],[224,5,224,7],[229,1,229,3],[229,5,229,7],[245,1,245,3],[245,5,245,7],[246,1,246,3],[246,5,246,7],[240,1,240,3],[240,5,240,7],[235,1,235,3],[235,5,235,7],[225,1,225,3],[225,5,225,7],[179,1,179,3],[179,5,179,7],[170,1,170,3],[170,5,170,7],[211,1,211,3],[211,5,211,7],[212,1,212,3],[212,5,212,7],[213,1,213,3],[213,5,213,7],[214,1,214,3],[214,5,214,7],[217,1,217,3],[217,5,217,7],[188,1,188,3],[188,5,188,7],[189,1,189,3],[189,5,189,7],[193,1,193,3],[193,5,193,7],[194,1,194,3],[194,5,194,7],[199,1,199,3],[199,5,199,7],[200,1,200,3],[200,5,200,7],[201,1,201,3],[201,5,201,7],[202,1,202,3],[202,5,202,7],[203,1,203,3],[203,5,203,7],[163,1,163,3],[163,5,163,7],[164,1,164,3],[164,5,164,7],[169,1,169,3],[169,5,169,7],[175,1,175,3],[175,5,175,7],[176,1,176,3],[176,5,176,7],[177,1,177,3],[177,5,177,7],[178,1,178,3],[178,5,178,7],[171,1,171,3],[171,5,171,7],[172,1,172,3],[172,5,172,7],[173,1,173,3],[173,5,173,7],[174,1,174,3],[174,5,174,7],[165,1,165,3],[165,5,165,7],[166,1,166,3],[166,5,166,7],[167,1,167,3],[167,5,167,7],[168,1,168,3],[168,5,168,7],[139,1,139,3],[139,5,139,7],[155,1,155,3],[155,5,155,7],[156,1,156,3],[156,5,156,7],[150,1,150,3],[150,5,150,7],[145,1,145,3],[145,5,145,7],[146,1,146,3],[146,5,146,7],[147,1,147,3],[147,5,147,7],[158,1,158,3],[158,5,158,7],[159,1,159,3],[159,5,159,7],[103,1,103,3],[103,5,103,7],[104,1,104,3],[104,5,104,7],[109,1,109,3],[109,5,109,7],[110,1,110,3],[110,5,110,7],[111,1,111,3],[111,5,111,7],[112,1,112,3],[112,5,112,7],[113,1,113,3],[113,5,113,7],[114,1,114,3],[114,5,114,7],[105,1,105,3],[105,5,105,7],[61,1,61,3],[61,5,61,7],[62,1,62,3],[62,5,62,7],[63,1,63,3],[63,5,63,7],[64,1,64,3],[64,5,64,7],[67,1,67,3],[67,5,67,7],[68,1,68,3],[68,5,68,7],[69,1,69,3],[69,5,69,7],[73,1,73,3],[73,5,73,7],[74,1,74,3],[74,5,74,7],[121,1,121,3],[121,5,121,7],[122,1,122,3],[122,5,122,7],[123,1,123,3],[123,5,123,7],[124,1,124,3],[124,5,124,7],[127,1,127,3],[127,5,127,7],[79,1,79,3],[79,5,79,7],[450,1,450,3],[450,5,450,7],[445,1,445,3],[445,5,445,7],[446,1,446,3],[446,5,446,7],[447,1,447,3],[447,5,447,7],[448,1,448,3],[448,5,448,7],[449,1,449,3],[449,5,449,7],[440,1,440,3],[440,5,440,7],[441,1,441,3],[441,5,441,7],[442,1,442,3],[442,5,442,7],[443,1,443,3],[443,5,443,7],[418,1,418,3],[418,5,418,7],[419,1,419,3],[419,5,419,7],[410,1,410,3],[410,5,410,7],[411,1,411,3],[411,5,411,7],[412,1,412,3],[412,5,412,7],[413,1,413,3],[413,5,413,7],[414,1,414,3],[414,5,414,7],[406,1,406,3],[406,5,406,7],[407,1,407,3],[407,5,407,7],[408,1,408,3],[408,5,408,7],[416,1,416,3],[416,5,416,7],[417,1,417,3],[417,5,417,7],[400,1,400,3],[400,5,400,7],[401,1,401,3],[401,5,401,7],[402,1,402,3],[402,5,402,7],[395,1,395,3],[395,5,395,7],[396,1,396,3],[396,5,396,7],[390,1,390,3],[390,5,390,7],[385,1,385,3],[385,5,385,7],[386,1,386,3],[386,5,386,7],[387,1,387,3],[387,5,387,7],[388,1,388,3],[388,5,388,7],[389,1,389,3],[389,5,389,7],[394,1,394,3],[394,5,394,7],[397,1,397,3],[397,5,397,7],[367,1,367,3],[367,5,367,7],[348,1,348,3],[348,5,348,7],[376,1,376,3],[376,5,376,7],[377,1,377,3],[377,5,377,7],[378,1,378,3],[378,5,378,7],[382,1,382,3],[382,5,382,7],[383,1,383,3],[383,5,383,7],[384,1,384,3],[384,5,384,7],[370,1,370,3],[370,5,370,7],[371,1,371,3],[371,5,371,7],[372,1,372,3],[372,5,372,7],[349,1,349,3],[349,5,349,7],[355,1,355,3],[355,5,355,7],[356,1,356,3],[356,5,356,7],[357,1,357,3],[357,5,357,7],[358,1,358,3],[358,5,358,7],[320,1,320,3],[320,5,320,7],[321,1,321,3],[321,5,321,7],[322,1,322,3],[322,5,322,7],[323,1,323,3],[323,5,323,7],[324,1,324,3],[324,5,324,7],[338,1,338,3],[338,5,338,7],[339,1,339,3],[339,5,339,7],[365,1,365,3],[365,5,365,7],[366,1,366,3],[366,5,366,7],[360,1,360,3],[360,5,360,7],[361,1,361,3],[361,5,361,7],[362,1,362,3],[362,5,362,7],[363,1,363,3],[363,5,363,7],[364,1,364,3],[364,5,364,7],[351,1,351,3],[351,5,351,7],[352,1,352,3],[352,5,352,7],[343,1,343,3],[343,5,343,7],[344,1,344,3],[344,5,344,7],[345,1,345,3],[345,5,345,7],[316,1,316,3],[316,5,316,7],[317,1,317,3],[317,5,317,7],[318,1,318,3],[318,5,318,7],[326,1,326,3],[326,5,326,7],[327,1,327,3],[327,5,327,7],[310,1,310,3],[310,5,310,7],[311,1,311,3],[311,5,311,7],[312,1,312,3],[312,5,312,7],[340,1,340,3],[340,5,340,7],[341,1,341,3],[341,5,341,7],[342,1,342,3],[342,5,342,7],[328,1,328,3],[328,5,328,7],[329,1,329,3],[329,5,329,7],[305,1,305,3],[305,5,305,7],[306,1,306,3],[306,5,306,7],[300,1,300,3],[300,5,300,7],[295,1,295,3],[295,5,295,7],[296,1,296,3],[296,5,296,7],[297,1,297,3],[297,5,297,7],[298,1,298,3],[298,5,298,7],[299,1,299,3],[299,5,299,7],[286,1,286,3],[286,5,286,7],[287,1,287,3],[287,5,287,7],[288,1,288,3],[288,5,288,7],[292,1,292,3],[292,5,292,7],[293,1,293,3],[293,5,293,7],[294,1,294,3],[294,5,294,7],[280,1,280,3],[280,5,280,7],[281,1,281,3],[281,5,281,7],[282,1,282,3],[282,5,282,7],[275,1,275,3],[275,5,275,7],[276,1,276,3],[276,5,276,7],[270,1,270,3],[270,5,270,7],[271,1,271,3],[271,5,271,7],[272,1,272,3],[272,5,272,7],[273,1,273,3],[273,5,273,7],[274,1,274,3],[274,5,274,7],[277,1,277,3],[277,5,277,7],[258,1,258,3],[258,5,258,7],[250,1,250,3],[250,5,250,7],[251,1,251,3],[251,5,251,7],[252,1,252,3],[252,5,252,7],[238,1,238,3],[238,5,238,7],[239,1,239,3],[239,5,239,7],[230,1,230,3],[230,5,230,7],[231,1,231,3],[231,5,231,7],[232,1,232,3],[232,5,232,7],[233,1,233,3],[233,5,233,7],[234,1,234,3],[234,5,234,7],[248,1,248,3],[248,5,248,7],[249,1,249,3],[249,5,249,7],[253,1,253,3],[253,5,253,7],[254,1,254,3],[254,5,254,7],[255,1,255,3],[255,5,255,7],[226,1,226,3],[226,5,226,7],[227,1,227,3],[227,5,227,7],[228,1,228,3],[228,5,228,7],[236,1,236,3],[236,5,236,7],[237,1,237,3],[237,5,237,7],[220,1,220,3],[220,5,220,7],[221,1,221,3],[221,5,221,7],[222,1,222,3],[222,5,222,7],[215,1,215,3],[215,5,215,7],[216,1,216,3],[216,5,216,7],[210,1,210,3],[210,5,210,7],[205,1,205,3],[205,5,205,7],[206,1,206,3],[206,5,206,7],[207,1,207,3],[207,5,207,7],[208,1,208,3],[208,5,208,7],[209,1,209,3],[209,5,209,7],[196,1,196,3],[196,5,196,7],[197,1,197,3],[197,5,197,7],[198,1,198,3],[198,5,198,7],[204,1,204,3],[204,5,204,7],[190,1,190,3],[190,5,190,7],[191,1,191,3],[191,5,191,7],[192,1,192,3],[192,5,192,7],[185,1,185,3],[185,5,185,7],[186,1,186,3],[186,5,186,7],[180,1,180,3],[180,5,180,7],[181,1,181,3],[181,5,181,7],[182,1,182,3],[182,5,182,7],[183,1,183,3],[183,5,183,7],[184,1,184,3],[184,5,184,7],[187,1,187,3],[187,5,187,7],[160,1,160,3],[160,5,160,7],[161,1,161,3],[161,5,161,7],[162,1,162,3],[162,5,162,7],[148,1,148,3],[148,5,148,7],[149,1,149,3],[149,5,149,7],[140,1,140,3],[140,5,140,7],[141,1,141,3],[141,5,141,7],[142,1,142,3],[142,5,142,7],[143,1,143,3],[143,5,143,7],[144,1,144,3],[144,5,144,7],[151,1,151,3],[151,5,151,7],[152,1,152,3],[152,5,152,7],[153,1,153,3],[153,5,153,7],[154,1,154,3],[154,5,154,7],[157,1,157,3],[157,5,157,7],[135,1,135,3],[135,5,135,7],[136,1,136,3],[136,5,136,7],[137,1,137,3],[137,5,137,7],[138,1,138,3],[138,5,138,7],[130,1,130,3],[130,5,130,7],[131,1,131,3],[131,5,131,7],[132,1,132,3],[132,5,132,7],[125,1,125,3],[125,5,125,7],[126,1,126,3],[126,5,126,7],[128,1,128,3],[128,5,128,7],[129,1,129,3],[129,5,129,7],[133,1,133,3],[133,5,133,7],[134,1,134,3],[134,5,134,7],[120,1,120,3],[120,5,120,7],[115,1,115,3],[115,5,115,7],[116,1,116,3],[116,5,116,7],[117,1,117,3],[117,5,117,7],[118,1,118,3],[118,5,118,7],[119,1,119,3],[119,5,119,7],[106,1,106,3],[106,5,106,7],[107,1,107,3],[107,5,107,7],[108,1,108,3],[108,5,108,7],[100,1,100,3],[100,5,100,7],[101,1,101,3],[101,5,101,7],[102,1,102,3],[102,5,102,7],[95,1,95,3],[95,5,95,7],[96,1,96,3],[96,5,96,7],[90,1,90,3],[90,5,90,7],[91,1,91,3],[91,5,91,7],[92,1,92,3],[92,5,92,7],[93,1,93,3],[93,5,93,7],[94,1,94,3],[94,5,94,7],[97,1,97,3],[97,5,97,7],[98,1,98,3],[98,5,98,7],[99,1,99,3],[99,5,99,7],[85,1,85,3],[85,5,85,7],[86,1,86,3],[86,5,86,7],[87,1,87,3],[87,5,87,7],[88,1,88,3],[88,5,88,7],[89,1,89,3],[89,5,89,7],[80,1,80,3],[80,5,80,7],[81,1,81,3],[81,5,81,7],[82,1,82,3],[82,5,82,7],[83,1,83,3],[83,5,83,7],[84,1,84,3],[84,5,84,7],[75,1,75,3],[75,5,75,7],[76,1,76,3],[76,5,76,7],[77,1,77,3],[77,5,77,7],[78,1,78,3],[78,5,78,7],[70,1,70,3],[70,5,70,7],[71,1,71,3],[71,5,71,7],[72,1,72,3],[72,5,72,7],[65,1,65,3],[65,5,65,7],[66,1,66,3],[66,5,66,7],[60,1,60,3],[60,5,60,7],[55,5,55,7],[56,1,56,3],[56,5,56,7],[57,1,57,3],[57,5,57,7],[58,1,58,3],[58,5,58,7],[59,1,59,3],[59,5,59,7],[11,1,11,2],[12,1,12,2],[36,5,36,7],[34,5,34,7],[35,5,35,7],[37,5,37,7],[36,1,36,3],[33,1,33,3],[35,1,35,3],[33,5,33,7],[37,1,37,3],[30,1,30,3],[34,1,34,3],[31,1,31,3],[32,1,32,3],[15,1,17,3],[16,4,17,4],[23,1,23,3],[24,1,24,3],[25,1,25,3],[21,1,21,3],[20,1,20,3],[0,52,0,56],[0,1,0,31],[3,8,3,10],[7,8,7,11],[7,14,7,16],[6,14,6,16],[2,14,2,16],[0,46,0,51],[2,8,2,11],[4,14,4,16],[10,1,10,2],[9,1,9,2],[8,1,8,2],[2,1,2,6],[4,1,4,2],[5,1,5,2],[7,1,7,2],[3,1,3,3],[6,1,6,2],[8,8,8,10],[20,5,20,7],[12,9,12,10],[11,9,11,10],[10,8,10,10],[16,9,17,9],[9,8,9,10],[16,20,17,20],[15,25,15,28],[16,17,17,17],[13,1,13,2],[16,14,17,14],[16,22,17,22],[16,5,17,7],[16,10,17,10],[16,19,17,19],[21,5,21,7],[16,13,17,13],[18,5,18,7],[16,47,16,49],[500,18,500,19],[16,42,16,43],[16,44,16,46],[16,18,17,18],[15,24,17,24],[16,21,17,21],[15,23,17,23],[499,5,499,7],[500,6,500,7],[16,8,17,8],[19,5,19,7],[24,5,24,7],[23,5,23,7],[39,5,39,7],[26,5,26,7],[16,12,17,12],[16,11,17,11],[487,5,487,7],[16,15,17,15],[15,17,15,22],[15,5,15,16],[16,16,17,16],[16,29,17,31],[530,20,539,24],[518,20,518,24],[508,20,508,24],[518,15,518,19],[530,15,539,19],[519,15,528,19],[507,13,507,24],[509,20,517,24],[502,24,502,25],[509,15,517,19],[519,20,528,24],[530,13,539,14],[508,13,529,14],[529,15,529,19],[508,15,508,19],[529,20,529,24],[507,3,507,9],[29,1,29,3],[28,5,28,7],[29,5,29,7],[26,1,26,3],[27,5,27,7],[32,5,32,7],[30,5,30,7],[31,5,31,7],[27,1,27,3],[28,1,28,3],[44,1,44,3],[44,5,44,7]],"merged_total":1038,"flags":["merged_cut"]}
[null,"I/O Power",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(TRUE,\"AJ1:AJ2\",IF(AND(NUM_33IOS>0,NUM_PINS<>NUM_33IOS),IF(MID(PACKAGE,2,1)<>\"B\",\"AJ1:AJ3\",\"AJ1:AJ2\"),IF(NUM_33IOS=0,IF(MID(PACKAGE,2,1)<>\"B\",\"AJ2:AJ3\",\"AJ2\"),\"AJ1\")))","v":"AJ1:AJ2"},"HR",{"$f":"IF(AND(NUM_33IOS>0,NUM_PINS<>NUM_33IOS),\"AJ1:AJ2\",IF(NUM_33IOS=0,\"AJ2\",\"AJ1\"))","v":"AJ2"},{"$f":"IF(PROCESS_FACTOR>1,2,1)","v":1},null,null,null,null,null,null,null,{"$f":"OFFSET(POWER_SCALE,8,OFFSET(POWER_SCALE,1,1))*PL_POWERED","v":1},"On-Chip Current",null,null,null,null,null,"Off-Chip Current",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,"2:1","DIFF_TERM","None",{"$f":"\"BX2:BX5\"","v":"BX2:BX5"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,"4:1",null,100,"No","DCI 40Ω","RTT_40","RDRV_NONE",null,"Yes"]
[null,"Active Current",null,null,null,null,null,null,"Summary",null,null,null,null,null,"Select I/O User Guide",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HP_PD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,32,null,"RTT_40",40,"Yes",null,"RTT_48","RDRV_40",null,"No"]
[null,"Source",null,null,"On-Chip","Off-Chip","Active",null,"   Power (on-chip)",null,null,{"$f":"SUM(D5*E5,D6*E6,D7*E7,D8*E8,D9*E9,D10*E10,D11*E11,D12*E12,D13*E13,D14*E14)","v":3.2996935816898465},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,36,null,"RTT_48",48,"SERDES",null,"RTT_60","RDRV_48"]
[null,"VCCINT_IO",null,{"$f":"VCCINT_IO","v":0.95},{"$f":"IOINT_POWER/VCCINT_IO*PL_POWERED","v":0.66009937413707198},null,{"$f":"E5","v":0.66009937413707198},null,null,"Logic",null,{"$f":"$AI18","v":0.54443646533021828},null,null,"XPE User Guide",null,null,null,"Introduction to XPE (video)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,64,null,"RTT_60",60,"DELAY",null,null,"RDRV_60"]
[null,"VCCAUX_IO",null,{"$f":"VCCAUX_IO","v":1.8},{"$f":"SUM(AA19:AA500)/VCCAUX_IO*OFFSET(POWER_SCALE,8,1)*PL_POWERED","v":0.33793104000000007},null,{"$f":"E6","v":0.33793104000000007},null,null,"Buffer",null,{"$f":"L4-L5-L7","v":2.6281104264678157},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"pairs",{"$f":"SUM(IF(RIGHT(F19:F500,14)=\"DS 2.5V (pair)\",J19:K500))","v":0},{"$f":"SUM(IF(F19:F500=\"LVDS 1.8V (pair)\",J19:K500))","v":96},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,72,null,null,50]
[null,"VCCO33",null,{"$f":"VCCO33","v":3.3},{"$f":"SUM(BC19:BC500)*PL_POWERED","v":0},{"$f":"SUM(BJ19:BJ500)","v":0},{"$f":"SUM(E7:F7)","v":0},null,null,"Other",null,{"$f":"$AH18","v":0.12714668989181249},null,null,"Banks With Internal Vref",null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"out",{"$f":"SUM(IF(RIGHT(F19:F500,14)=\"DS 2.5V (pair)\",J19:K500))","v":0},{"$f":"SUM(IF(F19:F500=\"LVDS 1.8V (pair)\",J19:K500))","v":96},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,80,null,"DCI 40Ω","None"]
[null,"VCCO25",null,{"$f":"VCCO25","v":2.5},{"$f":"SUM(BB9,BD19:BD500)*PL_POWERED","v":0},{"$f":"SUM(BK19:BK500)","v":0},0,null,{"$f":"TEXT(IO_POWER/TOTAL_POWER,\"0%\")&\" of total on-chip power \"&TEXT(TOTAL_POWER,\"0.000\")&\"W\"","v":"4% of total on-chip power 0.084W"},null,null,null,null,null,"IO Delay Controllers",null,null,0,{"$f":"SUM(IF(\"Off\"=$M19:$M500,0,1))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"banks",{"$f":"IF(BB6>0,INT(($BB6*2+48)/48),0)","v":0},{"$f":"IF(BC6>0,INT((BC6*2+48)/48),0)","v":5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DCI 48Ω","RTT_120"]
[null,"VCCO18",null,{"$f":"VCCO18","v":1.8},{"$f":"SUM(BC9,BC13,BE19:BE500)*PL_POWERED","v":1.0762092302043422},{"$f":"SUM(BL19:BL500)","v":0},1.0762092302043422,null,"   Power (off-chip)",null,null,{"$f":"SUM(AG19:AG500)","v":0},null,null,"Bitslice Controls",null,{"$f":"SUM(CC19:CC500)","v":37},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"pwr",{"$f":"OFFSET(IODELAY_DATA,27,1)*BB8/1000","v":0},{"$f":"OFFSET(IODELAY_DATA,26,1)*BC8/1000","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DCI 60Ω","RTT_240"]
[null,"VCCO15",null,{"$f":"VCCO15","v":1.5},{"$f":"SUM(BD13,BF19:BF500)*PL_POWERED","v":0},{"$f":"SUM(BM19:BM500)","v":0},0,null,"   I/O Count",null,null,{"$f":"SUM(I501:K501)","v":444},null,null,"Tx Tristates",null,{"$f":"SUM(CD19:CD500)","v":37}]
[null,"VCCO135",null,{"$f":"VCCO135","v":1.35},{"$f":"SUM(BE13,BG19:BG500)*PL_POWERED","v":0},{"$f":"SUM(BN19:BN500)","v":0},0,null,"   I/O Utilization",null,null,{"$f":"IF(AND(L10/NUM_PINS>=0.995, L10/NUM_PINS<0.9999),0.99,L10/NUM_PINS)","v":0.9910714285714286},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"pins",{"$f":"SUM(IF(AP19:AP500=VCCO18,IF(AZ19:AZ500>0,AS19:AS500)))","v":0},{"$f":"SUM(IF(AP19:AP500=VCCO15,IF(AZ19:AZ500>0,AS19:AS500)))","v":0},{"$f":"SUM(IF(AP19:AP500=VCCO135,IF(AZ19:AZ500>0,AS19:AS500)))","v":0},{"$f":"SUM(IF(AP19:AP500=VCCO12,IF(AZ19:AZ500>0,AS19:AS500)))","v":0},{"$f":"SUM(IF(AP19:AP500=VCCO10,IF(AZ19:AZ500>0,AS19:AS500)))","v":0}]
[null,"VCCO12",null,{"$f":"VCCO12","v":1.2},{"$f":"SUM(BF13,BH19:BH500)*PL_POWERED","v":0},{"$f":"SUM(BO19:BO500)","v":0},0,null,null,"High Performance",null,{"$f":"IF(M12<=0,0,N12/M12)","v":0.9910714285714286},{"$f":"NUM_PINS-NUM_33IOS","v":448},{"$f":"SUM(IF(E19:E500<>\"HR\",IF(\"(pair)\"=RIGHT($F19:$F500,6),I19:K500*2,I19:K500),0))","v":444},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"banks",{"$f":"IF(BC11>0,INT((BC11+48)/48),0)","v":0},{"$f":"IF(BD11>0,INT((BD11+48)/48),0)","v":0},{"$f":"IF(BE11>0,INT((BE11+48)/48),0)","v":0},{"$f":"IF(BF11>0,INT((BF11+48)/48),0)","v":0},{"$f":"IF(BG11>0,INT((BG11+48)/48),0)","v":0}]
[null,"VCCO10",null,{"$f":"VCCO10","v":1},{"$f":"SUM(BG13,BI19:BI500)*PL_POWERED","v":0},{"$f":"SUM(BP19:BP500)","v":0},0,null,null,"High Range",null,{"$f":"IF(M13<=0,0,N13/M13)","v":0},{"$f":"NUM_33IOS","v":0},{"$f":"SUM(IF(E19:E500=\"HR\",IF(\"(pair)\"=RIGHT($F19:$F500,6),I19:K500*2,I19:K500),0))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"pwr",{"$f":"BC12*0.021","v":0},{"$f":"BD12*0.015","v":0},{"$f":"BE12*0.015","v":0},{"$f":"BF12*0.015","v":0},{"$f":"BG12*0.015","v":0}]
[null,"VCCINT",null,{"$f":"VCCINT","v":0.95},{"$f":"$AH18/VCCINT*PL_POWERED","v":0.13383862093874999},null,{"$f":"E14","v":0.13383862093874999}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(IF(L19:L500<>\"No\",IF(BA19:BA500>0,AS19:AS500),0))","v":222}]
[null,"Name",null,null,"Bank","I/O Settings",null,null,null,null,null,null,null,null,null,null,null,"Activity",null,null,null,null,null,"Output Load (pF)","Signal Rate (Mtr/s)","On Chip Power (W)",null,null,null,"External",null,null,"Off Chip",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VCCINT_IO/1000*VCCINT_N*AY14*$R19*(OFFSET(IODELAY_DATA,6,1)+OFFSET(IODELAY_DATA,5,1))","v":0},null,{"$f":"IF($AZ14<=0,0,OFFSET(IODELAY_DATA,IF($E19=\"HR\",27,26),1)*INT(($BB16*2+48)/48)/1000)","v":0}]
[null,null,null,null,"I/O Type","I/O Standard",null,null,"Input Pins","Output Pins","Bidir Pins","BITSLICE",null,"IBUF","Input Term","Output Impedance","Pre-Emphasis","Clock (MHz)","Toggle Rate","Data Rate","Output Enable","Term Disable","IBUF Disable",null,null,"VCCINT_IO","VCCAUX_IO","VCCINT","VCCO","Output Termination",null,null,"VCCO",null,null,null,null,null,null,null,null,null,null,null,"DELAY",null,null,"OBUF",null,null,null,"DCI","IOI","LVDS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Output Term",null,null,null,null,null,null,null,null,null,{"$f":"TEXT(VCCINT_IO,\"0.000\")&\"V\"","v":"0.001V"},{"$f":"TEXT(VCCAUX_IO,\"0.000\")&\"V\"","v":"0.002V"},{"$f":"TEXT(VCCAUX_IO,\"0.000\")&\"V\"","v":"0.002V"},"all rails",null,null,null,"all rails",{"$f":"(SUM(AH19:AH500))*OFFSET(POWER_SCALE,7,1)*PL_POWERED","v":0.12714668989181249},{"$f":"(SUM(AI19:AI500))*OFFSET(POWER_SCALE,7,1)*PL_POWERED","v":0.54443646533021828},"Index","Fclk","Type","Typ1","Typ2","Typ3","Vcco","Vtt","Voh-Vol","Pins","Iccint","Iccaux","Iccint","Iccaux","Icco","term","bank","Iccint","Bias","Vcco33","Vcco25","Vcco18","Vcco15","Vcco135","Vcco12","Vcco10","Vcco33","Vcco25","Vcco18","Vcco15","Vcco135","Vcco12","Vcco10","IBUF Iccint","IBUF Iccaux","IBUF Icco","IBUF LP/HP ROffset","IBUF LP/HP COffset","Routing","Offchip Term","R_equiv","Pon-chip","Poff-chip","InTerm","Requiv","Bitslice ctrls","Tx Tris","O Term",null,"outterm","Pre-emphasis","dbi"]
[null,"in",null,null,"HP","LVDS 1.8V (pair)",null,null,96,null,0,"DELAY","Off","High Perf","DIFF_TERM",null,"Yes",1000,0.5,"SDR",1,0,0,null,{"$f":"R19*IF(RIGHT(T19,1)=\"R\",S19*IF(T19=\"DDR\",2,1),2)","v":500},{"$f":"IF(ISERROR($AJ19),0,VCCINT_IO/1000*VCCINT_N*(BA19+AV19+BQ19))","v":0.60005309730975342},{"$f":"IF(ISERROR($AJ19),0,MAX(0,($AU19+$AW19+$BR19)*VCCAUX_IO/1000))","v":0.40794127200000008},{"$f":"$AH19","v":9.19247859852E-2},{"$f":"IF(ISERROR($AJ19),0,MAX(0,OFFSET($AL19,0,$AL19)+(($J19*IF(AND($AL19<>2,LEFT($F19,2)<>\"LV\",RIGHT(T19,1)=\"R\"),S19+(1-S19)/2,1)+K19*IF(AND($AL19<>2,LEFT($F19,2)<>\"LV\",RIGHT(T19,1)=\"R\"),S19,1))*$U19)*$BY19+$I19*OFFSET(IO_STANDARDS,$AJ19,14)/1000+($AY19+$BS19)*$AP19))","v":0.21168000000000001},null,null,null,{"$f":"IF(ISERROR($AJ19),0,IF(AD19=\"None\",0,$BZ19*(($J19+K19)*$U19)))","v":0},{"$f":"IF(ISERROR($AJ19),0,VCCINT/1000*VCCINT_N*(IF($L19=\"No\",0,$R19*$AS19*OFFSET(IODELAY_DATA,9,3))+BV19))","v":9.19247859852E-2},{"$f":"IF(ISERROR($AJ19),0,VCCINT_IO/1000*VCCINT_N*(BA19))","v":0.53606051970975332},{"$f":"MATCH($F19,IF($E19=\"HR\",SIOSTD_LIST,VIOSTD_LIST),FALSE)+IF($E19=\"HR\",0,ROW(VIOSTD_LIST)-ROW(SIOSTD_LIST))","v":143},{"$f":"R19*IF(RIGHT(T19,1)=\"R\",S19*IF(T19=\"DDR\",1,0.5),1)","v":250},{"$f":"IF(AND($K19>0,$E19=\"HR\",OFFSET(IO_STANDARDS,$AJ19,19)>0),3,OFFSET(IO_STANDARDS,$AJ19,2))","v":2},{"$f":"(OFFSET(IO_STANDARDS,$AJ19,35)*($X19+OFFSET(IO_STANDARDS,$AJ19,3))*($J19+$K19*IF($CI19>0,0.93,1))*$AP19*$AK19*$U19*$AT$1)/1000","v":0},{"$f":"MAX(0,(OFFSET(IO_STANDARDS,$AJ19,35)*($X19+OFFSET(IO_STANDARDS,$AJ19,3))*($J19+$K19)*$AP19*$AK19*$U19*$AT$1/1000))","v":0},{"$f":"(((OFFSET(IO_STANDARDS,$AJ19,35)*($X19+OFFSET(IO_STANDARDS,$AJ19,3))*$AP19/1000)*($J19+$K19*IF($CI19>0,0.93,1))*$AK19*$U19*$AT$1))","v":0},{"$f":"IF(ISERROR($AJ19),0,OFFSET(IO_STANDARDS,$AJ19,1))","v":1.8},{"$f":"IF(OFFSET(IO_STANDARDS,$AJ19,9)=0,0,IF(OR(LEFT($F19,14)=\"HSTL Class III\",LEFT($F19,13)=\"HSTL Class IV\",LEFT($F19,3)=\"GTL\",LEFT($F19,3)=\"POD\",LEFT($F19,8)=\"Diff POD\"),$AP19,$AP19/2))","v":0},{"$f":"IF(OFFSET(IO_STANDARDS,$AJ19,10)=0,$AP19,$AP19/2)","v":0.9},{"$f":"IF(RIGHT($F19,6) =\"(pair)\",2,1)*SUM(I19:K19)","v":192},{"$f":"IF($M19=\"Off\",0,$AK19*OFFSET(IODELAY_DATA,2,3)*$AS19)","v":0},{"$f":"0","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ19,33)*$AK19*$U19*($J19+$K19)*IF(AND($Q19=\"Yes\",OR(LEFT($F19,3)=\"POD\",LEFT($F19,8)=\"Diff POD\",LEFT($F19,4)=\"LVDS\")),2,1)*IF($CI19>0,0.93,1)+OFFSET(IO_STANDARDS,$AJ19,36)*$U19*($J19+$K19)","v":0},{"$f":"(OFFSET(IO_STANDARDS,$AJ19,34)*IF($CF19>0,40/$CF19,1)*$AK19*$U19*IF($Q19=\"Yes\",IF(OR(LEFT($F19,3)=\"POD\",LEFT($F19,8)=\"Diff POD\"),1.17,IF(LEFT($F19,4)=\"LVDS\",2,1)),1)*IF($CI19>0,0.93,1)*$AT$1+OFFSET(IO_STANDARDS,$AJ19,37)*$U19*$AT$1)*($J19+$K19)","v":0},{"$f":"((($I19*(1-$W19)+$K19*(1-$U19))*OFFSET(IO_STANDARDS,$AJ19,11)) + ((($J19+$K19)*$U19)*OFFSET(IO_STANDARDS,$AJ19,10)))/1000  + $AZ19","v":0},{"$f":"IF($CB19>0,IF(LEFT($F19,4)=\"Diff\",2,1)*($I19+$K19*(1-$U19))*IF(AND($AL19=2,$O19=\"DIFF_TERM\"),OFFSET(IO_STANDARDS,$AJ19,18),IF($E19<>\"HR\",IF($CB19>0,1,0)*IF(AL19<>2,IF(OR(LEFT($F19,3)=\"POD\",LEFT($F19,8)=\"Diff POD\"),0.5*1000*$AP19/($CB19+40)*IF($CI19>0,0.36/0.5,1),$AQ19*500/$CB19),OFFSET(IO_STANDARDS,$AJ19,11)),IF(LEFT($O19,3)=\"RTT\",$AQ19*500/$CB19,0))*(1-$V19))/1000,0)","v":0.1176},{"$f":"IF(OR(LEFT($F19,3)=\"POD\",LEFT($F19,8)=\"Diff POD\"),0,IF(IF(LEFT($F19,5)=\"LVDCI\",$J19+$K19,SUM($I19:$K19))>0,((OFFSET(IO_STANDARDS,$AJ19,6)*IF(AND($I19+$K19>0,OFFSET(IO_STANDARDS,$AJ19,6)<1),100,1)*INT((SUM($I19:$K19)+50)/50))/1000),0))","v":0},{"$f":"IF($L19=\"No\",0,$R19*(IF($L19=\"SERDES\",OFFSET(IODELAY_DATA,3,1),IF($L19=\"DELAY\",OFFSET(IODELAY_DATA,2,1),OFFSET(IODELAY_DATA,4,1)))*$AS19+$CC19*OFFSET(IODELAY_DATA,6,1)+$CD19*OFFSET(IODELAY_DATA,5,1)))","v":564.27423127342456},{"$f":"IF(OR($J19+$K19=0,$AL19<>2),0,OFFSET(IODELAY_DATA,IF($E19=\"HR\",27,26),1)*INT((SUM($I19:$K19)+50)/50)/1000)","v":0},{"$f":"IF(ISERROR($AJ19),0,IF($AP19=VCCO33,$AC19/$AP19+$AZ19,0))","v":0},{"$f":"IF(ISERROR($AJ19),0,IF($AP19=VCCO25,$AC19/$AP19+$AZ19,0))","v":0},{"$f":"IF(ISERROR($AJ19),0,IF($AP19=VCCO18,$AC19/$AP19,0))","v":0.1176},{"$f":"IF(ISERROR($AJ19),0,IF($AP19=VCCO15,$AC19/$AP19,0))","v":0},{"$f":"IF(ISERROR($AJ19),0,IF($AP19=VCCO135,$AC19/$AP19,0))","v":0},{"$f":"IF(ISERROR($AJ19),0,IF($AP19=VCCO12,$AC19/$AP19,0))","v":0},{"$f":"IF(ISERROR($AJ19),0,IF($AP19=VCCO10,$AC19/$AP19,0))","v":0},{"$f":"IF(ISERROR($AJ19),0,IF($AP19=VCCO33,$AG19/$AP19,0))","v":0},{"$f":"IF(ISERROR($AJ19),0,IF($AP19=VCCO25,$AG19/$AP19,0))","v":0},{"$f":"IF(ISERROR($AJ19),0,IF($AP19=VCCO18,$AG19/$AP19,0))","v":0},{"$f":"IF(ISERROR($AJ19),0,IF($AP19=VCCO15,$AG19/$AP19,0))","v":0},{"$f":"IF(ISERROR($AJ19),0,IF($AP19=VCCO135,$AG19/$AP19,0))","v":0},{"$f":"IF(ISERROR($AJ19),0,IF($AP19=VCCO12,$AG19/$AP19,0))","v":0},{"$f":"IF(ISERROR($AJ19),0,IF($AP19=VCCO10,$AG19/$AP19,0))","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ19,24+$BU19)*((1-$W19)*I19+(1-U19)*K19)+(OFFSET(IO_STANDARDS,$AJ19,21+$BU19)*$AK19)*((1-$W19)*I19+(1-U19)*K19*IF($CI19>0,0.93,1))","v":67.360608000000013},{"$f":"OFFSET(IO_STANDARDS,$AJ19,25+$BU19)*(I19*(1-W19)+K19*(1-U19))+(OFFSET(IO_STANDARDS,$AJ19,22+$BU19)*(I19*(1-W19)+K19*(1-U19)*IF($CI19>0,0.93,1))*$AK19)","v":226.63404000000003},{"$f":"(IF($AY19=0,OFFSET(IO_STANDARDS,$AJ19,11)*(I19*(1-$V19)+K19*(1-$U19)),0)+OFFSET(IO_STANDARDS,$AJ19,23+$BU19)*(I19*(1-$W19)+K19*(1-$U19))*$AK19)/1000","v":0},{"$f":"IF($E19=\"HR\",22,15)+IF(OFFSET(IO_STANDARDS,$AJ19,5)=0,0,IF(ISERR(FIND(\"pair\",OFFSET(IO_STANDARDS,$AJ19,0))),1,2))+IF(OR(LEFT($F19,3)=\"POD\",LEFT($F19,8)=\"Diff POD\"),2,0)","v":15},{"$f":"IF(LEFT($N19,3)=\"Low\",0,6)","v":6},{"$f":"$AK19*2*OFFSET(FANOUT,3,6)*$AS19","v":35.016632615999995},{"$f":"IF(OR($AL19=2),\"BW2\",IF(OR(MID(F19,IF(LEFT($F19,4)=\"Diff\",6,1),4)=\"HSTL\",MID(F19,IF(LEFT($F19,4)=\"Diff\",6,1),4)=\"SSTL\",MID(F19,IF(LEFT($F19,4)=\"Diff\",6,1),3)=\"POD\"),IF(E19=\"HR\",\"BW6\",\"BW3:BW5\"),\"BW1\"))","v":"BW2"},{"$f":" IF(OR(ISTEXT($AD19),$AD19=\"None\"),0,$AD19)","v":0},{"$f":"IF(TRUE,IF($CE19>0,$CE19*$AP19,OFFSET(IO_STANDARDS,$AJ19,13))/1000,(($AP19-OFFSET(IO_STANDARDS,$AJ19,8))*(ABS($AQ19-OFFSET(IO_STANDARDS,$AJ19,8))/$BX19)+OFFSET(IO_STANDARDS,$AJ19,9)*($AQ19-OFFSET(IO_STANDARDS,$AJ19,9))/$BX19)/2)*IF(AND($Q19=\"Yes\",LEFT($F19,4)=\"LVDS\"),1.25,1)","v":2.1150000000000002E-2},0,{"$f":"IF(OR(($I19+$K19)<1,LEFT($F19,3)=\"LVC\",LEFT($F19,3)=\"LVT\"),\"BV2\",IF(OFFSET(IO_STANDARDS,$AJ19,18)>0,\"BV1:BV2\",IF(OR(LEFT($F19,3)=\"HSU\",LEFT($F19,8)=\"Diff HSU\"),\"BW7:BW9\",IF(OR(OFFSET(IO_STANDARDS,$AJ19,19)>0,OFFSET(IO_STANDARDS,$AJ19,20)>0,OR(MID($F19,2,3)=\"STL\",LEFT($F19,9)=\"Diff HSTL\",LEFT($F19,9)=\"Diff SSTL\")),IF(OR(E19=\"HR\",OFFSET(IO_STANDARDS,$AJ19,20)=0),\"BV2:BV5\",\"BV7:BV9\"),\"BV2\"))))","v":"BV1:BV2"},{"$f":"IF(OR(LEN($O19)<1,RIGHT($O19,4)=\"NONE\",RIGHT($O19,4)=\"None\"),0,IF(LEN($O19)<5,IF(E19=\"HR\",48,40),IF(LEFT($O19,3)=\"DCI\",MID($O19,5,2),IF(LEN($O19)>6,IF(RIGHT($O19,3)=\"240\",240,120),RIGHT($O19,2)))))","v":120},{"$f":"IF($L19=\"No\",0,$AS19/6)","v":32},{"$f":"IF($L19=\"No\",0,IF($K19>0,$AS19/4,$AS19/6))","v":32},{"$f":"IF(AND(OFFSET(IO_STANDARDS,$AJ19,13)>0,$AL19<>2),IF($CF19>0,IF(LEFT($F19,4)=\"Diff\",2,1)*1000*($AP19/2)/($CF19+MAX(40,$BX19))/2,0),0)","v":0},{"$f":"IF(OR(LEN($P19)<1,RIGHT($P19,4)=\"NONE\"),IF(RIGHT(INDIRECT(LEFT($CG19,3)),2)=\"40\",40,0),IF(LEFT($P19,3)=\"DCI\",MID($P19,5,2),RIGHT($P19,2)))","v":0},{"$f":"IF(AND(E19<>\"HR\",OR(LEFT($F19,3)<>\"LVC\",OFFSET(IO_STANDARDS,$AJ19,13)>0),$AL19<>2,($J19+$K19)>0),\"CA3:CA5\",\"CA1\")","v":"CA1"},{"$f":"IF(OR(LEFT($F19,3)=\"POD\",LEFT($F19,8)=\"Diff POD\",LEFT($F19,4)=\"LVDS\",($J19+$K19)>0),\"CC2:CC3\",\"CC1\")","v":"CC2:CC3"},{"$f":"IF(AND(LEFT($F19,3)=\"POD\",$K19>0,$T19=\"DDR\",NOT(ISERROR(SEARCH(\"ddr4_dq<\",$B19,1)))),1,0)","v":0}]
[null,"ins",null,null,"HP","LVCMOS 1.8V 12mA (Fast)",null,null,30,null,null,"DELAY","Off","High Perf",null,null,null,100,0.5,"SDR",1,0,0,0,50,{"$f":"IF(ISERROR($AJ20),0,VCCINT_IO/1000*VCCINT_N*(BA20+AV20+BQ20))","v":9.4397081204648965E-3},0,{"$f":"$AH20","v":1.43632478101875E-3},7.5734999999999995E-4,"None",null,null,0,1.43632478101875E-3,8.3759456204648974E-3,140,{"$f":"R20*IF(RIGHT(T20,1)=\"R\",S20*IF(T20=\"DDR\",1,0.5),1)","v":25},1,0,0,0,1.8,0,1.8,30,0,{"$f":"0","v":0},0,0,0,0,0,8.8167848636472606,0,0,0,4.2074999999999995E-4,0,0,0,0,0,0,0,0,0,0,0,1.1197499999999998,0,4.2074999999999995E-4,15,{"$f":"IF(LEFT($N20,3)=\"Low\",0,6)","v":6},0.54713488462499993,{"$f":"IF(OR($AL20=2),\"BW2\",IF(OR(MID(F20,IF(LEFT($F20,4)=\"Diff\",6,1),4)=\"HSTL\",MID(F20,IF(LEFT($F20,4)=\"Diff\",6,1),4)=\"SSTL\",MID(F20,IF(LEFT($F20,4)=\"Diff\",6,1),3)=\"POD\"),IF(E20=\"HR\",\"BW6\",\"BW3:BW5\"),\"BW1\"))","v":"BW1"},{"$f":" IF(OR(ISTEXT($AD20),$AD20=\"None\"),0,$AD20)","v":0},0,0,"BV2",{"$f":"IF(OR(LEN($O20)<1,RIGHT($O20,4)=\"NONE\",RIGHT($O20,4)=\"None\"),0,IF(LEN($O20)<5,IF(E20=\"HR\",48,40),IF(LEFT($O20,3)=\"DCI\",MID($O20,5,2),IF(LEN($O20)>6,IF(RIGHT($O20,3)=\"240\",240,120),RIGHT($O20,2)))))","v":0},5,{"$f":"IF($L20=\"No\",0,IF($K20>0,$AS20/4,$AS20/6))","v":5},0,{"$f":"IF(OR(LEN($P20)<1,RIGHT($P20,4)=\"NONE\"),IF(RIGHT(INDIRECT(LEFT($CG20,3)),2)=\"40\",40,0),IF(LEFT($P20,3)=\"DCI\",MID($P20,5,2),RIGHT($P20,2)))","v":0},"CA1",{"$f":"IF(OR(LEFT($F20,3)=\"POD\",LEFT($F20,8)=\"Diff POD\",LEFT($F20,4)=\"LVDS\",($J20+$K20)>0),\"CC2:CC3\",\"CC1\")","v":"CC1"},{"$f":"IF(AND(LEFT($F20,3)=\"POD\",$K20>0,$T20=\"DDR\",NOT(ISERROR(SEARCH(\"ddr4_dq<\",$B20,1)))),1,0)","v":0}]
[null,"out",null,null,"HP","LVDS 1.8V (pair)",null,null,null,96,0,"No","Off","Low Power",null,null,null,1000,0.5,"SDR",1,0,0,5,500,1.7100000000000001E-2,0.16632,3.3265800985199996E-2,1.6966179310344827,100,null,null,0,3.3265800985199996E-2,0,143,250,2,7.229793103448276E-2,7.229793103448276E-2,7.2297931034482774E-2,1.8,0,0.9,192,0,{"$f":"0","v":0},18,92.399999999999991,0.88319999999999999,0,0,0,0,0,0,0.94256551724137927,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,35.016632615999995,"BW2",100,1.6920000000000001E-2,0,"BV2",0,0,0,0,0,"CA1","CC2:CC3",0]
[null,"outs",null,null,"HP","LVCMOS 1.8V 12mA (Fast)",null,null,null,30,null,"No","Off","Low Power",null,null,null,100,0.5,"SDR",1,0,{"$f":"$V22","v":0},10,50,5.0160000000000005E-4,3.4014599999999999E-2,5.1977814039374994E-4,2.8121333333333335E-2,"None",null,null,0,5.1977814039374994E-4,0,140,25,1,2.8121333333333335E-2,2.8121333333333335E-2,2.8121333333333338E-2,1.8,0,1.8,30,0,{"$f":"0","v":0},0.52800000000000002,18.897000000000002,0,0,0,0,0,0,0,1.5622962962962963E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0.54713488462499993,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC2:CC3",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R49*IF(RIGHT(T49,1)=\"R\",S49*IF(T49=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R50*IF(RIGHT(T50,1)=\"R\",S50*IF(T50=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R56*IF(RIGHT(T56,1)=\"R\",S56*IF(T56=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R62*IF(RIGHT(T62,1)=\"R\",S62*IF(T62=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R68*IF(RIGHT(T68,1)=\"R\",S68*IF(T68=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R74*IF(RIGHT(T74,1)=\"R\",S74*IF(T74=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R80*IF(RIGHT(T80,1)=\"R\",S80*IF(T80=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,{"$f":"$V83","v":0},0,0,0,{"$f":"IF(ISERROR($AJ83),0,MAX(0,($AU83+$AW83+$BR83)*VCCAUX_IO/1000))","v":0},0,{"$f":"IF(ISERROR($AJ83),0,MAX(0,OFFSET($AL83,0,$AL83)+(($J83*IF(AND($AL83<>2,LEFT($F83,2)<>\"LV\",RIGHT(T83,1)=\"R\"),S83+(1-S83)/2,1)+K83*IF(AND($AL83<>2,LEFT($F83,2)<>\"LV\",RIGHT(T83,1)=\"R\"),S83,1))*$U83)*$BY83+$I83*OFFSET(IO_STANDARDS,$AJ83,14)/1000+($AY83+$BS83)*$AP83))","v":0},"None",null,null,{"$f":"IF(ISERROR($AJ83),0,IF(AD83=\"None\",0,$BZ83*(($J83+K83)*$U83)))","v":0},{"$f":"IF(ISERROR($AJ83),0,VCCINT/1000*VCCINT_N*(IF($L83=\"No\",0,$R83*$AS83*OFFSET(IODELAY_DATA,9,3))+BV83))","v":0},{"$f":"IF(ISERROR($AJ83),0,VCCINT_IO/1000*VCCINT_N*(BA83))","v":0},139,0,{"$f":"IF(AND($K83>0,$E83=\"HR\",OFFSET(IO_STANDARDS,$AJ83,19)>0),3,OFFSET(IO_STANDARDS,$AJ83,2))","v":1},{"$f":"(OFFSET(IO_STANDARDS,$AJ83,35)*($X83+OFFSET(IO_STANDARDS,$AJ83,3))*($J83+$K83*IF($CI83>0,0.93,1))*$AP83*$AK83*$U83*$AT$1)/1000","v":0},{"$f":"MAX(0,(OFFSET(IO_STANDARDS,$AJ83,35)*($X83+OFFSET(IO_STANDARDS,$AJ83,3))*($J83+$K83)*$AP83*$AK83*$U83*$AT$1/1000))","v":0},{"$f":"(((OFFSET(IO_STANDARDS,$AJ83,35)*($X83+OFFSET(IO_STANDARDS,$AJ83,3))*$AP83/1000)*($J83+$K83*IF($CI83>0,0.93,1))*$AK83*$U83*$AT$1))","v":0},{"$f":"IF(ISERROR($AJ83),0,OFFSET(IO_STANDARDS,$AJ83,1))","v":1.8},{"$f":"IF(OFFSET(IO_STANDARDS,$AJ83,9)=0,0,IF(OR(LEFT($F83,14)=\"HSTL Class III\",LEFT($F83,13)=\"HSTL Class IV\",LEFT($F83,3)=\"GTL\",LEFT($F83,3)=\"POD\",LEFT($F83,8)=\"Diff POD\"),$AP83,$AP83/2))","v":0},{"$f":"IF(OFFSET(IO_STANDARDS,$AJ83,10)=0,$AP83,$AP83/2)","v":1.8},{"$f":"IF(RIGHT($F83,6) =\"(pair)\",2,1)*SUM(I83:K83)","v":0},{"$f":"IF($M83=\"Off\",0,$AK83*OFFSET(IODELAY_DATA,2,3)*$AS83)","v":0},{"$f":"0","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ83,33)*$AK83*$U83*($J83+$K83)*IF(AND($Q83=\"Yes\",OR(LEFT($F83,3)=\"POD\",LEFT($F83,8)=\"Diff POD\",LEFT($F83,4)=\"LVDS\")),2,1)*IF($CI83>0,0.93,1)+OFFSET(IO_STANDARDS,$AJ83,36)*$U83*($J83+$K83)","v":0},{"$f":"(OFFSET(IO_STANDARDS,$AJ83,34)*IF($CF83>0,40/$CF83,1)*$AK83*$U83*IF($Q83=\"Yes\",IF(OR(LEFT($F83,3)=\"POD\",LEFT($F83,8)=\"Diff POD\"),1.17,IF(LEFT($F83,4)=\"LVDS\",2,1)),1)*IF($CI83>0,0.93,1)*$AT$1+OFFSET(IO_STANDARDS,$AJ83,37)*$U83*$AT$1)*($J83+$K83)","v":0},{"$f":"((($I83*(1-$W83)+$K83*(1-$U83))*OFFSET(IO_STANDARDS,$AJ83,11)) + ((($J83+$K83)*$U83)*OFFSET(IO_STANDARDS,$AJ83,10)))/1000  + $AZ83","v":0},{"$f":"IF($CB83>0,IF(LEFT($F83,4)=\"Diff\",2,1)*($I83+$K83*(1-$U83))*IF(AND($AL83=2,$O83=\"DIFF_TERM\"),OFFSET(IO_STANDARDS,$AJ83,18),IF($E83<>\"HR\",IF($CB83>0,1,0)*IF(AL83<>2,IF(OR(LEFT($F83,3)=\"POD\",LEFT($F83,8)=\"Diff POD\"),0.5*1000*$AP83/($CB83+40)*IF($CI83>0,0.36/0.5,1),$AQ83*500/$CB83),OFFSET(IO_STANDARDS,$AJ83,11)),IF(LEFT($O83,3)=\"RTT\",$AQ83*500/$CB83,0))*(1-$V83))/1000,0)","v":0},{"$f":"IF(OR(LEFT($F83,3)=\"POD\",LEFT($F83,8)=\"Diff POD\"),0,IF(IF(LEFT($F83,5)=\"LVDCI\",$J83+$K83,SUM($I83:$K83))>0,((OFFSET(IO_STANDARDS,$AJ83,6)*IF(AND($I83+$K83>0,OFFSET(IO_STANDARDS,$AJ83,6)<1),100,1)*INT((SUM($I83:$K83)+50)/50))/1000),0))","v":0},{"$f":"IF($L83=\"No\",0,$R83*(IF($L83=\"SERDES\",OFFSET(IODELAY_DATA,3,1),IF($L83=\"DELAY\",OFFSET(IODELAY_DATA,2,1),OFFSET(IODELAY_DATA,4,1)))*$AS83+$CC83*OFFSET(IODELAY_DATA,6,1)+$CD83*OFFSET(IODELAY_DATA,5,1)))","v":0},{"$f":"IF(OR($J83+$K83=0,$AL83<>2),0,OFFSET(IODELAY_DATA,IF($E83=\"HR\",27,26),1)*INT((SUM($I83:$K83)+50)/50)/1000)","v":0},0,0,0,0,0,0,{"$f":"IF(ISERROR($AJ83),0,IF($AP83=VCCO10,$AC83/$AP83,0))","v":0},{"$f":"IF(ISERROR($AJ83),0,IF($AP83=VCCO33,$AG83/$AP83,0))","v":0},{"$f":"IF(ISERROR($AJ83),0,IF($AP83=VCCO25,$AG83/$AP83,0))","v":0},{"$f":"IF(ISERROR($AJ83),0,IF($AP83=VCCO18,$AG83/$AP83,0))","v":0},{"$f":"IF(ISERROR($AJ83),0,IF($AP83=VCCO15,$AG83/$AP83,0))","v":0},{"$f":"IF(ISERROR($AJ83),0,IF($AP83=VCCO135,$AG83/$AP83,0))","v":0},{"$f":"IF(ISERROR($AJ83),0,IF($AP83=VCCO12,$AG83/$AP83,0))","v":0},{"$f":"IF(ISERROR($AJ83),0,IF($AP83=VCCO10,$AG83/$AP83,0))","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ83,24+$BU83)*((1-$W83)*I83+(1-U83)*K83)+(OFFSET(IO_STANDARDS,$AJ83,21+$BU83)*$AK83)*((1-$W83)*I83+(1-U83)*K83*IF($CI83>0,0.93,1))","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ83,25+$BU83)*(I83*(1-W83)+K83*(1-U83))+(OFFSET(IO_STANDARDS,$AJ83,22+$BU83)*(I83*(1-W83)+K83*(1-U83)*IF($CI83>0,0.93,1))*$AK83)","v":0},{"$f":"(IF($AY83=0,OFFSET(IO_STANDARDS,$AJ83,11)*(I83*(1-$V83)+K83*(1-$U83)),0)+OFFSET(IO_STANDARDS,$AJ83,23+$BU83)*(I83*(1-$W83)+K83*(1-$U83))*$AK83)/1000","v":0},{"$f":"IF($E83=\"HR\",22,15)+IF(OFFSET(IO_STANDARDS,$AJ83,5)=0,0,IF(ISERR(FIND(\"pair\",OFFSET(IO_STANDARDS,$AJ83,0))),1,2))+IF(OR(LEFT($F83,3)=\"POD\",LEFT($F83,8)=\"Diff POD\"),2,0)","v":15},0,{"$f":"$AK83*2*OFFSET(FANOUT,3,6)*$AS83","v":0},"BW1",0,{"$f":"IF(TRUE,IF($CE83>0,$CE83*$AP83,OFFSET(IO_STANDARDS,$AJ83,13))/1000,(($AP83-OFFSET(IO_STANDARDS,$AJ83,8))*(ABS($AQ83-OFFSET(IO_STANDARDS,$AJ83,8))/$BX83)+OFFSET(IO_STANDARDS,$AJ83,9)*($AQ83-OFFSET(IO_STANDARDS,$AJ83,9))/$BX83)/2)*IF(AND($Q83=\"Yes\",LEFT($F83,4)=\"LVDS\"),1.25,1)","v":0},0,{"$f":"IF(OR(($I83+$K83)<1,LEFT($F83,3)=\"LVC\",LEFT($F83,3)=\"LVT\"),\"BV2\",IF(OFFSET(IO_STANDARDS,$AJ83,18)>0,\"BV1:BV2\",IF(OR(LEFT($F83,3)=\"HSU\",LEFT($F83,8)=\"Diff HSU\"),\"BW7:BW9\",IF(OR(OFFSET(IO_STANDARDS,$AJ83,19)>0,OFFSET(IO_STANDARDS,$AJ83,20)>0,OR(MID($F83,2,3)=\"STL\",LEFT($F83,9)=\"Diff HSTL\",LEFT($F83,9)=\"Diff SSTL\")),IF(OR(E83=\"HR\",OFFSET(IO_STANDARDS,$AJ83,20)=0),\"BV2:BV5\",\"BV7:BV9\"),\"BV2\"))))","v":"BV2"},0,{"$f":"IF($L83=\"No\",0,$AS83/6)","v":0},0,{"$f":"IF(AND(OFFSET(IO_STANDARDS,$AJ83,13)>0,$AL83<>2),IF($CF83>0,IF(LEFT($F83,4)=\"Diff\",2,1)*1000*($AP83/2)/($CF83+MAX(40,$BX83))/2,0),0)","v":0},0,{"$f":"IF(AND(E83<>\"HR\",OR(LEFT($F83,3)<>\"LVC\",OFFSET(IO_STANDARDS,$AJ83,13)>0),$AL83<>2,($J83+$K83)>0),\"CA3:CA5\",\"CA1\")","v":"CA1"},"CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,{"$f":"IF(ISERROR($AJ84),0,VCCINT_IO/1000*VCCINT_N*(BA84+AV84+BQ84))","v":0},0,{"$f":"$AH84","v":0},0,"None",null,null,0,0,0,139,{"$f":"R84*IF(RIGHT(T84,1)=\"R\",S84*IF(T84=\"DDR\",1,0.5),1)","v":0},1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,{"$f":"IF(LEFT($N84,3)=\"Low\",0,6)","v":0},0,{"$f":"IF(OR($AL84=2),\"BW2\",IF(OR(MID(F84,IF(LEFT($F84,4)=\"Diff\",6,1),4)=\"HSTL\",MID(F84,IF(LEFT($F84,4)=\"Diff\",6,1),4)=\"SSTL\",MID(F84,IF(LEFT($F84,4)=\"Diff\",6,1),3)=\"POD\"),IF(E84=\"HR\",\"BW6\",\"BW3:BW5\"),\"BW1\"))","v":"BW1"},{"$f":" IF(OR(ISTEXT($AD84),$AD84=\"None\"),0,$AD84)","v":0},0,0,"BV2",{"$f":"IF(OR(LEN($O84)<1,RIGHT($O84,4)=\"NONE\",RIGHT($O84,4)=\"None\"),0,IF(LEN($O84)<5,IF(E84=\"HR\",48,40),IF(LEFT($O84,3)=\"DCI\",MID($O84,5,2),IF(LEN($O84)>6,IF(RIGHT($O84,3)=\"240\",240,120),RIGHT($O84,2)))))","v":0},0,{"$f":"IF($L84=\"No\",0,IF($K84>0,$AS84/4,$AS84/6))","v":0},0,{"$f":"IF(OR(LEN($P84)<1,RIGHT($P84,4)=\"NONE\"),IF(RIGHT(INDIRECT(LEFT($CG84,3)),2)=\"40\",40,0),IF(LEFT($P84,3)=\"DCI\",MID($P84,5,2),RIGHT($P84,2)))","v":0},"CA1",{"$f":"IF(OR(LEFT($F84,3)=\"POD\",LEFT($F84,8)=\"Diff POD\",LEFT($F84,4)=\"LVDS\",($J84+$K84)>0),\"CC2:CC3\",\"CC1\")","v":"CC1"},{"$f":"IF(AND(LEFT($F84,3)=\"POD\",$K84>0,$T84=\"DDR\",NOT(ISERROR(SEARCH(\"ddr4_dq<\",$B84,1)))),1,0)","v":0}]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R86*IF(RIGHT(T86,1)=\"R\",S86*IF(T86=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R92*IF(RIGHT(T92,1)=\"R\",S92*IF(T92=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R98*IF(RIGHT(T98,1)=\"R\",S98*IF(T98=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R104*IF(RIGHT(T104,1)=\"R\",S104*IF(T104=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R110*IF(RIGHT(T110,1)=\"R\",S110*IF(T110=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R116*IF(RIGHT(T116,1)=\"R\",S116*IF(T116=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R122*IF(RIGHT(T122,1)=\"R\",S122*IF(T122=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R128*IF(RIGHT(T128,1)=\"R\",S128*IF(T128=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,{"$f":"MATCH($F129,IF($E129=\"HR\",SIOSTD_LIST,VIOSTD_LIST),FALSE)+IF($E129=\"HR\",0,ROW(VIOSTD_LIST)-ROW(SIOSTD_LIST))","v":139},0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,{"$f":"IF(ISERROR($AJ129),0,IF($AP129=VCCO33,$AC129/$AP129+$AZ129,0))","v":0},{"$f":"IF(ISERROR($AJ129),0,IF($AP129=VCCO25,$AC129/$AP129+$AZ129,0))","v":0},{"$f":"IF(ISERROR($AJ129),0,IF($AP129=VCCO18,$AC129/$AP129,0))","v":0},{"$f":"IF(ISERROR($AJ129),0,IF($AP129=VCCO15,$AC129/$AP129,0))","v":0},{"$f":"IF(ISERROR($AJ129),0,IF($AP129=VCCO135,$AC129/$AP129,0))","v":0},{"$f":"IF(ISERROR($AJ129),0,IF($AP129=VCCO12,$AC129/$AP129,0))","v":0},0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R134*IF(RIGHT(T134,1)=\"R\",S134*IF(T134=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R140*IF(RIGHT(T140,1)=\"R\",S140*IF(T140=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R146*IF(RIGHT(T146,1)=\"R\",S146*IF(T146=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,{"$f":"$V147","v":0},0,0,0,{"$f":"IF(ISERROR($AJ147),0,MAX(0,($AU147+$AW147+$BR147)*VCCAUX_IO/1000))","v":0},0,{"$f":"IF(ISERROR($AJ147),0,MAX(0,OFFSET($AL147,0,$AL147)+(($J147*IF(AND($AL147<>2,LEFT($F147,2)<>\"LV\",RIGHT(T147,1)=\"R\"),S147+(1-S147)/2,1)+K147*IF(AND($AL147<>2,LEFT($F147,2)<>\"LV\",RIGHT(T147,1)=\"R\"),S147,1))*$U147)*$BY147+$I147*OFFSET(IO_STANDARDS,$AJ147,14)/1000+($AY147+$BS147)*$AP147))","v":0},"None",null,null,{"$f":"IF(ISERROR($AJ147),0,IF(AD147=\"None\",0,$BZ147*(($J147+K147)*$U147)))","v":0},{"$f":"IF(ISERROR($AJ147),0,VCCINT/1000*VCCINT_N*(IF($L147=\"No\",0,$R147*$AS147*OFFSET(IODELAY_DATA,9,3))+BV147))","v":0},{"$f":"IF(ISERROR($AJ147),0,VCCINT_IO/1000*VCCINT_N*(BA147))","v":0},139,0,{"$f":"IF(AND($K147>0,$E147=\"HR\",OFFSET(IO_STANDARDS,$AJ147,19)>0),3,OFFSET(IO_STANDARDS,$AJ147,2))","v":1},{"$f":"(OFFSET(IO_STANDARDS,$AJ147,35)*($X147+OFFSET(IO_STANDARDS,$AJ147,3))*($J147+$K147*IF($CI147>0,0.93,1))*$AP147*$AK147*$U147*$AT$1)/1000","v":0},{"$f":"MAX(0,(OFFSET(IO_STANDARDS,$AJ147,35)*($X147+OFFSET(IO_STANDARDS,$AJ147,3))*($J147+$K147)*$AP147*$AK147*$U147*$AT$1/1000))","v":0},{"$f":"(((OFFSET(IO_STANDARDS,$AJ147,35)*($X147+OFFSET(IO_STANDARDS,$AJ147,3))*$AP147/1000)*($J147+$K147*IF($CI147>0,0.93,1))*$AK147*$U147*$AT$1))","v":0},{"$f":"IF(ISERROR($AJ147),0,OFFSET(IO_STANDARDS,$AJ147,1))","v":1.8},{"$f":"IF(OFFSET(IO_STANDARDS,$AJ147,9)=0,0,IF(OR(LEFT($F147,14)=\"HSTL Class III\",LEFT($F147,13)=\"HSTL Class IV\",LEFT($F147,3)=\"GTL\",LEFT($F147,3)=\"POD\",LEFT($F147,8)=\"Diff POD\"),$AP147,$AP147/2))","v":0},{"$f":"IF(OFFSET(IO_STANDARDS,$AJ147,10)=0,$AP147,$AP147/2)","v":1.8},{"$f":"IF(RIGHT($F147,6) =\"(pair)\",2,1)*SUM(I147:K147)","v":0},{"$f":"IF($M147=\"Off\",0,$AK147*OFFSET(IODELAY_DATA,2,3)*$AS147)","v":0},{"$f":"0","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ147,33)*$AK147*$U147*($J147+$K147)*IF(AND($Q147=\"Yes\",OR(LEFT($F147,3)=\"POD\",LEFT($F147,8)=\"Diff POD\",LEFT($F147,4)=\"LVDS\")),2,1)*IF($CI147>0,0.93,1)+OFFSET(IO_STANDARDS,$AJ147,36)*$U147*($J147+$K147)","v":0},{"$f":"(OFFSET(IO_STANDARDS,$AJ147,34)*IF($CF147>0,40/$CF147,1)*$AK147*$U147*IF($Q147=\"Yes\",IF(OR(LEFT($F147,3)=\"POD\",LEFT($F147,8)=\"Diff POD\"),1.17,IF(LEFT($F147,4)=\"LVDS\",2,1)),1)*IF($CI147>0,0.93,1)*$AT$1+OFFSET(IO_STANDARDS,$AJ147,37)*$U147*$AT$1)*($J147+$K147)","v":0},{"$f":"((($I147*(1-$W147)+$K147*(1-$U147))*OFFSET(IO_STANDARDS,$AJ147,11)) + ((($J147+$K147)*$U147)*OFFSET(IO_STANDARDS,$AJ147,10)))/1000  + $AZ147","v":0},{"$f":"IF($CB147>0,IF(LEFT($F147,4)=\"Diff\",2,1)*($I147+$K147*(1-$U147))*IF(AND($AL147=2,$O147=\"DIFF_TERM\"),OFFSET(IO_STANDARDS,$AJ147,18),IF($E147<>\"HR\",IF($CB147>0,1,0)*IF(AL147<>2,IF(OR(LEFT($F147,3)=\"POD\",LEFT($F147,8)=\"Diff POD\"),0.5*1000*$AP147/($CB147+40)*IF($CI147>0,0.36/0.5,1),$AQ147*500/$CB147),OFFSET(IO_STANDARDS,$AJ147,11)),IF(LEFT($O147,3)=\"RTT\",$AQ147*500/$CB147,0))*(1-$V147))/1000,0)","v":0},{"$f":"IF(OR(LEFT($F147,3)=\"POD\",LEFT($F147,8)=\"Diff POD\"),0,IF(IF(LEFT($F147,5)=\"LVDCI\",$J147+$K147,SUM($I147:$K147))>0,((OFFSET(IO_STANDARDS,$AJ147,6)*IF(AND($I147+$K147>0,OFFSET(IO_STANDARDS,$AJ147,6)<1),100,1)*INT((SUM($I147:$K147)+50)/50))/1000),0))","v":0},{"$f":"IF($L147=\"No\",0,$R147*(IF($L147=\"SERDES\",OFFSET(IODELAY_DATA,3,1),IF($L147=\"DELAY\",OFFSET(IODELAY_DATA,2,1),OFFSET(IODELAY_DATA,4,1)))*$AS147+$CC147*OFFSET(IODELAY_DATA,6,1)+$CD147*OFFSET(IODELAY_DATA,5,1)))","v":0},{"$f":"IF(OR($J147+$K147=0,$AL147<>2),0,OFFSET(IODELAY_DATA,IF($E147=\"HR\",27,26),1)*INT((SUM($I147:$K147)+50)/50)/1000)","v":0},0,0,0,0,0,0,{"$f":"IF(ISERROR($AJ147),0,IF($AP147=VCCO10,$AC147/$AP147,0))","v":0},{"$f":"IF(ISERROR($AJ147),0,IF($AP147=VCCO33,$AG147/$AP147,0))","v":0},{"$f":"IF(ISERROR($AJ147),0,IF($AP147=VCCO25,$AG147/$AP147,0))","v":0},{"$f":"IF(ISERROR($AJ147),0,IF($AP147=VCCO18,$AG147/$AP147,0))","v":0},{"$f":"IF(ISERROR($AJ147),0,IF($AP147=VCCO15,$AG147/$AP147,0))","v":0},{"$f":"IF(ISERROR($AJ147),0,IF($AP147=VCCO135,$AG147/$AP147,0))","v":0},{"$f":"IF(ISERROR($AJ147),0,IF($AP147=VCCO12,$AG147/$AP147,0))","v":0},{"$f":"IF(ISERROR($AJ147),0,IF($AP147=VCCO10,$AG147/$AP147,0))","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ147,24+$BU147)*((1-$W147)*I147+(1-U147)*K147)+(OFFSET(IO_STANDARDS,$AJ147,21+$BU147)*$AK147)*((1-$W147)*I147+(1-U147)*K147*IF($CI147>0,0.93,1))","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ147,25+$BU147)*(I147*(1-W147)+K147*(1-U147))+(OFFSET(IO_STANDARDS,$AJ147,22+$BU147)*(I147*(1-W147)+K147*(1-U147)*IF($CI147>0,0.93,1))*$AK147)","v":0},{"$f":"(IF($AY147=0,OFFSET(IO_STANDARDS,$AJ147,11)*(I147*(1-$V147)+K147*(1-$U147)),0)+OFFSET(IO_STANDARDS,$AJ147,23+$BU147)*(I147*(1-$W147)+K147*(1-$U147))*$AK147)/1000","v":0},{"$f":"IF($E147=\"HR\",22,15)+IF(OFFSET(IO_STANDARDS,$AJ147,5)=0,0,IF(ISERR(FIND(\"pair\",OFFSET(IO_STANDARDS,$AJ147,0))),1,2))+IF(OR(LEFT($F147,3)=\"POD\",LEFT($F147,8)=\"Diff POD\"),2,0)","v":15},0,{"$f":"$AK147*2*OFFSET(FANOUT,3,6)*$AS147","v":0},"BW1",0,{"$f":"IF(TRUE,IF($CE147>0,$CE147*$AP147,OFFSET(IO_STANDARDS,$AJ147,13))/1000,(($AP147-OFFSET(IO_STANDARDS,$AJ147,8))*(ABS($AQ147-OFFSET(IO_STANDARDS,$AJ147,8))/$BX147)+OFFSET(IO_STANDARDS,$AJ147,9)*($AQ147-OFFSET(IO_STANDARDS,$AJ147,9))/$BX147)/2)*IF(AND($Q147=\"Yes\",LEFT($F147,4)=\"LVDS\"),1.25,1)","v":0},0,{"$f":"IF(OR(($I147+$K147)<1,LEFT($F147,3)=\"LVC\",LEFT($F147,3)=\"LVT\"),\"BV2\",IF(OFFSET(IO_STANDARDS,$AJ147,18)>0,\"BV1:BV2\",IF(OR(LEFT($F147,3)=\"HSU\",LEFT($F147,8)=\"Diff HSU\"),\"BW7:BW9\",IF(OR(OFFSET(IO_STANDARDS,$AJ147,19)>0,OFFSET(IO_STANDARDS,$AJ147,20)>0,OR(MID($F147,2,3)=\"STL\",LEFT($F147,9)=\"Diff HSTL\",LEFT($F147,9)=\"Diff SSTL\")),IF(OR(E147=\"HR\",OFFSET(IO_STANDARDS,$AJ147,20)=0),\"BV2:BV5\",\"BV7:BV9\"),\"BV2\"))))","v":"BV2"},0,{"$f":"IF($L147=\"No\",0,$AS147/6)","v":0},0,{"$f":"IF(AND(OFFSET(IO_STANDARDS,$AJ147,13)>0,$AL147<>2),IF($CF147>0,IF(LEFT($F147,4)=\"Diff\",2,1)*1000*($AP147/2)/($CF147+MAX(40,$BX147))/2,0),0)","v":0},0,{"$f":"IF(AND(E147<>\"HR\",OR(LEFT($F147,3)<>\"LVC\",OFFSET(IO_STANDARDS,$AJ147,13)>0),$AL147<>2,($J147+$K147)>0),\"CA3:CA5\",\"CA1\")","v":"CA1"},"CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,{"$f":"IF(ISERROR($AJ148),0,VCCINT_IO/1000*VCCINT_N*(BA148+AV148+BQ148))","v":0},0,{"$f":"$AH148","v":0},0,"None",null,null,0,0,0,139,{"$f":"R148*IF(RIGHT(T148,1)=\"R\",S148*IF(T148=\"DDR\",1,0.5),1)","v":0},1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,{"$f":"IF(LEFT($N148,3)=\"Low\",0,6)","v":0},0,{"$f":"IF(OR($AL148=2),\"BW2\",IF(OR(MID(F148,IF(LEFT($F148,4)=\"Diff\",6,1),4)=\"HSTL\",MID(F148,IF(LEFT($F148,4)=\"Diff\",6,1),4)=\"SSTL\",MID(F148,IF(LEFT($F148,4)=\"Diff\",6,1),3)=\"POD\"),IF(E148=\"HR\",\"BW6\",\"BW3:BW5\"),\"BW1\"))","v":"BW1"},{"$f":" IF(OR(ISTEXT($AD148),$AD148=\"None\"),0,$AD148)","v":0},0,0,"BV2",{"$f":"IF(OR(LEN($O148)<1,RIGHT($O148,4)=\"NONE\",RIGHT($O148,4)=\"None\"),0,IF(LEN($O148)<5,IF(E148=\"HR\",48,40),IF(LEFT($O148,3)=\"DCI\",MID($O148,5,2),IF(LEN($O148)>6,IF(RIGHT($O148,3)=\"240\",240,120),RIGHT($O148,2)))))","v":0},0,{"$f":"IF($L148=\"No\",0,IF($K148>0,$AS148/4,$AS148/6))","v":0},0,{"$f":"IF(OR(LEN($P148)<1,RIGHT($P148,4)=\"NONE\"),IF(RIGHT(INDIRECT(LEFT($CG148,3)),2)=\"40\",40,0),IF(LEFT($P148,3)=\"DCI\",MID($P148,5,2),RIGHT($P148,2)))","v":0},"CA1",{"$f":"IF(OR(LEFT($F148,3)=\"POD\",LEFT($F148,8)=\"Diff POD\",LEFT($F148,4)=\"LVDS\",($J148+$K148)>0),\"CC2:CC3\",\"CC1\")","v":"CC1"},{"$f":"IF(AND(LEFT($F148,3)=\"POD\",$K148>0,$T148=\"DDR\",NOT(ISERROR(SEARCH(\"ddr4_dq<\",$B148,1)))),1,0)","v":0}]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R152*IF(RIGHT(T152,1)=\"R\",S152*IF(T152=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R158*IF(RIGHT(T158,1)=\"R\",S158*IF(T158=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R164*IF(RIGHT(T164,1)=\"R\",S164*IF(T164=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R170*IF(RIGHT(T170,1)=\"R\",S170*IF(T170=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R176*IF(RIGHT(T176,1)=\"R\",S176*IF(T176=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R182*IF(RIGHT(T182,1)=\"R\",S182*IF(T182=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R188*IF(RIGHT(T188,1)=\"R\",S188*IF(T188=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,{"$f":"MATCH($F193,IF($E193=\"HR\",SIOSTD_LIST,VIOSTD_LIST),FALSE)+IF($E193=\"HR\",0,ROW(VIOSTD_LIST)-ROW(SIOSTD_LIST))","v":139},0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,{"$f":"IF(ISERROR($AJ193),0,IF($AP193=VCCO33,$AC193/$AP193+$AZ193,0))","v":0},{"$f":"IF(ISERROR($AJ193),0,IF($AP193=VCCO25,$AC193/$AP193+$AZ193,0))","v":0},{"$f":"IF(ISERROR($AJ193),0,IF($AP193=VCCO18,$AC193/$AP193,0))","v":0},{"$f":"IF(ISERROR($AJ193),0,IF($AP193=VCCO15,$AC193/$AP193,0))","v":0},{"$f":"IF(ISERROR($AJ193),0,IF($AP193=VCCO135,$AC193/$AP193,0))","v":0},{"$f":"IF(ISERROR($AJ193),0,IF($AP193=VCCO12,$AC193/$AP193,0))","v":0},0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R194*IF(RIGHT(T194,1)=\"R\",S194*IF(T194=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R200*IF(RIGHT(T200,1)=\"R\",S200*IF(T200=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R206*IF(RIGHT(T206,1)=\"R\",S206*IF(T206=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,{"$f":"$V211","v":0},0,0,0,{"$f":"IF(ISERROR($AJ211),0,MAX(0,($AU211+$AW211+$BR211)*VCCAUX_IO/1000))","v":0},0,{"$f":"IF(ISERROR($AJ211),0,MAX(0,OFFSET($AL211,0,$AL211)+(($J211*IF(AND($AL211<>2,LEFT($F211,2)<>\"LV\",RIGHT(T211,1)=\"R\"),S211+(1-S211)/2,1)+K211*IF(AND($AL211<>2,LEFT($F211,2)<>\"LV\",RIGHT(T211,1)=\"R\"),S211,1))*$U211)*$BY211+$I211*OFFSET(IO_STANDARDS,$AJ211,14)/1000+($AY211+$BS211)*$AP211))","v":0},"None",null,null,{"$f":"IF(ISERROR($AJ211),0,IF(AD211=\"None\",0,$BZ211*(($J211+K211)*$U211)))","v":0},{"$f":"IF(ISERROR($AJ211),0,VCCINT/1000*VCCINT_N*(IF($L211=\"No\",0,$R211*$AS211*OFFSET(IODELAY_DATA,9,3))+BV211))","v":0},{"$f":"IF(ISERROR($AJ211),0,VCCINT_IO/1000*VCCINT_N*(BA211))","v":0},139,0,{"$f":"IF(AND($K211>0,$E211=\"HR\",OFFSET(IO_STANDARDS,$AJ211,19)>0),3,OFFSET(IO_STANDARDS,$AJ211,2))","v":1},{"$f":"(OFFSET(IO_STANDARDS,$AJ211,35)*($X211+OFFSET(IO_STANDARDS,$AJ211,3))*($J211+$K211*IF($CI211>0,0.93,1))*$AP211*$AK211*$U211*$AT$1)/1000","v":0},{"$f":"MAX(0,(OFFSET(IO_STANDARDS,$AJ211,35)*($X211+OFFSET(IO_STANDARDS,$AJ211,3))*($J211+$K211)*$AP211*$AK211*$U211*$AT$1/1000))","v":0},{"$f":"(((OFFSET(IO_STANDARDS,$AJ211,35)*($X211+OFFSET(IO_STANDARDS,$AJ211,3))*$AP211/1000)*($J211+$K211*IF($CI211>0,0.93,1))*$AK211*$U211*$AT$1))","v":0},{"$f":"IF(ISERROR($AJ211),0,OFFSET(IO_STANDARDS,$AJ211,1))","v":1.8},{"$f":"IF(OFFSET(IO_STANDARDS,$AJ211,9)=0,0,IF(OR(LEFT($F211,14)=\"HSTL Class III\",LEFT($F211,13)=\"HSTL Class IV\",LEFT($F211,3)=\"GTL\",LEFT($F211,3)=\"POD\",LEFT($F211,8)=\"Diff POD\"),$AP211,$AP211/2))","v":0},{"$f":"IF(OFFSET(IO_STANDARDS,$AJ211,10)=0,$AP211,$AP211/2)","v":1.8},{"$f":"IF(RIGHT($F211,6) =\"(pair)\",2,1)*SUM(I211:K211)","v":0},{"$f":"IF($M211=\"Off\",0,$AK211*OFFSET(IODELAY_DATA,2,3)*$AS211)","v":0},{"$f":"0","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ211,33)*$AK211*$U211*($J211+$K211)*IF(AND($Q211=\"Yes\",OR(LEFT($F211,3)=\"POD\",LEFT($F211,8)=\"Diff POD\",LEFT($F211,4)=\"LVDS\")),2,1)*IF($CI211>0,0.93,1)+OFFSET(IO_STANDARDS,$AJ211,36)*$U211*($J211+$K211)","v":0},{"$f":"(OFFSET(IO_STANDARDS,$AJ211,34)*IF($CF211>0,40/$CF211,1)*$AK211*$U211*IF($Q211=\"Yes\",IF(OR(LEFT($F211,3)=\"POD\",LEFT($F211,8)=\"Diff POD\"),1.17,IF(LEFT($F211,4)=\"LVDS\",2,1)),1)*IF($CI211>0,0.93,1)*$AT$1+OFFSET(IO_STANDARDS,$AJ211,37)*$U211*$AT$1)*($J211+$K211)","v":0},{"$f":"((($I211*(1-$W211)+$K211*(1-$U211))*OFFSET(IO_STANDARDS,$AJ211,11)) + ((($J211+$K211)*$U211)*OFFSET(IO_STANDARDS,$AJ211,10)))/1000  + $AZ211","v":0},{"$f":"IF($CB211>0,IF(LEFT($F211,4)=\"Diff\",2,1)*($I211+$K211*(1-$U211))*IF(AND($AL211=2,$O211=\"DIFF_TERM\"),OFFSET(IO_STANDARDS,$AJ211,18),IF($E211<>\"HR\",IF($CB211>0,1,0)*IF(AL211<>2,IF(OR(LEFT($F211,3)=\"POD\",LEFT($F211,8)=\"Diff POD\"),0.5*1000*$AP211/($CB211+40)*IF($CI211>0,0.36/0.5,1),$AQ211*500/$CB211),OFFSET(IO_STANDARDS,$AJ211,11)),IF(LEFT($O211,3)=\"RTT\",$AQ211*500/$CB211,0))*(1-$V211))/1000,0)","v":0},{"$f":"IF(OR(LEFT($F211,3)=\"POD\",LEFT($F211,8)=\"Diff POD\"),0,IF(IF(LEFT($F211,5)=\"LVDCI\",$J211+$K211,SUM($I211:$K211))>0,((OFFSET(IO_STANDARDS,$AJ211,6)*IF(AND($I211+$K211>0,OFFSET(IO_STANDARDS,$AJ211,6)<1),100,1)*INT((SUM($I211:$K211)+50)/50))/1000),0))","v":0},{"$f":"IF($L211=\"No\",0,$R211*(IF($L211=\"SERDES\",OFFSET(IODELAY_DATA,3,1),IF($L211=\"DELAY\",OFFSET(IODELAY_DATA,2,1),OFFSET(IODELAY_DATA,4,1)))*$AS211+$CC211*OFFSET(IODELAY_DATA,6,1)+$CD211*OFFSET(IODELAY_DATA,5,1)))","v":0},{"$f":"IF(OR($J211+$K211=0,$AL211<>2),0,OFFSET(IODELAY_DATA,IF($E211=\"HR\",27,26),1)*INT((SUM($I211:$K211)+50)/50)/1000)","v":0},0,0,0,0,0,0,{"$f":"IF(ISERROR($AJ211),0,IF($AP211=VCCO10,$AC211/$AP211,0))","v":0},{"$f":"IF(ISERROR($AJ211),0,IF($AP211=VCCO33,$AG211/$AP211,0))","v":0},{"$f":"IF(ISERROR($AJ211),0,IF($AP211=VCCO25,$AG211/$AP211,0))","v":0},{"$f":"IF(ISERROR($AJ211),0,IF($AP211=VCCO18,$AG211/$AP211,0))","v":0},{"$f":"IF(ISERROR($AJ211),0,IF($AP211=VCCO15,$AG211/$AP211,0))","v":0},{"$f":"IF(ISERROR($AJ211),0,IF($AP211=VCCO135,$AG211/$AP211,0))","v":0},{"$f":"IF(ISERROR($AJ211),0,IF($AP211=VCCO12,$AG211/$AP211,0))","v":0},{"$f":"IF(ISERROR($AJ211),0,IF($AP211=VCCO10,$AG211/$AP211,0))","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ211,24+$BU211)*((1-$W211)*I211+(1-U211)*K211)+(OFFSET(IO_STANDARDS,$AJ211,21+$BU211)*$AK211)*((1-$W211)*I211+(1-U211)*K211*IF($CI211>0,0.93,1))","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ211,25+$BU211)*(I211*(1-W211)+K211*(1-U211))+(OFFSET(IO_STANDARDS,$AJ211,22+$BU211)*(I211*(1-W211)+K211*(1-U211)*IF($CI211>0,0.93,1))*$AK211)","v":0},{"$f":"(IF($AY211=0,OFFSET(IO_STANDARDS,$AJ211,11)*(I211*(1-$V211)+K211*(1-$U211)),0)+OFFSET(IO_STANDARDS,$AJ211,23+$BU211)*(I211*(1-$W211)+K211*(1-$U211))*$AK211)/1000","v":0},{"$f":"IF($E211=\"HR\",22,15)+IF(OFFSET(IO_STANDARDS,$AJ211,5)=0,0,IF(ISERR(FIND(\"pair\",OFFSET(IO_STANDARDS,$AJ211,0))),1,2))+IF(OR(LEFT($F211,3)=\"POD\",LEFT($F211,8)=\"Diff POD\"),2,0)","v":15},0,{"$f":"$AK211*2*OFFSET(FANOUT,3,6)*$AS211","v":0},"BW1",0,{"$f":"IF(TRUE,IF($CE211>0,$CE211*$AP211,OFFSET(IO_STANDARDS,$AJ211,13))/1000,(($AP211-OFFSET(IO_STANDARDS,$AJ211,8))*(ABS($AQ211-OFFSET(IO_STANDARDS,$AJ211,8))/$BX211)+OFFSET(IO_STANDARDS,$AJ211,9)*($AQ211-OFFSET(IO_STANDARDS,$AJ211,9))/$BX211)/2)*IF(AND($Q211=\"Yes\",LEFT($F211,4)=\"LVDS\"),1.25,1)","v":0},0,{"$f":"IF(OR(($I211+$K211)<1,LEFT($F211,3)=\"LVC\",LEFT($F211,3)=\"LVT\"),\"BV2\",IF(OFFSET(IO_STANDARDS,$AJ211,18)>0,\"BV1:BV2\",IF(OR(LEFT($F211,3)=\"HSU\",LEFT($F211,8)=\"Diff HSU\"),\"BW7:BW9\",IF(OR(OFFSET(IO_STANDARDS,$AJ211,19)>0,OFFSET(IO_STANDARDS,$AJ211,20)>0,OR(MID($F211,2,3)=\"STL\",LEFT($F211,9)=\"Diff HSTL\",LEFT($F211,9)=\"Diff SSTL\")),IF(OR(E211=\"HR\",OFFSET(IO_STANDARDS,$AJ211,20)=0),\"BV2:BV5\",\"BV7:BV9\"),\"BV2\"))))","v":"BV2"},0,{"$f":"IF($L211=\"No\",0,$AS211/6)","v":0},0,{"$f":"IF(AND(OFFSET(IO_STANDARDS,$AJ211,13)>0,$AL211<>2),IF($CF211>0,IF(LEFT($F211,4)=\"Diff\",2,1)*1000*($AP211/2)/($CF211+MAX(40,$BX211))/2,0),0)","v":0},0,{"$f":"IF(AND(E211<>\"HR\",OR(LEFT($F211,3)<>\"LVC\",OFFSET(IO_STANDARDS,$AJ211,13)>0),$AL211<>2,($J211+$K211)>0),\"CA3:CA5\",\"CA1\")","v":"CA1"},"CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R212*IF(RIGHT(T212,1)=\"R\",S212*IF(T212=\"DDR\",2,1),2)","v":0},{"$f":"IF(ISERROR($AJ212),0,VCCINT_IO/1000*VCCINT_N*(BA212+AV212+BQ212))","v":0},0,{"$f":"$AH212","v":0},0,"None",null,null,0,0,0,139,{"$f":"R212*IF(RIGHT(T212,1)=\"R\",S212*IF(T212=\"DDR\",1,0.5),1)","v":0},1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,{"$f":"IF(LEFT($N212,3)=\"Low\",0,6)","v":0},0,{"$f":"IF(OR($AL212=2),\"BW2\",IF(OR(MID(F212,IF(LEFT($F212,4)=\"Diff\",6,1),4)=\"HSTL\",MID(F212,IF(LEFT($F212,4)=\"Diff\",6,1),4)=\"SSTL\",MID(F212,IF(LEFT($F212,4)=\"Diff\",6,1),3)=\"POD\"),IF(E212=\"HR\",\"BW6\",\"BW3:BW5\"),\"BW1\"))","v":"BW1"},{"$f":" IF(OR(ISTEXT($AD212),$AD212=\"None\"),0,$AD212)","v":0},0,0,"BV2",{"$f":"IF(OR(LEN($O212)<1,RIGHT($O212,4)=\"NONE\",RIGHT($O212,4)=\"None\"),0,IF(LEN($O212)<5,IF(E212=\"HR\",48,40),IF(LEFT($O212,3)=\"DCI\",MID($O212,5,2),IF(LEN($O212)>6,IF(RIGHT($O212,3)=\"240\",240,120),RIGHT($O212,2)))))","v":0},0,{"$f":"IF($L212=\"No\",0,IF($K212>0,$AS212/4,$AS212/6))","v":0},0,{"$f":"IF(OR(LEN($P212)<1,RIGHT($P212,4)=\"NONE\"),IF(RIGHT(INDIRECT(LEFT($CG212,3)),2)=\"40\",40,0),IF(LEFT($P212,3)=\"DCI\",MID($P212,5,2),RIGHT($P212,2)))","v":0},"CA1",{"$f":"IF(OR(LEFT($F212,3)=\"POD\",LEFT($F212,8)=\"Diff POD\",LEFT($F212,4)=\"LVDS\",($J212+$K212)>0),\"CC2:CC3\",\"CC1\")","v":"CC1"},{"$f":"IF(AND(LEFT($F212,3)=\"POD\",$K212>0,$T212=\"DDR\",NOT(ISERROR(SEARCH(\"ddr4_dq<\",$B212,1)))),1,0)","v":0}]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R218*IF(RIGHT(T218,1)=\"R\",S218*IF(T218=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R224*IF(RIGHT(T224,1)=\"R\",S224*IF(T224=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R230*IF(RIGHT(T230,1)=\"R\",S230*IF(T230=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R236*IF(RIGHT(T236,1)=\"R\",S236*IF(T236=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R242*IF(RIGHT(T242,1)=\"R\",S242*IF(T242=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R248*IF(RIGHT(T248,1)=\"R\",S248*IF(T248=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R254*IF(RIGHT(T254,1)=\"R\",S254*IF(T254=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,{"$f":"MATCH($F257,IF($E257=\"HR\",SIOSTD_LIST,VIOSTD_LIST),FALSE)+IF($E257=\"HR\",0,ROW(VIOSTD_LIST)-ROW(SIOSTD_LIST))","v":139},0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,{"$f":"IF(ISERROR($AJ257),0,IF($AP257=VCCO33,$AC257/$AP257+$AZ257,0))","v":0},{"$f":"IF(ISERROR($AJ257),0,IF($AP257=VCCO25,$AC257/$AP257+$AZ257,0))","v":0},{"$f":"IF(ISERROR($AJ257),0,IF($AP257=VCCO18,$AC257/$AP257,0))","v":0},{"$f":"IF(ISERROR($AJ257),0,IF($AP257=VCCO15,$AC257/$AP257,0))","v":0},{"$f":"IF(ISERROR($AJ257),0,IF($AP257=VCCO135,$AC257/$AP257,0))","v":0},{"$f":"IF(ISERROR($AJ257),0,IF($AP257=VCCO12,$AC257/$AP257,0))","v":0},0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R260*IF(RIGHT(T260,1)=\"R\",S260*IF(T260=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R266*IF(RIGHT(T266,1)=\"R\",S266*IF(T266=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R272*IF(RIGHT(T272,1)=\"R\",S272*IF(T272=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,{"$f":"$V275","v":0},0,0,0,{"$f":"IF(ISERROR($AJ275),0,MAX(0,($AU275+$AW275+$BR275)*VCCAUX_IO/1000))","v":0},0,{"$f":"IF(ISERROR($AJ275),0,MAX(0,OFFSET($AL275,0,$AL275)+(($J275*IF(AND($AL275<>2,LEFT($F275,2)<>\"LV\",RIGHT(T275,1)=\"R\"),S275+(1-S275)/2,1)+K275*IF(AND($AL275<>2,LEFT($F275,2)<>\"LV\",RIGHT(T275,1)=\"R\"),S275,1))*$U275)*$BY275+$I275*OFFSET(IO_STANDARDS,$AJ275,14)/1000+($AY275+$BS275)*$AP275))","v":0},"None",null,null,{"$f":"IF(ISERROR($AJ275),0,IF(AD275=\"None\",0,$BZ275*(($J275+K275)*$U275)))","v":0},{"$f":"IF(ISERROR($AJ275),0,VCCINT/1000*VCCINT_N*(IF($L275=\"No\",0,$R275*$AS275*OFFSET(IODELAY_DATA,9,3))+BV275))","v":0},{"$f":"IF(ISERROR($AJ275),0,VCCINT_IO/1000*VCCINT_N*(BA275))","v":0},139,0,{"$f":"IF(AND($K275>0,$E275=\"HR\",OFFSET(IO_STANDARDS,$AJ275,19)>0),3,OFFSET(IO_STANDARDS,$AJ275,2))","v":1},{"$f":"(OFFSET(IO_STANDARDS,$AJ275,35)*($X275+OFFSET(IO_STANDARDS,$AJ275,3))*($J275+$K275*IF($CI275>0,0.93,1))*$AP275*$AK275*$U275*$AT$1)/1000","v":0},{"$f":"MAX(0,(OFFSET(IO_STANDARDS,$AJ275,35)*($X275+OFFSET(IO_STANDARDS,$AJ275,3))*($J275+$K275)*$AP275*$AK275*$U275*$AT$1/1000))","v":0},{"$f":"(((OFFSET(IO_STANDARDS,$AJ275,35)*($X275+OFFSET(IO_STANDARDS,$AJ275,3))*$AP275/1000)*($J275+$K275*IF($CI275>0,0.93,1))*$AK275*$U275*$AT$1))","v":0},{"$f":"IF(ISERROR($AJ275),0,OFFSET(IO_STANDARDS,$AJ275,1))","v":1.8},{"$f":"IF(OFFSET(IO_STANDARDS,$AJ275,9)=0,0,IF(OR(LEFT($F275,14)=\"HSTL Class III\",LEFT($F275,13)=\"HSTL Class IV\",LEFT($F275,3)=\"GTL\",LEFT($F275,3)=\"POD\",LEFT($F275,8)=\"Diff POD\"),$AP275,$AP275/2))","v":0},{"$f":"IF(OFFSET(IO_STANDARDS,$AJ275,10)=0,$AP275,$AP275/2)","v":1.8},{"$f":"IF(RIGHT($F275,6) =\"(pair)\",2,1)*SUM(I275:K275)","v":0},{"$f":"IF($M275=\"Off\",0,$AK275*OFFSET(IODELAY_DATA,2,3)*$AS275)","v":0},{"$f":"0","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ275,33)*$AK275*$U275*($J275+$K275)*IF(AND($Q275=\"Yes\",OR(LEFT($F275,3)=\"POD\",LEFT($F275,8)=\"Diff POD\",LEFT($F275,4)=\"LVDS\")),2,1)*IF($CI275>0,0.93,1)+OFFSET(IO_STANDARDS,$AJ275,36)*$U275*($J275+$K275)","v":0},{"$f":"(OFFSET(IO_STANDARDS,$AJ275,34)*IF($CF275>0,40/$CF275,1)*$AK275*$U275*IF($Q275=\"Yes\",IF(OR(LEFT($F275,3)=\"POD\",LEFT($F275,8)=\"Diff POD\"),1.17,IF(LEFT($F275,4)=\"LVDS\",2,1)),1)*IF($CI275>0,0.93,1)*$AT$1+OFFSET(IO_STANDARDS,$AJ275,37)*$U275*$AT$1)*($J275+$K275)","v":0},{"$f":"((($I275*(1-$W275)+$K275*(1-$U275))*OFFSET(IO_STANDARDS,$AJ275,11)) + ((($J275+$K275)*$U275)*OFFSET(IO_STANDARDS,$AJ275,10)))/1000  + $AZ275","v":0},{"$f":"IF($CB275>0,IF(LEFT($F275,4)=\"Diff\",2,1)*($I275+$K275*(1-$U275))*IF(AND($AL275=2,$O275=\"DIFF_TERM\"),OFFSET(IO_STANDARDS,$AJ275,18),IF($E275<>\"HR\",IF($CB275>0,1,0)*IF(AL275<>2,IF(OR(LEFT($F275,3)=\"POD\",LEFT($F275,8)=\"Diff POD\"),0.5*1000*$AP275/($CB275+40)*IF($CI275>0,0.36/0.5,1),$AQ275*500/$CB275),OFFSET(IO_STANDARDS,$AJ275,11)),IF(LEFT($O275,3)=\"RTT\",$AQ275*500/$CB275,0))*(1-$V275))/1000,0)","v":0},{"$f":"IF(OR(LEFT($F275,3)=\"POD\",LEFT($F275,8)=\"Diff POD\"),0,IF(IF(LEFT($F275,5)=\"LVDCI\",$J275+$K275,SUM($I275:$K275))>0,((OFFSET(IO_STANDARDS,$AJ275,6)*IF(AND($I275+$K275>0,OFFSET(IO_STANDARDS,$AJ275,6)<1),100,1)*INT((SUM($I275:$K275)+50)/50))/1000),0))","v":0},{"$f":"IF($L275=\"No\",0,$R275*(IF($L275=\"SERDES\",OFFSET(IODELAY_DATA,3,1),IF($L275=\"DELAY\",OFFSET(IODELAY_DATA,2,1),OFFSET(IODELAY_DATA,4,1)))*$AS275+$CC275*OFFSET(IODELAY_DATA,6,1)+$CD275*OFFSET(IODELAY_DATA,5,1)))","v":0},{"$f":"IF(OR($J275+$K275=0,$AL275<>2),0,OFFSET(IODELAY_DATA,IF($E275=\"HR\",27,26),1)*INT((SUM($I275:$K275)+50)/50)/1000)","v":0},0,0,0,0,0,0,{"$f":"IF(ISERROR($AJ275),0,IF($AP275=VCCO10,$AC275/$AP275,0))","v":0},{"$f":"IF(ISERROR($AJ275),0,IF($AP275=VCCO33,$AG275/$AP275,0))","v":0},{"$f":"IF(ISERROR($AJ275),0,IF($AP275=VCCO25,$AG275/$AP275,0))","v":0},{"$f":"IF(ISERROR($AJ275),0,IF($AP275=VCCO18,$AG275/$AP275,0))","v":0},{"$f":"IF(ISERROR($AJ275),0,IF($AP275=VCCO15,$AG275/$AP275,0))","v":0},{"$f":"IF(ISERROR($AJ275),0,IF($AP275=VCCO135,$AG275/$AP275,0))","v":0},{"$f":"IF(ISERROR($AJ275),0,IF($AP275=VCCO12,$AG275/$AP275,0))","v":0},{"$f":"IF(ISERROR($AJ275),0,IF($AP275=VCCO10,$AG275/$AP275,0))","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ275,24+$BU275)*((1-$W275)*I275+(1-U275)*K275)+(OFFSET(IO_STANDARDS,$AJ275,21+$BU275)*$AK275)*((1-$W275)*I275+(1-U275)*K275*IF($CI275>0,0.93,1))","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ275,25+$BU275)*(I275*(1-W275)+K275*(1-U275))+(OFFSET(IO_STANDARDS,$AJ275,22+$BU275)*(I275*(1-W275)+K275*(1-U275)*IF($CI275>0,0.93,1))*$AK275)","v":0},{"$f":"(IF($AY275=0,OFFSET(IO_STANDARDS,$AJ275,11)*(I275*(1-$V275)+K275*(1-$U275)),0)+OFFSET(IO_STANDARDS,$AJ275,23+$BU275)*(I275*(1-$W275)+K275*(1-$U275))*$AK275)/1000","v":0},{"$f":"IF($E275=\"HR\",22,15)+IF(OFFSET(IO_STANDARDS,$AJ275,5)=0,0,IF(ISERR(FIND(\"pair\",OFFSET(IO_STANDARDS,$AJ275,0))),1,2))+IF(OR(LEFT($F275,3)=\"POD\",LEFT($F275,8)=\"Diff POD\"),2,0)","v":15},0,{"$f":"$AK275*2*OFFSET(FANOUT,3,6)*$AS275","v":0},"BW1",0,{"$f":"IF(TRUE,IF($CE275>0,$CE275*$AP275,OFFSET(IO_STANDARDS,$AJ275,13))/1000,(($AP275-OFFSET(IO_STANDARDS,$AJ275,8))*(ABS($AQ275-OFFSET(IO_STANDARDS,$AJ275,8))/$BX275)+OFFSET(IO_STANDARDS,$AJ275,9)*($AQ275-OFFSET(IO_STANDARDS,$AJ275,9))/$BX275)/2)*IF(AND($Q275=\"Yes\",LEFT($F275,4)=\"LVDS\"),1.25,1)","v":0},0,{"$f":"IF(OR(($I275+$K275)<1,LEFT($F275,3)=\"LVC\",LEFT($F275,3)=\"LVT\"),\"BV2\",IF(OFFSET(IO_STANDARDS,$AJ275,18)>0,\"BV1:BV2\",IF(OR(LEFT($F275,3)=\"HSU\",LEFT($F275,8)=\"Diff HSU\"),\"BW7:BW9\",IF(OR(OFFSET(IO_STANDARDS,$AJ275,19)>0,OFFSET(IO_STANDARDS,$AJ275,20)>0,OR(MID($F275,2,3)=\"STL\",LEFT($F275,9)=\"Diff HSTL\",LEFT($F275,9)=\"Diff SSTL\")),IF(OR(E275=\"HR\",OFFSET(IO_STANDARDS,$AJ275,20)=0),\"BV2:BV5\",\"BV7:BV9\"),\"BV2\"))))","v":"BV2"},0,{"$f":"IF($L275=\"No\",0,$AS275/6)","v":0},0,{"$f":"IF(AND(OFFSET(IO_STANDARDS,$AJ275,13)>0,$AL275<>2),IF($CF275>0,IF(LEFT($F275,4)=\"Diff\",2,1)*1000*($AP275/2)/($CF275+MAX(40,$BX275))/2,0),0)","v":0},0,{"$f":"IF(AND(E275<>\"HR\",OR(LEFT($F275,3)<>\"LVC\",OFFSET(IO_STANDARDS,$AJ275,13)>0),$AL275<>2,($J275+$K275)>0),\"CA3:CA5\",\"CA1\")","v":"CA1"},"CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,{"$f":"IF(ISERROR($AJ276),0,VCCINT_IO/1000*VCCINT_N*(BA276+AV276+BQ276))","v":0},0,{"$f":"$AH276","v":0},0,"None",null,null,0,0,0,139,{"$f":"R276*IF(RIGHT(T276,1)=\"R\",S276*IF(T276=\"DDR\",1,0.5),1)","v":0},1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,{"$f":"IF(LEFT($N276,3)=\"Low\",0,6)","v":0},0,{"$f":"IF(OR($AL276=2),\"BW2\",IF(OR(MID(F276,IF(LEFT($F276,4)=\"Diff\",6,1),4)=\"HSTL\",MID(F276,IF(LEFT($F276,4)=\"Diff\",6,1),4)=\"SSTL\",MID(F276,IF(LEFT($F276,4)=\"Diff\",6,1),3)=\"POD\"),IF(E276=\"HR\",\"BW6\",\"BW3:BW5\"),\"BW1\"))","v":"BW1"},{"$f":" IF(OR(ISTEXT($AD276),$AD276=\"None\"),0,$AD276)","v":0},0,0,"BV2",{"$f":"IF(OR(LEN($O276)<1,RIGHT($O276,4)=\"NONE\",RIGHT($O276,4)=\"None\"),0,IF(LEN($O276)<5,IF(E276=\"HR\",48,40),IF(LEFT($O276,3)=\"DCI\",MID($O276,5,2),IF(LEN($O276)>6,IF(RIGHT($O276,3)=\"240\",240,120),RIGHT($O276,2)))))","v":0},0,{"$f":"IF($L276=\"No\",0,IF($K276>0,$AS276/4,$AS276/6))","v":0},0,{"$f":"IF(OR(LEN($P276)<1,RIGHT($P276,4)=\"NONE\"),IF(RIGHT(INDIRECT(LEFT($CG276,3)),2)=\"40\",40,0),IF(LEFT($P276,3)=\"DCI\",MID($P276,5,2),RIGHT($P276,2)))","v":0},"CA1",{"$f":"IF(OR(LEFT($F276,3)=\"POD\",LEFT($F276,8)=\"Diff POD\",LEFT($F276,4)=\"LVDS\",($J276+$K276)>0),\"CC2:CC3\",\"CC1\")","v":"CC1"},{"$f":"IF(AND(LEFT($F276,3)=\"POD\",$K276>0,$T276=\"DDR\",NOT(ISERROR(SEARCH(\"ddr4_dq<\",$B276,1)))),1,0)","v":0}]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R278*IF(RIGHT(T278,1)=\"R\",S278*IF(T278=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R284*IF(RIGHT(T284,1)=\"R\",S284*IF(T284=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R290*IF(RIGHT(T290,1)=\"R\",S290*IF(T290=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R296*IF(RIGHT(T296,1)=\"R\",S296*IF(T296=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R302*IF(RIGHT(T302,1)=\"R\",S302*IF(T302=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R308*IF(RIGHT(T308,1)=\"R\",S308*IF(T308=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R314*IF(RIGHT(T314,1)=\"R\",S314*IF(T314=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R320*IF(RIGHT(T320,1)=\"R\",S320*IF(T320=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,{"$f":"MATCH($F321,IF($E321=\"HR\",SIOSTD_LIST,VIOSTD_LIST),FALSE)+IF($E321=\"HR\",0,ROW(VIOSTD_LIST)-ROW(SIOSTD_LIST))","v":139},0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,{"$f":"IF(ISERROR($AJ321),0,IF($AP321=VCCO33,$AC321/$AP321+$AZ321,0))","v":0},{"$f":"IF(ISERROR($AJ321),0,IF($AP321=VCCO25,$AC321/$AP321+$AZ321,0))","v":0},{"$f":"IF(ISERROR($AJ321),0,IF($AP321=VCCO18,$AC321/$AP321,0))","v":0},{"$f":"IF(ISERROR($AJ321),0,IF($AP321=VCCO15,$AC321/$AP321,0))","v":0},{"$f":"IF(ISERROR($AJ321),0,IF($AP321=VCCO135,$AC321/$AP321,0))","v":0},{"$f":"IF(ISERROR($AJ321),0,IF($AP321=VCCO12,$AC321/$AP321,0))","v":0},0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R326*IF(RIGHT(T326,1)=\"R\",S326*IF(T326=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R332*IF(RIGHT(T332,1)=\"R\",S332*IF(T332=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R338*IF(RIGHT(T338,1)=\"R\",S338*IF(T338=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,{"$f":"$V339","v":0},0,0,0,{"$f":"IF(ISERROR($AJ339),0,MAX(0,($AU339+$AW339+$BR339)*VCCAUX_IO/1000))","v":0},0,{"$f":"IF(ISERROR($AJ339),0,MAX(0,OFFSET($AL339,0,$AL339)+(($J339*IF(AND($AL339<>2,LEFT($F339,2)<>\"LV\",RIGHT(T339,1)=\"R\"),S339+(1-S339)/2,1)+K339*IF(AND($AL339<>2,LEFT($F339,2)<>\"LV\",RIGHT(T339,1)=\"R\"),S339,1))*$U339)*$BY339+$I339*OFFSET(IO_STANDARDS,$AJ339,14)/1000+($AY339+$BS339)*$AP339))","v":0},"None",null,null,{"$f":"IF(ISERROR($AJ339),0,IF(AD339=\"None\",0,$BZ339*(($J339+K339)*$U339)))","v":0},{"$f":"IF(ISERROR($AJ339),0,VCCINT/1000*VCCINT_N*(IF($L339=\"No\",0,$R339*$AS339*OFFSET(IODELAY_DATA,9,3))+BV339))","v":0},{"$f":"IF(ISERROR($AJ339),0,VCCINT_IO/1000*VCCINT_N*(BA339))","v":0},139,0,{"$f":"IF(AND($K339>0,$E339=\"HR\",OFFSET(IO_STANDARDS,$AJ339,19)>0),3,OFFSET(IO_STANDARDS,$AJ339,2))","v":1},{"$f":"(OFFSET(IO_STANDARDS,$AJ339,35)*($X339+OFFSET(IO_STANDARDS,$AJ339,3))*($J339+$K339*IF($CI339>0,0.93,1))*$AP339*$AK339*$U339*$AT$1)/1000","v":0},{"$f":"MAX(0,(OFFSET(IO_STANDARDS,$AJ339,35)*($X339+OFFSET(IO_STANDARDS,$AJ339,3))*($J339+$K339)*$AP339*$AK339*$U339*$AT$1/1000))","v":0},{"$f":"(((OFFSET(IO_STANDARDS,$AJ339,35)*($X339+OFFSET(IO_STANDARDS,$AJ339,3))*$AP339/1000)*($J339+$K339*IF($CI339>0,0.93,1))*$AK339*$U339*$AT$1))","v":0},{"$f":"IF(ISERROR($AJ339),0,OFFSET(IO_STANDARDS,$AJ339,1))","v":1.8},{"$f":"IF(OFFSET(IO_STANDARDS,$AJ339,9)=0,0,IF(OR(LEFT($F339,14)=\"HSTL Class III\",LEFT($F339,13)=\"HSTL Class IV\",LEFT($F339,3)=\"GTL\",LEFT($F339,3)=\"POD\",LEFT($F339,8)=\"Diff POD\"),$AP339,$AP339/2))","v":0},{"$f":"IF(OFFSET(IO_STANDARDS,$AJ339,10)=0,$AP339,$AP339/2)","v":1.8},{"$f":"IF(RIGHT($F339,6) =\"(pair)\",2,1)*SUM(I339:K339)","v":0},{"$f":"IF($M339=\"Off\",0,$AK339*OFFSET(IODELAY_DATA,2,3)*$AS339)","v":0},{"$f":"0","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ339,33)*$AK339*$U339*($J339+$K339)*IF(AND($Q339=\"Yes\",OR(LEFT($F339,3)=\"POD\",LEFT($F339,8)=\"Diff POD\",LEFT($F339,4)=\"LVDS\")),2,1)*IF($CI339>0,0.93,1)+OFFSET(IO_STANDARDS,$AJ339,36)*$U339*($J339+$K339)","v":0},{"$f":"(OFFSET(IO_STANDARDS,$AJ339,34)*IF($CF339>0,40/$CF339,1)*$AK339*$U339*IF($Q339=\"Yes\",IF(OR(LEFT($F339,3)=\"POD\",LEFT($F339,8)=\"Diff POD\"),1.17,IF(LEFT($F339,4)=\"LVDS\",2,1)),1)*IF($CI339>0,0.93,1)*$AT$1+OFFSET(IO_STANDARDS,$AJ339,37)*$U339*$AT$1)*($J339+$K339)","v":0},{"$f":"((($I339*(1-$W339)+$K339*(1-$U339))*OFFSET(IO_STANDARDS,$AJ339,11)) + ((($J339+$K339)*$U339)*OFFSET(IO_STANDARDS,$AJ339,10)))/1000  + $AZ339","v":0},{"$f":"IF($CB339>0,IF(LEFT($F339,4)=\"Diff\",2,1)*($I339+$K339*(1-$U339))*IF(AND($AL339=2,$O339=\"DIFF_TERM\"),OFFSET(IO_STANDARDS,$AJ339,18),IF($E339<>\"HR\",IF($CB339>0,1,0)*IF(AL339<>2,IF(OR(LEFT($F339,3)=\"POD\",LEFT($F339,8)=\"Diff POD\"),0.5*1000*$AP339/($CB339+40)*IF($CI339>0,0.36/0.5,1),$AQ339*500/$CB339),OFFSET(IO_STANDARDS,$AJ339,11)),IF(LEFT($O339,3)=\"RTT\",$AQ339*500/$CB339,0))*(1-$V339))/1000,0)","v":0},{"$f":"IF(OR(LEFT($F339,3)=\"POD\",LEFT($F339,8)=\"Diff POD\"),0,IF(IF(LEFT($F339,5)=\"LVDCI\",$J339+$K339,SUM($I339:$K339))>0,((OFFSET(IO_STANDARDS,$AJ339,6)*IF(AND($I339+$K339>0,OFFSET(IO_STANDARDS,$AJ339,6)<1),100,1)*INT((SUM($I339:$K339)+50)/50))/1000),0))","v":0},{"$f":"IF($L339=\"No\",0,$R339*(IF($L339=\"SERDES\",OFFSET(IODELAY_DATA,3,1),IF($L339=\"DELAY\",OFFSET(IODELAY_DATA,2,1),OFFSET(IODELAY_DATA,4,1)))*$AS339+$CC339*OFFSET(IODELAY_DATA,6,1)+$CD339*OFFSET(IODELAY_DATA,5,1)))","v":0},{"$f":"IF(OR($J339+$K339=0,$AL339<>2),0,OFFSET(IODELAY_DATA,IF($E339=\"HR\",27,26),1)*INT((SUM($I339:$K339)+50)/50)/1000)","v":0},0,0,0,0,0,0,{"$f":"IF(ISERROR($AJ339),0,IF($AP339=VCCO10,$AC339/$AP339,0))","v":0},{"$f":"IF(ISERROR($AJ339),0,IF($AP339=VCCO33,$AG339/$AP339,0))","v":0},{"$f":"IF(ISERROR($AJ339),0,IF($AP339=VCCO25,$AG339/$AP339,0))","v":0},{"$f":"IF(ISERROR($AJ339),0,IF($AP339=VCCO18,$AG339/$AP339,0))","v":0},{"$f":"IF(ISERROR($AJ339),0,IF($AP339=VCCO15,$AG339/$AP339,0))","v":0},{"$f":"IF(ISERROR($AJ339),0,IF($AP339=VCCO135,$AG339/$AP339,0))","v":0},{"$f":"IF(ISERROR($AJ339),0,IF($AP339=VCCO12,$AG339/$AP339,0))","v":0},{"$f":"IF(ISERROR($AJ339),0,IF($AP339=VCCO10,$AG339/$AP339,0))","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ339,24+$BU339)*((1-$W339)*I339+(1-U339)*K339)+(OFFSET(IO_STANDARDS,$AJ339,21+$BU339)*$AK339)*((1-$W339)*I339+(1-U339)*K339*IF($CI339>0,0.93,1))","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ339,25+$BU339)*(I339*(1-W339)+K339*(1-U339))+(OFFSET(IO_STANDARDS,$AJ339,22+$BU339)*(I339*(1-W339)+K339*(1-U339)*IF($CI339>0,0.93,1))*$AK339)","v":0},{"$f":"(IF($AY339=0,OFFSET(IO_STANDARDS,$AJ339,11)*(I339*(1-$V339)+K339*(1-$U339)),0)+OFFSET(IO_STANDARDS,$AJ339,23+$BU339)*(I339*(1-$W339)+K339*(1-$U339))*$AK339)/1000","v":0},{"$f":"IF($E339=\"HR\",22,15)+IF(OFFSET(IO_STANDARDS,$AJ339,5)=0,0,IF(ISERR(FIND(\"pair\",OFFSET(IO_STANDARDS,$AJ339,0))),1,2))+IF(OR(LEFT($F339,3)=\"POD\",LEFT($F339,8)=\"Diff POD\"),2,0)","v":15},0,{"$f":"$AK339*2*OFFSET(FANOUT,3,6)*$AS339","v":0},"BW1",0,{"$f":"IF(TRUE,IF($CE339>0,$CE339*$AP339,OFFSET(IO_STANDARDS,$AJ339,13))/1000,(($AP339-OFFSET(IO_STANDARDS,$AJ339,8))*(ABS($AQ339-OFFSET(IO_STANDARDS,$AJ339,8))/$BX339)+OFFSET(IO_STANDARDS,$AJ339,9)*($AQ339-OFFSET(IO_STANDARDS,$AJ339,9))/$BX339)/2)*IF(AND($Q339=\"Yes\",LEFT($F339,4)=\"LVDS\"),1.25,1)","v":0},0,{"$f":"IF(OR(($I339+$K339)<1,LEFT($F339,3)=\"LVC\",LEFT($F339,3)=\"LVT\"),\"BV2\",IF(OFFSET(IO_STANDARDS,$AJ339,18)>0,\"BV1:BV2\",IF(OR(LEFT($F339,3)=\"HSU\",LEFT($F339,8)=\"Diff HSU\"),\"BW7:BW9\",IF(OR(OFFSET(IO_STANDARDS,$AJ339,19)>0,OFFSET(IO_STANDARDS,$AJ339,20)>0,OR(MID($F339,2,3)=\"STL\",LEFT($F339,9)=\"Diff HSTL\",LEFT($F339,9)=\"Diff SSTL\")),IF(OR(E339=\"HR\",OFFSET(IO_STANDARDS,$AJ339,20)=0),\"BV2:BV5\",\"BV7:BV9\"),\"BV2\"))))","v":"BV2"},0,{"$f":"IF($L339=\"No\",0,$AS339/6)","v":0},0,{"$f":"IF(AND(OFFSET(IO_STANDARDS,$AJ339,13)>0,$AL339<>2),IF($CF339>0,IF(LEFT($F339,4)=\"Diff\",2,1)*1000*($AP339/2)/($CF339+MAX(40,$BX339))/2,0),0)","v":0},0,{"$f":"IF(AND(E339<>\"HR\",OR(LEFT($F339,3)<>\"LVC\",OFFSET(IO_STANDARDS,$AJ339,13)>0),$AL339<>2,($J339+$K339)>0),\"CA3:CA5\",\"CA1\")","v":"CA1"},"CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,{"$f":"IF(ISERROR($AJ340),0,VCCINT_IO/1000*VCCINT_N*(BA340+AV340+BQ340))","v":0},0,{"$f":"$AH340","v":0},0,"None",null,null,0,0,0,139,{"$f":"R340*IF(RIGHT(T340,1)=\"R\",S340*IF(T340=\"DDR\",1,0.5),1)","v":0},1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,{"$f":"IF(LEFT($N340,3)=\"Low\",0,6)","v":0},0,{"$f":"IF(OR($AL340=2),\"BW2\",IF(OR(MID(F340,IF(LEFT($F340,4)=\"Diff\",6,1),4)=\"HSTL\",MID(F340,IF(LEFT($F340,4)=\"Diff\",6,1),4)=\"SSTL\",MID(F340,IF(LEFT($F340,4)=\"Diff\",6,1),3)=\"POD\"),IF(E340=\"HR\",\"BW6\",\"BW3:BW5\"),\"BW1\"))","v":"BW1"},{"$f":" IF(OR(ISTEXT($AD340),$AD340=\"None\"),0,$AD340)","v":0},0,0,"BV2",{"$f":"IF(OR(LEN($O340)<1,RIGHT($O340,4)=\"NONE\",RIGHT($O340,4)=\"None\"),0,IF(LEN($O340)<5,IF(E340=\"HR\",48,40),IF(LEFT($O340,3)=\"DCI\",MID($O340,5,2),IF(LEN($O340)>6,IF(RIGHT($O340,3)=\"240\",240,120),RIGHT($O340,2)))))","v":0},0,{"$f":"IF($L340=\"No\",0,IF($K340>0,$AS340/4,$AS340/6))","v":0},0,{"$f":"IF(OR(LEN($P340)<1,RIGHT($P340,4)=\"NONE\"),IF(RIGHT(INDIRECT(LEFT($CG340,3)),2)=\"40\",40,0),IF(LEFT($P340,3)=\"DCI\",MID($P340,5,2),RIGHT($P340,2)))","v":0},"CA1",{"$f":"IF(OR(LEFT($F340,3)=\"POD\",LEFT($F340,8)=\"Diff POD\",LEFT($F340,4)=\"LVDS\",($J340+$K340)>0),\"CC2:CC3\",\"CC1\")","v":"CC1"},{"$f":"IF(AND(LEFT($F340,3)=\"POD\",$K340>0,$T340=\"DDR\",NOT(ISERROR(SEARCH(\"ddr4_dq<\",$B340,1)))),1,0)","v":0}]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R344*IF(RIGHT(T344,1)=\"R\",S344*IF(T344=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R350*IF(RIGHT(T350,1)=\"R\",S350*IF(T350=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R356*IF(RIGHT(T356,1)=\"R\",S356*IF(T356=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R362*IF(RIGHT(T362,1)=\"R\",S362*IF(T362=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R368*IF(RIGHT(T368,1)=\"R\",S368*IF(T368=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R374*IF(RIGHT(T374,1)=\"R\",S374*IF(T374=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R380*IF(RIGHT(T380,1)=\"R\",S380*IF(T380=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,{"$f":"MATCH($F385,IF($E385=\"HR\",SIOSTD_LIST,VIOSTD_LIST),FALSE)+IF($E385=\"HR\",0,ROW(VIOSTD_LIST)-ROW(SIOSTD_LIST))","v":139},0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,{"$f":"IF(ISERROR($AJ385),0,IF($AP385=VCCO33,$AC385/$AP385+$AZ385,0))","v":0},{"$f":"IF(ISERROR($AJ385),0,IF($AP385=VCCO25,$AC385/$AP385+$AZ385,0))","v":0},{"$f":"IF(ISERROR($AJ385),0,IF($AP385=VCCO18,$AC385/$AP385,0))","v":0},{"$f":"IF(ISERROR($AJ385),0,IF($AP385=VCCO15,$AC385/$AP385,0))","v":0},{"$f":"IF(ISERROR($AJ385),0,IF($AP385=VCCO135,$AC385/$AP385,0))","v":0},{"$f":"IF(ISERROR($AJ385),0,IF($AP385=VCCO12,$AC385/$AP385,0))","v":0},0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R386*IF(RIGHT(T386,1)=\"R\",S386*IF(T386=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R392*IF(RIGHT(T392,1)=\"R\",S392*IF(T392=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R398*IF(RIGHT(T398,1)=\"R\",S398*IF(T398=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,{"$f":"$V403","v":0},0,0,0,{"$f":"IF(ISERROR($AJ403),0,MAX(0,($AU403+$AW403+$BR403)*VCCAUX_IO/1000))","v":0},0,{"$f":"IF(ISERROR($AJ403),0,MAX(0,OFFSET($AL403,0,$AL403)+(($J403*IF(AND($AL403<>2,LEFT($F403,2)<>\"LV\",RIGHT(T403,1)=\"R\"),S403+(1-S403)/2,1)+K403*IF(AND($AL403<>2,LEFT($F403,2)<>\"LV\",RIGHT(T403,1)=\"R\"),S403,1))*$U403)*$BY403+$I403*OFFSET(IO_STANDARDS,$AJ403,14)/1000+($AY403+$BS403)*$AP403))","v":0},"None",null,null,{"$f":"IF(ISERROR($AJ403),0,IF(AD403=\"None\",0,$BZ403*(($J403+K403)*$U403)))","v":0},{"$f":"IF(ISERROR($AJ403),0,VCCINT/1000*VCCINT_N*(IF($L403=\"No\",0,$R403*$AS403*OFFSET(IODELAY_DATA,9,3))+BV403))","v":0},{"$f":"IF(ISERROR($AJ403),0,VCCINT_IO/1000*VCCINT_N*(BA403))","v":0},139,0,{"$f":"IF(AND($K403>0,$E403=\"HR\",OFFSET(IO_STANDARDS,$AJ403,19)>0),3,OFFSET(IO_STANDARDS,$AJ403,2))","v":1},{"$f":"(OFFSET(IO_STANDARDS,$AJ403,35)*($X403+OFFSET(IO_STANDARDS,$AJ403,3))*($J403+$K403*IF($CI403>0,0.93,1))*$AP403*$AK403*$U403*$AT$1)/1000","v":0},{"$f":"MAX(0,(OFFSET(IO_STANDARDS,$AJ403,35)*($X403+OFFSET(IO_STANDARDS,$AJ403,3))*($J403+$K403)*$AP403*$AK403*$U403*$AT$1/1000))","v":0},{"$f":"(((OFFSET(IO_STANDARDS,$AJ403,35)*($X403+OFFSET(IO_STANDARDS,$AJ403,3))*$AP403/1000)*($J403+$K403*IF($CI403>0,0.93,1))*$AK403*$U403*$AT$1))","v":0},{"$f":"IF(ISERROR($AJ403),0,OFFSET(IO_STANDARDS,$AJ403,1))","v":1.8},{"$f":"IF(OFFSET(IO_STANDARDS,$AJ403,9)=0,0,IF(OR(LEFT($F403,14)=\"HSTL Class III\",LEFT($F403,13)=\"HSTL Class IV\",LEFT($F403,3)=\"GTL\",LEFT($F403,3)=\"POD\",LEFT($F403,8)=\"Diff POD\"),$AP403,$AP403/2))","v":0},{"$f":"IF(OFFSET(IO_STANDARDS,$AJ403,10)=0,$AP403,$AP403/2)","v":1.8},{"$f":"IF(RIGHT($F403,6) =\"(pair)\",2,1)*SUM(I403:K403)","v":0},{"$f":"IF($M403=\"Off\",0,$AK403*OFFSET(IODELAY_DATA,2,3)*$AS403)","v":0},{"$f":"0","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ403,33)*$AK403*$U403*($J403+$K403)*IF(AND($Q403=\"Yes\",OR(LEFT($F403,3)=\"POD\",LEFT($F403,8)=\"Diff POD\",LEFT($F403,4)=\"LVDS\")),2,1)*IF($CI403>0,0.93,1)+OFFSET(IO_STANDARDS,$AJ403,36)*$U403*($J403+$K403)","v":0},{"$f":"(OFFSET(IO_STANDARDS,$AJ403,34)*IF($CF403>0,40/$CF403,1)*$AK403*$U403*IF($Q403=\"Yes\",IF(OR(LEFT($F403,3)=\"POD\",LEFT($F403,8)=\"Diff POD\"),1.17,IF(LEFT($F403,4)=\"LVDS\",2,1)),1)*IF($CI403>0,0.93,1)*$AT$1+OFFSET(IO_STANDARDS,$AJ403,37)*$U403*$AT$1)*($J403+$K403)","v":0},{"$f":"((($I403*(1-$W403)+$K403*(1-$U403))*OFFSET(IO_STANDARDS,$AJ403,11)) + ((($J403+$K403)*$U403)*OFFSET(IO_STANDARDS,$AJ403,10)))/1000  + $AZ403","v":0},{"$f":"IF($CB403>0,IF(LEFT($F403,4)=\"Diff\",2,1)*($I403+$K403*(1-$U403))*IF(AND($AL403=2,$O403=\"DIFF_TERM\"),OFFSET(IO_STANDARDS,$AJ403,18),IF($E403<>\"HR\",IF($CB403>0,1,0)*IF(AL403<>2,IF(OR(LEFT($F403,3)=\"POD\",LEFT($F403,8)=\"Diff POD\"),0.5*1000*$AP403/($CB403+40)*IF($CI403>0,0.36/0.5,1),$AQ403*500/$CB403),OFFSET(IO_STANDARDS,$AJ403,11)),IF(LEFT($O403,3)=\"RTT\",$AQ403*500/$CB403,0))*(1-$V403))/1000,0)","v":0},{"$f":"IF(OR(LEFT($F403,3)=\"POD\",LEFT($F403,8)=\"Diff POD\"),0,IF(IF(LEFT($F403,5)=\"LVDCI\",$J403+$K403,SUM($I403:$K403))>0,((OFFSET(IO_STANDARDS,$AJ403,6)*IF(AND($I403+$K403>0,OFFSET(IO_STANDARDS,$AJ403,6)<1),100,1)*INT((SUM($I403:$K403)+50)/50))/1000),0))","v":0},{"$f":"IF($L403=\"No\",0,$R403*(IF($L403=\"SERDES\",OFFSET(IODELAY_DATA,3,1),IF($L403=\"DELAY\",OFFSET(IODELAY_DATA,2,1),OFFSET(IODELAY_DATA,4,1)))*$AS403+$CC403*OFFSET(IODELAY_DATA,6,1)+$CD403*OFFSET(IODELAY_DATA,5,1)))","v":0},{"$f":"IF(OR($J403+$K403=0,$AL403<>2),0,OFFSET(IODELAY_DATA,IF($E403=\"HR\",27,26),1)*INT((SUM($I403:$K403)+50)/50)/1000)","v":0},0,0,0,0,0,0,{"$f":"IF(ISERROR($AJ403),0,IF($AP403=VCCO10,$AC403/$AP403,0))","v":0},{"$f":"IF(ISERROR($AJ403),0,IF($AP403=VCCO33,$AG403/$AP403,0))","v":0},{"$f":"IF(ISERROR($AJ403),0,IF($AP403=VCCO25,$AG403/$AP403,0))","v":0},{"$f":"IF(ISERROR($AJ403),0,IF($AP403=VCCO18,$AG403/$AP403,0))","v":0},{"$f":"IF(ISERROR($AJ403),0,IF($AP403=VCCO15,$AG403/$AP403,0))","v":0},{"$f":"IF(ISERROR($AJ403),0,IF($AP403=VCCO135,$AG403/$AP403,0))","v":0},{"$f":"IF(ISERROR($AJ403),0,IF($AP403=VCCO12,$AG403/$AP403,0))","v":0},{"$f":"IF(ISERROR($AJ403),0,IF($AP403=VCCO10,$AG403/$AP403,0))","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ403,24+$BU403)*((1-$W403)*I403+(1-U403)*K403)+(OFFSET(IO_STANDARDS,$AJ403,21+$BU403)*$AK403)*((1-$W403)*I403+(1-U403)*K403*IF($CI403>0,0.93,1))","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ403,25+$BU403)*(I403*(1-W403)+K403*(1-U403))+(OFFSET(IO_STANDARDS,$AJ403,22+$BU403)*(I403*(1-W403)+K403*(1-U403)*IF($CI403>0,0.93,1))*$AK403)","v":0},{"$f":"(IF($AY403=0,OFFSET(IO_STANDARDS,$AJ403,11)*(I403*(1-$V403)+K403*(1-$U403)),0)+OFFSET(IO_STANDARDS,$AJ403,23+$BU403)*(I403*(1-$W403)+K403*(1-$U403))*$AK403)/1000","v":0},{"$f":"IF($E403=\"HR\",22,15)+IF(OFFSET(IO_STANDARDS,$AJ403,5)=0,0,IF(ISERR(FIND(\"pair\",OFFSET(IO_STANDARDS,$AJ403,0))),1,2))+IF(OR(LEFT($F403,3)=\"POD\",LEFT($F403,8)=\"Diff POD\"),2,0)","v":15},0,{"$f":"$AK403*2*OFFSET(FANOUT,3,6)*$AS403","v":0},"BW1",0,{"$f":"IF(TRUE,IF($CE403>0,$CE403*$AP403,OFFSET(IO_STANDARDS,$AJ403,13))/1000,(($AP403-OFFSET(IO_STANDARDS,$AJ403,8))*(ABS($AQ403-OFFSET(IO_STANDARDS,$AJ403,8))/$BX403)+OFFSET(IO_STANDARDS,$AJ403,9)*($AQ403-OFFSET(IO_STANDARDS,$AJ403,9))/$BX403)/2)*IF(AND($Q403=\"Yes\",LEFT($F403,4)=\"LVDS\"),1.25,1)","v":0},0,{"$f":"IF(OR(($I403+$K403)<1,LEFT($F403,3)=\"LVC\",LEFT($F403,3)=\"LVT\"),\"BV2\",IF(OFFSET(IO_STANDARDS,$AJ403,18)>0,\"BV1:BV2\",IF(OR(LEFT($F403,3)=\"HSU\",LEFT($F403,8)=\"Diff HSU\"),\"BW7:BW9\",IF(OR(OFFSET(IO_STANDARDS,$AJ403,19)>0,OFFSET(IO_STANDARDS,$AJ403,20)>0,OR(MID($F403,2,3)=\"STL\",LEFT($F403,9)=\"Diff HSTL\",LEFT($F403,9)=\"Diff SSTL\")),IF(OR(E403=\"HR\",OFFSET(IO_STANDARDS,$AJ403,20)=0),\"BV2:BV5\",\"BV7:BV9\"),\"BV2\"))))","v":"BV2"},0,{"$f":"IF($L403=\"No\",0,$AS403/6)","v":0},0,{"$f":"IF(AND(OFFSET(IO_STANDARDS,$AJ403,13)>0,$AL403<>2),IF($CF403>0,IF(LEFT($F403,4)=\"Diff\",2,1)*1000*($AP403/2)/($CF403+MAX(40,$BX403))/2,0),0)","v":0},0,{"$f":"IF(AND(E403<>\"HR\",OR(LEFT($F403,3)<>\"LVC\",OFFSET(IO_STANDARDS,$AJ403,13)>0),$AL403<>2,($J403+$K403)>0),\"CA3:CA5\",\"CA1\")","v":"CA1"},"CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R404*IF(RIGHT(T404,1)=\"R\",S404*IF(T404=\"DDR\",2,1),2)","v":0},{"$f":"IF(ISERROR($AJ404),0,VCCINT_IO/1000*VCCINT_N*(BA404+AV404+BQ404))","v":0},0,{"$f":"$AH404","v":0},0,"None",null,null,0,0,0,139,{"$f":"R404*IF(RIGHT(T404,1)=\"R\",S404*IF(T404=\"DDR\",1,0.5),1)","v":0},1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,{"$f":"IF(LEFT($N404,3)=\"Low\",0,6)","v":0},0,{"$f":"IF(OR($AL404=2),\"BW2\",IF(OR(MID(F404,IF(LEFT($F404,4)=\"Diff\",6,1),4)=\"HSTL\",MID(F404,IF(LEFT($F404,4)=\"Diff\",6,1),4)=\"SSTL\",MID(F404,IF(LEFT($F404,4)=\"Diff\",6,1),3)=\"POD\"),IF(E404=\"HR\",\"BW6\",\"BW3:BW5\"),\"BW1\"))","v":"BW1"},{"$f":" IF(OR(ISTEXT($AD404),$AD404=\"None\"),0,$AD404)","v":0},0,0,"BV2",{"$f":"IF(OR(LEN($O404)<1,RIGHT($O404,4)=\"NONE\",RIGHT($O404,4)=\"None\"),0,IF(LEN($O404)<5,IF(E404=\"HR\",48,40),IF(LEFT($O404,3)=\"DCI\",MID($O404,5,2),IF(LEN($O404)>6,IF(RIGHT($O404,3)=\"240\",240,120),RIGHT($O404,2)))))","v":0},0,{"$f":"IF($L404=\"No\",0,IF($K404>0,$AS404/4,$AS404/6))","v":0},0,{"$f":"IF(OR(LEN($P404)<1,RIGHT($P404,4)=\"NONE\"),IF(RIGHT(INDIRECT(LEFT($CG404,3)),2)=\"40\",40,0),IF(LEFT($P404,3)=\"DCI\",MID($P404,5,2),RIGHT($P404,2)))","v":0},"CA1",{"$f":"IF(OR(LEFT($F404,3)=\"POD\",LEFT($F404,8)=\"Diff POD\",LEFT($F404,4)=\"LVDS\",($J404+$K404)>0),\"CC2:CC3\",\"CC1\")","v":"CC1"},{"$f":"IF(AND(LEFT($F404,3)=\"POD\",$K404>0,$T404=\"DDR\",NOT(ISERROR(SEARCH(\"ddr4_dq<\",$B404,1)))),1,0)","v":0}]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R410*IF(RIGHT(T410,1)=\"R\",S410*IF(T410=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R416*IF(RIGHT(T416,1)=\"R\",S416*IF(T416=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R422*IF(RIGHT(T422,1)=\"R\",S422*IF(T422=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R428*IF(RIGHT(T428,1)=\"R\",S428*IF(T428=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R434*IF(RIGHT(T434,1)=\"R\",S434*IF(T434=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R440*IF(RIGHT(T440,1)=\"R\",S440*IF(T440=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R446*IF(RIGHT(T446,1)=\"R\",S446*IF(T446=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,{"$f":"MATCH($F449,IF($E449=\"HR\",SIOSTD_LIST,VIOSTD_LIST),FALSE)+IF($E449=\"HR\",0,ROW(VIOSTD_LIST)-ROW(SIOSTD_LIST))","v":139},0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,{"$f":"IF(ISERROR($AJ449),0,IF($AP449=VCCO33,$AC449/$AP449+$AZ449,0))","v":0},{"$f":"IF(ISERROR($AJ449),0,IF($AP449=VCCO25,$AC449/$AP449+$AZ449,0))","v":0},{"$f":"IF(ISERROR($AJ449),0,IF($AP449=VCCO18,$AC449/$AP449,0))","v":0},{"$f":"IF(ISERROR($AJ449),0,IF($AP449=VCCO15,$AC449/$AP449,0))","v":0},{"$f":"IF(ISERROR($AJ449),0,IF($AP449=VCCO135,$AC449/$AP449,0))","v":0},{"$f":"IF(ISERROR($AJ449),0,IF($AP449=VCCO12,$AC449/$AP449,0))","v":0},0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R452*IF(RIGHT(T452,1)=\"R\",S452*IF(T452=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R458*IF(RIGHT(T458,1)=\"R\",S458*IF(T458=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R464*IF(RIGHT(T464,1)=\"R\",S464*IF(T464=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,{"$f":"$V467","v":0},0,0,0,{"$f":"IF(ISERROR($AJ467),0,MAX(0,($AU467+$AW467+$BR467)*VCCAUX_IO/1000))","v":0},0,{"$f":"IF(ISERROR($AJ467),0,MAX(0,OFFSET($AL467,0,$AL467)+(($J467*IF(AND($AL467<>2,LEFT($F467,2)<>\"LV\",RIGHT(T467,1)=\"R\"),S467+(1-S467)/2,1)+K467*IF(AND($AL467<>2,LEFT($F467,2)<>\"LV\",RIGHT(T467,1)=\"R\"),S467,1))*$U467)*$BY467+$I467*OFFSET(IO_STANDARDS,$AJ467,14)/1000+($AY467+$BS467)*$AP467))","v":0},"None",null,null,{"$f":"IF(ISERROR($AJ467),0,IF(AD467=\"None\",0,$BZ467*(($J467+K467)*$U467)))","v":0},{"$f":"IF(ISERROR($AJ467),0,VCCINT/1000*VCCINT_N*(IF($L467=\"No\",0,$R467*$AS467*OFFSET(IODELAY_DATA,9,3))+BV467))","v":0},{"$f":"IF(ISERROR($AJ467),0,VCCINT_IO/1000*VCCINT_N*(BA467))","v":0},139,0,{"$f":"IF(AND($K467>0,$E467=\"HR\",OFFSET(IO_STANDARDS,$AJ467,19)>0),3,OFFSET(IO_STANDARDS,$AJ467,2))","v":1},{"$f":"(OFFSET(IO_STANDARDS,$AJ467,35)*($X467+OFFSET(IO_STANDARDS,$AJ467,3))*($J467+$K467*IF($CI467>0,0.93,1))*$AP467*$AK467*$U467*$AT$1)/1000","v":0},{"$f":"MAX(0,(OFFSET(IO_STANDARDS,$AJ467,35)*($X467+OFFSET(IO_STANDARDS,$AJ467,3))*($J467+$K467)*$AP467*$AK467*$U467*$AT$1/1000))","v":0},{"$f":"(((OFFSET(IO_STANDARDS,$AJ467,35)*($X467+OFFSET(IO_STANDARDS,$AJ467,3))*$AP467/1000)*($J467+$K467*IF($CI467>0,0.93,1))*$AK467*$U467*$AT$1))","v":0},{"$f":"IF(ISERROR($AJ467),0,OFFSET(IO_STANDARDS,$AJ467,1))","v":1.8},{"$f":"IF(OFFSET(IO_STANDARDS,$AJ467,9)=0,0,IF(OR(LEFT($F467,14)=\"HSTL Class III\",LEFT($F467,13)=\"HSTL Class IV\",LEFT($F467,3)=\"GTL\",LEFT($F467,3)=\"POD\",LEFT($F467,8)=\"Diff POD\"),$AP467,$AP467/2))","v":0},{"$f":"IF(OFFSET(IO_STANDARDS,$AJ467,10)=0,$AP467,$AP467/2)","v":1.8},{"$f":"IF(RIGHT($F467,6) =\"(pair)\",2,1)*SUM(I467:K467)","v":0},{"$f":"IF($M467=\"Off\",0,$AK467*OFFSET(IODELAY_DATA,2,3)*$AS467)","v":0},{"$f":"0","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ467,33)*$AK467*$U467*($J467+$K467)*IF(AND($Q467=\"Yes\",OR(LEFT($F467,3)=\"POD\",LEFT($F467,8)=\"Diff POD\",LEFT($F467,4)=\"LVDS\")),2,1)*IF($CI467>0,0.93,1)+OFFSET(IO_STANDARDS,$AJ467,36)*$U467*($J467+$K467)","v":0},{"$f":"(OFFSET(IO_STANDARDS,$AJ467,34)*IF($CF467>0,40/$CF467,1)*$AK467*$U467*IF($Q467=\"Yes\",IF(OR(LEFT($F467,3)=\"POD\",LEFT($F467,8)=\"Diff POD\"),1.17,IF(LEFT($F467,4)=\"LVDS\",2,1)),1)*IF($CI467>0,0.93,1)*$AT$1+OFFSET(IO_STANDARDS,$AJ467,37)*$U467*$AT$1)*($J467+$K467)","v":0},{"$f":"((($I467*(1-$W467)+$K467*(1-$U467))*OFFSET(IO_STANDARDS,$AJ467,11)) + ((($J467+$K467)*$U467)*OFFSET(IO_STANDARDS,$AJ467,10)))/1000  + $AZ467","v":0},{"$f":"IF($CB467>0,IF(LEFT($F467,4)=\"Diff\",2,1)*($I467+$K467*(1-$U467))*IF(AND($AL467=2,$O467=\"DIFF_TERM\"),OFFSET(IO_STANDARDS,$AJ467,18),IF($E467<>\"HR\",IF($CB467>0,1,0)*IF(AL467<>2,IF(OR(LEFT($F467,3)=\"POD\",LEFT($F467,8)=\"Diff POD\"),0.5*1000*$AP467/($CB467+40)*IF($CI467>0,0.36/0.5,1),$AQ467*500/$CB467),OFFSET(IO_STANDARDS,$AJ467,11)),IF(LEFT($O467,3)=\"RTT\",$AQ467*500/$CB467,0))*(1-$V467))/1000,0)","v":0},{"$f":"IF(OR(LEFT($F467,3)=\"POD\",LEFT($F467,8)=\"Diff POD\"),0,IF(IF(LEFT($F467,5)=\"LVDCI\",$J467+$K467,SUM($I467:$K467))>0,((OFFSET(IO_STANDARDS,$AJ467,6)*IF(AND($I467+$K467>0,OFFSET(IO_STANDARDS,$AJ467,6)<1),100,1)*INT((SUM($I467:$K467)+50)/50))/1000),0))","v":0},{"$f":"IF($L467=\"No\",0,$R467*(IF($L467=\"SERDES\",OFFSET(IODELAY_DATA,3,1),IF($L467=\"DELAY\",OFFSET(IODELAY_DATA,2,1),OFFSET(IODELAY_DATA,4,1)))*$AS467+$CC467*OFFSET(IODELAY_DATA,6,1)+$CD467*OFFSET(IODELAY_DATA,5,1)))","v":0},{"$f":"IF(OR($J467+$K467=0,$AL467<>2),0,OFFSET(IODELAY_DATA,IF($E467=\"HR\",27,26),1)*INT((SUM($I467:$K467)+50)/50)/1000)","v":0},0,0,0,0,0,0,{"$f":"IF(ISERROR($AJ467),0,IF($AP467=VCCO10,$AC467/$AP467,0))","v":0},{"$f":"IF(ISERROR($AJ467),0,IF($AP467=VCCO33,$AG467/$AP467,0))","v":0},{"$f":"IF(ISERROR($AJ467),0,IF($AP467=VCCO25,$AG467/$AP467,0))","v":0},{"$f":"IF(ISERROR($AJ467),0,IF($AP467=VCCO18,$AG467/$AP467,0))","v":0},{"$f":"IF(ISERROR($AJ467),0,IF($AP467=VCCO15,$AG467/$AP467,0))","v":0},{"$f":"IF(ISERROR($AJ467),0,IF($AP467=VCCO135,$AG467/$AP467,0))","v":0},{"$f":"IF(ISERROR($AJ467),0,IF($AP467=VCCO12,$AG467/$AP467,0))","v":0},{"$f":"IF(ISERROR($AJ467),0,IF($AP467=VCCO10,$AG467/$AP467,0))","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ467,24+$BU467)*((1-$W467)*I467+(1-U467)*K467)+(OFFSET(IO_STANDARDS,$AJ467,21+$BU467)*$AK467)*((1-$W467)*I467+(1-U467)*K467*IF($CI467>0,0.93,1))","v":0},{"$f":"OFFSET(IO_STANDARDS,$AJ467,25+$BU467)*(I467*(1-W467)+K467*(1-U467))+(OFFSET(IO_STANDARDS,$AJ467,22+$BU467)*(I467*(1-W467)+K467*(1-U467)*IF($CI467>0,0.93,1))*$AK467)","v":0},{"$f":"(IF($AY467=0,OFFSET(IO_STANDARDS,$AJ467,11)*(I467*(1-$V467)+K467*(1-$U467)),0)+OFFSET(IO_STANDARDS,$AJ467,23+$BU467)*(I467*(1-$W467)+K467*(1-$U467))*$AK467)/1000","v":0},{"$f":"IF($E467=\"HR\",22,15)+IF(OFFSET(IO_STANDARDS,$AJ467,5)=0,0,IF(ISERR(FIND(\"pair\",OFFSET(IO_STANDARDS,$AJ467,0))),1,2))+IF(OR(LEFT($F467,3)=\"POD\",LEFT($F467,8)=\"Diff POD\"),2,0)","v":15},0,{"$f":"$AK467*2*OFFSET(FANOUT,3,6)*$AS467","v":0},"BW1",0,{"$f":"IF(TRUE,IF($CE467>0,$CE467*$AP467,OFFSET(IO_STANDARDS,$AJ467,13))/1000,(($AP467-OFFSET(IO_STANDARDS,$AJ467,8))*(ABS($AQ467-OFFSET(IO_STANDARDS,$AJ467,8))/$BX467)+OFFSET(IO_STANDARDS,$AJ467,9)*($AQ467-OFFSET(IO_STANDARDS,$AJ467,9))/$BX467)/2)*IF(AND($Q467=\"Yes\",LEFT($F467,4)=\"LVDS\"),1.25,1)","v":0},0,{"$f":"IF(OR(($I467+$K467)<1,LEFT($F467,3)=\"LVC\",LEFT($F467,3)=\"LVT\"),\"BV2\",IF(OFFSET(IO_STANDARDS,$AJ467,18)>0,\"BV1:BV2\",IF(OR(LEFT($F467,3)=\"HSU\",LEFT($F467,8)=\"Diff HSU\"),\"BW7:BW9\",IF(OR(OFFSET(IO_STANDARDS,$AJ467,19)>0,OFFSET(IO_STANDARDS,$AJ467,20)>0,OR(MID($F467,2,3)=\"STL\",LEFT($F467,9)=\"Diff HSTL\",LEFT($F467,9)=\"Diff SSTL\")),IF(OR(E467=\"HR\",OFFSET(IO_STANDARDS,$AJ467,20)=0),\"BV2:BV5\",\"BV7:BV9\"),\"BV2\"))))","v":"BV2"},0,{"$f":"IF($L467=\"No\",0,$AS467/6)","v":0},0,{"$f":"IF(AND(OFFSET(IO_STANDARDS,$AJ467,13)>0,$AL467<>2),IF($CF467>0,IF(LEFT($F467,4)=\"Diff\",2,1)*1000*($AP467/2)/($CF467+MAX(40,$BX467))/2,0),0)","v":0},0,{"$f":"IF(AND(E467<>\"HR\",OR(LEFT($F467,3)<>\"LVC\",OFFSET(IO_STANDARDS,$AJ467,13)>0),$AL467<>2,($J467+$K467)>0),\"CA3:CA5\",\"CA1\")","v":"CA1"},"CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,{"$f":"IF(ISERROR($AJ468),0,VCCINT_IO/1000*VCCINT_N*(BA468+AV468+BQ468))","v":0},0,{"$f":"$AH468","v":0},0,"None",null,null,0,0,0,139,{"$f":"R468*IF(RIGHT(T468,1)=\"R\",S468*IF(T468=\"DDR\",1,0.5),1)","v":0},1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,{"$f":"IF(LEFT($N468,3)=\"Low\",0,6)","v":0},0,{"$f":"IF(OR($AL468=2),\"BW2\",IF(OR(MID(F468,IF(LEFT($F468,4)=\"Diff\",6,1),4)=\"HSTL\",MID(F468,IF(LEFT($F468,4)=\"Diff\",6,1),4)=\"SSTL\",MID(F468,IF(LEFT($F468,4)=\"Diff\",6,1),3)=\"POD\"),IF(E468=\"HR\",\"BW6\",\"BW3:BW5\"),\"BW1\"))","v":"BW1"},{"$f":" IF(OR(ISTEXT($AD468),$AD468=\"None\"),0,$AD468)","v":0},0,0,"BV2",{"$f":"IF(OR(LEN($O468)<1,RIGHT($O468,4)=\"NONE\",RIGHT($O468,4)=\"None\"),0,IF(LEN($O468)<5,IF(E468=\"HR\",48,40),IF(LEFT($O468,3)=\"DCI\",MID($O468,5,2),IF(LEN($O468)>6,IF(RIGHT($O468,3)=\"240\",240,120),RIGHT($O468,2)))))","v":0},0,{"$f":"IF($L468=\"No\",0,IF($K468>0,$AS468/4,$AS468/6))","v":0},0,{"$f":"IF(OR(LEN($P468)<1,RIGHT($P468,4)=\"NONE\"),IF(RIGHT(INDIRECT(LEFT($CG468,3)),2)=\"40\",40,0),IF(LEFT($P468,3)=\"DCI\",MID($P468,5,2),RIGHT($P468,2)))","v":0},"CA1",{"$f":"IF(OR(LEFT($F468,3)=\"POD\",LEFT($F468,8)=\"Diff POD\",LEFT($F468,4)=\"LVDS\",($J468+$K468)>0),\"CC2:CC3\",\"CC1\")","v":"CC1"},{"$f":"IF(AND(LEFT($F468,3)=\"POD\",$K468>0,$T468=\"DDR\",NOT(ISERROR(SEARCH(\"ddr4_dq<\",$B468,1)))),1,0)","v":0}]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R470*IF(RIGHT(T470,1)=\"R\",S470*IF(T470=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R476*IF(RIGHT(T476,1)=\"R\",S476*IF(T476=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R482*IF(RIGHT(T482,1)=\"R\",S482*IF(T482=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R488*IF(RIGHT(T488,1)=\"R\",S488*IF(T488=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R494*IF(RIGHT(T494,1)=\"R\",S494*IF(T494=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,0,0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,null,null,null,"HP","LVCMOS 1.8V 12mA (Slow)",null,null,null,null,null,"No","Off","Low Power",null,null,null,null,0.125,"SDR",1,0,0,0,{"$f":"R500*IF(RIGHT(T500,1)=\"R\",S500*IF(T500=\"DDR\",2,1),2)","v":0},0,0,0,0,"None",null,null,0,0,0,139,0,1,0,0,0,1.8,0,1.8,0,0,{"$f":"0","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,0,0,"BW1",0,0,0,"BV2",0,0,0,0,0,"CA1","CC1",0]
[null,{"$f":"ROW(IOROWS)-19","v":482},null,null,null,null,"Package Pins",null,{"$f":"SUM(IF(\"(pair)\"=RIGHT($F19:$F500,6),I19:I500*2,I19:I500))","v":222},{"$f":"SUM(IF(\"(pair)\"=RIGHT($F19:$F500,6),J19:J500*2,J19:J500))","v":222},{"$f":"SUM(IF(\"(pair)\"=RIGHT($F19:$F500,6),K19:K500*2,K19:K500))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(SUM(Z19:Z500))*OFFSET(POWER_SCALE,7,1)*PL_POWERED","v":0.62709440543021833},{"$f":"(SUM(AA19:AB500)+(DELAYCTRL*OFFSET(IODELAY_DATA,6,4)+INTERNALVREF*OFFSET(IODELAY_DATA,8,1))*VCCAUX/1000)*OFFSET(POWER_SCALE,8,1)*PL_POWERED","v":0.73542256189181265},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pins",{"$f":"SUM(IF(AP19:AP500=VCCO33,I19:K500))","v":0},{"$f":"SUM(IF(AP19:AP500=VCCO25,I19:K500))","v":0},{"$f":"SUM(IF(AP19:AP500=VCCO18,I19:K500))","v":252},{"$f":"SUM(IF(AP19:AP500=VCCO15,I19:K500))","v":0},{"$f":"SUM(IF(AP19:AP500=VCCO135,I19:K500))","v":0},{"$f":"SUM(IF(AP19:AP500=VCCO12,I19:K500))","v":0},{"$f":"SUM(IF(AP19:AP500=VCCO10,I19:K500))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(LEFT($F501,3)=\"POD\",$K501>0,$T501=\"DDR\",LEFT($B501,8)=\"ddr4_dq<\"),1,0)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Banks",{"$f":"IF(AND(BA501=0,LEFT(CFG_BANK,1)<>\"3\"),0,MAX(1,INT((BA501+49)/50)))","v":0},{"$f":"IF(AND(BB501=0,LEFT(CFG_BANK,1)<>\"2\"),0,MAX(1,INT((BB501+49)/50)))","v":0},{"$f":"IF(AND(BC501=0,LEFT(CFG_BANK,1)<>\"1\"),0,MAX(1,INT((BC501+49)/50)))","v":6},{"$f":"IF(BD501=0,0,MAX(1,INT((BD501+49)/50)))","v":0},{"$f":"IF(BE501=0,0,MAX(1,INT((BE501+49)/50)))","v":0},0,{"$f":"IF(BG501=0,0,MAX(1,INT((BG501+49)/50)))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Errors",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3.3V",{"$f":"SUM(IF(3.3=$AP19:$AP500,I19:K500,0))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(OFFSET(IO_STANDARDS,$AI504,13)>0,$AE504<>2),\"CA2:CA5\",\"CA1\")","v":"CA2:CA5"},null,null,0]
[]
[]
[]
[null,null,null,{"$f":"IF(ISERROR(IO_POWER),\"ERROR: Unsupported I/O standard(s) for target device\",\"\")","v":""},null,null,null,null,null,null,null,null,null,"Output Termination Topologies",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5V",{"$f":"SUM(IF(2.5=$AP19:$AP500,I19:K500,0))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Single Ended",null,"On-Chip",null,null,null,null,"Off-Chip",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1.8V",{"$f":"SUM(IF(1.8=$AP19:$AP500,I19:K500,0))","v":252}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1.5V",{"$f":"SUM(IF(1.5=$AP19:$AP500,I19:K500,0))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1.35V",{"$f":"SUM(IF(1.35=$AP19:$AP500,I19:K500,0))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1.2V",{"$f":"SUM(IF(1.2=$AP19:$AP500,J19:L500,0))","v":0}]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Series",null,null,null,null,"Parallel (Vtt)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Split-Thevenin"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Differential",null,"N/A"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Notes:"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"* On-chip terminations are shown for completeness."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pseudo-differential terminations are not supported in this version"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"* More details on I/O terminations are available in the device family \"SelectIO Resources User Guide\"...:"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(IF(ISERROR(AJ19:AJ500),1,0))","v":0}]

{"sheet":"BRAM","index":7,"n_rows":502,"n_cols":44,"rows_kept":502,"cut":false,"hidden":false,"merged":[[4,13,4,15],[118,1,118,3],[119,1,119,3],[496,1,496,3],[109,1,109,3],[110,1,110,3],[111,1,111,3],[112,1,112,3],[113,1,113,3],[114,1,114,3],[115,1,115,3],[116,1,116,3],[117,1,117,3],[300,1,300,3],[301,1,301,3],[302,1,302,3],[303,1,303,3],[304,1,304,3],[305,1,305,3],[306,1,306,3],[307,1,307,3],[308,1,308,3],[291,1,291,3],[292,1,292,3],[273,1,273,3],[274,1,274,3],[275,1,275,3],[276,1,276,3],[277,1,277,3],[278,1,278,3],[279,1,279,3],[280,1,280,3],[281,1,281,3],[100,1,100,3],[101,1,101,3],[102,1,102,3],[103,1,103,3],[104,1,104,3],[105,1,105,3],[106,1,106,3],[107,1,107,3],[108,1,108,3],[91,1,91,3],[92,1,92,3],[93,1,93,3],[94,1,94,3],[95,1,95,3],[96,1,96,3],[97,1,97,3],[98,1,98,3],[99,1,99,3],[82,1,82,3],[83,1,83,3],[84,1,84,3],[85,1,85,3],[86,1,86,3],[87,1,87,3],[88,1,88,3],[89,1,89,3],[90,1,90,3],[73,1,73,3],[74,1,74,3],[75,1,75,3],[76,1,76,3],[77,1,77,3],[78,1,78,3],[79,1,79,3],[80,1,80,3],[81,1,81,3],[64,1,64,3],[65,1,65,3],[66,1,66,3],[67,1,67,3],[68,1,68,3],[69,1,69,3],[70,1,70,3],[71,1,71,3],[72,1,72,3],[55,1,55,3],[56,1,56,3],[57,1,57,3],[58,1,58,3],[59,1,59,3],[60,1,60,3],[61,1,61,3],[62,1,62,3],[63,1,63,3],[46,1,46,3],[47,1,47,3],[48,1,48,3],[49,1,49,3],[50,1,50,3],[51,1,51,3],[52,1,52,3],[53,1,53,3],[54,1,54,3],[37,1,37,3],[38,1,38,3],[39,1,39,3],[40,1,40,3],[41,1,41,3],[42,1,42,3],[43,1,43,3],[44,1,44,3],[45,1,45,3],[28,1,28,3],[29,1,29,3],[30,1,30,3],[31,1,31,3],[32,1,32,3],[33,1,33,3],[34,1,34,3],[35,1,35,3],[36,1,36,3],[19,1,19,3],[20,1,20,3],[21,1,21,3],[22,1,22,3],[23,1,23,3],[24,1,24,3],[25,1,25,3],[26,1,26,3],[27,1,27,3],[10,1,10,3],[11,1,11,3],[12,1,12,3],[13,1,13,3],[14,1,14,3],[15,1,15,3],[16,1,16,3],[17,1,17,3],[18,1,18,3],[294,1,294,3],[295,1,295,3],[296,1,296,3],[297,1,297,3],[298,1,298,3],[299,1,299,3],[282,1,282,3],[283,1,283,3],[284,1,284,3],[285,1,285,3],[286,1,286,3],[287,1,287,3],[288,1,288,3],[289,1,289,3],[290,1,290,3],[293,1,293,3],[269,1,269,3],[270,1,270,3],[271,1,271,3],[272,1,272,3],[255,1,255,3],[256,1,256,3],[257,1,257,3],[258,1,258,3],[259,1,259,3],[260,1,260,3],[261,1,261,3],[262,1,262,3],[263,1,263,3],[264,1,264,3],[265,1,265,3],[266,1,266,3],[267,1,267,3],[268,1,268,3],[246,1,246,3],[247,1,247,3],[248,1,248,3],[249,1,249,3],[250,1,250,3],[251,1,251,3],[252,1,252,3],[253,1,253,3],[254,1,254,3],[237,1,237,3],[238,1,238,3],[239,1,239,3],[240,1,240,3],[241,1,241,3],[242,1,242,3],[243,1,243,3],[244,1,244,3],[245,1,245,3],[228,1,228,3],[229,1,229,3],[230,1,230,3],[231,1,231,3],[232,1,232,3],[233,1,233,3],[234,1,234,3],[235,1,235,3],[236,1,236,3],[219,1,219,3],[220,1,220,3],[221,1,221,3],[222,1,222,3],[223,1,223,3],[224,1,224,3],[225,1,225,3],[226,1,226,3],[227,1,227,3],[210,1,210,3],[211,1,211,3],[212,1,212,3],[213,1,213,3],[214,1,214,3],[215,1,215,3],[216,1,216,3],[217,1,217,3],[218,1,218,3],[201,1,201,3],[202,1,202,3],[203,1,203,3],[204,1,204,3],[205,1,205,3],[206,1,206,3],[207,1,207,3],[208,1,208,3],[209,1,209,3],[192,1,192,3],[193,1,193,3],[194,1,194,3],[195,1,195,3],[196,1,196,3],[197,1,197,3],[198,1,198,3],[199,1,199,3],[200,1,200,3],[183,1,183,3],[184,1,184,3],[185,1,185,3],[186,1,186,3],[187,1,187,3],[188,1,188,3],[189,1,189,3],[190,1,190,3],[191,1,191,3],[174,1,174,3],[175,1,175,3],[176,1,176,3],[177,1,177,3],[178,1,178,3],[179,1,179,3],[180,1,180,3],[181,1,181,3],[182,1,182,3],[165,1,165,3],[166,1,166,3],[167,1,167,3],[168,1,168,3],[169,1,169,3],[170,1,170,3],[171,1,171,3],[172,1,172,3],[173,1,173,3],[156,1,156,3],[157,1,157,3],[158,1,158,3],[159,1,159,3],[160,1,160,3],[161,1,161,3],[162,1,162,3],[163,1,163,3],[164,1,164,3],[147,1,147,3],[148,1,148,3],[149,1,149,3],[150,1,150,3],[151,1,151,3],[152,1,152,3],[153,1,153,3],[154,1,154,3],[155,1,155,3],[138,1,138,3],[139,1,139,3],[140,1,140,3],[141,1,141,3],[142,1,142,3],[143,1,143,3],[144,1,144,3],[145,1,145,3],[146,1,146,3],[129,1,129,3],[130,1,130,3],[131,1,131,3],[132,1,132,3],[133,1,133,3],[134,1,134,3],[135,1,135,3],[136,1,136,3],[137,1,137,3],[120,1,120,3],[121,1,121,3],[122,1,122,3],[123,1,123,3],[124,1,124,3],[125,1,125,3],[126,1,126,3],[127,1,127,3],[128,1,128,3],[7,32,7,33],[435,1,435,3],[444,1,444,3],[7,7,8,7],[416,1,416,3],[7,17,8,17],[7,6,8,6],[7,12,8,12],[438,1,438,3],[440,1,440,3],[7,30,7,31],[325,1,325,3],[326,1,326,3],[327,1,327,3],[328,1,328,3],[329,1,329,3],[330,1,330,3],[333,1,333,3],[334,1,334,3],[335,1,335,3],[336,1,336,3],[337,1,337,3],[338,1,338,3],[339,1,339,3],[340,1,340,3],[7,5,8,5],[9,1,9,3],[483,1,483,3],[481,1,481,3],[480,1,480,3],[478,1,478,3],[479,1,479,3],[476,1,476,3],[477,1,477,3],[468,1,468,3],[331,1,331,3],[466,1,466,3],[443,1,443,3],[464,1,464,3],[453,1,453,3],[462,1,462,3],[446,1,446,3],[447,1,447,3],[449,1,449,3],[445,1,445,3],[452,1,452,3],[456,1,456,3],[457,1,457,3],[422,1,422,3],[433,1,433,3],[429,1,429,3],[425,1,425,3],[423,1,423,3],[424,1,424,3],[441,1,441,3],[430,1,430,3],[426,1,426,3],[428,1,428,3],[432,1,432,3],[436,1,436,3],[427,1,427,3],[332,1,332,3],[316,1,316,3],[317,1,317,3],[318,1,318,3],[319,1,319,3],[320,1,320,3],[321,1,321,3],[322,1,322,3],[323,1,323,3],[324,1,324,3],[499,1,499,3],[492,1,492,3],[493,1,493,3],[494,1,494,3],[495,1,495,3],[497,1,497,3],[498,1,498,3],[488,1,488,3],[475,1,475,3],[491,1,491,3],[484,1,484,3],[482,1,482,3],[490,1,490,3],[489,1,489,3],[486,1,486,3],[487,1,487,3],[485,1,485,3],[442,1,442,3],[469,1,469,3],[465,1,465,3],[463,1,463,3],[459,1,459,3],[460,1,460,3],[454,1,454,3],[448,1,448,3],[431,1,431,3],[434,1,434,3],[451,1,451,3],[439,1,439,3],[437,1,437,3],[472,1,472,3],[474,1,474,3],[458,1,458,3],[450,1,450,3],[470,1,470,3],[455,1,455,3],[473,1,473,3],[461,1,461,3],[471,1,471,3],[467,1,467,3],[6,19,6,20],[7,10,8,10],[7,8,8,8],[6,18,8,18],[6,8,6,12],[6,13,6,17],[7,14,8,14],[7,16,8,16],[7,13,8,13],[7,11,8,11],[419,1,419,3],[421,1,421,3],[417,1,417,3],[415,1,415,3],[5,1,5,3],[7,9,8,9],[312,1,312,3],[2,9,2,11],[7,15,8,15],[4,9,4,11],[7,4,8,4],[7,1,8,3],[414,1,414,3],[2,5,2,7],[2,1,2,2],[420,1,420,3],[413,1,413,3],[309,1,309,3],[310,1,310,3],[311,1,311,3],[418,1,418,3],[313,1,313,3],[314,1,314,3],[315,1,315,3],[341,1,341,3],[342,1,342,3],[343,1,343,3],[344,1,344,3],[345,1,345,3],[346,1,346,3],[347,1,347,3],[348,1,348,3],[349,1,349,3],[350,1,350,3],[351,1,351,3],[352,1,352,3],[353,1,353,3],[354,1,354,3],[355,1,355,3],[356,1,356,3],[357,1,357,3],[358,1,358,3],[380,1,380,3],[381,1,381,3],[382,1,382,3],[359,1,359,3],[360,1,360,3],[361,1,361,3],[362,1,362,3],[363,1,363,3],[364,1,364,3],[365,1,365,3],[366,1,366,3],[367,1,367,3],[394,1,394,3],[412,1,412,3],[395,1,395,3],[396,1,396,3],[397,1,397,3],[398,1,398,3],[399,1,399,3],[400,1,400,3],[401,1,401,3],[402,1,402,3],[403,1,403,3],[404,1,404,3],[405,1,405,3],[406,1,406,3],[407,1,407,3],[408,1,408,3],[409,1,409,3],[410,1,410,3],[411,1,411,3],[0,1,0,20],[386,1,386,3],[387,1,387,3],[388,1,388,3],[389,1,389,3],[390,1,390,3],[391,1,391,3],[392,1,392,3],[393,1,393,3],[383,1,383,3],[384,1,384,3],[385,1,385,3],[368,1,368,3],[369,1,369,3],[370,1,370,3],[371,1,371,3],[372,1,372,3],[373,1,373,3],[374,1,374,3],[375,1,375,3],[376,1,376,3],[377,1,377,3],[378,1,378,3],[379,1,379,3]]}
[null,"Block RAM Power",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($AD$1>0,OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),3),1)","v":0.97499999999999998},{"$f":"IF(TRUE,1,OFFSET(POWER_SCALE,4,OFFSET(POWER_SCALE,1,1))*PL_POWERED/0.9025)","v":1},{"$f":"IF(OPTIMIZATION=\"None\",0,1)","v":1},{"$f":"IF(Summary!$Y$1=\"noint\",0,1)","v":1},null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"READ_FIRST"]
[null,"Power",null,null,null,"Utilization",null,null,null,"Memory Resources User Guide",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"WRITE_FIRST"]
[null,"VCCINT",{"$f":"VCCINT","v":0.95},{"$f":"SUM(T10:T500)","v":5.6296464414106842},{"$f":"D4+D5","v":5.7806426049106845},"  RAMB18",{"$f":"SUM(IF((LEFT(G10:G500,6)=\"RAMB18\")+(LEFT(G10:G500,6)=\"FIFO18\"),E10:E500))","v":5000},{"$f":"IF(AND(G4/(NUM_BRAMS*2)>=0.995, G4/(NUM_BRAMS*2)<0.9999),0.99,G4/(NUM_BRAMS*2))","v":0.66137566137566139},{"$f":"G5+INT((G4+1)/2)","v":3700},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,"NO_CHANGE"]
[null,"VCCBRAM",{"$f":"VCCBRAM","v":0.95},{"$f":"SUM(U10:U500)","v":0.1509961635},null,"  RAMB36",{"$f":"SUM(IF((LEFT(G10:G500,6)<>\"RAMB18\")*(LEFT(G10:G500,6)<>\"FIFO18\"),E10:E500))+SUM(IF(LEFT(G10:G500,4)=\"CASC\",E10:E500))","v":1200},{"$f":"IF(AND(G5/NUM_BRAMS>=0.995, G5/NUM_BRAMS<0.9999),0.99,G5/NUM_BRAMS)","v":0.31746031746031744},null,"XPE User Guide",null,null,null,"Introduction to XPE (video)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9]
[null,{"$f":"TEXT(BRAM_POWER/TOTAL_POWER,\"0%\")&\" of total on-chip power \"&TEXT(TOTAL_POWER,\"0.000\")&\"W\"","v":"7% of total on-chip power 0.084W"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18]
[null,null,null,null,null,null,null,null,"Port A",null,null,null,null,"Port B",null,null,null,null,"Signal Rate (Mtr/s)","Power (W)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,36,null,null,"optimized"]
[null,"Name",null,null,"Block RAMs","Cascade Group Size","Mode","Toggle Rate","Clock (MHz)","Enable Rate","Bit Width","Write Mode","Write Rate","Clock (MHz)","Enable Rate","Bit Width","Write Mode","Write Rate",null,"VCCINT","VCCBRAM","PortA Column index into BRAM data table","PortB Column index into BRAM data table","PortA Row index into BRAM data table","PortB Row index into BRAM data table","# RAMB36 blocks used","FIFO or SDP (yes = 1)","Bit width range",null,"Clocking","PortA power",null,"PortB power",null,72,"Routing power",null,null,"PortA","PortB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"TEXT(VCCINT,\"0.000\")&\"V\"","v":"0.001V"},{"$f":"TEXT(VCCBRAM,\"0.000\")&\"V\"","v":"0.001V"},null,null,null,null,null,null,null,null,null,"Vccint","Vccbram","Vccint","Vccbram",64,null,null,"optimize","no change","no change",null,"Vccint Stdby Row","BRAM Enabled ","BRAM Disabled "]
[null,null,null,null,5000,4,"RAMB18",0.5,160,1,1,"NO_CHANGE",0.5,40,0.5,1,"NO_CHANGE",0.5,{"$f":"IF((AE10+AG10)<=0,0,((IF($AG10>0,$P10+8,0)*$N10*IF(AND($AA10=0,$AL10=1,$O10=1,$R10>0,$J10>0,$M10=0),$R10,$O10)+IF($AE10>0,$K10+8,0)*$I10*IF(AND($AL10=1,$O10=1,$AA10=2),MIN($J10,$R10),IF(AND($J10=1,$M10>0,$O10>0,$R10=0),$M10,$J10)))*$H10/(IF($AG10>0,$P10+8,0)+IF($AE10>0,$K10+8,0))))","v":45},{"$f":"(VCCINT/1000)*VCCINT_N*($AE10+$AG10+($AD10+$AJ10)*$AE$1)*IF(AND($AA10<>1,$A10<>1),OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),3),1)*$AC$1","v":2.9900594405172818},{"$f":"VCCBRAM/1000*(VCCBRAM/0.95)*($AF10+$AH10)*IF(AND($AA10<>1,$A10<>1),$AB$1,1)*$AC$1","v":8.2278787499999992E-2},{"$f":"IF(LEN($G10)=0,0,MATCH(IF((LEFT($G10,4)=\"RAMB\")+($G10=\"CASC (pair)\"),$G10 & IF($AM10=1,\"NO_CHANGE\",$L10),IF(AND($I10<>$N10,OR($G10=\"FIFO18\",$G10=\"FIFO36\")),\"ASYNC_\" & $G10,$G10)),BRAM_MODE_LIST,FALSE))","v":5},{"$f":"IF(LEN($G10)=0,0,MATCH(IF((LEFT($G10,4)=\"RAMB\")+($G10=\"CASC (pair)\"),$G10 &  IF($AN10=1,\"NO_CHANGE\",$Q10),IF(AND($I10<>$N10,OR($G10=\"FIFO18\",$G10=\"FIFO36\")),\"ASYNC_\" & $G10,$G10)),BRAM_MODE_LIST,FALSE))","v":5},{"$f":"MATCH(IF(K10=64,72,K10),BRAM_WIDTH_LIST,FALSE)","v":2},{"$f":"MATCH(IF(P10=64,72,P10),BRAM_WIDTH_LIST,FALSE)","v":2},{"$f":"IF(($G10=\"RAMB18\")+($G10=\"RAMB18SDP\")+($G10=\"FIFO18\")+($G10=\"FIFO18_36\"),INT(($E10+1)/2),IF(($G10=\"CASC (pair)\"),2*$E10,$E10))","v":2500},{"$f":"IF(($G10=\"RAMB18\")+($G10=\"RAMB36\")+($G10=\"CASC (pair)\"),0,IF(ISERR(FIND(\"SDP\", $G10)),1,2))","v":0},{"$f":"IF(LEN($G10)=0,\"AI1:AI1\",IF($G10=\"RAMB18\",\"AI1:AI6\",IF($G10=\"RAMB36\",\"AI1:AI7\",IF($G10=\"FIFO18\",\"AI4:AI7\",IF($G10=\"FIFO36\",\"AI4:AI8\",IF(G10=\"RAMB18SDP\",IF(P10<$AI$7,\"AI7\",\"AI2:AI7\"),IF(($G10=\"FIFO18_36\")+(G10=\"RAMB18SDP\"),\"AI1:AI7\",IF($G10=\"CASC (pair)\",\"AI2\",IF(OR(RIGHT(G10,3)=\"ECC\",LEFT(G10,13)=\"RAMB36SDP_ECC\"),\"AI9\",IF(G10=\"RAMB36SDP\",IF(P10<$AI$8,\"AI8\",\"AI2:AI8\"),\"AI8\"))))))))))","v":"AI1:AI6"},{"$f":"IF(LEFT($G10,4)=\"FIFO\",\"AJ1\",IF((LEN($G10)>8)*(MID($G10,7,3)=\"SDP\"),\"AJ2:AJ4\",\"AJ2:AJ4\"))","v":"AJ2:AJ4"},{"$f":"$Z10*4*($I10+$N10)*OFFSET(CLOCK_DATA,5,4)","v":75.54285714285713},{"$f":"($AQ10*MIN(1,LN(1+$H10*5 + 1.33))*(($I10*IF(AND($AL10=1,$O10=1,$AA10=2),MIN($J10,$J10),IF(AND($AL10=1,$J10=1,$M10>0,$O10>0,$R10=0),$M10,$J10))*IF($AA10=0,(1-$M10),1)*OFFSET(BRAM_TABLE,$X10,$V10)) + ($I10*IF(AND($AL10=1,$O10=1,$AA10=2),MIN($J10,$R10),IF(AND($AL10=1,$J10=1,$M10>0,$O10>0,$R10=0),$M10,$J10))*IF($AA10=0,$M10,0)*OFFSET(BRAM_TABLE,$X10,$V10+1)))+($AR10 + $AQ10 *(1-$J10))*$I10*(OFFSET(BRAM_TABLE,$AP10,68) +OFFSET(BRAM_TABLE,$AP10,68+1)))/1000","v":2730.1042147499998},{"$f":"$AQ10*0.7*(($I10*IF(AND($AL10=1,$O10=1,$AA10=2),MIN($J10,$J10),IF(AND($AL10=1,$J10=1,$M10>0,$O10>0,$R10=0),$M10,$J10))*IF($AA10=0,(1-$M10),1))*OFFSET(BRAM_TABLE,IF(AND($AA10=2,$K10>$P10,$P10>0),$Y10,$X10)+9,$V10) + ($I10*IF(AND($AL10=1,$O10=1,$AA10=2),MIN($J10,$R10),IF(AND($AL10=1,$J10=1,$M10>0,$O10>0,$R10=0),$M10,$J10))*IF($AA10=0,$M10,0))*OFFSET(BRAM_TABLE,IF(AND($AA10=2,$K10>$P10,$P10>0),$Y10,$X10)+9,$V10+1))/1000","v":78.959999999999994},{"$f":"($AQ10*MIN(1,LN(1+$H10*5+1.33))*($N10*IF(AND($AA10=0,$AL10=1,$O10=1,$R10>0,$J10>0,$M10=0),$R10,$O10)*IF($AA10=0,1-$R10,0)*OFFSET(BRAM_TABLE,$Y10,$W10)+($N10*IF(AND($AA10=0,$AL10=1,$O10=1,$R10>0,$J10>0,$M10=0),$R10,$O10)*$R10)*OFFSET(BRAM_TABLE,$Y10,$W10+1))+($AR10 + $AQ10 *(1-$O10))*$N10*(OFFSET(BRAM_TABLE,$AP10,68) +OFFSET(BRAM_TABLE,$AP10,68+1)))/1000","v":415.17702684374996},{"$f":"$AQ10*0.7*($N10*IF(AND($AA10=0,$AL10=1,$O10=1,$R10>0,$J10>0,$M10=0),$R10,$O10)*IF($AA10=0,1-$R10,0)*OFFSET(BRAM_TABLE,IF(AND($AA10=2,$P10>$K10,$K10>0),$X10,$Y10)+9,$W10)+$R10*$N10*IF(AND($AA10=0,$AL10=1,$O10=1,$R10>0,$J10>0,$M10=0),$R10,$O10)*OFFSET(BRAM_TABLE,IF(AND($AA10=2,$P10>$K10,$K10>0),$X10,$Y10)+9,$W10+1))/1000","v":9.8699999999999992},null,{"$f":"(IF(AA10=0,IF(OR($Q10=\"NO_CHANGE\",$AN10=1),1-$R10,2),0)*$P10*$N10*IF(AND($AA10=0,$AL10=1,$O10=1,$R10>0,$J10>0,$M10=0),$R10,$O10)+IF(AA10>0,1,IF(OR($L10=\"NO_CHANGE\",$AM10=1),1-$M10,2))*$K10*$I10*IF(AND($AL10=1,$O10=1,$AA10=2),MIN($J10,$R10),IF(AND($AL10=1,$AA10=0,$J10=1,$M10>0,$O10>0,$R10=0),$M10,$J10)))*IF($F10>0,IF(INT($E10/$F10)>0,($E10/$F10)+MOD($E10,$F10),$E10),$E10)*$H10*OFFSET(FANOUT,5,13)","v":7.310249999999999},null,{"$f":"IF(AND($AA10<>1,$AD$1>0,$A10<>1),1,0)","v":1},{"$f":"IF(AND($AL10=1,OR($AA10=2,$R10=0,$M10=0),$I10<>$N10),1,0)","v":0},0,{"$f":"IF(LEN($G10)=0,\"AI1:AI1\",IF($G10=\"RAMB18\",\"AI1:AI6\",IF($G10=\"RAMB36\",\"AI1:AI7\",IF($G10=\"FIFO18\",\"AI4:AI7\",IF($G10=\"FIFO36\",\"AI4:AI8\",IF(G10=\"RAMB18SDP\",IF(K10<$AI$7,\"AI7\",\"AI2:AI7\"),IF(($G10=\"FIFO18_36\")+(G10=\"RAMB18SDP\"),\"AI1:AI7\",IF($G10=\"CASC (pair)\",\"AI2\",IF(OR(RIGHT(G10,3)=\"ECC\",LEFT(G10,13)=\"RAMB36SDP_ECC\"),\"AI9\",IF(G10=\"RAMB36SDP\",IF(K10<$AI$8,\"AI8\",\"AI2:AI8\"),\"AI8\"))))))))))","v":"AI1:AI6"},{"$f":"IF($G10=\"RAMB18SDP\",3,IF(LEFT($G10,9)=\"RAMB36SDP\",4,IF(LEFT($G10,6)=\"FIFO18\",5,IF(LEFT($G10,6)=\"FIFO36\",6,IF(LEFT($G10,6)=\"RAMB36\",2,1)))))","v":1},{"$f":"IF($F10>0,IF(INT($E10/$F10)>0,($E10-MOD($E10,$F10))/($F10),$E10),$E10)","v":1250},{"$f":"IF(AND($AQ10>0,$E10>$AQ10),$E10-$AQ10,0)","v":3750}]
[null,null,null,null,1200,4,"RAMB36",0.125,320,1,1,"NO_CHANGE",0.1,null,0.25,1,"NO_CHANGE",0.5,40,{"$f":"(VCCINT/1000)*VCCINT_N*($AE11+$AG11+($AD11+$AJ11)*$AE$1)*IF(AND($AA11<>1,$A11<>1),OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),3),1)*$AC$1","v":2.6395870008934024},6.8717375999999997E-2,11,11,2,2,{"$f":"IF(($G11=\"RAMB18\")+($G11=\"RAMB18SDP\")+($G11=\"FIFO18\")+($G11=\"FIFO18_36\"),INT(($E11+1)/2),IF(($G11=\"CASC (pair)\"),2*$E11,$E11))","v":1200},{"$f":"IF(($G11=\"RAMB18\")+($G11=\"RAMB36\")+($G11=\"CASC (pair)\"),0,IF(ISERR(FIND(\"SDP\", $G11)),1,2))","v":0},{"$f":"IF(LEN($G11)=0,\"AI1:AI1\",IF($G11=\"RAMB18\",\"AI1:AI6\",IF($G11=\"RAMB36\",\"AI1:AI7\",IF($G11=\"FIFO18\",\"AI4:AI7\",IF($G11=\"FIFO36\",\"AI4:AI8\",IF(G11=\"RAMB18SDP\",IF(P11<$AI$7,\"AI7\",\"AI2:AI7\"),IF(($G11=\"FIFO18_36\")+(G11=\"RAMB18SDP\"),\"AI1:AI7\",IF($G11=\"CASC (pair)\",\"AI2\",IF(OR(RIGHT(G11,3)=\"ECC\",LEFT(G11,13)=\"RAMB36SDP_ECC\"),\"AI9\",IF(G11=\"RAMB36SDP\",IF(P11<$AI$8,\"AI8\",\"AI2:AI8\"),\"AI8\"))))))))))","v":"AI1:AI7"},{"$f":"IF(LEFT($G11,4)=\"FIFO\",\"AJ1\",IF((LEN($G11)>8)*(MID($G11,7,3)=\"SDP\"),\"AJ2:AJ4\",\"AJ2:AJ4\"))","v":"AJ2:AJ4"},{"$f":"$Z11*4*($I11+$N11)*OFFSET(CLOCK_DATA,5,4)","v":58.016914285714272},2790.3360638879994,74.188800000000001,0,0,null,1.4035679999999997,null,{"$f":"IF(AND($AA11<>1,$AD$1>0,$A11<>1),1,0)","v":1},{"$f":"IF(AND($AL11=1,OR($AA11=2,$R11=0,$M11=0),$I11<>$N11),1,0)","v":0},0,{"$f":"IF(LEN($G11)=0,\"AI1:AI1\",IF($G11=\"RAMB18\",\"AI1:AI6\",IF($G11=\"RAMB36\",\"AI1:AI7\",IF($G11=\"FIFO18\",\"AI4:AI7\",IF($G11=\"FIFO36\",\"AI4:AI8\",IF(G11=\"RAMB18SDP\",IF(K11<$AI$7,\"AI7\",\"AI2:AI7\"),IF(($G11=\"FIFO18_36\")+(G11=\"RAMB18SDP\"),\"AI1:AI7\",IF($G11=\"CASC (pair)\",\"AI2\",IF(OR(RIGHT(G11,3)=\"ECC\",LEFT(G11,13)=\"RAMB36SDP_ECC\"),\"AI9\",IF(G11=\"RAMB36SDP\",IF(K11<$AI$8,\"AI8\",\"AI2:AI8\"),\"AI8\"))))))))))","v":"AI1:AI7"},{"$f":"IF($G11=\"RAMB18SDP\",3,IF(LEFT($G11,9)=\"RAMB36SDP\",4,IF(LEFT($G11,6)=\"FIFO18\",5,IF(LEFT($G11,6)=\"FIFO36\",6,IF(LEFT($G11,6)=\"RAMB36\",2,1)))))","v":2},{"$f":"IF($F11>0,IF(INT($E11/$F11)>0,($E11-MOD($E11,$F11))/($F11),$E11),$E11)","v":300},{"$f":"IF(AND($AQ11>0,$E11>$AQ11),$E11-$AQ11,0)","v":900}]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,{"$f":"VCCBRAM/1000*(VCCBRAM/0.95)*($AF74+$AH74)*IF(AND($AA74<>1,$A74<>1),$AB$1,1)*$AC$1","v":0},{"$f":"IF(LEN($G74)=0,0,MATCH(IF((LEFT($G74,4)=\"RAMB\")+($G74=\"CASC (pair)\"),$G74 & IF($AM74=1,\"NO_CHANGE\",$L74),IF(AND($I74<>$N74,OR($G74=\"FIFO18\",$G74=\"FIFO36\")),\"ASYNC_\" & $G74,$G74)),BRAM_MODE_LIST,FALSE))","v":5},{"$f":"IF(LEN($G74)=0,0,MATCH(IF((LEFT($G74,4)=\"RAMB\")+($G74=\"CASC (pair)\"),$G74 &  IF($AN74=1,\"NO_CHANGE\",$Q74),IF(AND($I74<>$N74,OR($G74=\"FIFO18\",$G74=\"FIFO36\")),\"ASYNC_\" & $G74,$G74)),BRAM_MODE_LIST,FALSE))","v":5},{"$f":"MATCH(IF(K74=64,72,K74),BRAM_WIDTH_LIST,FALSE)","v":2},{"$f":"MATCH(IF(P74=64,72,P74),BRAM_WIDTH_LIST,FALSE)","v":2},0,0,"AI1:AI6","AJ2:AJ4",0,{"$f":"($AQ74*MIN(1,LN(1+$H74*5 + 1.33))*(($I74*IF(AND($AL74=1,$O74=1,$AA74=2),MIN($J74,$J74),IF(AND($AL74=1,$J74=1,$M74>0,$O74>0,$R74=0),$M74,$J74))*IF($AA74=0,(1-$M74),1)*OFFSET(BRAM_TABLE,$X74,$V74)) + ($I74*IF(AND($AL74=1,$O74=1,$AA74=2),MIN($J74,$R74),IF(AND($AL74=1,$J74=1,$M74>0,$O74>0,$R74=0),$M74,$J74))*IF($AA74=0,$M74,0)*OFFSET(BRAM_TABLE,$X74,$V74+1)))+($AR74 + $AQ74 *(1-$J74))*$I74*(OFFSET(BRAM_TABLE,$AP74,68) +OFFSET(BRAM_TABLE,$AP74,68+1)))/1000","v":0},{"$f":"$AQ74*0.7*(($I74*IF(AND($AL74=1,$O74=1,$AA74=2),MIN($J74,$J74),IF(AND($AL74=1,$J74=1,$M74>0,$O74>0,$R74=0),$M74,$J74))*IF($AA74=0,(1-$M74),1))*OFFSET(BRAM_TABLE,IF(AND($AA74=2,$K74>$P74,$P74>0),$Y74,$X74)+9,$V74) + ($I74*IF(AND($AL74=1,$O74=1,$AA74=2),MIN($J74,$R74),IF(AND($AL74=1,$J74=1,$M74>0,$O74>0,$R74=0),$M74,$J74))*IF($AA74=0,$M74,0))*OFFSET(BRAM_TABLE,IF(AND($AA74=2,$K74>$P74,$P74>0),$Y74,$X74)+9,$V74+1))/1000","v":0},{"$f":"($AQ74*MIN(1,LN(1+$H74*5+1.33))*($N74*IF(AND($AA74=0,$AL74=1,$O74=1,$R74>0,$J74>0,$M74=0),$R74,$O74)*IF($AA74=0,1-$R74,0)*OFFSET(BRAM_TABLE,$Y74,$W74)+($N74*IF(AND($AA74=0,$AL74=1,$O74=1,$R74>0,$J74>0,$M74=0),$R74,$O74)*$R74)*OFFSET(BRAM_TABLE,$Y74,$W74+1))+($AR74 + $AQ74 *(1-$O74))*$N74*(OFFSET(BRAM_TABLE,$AP74,68) +OFFSET(BRAM_TABLE,$AP74,68+1)))/1000","v":0},{"$f":"$AQ74*0.7*($N74*IF(AND($AA74=0,$AL74=1,$O74=1,$R74>0,$J74>0,$M74=0),$R74,$O74)*IF($AA74=0,1-$R74,0)*OFFSET(BRAM_TABLE,IF(AND($AA74=2,$P74>$K74,$K74>0),$X74,$Y74)+9,$W74)+$R74*$N74*IF(AND($AA74=0,$AL74=1,$O74=1,$R74>0,$J74>0,$M74=0),$R74,$O74)*OFFSET(BRAM_TABLE,IF(AND($AA74=2,$P74>$K74,$K74>0),$X74,$Y74)+9,$W74+1))/1000","v":0},null,{"$f":"(IF(AA74=0,IF(OR($Q74=\"NO_CHANGE\",$AN74=1),1-$R74,2),0)*$P74*$N74*IF(AND($AA74=0,$AL74=1,$O74=1,$R74>0,$J74>0,$M74=0),$R74,$O74)+IF(AA74>0,1,IF(OR($L74=\"NO_CHANGE\",$AM74=1),1-$M74,2))*$K74*$I74*IF(AND($AL74=1,$O74=1,$AA74=2),MIN($J74,$R74),IF(AND($AL74=1,$AA74=0,$J74=1,$M74>0,$O74>0,$R74=0),$M74,$J74)))*IF($F74>0,IF(INT($E74/$F74)>0,($E74/$F74)+MOD($E74,$F74),$E74),$E74)*$H74*OFFSET(FANOUT,5,13)","v":0},null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,{"$f":"(VCCINT/1000)*VCCINT_N*($AE75+$AG75+($AD75+$AJ75)*$AE$1)*IF(AND($AA75<>1,$A75<>1),OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),3),1)*$AC$1","v":0},0,5,5,2,2,{"$f":"IF(($G75=\"RAMB18\")+($G75=\"RAMB18SDP\")+($G75=\"FIFO18\")+($G75=\"FIFO18_36\"),INT(($E75+1)/2),IF(($G75=\"CASC (pair)\"),2*$E75,$E75))","v":0},{"$f":"IF(($G75=\"RAMB18\")+($G75=\"RAMB36\")+($G75=\"CASC (pair)\"),0,IF(ISERR(FIND(\"SDP\", $G75)),1,2))","v":0},{"$f":"IF(LEN($G75)=0,\"AI1:AI1\",IF($G75=\"RAMB18\",\"AI1:AI6\",IF($G75=\"RAMB36\",\"AI1:AI7\",IF($G75=\"FIFO18\",\"AI4:AI7\",IF($G75=\"FIFO36\",\"AI4:AI8\",IF(G75=\"RAMB18SDP\",IF(P75<$AI$7,\"AI7\",\"AI2:AI7\"),IF(($G75=\"FIFO18_36\")+(G75=\"RAMB18SDP\"),\"AI1:AI7\",IF($G75=\"CASC (pair)\",\"AI2\",IF(OR(RIGHT(G75,3)=\"ECC\",LEFT(G75,13)=\"RAMB36SDP_ECC\"),\"AI9\",IF(G75=\"RAMB36SDP\",IF(P75<$AI$8,\"AI8\",\"AI2:AI8\"),\"AI8\"))))))))))","v":"AI1:AI6"},{"$f":"IF(LEFT($G75,4)=\"FIFO\",\"AJ1\",IF((LEN($G75)>8)*(MID($G75,7,3)=\"SDP\"),\"AJ2:AJ4\",\"AJ2:AJ4\"))","v":"AJ2:AJ4"},{"$f":"$Z75*4*($I75+$N75)*OFFSET(CLOCK_DATA,5,4)","v":0},0,0,0,0,null,0,null,{"$f":"IF(AND($AA75<>1,$AD$1>0,$A75<>1),1,0)","v":1},0,0,{"$f":"IF(LEN($G75)=0,\"AI1:AI1\",IF($G75=\"RAMB18\",\"AI1:AI6\",IF($G75=\"RAMB36\",\"AI1:AI7\",IF($G75=\"FIFO18\",\"AI4:AI7\",IF($G75=\"FIFO36\",\"AI4:AI8\",IF(G75=\"RAMB18SDP\",IF(K75<$AI$7,\"AI7\",\"AI2:AI7\"),IF(($G75=\"FIFO18_36\")+(G75=\"RAMB18SDP\"),\"AI1:AI7\",IF($G75=\"CASC (pair)\",\"AI2\",IF(OR(RIGHT(G75,3)=\"ECC\",LEFT(G75,13)=\"RAMB36SDP_ECC\"),\"AI9\",IF(G75=\"RAMB36SDP\",IF(K75<$AI$8,\"AI8\",\"AI2:AI8\"),\"AI8\"))))))))))","v":"AI1:AI6"},{"$f":"IF($G75=\"RAMB18SDP\",3,IF(LEFT($G75,9)=\"RAMB36SDP\",4,IF(LEFT($G75,6)=\"FIFO18\",5,IF(LEFT($G75,6)=\"FIFO36\",6,IF(LEFT($G75,6)=\"RAMB36\",2,1)))))","v":1},{"$f":"IF($F75>0,IF(INT($E75/$F75)>0,($E75-MOD($E75,$F75))/($F75),$E75),$E75)","v":0},{"$f":"IF(AND($AQ75>0,$E75>$AQ75),$E75-$AQ75,0)","v":0}]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,{"$f":"IF((AE121+AG121)<=0,0,((IF($AG121>0,$P121+8,0)*$N121*IF(AND($AA121=0,$AL121=1,$O121=1,$R121>0,$J121>0,$M121=0),$R121,$O121)+IF($AE121>0,$K121+8,0)*$I121*IF(AND($AL121=1,$O121=1,$AA121=2),MIN($J121,$R121),IF(AND($J121=1,$M121>0,$O121>0,$R121=0),$M121,$J121)))*$H121/(IF($AG121>0,$P121+8,0)+IF($AE121>0,$K121+8,0))))","v":0},0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,{"$f":"VCCBRAM/1000*(VCCBRAM/0.95)*($AF138+$AH138)*IF(AND($AA138<>1,$A138<>1),$AB$1,1)*$AC$1","v":0},{"$f":"IF(LEN($G138)=0,0,MATCH(IF((LEFT($G138,4)=\"RAMB\")+($G138=\"CASC (pair)\"),$G138 & IF($AM138=1,\"NO_CHANGE\",$L138),IF(AND($I138<>$N138,OR($G138=\"FIFO18\",$G138=\"FIFO36\")),\"ASYNC_\" & $G138,$G138)),BRAM_MODE_LIST,FALSE))","v":5},{"$f":"IF(LEN($G138)=0,0,MATCH(IF((LEFT($G138,4)=\"RAMB\")+($G138=\"CASC (pair)\"),$G138 &  IF($AN138=1,\"NO_CHANGE\",$Q138),IF(AND($I138<>$N138,OR($G138=\"FIFO18\",$G138=\"FIFO36\")),\"ASYNC_\" & $G138,$G138)),BRAM_MODE_LIST,FALSE))","v":5},{"$f":"MATCH(IF(K138=64,72,K138),BRAM_WIDTH_LIST,FALSE)","v":2},{"$f":"MATCH(IF(P138=64,72,P138),BRAM_WIDTH_LIST,FALSE)","v":2},0,0,"AI1:AI6","AJ2:AJ4",0,{"$f":"($AQ138*MIN(1,LN(1+$H138*5 + 1.33))*(($I138*IF(AND($AL138=1,$O138=1,$AA138=2),MIN($J138,$J138),IF(AND($AL138=1,$J138=1,$M138>0,$O138>0,$R138=0),$M138,$J138))*IF($AA138=0,(1-$M138),1)*OFFSET(BRAM_TABLE,$X138,$V138)) + ($I138*IF(AND($AL138=1,$O138=1,$AA138=2),MIN($J138,$R138),IF(AND($AL138=1,$J138=1,$M138>0,$O138>0,$R138=0),$M138,$J138))*IF($AA138=0,$M138,0)*OFFSET(BRAM_TABLE,$X138,$V138+1)))+($AR138 + $AQ138 *(1-$J138))*$I138*(OFFSET(BRAM_TABLE,$AP138,68) +OFFSET(BRAM_TABLE,$AP138,68+1)))/1000","v":0},{"$f":"$AQ138*0.7*(($I138*IF(AND($AL138=1,$O138=1,$AA138=2),MIN($J138,$J138),IF(AND($AL138=1,$J138=1,$M138>0,$O138>0,$R138=0),$M138,$J138))*IF($AA138=0,(1-$M138),1))*OFFSET(BRAM_TABLE,IF(AND($AA138=2,$K138>$P138,$P138>0),$Y138,$X138)+9,$V138) + ($I138*IF(AND($AL138=1,$O138=1,$AA138=2),MIN($J138,$R138),IF(AND($AL138=1,$J138=1,$M138>0,$O138>0,$R138=0),$M138,$J138))*IF($AA138=0,$M138,0))*OFFSET(BRAM_TABLE,IF(AND($AA138=2,$K138>$P138,$P138>0),$Y138,$X138)+9,$V138+1))/1000","v":0},{"$f":"($AQ138*MIN(1,LN(1+$H138*5+1.33))*($N138*IF(AND($AA138=0,$AL138=1,$O138=1,$R138>0,$J138>0,$M138=0),$R138,$O138)*IF($AA138=0,1-$R138,0)*OFFSET(BRAM_TABLE,$Y138,$W138)+($N138*IF(AND($AA138=0,$AL138=1,$O138=1,$R138>0,$J138>0,$M138=0),$R138,$O138)*$R138)*OFFSET(BRAM_TABLE,$Y138,$W138+1))+($AR138 + $AQ138 *(1-$O138))*$N138*(OFFSET(BRAM_TABLE,$AP138,68) +OFFSET(BRAM_TABLE,$AP138,68+1)))/1000","v":0},{"$f":"$AQ138*0.7*($N138*IF(AND($AA138=0,$AL138=1,$O138=1,$R138>0,$J138>0,$M138=0),$R138,$O138)*IF($AA138=0,1-$R138,0)*OFFSET(BRAM_TABLE,IF(AND($AA138=2,$P138>$K138,$K138>0),$X138,$Y138)+9,$W138)+$R138*$N138*IF(AND($AA138=0,$AL138=1,$O138=1,$R138>0,$J138>0,$M138=0),$R138,$O138)*OFFSET(BRAM_TABLE,IF(AND($AA138=2,$P138>$K138,$K138>0),$X138,$Y138)+9,$W138+1))/1000","v":0},null,{"$f":"(IF(AA138=0,IF(OR($Q138=\"NO_CHANGE\",$AN138=1),1-$R138,2),0)*$P138*$N138*IF(AND($AA138=0,$AL138=1,$O138=1,$R138>0,$J138>0,$M138=0),$R138,$O138)+IF(AA138>0,1,IF(OR($L138=\"NO_CHANGE\",$AM138=1),1-$M138,2))*$K138*$I138*IF(AND($AL138=1,$O138=1,$AA138=2),MIN($J138,$R138),IF(AND($AL138=1,$AA138=0,$J138=1,$M138>0,$O138>0,$R138=0),$M138,$J138)))*IF($F138>0,IF(INT($E138/$F138)>0,($E138/$F138)+MOD($E138,$F138),$E138),$E138)*$H138*OFFSET(FANOUT,5,13)","v":0},null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,{"$f":"(VCCINT/1000)*VCCINT_N*($AE139+$AG139+($AD139+$AJ139)*$AE$1)*IF(AND($AA139<>1,$A139<>1),OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),3),1)*$AC$1","v":0},0,5,5,2,2,{"$f":"IF(($G139=\"RAMB18\")+($G139=\"RAMB18SDP\")+($G139=\"FIFO18\")+($G139=\"FIFO18_36\"),INT(($E139+1)/2),IF(($G139=\"CASC (pair)\"),2*$E139,$E139))","v":0},{"$f":"IF(($G139=\"RAMB18\")+($G139=\"RAMB36\")+($G139=\"CASC (pair)\"),0,IF(ISERR(FIND(\"SDP\", $G139)),1,2))","v":0},{"$f":"IF(LEN($G139)=0,\"AI1:AI1\",IF($G139=\"RAMB18\",\"AI1:AI6\",IF($G139=\"RAMB36\",\"AI1:AI7\",IF($G139=\"FIFO18\",\"AI4:AI7\",IF($G139=\"FIFO36\",\"AI4:AI8\",IF(G139=\"RAMB18SDP\",IF(P139<$AI$7,\"AI7\",\"AI2:AI7\"),IF(($G139=\"FIFO18_36\")+(G139=\"RAMB18SDP\"),\"AI1:AI7\",IF($G139=\"CASC (pair)\",\"AI2\",IF(OR(RIGHT(G139,3)=\"ECC\",LEFT(G139,13)=\"RAMB36SDP_ECC\"),\"AI9\",IF(G139=\"RAMB36SDP\",IF(P139<$AI$8,\"AI8\",\"AI2:AI8\"),\"AI8\"))))))))))","v":"AI1:AI6"},{"$f":"IF(LEFT($G139,4)=\"FIFO\",\"AJ1\",IF((LEN($G139)>8)*(MID($G139,7,3)=\"SDP\"),\"AJ2:AJ4\",\"AJ2:AJ4\"))","v":"AJ2:AJ4"},{"$f":"$Z139*4*($I139+$N139)*OFFSET(CLOCK_DATA,5,4)","v":0},0,0,0,0,null,0,null,{"$f":"IF(AND($AA139<>1,$AD$1>0,$A139<>1),1,0)","v":1},0,0,{"$f":"IF(LEN($G139)=0,\"AI1:AI1\",IF($G139=\"RAMB18\",\"AI1:AI6\",IF($G139=\"RAMB36\",\"AI1:AI7\",IF($G139=\"FIFO18\",\"AI4:AI7\",IF($G139=\"FIFO36\",\"AI4:AI8\",IF(G139=\"RAMB18SDP\",IF(K139<$AI$7,\"AI7\",\"AI2:AI7\"),IF(($G139=\"FIFO18_36\")+(G139=\"RAMB18SDP\"),\"AI1:AI7\",IF($G139=\"CASC (pair)\",\"AI2\",IF(OR(RIGHT(G139,3)=\"ECC\",LEFT(G139,13)=\"RAMB36SDP_ECC\"),\"AI9\",IF(G139=\"RAMB36SDP\",IF(K139<$AI$8,\"AI8\",\"AI2:AI8\"),\"AI8\"))))))))))","v":"AI1:AI6"},{"$f":"IF($G139=\"RAMB18SDP\",3,IF(LEFT($G139,9)=\"RAMB36SDP\",4,IF(LEFT($G139,6)=\"FIFO18\",5,IF(LEFT($G139,6)=\"FIFO36\",6,IF(LEFT($G139,6)=\"RAMB36\",2,1)))))","v":1},{"$f":"IF($F139>0,IF(INT($E139/$F139)>0,($E139-MOD($E139,$F139))/($F139),$E139),$E139)","v":0},{"$f":"IF(AND($AQ139>0,$E139>$AQ139),$E139-$AQ139,0)","v":0}]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,{"$f":"VCCBRAM/1000*(VCCBRAM/0.95)*($AF202+$AH202)*IF(AND($AA202<>1,$A202<>1),$AB$1,1)*$AC$1","v":0},{"$f":"IF(LEN($G202)=0,0,MATCH(IF((LEFT($G202,4)=\"RAMB\")+($G202=\"CASC (pair)\"),$G202 & IF($AM202=1,\"NO_CHANGE\",$L202),IF(AND($I202<>$N202,OR($G202=\"FIFO18\",$G202=\"FIFO36\")),\"ASYNC_\" & $G202,$G202)),BRAM_MODE_LIST,FALSE))","v":5},{"$f":"IF(LEN($G202)=0,0,MATCH(IF((LEFT($G202,4)=\"RAMB\")+($G202=\"CASC (pair)\"),$G202 &  IF($AN202=1,\"NO_CHANGE\",$Q202),IF(AND($I202<>$N202,OR($G202=\"FIFO18\",$G202=\"FIFO36\")),\"ASYNC_\" & $G202,$G202)),BRAM_MODE_LIST,FALSE))","v":5},{"$f":"MATCH(IF(K202=64,72,K202),BRAM_WIDTH_LIST,FALSE)","v":2},{"$f":"MATCH(IF(P202=64,72,P202),BRAM_WIDTH_LIST,FALSE)","v":2},0,0,"AI1:AI6","AJ2:AJ4",0,{"$f":"($AQ202*MIN(1,LN(1+$H202*5 + 1.33))*(($I202*IF(AND($AL202=1,$O202=1,$AA202=2),MIN($J202,$J202),IF(AND($AL202=1,$J202=1,$M202>0,$O202>0,$R202=0),$M202,$J202))*IF($AA202=0,(1-$M202),1)*OFFSET(BRAM_TABLE,$X202,$V202)) + ($I202*IF(AND($AL202=1,$O202=1,$AA202=2),MIN($J202,$R202),IF(AND($AL202=1,$J202=1,$M202>0,$O202>0,$R202=0),$M202,$J202))*IF($AA202=0,$M202,0)*OFFSET(BRAM_TABLE,$X202,$V202+1)))+($AR202 + $AQ202 *(1-$J202))*$I202*(OFFSET(BRAM_TABLE,$AP202,68) +OFFSET(BRAM_TABLE,$AP202,68+1)))/1000","v":0},{"$f":"$AQ202*0.7*(($I202*IF(AND($AL202=1,$O202=1,$AA202=2),MIN($J202,$J202),IF(AND($AL202=1,$J202=1,$M202>0,$O202>0,$R202=0),$M202,$J202))*IF($AA202=0,(1-$M202),1))*OFFSET(BRAM_TABLE,IF(AND($AA202=2,$K202>$P202,$P202>0),$Y202,$X202)+9,$V202) + ($I202*IF(AND($AL202=1,$O202=1,$AA202=2),MIN($J202,$R202),IF(AND($AL202=1,$J202=1,$M202>0,$O202>0,$R202=0),$M202,$J202))*IF($AA202=0,$M202,0))*OFFSET(BRAM_TABLE,IF(AND($AA202=2,$K202>$P202,$P202>0),$Y202,$X202)+9,$V202+1))/1000","v":0},{"$f":"($AQ202*MIN(1,LN(1+$H202*5+1.33))*($N202*IF(AND($AA202=0,$AL202=1,$O202=1,$R202>0,$J202>0,$M202=0),$R202,$O202)*IF($AA202=0,1-$R202,0)*OFFSET(BRAM_TABLE,$Y202,$W202)+($N202*IF(AND($AA202=0,$AL202=1,$O202=1,$R202>0,$J202>0,$M202=0),$R202,$O202)*$R202)*OFFSET(BRAM_TABLE,$Y202,$W202+1))+($AR202 + $AQ202 *(1-$O202))*$N202*(OFFSET(BRAM_TABLE,$AP202,68) +OFFSET(BRAM_TABLE,$AP202,68+1)))/1000","v":0},{"$f":"$AQ202*0.7*($N202*IF(AND($AA202=0,$AL202=1,$O202=1,$R202>0,$J202>0,$M202=0),$R202,$O202)*IF($AA202=0,1-$R202,0)*OFFSET(BRAM_TABLE,IF(AND($AA202=2,$P202>$K202,$K202>0),$X202,$Y202)+9,$W202)+$R202*$N202*IF(AND($AA202=0,$AL202=1,$O202=1,$R202>0,$J202>0,$M202=0),$R202,$O202)*OFFSET(BRAM_TABLE,IF(AND($AA202=2,$P202>$K202,$K202>0),$X202,$Y202)+9,$W202+1))/1000","v":0},null,{"$f":"(IF(AA202=0,IF(OR($Q202=\"NO_CHANGE\",$AN202=1),1-$R202,2),0)*$P202*$N202*IF(AND($AA202=0,$AL202=1,$O202=1,$R202>0,$J202>0,$M202=0),$R202,$O202)+IF(AA202>0,1,IF(OR($L202=\"NO_CHANGE\",$AM202=1),1-$M202,2))*$K202*$I202*IF(AND($AL202=1,$O202=1,$AA202=2),MIN($J202,$R202),IF(AND($AL202=1,$AA202=0,$J202=1,$M202>0,$O202>0,$R202=0),$M202,$J202)))*IF($F202>0,IF(INT($E202/$F202)>0,($E202/$F202)+MOD($E202,$F202),$E202),$E202)*$H202*OFFSET(FANOUT,5,13)","v":0},null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,{"$f":"(VCCINT/1000)*VCCINT_N*($AE203+$AG203+($AD203+$AJ203)*$AE$1)*IF(AND($AA203<>1,$A203<>1),OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),3),1)*$AC$1","v":0},0,5,5,2,2,{"$f":"IF(($G203=\"RAMB18\")+($G203=\"RAMB18SDP\")+($G203=\"FIFO18\")+($G203=\"FIFO18_36\"),INT(($E203+1)/2),IF(($G203=\"CASC (pair)\"),2*$E203,$E203))","v":0},{"$f":"IF(($G203=\"RAMB18\")+($G203=\"RAMB36\")+($G203=\"CASC (pair)\"),0,IF(ISERR(FIND(\"SDP\", $G203)),1,2))","v":0},{"$f":"IF(LEN($G203)=0,\"AI1:AI1\",IF($G203=\"RAMB18\",\"AI1:AI6\",IF($G203=\"RAMB36\",\"AI1:AI7\",IF($G203=\"FIFO18\",\"AI4:AI7\",IF($G203=\"FIFO36\",\"AI4:AI8\",IF(G203=\"RAMB18SDP\",IF(P203<$AI$7,\"AI7\",\"AI2:AI7\"),IF(($G203=\"FIFO18_36\")+(G203=\"RAMB18SDP\"),\"AI1:AI7\",IF($G203=\"CASC (pair)\",\"AI2\",IF(OR(RIGHT(G203,3)=\"ECC\",LEFT(G203,13)=\"RAMB36SDP_ECC\"),\"AI9\",IF(G203=\"RAMB36SDP\",IF(P203<$AI$8,\"AI8\",\"AI2:AI8\"),\"AI8\"))))))))))","v":"AI1:AI6"},{"$f":"IF(LEFT($G203,4)=\"FIFO\",\"AJ1\",IF((LEN($G203)>8)*(MID($G203,7,3)=\"SDP\"),\"AJ2:AJ4\",\"AJ2:AJ4\"))","v":"AJ2:AJ4"},{"$f":"$Z203*4*($I203+$N203)*OFFSET(CLOCK_DATA,5,4)","v":0},0,0,0,0,null,0,null,{"$f":"IF(AND($AA203<>1,$AD$1>0,$A203<>1),1,0)","v":1},0,0,{"$f":"IF(LEN($G203)=0,\"AI1:AI1\",IF($G203=\"RAMB18\",\"AI1:AI6\",IF($G203=\"RAMB36\",\"AI1:AI7\",IF($G203=\"FIFO18\",\"AI4:AI7\",IF($G203=\"FIFO36\",\"AI4:AI8\",IF(G203=\"RAMB18SDP\",IF(K203<$AI$7,\"AI7\",\"AI2:AI7\"),IF(($G203=\"FIFO18_36\")+(G203=\"RAMB18SDP\"),\"AI1:AI7\",IF($G203=\"CASC (pair)\",\"AI2\",IF(OR(RIGHT(G203,3)=\"ECC\",LEFT(G203,13)=\"RAMB36SDP_ECC\"),\"AI9\",IF(G203=\"RAMB36SDP\",IF(K203<$AI$8,\"AI8\",\"AI2:AI8\"),\"AI8\"))))))))))","v":"AI1:AI6"},{"$f":"IF($G203=\"RAMB18SDP\",3,IF(LEFT($G203,9)=\"RAMB36SDP\",4,IF(LEFT($G203,6)=\"FIFO18\",5,IF(LEFT($G203,6)=\"FIFO36\",6,IF(LEFT($G203,6)=\"RAMB36\",2,1)))))","v":1},{"$f":"IF($F203>0,IF(INT($E203/$F203)>0,($E203-MOD($E203,$F203))/($F203),$E203),$E203)","v":0},{"$f":"IF(AND($AQ203>0,$E203>$AQ203),$E203-$AQ203,0)","v":0}]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,{"$f":"IF(AND($AL228=1,OR($AA228=2,$R228=0,$M228=0),$I228<>$N228),1,0)","v":0},"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,{"$f":"IF(AND($AL248=1,OR($AA248=2,$R248=0,$M248=0),$I248<>$N248),1,0)","v":0},0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,{"$f":"VCCBRAM/1000*(VCCBRAM/0.95)*($AF266+$AH266)*IF(AND($AA266<>1,$A266<>1),$AB$1,1)*$AC$1","v":0},{"$f":"IF(LEN($G266)=0,0,MATCH(IF((LEFT($G266,4)=\"RAMB\")+($G266=\"CASC (pair)\"),$G266 & IF($AM266=1,\"NO_CHANGE\",$L266),IF(AND($I266<>$N266,OR($G266=\"FIFO18\",$G266=\"FIFO36\")),\"ASYNC_\" & $G266,$G266)),BRAM_MODE_LIST,FALSE))","v":5},{"$f":"IF(LEN($G266)=0,0,MATCH(IF((LEFT($G266,4)=\"RAMB\")+($G266=\"CASC (pair)\"),$G266 &  IF($AN266=1,\"NO_CHANGE\",$Q266),IF(AND($I266<>$N266,OR($G266=\"FIFO18\",$G266=\"FIFO36\")),\"ASYNC_\" & $G266,$G266)),BRAM_MODE_LIST,FALSE))","v":5},{"$f":"MATCH(IF(K266=64,72,K266),BRAM_WIDTH_LIST,FALSE)","v":2},{"$f":"MATCH(IF(P266=64,72,P266),BRAM_WIDTH_LIST,FALSE)","v":2},0,0,"AI1:AI6","AJ2:AJ4",0,{"$f":"($AQ266*MIN(1,LN(1+$H266*5 + 1.33))*(($I266*IF(AND($AL266=1,$O266=1,$AA266=2),MIN($J266,$J266),IF(AND($AL266=1,$J266=1,$M266>0,$O266>0,$R266=0),$M266,$J266))*IF($AA266=0,(1-$M266),1)*OFFSET(BRAM_TABLE,$X266,$V266)) + ($I266*IF(AND($AL266=1,$O266=1,$AA266=2),MIN($J266,$R266),IF(AND($AL266=1,$J266=1,$M266>0,$O266>0,$R266=0),$M266,$J266))*IF($AA266=0,$M266,0)*OFFSET(BRAM_TABLE,$X266,$V266+1)))+($AR266 + $AQ266 *(1-$J266))*$I266*(OFFSET(BRAM_TABLE,$AP266,68) +OFFSET(BRAM_TABLE,$AP266,68+1)))/1000","v":0},{"$f":"$AQ266*0.7*(($I266*IF(AND($AL266=1,$O266=1,$AA266=2),MIN($J266,$J266),IF(AND($AL266=1,$J266=1,$M266>0,$O266>0,$R266=0),$M266,$J266))*IF($AA266=0,(1-$M266),1))*OFFSET(BRAM_TABLE,IF(AND($AA266=2,$K266>$P266,$P266>0),$Y266,$X266)+9,$V266) + ($I266*IF(AND($AL266=1,$O266=1,$AA266=2),MIN($J266,$R266),IF(AND($AL266=1,$J266=1,$M266>0,$O266>0,$R266=0),$M266,$J266))*IF($AA266=0,$M266,0))*OFFSET(BRAM_TABLE,IF(AND($AA266=2,$K266>$P266,$P266>0),$Y266,$X266)+9,$V266+1))/1000","v":0},{"$f":"($AQ266*MIN(1,LN(1+$H266*5+1.33))*($N266*IF(AND($AA266=0,$AL266=1,$O266=1,$R266>0,$J266>0,$M266=0),$R266,$O266)*IF($AA266=0,1-$R266,0)*OFFSET(BRAM_TABLE,$Y266,$W266)+($N266*IF(AND($AA266=0,$AL266=1,$O266=1,$R266>0,$J266>0,$M266=0),$R266,$O266)*$R266)*OFFSET(BRAM_TABLE,$Y266,$W266+1))+($AR266 + $AQ266 *(1-$O266))*$N266*(OFFSET(BRAM_TABLE,$AP266,68) +OFFSET(BRAM_TABLE,$AP266,68+1)))/1000","v":0},{"$f":"$AQ266*0.7*($N266*IF(AND($AA266=0,$AL266=1,$O266=1,$R266>0,$J266>0,$M266=0),$R266,$O266)*IF($AA266=0,1-$R266,0)*OFFSET(BRAM_TABLE,IF(AND($AA266=2,$P266>$K266,$K266>0),$X266,$Y266)+9,$W266)+$R266*$N266*IF(AND($AA266=0,$AL266=1,$O266=1,$R266>0,$J266>0,$M266=0),$R266,$O266)*OFFSET(BRAM_TABLE,IF(AND($AA266=2,$P266>$K266,$K266>0),$X266,$Y266)+9,$W266+1))/1000","v":0},null,{"$f":"(IF(AA266=0,IF(OR($Q266=\"NO_CHANGE\",$AN266=1),1-$R266,2),0)*$P266*$N266*IF(AND($AA266=0,$AL266=1,$O266=1,$R266>0,$J266>0,$M266=0),$R266,$O266)+IF(AA266>0,1,IF(OR($L266=\"NO_CHANGE\",$AM266=1),1-$M266,2))*$K266*$I266*IF(AND($AL266=1,$O266=1,$AA266=2),MIN($J266,$R266),IF(AND($AL266=1,$AA266=0,$J266=1,$M266>0,$O266>0,$R266=0),$M266,$J266)))*IF($F266>0,IF(INT($E266/$F266)>0,($E266/$F266)+MOD($E266,$F266),$E266),$E266)*$H266*OFFSET(FANOUT,5,13)","v":0},null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,{"$f":"(VCCINT/1000)*VCCINT_N*($AE267+$AG267+($AD267+$AJ267)*$AE$1)*IF(AND($AA267<>1,$A267<>1),OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),3),1)*$AC$1","v":0},0,5,5,2,2,{"$f":"IF(($G267=\"RAMB18\")+($G267=\"RAMB18SDP\")+($G267=\"FIFO18\")+($G267=\"FIFO18_36\"),INT(($E267+1)/2),IF(($G267=\"CASC (pair)\"),2*$E267,$E267))","v":0},{"$f":"IF(($G267=\"RAMB18\")+($G267=\"RAMB36\")+($G267=\"CASC (pair)\"),0,IF(ISERR(FIND(\"SDP\", $G267)),1,2))","v":0},{"$f":"IF(LEN($G267)=0,\"AI1:AI1\",IF($G267=\"RAMB18\",\"AI1:AI6\",IF($G267=\"RAMB36\",\"AI1:AI7\",IF($G267=\"FIFO18\",\"AI4:AI7\",IF($G267=\"FIFO36\",\"AI4:AI8\",IF(G267=\"RAMB18SDP\",IF(P267<$AI$7,\"AI7\",\"AI2:AI7\"),IF(($G267=\"FIFO18_36\")+(G267=\"RAMB18SDP\"),\"AI1:AI7\",IF($G267=\"CASC (pair)\",\"AI2\",IF(OR(RIGHT(G267,3)=\"ECC\",LEFT(G267,13)=\"RAMB36SDP_ECC\"),\"AI9\",IF(G267=\"RAMB36SDP\",IF(P267<$AI$8,\"AI8\",\"AI2:AI8\"),\"AI8\"))))))))))","v":"AI1:AI6"},{"$f":"IF(LEFT($G267,4)=\"FIFO\",\"AJ1\",IF((LEN($G267)>8)*(MID($G267,7,3)=\"SDP\"),\"AJ2:AJ4\",\"AJ2:AJ4\"))","v":"AJ2:AJ4"},{"$f":"$Z267*4*($I267+$N267)*OFFSET(CLOCK_DATA,5,4)","v":0},0,0,0,0,null,0,null,{"$f":"IF(AND($AA267<>1,$AD$1>0,$A267<>1),1,0)","v":1},0,0,{"$f":"IF(LEN($G267)=0,\"AI1:AI1\",IF($G267=\"RAMB18\",\"AI1:AI6\",IF($G267=\"RAMB36\",\"AI1:AI7\",IF($G267=\"FIFO18\",\"AI4:AI7\",IF($G267=\"FIFO36\",\"AI4:AI8\",IF(G267=\"RAMB18SDP\",IF(K267<$AI$7,\"AI7\",\"AI2:AI7\"),IF(($G267=\"FIFO18_36\")+(G267=\"RAMB18SDP\"),\"AI1:AI7\",IF($G267=\"CASC (pair)\",\"AI2\",IF(OR(RIGHT(G267,3)=\"ECC\",LEFT(G267,13)=\"RAMB36SDP_ECC\"),\"AI9\",IF(G267=\"RAMB36SDP\",IF(K267<$AI$8,\"AI8\",\"AI2:AI8\"),\"AI8\"))))))))))","v":"AI1:AI6"},{"$f":"IF($G267=\"RAMB18SDP\",3,IF(LEFT($G267,9)=\"RAMB36SDP\",4,IF(LEFT($G267,6)=\"FIFO18\",5,IF(LEFT($G267,6)=\"FIFO36\",6,IF(LEFT($G267,6)=\"RAMB36\",2,1)))))","v":1},{"$f":"IF($F267>0,IF(INT($E267/$F267)>0,($E267-MOD($E267,$F267))/($F267),$E267),$E267)","v":0},{"$f":"IF(AND($AQ267>0,$E267>$AQ267),$E267-$AQ267,0)","v":0}]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,{"$f":"IF(AND($AL268=1,OR($AA268=2,$R268=0,$M268=0),$I268<>$N268),1,0)","v":0},0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,{"$f":"IF(AND($AL288=1,OR($AA288=2,$R288=0,$M288=0),$I288<>$N288),1,0)","v":0},0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,{"$f":"IF(AND($AL308=1,OR($AA308=2,$R308=0,$M308=0),$I308<>$N308),1,0)","v":0},0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,{"$f":"IF(AND($AL329=1,OR($AA329=2,$R329=0,$M329=0),$I329<>$N329),1,0)","v":0},0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,{"$f":"VCCBRAM/1000*(VCCBRAM/0.95)*($AF330+$AH330)*IF(AND($AA330<>1,$A330<>1),$AB$1,1)*$AC$1","v":0},{"$f":"IF(LEN($G330)=0,0,MATCH(IF((LEFT($G330,4)=\"RAMB\")+($G330=\"CASC (pair)\"),$G330 & IF($AM330=1,\"NO_CHANGE\",$L330),IF(AND($I330<>$N330,OR($G330=\"FIFO18\",$G330=\"FIFO36\")),\"ASYNC_\" & $G330,$G330)),BRAM_MODE_LIST,FALSE))","v":5},{"$f":"IF(LEN($G330)=0,0,MATCH(IF((LEFT($G330,4)=\"RAMB\")+($G330=\"CASC (pair)\"),$G330 &  IF($AN330=1,\"NO_CHANGE\",$Q330),IF(AND($I330<>$N330,OR($G330=\"FIFO18\",$G330=\"FIFO36\")),\"ASYNC_\" & $G330,$G330)),BRAM_MODE_LIST,FALSE))","v":5},{"$f":"MATCH(IF(K330=64,72,K330),BRAM_WIDTH_LIST,FALSE)","v":2},{"$f":"MATCH(IF(P330=64,72,P330),BRAM_WIDTH_LIST,FALSE)","v":2},0,0,"AI1:AI6","AJ2:AJ4",0,{"$f":"($AQ330*MIN(1,LN(1+$H330*5 + 1.33))*(($I330*IF(AND($AL330=1,$O330=1,$AA330=2),MIN($J330,$J330),IF(AND($AL330=1,$J330=1,$M330>0,$O330>0,$R330=0),$M330,$J330))*IF($AA330=0,(1-$M330),1)*OFFSET(BRAM_TABLE,$X330,$V330)) + ($I330*IF(AND($AL330=1,$O330=1,$AA330=2),MIN($J330,$R330),IF(AND($AL330=1,$J330=1,$M330>0,$O330>0,$R330=0),$M330,$J330))*IF($AA330=0,$M330,0)*OFFSET(BRAM_TABLE,$X330,$V330+1)))+($AR330 + $AQ330 *(1-$J330))*$I330*(OFFSET(BRAM_TABLE,$AP330,68) +OFFSET(BRAM_TABLE,$AP330,68+1)))/1000","v":0},{"$f":"$AQ330*0.7*(($I330*IF(AND($AL330=1,$O330=1,$AA330=2),MIN($J330,$J330),IF(AND($AL330=1,$J330=1,$M330>0,$O330>0,$R330=0),$M330,$J330))*IF($AA330=0,(1-$M330),1))*OFFSET(BRAM_TABLE,IF(AND($AA330=2,$K330>$P330,$P330>0),$Y330,$X330)+9,$V330) + ($I330*IF(AND($AL330=1,$O330=1,$AA330=2),MIN($J330,$R330),IF(AND($AL330=1,$J330=1,$M330>0,$O330>0,$R330=0),$M330,$J330))*IF($AA330=0,$M330,0))*OFFSET(BRAM_TABLE,IF(AND($AA330=2,$K330>$P330,$P330>0),$Y330,$X330)+9,$V330+1))/1000","v":0},{"$f":"($AQ330*MIN(1,LN(1+$H330*5+1.33))*($N330*IF(AND($AA330=0,$AL330=1,$O330=1,$R330>0,$J330>0,$M330=0),$R330,$O330)*IF($AA330=0,1-$R330,0)*OFFSET(BRAM_TABLE,$Y330,$W330)+($N330*IF(AND($AA330=0,$AL330=1,$O330=1,$R330>0,$J330>0,$M330=0),$R330,$O330)*$R330)*OFFSET(BRAM_TABLE,$Y330,$W330+1))+($AR330 + $AQ330 *(1-$O330))*$N330*(OFFSET(BRAM_TABLE,$AP330,68) +OFFSET(BRAM_TABLE,$AP330,68+1)))/1000","v":0},{"$f":"$AQ330*0.7*($N330*IF(AND($AA330=0,$AL330=1,$O330=1,$R330>0,$J330>0,$M330=0),$R330,$O330)*IF($AA330=0,1-$R330,0)*OFFSET(BRAM_TABLE,IF(AND($AA330=2,$P330>$K330,$K330>0),$X330,$Y330)+9,$W330)+$R330*$N330*IF(AND($AA330=0,$AL330=1,$O330=1,$R330>0,$J330>0,$M330=0),$R330,$O330)*OFFSET(BRAM_TABLE,IF(AND($AA330=2,$P330>$K330,$K330>0),$X330,$Y330)+9,$W330+1))/1000","v":0},null,{"$f":"(IF(AA330=0,IF(OR($Q330=\"NO_CHANGE\",$AN330=1),1-$R330,2),0)*$P330*$N330*IF(AND($AA330=0,$AL330=1,$O330=1,$R330>0,$J330>0,$M330=0),$R330,$O330)+IF(AA330>0,1,IF(OR($L330=\"NO_CHANGE\",$AM330=1),1-$M330,2))*$K330*$I330*IF(AND($AL330=1,$O330=1,$AA330=2),MIN($J330,$R330),IF(AND($AL330=1,$AA330=0,$J330=1,$M330>0,$O330>0,$R330=0),$M330,$J330)))*IF($F330>0,IF(INT($E330/$F330)>0,($E330/$F330)+MOD($E330,$F330),$E330),$E330)*$H330*OFFSET(FANOUT,5,13)","v":0},null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,{"$f":"(VCCINT/1000)*VCCINT_N*($AE331+$AG331+($AD331+$AJ331)*$AE$1)*IF(AND($AA331<>1,$A331<>1),OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),3),1)*$AC$1","v":0},0,5,5,2,2,{"$f":"IF(($G331=\"RAMB18\")+($G331=\"RAMB18SDP\")+($G331=\"FIFO18\")+($G331=\"FIFO18_36\"),INT(($E331+1)/2),IF(($G331=\"CASC (pair)\"),2*$E331,$E331))","v":0},{"$f":"IF(($G331=\"RAMB18\")+($G331=\"RAMB36\")+($G331=\"CASC (pair)\"),0,IF(ISERR(FIND(\"SDP\", $G331)),1,2))","v":0},{"$f":"IF(LEN($G331)=0,\"AI1:AI1\",IF($G331=\"RAMB18\",\"AI1:AI6\",IF($G331=\"RAMB36\",\"AI1:AI7\",IF($G331=\"FIFO18\",\"AI4:AI7\",IF($G331=\"FIFO36\",\"AI4:AI8\",IF(G331=\"RAMB18SDP\",IF(P331<$AI$7,\"AI7\",\"AI2:AI7\"),IF(($G331=\"FIFO18_36\")+(G331=\"RAMB18SDP\"),\"AI1:AI7\",IF($G331=\"CASC (pair)\",\"AI2\",IF(OR(RIGHT(G331,3)=\"ECC\",LEFT(G331,13)=\"RAMB36SDP_ECC\"),\"AI9\",IF(G331=\"RAMB36SDP\",IF(P331<$AI$8,\"AI8\",\"AI2:AI8\"),\"AI8\"))))))))))","v":"AI1:AI6"},{"$f":"IF(LEFT($G331,4)=\"FIFO\",\"AJ1\",IF((LEN($G331)>8)*(MID($G331,7,3)=\"SDP\"),\"AJ2:AJ4\",\"AJ2:AJ4\"))","v":"AJ2:AJ4"},{"$f":"$Z331*4*($I331+$N331)*OFFSET(CLOCK_DATA,5,4)","v":0},0,0,0,0,null,0,null,{"$f":"IF(AND($AA331<>1,$AD$1>0,$A331<>1),1,0)","v":1},0,0,{"$f":"IF(LEN($G331)=0,\"AI1:AI1\",IF($G331=\"RAMB18\",\"AI1:AI6\",IF($G331=\"RAMB36\",\"AI1:AI7\",IF($G331=\"FIFO18\",\"AI4:AI7\",IF($G331=\"FIFO36\",\"AI4:AI8\",IF(G331=\"RAMB18SDP\",IF(K331<$AI$7,\"AI7\",\"AI2:AI7\"),IF(($G331=\"FIFO18_36\")+(G331=\"RAMB18SDP\"),\"AI1:AI7\",IF($G331=\"CASC (pair)\",\"AI2\",IF(OR(RIGHT(G331,3)=\"ECC\",LEFT(G331,13)=\"RAMB36SDP_ECC\"),\"AI9\",IF(G331=\"RAMB36SDP\",IF(K331<$AI$8,\"AI8\",\"AI2:AI8\"),\"AI8\"))))))))))","v":"AI1:AI6"},{"$f":"IF($G331=\"RAMB18SDP\",3,IF(LEFT($G331,9)=\"RAMB36SDP\",4,IF(LEFT($G331,6)=\"FIFO18\",5,IF(LEFT($G331,6)=\"FIFO36\",6,IF(LEFT($G331,6)=\"RAMB36\",2,1)))))","v":1},{"$f":"IF($F331>0,IF(INT($E331/$F331)>0,($E331-MOD($E331,$F331))/($F331),$E331),$E331)","v":0},{"$f":"IF(AND($AQ331>0,$E331>$AQ331),$E331-$AQ331,0)","v":0}]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,{"$f":"IF((AE341+AG341)<=0,0,((IF($AG341>0,$P341+8,0)*$N341*IF(AND($AA341=0,$AL341=1,$O341=1,$R341>0,$J341>0,$M341=0),$R341,$O341)+IF($AE341>0,$K341+8,0)*$I341*IF(AND($AL341=1,$O341=1,$AA341=2),MIN($J341,$R341),IF(AND($J341=1,$M341>0,$O341>0,$R341=0),$M341,$J341)))*$H341/(IF($AG341>0,$P341+8,0)+IF($AE341>0,$K341+8,0))))","v":0},0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,{"$f":"IF(AND($AL349=1,OR($AA349=2,$R349=0,$M349=0),$I349<>$N349),1,0)","v":0},0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,{"$f":"IF(AND($AL369=1,OR($AA369=2,$R369=0,$M369=0),$I369<>$N369),1,0)","v":0},0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,{"$f":"IF((AE373+AG373)<=0,0,((IF($AG373>0,$P373+8,0)*$N373*IF(AND($AA373=0,$AL373=1,$O373=1,$R373>0,$J373>0,$M373=0),$R373,$O373)+IF($AE373>0,$K373+8,0)*$I373*IF(AND($AL373=1,$O373=1,$AA373=2),MIN($J373,$R373),IF(AND($J373=1,$M373>0,$O373>0,$R373=0),$M373,$J373)))*$H373/(IF($AG373>0,$P373+8,0)+IF($AE373>0,$K373+8,0))))","v":0},0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,{"$f":"IF(AND($AL389=1,OR($AA389=2,$R389=0,$M389=0),$I389<>$N389),1,0)","v":0},0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,{"$f":"VCCBRAM/1000*(VCCBRAM/0.95)*($AF394+$AH394)*IF(AND($AA394<>1,$A394<>1),$AB$1,1)*$AC$1","v":0},{"$f":"IF(LEN($G394)=0,0,MATCH(IF((LEFT($G394,4)=\"RAMB\")+($G394=\"CASC (pair)\"),$G394 & IF($AM394=1,\"NO_CHANGE\",$L394),IF(AND($I394<>$N394,OR($G394=\"FIFO18\",$G394=\"FIFO36\")),\"ASYNC_\" & $G394,$G394)),BRAM_MODE_LIST,FALSE))","v":5},{"$f":"IF(LEN($G394)=0,0,MATCH(IF((LEFT($G394,4)=\"RAMB\")+($G394=\"CASC (pair)\"),$G394 &  IF($AN394=1,\"NO_CHANGE\",$Q394),IF(AND($I394<>$N394,OR($G394=\"FIFO18\",$G394=\"FIFO36\")),\"ASYNC_\" & $G394,$G394)),BRAM_MODE_LIST,FALSE))","v":5},{"$f":"MATCH(IF(K394=64,72,K394),BRAM_WIDTH_LIST,FALSE)","v":2},{"$f":"MATCH(IF(P394=64,72,P394),BRAM_WIDTH_LIST,FALSE)","v":2},0,0,"AI1:AI6","AJ2:AJ4",0,{"$f":"($AQ394*MIN(1,LN(1+$H394*5 + 1.33))*(($I394*IF(AND($AL394=1,$O394=1,$AA394=2),MIN($J394,$J394),IF(AND($AL394=1,$J394=1,$M394>0,$O394>0,$R394=0),$M394,$J394))*IF($AA394=0,(1-$M394),1)*OFFSET(BRAM_TABLE,$X394,$V394)) + ($I394*IF(AND($AL394=1,$O394=1,$AA394=2),MIN($J394,$R394),IF(AND($AL394=1,$J394=1,$M394>0,$O394>0,$R394=0),$M394,$J394))*IF($AA394=0,$M394,0)*OFFSET(BRAM_TABLE,$X394,$V394+1)))+($AR394 + $AQ394 *(1-$J394))*$I394*(OFFSET(BRAM_TABLE,$AP394,68) +OFFSET(BRAM_TABLE,$AP394,68+1)))/1000","v":0},{"$f":"$AQ394*0.7*(($I394*IF(AND($AL394=1,$O394=1,$AA394=2),MIN($J394,$J394),IF(AND($AL394=1,$J394=1,$M394>0,$O394>0,$R394=0),$M394,$J394))*IF($AA394=0,(1-$M394),1))*OFFSET(BRAM_TABLE,IF(AND($AA394=2,$K394>$P394,$P394>0),$Y394,$X394)+9,$V394) + ($I394*IF(AND($AL394=1,$O394=1,$AA394=2),MIN($J394,$R394),IF(AND($AL394=1,$J394=1,$M394>0,$O394>0,$R394=0),$M394,$J394))*IF($AA394=0,$M394,0))*OFFSET(BRAM_TABLE,IF(AND($AA394=2,$K394>$P394,$P394>0),$Y394,$X394)+9,$V394+1))/1000","v":0},{"$f":"($AQ394*MIN(1,LN(1+$H394*5+1.33))*($N394*IF(AND($AA394=0,$AL394=1,$O394=1,$R394>0,$J394>0,$M394=0),$R394,$O394)*IF($AA394=0,1-$R394,0)*OFFSET(BRAM_TABLE,$Y394,$W394)+($N394*IF(AND($AA394=0,$AL394=1,$O394=1,$R394>0,$J394>0,$M394=0),$R394,$O394)*$R394)*OFFSET(BRAM_TABLE,$Y394,$W394+1))+($AR394 + $AQ394 *(1-$O394))*$N394*(OFFSET(BRAM_TABLE,$AP394,68) +OFFSET(BRAM_TABLE,$AP394,68+1)))/1000","v":0},{"$f":"$AQ394*0.7*($N394*IF(AND($AA394=0,$AL394=1,$O394=1,$R394>0,$J394>0,$M394=0),$R394,$O394)*IF($AA394=0,1-$R394,0)*OFFSET(BRAM_TABLE,IF(AND($AA394=2,$P394>$K394,$K394>0),$X394,$Y394)+9,$W394)+$R394*$N394*IF(AND($AA394=0,$AL394=1,$O394=1,$R394>0,$J394>0,$M394=0),$R394,$O394)*OFFSET(BRAM_TABLE,IF(AND($AA394=2,$P394>$K394,$K394>0),$X394,$Y394)+9,$W394+1))/1000","v":0},null,{"$f":"(IF(AA394=0,IF(OR($Q394=\"NO_CHANGE\",$AN394=1),1-$R394,2),0)*$P394*$N394*IF(AND($AA394=0,$AL394=1,$O394=1,$R394>0,$J394>0,$M394=0),$R394,$O394)+IF(AA394>0,1,IF(OR($L394=\"NO_CHANGE\",$AM394=1),1-$M394,2))*$K394*$I394*IF(AND($AL394=1,$O394=1,$AA394=2),MIN($J394,$R394),IF(AND($AL394=1,$AA394=0,$J394=1,$M394>0,$O394>0,$R394=0),$M394,$J394)))*IF($F394>0,IF(INT($E394/$F394)>0,($E394/$F394)+MOD($E394,$F394),$E394),$E394)*$H394*OFFSET(FANOUT,5,13)","v":0},null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,{"$f":"(VCCINT/1000)*VCCINT_N*($AE395+$AG395+($AD395+$AJ395)*$AE$1)*IF(AND($AA395<>1,$A395<>1),OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),3),1)*$AC$1","v":0},0,5,5,2,2,{"$f":"IF(($G395=\"RAMB18\")+($G395=\"RAMB18SDP\")+($G395=\"FIFO18\")+($G395=\"FIFO18_36\"),INT(($E395+1)/2),IF(($G395=\"CASC (pair)\"),2*$E395,$E395))","v":0},{"$f":"IF(($G395=\"RAMB18\")+($G395=\"RAMB36\")+($G395=\"CASC (pair)\"),0,IF(ISERR(FIND(\"SDP\", $G395)),1,2))","v":0},{"$f":"IF(LEN($G395)=0,\"AI1:AI1\",IF($G395=\"RAMB18\",\"AI1:AI6\",IF($G395=\"RAMB36\",\"AI1:AI7\",IF($G395=\"FIFO18\",\"AI4:AI7\",IF($G395=\"FIFO36\",\"AI4:AI8\",IF(G395=\"RAMB18SDP\",IF(P395<$AI$7,\"AI7\",\"AI2:AI7\"),IF(($G395=\"FIFO18_36\")+(G395=\"RAMB18SDP\"),\"AI1:AI7\",IF($G395=\"CASC (pair)\",\"AI2\",IF(OR(RIGHT(G395,3)=\"ECC\",LEFT(G395,13)=\"RAMB36SDP_ECC\"),\"AI9\",IF(G395=\"RAMB36SDP\",IF(P395<$AI$8,\"AI8\",\"AI2:AI8\"),\"AI8\"))))))))))","v":"AI1:AI6"},{"$f":"IF(LEFT($G395,4)=\"FIFO\",\"AJ1\",IF((LEN($G395)>8)*(MID($G395,7,3)=\"SDP\"),\"AJ2:AJ4\",\"AJ2:AJ4\"))","v":"AJ2:AJ4"},{"$f":"$Z395*4*($I395+$N395)*OFFSET(CLOCK_DATA,5,4)","v":0},0,0,0,0,null,0,null,{"$f":"IF(AND($AA395<>1,$AD$1>0,$A395<>1),1,0)","v":1},0,0,{"$f":"IF(LEN($G395)=0,\"AI1:AI1\",IF($G395=\"RAMB18\",\"AI1:AI6\",IF($G395=\"RAMB36\",\"AI1:AI7\",IF($G395=\"FIFO18\",\"AI4:AI7\",IF($G395=\"FIFO36\",\"AI4:AI8\",IF(G395=\"RAMB18SDP\",IF(K395<$AI$7,\"AI7\",\"AI2:AI7\"),IF(($G395=\"FIFO18_36\")+(G395=\"RAMB18SDP\"),\"AI1:AI7\",IF($G395=\"CASC (pair)\",\"AI2\",IF(OR(RIGHT(G395,3)=\"ECC\",LEFT(G395,13)=\"RAMB36SDP_ECC\"),\"AI9\",IF(G395=\"RAMB36SDP\",IF(K395<$AI$8,\"AI8\",\"AI2:AI8\"),\"AI8\"))))))))))","v":"AI1:AI6"},{"$f":"IF($G395=\"RAMB18SDP\",3,IF(LEFT($G395,9)=\"RAMB36SDP\",4,IF(LEFT($G395,6)=\"FIFO18\",5,IF(LEFT($G395,6)=\"FIFO36\",6,IF(LEFT($G395,6)=\"RAMB36\",2,1)))))","v":1},{"$f":"IF($F395>0,IF(INT($E395/$F395)>0,($E395-MOD($E395,$F395))/($F395),$E395),$E395)","v":0},{"$f":"IF(AND($AQ395>0,$E395>$AQ395),$E395-$AQ395,0)","v":0}]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,{"$f":"IF((AE405+AG405)<=0,0,((IF($AG405>0,$P405+8,0)*$N405*IF(AND($AA405=0,$AL405=1,$O405=1,$R405>0,$J405>0,$M405=0),$R405,$O405)+IF($AE405>0,$K405+8,0)*$I405*IF(AND($AL405=1,$O405=1,$AA405=2),MIN($J405,$R405),IF(AND($J405=1,$M405>0,$O405>0,$R405=0),$M405,$J405)))*$H405/(IF($AG405>0,$P405+8,0)+IF($AE405>0,$K405+8,0))))","v":0},0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,{"$f":"IF(AND($AL409=1,OR($AA409=2,$R409=0,$M409=0),$I409<>$N409),1,0)","v":0},0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,{"$f":"IF(AND($AL429=1,OR($AA429=2,$R429=0,$M429=0),$I429<>$N429),1,0)","v":0},0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,{"$f":"IF((AE437+AG437)<=0,0,((IF($AG437>0,$P437+8,0)*$N437*IF(AND($AA437=0,$AL437=1,$O437=1,$R437>0,$J437>0,$M437=0),$R437,$O437)+IF($AE437>0,$K437+8,0)*$I437*IF(AND($AL437=1,$O437=1,$AA437=2),MIN($J437,$R437),IF(AND($J437=1,$M437>0,$O437>0,$R437=0),$M437,$J437)))*$H437/(IF($AG437>0,$P437+8,0)+IF($AE437>0,$K437+8,0))))","v":0},0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,{"$f":"IF(AND($AL449=1,OR($AA449=2,$R449=0,$M449=0),$I449<>$N449),1,0)","v":0},0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,{"$f":"VCCBRAM/1000*(VCCBRAM/0.95)*($AF458+$AH458)*IF(AND($AA458<>1,$A458<>1),$AB$1,1)*$AC$1","v":0},{"$f":"IF(LEN($G458)=0,0,MATCH(IF((LEFT($G458,4)=\"RAMB\")+($G458=\"CASC (pair)\"),$G458 & IF($AM458=1,\"NO_CHANGE\",$L458),IF(AND($I458<>$N458,OR($G458=\"FIFO18\",$G458=\"FIFO36\")),\"ASYNC_\" & $G458,$G458)),BRAM_MODE_LIST,FALSE))","v":5},{"$f":"IF(LEN($G458)=0,0,MATCH(IF((LEFT($G458,4)=\"RAMB\")+($G458=\"CASC (pair)\"),$G458 &  IF($AN458=1,\"NO_CHANGE\",$Q458),IF(AND($I458<>$N458,OR($G458=\"FIFO18\",$G458=\"FIFO36\")),\"ASYNC_\" & $G458,$G458)),BRAM_MODE_LIST,FALSE))","v":5},{"$f":"MATCH(IF(K458=64,72,K458),BRAM_WIDTH_LIST,FALSE)","v":2},{"$f":"MATCH(IF(P458=64,72,P458),BRAM_WIDTH_LIST,FALSE)","v":2},0,0,"AI1:AI6","AJ2:AJ4",0,{"$f":"($AQ458*MIN(1,LN(1+$H458*5 + 1.33))*(($I458*IF(AND($AL458=1,$O458=1,$AA458=2),MIN($J458,$J458),IF(AND($AL458=1,$J458=1,$M458>0,$O458>0,$R458=0),$M458,$J458))*IF($AA458=0,(1-$M458),1)*OFFSET(BRAM_TABLE,$X458,$V458)) + ($I458*IF(AND($AL458=1,$O458=1,$AA458=2),MIN($J458,$R458),IF(AND($AL458=1,$J458=1,$M458>0,$O458>0,$R458=0),$M458,$J458))*IF($AA458=0,$M458,0)*OFFSET(BRAM_TABLE,$X458,$V458+1)))+($AR458 + $AQ458 *(1-$J458))*$I458*(OFFSET(BRAM_TABLE,$AP458,68) +OFFSET(BRAM_TABLE,$AP458,68+1)))/1000","v":0},{"$f":"$AQ458*0.7*(($I458*IF(AND($AL458=1,$O458=1,$AA458=2),MIN($J458,$J458),IF(AND($AL458=1,$J458=1,$M458>0,$O458>0,$R458=0),$M458,$J458))*IF($AA458=0,(1-$M458),1))*OFFSET(BRAM_TABLE,IF(AND($AA458=2,$K458>$P458,$P458>0),$Y458,$X458)+9,$V458) + ($I458*IF(AND($AL458=1,$O458=1,$AA458=2),MIN($J458,$R458),IF(AND($AL458=1,$J458=1,$M458>0,$O458>0,$R458=0),$M458,$J458))*IF($AA458=0,$M458,0))*OFFSET(BRAM_TABLE,IF(AND($AA458=2,$K458>$P458,$P458>0),$Y458,$X458)+9,$V458+1))/1000","v":0},{"$f":"($AQ458*MIN(1,LN(1+$H458*5+1.33))*($N458*IF(AND($AA458=0,$AL458=1,$O458=1,$R458>0,$J458>0,$M458=0),$R458,$O458)*IF($AA458=0,1-$R458,0)*OFFSET(BRAM_TABLE,$Y458,$W458)+($N458*IF(AND($AA458=0,$AL458=1,$O458=1,$R458>0,$J458>0,$M458=0),$R458,$O458)*$R458)*OFFSET(BRAM_TABLE,$Y458,$W458+1))+($AR458 + $AQ458 *(1-$O458))*$N458*(OFFSET(BRAM_TABLE,$AP458,68) +OFFSET(BRAM_TABLE,$AP458,68+1)))/1000","v":0},{"$f":"$AQ458*0.7*($N458*IF(AND($AA458=0,$AL458=1,$O458=1,$R458>0,$J458>0,$M458=0),$R458,$O458)*IF($AA458=0,1-$R458,0)*OFFSET(BRAM_TABLE,IF(AND($AA458=2,$P458>$K458,$K458>0),$X458,$Y458)+9,$W458)+$R458*$N458*IF(AND($AA458=0,$AL458=1,$O458=1,$R458>0,$J458>0,$M458=0),$R458,$O458)*OFFSET(BRAM_TABLE,IF(AND($AA458=2,$P458>$K458,$K458>0),$X458,$Y458)+9,$W458+1))/1000","v":0},null,{"$f":"(IF(AA458=0,IF(OR($Q458=\"NO_CHANGE\",$AN458=1),1-$R458,2),0)*$P458*$N458*IF(AND($AA458=0,$AL458=1,$O458=1,$R458>0,$J458>0,$M458=0),$R458,$O458)+IF(AA458>0,1,IF(OR($L458=\"NO_CHANGE\",$AM458=1),1-$M458,2))*$K458*$I458*IF(AND($AL458=1,$O458=1,$AA458=2),MIN($J458,$R458),IF(AND($AL458=1,$AA458=0,$J458=1,$M458>0,$O458>0,$R458=0),$M458,$J458)))*IF($F458>0,IF(INT($E458/$F458)>0,($E458/$F458)+MOD($E458,$F458),$E458),$E458)*$H458*OFFSET(FANOUT,5,13)","v":0},null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,{"$f":"(VCCINT/1000)*VCCINT_N*($AE459+$AG459+($AD459+$AJ459)*$AE$1)*IF(AND($AA459<>1,$A459<>1),OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),3),1)*$AC$1","v":0},0,5,5,2,2,{"$f":"IF(($G459=\"RAMB18\")+($G459=\"RAMB18SDP\")+($G459=\"FIFO18\")+($G459=\"FIFO18_36\"),INT(($E459+1)/2),IF(($G459=\"CASC (pair)\"),2*$E459,$E459))","v":0},{"$f":"IF(($G459=\"RAMB18\")+($G459=\"RAMB36\")+($G459=\"CASC (pair)\"),0,IF(ISERR(FIND(\"SDP\", $G459)),1,2))","v":0},{"$f":"IF(LEN($G459)=0,\"AI1:AI1\",IF($G459=\"RAMB18\",\"AI1:AI6\",IF($G459=\"RAMB36\",\"AI1:AI7\",IF($G459=\"FIFO18\",\"AI4:AI7\",IF($G459=\"FIFO36\",\"AI4:AI8\",IF(G459=\"RAMB18SDP\",IF(P459<$AI$7,\"AI7\",\"AI2:AI7\"),IF(($G459=\"FIFO18_36\")+(G459=\"RAMB18SDP\"),\"AI1:AI7\",IF($G459=\"CASC (pair)\",\"AI2\",IF(OR(RIGHT(G459,3)=\"ECC\",LEFT(G459,13)=\"RAMB36SDP_ECC\"),\"AI9\",IF(G459=\"RAMB36SDP\",IF(P459<$AI$8,\"AI8\",\"AI2:AI8\"),\"AI8\"))))))))))","v":"AI1:AI6"},{"$f":"IF(LEFT($G459,4)=\"FIFO\",\"AJ1\",IF((LEN($G459)>8)*(MID($G459,7,3)=\"SDP\"),\"AJ2:AJ4\",\"AJ2:AJ4\"))","v":"AJ2:AJ4"},{"$f":"$Z459*4*($I459+$N459)*OFFSET(CLOCK_DATA,5,4)","v":0},0,0,0,0,null,0,null,{"$f":"IF(AND($AA459<>1,$AD$1>0,$A459<>1),1,0)","v":1},0,0,{"$f":"IF(LEN($G459)=0,\"AI1:AI1\",IF($G459=\"RAMB18\",\"AI1:AI6\",IF($G459=\"RAMB36\",\"AI1:AI7\",IF($G459=\"FIFO18\",\"AI4:AI7\",IF($G459=\"FIFO36\",\"AI4:AI8\",IF(G459=\"RAMB18SDP\",IF(K459<$AI$7,\"AI7\",\"AI2:AI7\"),IF(($G459=\"FIFO18_36\")+(G459=\"RAMB18SDP\"),\"AI1:AI7\",IF($G459=\"CASC (pair)\",\"AI2\",IF(OR(RIGHT(G459,3)=\"ECC\",LEFT(G459,13)=\"RAMB36SDP_ECC\"),\"AI9\",IF(G459=\"RAMB36SDP\",IF(K459<$AI$8,\"AI8\",\"AI2:AI8\"),\"AI8\"))))))))))","v":"AI1:AI6"},{"$f":"IF($G459=\"RAMB18SDP\",3,IF(LEFT($G459,9)=\"RAMB36SDP\",4,IF(LEFT($G459,6)=\"FIFO18\",5,IF(LEFT($G459,6)=\"FIFO36\",6,IF(LEFT($G459,6)=\"RAMB36\",2,1)))))","v":1},{"$f":"IF($F459>0,IF(INT($E459/$F459)>0,($E459-MOD($E459,$F459))/($F459),$E459),$E459)","v":0},{"$f":"IF(AND($AQ459>0,$E459>$AQ459),$E459-$AQ459,0)","v":0}]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,{"$f":"IF((AE469+AG469)<=0,0,((IF($AG469>0,$P469+8,0)*$N469*IF(AND($AA469=0,$AL469=1,$O469=1,$R469>0,$J469>0,$M469=0),$R469,$O469)+IF($AE469>0,$K469+8,0)*$I469*IF(AND($AL469=1,$O469=1,$AA469=2),MIN($J469,$R469),IF(AND($J469=1,$M469>0,$O469>0,$R469=0),$M469,$J469)))*$H469/(IF($AG469>0,$P469+8,0)+IF($AE469>0,$K469+8,0))))","v":0},0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,{"$f":"IF(AND($AL469=1,OR($AA469=2,$R469=0,$M469=0),$I469<>$N469),1,0)","v":0},0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,{"$f":"IF(AND($AL489=1,OR($AA489=2,$R489=0,$M489=0),$I489<>$N489),1,0)","v":0},0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,{"$f":"IF((AE497+AG497)<=0,0,((IF($AG497>0,$P497+8,0)*$N497*IF(AND($AA497=0,$AL497=1,$O497=1,$R497>0,$J497>0,$M497=0),$R497,$O497)+IF($AE497>0,$K497+8,0)*$I497*IF(AND($AL497=1,$O497=1,$AA497=2),MIN($J497,$R497),IF(AND($J497=1,$M497>0,$O497>0,$R497=0),$M497,$J497)))*$H497/(IF($AG497>0,$P497+8,0)+IF($AE497>0,$K497+8,0))))","v":0},0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,null,null,null,null,4,"RAMB18",0.125,null,0.25,1,"NO_CHANGE",0.5,null,0.25,1,"NO_CHANGE",0.5,0,0,0,5,5,2,2,0,0,"AI1:AI6","AJ2:AJ4",0,0,0,0,0,null,0,null,1,0,0,"AI1:AI6",1,0,0]
[null,{"$f":"ROW(BRAMROWS)-10","v":491},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND($Z501<>1,$A$1<>1),1,0)","v":1},{"$f":"IF(AND($AJ501=1,OR($Z501=2,$Q501=0,$L501=0),$H501<>$M501),1,0)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(VCCINT/1000)*VCCINT_N*(SUM(AJ10:AJ500))*IF(AND($AA500<>1,$A500<>1),OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),3),1)*$AC$1","v":8.0711739224999975E-3}]

{"sheet":"DSP","index":8,"n_rows":502,"n_cols":32,"rows_kept":502,"cut":false,"hidden":false,"merged":[[352,1,352,3],[353,1,353,3],[354,1,354,3],[355,1,355,3],[356,1,356,3],[347,1,347,3],[348,1,348,3],[349,1,349,3],[350,1,350,3],[351,1,351,3],[342,1,342,3],[343,1,343,3],[344,1,344,3],[345,1,345,3],[346,1,346,3],[337,1,337,3],[338,1,338,3],[339,1,339,3],[340,1,340,3],[341,1,341,3],[332,1,332,3],[333,1,333,3],[334,1,334,3],[335,1,335,3],[336,1,336,3],[327,1,327,3],[328,1,328,3],[329,1,329,3],[330,1,330,3],[331,1,331,3],[322,1,322,3],[323,1,323,3],[324,1,324,3],[325,1,325,3],[326,1,326,3],[317,1,317,3],[318,1,318,3],[319,1,319,3],[320,1,320,3],[321,1,321,3],[312,1,312,3],[313,1,313,3],[314,1,314,3],[315,1,315,3],[316,1,316,3],[307,1,307,3],[308,1,308,3],[309,1,309,3],[310,1,310,3],[311,1,311,3],[302,1,302,3],[303,1,303,3],[304,1,304,3],[305,1,305,3],[306,1,306,3],[297,1,297,3],[298,1,298,3],[299,1,299,3],[300,1,300,3],[301,1,301,3],[292,1,292,3],[293,1,293,3],[294,1,294,3],[295,1,295,3],[296,1,296,3],[287,1,287,3],[288,1,288,3],[289,1,289,3],[290,1,290,3],[291,1,291,3],[282,1,282,3],[283,1,283,3],[284,1,284,3],[285,1,285,3],[286,1,286,3],[277,1,277,3],[278,1,278,3],[279,1,279,3],[280,1,280,3],[281,1,281,3],[272,1,272,3],[273,1,273,3],[274,1,274,3],[275,1,275,3],[276,1,276,3],[267,1,267,3],[268,1,268,3],[269,1,269,3],[270,1,270,3],[271,1,271,3],[188,1,188,3],[189,1,189,3],[228,1,228,3],[229,1,229,3],[230,1,230,3],[226,1,226,3],[227,1,227,3],[221,1,221,3],[222,1,222,3],[223,1,223,3],[224,1,224,3],[225,1,225,3],[216,1,216,3],[217,1,217,3],[218,1,218,3],[219,1,219,3],[220,1,220,3],[211,1,211,3],[212,1,212,3],[195,1,195,3],[213,1,213,3],[214,1,214,3],[215,1,215,3],[206,1,206,3],[183,1,183,3],[184,1,184,3],[185,1,185,3],[186,1,186,3],[187,1,187,3],[178,1,178,3],[179,1,179,3],[180,1,180,3],[181,1,181,3],[182,1,182,3],[173,1,173,3],[174,1,174,3],[175,1,175,3],[176,1,176,3],[177,1,177,3],[168,1,168,3],[169,1,169,3],[170,1,170,3],[171,1,171,3],[172,1,172,3],[163,1,163,3],[164,1,164,3],[165,1,165,3],[166,1,166,3],[167,1,167,3],[158,1,158,3],[159,1,159,3],[160,1,160,3],[161,1,161,3],[162,1,162,3],[153,1,153,3],[154,1,154,3],[155,1,155,3],[156,1,156,3],[157,1,157,3],[148,1,148,3],[149,1,149,3],[150,1,150,3],[151,1,151,3],[152,1,152,3],[143,1,143,3],[144,1,144,3],[145,1,145,3],[146,1,146,3],[147,1,147,3],[138,1,138,3],[139,1,139,3],[140,1,140,3],[141,1,141,3],[142,1,142,3],[133,1,133,3],[134,1,134,3],[135,1,135,3],[136,1,136,3],[137,1,137,3],[128,1,128,3],[129,1,129,3],[130,1,130,3],[131,1,131,3],[132,1,132,3],[123,1,123,3],[124,1,124,3],[125,1,125,3],[126,1,126,3],[127,1,127,3],[118,1,118,3],[119,1,119,3],[120,1,120,3],[121,1,121,3],[122,1,122,3],[113,1,113,3],[114,1,114,3],[115,1,115,3],[116,1,116,3],[117,1,117,3],[108,1,108,3],[109,1,109,3],[110,1,110,3],[111,1,111,3],[112,1,112,3],[103,1,103,3],[104,1,104,3],[105,1,105,3],[106,1,106,3],[107,1,107,3],[98,1,98,3],[99,1,99,3],[100,1,100,3],[101,1,101,3],[102,1,102,3],[93,1,93,3],[94,1,94,3],[95,1,95,3],[96,1,96,3],[97,1,97,3],[88,1,88,3],[89,1,89,3],[90,1,90,3],[91,1,91,3],[92,1,92,3],[83,1,83,3],[84,1,84,3],[85,1,85,3],[86,1,86,3],[87,1,87,3],[78,1,78,3],[79,1,79,3],[80,1,80,3],[81,1,81,3],[82,1,82,3],[73,1,73,3],[74,1,74,3],[75,1,75,3],[76,1,76,3],[77,1,77,3],[68,1,68,3],[69,1,69,3],[70,1,70,3],[71,1,71,3],[72,1,72,3],[63,1,63,3],[64,1,64,3],[65,1,65,3],[66,1,66,3],[67,1,67,3],[58,1,58,3],[59,1,59,3],[60,1,60,3],[61,1,61,3],[62,1,62,3],[53,1,53,3],[54,1,54,3],[55,1,55,3],[56,1,56,3],[57,1,57,3],[48,1,48,3],[49,1,49,3],[50,1,50,3],[51,1,51,3],[52,1,52,3],[43,1,43,3],[44,1,44,3],[45,1,45,3],[46,1,46,3],[47,1,47,3],[38,1,38,3],[39,1,39,3],[40,1,40,3],[41,1,41,3],[42,1,42,3],[33,1,33,3],[34,1,34,3],[35,1,35,3],[36,1,36,3],[37,1,37,3],[28,1,28,3],[29,1,29,3],[30,1,30,3],[31,1,31,3],[32,1,32,3],[23,1,23,3],[24,1,24,3],[25,1,25,3],[26,1,26,3],[27,1,27,3],[18,1,18,3],[19,1,19,3],[20,1,20,3],[21,1,21,3],[22,1,22,3],[13,1,13,3],[14,1,14,3],[15,1,15,3],[16,1,16,3],[17,1,17,3],[8,1,8,3],[9,1,9,3],[10,1,10,3],[11,1,11,3],[12,1,12,3],[405,1,405,3],[406,1,406,3],[407,1,407,3],[408,1,408,3],[409,1,409,3],[400,1,400,3],[401,1,401,3],[402,1,402,3],[403,1,403,3],[404,1,404,3],[395,1,395,3],[396,1,396,3],[397,1,397,3],[398,1,398,3],[399,1,399,3],[390,1,390,3],[391,1,391,3],[392,1,392,3],[393,1,393,3],[394,1,394,3],[385,1,385,3],[386,1,386,3],[387,1,387,3],[388,1,388,3],[389,1,389,3],[380,1,380,3],[381,1,381,3],[382,1,382,3],[383,1,383,3],[384,1,384,3],[375,1,375,3],[376,1,376,3],[377,1,377,3],[378,1,378,3],[379,1,379,3],[370,1,370,3],[371,1,371,3],[372,1,372,3],[373,1,373,3],[374,1,374,3],[253,1,253,3],[254,1,254,3],[255,1,255,3],[256,1,256,3],[365,1,365,3],[366,1,366,3],[367,1,367,3],[368,1,368,3],[369,1,369,3],[360,1,360,3],[361,1,361,3],[362,1,362,3],[363,1,363,3],[364,1,364,3],[262,1,262,3],[263,1,263,3],[264,1,264,3],[265,1,265,3],[266,1,266,3],[257,1,257,3],[258,1,258,3],[259,1,259,3],[260,1,260,3],[261,1,261,3],[239,1,239,3],[240,1,240,3],[241,1,241,3],[242,1,242,3],[243,1,243,3],[244,1,244,3],[245,1,245,3],[246,1,246,3],[252,1,252,3],[247,1,247,3],[248,1,248,3],[249,1,249,3],[250,1,250,3],[251,1,251,3],[477,1,477,3],[478,1,478,3],[446,1,446,3],[447,1,447,3],[476,1,476,3],[473,1,473,3],[454,1,454,3],[452,1,452,3],[448,1,448,3],[449,1,449,3],[469,1,469,3],[471,1,471,3],[472,1,472,3],[474,1,474,3],[475,1,475,3],[470,1,470,3],[457,1,457,3],[450,1,450,3],[468,1,468,3],[467,1,467,3],[455,1,455,3],[466,1,466,3],[451,1,451,3],[463,1,463,3],[499,1,499,3],[494,1,494,3],[495,1,495,3],[496,1,496,3],[497,1,497,3],[498,1,498,3],[492,1,492,3],[493,1,493,3],[491,1,491,3],[489,1,489,3],[484,1,484,3],[490,1,490,3],[485,1,485,3],[488,1,488,3],[486,1,486,3],[487,1,487,3],[482,1,482,3],[479,1,479,3],[483,1,483,3],[481,1,481,3],[480,1,480,3],[456,1,456,3],[438,1,438,3],[442,1,442,3],[441,1,441,3],[443,1,443,3],[444,1,444,3],[445,1,445,3],[453,1,453,3],[460,1,460,3],[458,1,458,3],[459,1,459,3],[465,1,465,3],[462,1,462,3],[461,1,461,3],[464,1,464,3],[439,1,439,3],[440,1,440,3],[413,1,413,3],[416,1,416,3],[426,1,426,3],[427,1,427,3],[425,1,425,3],[434,1,434,3],[435,1,435,3],[437,1,437,3],[436,1,436,3],[432,1,432,3],[433,1,433,3],[431,1,431,3],[417,1,417,3],[420,1,420,3],[414,1,414,3],[419,1,419,3],[423,1,423,3],[424,1,424,3],[0,1,0,11],[6,1,6,3],[2,1,2,3],[4,1,4,3],[2,5,2,7],[2,9,2,11],[410,1,410,3],[4,9,4,11],[411,1,411,3],[196,1,196,3],[197,1,197,3],[198,1,198,3],[199,1,199,3],[200,1,200,3],[207,1,207,3],[208,1,208,3],[209,1,209,3],[210,1,210,3],[201,1,201,3],[202,1,202,3],[203,1,203,3],[204,1,204,3],[205,1,205,3],[357,1,357,3],[191,1,191,3],[192,1,192,3],[193,1,193,3],[194,1,194,3],[428,1,428,3],[429,1,429,3],[430,1,430,3],[422,1,422,3],[7,1,7,3],[418,1,418,3],[421,1,421,3],[190,1,190,3],[412,1,412,3],[415,1,415,3],[358,1,358,3],[359,1,359,3],[231,1,231,3],[232,1,232,3],[233,1,233,3],[234,1,234,3],[235,1,235,3],[236,1,236,3],[237,1,237,3],[238,1,238,3]]}
[null,"DSP48Power",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(TRUE,1,OFFSET(POWER_SCALE,5,OFFSET(POWER_SCALE,1,1))*PL_POWERED/0.9025)*IF(OPTIMIZATION<>\"Power Optimization\",1,0.8)","v":1},{"$f":"IF(Summary!$Y$1=\"noint\",0,1)","v":1},null,null,null,null,null,null,null,null,null,null,null,"Block or Component","Oly"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mult-ALU aregCurrent",4.9050400000000001E-4]
[null,"Power",null,null,null,"Utilization",null,null,null,"DSP48 User Guide",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mult-ALU bregCurrent",2.9537699999999999E-4]
[null,"VCCINT",{"$f":"VCCINT","v":0.95},{"$f":"SUM(L8:L500)","v":5.5196240740114275},null,"DSP48",{"$f":"SUM(E8:E500)","v":1200},{"$f":"IF(AND(G4/NUM_DSPS>=0.995, G4/NUM_DSPS<0.9999),0.99,G4/NUM_DSPS)","v":0.66666666666666663},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mult-ALU cregCurrent",3.6693199999999999E-4]
[null,{"$f":"TEXT(DSP_POWER/TOTAL_POWER,\"0%\")&\" of total on-chip power \"&TEXT(TOTAL_POWER,\"0.000\")&\"W\"","v":"7% of total on-chip power 0.084W"},null,null,null,null,null,null,null,"XPE User Guide",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mult-ALU pregCurrent",1.375177E-3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mult-ALU aluCurrent",3.3489750000000001E-3]
[null,"Name",null,null,"DSP Slices","Clock (MHz)","Toggle Rate","MULT Used?","MREG Used?","Pre-add Used?","Signal Rate (Mtr/s)","Power (W)",null,null,null,null,null,"Routing Power","Clocking Power","Mult_Alu","Preadde_mult_Alu","ALU only","Mult-ALU no MREG","Preadd-mult-ALU no MREG",null,null,null,null,null,null,"Mult-ALU preAdderCurrent",2.3981600000000001E-4]
[null,null,null,null,1200,320,0.5,"Yes","Yes","Yes",{"$f":"F8*G8*IF(OR(H8=\"No\",I8=\"Yes\"),1,1.15)","v":160},{"$f":"(($E8*VCCINT/1000)*(VCCINT/1)*$N8+(R8+S8)*$S$1)*$R$1*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),5)","v":5.5196240740114275},null,{"$f":"IF($H8=\"Yes\",IF($J8=\"Yes\",IF($I8=\"Yes\",$U8,$X8),IF($I8=\"Yes\",$T8,$W8)),$V8)","v":4.5069436799999991},null,null,null,{"$f":"E8*OFFSET(FANOUT,5,13)*K8/2*48*VCCINT_N/1000","v":0.59885567999999989},{"$f":"$E8*$F8*(OFFSET(CLOCK_DATA,5,4)+OFFSET(CLOCK_DATA,5,5))*VCCINT_N/1000","v":3.9748388571428567E-2},{"$f":"$F8*($G8/0.5)*($AF$2+$AF$3+$AF$4+$AF$5+$AF$6+$AF$7+$AF$8+($AF$10-$AF$9))","v":4.1207043199999998},{"$f":"$F8*($G8/0.5)*($AF$14+$AF$15+$AF$16+$AF$17+$AF$18+$AF$19+$AF$20+($AF$22-$AF$21))","v":4.5069436799999991},{"$f":"$F8*($G8/0.5)*($AF$26+$AF$27+$AF$28+$AF$29+$AF$30+$AF$31+$AF$32+($AF$34-$AF$33))","v":3.0455040000000007},{"$f":"$F8*($G8/0.5)*($AF$38+$AF$39+$AF$40+$AF$41+$AF$42+$AF$43+$AF$44+($AF$46-$AF$45))","v":4.643904319999999},{"$f":"$F8*($G8/0.5)*($AF$50+$AF$51+$AF$52+$AF$53+$AF$54+$AF$55+$AF$56+($AF$58-$AF$57))","v":4.6616963199999999},null,null,null,null,null,null,"Mult-ALU multCurrent",4.2553840000000001E-3]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",{"$f":"F9*G9*IF(OR(H9=\"No\",I9=\"Yes\"),1,1.15)","v":0},0,null,{"$f":"IF($H9=\"Yes\",IF($J9=\"Yes\",IF($I9=\"Yes\",$U9,$X9),IF($I9=\"Yes\",$T9,$W9)),$V9)","v":0},null,null,null,0,0,{"$f":"$F9*($G9/0.5)*($AF$2+$AF$3+$AF$4+$AF$5+$AF$6+$AF$7+$AF$8+($AF$10-$AF$9))","v":0},{"$f":"$F9*($G9/0.5)*($AF$14+$AF$15+$AF$16+$AF$17+$AF$18+$AF$19+$AF$20+($AF$22-$AF$21))","v":0},{"$f":"$F9*($G9/0.5)*($AF$26+$AF$27+$AF$28+$AF$29+$AF$30+$AF$31+$AF$32+($AF$34-$AF$33))","v":0},{"$f":"$F9*($G9/0.5)*($AF$38+$AF$39+$AF$40+$AF$41+$AF$42+$AF$43+$AF$44+($AF$46-$AF$45))","v":0},{"$f":"$F9*($G9/0.5)*($AF$50+$AF$51+$AF$52+$AF$53+$AF$54+$AF$55+$AF$56+($AF$58-$AF$57))","v":0},null,null,null,null,null,null,"Mult-ALU Component Sum Current",1.0372164E-2]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Mult-ALU Total Measured Current",1.28772E-2]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU aregCurrent",4.9050400000000001E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU bregCurrent",2.95712E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU cregCurrent",3.6685899999999998E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU pregCurrent",1.524786E-3]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU aluCurrent",5.6254929999999996E-3]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU preAdderCurrent",8.2009499999999996E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU multCurrent",3.9665999999999998E-3]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU Component Sum Current",1.3090050000000001E-2]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU Total Measured Current",1.40842E-2]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"ALU Only aregCurrent",4.9031499999999996E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"ALU Only bregCurrent",2.9546800000000001E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"ALU Only cregCurrent",3.6968899999999998E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"ALU Only pregCurrent",1.525916E-3]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"ALU Only aluCurrent",5.36835E-3]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"ALU Only preAdderCurrent",2.19385E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"ALU Only multCurrent",4.7213600000000001E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"ALU Only Component Sum Current",8.7412589999999995E-3]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"ALU Only Total Measured Current",9.5172E-3]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Mult-ALU no MREG aregCurrent",5.4349499999999996E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Mult-ALU no MREG bregCurrent",3.2728800000000001E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Mult-ALU no MREG cregCurrent",4.0657300000000003E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Mult-ALU no MREG pregCurrent",1.849336E-3]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Mult-ALU no MREG aluCurrent",6.9502619999999996E-3]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Mult-ALU no MREG preAdderCurrent",2.6572400000000001E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Mult-ALU no MREG multCurrent",4.6070770000000002E-3]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Mult-ALU no MREG Component Sum Current",1.4949754000000001E-2]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Mult-ALU no MREG Total Measured Current",1.4512199999999999E-2]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no MREG aregCurrent",5.4349499999999996E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no MREG bregCurrent",3.2765799999999999E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no MREG cregCurrent",4.06492E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no MREG pregCurrent",1.785095E-3]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no MREG aluCurrent",6.981938E-3]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no MREG preAdderCurrent",9.0869300000000002E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no MREG multCurrent",4.25969E-3]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no MREG Component Sum Current",1.521306E-2]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no MREG Total Measured Current",1.4567800000000001E-2]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no AD&MREG aregCurrent",5.4349499999999996E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no AD&MREG bregCurrent",3.2765799999999999E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no AD&MREG cregCurrent",4.06492E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no AD&MREG pregCurrent",1.8307499999999999E-3]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no AD&MREG aluCurrent",7.451053E-3]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no AD&MREG preAdderCurrent",8.99506E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no AD&MREG multCurrent",7.7255559999999997E-3]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no AD&MREG Component Sum Current",1.9184511000000001E-2]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no AD&MREG Total Measured Current",1.8533600000000001E-2]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,{"$f":"(($E72*VCCINT/1000)*(VCCINT/1)*$N72+(R72+S72)*$S$1)*$R$1*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),5)","v":0},null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",{"$f":"F73*G73*IF(OR(H73=\"No\",I73=\"Yes\"),1,1.15)","v":0},0,null,{"$f":"IF($H73=\"Yes\",IF($J73=\"Yes\",IF($I73=\"Yes\",$U73,$X73),IF($I73=\"Yes\",$T73,$W73)),$V73)","v":0},null,null,null,0,0,{"$f":"$F73*($G73/0.5)*($AF$2+$AF$3+$AF$4+$AF$5+$AF$6+$AF$7+$AF$8+($AF$10-$AF$9))","v":0},{"$f":"$F73*($G73/0.5)*($AF$14+$AF$15+$AF$16+$AF$17+$AF$18+$AF$19+$AF$20+($AF$22-$AF$21))","v":0},{"$f":"$F73*($G73/0.5)*($AF$26+$AF$27+$AF$28+$AF$29+$AF$30+$AF$31+$AF$32+($AF$34-$AF$33))","v":0},{"$f":"$F73*($G73/0.5)*($AF$38+$AF$39+$AF$40+$AF$41+$AF$42+$AF$43+$AF$44+($AF$46-$AF$45))","v":0},{"$f":"$F73*($G73/0.5)*($AF$50+$AF$51+$AF$52+$AF$53+$AF$54+$AF$55+$AF$56+($AF$58-$AF$57))","v":0}]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no AD aregCurrent",4.8914499999999997E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no AD bregCurrent",2.9489300000000001E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no AD cregCurrent",3.6584299999999997E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no AD pregCurrent",5.3442189999999999E-3]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no AD  aluCurrent",7.7908999999999997E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no AD  preAdderCurrent",8.0955600000000001E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no AD  multCurrent",6.953E-3]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no AD Component Sum Current",1.5035745E-2]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Preadd-mult-ALU no AD Total Measured Current",1.4914353999999999E-2]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0,null,null,null,null,null,null,"Wide-XOR current",3.0118000000000001E-4]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,{"$f":"E100*OFFSET(FANOUT,5,13)*K100/2*48*VCCINT_N/1000","v":0},0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,{"$f":"(($E136*VCCINT/1000)*(VCCINT/1)*$N136+(R136+S136)*$S$1)*$R$1*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),5)","v":0},null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",{"$f":"F137*G137*IF(OR(H137=\"No\",I137=\"Yes\"),1,1.15)","v":0},0,null,{"$f":"IF($H137=\"Yes\",IF($J137=\"Yes\",IF($I137=\"Yes\",$U137,$X137),IF($I137=\"Yes\",$T137,$W137)),$V137)","v":0},null,null,null,0,0,{"$f":"$F137*($G137/0.5)*($AF$2+$AF$3+$AF$4+$AF$5+$AF$6+$AF$7+$AF$8+($AF$10-$AF$9))","v":0},{"$f":"$F137*($G137/0.5)*($AF$14+$AF$15+$AF$16+$AF$17+$AF$18+$AF$19+$AF$20+($AF$22-$AF$21))","v":0},{"$f":"$F137*($G137/0.5)*($AF$26+$AF$27+$AF$28+$AF$29+$AF$30+$AF$31+$AF$32+($AF$34-$AF$33))","v":0},{"$f":"$F137*($G137/0.5)*($AF$38+$AF$39+$AF$40+$AF$41+$AF$42+$AF$43+$AF$44+($AF$46-$AF$45))","v":0},{"$f":"$F137*($G137/0.5)*($AF$50+$AF$51+$AF$52+$AF$53+$AF$54+$AF$55+$AF$56+($AF$58-$AF$57))","v":0}]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,{"$f":"$E141*$F141*(OFFSET(CLOCK_DATA,5,4)+OFFSET(CLOCK_DATA,5,5))*VCCINT_N/1000","v":0},0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",{"$f":"F191*G191*IF(OR(H191=\"No\",I191=\"Yes\"),1,1.15)","v":0},0,null,0,null,null,null,{"$f":"E191*OFFSET(FANOUT,5,13)*K191/2*48*VCCINT_N/1000","v":0},0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,{"$f":"(($E200*VCCINT/1000)*(VCCINT/1)*$N200+(R200+S200)*$S$1)*$R$1*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),5)","v":0},null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,{"$f":"IF($H201=\"Yes\",IF($J201=\"Yes\",IF($I201=\"Yes\",$U201,$X201),IF($I201=\"Yes\",$T201,$W201)),$V201)","v":0},null,null,null,0,0,{"$f":"$F201*($G201/0.5)*($AF$2+$AF$3+$AF$4+$AF$5+$AF$6+$AF$7+$AF$8+($AF$10-$AF$9))","v":0},{"$f":"$F201*($G201/0.5)*($AF$14+$AF$15+$AF$16+$AF$17+$AF$18+$AF$19+$AF$20+($AF$22-$AF$21))","v":0},{"$f":"$F201*($G201/0.5)*($AF$26+$AF$27+$AF$28+$AF$29+$AF$30+$AF$31+$AF$32+($AF$34-$AF$33))","v":0},{"$f":"$F201*($G201/0.5)*($AF$38+$AF$39+$AF$40+$AF$41+$AF$42+$AF$43+$AF$44+($AF$46-$AF$45))","v":0},{"$f":"$F201*($G201/0.5)*($AF$50+$AF$51+$AF$52+$AF$53+$AF$54+$AF$55+$AF$56+($AF$58-$AF$57))","v":0}]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,{"$f":"$E229*$F229*(OFFSET(CLOCK_DATA,5,4)+OFFSET(CLOCK_DATA,5,5))*VCCINT_N/1000","v":0},0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,{"$f":"(($E264*VCCINT/1000)*(VCCINT/1)*$N264+(R264+S264)*$S$1)*$R$1*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),5)","v":0},null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,{"$f":"IF($H265=\"Yes\",IF($J265=\"Yes\",IF($I265=\"Yes\",$U265,$X265),IF($I265=\"Yes\",$T265,$W265)),$V265)","v":0},null,null,null,0,0,{"$f":"$F265*($G265/0.5)*($AF$2+$AF$3+$AF$4+$AF$5+$AF$6+$AF$7+$AF$8+($AF$10-$AF$9))","v":0},{"$f":"$F265*($G265/0.5)*($AF$14+$AF$15+$AF$16+$AF$17+$AF$18+$AF$19+$AF$20+($AF$22-$AF$21))","v":0},{"$f":"$F265*($G265/0.5)*($AF$26+$AF$27+$AF$28+$AF$29+$AF$30+$AF$31+$AF$32+($AF$34-$AF$33))","v":0},{"$f":"$F265*($G265/0.5)*($AF$38+$AF$39+$AF$40+$AF$41+$AF$42+$AF$43+$AF$44+($AF$46-$AF$45))","v":0},{"$f":"$F265*($G265/0.5)*($AF$50+$AF$51+$AF$52+$AF$53+$AF$54+$AF$55+$AF$56+($AF$58-$AF$57))","v":0}]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",{"$f":"F320*G320*IF(OR(H320=\"No\",I320=\"Yes\"),1,1.15)","v":0},0,null,0,null,null,null,{"$f":"E320*OFFSET(FANOUT,5,13)*K320/2*48*VCCINT_N/1000","v":0},0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,{"$f":"(($E328*VCCINT/1000)*(VCCINT/1)*$N328+(R328+S328)*$S$1)*$R$1*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),5)","v":0},null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,{"$f":"IF($H329=\"Yes\",IF($J329=\"Yes\",IF($I329=\"Yes\",$U329,$X329),IF($I329=\"Yes\",$T329,$W329)),$V329)","v":0},null,null,null,0,0,{"$f":"$F329*($G329/0.5)*($AF$2+$AF$3+$AF$4+$AF$5+$AF$6+$AF$7+$AF$8+($AF$10-$AF$9))","v":0},{"$f":"$F329*($G329/0.5)*($AF$14+$AF$15+$AF$16+$AF$17+$AF$18+$AF$19+$AF$20+($AF$22-$AF$21))","v":0},{"$f":"$F329*($G329/0.5)*($AF$26+$AF$27+$AF$28+$AF$29+$AF$30+$AF$31+$AF$32+($AF$34-$AF$33))","v":0},{"$f":"$F329*($G329/0.5)*($AF$38+$AF$39+$AF$40+$AF$41+$AF$42+$AF$43+$AF$44+($AF$46-$AF$45))","v":0},{"$f":"$F329*($G329/0.5)*($AF$50+$AF$51+$AF$52+$AF$53+$AF$54+$AF$55+$AF$56+($AF$58-$AF$57))","v":0}]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",{"$f":"F384*G384*IF(OR(H384=\"No\",I384=\"Yes\"),1,1.15)","v":0},0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,{"$f":"(($E392*VCCINT/1000)*(VCCINT/1)*$N392+(R392+S392)*$S$1)*$R$1*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),5)","v":0},null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,{"$f":"IF($H393=\"Yes\",IF($J393=\"Yes\",IF($I393=\"Yes\",$U393,$X393),IF($I393=\"Yes\",$T393,$W393)),$V393)","v":0},null,null,null,0,0,{"$f":"$F393*($G393/0.5)*($AF$2+$AF$3+$AF$4+$AF$5+$AF$6+$AF$7+$AF$8+($AF$10-$AF$9))","v":0},{"$f":"$F393*($G393/0.5)*($AF$14+$AF$15+$AF$16+$AF$17+$AF$18+$AF$19+$AF$20+($AF$22-$AF$21))","v":0},{"$f":"$F393*($G393/0.5)*($AF$26+$AF$27+$AF$28+$AF$29+$AF$30+$AF$31+$AF$32+($AF$34-$AF$33))","v":0},{"$f":"$F393*($G393/0.5)*($AF$38+$AF$39+$AF$40+$AF$41+$AF$42+$AF$43+$AF$44+($AF$46-$AF$45))","v":0},{"$f":"$F393*($G393/0.5)*($AF$50+$AF$51+$AF$52+$AF$53+$AF$54+$AF$55+$AF$56+($AF$58-$AF$57))","v":0}]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",{"$f":"F411*G411*IF(OR(H411=\"No\",I411=\"Yes\"),1,1.15)","v":0},0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,{"$f":"E442*OFFSET(FANOUT,5,13)*K442/2*48*VCCINT_N/1000","v":0},{"$f":"$E442*$F442*(OFFSET(CLOCK_DATA,5,4)+OFFSET(CLOCK_DATA,5,5))*VCCINT_N/1000","v":0},0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,{"$f":"(($E456*VCCINT/1000)*(VCCINT/1)*$N456+(R456+S456)*$S$1)*$R$1*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),5)","v":0},null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,{"$f":"IF($H457=\"Yes\",IF($J457=\"Yes\",IF($I457=\"Yes\",$U457,$X457),IF($I457=\"Yes\",$T457,$W457)),$V457)","v":0},null,null,null,0,0,{"$f":"$F457*($G457/0.5)*($AF$2+$AF$3+$AF$4+$AF$5+$AF$6+$AF$7+$AF$8+($AF$10-$AF$9))","v":0},{"$f":"$F457*($G457/0.5)*($AF$14+$AF$15+$AF$16+$AF$17+$AF$18+$AF$19+$AF$20+($AF$22-$AF$21))","v":0},{"$f":"$F457*($G457/0.5)*($AF$26+$AF$27+$AF$28+$AF$29+$AF$30+$AF$31+$AF$32+($AF$34-$AF$33))","v":0},{"$f":"$F457*($G457/0.5)*($AF$38+$AF$39+$AF$40+$AF$41+$AF$42+$AF$43+$AF$44+($AF$46-$AF$45))","v":0},{"$f":"$F457*($G457/0.5)*($AF$50+$AF$51+$AF$52+$AF$53+$AF$54+$AF$55+$AF$56+($AF$58-$AF$57))","v":0}]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,{"$f":"E474*OFFSET(FANOUT,5,13)*K474/2*48*VCCINT_N/1000","v":0},{"$f":"$E474*$F474*(OFFSET(CLOCK_DATA,5,4)+OFFSET(CLOCK_DATA,5,5))*VCCINT_N/1000","v":0},0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",{"$f":"F475*G475*IF(OR(H475=\"No\",I475=\"Yes\"),1,1.15)","v":0},0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",0,0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,null,null,0.125,"Yes","Yes","No",{"$f":"F500*G500*IF(OR(H500=\"No\",I500=\"Yes\"),1,1.15)","v":0},0,null,0,null,null,null,0,0,0,0,0,0,0]
[null,{"$f":"ROW(DSPROWS)-8","v":493}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(R8:S500)*$R$1*OFFSET(POWER_OPT,OFFSET(OPTIMIZATION,0,3),5)","v":0.63860406857142848}]

{"sheet":"PLL","index":9,"n_rows":129,"n_cols":37,"rows_kept":129,"cut":false,"hidden":true,"merged":[[32,1,32,3],[10,1,10,3],[29,1,29,3],[30,1,30,3],[31,1,31,3],[28,1,28,3],[27,1,27,3],[24,1,24,3],[17,1,17,3],[21,1,21,3],[23,1,23,3],[19,1,19,3],[22,1,22,3],[18,1,18,3],[26,1,26,3],[20,1,20,3],[0,1,0,15],[9,1,9,3],[2,5,2,7],[8,1,8,3],[2,1,2,3],[2,9,2,11],[5,1,5,2],[4,9,4,11],[11,1,11,3],[16,1,16,3],[25,1,25,3],[15,1,15,3],[6,1,6,3],[14,1,14,3],[12,1,12,3],[13,1,13,3]]}
[null,"PLL Power",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"off"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1]
[null,"Power",null,null,null,"Utilization",null,null,null,"Clocking Resources User Guide",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2]
[null,"VCCINT",{"$f":"TEXT(VCCINT,\"0.000\")&\"V\"","v":"0.001V"},{"$f":"PLLINT_POWER","v":6.3644679999999988E-4},null,"PLL",{"$f":"IF(NUM_PLLS>0,COUNTIF(E10:E33,\">0\"),\"N/A\")","v":0},{"$f":"IF(NUM_PLLS>0,G4/NUM_PLLS,\"N/A\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3]
[null,"VCCAUX",{"$f":"TEXT(VCCAUX,\"0.000\")&\"V\"","v":"0.002V"},{"$f":"PLLAUX_POWER","v":0.10725398746906636},null,null,null,null,null,"XPower Estimator User Guide",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4]
[null,"Total   ",null,{"$f":"SUM(D4:D5)","v":0.10789043426906636},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5]
[null,{"$f":"TEXT(PLL_POWER/TOTAL_POWER,\"0%\")&\" of total on-chip power \"&TEXT(TOTAL_POWER,\"0.000\")&\"W\"","v":"0% of total on-chip power 0.084W"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"clkout0","clkout1","clkout2","clkout3","clkout4","clkout5",null,7]
[null,"Name",null,null,"Clock (MHz)","Divide Counter","Multiply Counter","Clock 0 Divide","Clock 1 Divide","Clock 2 Divide","Clock 3 Divide","Clock 4 Divide","Clock 5 Divide","Power Down","VCCINT (W)","VCCAUX (W)","ICCAUXQ (mA)",null,"VCO (MHz)","clkfb (MHz)","VCO Ring (Vccaux)","PFD/fb (Vccaux)","fb (Vccint)","clkout0 (Vccint)","clkout1 (Vccint)","clkout2 (Vccint)","clkout3 (Vccint)","clkout4 (Vccint)","clkout5 (Vccint)","clkout0 (Vccaux)","clkout1 (Vccaux)","clkout2 (Vccaux)","clkout3 (Vccaux)","clkout4 (Vccaux)","clkout5 (Vccaux)",null,8]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,{"$f":" IF($E10>0,SUM(W10:AC10)*(VCCINT/1000)*VCCINT_N,0)*(1-$N10)*1.1","v":0},{"$f":" IF($E10>0,$Q10+$U10+$V10+SUM($AD10:$AI10),0)*VCCAUX/1000*(1-$N10)*1.1","v":0},{"$f":" IF($E10>0, (OFFSET(PLL_DATA,1,1)+OFFSET(PLL_DATA,2,1)+OFFSET(PLL_DATA,3,1)),0)","v":0},null,{"$f":"$E10/$F10*$G10","v":0},{"$f":"$E10/$F10","v":0},{"$f":"OFFSET(PLL_DATA,4,2)*S10","v":0},{"$f":"(OFFSET(PLL_DATA,5,2)+OFFSET(PLL_DATA,6,2)+OFFSET(PLL_DATA,7,2))*T10","v":0},{"$f":"OFFSET(PLL_DATA,8,2)*T10","v":0},{"$f":"IF($H10=\"off\",0,$S10/$H10*OFFSET(PLL_DATA,8,2))","v":0},{"$f":"IF($I10=\"off\",0,$S10/$I10*OFFSET(PLL_DATA,8,2))","v":0},{"$f":"IF($J10=\"off\",0,$S10/$J10*OFFSET(PLL_DATA,8,2))","v":0},{"$f":"IF($K10=\"off\",0,$S10/$K10*OFFSET(PLL_DATA,8,2))","v":0},{"$f":"IF($L10=\"off\",0,$S10/$L10*OFFSET(PLL_DATA,8,2))","v":0},{"$f":"IF($M10=\"off\",0,$S10/$M10*OFFSET(PLL_DATA,8,2))","v":0},{"$f":"IF($H10=\"off\",0,$S10/$H10*OFFSET(PLL_DATA,5,2))","v":0},{"$f":"IF($I10=\"off\",0,$S10/$I10*OFFSET(PLL_DATA,5,2))","v":0},{"$f":"IF($J10=\"off\",0,$S10/$J10*OFFSET(PLL_DATA,5,2))","v":0},{"$f":"IF($K10=\"off\",0,$S10/$K10*OFFSET(PLL_DATA,5,2))","v":0},{"$f":"IF($L10=\"off\",0,$S10/$L10*OFFSET(PLL_DATA,5,2))","v":0},{"$f":"IF($M10=\"off\",0,$S10/$M10*OFFSET(PLL_DATA,5,2))","v":0},null,9]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,{"$f":" IF($E11>0, (OFFSET(PLL_DATA,1,1)+OFFSET(PLL_DATA,2,1)+OFFSET(PLL_DATA,3,1)),0)","v":0},null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,10]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,11]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,12]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,13]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,14]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,15]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,16]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,17]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,18]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,19]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,20]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,21]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,22]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,23]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,24]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,25]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,26]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,27]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,28]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,29]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,30]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,0,0,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,31]
[null,null,null,null,null,1,1,"off","off","off","off","off","off",null,{"$f":" IF($E33>0,SUM(W33:AC33)*(VCCINT/1000)*VCCINT_N,0)*(1-$N10)*1.1","v":0},{"$f":" IF($E33>0,$Q33+$U33+$V33+SUM($AD33:$AI33),0)*VCCAUX/1000*(1-$N10)*1.1","v":0},0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(NUM_PLLS>0,SUM(O10:O33),0)*PL_POWERED","v":0},{"$f":"IF(NUM_PLLS>0,SUM(P10:P33),0)*PL_POWERED","v":0},{"$f":"IF(NUM_PLLS>0,SUM(Q10:Q33),0)*VCCAUX/1000","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,33]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,34]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,36]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,37]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,38]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,39]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,42]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,43]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,44]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,45]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,46]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,47]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,48]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,49]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,51]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,52]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,53]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,54]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,61]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,62]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,64]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,65]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,66]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,67]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,68]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,69]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,71]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,72]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,73]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,75]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,76]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,77]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,78]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,79]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,80]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,81]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,82]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,83]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,84]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,85]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,86]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,87]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,88]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,89]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,90]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,91]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,92]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,93]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,96]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,97]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,98]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,99]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,101]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,102]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,103]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,104]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,105]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,106]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,107]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,108]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,109]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,110]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,111]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,112]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,113]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,114]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,116]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,117]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,118]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,119]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,120]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,121]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,122]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,123]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,124]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,125]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,126]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,127]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,128]

{"sheet":"CLKMGR","index":10,"n_rows":182,"n_cols":56,"rows_kept":182,"cut":false,"hidden":false,"merged":[[43,1,43,3],[44,1,44,3],[38,1,38,3],[39,1,39,3],[40,1,40,3],[41,1,41,3],[42,1,42,3],[33,1,33,3],[34,1,34,3],[35,1,35,3],[36,1,36,3],[37,1,37,3],[17,1,17,3],[18,1,18,3],[21,1,21,3],[20,1,20,3],[19,1,19,3],[15,1,15,3],[16,1,16,3],[11,1,11,3],[12,1,12,3],[13,1,13,3],[14,1,14,3],[49,1,49,3],[22,1,22,3],[24,1,24,3],[26,1,26,3],[48,1,48,3],[47,1,47,3],[45,1,45,3],[46,1,46,3],[25,1,25,3],[27,1,27,3],[23,1,23,3],[28,1,28,3],[29,1,29,3],[30,1,30,3],[31,1,31,3],[32,1,32,3],[10,1,10,3],[2,1,2,3],[6,1,6,3],[5,1,5,2],[2,5,2,7],[2,9,2,11],[8,1,8,3],[9,1,9,3],[4,9,4,11],[0,1,0,18],[6,9,6,11]]}
[null,"Clock Manager Power",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MMCM","PLL",null,16]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(IF(E10:E50=\"MMCM\",R10:R50))","v":6.1974769999999998E-3},{"$f":"SUM(IF(E10:E50=\"PLL\",R10:R50))","v":6.3644679999999988E-4}]
[null,"Power",null,null,null,"Utilization",null,null,null,"Clocking Resources User Guide",null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(IF(E10:E50=\"MMCM\",S10:S50))","v":0.50406840000000008},{"$f":"SUM(IF(E10:E50=\"PLL\",S10:S50))","v":0.10725398746906636}]
[null,"VCCINT",{"$f":"TEXT(VCCINT,\"0.000\")&\"V\"","v":"0.001V"},{"$f":"(MMCMINT_POWER+PLLINT_POWER)*PL_POWERED","v":6.8339237999999998E-3},null,"MMCM",{"$f":"IF(NUM_PLLS>0,COUNTIF(E10:E50,\"=MMCM\"),\"N/A\")","v":5},{"$f":"G4/NUM_MMCMS","v":0.16666666666666666},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(MMCMINT_POWER+MMCMAUX_POWER)*PL_POWERED","v":0.51026587700000003},{"$f":"(PLLINT_POWER+PLLAUX_POWER)*PL_POWERED","v":0.10789043426906636}]
[null,"VCCAUX",{"$f":"TEXT(VCCAUX,\"0.000\")&\"V\"","v":"0.002V"},{"$f":"(MMCMAUX_POWER+PLLAUX_POWER)*PL_POWERED","v":0.61132238746906642},null,"PLL",{"$f":"IF(NUM_PLLS>0,COUNTIF(E10:E50,\"=PLL\"),\"N/A\")","v":2},{"$f":"G5/NUM_PLLS","v":3.3333333333333333E-2},null,"XPE User Guide"]
[null,"Total   ",null,{"$f":"SUM(D4:D5)","v":0.61815631126906645}]
[null,{"$f":"TEXT((PLL_POWER+MMCM_POWER)/TOTAL_POWER,\"0%\")&\" of total on-chip power \"&TEXT(TOTAL_POWER,\"0.000\")&\"W\"","v":"1% of total on-chip power 0.084W"},null,null,null,null,null,null,null,"Introduction to XPE (video)"]
[]
[null,"Name",null,null,"MMCM or PLL","Clock (MHz)","Phase Shift","Divide Counter","Multiply Counter","Clock 0 Divide","Clock 1 Divide","Clock 2 Divide","Clock 3 Divide","Clock 4 Divide","Clock 5 Divide","Clock 6 Divide","Power Down","VCCINT (W)","VCCAUX (W)","VCCAUXQ (W)",null,null,"NO INTERPOLATORS","MMCM PLL Offset","fVco","clkfb (same as PFD clock)","clkout0","clkout1","clkout2","clkout3","clkout4","clkout5","clkout6","Base Current (Iccauxq)","fVCO (iccaux)","PFD Clock (Iccaux)","clkfbout (Iccaux)","clkout0 current (iccaux)","clkout1 current (Iccaux)","clkout2 current (Iccaux)","clkout3 current (Iccaux)","clkout4 current (Iccaux)","clkout5 current (Iccaux)","clkout6 current (Iccaux)","Base Current (Vccint)","PFD Clock (Vccint)","clkfbout (Vccint)","clkout0 current (vccint)","clkout1 current (vccint)","clkout2 current (vccint)","clkout3 current (vccint)","clkout4 current (vccint)","clkout05 current (vccint)","clkout6 current (vccint)","xiphy clk","xiphy (aux)"]
[null,"ck1",null,null,"MMCM",40,"None",1,4,1,2,4,"off","off","off","off",null,{"$f":"SUM(AS10:BB10)*(VCCINT/1000)*VCCINT_N*(1-MIN(1,IF(ISBLANK($Q10),0,$Q10)))*1.1","v":3.1822339999999994E-4},{"$f":"(SUM($AH10:$AR10)+BD10)*VCCAUX/1000*(1-MIN(1,IF(ISBLANK($Q10),0,$Q10)))*1.1","v":6.8796090000000004E-2},{"$f":" IF($F10>0,$AH10,0)*VCCAUX/1000","v":5.4576E-2},null,null,{"$f":"IF($G10=\"Dynamic\",5,IF($G10=\"Fixed\",2,1))","v":1},{"$f":"IF(E10=\"PLL\",0,$Y$1)","v":16},{"$f":"$F10/$H10*$I10","v":160},{"$f":"$F10/$H10","v":40},{"$f":"IF($J10=\"off\",0,$Y10/$J10)","v":160},{"$f":"IF($K10=\"off\",0,$Y10/$K10)","v":80},{"$f":"IF($L10=\"off\",0,$Y10/$L10)","v":40},{"$f":"IF(OR(E10<>\"MMCM\",$M10=\"off\"),0,$Y10/$M10)","v":0},{"$f":"IF(OR(E10<>\"MMCM\",$N10=\"off\"),0,$Y10/$N10)","v":0},{"$f":"IF(OR(E10<>\"MMCM\",$O10=\"off\"),0,$Y10/$O10)","v":0},{"$f":"IF(OR(E10<>\"MMCM\",P10=\"off\"),0,$Y10/$P10)","v":0},{"$f":"IF($F10=0,0,OFFSET(PLL_DATA,1+X10,1)+OFFSET(PLL_DATA,2+X10,1)+OFFSET(PLL_DATA,3+X10,1)+OFFSET(PLL_DATA,13+X10,1))","v":30.32},{"$f":"$Y10*(OFFSET(PLL_DATA,4+X10,2) + IF($E10=\"MMCM\",IF($W10>1,OFFSET(PLL_DATA,12+X10,2),0)+IF(OR($W10>2,$W10=1),OFFSET(PLL_DATA,16+X10,2)*3,0),0))","v":4.0939999999999994},{"$f":"$Z10 * (OFFSET(PLL_DATA,7+X10,2) + OFFSET(PLL_DATA,6+X10,2)*2)","v":7.1500000000000008E-2},{"$f":"$I10*Z10 * IF(E10=\"PLL\",OFFSET(PLL_DATA,5+$X10,2),OFFSET(PLL_DATA,14+$X10,2)+OFFSET(PLL_DATA,15+$X10,2))","v":0.13999999999999999},{"$f":"IF($J10=\"off\",0,$J10)*AA10 * IF($E10=\"MMCM\",OFFSET(PLL_DATA,14+$X10,2),OFFSET(PLL_DATA,5+$X10,2))","v":6.9999999999999993E-2},{"$f":"IF($K10=\"off\",0,$K10)*AB10 * OFFSET(PLL_DATA,5+$X10,2)","v":2.5000000000000001E-2},{"$f":"IF($L10=\"off\",0,$L10)*AC10 * OFFSET(PLL_DATA,5+$X10,2)","v":2.5000000000000001E-2},{"$f":"IF(AD10=0,0,$M10)*AD10 * OFFSET(PLL_DATA,5+$X10,2)","v":0},{"$f":"IF(AE10=0,0,$N10)*AE10 * OFFSET(PLL_DATA,5+$X10,2)","v":0},{"$f":"IF(AF10=0,0,$O10)*AF10 * OFFSET(PLL_DATA,5+$X10,2)","v":0},{"$f":"IF(AG10=0,0,$P10)*AG10 * OFFSET(PLL_DATA,5+$X10,2)","v":0},{"$f":"IF(F10>0,OFFSET(PLL_DATA,9+X10,1),0)","v":5.1999999999999995E-4},{"$f":"$Z10 * OFFSET(PLL_DATA,8+X10,2)","v":3.7999999999999999E-2},0,{"$f":"AA10 * OFFSET(PLL_DATA,8+$X10,2)","v":0.152},{"$f":"AB10 * OFFSET(PLL_DATA,8+$X10,2)","v":7.5999999999999998E-2},{"$f":"AC10 * OFFSET(PLL_DATA,8+$X10,2)","v":3.7999999999999999E-2},{"$f":"AD10 * OFFSET(PLL_DATA,8+$X10,2)","v":0},{"$f":"AE10 * OFFSET(PLL_DATA,8+$X10,2)","v":0},{"$f":"AF10 * OFFSET(PLL_DATA,8+$X10,2)","v":0},{"$f":"AG10 * OFFSET(PLL_DATA,8+$X10,2)","v":0},{"$f":"IF(E10<>\"PLL\",0,2*Y10)","v":0},{"$f":"IF(E10<>\"PLL\",0,$BC10* OFFSET(PLL_DATA,14,2))","v":0}]
[null,"ck2",null,null,"MMCM",40,"None",1,4,1,2,4,"off","off","off","off",null,3.1822339999999994E-4,6.8796090000000004E-2,5.4576E-2,null,null,{"$f":"IF($G11=\"Dynamic\",5,IF($G11=\"Fixed\",2,1))","v":1},{"$f":"IF(E11=\"PLL\",0,$Y$1)","v":16},{"$f":"$F11/$H11*$I11","v":160},{"$f":"$F11/$H11","v":40},{"$f":"IF($J11=\"off\",0,$Y11/$J11)","v":160},{"$f":"IF($K11=\"off\",0,$Y11/$K11)","v":80},{"$f":"IF($L11=\"off\",0,$Y11/$L11)","v":40},{"$f":"IF(OR(E11<>\"MMCM\",$M11=\"off\"),0,$Y11/$M11)","v":0},{"$f":"IF(OR(E11<>\"MMCM\",$N11=\"off\"),0,$Y11/$N11)","v":0},{"$f":"IF(OR(E11<>\"MMCM\",$O11=\"off\"),0,$Y11/$O11)","v":0},{"$f":"IF(OR(E11<>\"MMCM\",P11=\"off\"),0,$Y11/$P11)","v":0},{"$f":"IF($F11=0,0,OFFSET(PLL_DATA,1+X11,1)+OFFSET(PLL_DATA,2+X11,1)+OFFSET(PLL_DATA,3+X11,1)+OFFSET(PLL_DATA,13+X11,1))","v":30.32},4.0939999999999994,7.1500000000000008E-2,0.13999999999999999,6.9999999999999993E-2,2.5000000000000001E-2,2.5000000000000001E-2,{"$f":"IF(AD11=0,0,$M11)*AD11 * OFFSET(PLL_DATA,5+$X11,2)","v":0},0,0,0,5.1999999999999995E-4,3.7999999999999999E-2,0,0.152,7.5999999999999998E-2,3.7999999999999999E-2,0,0,0,0,{"$f":"IF(E11<>\"PLL\",0,2*Y11)","v":0},0]
[null,"ck3",null,null,"MMCM",40,"None",1,4,1,2,4,"off","off","off","off",null,3.1822339999999994E-4,6.8796090000000004E-2,5.4576E-2,null,null,1,16,160,40,160,80,40,0,0,0,0,30.32,4.0939999999999994,7.1500000000000008E-2,0.13999999999999999,6.9999999999999993E-2,2.5000000000000001E-2,2.5000000000000001E-2,0,0,0,0,5.1999999999999995E-4,3.7999999999999999E-2,0,0.152,7.5999999999999998E-2,3.7999999999999999E-2,0,0,0,0,0,0]
[null,"ck4",null,null,"MMCM",40,"None",1,4,1,2,4,"off","off","off","off",null,3.1822339999999994E-4,6.8796090000000004E-2,5.4576E-2,null,null,1,16,160,40,160,80,40,0,0,0,0,30.32,4.0939999999999994,7.1500000000000008E-2,0.13999999999999999,6.9999999999999993E-2,2.5000000000000001E-2,2.5000000000000001E-2,0,0,0,0,5.1999999999999995E-4,3.7999999999999999E-2,0,0.152,7.5999999999999998E-2,3.7999999999999999E-2,0,0,0,0,0,0]
[null,"ck5",null,null,"PLL",40,"None",1,4,1,2,4,"off","off","off","off",null,3.1822339999999994E-4,5.3626993734533182E-2,4.5873000000000004E-2,null,null,1,0,160,40,160,80,40,0,0,0,0,25.485000000000003,1.2778402699662541,7.1500000000000008E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,0,0,0,0,5.1999999999999995E-4,3.7999999999999999E-2,0,0.152,7.5999999999999998E-2,3.7999999999999999E-2,0,0,0,0,320,0.15]
[null,"ck6",null,null,"PLL",40,"None",1,4,1,2,4,"off","off","off","off",null,3.1822339999999994E-4,5.3626993734533182E-2,4.5873000000000004E-2,null,null,1,0,160,40,160,80,40,0,0,0,0,25.485000000000003,1.2778402699662541,7.1500000000000008E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,0,0,0,0,5.1999999999999995E-4,3.7999999999999999E-2,0,0.152,7.5999999999999998E-2,3.7999999999999999E-2,0,0,0,0,320,0.15]
[null,"ck7",null,null,"MMCM",160,"Dynamic",1,16,1,2,4,8,"off","off","off",null,4.9245833999999999E-3,0.22888404000000007,5.4576E-2,null,null,5,16,2560,160,2560,1280,640,320,0,0,0,30.32,80.432000000000002,0.28600000000000003,2.2399999999999998,1.1199999999999999,0.4,0.4,0.4,0,0,0,5.1999999999999995E-4,0.152,0,2.4319999999999999,1.216,0.60799999999999998,0.30399999999999999,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,{"$f":"SUM(AS29:BB29)*(VCCINT/1000)*VCCINT_N*(1-MIN(1,IF(ISBLANK($Q29),0,$Q29)))*1.1","v":0},{"$f":"(SUM($AH29:$AR29)+BD29)*VCCAUX/1000*(1-MIN(1,IF(ISBLANK($Q29),0,$Q29)))*1.1","v":0},0,null,null,1,{"$f":"IF(E29=\"PLL\",0,$Y$1)","v":16},0,0,0,0,0,{"$f":"IF(OR(E29<>\"MMCM\",$M29=\"off\"),0,$Y29/$M29)","v":0},{"$f":"IF(OR(E29<>\"MMCM\",$N29=\"off\"),0,$Y29/$N29)","v":0},{"$f":"IF(OR(E29<>\"MMCM\",$O29=\"off\"),0,$Y29/$O29)","v":0},{"$f":"IF(OR(E29<>\"MMCM\",P29=\"off\"),0,$Y29/$P29)","v":0},{"$f":"IF($F29=0,0,OFFSET(PLL_DATA,1+X29,1)+OFFSET(PLL_DATA,2+X29,1)+OFFSET(PLL_DATA,3+X29,1)+OFFSET(PLL_DATA,13+X29,1))","v":0},{"$f":"$Y29*(OFFSET(PLL_DATA,4+X29,2) + IF($E29=\"MMCM\",IF($W29>1,OFFSET(PLL_DATA,12+X29,2),0)+IF(OR($W29>2,$W29=1),OFFSET(PLL_DATA,16+X29,2)*3,0),0))","v":0},{"$f":"$Z29 * (OFFSET(PLL_DATA,7+X29,2) + OFFSET(PLL_DATA,6+X29,2)*2)","v":0},{"$f":"$I29*Z29 * IF(E29=\"PLL\",OFFSET(PLL_DATA,5+$X29,2),OFFSET(PLL_DATA,14+$X29,2)+OFFSET(PLL_DATA,15+$X29,2))","v":0},{"$f":"IF($J29=\"off\",0,$J29)*AA29 * IF($E29=\"MMCM\",OFFSET(PLL_DATA,14+$X29,2),OFFSET(PLL_DATA,5+$X29,2))","v":0},{"$f":"IF($K29=\"off\",0,$K29)*AB29 * OFFSET(PLL_DATA,5+$X29,2)","v":0},{"$f":"IF($L29=\"off\",0,$L29)*AC29 * OFFSET(PLL_DATA,5+$X29,2)","v":0},{"$f":"IF(AD29=0,0,$M29)*AD29 * OFFSET(PLL_DATA,5+$X29,2)","v":0},{"$f":"IF(AE29=0,0,$N29)*AE29 * OFFSET(PLL_DATA,5+$X29,2)","v":0},{"$f":"IF(AF29=0,0,$O29)*AF29 * OFFSET(PLL_DATA,5+$X29,2)","v":0},{"$f":"IF(AG29=0,0,$P29)*AG29 * OFFSET(PLL_DATA,5+$X29,2)","v":0},{"$f":"IF(F29>0,OFFSET(PLL_DATA,9+X29,1),0)","v":0},{"$f":"$Z29 * OFFSET(PLL_DATA,8+X29,2)","v":0},0,{"$f":"AA29 * OFFSET(PLL_DATA,8+$X29,2)","v":0},{"$f":"AB29 * OFFSET(PLL_DATA,8+$X29,2)","v":0},{"$f":"AC29 * OFFSET(PLL_DATA,8+$X29,2)","v":0},{"$f":"AD29 * OFFSET(PLL_DATA,8+$X29,2)","v":0},{"$f":"AE29 * OFFSET(PLL_DATA,8+$X29,2)","v":0},{"$f":"AF29 * OFFSET(PLL_DATA,8+$X29,2)","v":0},{"$f":"AG29 * OFFSET(PLL_DATA,8+$X29,2)","v":0},{"$f":"IF(E29<>\"PLL\",0,2*Y29)","v":0},{"$f":"IF(E29<>\"PLL\",0,$BC29* OFFSET(PLL_DATA,14,2))","v":0}]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,"None",1,1,"off","off","off","off","off","off","off",null,0,0,0,null,null,1,16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF($J50=\"off\",0,$K50)*AB50 * OFFSET(PLL_DATA,5+$X50,2)","v":0},{"$f":"IF($J50=\"off\",0,$L50)*AC50 * OFFSET(PLL_DATA,5+$X50,2)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,{"$f":"ROW(CLKMGRROWS)-10","v":41},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(NUM_PLLS>0,SUM(R10:R50)*PL_POWERED,0)","v":6.8339237999999998E-3},{"$f":"IF(NUM_PLLS>0,SUM(S10:S50)*PL_POWERED,0)","v":0.61132238746906642},{"$f":"SUM(T10:T50)","v":0.36462600000000001}]
[]
[]
[null,null,null,null,null,null,"off"]
[null,null,null,null,null,null,1]
[null,null,null,null,null,null,2]
[null,null,null,null,null,null,3]
[null,null,null,null,null,null,4]
[null,null,null,null,null,null,5]
[null,null,null,null,null,null,6]
[null,null,null,null,null,null,7]
[null,null,null,null,null,null,8]
[null,null,null,null,null,null,9]
[null,null,null,null,null,null,10]
[null,null,null,null,null,null,11]
[null,null,null,null,null,null,12]
[null,null,null,null,null,null,13]
[null,null,null,null,null,null,14]
[null,null,null,null,null,null,15]
[null,null,null,null,null,null,16]
[null,null,null,null,null,null,17]
[null,null,null,null,null,null,18]
[null,null,null,null,null,null,19]
[null,null,null,null,null,null,20]
[null,null,null,null,null,null,21]
[null,null,null,null,null,null,22]
[null,null,null,null,null,null,23]
[null,null,null,null,null,null,24]
[null,null,null,null,null,null,25]
[null,null,null,null,null,null,26]
[null,null,null,null,null,null,27]
[null,null,null,null,null,null,28]
[null,null,null,null,null,null,29]
[null,null,null,null,null,null,30]
[null,null,null,null,null,null,31]
[null,null,null,null,null,null,32]
[null,null,null,null,null,null,33]
[null,null,null,null,null,null,34]
[null,null,null,null,null,null,35]
[null,null,null,null,null,null,36]
[null,null,null,null,null,null,37]
[null,null,null,null,null,null,38]
[null,null,null,null,null,null,39]
[null,null,null,null,null,null,40]
[null,null,null,null,null,null,41]
[null,null,null,null,null,null,42]
[null,null,null,null,null,null,43]
[null,null,null,null,null,null,44]
[null,null,null,null,null,null,45]
[null,null,null,null,null,null,46]
[null,null,null,null,null,null,47]
[null,null,null,null,null,null,48]
[null,null,null,null,null,null,49]
[null,null,null,null,null,null,50]
[null,null,null,null,null,null,51]
[null,null,null,null,null,null,52]
[null,null,null,null,null,null,53]
[null,null,null,null,null,null,54]
[null,null,null,null,null,null,55]
[null,null,null,null,null,null,56]
[null,null,null,null,null,null,57]
[null,null,null,null,null,null,58]
[null,null,null,null,null,null,59]
[null,null,null,null,null,null,60]
[null,null,null,null,null,null,61]
[null,null,null,null,null,null,62]
[null,null,null,null,null,null,63]
[null,null,null,null,null,null,64]
[null,null,null,null,null,null,65]
[null,null,null,null,null,null,66]
[null,null,null,null,null,null,67]
[null,null,null,null,null,null,68]
[null,null,null,null,null,null,69]
[null,null,null,null,null,null,70]
[null,null,null,null,null,null,71]
[null,null,null,null,null,null,72]
[null,null,null,null,null,null,73]
[null,null,null,null,null,null,74]
[null,null,null,null,null,null,75]
[null,null,null,null,null,null,76]
[null,null,null,null,null,null,77]
[null,null,null,null,null,null,78]
[null,null,null,null,null,null,79]
[null,null,null,null,null,null,80]
[null,null,null,null,null,null,81]
[null,null,null,null,null,null,82]
[null,null,null,null,null,null,83]
[null,null,null,null,null,null,84]
[null,null,null,null,null,null,85]
[null,null,null,null,null,null,86]
[null,null,null,null,null,null,87]
[null,null,null,null,null,null,88]
[null,null,null,null,null,null,89]
[null,null,null,null,null,null,90]
[null,null,null,null,null,null,91]
[null,null,null,null,null,null,92]
[null,null,null,null,null,null,93]
[null,null,null,null,null,null,94]
[null,null,null,null,null,null,95]
[null,null,null,null,null,null,96]
[null,null,null,null,null,null,97]
[null,null,null,null,null,null,98]
[null,null,null,null,null,null,99]
[null,null,null,null,null,null,100]
[null,null,null,null,null,null,101]
[null,null,null,null,null,null,102]
[null,null,null,null,null,null,103]
[null,null,null,null,null,null,104]
[null,null,null,null,null,null,105]
[null,null,null,null,null,null,106]
[null,null,null,null,null,null,107]
[null,null,null,null,null,null,108]
[null,null,null,null,null,null,109]
[null,null,null,null,null,null,110]
[null,null,null,null,null,null,111]
[null,null,null,null,null,null,112]
[null,null,null,null,null,null,113]
[null,null,null,null,null,null,114]
[null,null,null,null,null,null,115]
[null,null,null,null,null,null,116]
[null,null,null,null,null,null,117]
[null,null,null,null,null,null,118]
[null,null,null,null,null,null,119]
[null,null,null,null,null,null,120]
[null,null,null,null,null,null,121]
[null,null,null,null,null,null,122]
[null,null,null,null,null,null,123]
[null,null,null,null,null,null,124]
[null,null,null,null,null,null,125]
[null,null,null,null,null,null,126]
[null,null,null,null,null,null,127]
[null,null,null,null,null,null,128]

{"sheet":"PHASER","index":11,"n_rows":34,"n_cols":22,"rows_kept":34,"cut":false,"hidden":true,"merged":[[9,1,9,3],[10,1,10,3],[2,1,2,3],[2,5,2,7],[5,1,5,2],[6,1,6,3],[8,1,8,3],[4,9,4,11],[25,1,25,3],[26,1,26,3],[15,1,15,3],[16,1,16,3],[17,1,17,3],[18,1,18,3],[19,1,19,3],[20,1,20,3],[21,1,21,3],[22,1,22,3],[23,1,23,3],[24,1,24,3],[11,1,11,3],[12,1,12,3],[13,1,13,3],[14,1,14,3],[31,1,31,3],[32,1,32,3],[27,1,27,3],[28,1,28,3],[29,1,29,3],[30,1,30,3]]}
[null,null,null,null,null,null,null,"Phaser Power"]
[]
[null,"Power",null,null,null,"Utilization"]
[null,"VCCINT",{"$f":"TEXT(VCCINT,\"0.000\")&\"V\"","v":"0.001V"},null,null,"Phaser",{"$f":"IF(NUM_PLLS>0,COUNTIF(J10:J33,\">0\"),\"N/A\")","v":0},{"$f":"IF(NUM_PLLS>0,V34/NUM_PLLS,\"N/A\")","v":0}]
[null,"VCCAUX",{"$f":"TEXT(VCCAUX,\"0.000\")&\"V\"","v":"0.002V"},null,null,null,null,null,null,"XPower Estimator User Guide"]
[null,"Total   "]
[null,{"$f":"TEXT(PHASER_POWER/TOTAL_POWER,\"0%\")&\" of total on-chip power \"&TEXT(TOTAL_POWER,\"0.000\")&\"W\"","v":{"$error":"#NAME?"}}]
[]
[null,"Name",null,null,"Input FIFOs","Output FIFOs","Phaser INs","Phaser OUTs","FIFO Clock (MHz)","Memory Clock (MHz)","VCCINT (W)","VCCAUX (W)",null,null,"FIFO","PhaserIn","PhaserOut","Control_Int","Ref_Int","Reg_Aux","Ref_Aux","Phasers"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(O10:S10)*(VCCINT/1000)*VCCINT_N","v":0},{"$f":"SUM($T10:$U10)*VCCAUX/1000","v":0},null,null,{"$f":"($E10+$F10)*$I10*OFFSET(PHASER_DATA,1,1)","v":0},{"$f":"$G10*$J10*OFFSET(PHASER_DATA,2,1)","v":0},{"$f":"$H10*$J10*OFFSET(PHASER_DATA,3,1)","v":0},{"$f":"IF($G10+$H10<=0,0,$J10*OFFSET(PHASER_DATA,4,1))*V10","v":0},{"$f":"IF($G10+$H10<=0,0,$J10*OFFSET(PHASER_DATA,5,1))*V10","v":0},{"$f":"MAX(G10:H10)*OFFSET(PHASER_DATA,2,3)*J10","v":0},{"$f":"IF($G10+$H10<=0,0,OFFSET(PHASER_DATA,5,2)+J10*OFFSET(PHASER_DATA,5,3))*V10","v":0},{"$f":"INT((MAX(G10,H10)+3)/4)","v":0}]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,{"$f":"INT((MAX(G11,H11)+3)/4)","v":0}]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,0,0,null,null,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(V10:V33)","v":0}]

{"sheet":"PCIE","index":12,"n_rows":11,"n_cols":17,"rows_kept":11,"cut":false,"hidden":true,"merged":[[4,9,4,11],[0,1,0,11],[2,9,2,11],[2,1,2,3],[4,1,4,3],[2,5,2,7],[10,1,10,3],[6,1,6,3],[7,1,7,3],[8,1,8,3],[9,1,9,3]]}
[null,"        PCI Express Power",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(NUM_GTHS>0,\"N1:N3\",\"N1:N2\")","v":"N1:N3"},"GEN1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"GEN2",31.25,62.5,1]
[null,"Power",null,null,null,"Utilization",null,null,null,"PCI Express User Guide",null,null,null,"GEN3",62.5,125,2]
[null,"VCCINT",{"$f":"TEXT(VCCINT,\"#.000\")&\"V\"","v":"001V"},{"$f":"IF(NUM_PCIES>0,(VCCINT/1000)*VCCINT_N*(SUM(GTH!AR13:AR100)+SUM(GTY!AR13:AR100)),0)*PL_POWERED","v":0},null,"PCIE",{"$f":"IF(NUM_PCIES>0,COUNTIF(F8:F11,\">0\"),\"N/A\")","v":0},{"$f":"IF(NUM_PCIES>0,COUNTIF(F8:F11,\">0\")/NUM_PCIES,\"N/A\")","v":0},null,null,null,null,null,null,125,250,4]
[null,{"$f":"TEXT(PCIE_POWER/TOTAL_POWER,\"0%\")&\" of total on-chip power \"&TEXT(TOTAL_POWER,\"0.000\")&\"W\"","v":"0% of total on-chip power 0.084W"},null,null,null,null,null,null,null,"XPower Estimator User Guide",null,null,null,null,250,{"$f":"IF(OR(SPEEDGRADE=-1,SPEEDGRADE=\"-1L\"),\"\",500)","v":500},8]
[]
[null,"Name",null,null,"Link Speed","User Clock (MHz)","Number of Lanes","Power (W)",null,null,"GEN1/2/3","Clock index",null,"Min Clock"]
[null,null,null,null,"GEN1",null,1,{"$f":"IF(ISNUMBER(F8),OFFSET(PCIE_DATA,L8+K8,1),0) *(VCCINT/1000)*VCCINT_N","v":0},null,null,{"$f":"IF(E8=\"GEN1\",0,IF(E8=\"GEN2\",3,7))+IF(NUM_GTHS>0,9,0)","v":9},{"$f":"IF(F8=500,5,IF(F8<125,F8/31.25,F8/125+2))","v":0},{"$f":"IF(K8=0,IF($G8=8,\"O5\",IF($G8=4,\"O4:O5\",IF($G8=2,\"O3:O5\",\"O1:O5\"))),IF($G8=8,\"P5\",IF($G8>=4,\"P4:P5\",IF($G8=2,\"P3:P5\",\"P1:P5\"))))","v":"P1:P5"},{"$f":"IF(K8=0,IF($F8>125,\"Q2:Q5\",IF($F8>62.5,\"Q2:Q4\",IF($F8>31.25,\"Q2:Q3\",\"Q2\"))),IF($F8>250,\"Q2:Q5\",IF($F8>125,\"Q2:Q4\",IF($F8>62.5,\"Q2:Q3\",\"Q2\"))))","v":"Q2"}]
[null,null,null,null,"GEN1",null,1,{"$f":"IF(ISNUMBER(F9),OFFSET(PCIE_DATA,L9+K9,1),0) *(VCCINT/1000)*VCCINT_N","v":0},null,null,{"$f":"IF(E9=\"GEN1\",0,IF(E9=\"GEN2\",3,7))+IF(NUM_GTHS>0,9,0)","v":9},{"$f":"IF(F9=500,5,IF(F9<125,F9/31.25,F9/125+2))","v":0},{"$f":"IF(K9=0,IF($G9=8,\"O5\",IF($G9=4,\"O4:O5\",IF($G9=2,\"O3:O5\",\"O1:O5\"))),IF($G9=8,\"P5\",IF($G9>=4,\"P4:P5\",IF($G9=2,\"P3:P5\",\"P1:P5\"))))","v":"P1:P5"},{"$f":"IF(K9=0,IF($F9>125,\"Q2:Q5\",IF($F9>62.5,\"Q2:Q4\",IF($F9>31.25,\"Q2:Q3\",\"Q2\"))),IF($F9>250,\"Q2:Q5\",IF($F9>125,\"Q2:Q4\",IF($F9>62.5,\"Q2:Q3\",\"Q2\"))))","v":"Q2"}]
[null,null,null,null,"GEN1",null,1,{"$f":"IF(ISNUMBER(F10),OFFSET(PCIE_DATA,L10+K10,1),0) *(VCCINT/1000)*VCCINT_N","v":0},null,null,{"$f":"IF(E10=\"GEN1\",0,IF(E10=\"GEN2\",3,7))+IF(NUM_GTHS>0,9,0)","v":9},{"$f":"IF(F10=500,5,IF(F10<125,F10/31.25,F10/125+2))","v":0},{"$f":"IF(K10=0,IF($G10=8,\"O5\",IF($G10=4,\"O4:O5\",IF($G10=2,\"O3:O5\",\"O1:O5\"))),IF($G10=8,\"P5\",IF($G10>=4,\"P4:P5\",IF($G10=2,\"P3:P5\",\"P1:P5\"))))","v":"P1:P5"},{"$f":"IF(K10=0,IF($F10>125,\"Q2:Q5\",IF($F10>62.5,\"Q2:Q4\",IF($F10>31.25,\"Q2:Q3\",\"Q2\"))),IF($F10>250,\"Q2:Q5\",IF($F10>125,\"Q2:Q4\",IF($F10>62.5,\"Q2:Q3\",\"Q2\"))))","v":"Q2"}]
[null,null,null,null,"GEN1",null,1,{"$f":"IF(ISNUMBER(F11),OFFSET(PCIE_DATA,L11+K11,1),0) *(VCCINT/1000)*VCCINT_N","v":0},null,null,{"$f":"IF(E11=\"GEN1\",0,IF(E11=\"GEN2\",3,7))+IF(NUM_GTHS>0,9,0)","v":9},{"$f":"IF(F11=500,5,IF(F11<125,F11/31.25,F11/125+2))","v":0},{"$f":"IF(K11=0,IF($G11=8,\"O5\",IF($G11=4,\"O4:O5\",IF($G11=2,\"O3:O5\",\"O1:O5\"))),IF($G11=8,\"P5\",IF($G11>=4,\"P4:P5\",IF($G11=2,\"P3:P5\",\"P1:P5\"))))","v":"P1:P5"},{"$f":"IF(K11=0,IF($F11>125,\"Q2:Q5\",IF($F11>62.5,\"Q2:Q4\",IF($F11>31.25,\"Q2:Q3\",\"Q2\"))),IF($F11>250,\"Q2:Q5\",IF($F11>125,\"Q2:Q4\",IF($F11>62.5,\"Q2:Q3\",\"Q2\"))))","v":"Q2"}]

{"sheet":"GTP","index":13,"n_rows":72,"n_cols":34,"rows_kept":72,"cut":false,"hidden":true,"merged":[[20,1,20,3],[2,12,2,15],[2,17,2,19],[3,12,3,13],[11,1,11,3],[15,1,15,3],[16,1,16,3],[5,12,5,13],[7,7,7,10],[8,1,8,3],[10,1,10,3],[4,17,4,19],[0,1,0,19],[49,1,49,3],[9,6,9,8],[9,9,9,12],[2,1,2,3],[2,5,2,9],[34,1,34,3],[3,1,3,2],[21,1,21,3],[22,1,22,3],[13,1,13,3],[14,1,14,3],[17,1,17,3],[18,1,18,3],[12,1,12,3],[19,1,19,3],[33,1,33,3],[46,1,46,3],[35,1,35,3],[36,1,36,3],[23,1,23,3],[24,1,24,3],[25,1,25,3],[26,1,26,3],[37,1,37,3],[38,1,38,3],[27,1,27,3],[28,1,28,3],[29,1,29,3],[30,1,30,3],[31,1,31,3],[32,1,32,3],[47,1,47,3],[48,1,48,3],[39,1,39,3],[40,1,40,3],[41,1,41,3],[42,1,42,3],[43,1,43,3],[44,1,44,3],[45,1,45,3]]}
[null,"GTP Transceiver Power",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(PROCESS_FACTOR>1,1,1)","v":1},{"$f":"IF(OR(EXACT(SPEEDGRADE,\"-1\"),RIGHT(SPEEDGRADE,3)=\"9V)\"),3.75,IF(ISWIREBOND,5.4,6.6))","v":6.6},null,null,null,null,null,null,null,{"$f":"\"AH2:AH17\"","v":"AH2:AH17"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PCIe",250]
[null,"Active Current",null,null,null,"Power",null,null,null,null,{"$f":"SUM(G6:G8)*OFFSET(POWER_SCALE,5,1)-I6","v":0},null,"Utilization",null,null,null,null,"Transceivers User Guide",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300]
[null,"Source",null,"Active",null,null,null,null,null,null,null,null,"GTP Channels",null,{"$f":"SUM(E12:E50)","v":0},{"$f":"IF(NUM_GTPS>0,O4/NUM_GTPS,\"N/A\")","v":"N/A"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,350]
[null,"VCCINT",{"$f":"VCCINT","v":0.95},{"$f":"IF(GTP_INTPOWER>0,GTP_INTPOWER/VCCINT,0)","v":0},null,"Source","Power",null,"PCIe","PCS","PMA",null,null,null,null,null,null,"XPE Guide",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400]
[null,"MGTAVCC",{"$f":"AVCC","v":1},{"$f":"IF(NUM_GTPS>1,GTP_AVCCPOWER/AVCC,0)","v":0},null,"VCCINT",{"$f":"IF(NUM_GTPS>0,SUM(P12:P50),0)","v":0},null,{"$f":"IF(NUM_GTPS>0,SUM(AG12:AG50)/1000,0)*PL_POWERED","v":0},{"$f":"GTP_INTPOWER-I6","v":0},{"$f":"SUM(G7:G8)","v":0},null,"Power Planes",null,{"$f":"INT(($O4+15)/16)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,450]
[null,"MGTAVTT",{"$f":"Summary!O29","v":1.2},{"$f":"IF(NUM_GTPS>1,GTP_AVTTPOWER/AVTT,0)","v":0},null,"MGTAVCC",{"$f":"IF(NUM_GTPS>0,SUM(Q12:Q50),0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,500]
[null,null,null,null,null,"MGTAVTT",{"$f":"IF(NUM_GTPS>0,SUM(R12:R50),0)","v":0},{"$f":"TEXT(GTP_POWER/TOTAL_POWER,\"0%\")&\" of total on-chip power \"&TEXT(TOTAL_POWER,\"0.000\")&\"W\"","v":"0% of total on-chip power 0.084W"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,550]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,600]
[null,null,null,null,null,null,"RX",null,null,"TX",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,650]
[null,"Name",null,null,"GTP Channels","Operational Mode","Data Rate (Gb/s)","Data Path","Data Mode","Data Rate (Gb/s)","Data Path","Data Mode","O/P (mV)","OOB Used","Hard PCIe","VCCINT Power (W)","MGTAVCC Power (W)","MGTAVTT Power (W)",null,"Operate Mode","Quads/PLLs","RX VCO Ring (MHz)","TX VCO Ring (MHz)","RX USERCLK","TX USERCLK","TX Voltage Swing Current","AVTT Current (ring)","AVCC Current (RX)","AVCC Current (TX)","AVCC Current (ring)","AVCC CLK","AVTT CLK","PCIe",700]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",{"$f":"$G12","v":3.125},{"$f":"$H12","v":16},{"$f":"$I12","v":"8b/10b"},250,null,null,{"$f":"(VCCINT/1000)*($E12*(OFFSET(GTP_DATA,1,$Y$1)+OFFSET(GTP_DATA,1,2+$Y$1)*MAX($X12,$Y12))+AG12)","v":0},{"$f":"(AVCC/1000)*($E12*($AB12+$AC12+$AE12)+$U12*$AD12)","v":0},{"$f":"(AVTT/1000)*$E12*($AF12+$AA12+IF(T12<>1,OFFSET(GTP_DATA,6,$Y$1)+$Z12+OFFSET(GTP_DATA,10,$Y$1),0)+IF(T12<>2,OFFSET(GTP_DATA,7,$Y$1),0)+IF($N12=\"Yes\",OFFSET(GTP_DATA,11,$Y$1),0))","v":0},null,{"$f":"IF($F12=\"Receiver\",1,IF($F12=\"Transmitter\",2,3))","v":3},{"$f":"INT((E12+3)/4)","v":0},{"$f":"IF($T12=2,0,1000*IF($G12>$Z$54,$G12/2,IF($G12>=$Z$53,$G12,IF($G12*4>$Z$54,$G12*2))))","v":3125},{"$f":"IF($T12=1,0,1000*IF($J12>$Z$54,$G12/2,IF($J12>=$Z$53,$J12,IF($J12*4>$Z$54,$J12*2))))","v":3125},{"$f":" IF(AND($T12<>2,$H12 > 0), $G12*1000/IF(OR($I12=\"8b/10b\",INT($H12/10)*10=$H12),20,16),0)","v":156.25},{"$f":" IF(AND($T12<>1,$K12 > 0), $J12*1000/IF(OR($L12=\"8b/10b\",INT($K12/10)*10=$K12),20,16),0)","v":156.25},{"$f":"IF($T12>1,$M12*OFFSET(GTP_DATA,6,$Y$1+2),0)","v":3.75},{"$f":"MAX(G12,J12)*1000*OFFSET(GTP_DATA,4,2+$Y$1)","v":2.8125},{"$f":"IF(T12=2,0,G12*1000*OFFSET(GTP_DATA,3,2+$Y$1)+OFFSET(GTP_DATA,3,$Y$1))","v":28.6875},{"$f":"IF(T12=1,0,J12*1000*OFFSET(GTP_DATA,2,2+$Y$1)+OFFSET(GTP_DATA,2,$Y$1))","v":22.375},{"$f":"MAX(V12,W12)*OFFSET(GTP_DATA,5,2+$Y$1)","v":11.5625},{"$f":"OFFSET(GTP_DATA,8,$Y$1)","v":10},{"$f":"OFFSET(GTP_DATA,9,$Y$1)","v":1.55},{"$f":"IF(AND(E12>0,O12=\"PCIe\"),OFFSET(PCIE_DATA,IF(G12<=2.5,0,4)+IF(E12=1,1,IF(E12=2,2,IF(E12<5,3,4))),1),0)","v":0},750]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,{"$f":"(VCCINT/1000)*$E13*(OFFSET(GTP_DATA,1,$Y$1)+OFFSET(GTP_DATA,1,2+$Y$1)*MAX($X13,$Y13)+AG13)","v":0},{"$f":"(AVCC/1000)*$E13*(SUM($AB13:$AE13))","v":0},0,null,{"$f":"IF($F13=\"Receiver\",1,IF($F13=\"Transmitter\",2,3))","v":3},0,{"$f":"IF($T13=2,0,1000*IF($G13>$Z$54,$G13/2,IF($G13>=$Z$53,$G13,IF($G13*4>$Z$54,$G13*2))))","v":3125},{"$f":"IF($T13=1,0,1000*IF($J13>$Z$54,$G13/2,IF($J13>=$Z$53,$J13,IF($J13*4>$Z$54,$J13*2))))","v":3125},156.25,156.25,3.75,2.8125,{"$f":"IF(T13=2,0,G13*1000*OFFSET(GTP_DATA,3,2+$Y$1)+OFFSET(GTP_DATA,3,$Y$1))","v":28.6875},{"$f":"IF(T13=1,0,J13*1000*OFFSET(GTP_DATA,2,2+$Y$1)+OFFSET(GTP_DATA,2,$Y$1))","v":22.375},{"$f":"MAX(V13,W13)*OFFSET(GTP_DATA,5,2+$Y$1)","v":11.5625},10,1.55,0,800]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0,850]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0,900]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0,950]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0,1000]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,3,0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,null,null,null,null,"Transceiver",3.125,16,"8b/10b",3.125,16,"8b/10b",250,null,null,0,0,0,null,{"$f":"IF($F50=\"Receiver\",1,IF($F50=\"Transmitter\",2,3))","v":3},0,3125,3125,156.25,156.25,3.75,2.8125,28.6875,22.375,11.5625,10,1.55,0]
[null,{"$f":"ROW(GTPROWS)-12","v":39}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VCO MIN",null,null,null,{"$f":"1.6","v":1.6}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VCO MAX",null,null,null,{"$f":" 3.3","v":3.3}]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,3]
[null,null,null,null,null,null,null,null,null,null,null,"Power Planes",0,4]
[null,null,null,null,null,null,null,null,null,null,null,"Used Quad",{"$f":"INT(($O4+3)/4)","v":0},5]
[null,null,null,null,null,null,null,null,null,null,null,"Used Pl",{"$f":"IF(GTP_PLANES>0,MAX(INT((M66+M68/2)/M68),GTPPOWERPLANE),0)","v":0},6]
[null,null,null,null,null,null,null,null,null,null,null,"Avg Quad",{"$f":"IF(GTP_PLANES>0,NUM_GTPS/GTP_PLANES/4,0)","v":0},{"$f":"\"N61:N6\" & TEXT(GTP_PLANES+1,\"#\")","v":"N61:N61"}]
[null,null,null,null,null,null,null,null,null,null,null,"Quads",null,{"$f":"IF(GTP_PLANES>0,MIN(NUM_GTPS/4,MAX(INT(($O4+15)/16)*4,GTPPOWERPLANE*4)),0)","v":0},null,null,"x^4","x^3","x^2","x","c"]
[null,null,null,null,null,null,null,null,null,null,null,"AVCCQ",null,{"$f":"N69*($Q$70*TemperatureEstimate^4+$R$70*TemperatureEstimate^3+$S$70*TemperatureEstimate^2+$T$70*TemperatureEstimate+$U$70)/1000","v":0},null,null,{"$f":"OFFSET(BLOCK_LEAKAGE,5,FACTORCOL)","v":3.8743880687599882E-9},{"$f":"OFFSET(BLOCK_LEAKAGE,5,FACTORCOL+1)","v":6.6997220269763771E-6},{"$f":"OFFSET(BLOCK_LEAKAGE,5,FACTORCOL+2)","v":1.1091806104240854E-3},{"$f":"OFFSET(BLOCK_LEAKAGE,5,FACTORCOL+3)","v":8.7707208420573238E-2},{"$f":"OFFSET(BLOCK_LEAKAGE,5,FACTORCOL+4)","v":2.854548824691669}]
[null,null,null,null,null,null,null,null,null,null,null,"AVTTQ",null,{"$f":"N69*($Q$71*TemperatureEstimate^4+$R$71*TemperatureEstimate^3+$S$71*TemperatureEstimate^2+$T$71*TemperatureEstimate+$U$71)/1000","v":0},null,null,{"$f":"OFFSET(BLOCK_LEAKAGE,5,FACTORCOL+5)","v":2.9566926386627962E-9},{"$f":"OFFSET(BLOCK_LEAKAGE,5,FACTORCOL+6)","v":6.8619488188000005E-8},{"$f":"OFFSET(BLOCK_LEAKAGE,5,FACTORCOL+7)","v":3.0651708042157973E-5},{"$f":"OFFSET(BLOCK_LEAKAGE,5,FACTORCOL+8)","v":4.0665640160207992E-3},{"$f":"OFFSET(BLOCK_LEAKAGE,5,FACTORCOL+9)","v":2.6746258995502563}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N70:N71)","v":0},{"$f":"IF(NUM_GTPS>0,GTPAVCCQ*AVCC +GTPVTTXQ*Summary!O29,0)","v":0}]

{"sheet":"GTX","index":14,"n_rows":123,"n_cols":46,"rows_kept":123,"cut":false,"hidden":true,"merged":[[0,1,0,22],[27,1,27,3],[32,1,32,3],[31,1,31,3],[23,1,23,3],[24,1,24,3],[25,1,25,3],[26,1,26,3],[29,1,29,3],[15,1,15,3],[28,1,28,3],[19,1,19,3],[21,1,21,3],[20,1,20,3],[2,19,2,21],[22,1,22,3],[30,1,30,3],[6,12,6,13],[10,12,10,16],[8,7,8,10],[10,1,10,3],[18,1,18,3],[11,1,11,3],[2,12,2,15],[79,1,79,3],[68,1,68,3],[69,1,69,3],[70,1,70,3],[71,1,71,3],[72,1,72,3],[73,1,73,3],[78,1,78,3],[75,1,75,3],[74,1,74,3],[76,1,76,3],[67,1,67,3],[61,1,61,3],[52,1,52,3],[55,1,55,3],[58,1,58,3],[63,1,63,3],[56,1,56,3],[65,1,65,3],[77,1,77,3],[60,1,60,3],[64,1,64,3],[66,1,66,3],[62,1,62,3],[59,1,59,3],[53,1,53,3],[57,1,57,3],[54,1,54,3],[91,1,91,3],[86,1,86,3],[80,1,80,3],[81,1,81,3],[82,1,82,3],[87,1,87,3],[88,1,88,3],[90,1,90,3],[85,1,85,3],[83,1,83,3],[89,1,89,3],[84,1,84,3],[105,1,105,23],[96,1,96,3],[99,1,99,3],[94,1,94,3],[95,1,95,3],[97,1,97,3],[98,1,98,3],[92,1,92,3],[93,1,93,3],[45,1,45,3],[47,1,47,3],[48,1,48,3],[49,1,49,3],[51,1,51,3],[50,1,50,3],[33,1,33,3],[37,1,37,3],[43,1,43,3],[40,1,40,3],[36,1,36,3],[34,1,34,3],[35,1,35,3],[38,1,38,3],[39,1,39,3],[46,1,46,3],[44,1,44,3],[41,1,41,3],[42,1,42,3],[2,1,2,3],[3,1,3,2],[2,5,2,9],[3,12,3,13],[10,8,10,11],[4,19,4,21],[12,1,12,3],[13,1,13,3],[17,1,17,3],[14,1,14,3],[16,1,16,3],[4,12,4,13]]}
[null,"GTX Transceiver Power",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(PROCESS<>\"Maximum\",1,1)","v":1},{"$f":"IF(OR(RIGHT(SPEEDGRADE,3)=\"9V)\",LEFT(PACKAGE,2)=\"FB\"),6.6,IF(EXACT(SPEEDGRADE,\"-1\"),8,IF(OR(RIGHT(SPEEDGRADE,1)=\"G\",EXACT(SPEEDGRADE,\"-3\")),12.5,10.3125)))","v":10.3125},null,"CPLL VCO range (MHz)","LC VCO range (MHz)",null,null,"Raised Voltage",null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"AT2:AT17\"","v":"AT2:AT17"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,5.93,9.8000000000000007,null,{"$f":"IF(K3>0,COUNTIF(J13:J100,\">10.3125\")+COUNTIF(N13:N100,\">10.3125\"),0)","v":0},null,null,null,null,null,null,null,null,null,null,"PCIe",250]
[null,"Active Current",null,null,null,"Power",null,null,null,null,{"$f":"SUM(G6:G9)*OFFSET(POWER_SCALE,5,1)-I6","v":0},null,"Utilization",null,null,null,null,null,null,"Transceivers User Guide",null,null,null,null,null,null,"Iccq",{"$f":"OFFSET(GTXE1_DATA,1,$AA1)*O4","v":0},null,3.3,{"$f":"IF( SPEEDGRADE=\"-1\",6.6,8)","v":8},12.5,null,null,null,null,null,null,null,null,null,null,null,null,null,300]
[null,"Source",null,"Active",null,null,null,null,null,null,null,null,"GTX Channels",null,{"$f":"SUM(E13:E100)","v":0},{"$f":"IF(NUM_GTS>0,O4/NUM_GTS,\"N/A\")","v":"N/A"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,350]
[null,"VCCINT",{"$f":"VCCINT","v":0.95},{"$f":"IF(GTX_INTPOWER>0,GTX_INTPOWER/VCCINT,0)","v":0},null,"Source","Power",null,"PCIe","PCS","PMA",null,"PCIe Blocks",null,{"$f":"COUNTIF(AS13:AS100,\">0\")","v":0},{"$f":"IF(NUM_PCIES>0,O5/NUM_PCIES,\"N/A\")","v":0},null,null,null,"XPE User Guide",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400]
[null,"MGTVCCAUX",{"$f":"GTVCCAUX","v":1.8},{"$f":"IF(GTX_AUXPOWER>0,GTX_AUXPOWER/GTVCCAUX,0)","v":0},null,"VCCINT",{"$f":"IF(NUM_GTS>0,SUM(T13:T100)*PL_POWERED,0)","v":0},null,{"$f":"IF(NUM_GTS>0,SUM(AS13:AS100)/1000,0)*PL_POWERED","v":0},{"$f":"GTX_INTPOWER-I6","v":0},{"$f":"SUM(G7:G9)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,450]
[null,"MGTAVCC",{"$f":"AVCC","v":1},{"$f":"IF(NUM_GTS>1,GTAVCC_POWER/AVCC,0)","v":0},null,"MGTVCCAUX",{"$f":"IF(NUM_GTS>0,SUM(U13:U100)*PL_POWERED,0)","v":0},null,null,null,null,null,"Power Planes",null,{"$f":"INT(($O4+11)/12)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,500]
[null,"MGTAVTT",{"$f":"AVTT","v":1.2},{"$f":"IF(NUM_GTS>1,GTAVTT_POWER/AVTT,0)","v":0},null,"MGTAVCC",{"$f":"IF(NUM_GTS>0,SUM(V13:V100)*PL_POWERED,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,550]
[null,null,null,null,null,"MGTAVTT",{"$f":"IF(NUM_GTS>0,SUM(W13:W100)*PL_POWERED,0)","v":0},{"$f":"TEXT(GTXE1_POWER/TOTAL_POWER,\"0%\")&\" of total on-chip power \"&TEXT(TOTAL_POWER,\"0.000\")&\"W\"","v":"0% of total on-chip power 0.084W"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,600]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,650]
[null,null,null,null,null,null,null,null,"RX",null,null,null,"TX",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,700]
[null,"Name",null,null,"GTX Channels","Operational Mode","Power Mode","Channels Sharing QPLL","Clock Source","Data Rate (Gb/s)","Data Path","Data Mode","Clock Source","Data Rate (Gb/s)","Data Path","Data Mode","O/P (mV)","OOB Used","Hard PCIe","VCCINT Power (W)","MGTVCCAUX Power (W)","MGTAVCC Power (W)","MGTAVTT Power (W)",null,"Operate Mode","Quads","RX VCO LC (MHz)","TX VCO LC (MHz)","RX VCO CPLL (MHz)","TX VCO CPLL (MHz)","RX USERCLK","TX USERCLK","RX Power Mode","TX Voltage Swing Current","AVTT Current (CPLL)","AVTT Current (LC)","AVCC Current (RX)","AVCC Current (TX)","AVCC Current (CPLL)","AVCC Current (LC)","AVCC CLK","AVTT CLK",null,null,"PCIe",750]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b",{"$f":"$J13","v":"QPLL"},{"$f":"$K13","v":5},{"$f":"$L13","v":32},{"$f":"$M13","v":"8b/10b"},269,"No",null,{"$f":"IF(AND(OR(Y13=2,I13=\"CPLL\"),OR(Y13=1,M13=\"CPLL\")),0,(IF(AND(Y13>1,M13=\"QPLL\"),AB13,IF(I13=\"QPLL\",AA13,0))*OFFSET(GTXE1_DATA,7,$AA$1+2)+OFFSET(GTXE1_DATA,7,$AA$1))/1000*Z13*GTVCCAUX)","v":0},{"$f":"(AVCC/1000)*$E13*(SUM($AK13:$AO13))","v":{"$error":"#VALUE!"}},{"$f":"(AVTT/1000)*$E13*($AP13+$AI13+$AJ13+IF(Y13<>1,OFFSET(GTXE1_DATA,10,$AA$1)+$AH13+OFFSET(GTXE1_DATA,15,$AA$1),0)+IF(Y13<>2,OFFSET(GTXE1_DATA,11+$AG13,$AA$1),0)+IF($R13=\"Yes\",OFFSET(GTXE1_DATA,16,$AA$1),0))","v":{"$error":"#VALUE!"}},null,{"$f":"IF($F13=\"Receiver\",1,IF($F13=\"Transmitter\",2,3))","v":3},{"$f":"INT((E13+3)/4)","v":0},{"$f":"IF(OR($Y13=2,$I13=\"CPLL\"),0,1000*IF(AND($G13=\"Low Power\",$AQ13/2>=$AE$2),$AQ13/2,IF(AND($G13=\"DFE\",$AQ13=$J13,$AQ13*2<=$AF$3), $AQ13*2,$AQ13)))","v":{"$error":"#VALUE!"}},{"$f":"IF(OR($Y13=1,$M13=\"CPLL\"),0,1000*IF(AND($G13=\"Low Power\",$AR13/2>=$AE$2),$AR13/2,IF(AND($G13=\"DFE\",$AR13=$N13,$AR13*2<=$AF$3), $AR13*2,$AR13)))","v":{"$error":"#VALUE!"}},{"$f":"IF($Y13=2,0,1000*IF($J13>$AB$104,$J13/2,IF($J13*4<$AB$103,$J13*8,IF($J13*2<$AB$103,$J13*4,IF($J13<$AB$103,$J13*2,IF($J13/2>=$AB$103,$J13/2,$J13))))))","v":{"$error":"#VALUE!"}},{"$f":"IF($Y13=1,0,1000*IF($N13>$AB$104,$N13/2,IF($N13*4<$AB$103,$N13*8,IF($N13*2<$AB$103,$N13*4,IF($N13<$AB$103,$N13*2,IF($N13/2>=$AB$103,$N13/2,$N13))))))","v":{"$error":"#VALUE!"}},{"$f":" IF(AND($Y13<>2,$K13 > 0), $J13*1000/IF(AND($K13=64,LEFT($L13,3)=\"64b\"),32,IF(OR($L13=\"8b/10b\",INT($K13/10)*10=$K13),IF($K13>=32,40,20),IF($K13>=32,32,16))),0)","v":{"$error":"#VALUE!"}},{"$f":" IF(AND($Y13<>1,$O13 > 0), $N13*1000/IF(AND($O13=64,LEFT($P13,3)=\"64b\"),32,IF(OR($P13=\"8b/10b\",INT($O13/10)*10=$O13),IF($O13>=32,40,20),IF($O13>=32,32,16))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF($G13=\"Low Power\",0,1)","v":1},{"$f":"IF($Y13>1,$Q13*OFFSET(GTXE1_DATA,10,$AA$1+2),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(AND(Y13>1,M13=\"CPLL\"),AD13,IF(I13=\"CPLL\",AC13,0))*OFFSET(GTXE1_DATA,5,2+$AA$1)+IF(AND(I13=\"QPLL\",M13=\"QPLL\"),0,OFFSET(GTXE1_DATA,5,$AA$1))","v":0},{"$f":"(IF(AND(Y13>1,M13=\"QPLL\"),AB13,IF(AND(Y13<>2,I13=\"QPLL\"),AA13,0))*OFFSET(GTXE1_DATA,8,2+$AA$1) + IF(AND(OR(Y13=2,I13=\"CPLL\"),OR(Y13=1,M13=\"CPLL\")),0,OFFSET(GTXE1_DATA,8,$AA$1)))*1/MAX(IF(E13>H13,H13,4),1)","v":6.9181749999999997},{"$f":"IF(Y13=2,0,J13*1000*OFFSET(GTXE1_DATA,3+$AG13,2+$AA$1)+OFFSET(GTXE1_DATA,3+$AG13,$AA$1))","v":{"$error":"#VALUE!"}},{"$f":"IF(Y13=1,0,N13*1000*OFFSET(GTXE1_DATA,2,2+$AA$1)+OFFSET(GTXE1_DATA,2,$AA$1))","v":{"$error":"#VALUE!"}},{"$f":" IF(AND(Y13>1,M13=\"CPLL\"),AD13,IF(I13=\"CPLL\",AC13,0))*OFFSET(GTXE1_DATA,6,2+$AA$1) + IF(OR(I13=\"CPLL\",M13=\"CPLL\"),OFFSET(GTXE1_DATA,6,$AA$1),0)","v":0},{"$f":"(IF(AND(Y13<>2,I13=\"QPLL\"),AA13,IF(AND(Y13<>1,M13=\"QPLL\"),AB13,0))*OFFSET(GTXE1_DATA,9,2+$AA$1) + IF(OR(AND(Y13<>2,I13=\"QPLL\"),AND(Y13<>1,M13=\"QPLL\")),OFFSET(GTXE1_DATA,9,$AA$1),0))*1/MAX(IF(E13>H13,H13,4),1)","v":0},{"$f":"OFFSET(GTXE1_DATA,13,$AA$1)","v":25.6},{"$f":"OFFSET(GTXE1_DATA,14,$AA$1)","v":1.55},{"$f":"IF(OR($Y13=2,$I13=\"CPLL\"),0,IF(OR(AND($J13*2>=$AE$2,$J13*2<=$AE$3),AND($J13*2>=$AF$2,$J13*2<=$AF$3)),$J13*2,IF(OR(AND($J13*4>=$AE$2,$J13*4<=$AE$3),AND($J13*4>=$AF$2,$J13*4<=$AF$3)),$J13*4,IF(OR(AND($J13*8>=$AE$2,$J13*8<=$AE$3),AND($J13*8>=$AF$2,$J13*8<=$AF$3)),$J13*8,IF(OR(AND($J13*16>=$AE$2,$J13*16<=$AE$3),AND($J13*16>=$AF$2,$J13*16<=$AF$3)),$J13*16,$J13)))))","v":{"$error":"#VALUE!"}},{"$f":"IF(OR($Y13=1,$M13=\"CPLL\"),0,IF(OR(AND($N13*2>=$AE$2,$N13*2<=$AE$3),AND($N13*2>=$AF$2,$N13*2<=$AF$3)),$N13*2,IF(OR(AND($N13*4>=$AE$2,$N13*4<=$AE$3),AND($N13*4>=$AF$2,$N13*4<=$AF$3)),$N13*4,IF(OR(AND($N13*8>=$AE$2,$N13*8<=$AE$3),AND($N13*8>=$AF$2,$N13*8<=$AF$3)),$N13*8,IF(OR(AND($N13*16>=$AE$2,$N13*16<=$AE$3),AND($N13*16>=$AF$2,$N13*16<=$AF$3)),$N13*16,$N13)))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND(E13>0,S13=\"PCIe\"),OFFSET(PCIE_DATA,IF(J13<=2.5,0,4)+IF(E13=1,1,IF(E13=2,2,IF(E13<5,3,4))),1),0)","v":0},800]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$f":"IF($F14=\"Receiver\",1,IF($F14=\"Transmitter\",2,3))","v":3},{"$f":"INT((E14+3)/4)","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF($Y14=2,0,1000*IF($J14>$AB$104,$J14/2,IF($J14*4<$AB$103,$J14*8,IF($J14*2<$AB$103,$J14*4,IF($J14<$AB$103,$J14*2,IF($J14/2>=$AB$103,$J14/2,$J14))))))","v":{"$error":"#VALUE!"}},{"$f":"IF($Y14=1,0,1000*IF($N14>$AB$104,$N14/2,IF($N14*4<$AB$103,$N14*8,IF($N14*2<$AB$103,$N14*4,IF($N14<$AB$103,$N14*2,IF($N14/2>=$AB$103,$N14/2,$N14))))))","v":{"$error":"#VALUE!"}},{"$f":" IF(AND($Y14<>2,$K14 > 0), $J14*1000/IF(AND($K14=64,LEFT($L14,3)=\"64b\"),32,IF(OR($L14=\"8b/10b\",INT($K14/10)*10=$K14),IF($K14>=32,40,20),IF($K14>=32,32,16))),0)","v":{"$error":"#VALUE!"}},{"$f":" IF(AND($Y14<>1,$O14 > 0), $N14*1000/IF(AND($O14=64,LEFT($P14,3)=\"64b\"),32,IF(OR($P14=\"8b/10b\",INT($O14/10)*10=$O14),IF($O14>=32,40,20),IF($O14>=32,32,16))),0)","v":{"$error":"#VALUE!"}},1,{"$error":"#VALUE!"},0,{"$f":"(IF(AND(Y14>1,M14=\"QPLL\"),AB14,IF(AND(Y14<>2,I14=\"QPLL\"),AA14,0))*OFFSET(GTXE1_DATA,8,2+$AA$1) + IF(AND(OR(Y14=2,I14=\"CPLL\"),OR(Y14=1,M14=\"CPLL\")),0,OFFSET(GTXE1_DATA,8,$AA$1)))*1/MAX(IF(E14>H14,H14,4),1)","v":6.9181749999999997},{"$f":"IF(Y14=2,0,J14*1000*OFFSET(GTXE1_DATA,3+$AG14,2+$AA$1)+OFFSET(GTXE1_DATA,3+$AG14,$AA$1))","v":{"$error":"#VALUE!"}},{"$f":"IF(Y14=1,0,N14*1000*OFFSET(GTXE1_DATA,2,2+$AA$1)+OFFSET(GTXE1_DATA,2,$AA$1))","v":{"$error":"#VALUE!"}},{"$f":" IF(AND(Y14>1,M14=\"CPLL\"),AD14,IF(I14=\"CPLL\",AC14,0))*OFFSET(GTXE1_DATA,6,2+$AA$1) + IF(OR(I14=\"CPLL\",M14=\"CPLL\"),OFFSET(GTXE1_DATA,6,$AA$1),0)","v":0},0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,850]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,900]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,950]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,1000]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b",{"$f":"$J45","v":"QPLL"},{"$f":"$K45","v":5},{"$f":"$L45","v":32},{"$f":"$M45","v":"8b/10b"},269,"No",null,{"$f":"IF(AND(OR(Y45=2,I45=\"CPLL\"),OR(Y45=1,M45=\"CPLL\")),0,(IF(AND(Y45>1,M45=\"QPLL\"),AB45,IF(I45=\"QPLL\",AA45,0))*OFFSET(GTXE1_DATA,7,$AA$1+2)+OFFSET(GTXE1_DATA,7,$AA$1))/1000*Z45*GTVCCAUX)","v":0},{"$f":"(AVCC/1000)*$E45*(SUM($AK45:$AO45))","v":{"$error":"#VALUE!"}},{"$f":"(AVTT/1000)*$E45*($AP45+$AI45+$AJ45+IF(Y45<>1,OFFSET(GTXE1_DATA,10,$AA$1)+$AH45+OFFSET(GTXE1_DATA,15,$AA$1),0)+IF(Y45<>2,OFFSET(GTXE1_DATA,11+$AG45,$AA$1),0)+IF($R45=\"Yes\",OFFSET(GTXE1_DATA,16,$AA$1),0))","v":{"$error":"#VALUE!"}},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},{"$f":"IF(AND(Y45>1,M45=\"CPLL\"),AD45,IF(I45=\"CPLL\",AC45,0))*OFFSET(GTXE1_DATA,5,2+$AA$1)+IF(AND(I45=\"QPLL\",M45=\"QPLL\"),0,OFFSET(GTXE1_DATA,5,$AA$1))","v":0},6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,{"$f":"(IF(AND(Y45<>2,I45=\"QPLL\"),AA45,IF(AND(Y45<>1,M45=\"QPLL\"),AB45,0))*OFFSET(GTXE1_DATA,9,2+$AA$1) + IF(OR(AND(Y45<>2,I45=\"QPLL\"),AND(Y45<>1,M45=\"QPLL\")),OFFSET(GTXE1_DATA,9,$AA$1),0))*1/MAX(IF(E45>H45,H45,4),1)","v":0},25.6,1.55,{"$f":"IF(OR($Y45=2,$I45=\"CPLL\"),0,IF(OR(AND($J45*2>=$AE$2,$J45*2<=$AE$3),AND($J45*2>=$AF$2,$J45*2<=$AF$3)),$J45*2,IF(OR(AND($J45*4>=$AE$2,$J45*4<=$AE$3),AND($J45*4>=$AF$2,$J45*4<=$AF$3)),$J45*4,IF(OR(AND($J45*8>=$AE$2,$J45*8<=$AE$3),AND($J45*8>=$AF$2,$J45*8<=$AF$3)),$J45*8,IF(OR(AND($J45*16>=$AE$2,$J45*16<=$AE$3),AND($J45*16>=$AF$2,$J45*16<=$AF$3)),$J45*16,$J45)))))","v":{"$error":"#VALUE!"}},{"$f":"IF(OR($Y45=1,$M45=\"CPLL\"),0,IF(OR(AND($N45*2>=$AE$2,$N45*2<=$AE$3),AND($N45*2>=$AF$2,$N45*2<=$AF$3)),$N45*2,IF(OR(AND($N45*4>=$AE$2,$N45*4<=$AE$3),AND($N45*4>=$AF$2,$N45*4<=$AF$3)),$N45*4,IF(OR(AND($N45*8>=$AE$2,$N45*8<=$AE$3),AND($N45*8>=$AF$2,$N45*8<=$AF$3)),$N45*8,IF(OR(AND($N45*16>=$AE$2,$N45*16<=$AE$3),AND($N45*16>=$AF$2,$N45*16<=$AF$3)),$N45*16,$N45)))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND(E45>0,S45=\"PCIe\"),OFFSET(PCIE_DATA,IF(J45<=2.5,0,4)+IF(E45=1,1,IF(E45=2,2,IF(E45<5,3,4))),1),0)","v":0}]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b",{"$f":"$J77","v":"QPLL"},{"$f":"$K77","v":5},{"$f":"$L77","v":32},{"$f":"$M77","v":"8b/10b"},269,"No",null,{"$f":"IF(AND(OR(Y77=2,I77=\"CPLL\"),OR(Y77=1,M77=\"CPLL\")),0,(IF(AND(Y77>1,M77=\"QPLL\"),AB77,IF(I77=\"QPLL\",AA77,0))*OFFSET(GTXE1_DATA,7,$AA$1+2)+OFFSET(GTXE1_DATA,7,$AA$1))/1000*Z77*GTVCCAUX)","v":0},{"$f":"(AVCC/1000)*$E77*(SUM($AK77:$AO77))","v":{"$error":"#VALUE!"}},{"$f":"(AVTT/1000)*$E77*($AP77+$AI77+$AJ77+IF(Y77<>1,OFFSET(GTXE1_DATA,10,$AA$1)+$AH77+OFFSET(GTXE1_DATA,15,$AA$1),0)+IF(Y77<>2,OFFSET(GTXE1_DATA,11+$AG77,$AA$1),0)+IF($R77=\"Yes\",OFFSET(GTXE1_DATA,16,$AA$1),0))","v":{"$error":"#VALUE!"}},null,3,0,{"$f":"IF(OR($Y77=2,$I77=\"CPLL\"),0,1000*IF(AND($G77=\"Low Power\",$AQ77/2>=$AE$2),$AQ77/2,IF(AND($G77=\"DFE\",$AQ77=$J77,$AQ77*2<=$AF$3), $AQ77*2,$AQ77)))","v":{"$error":"#VALUE!"}},{"$f":"IF(OR($Y77=1,$M77=\"CPLL\"),0,1000*IF(AND($G77=\"Low Power\",$AR77/2>=$AE$2),$AR77/2,IF(AND($G77=\"DFE\",$AR77=$N77,$AR77*2<=$AF$3), $AR77*2,$AR77)))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF($G77=\"Low Power\",0,1)","v":1},{"$f":"IF($Y77>1,$Q77*OFFSET(GTXE1_DATA,10,$AA$1+2),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(AND(Y77>1,M77=\"CPLL\"),AD77,IF(I77=\"CPLL\",AC77,0))*OFFSET(GTXE1_DATA,5,2+$AA$1)+IF(AND(I77=\"QPLL\",M77=\"QPLL\"),0,OFFSET(GTXE1_DATA,5,$AA$1))","v":0},6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,{"$f":"(IF(AND(Y77<>2,I77=\"QPLL\"),AA77,IF(AND(Y77<>1,M77=\"QPLL\"),AB77,0))*OFFSET(GTXE1_DATA,9,2+$AA$1) + IF(OR(AND(Y77<>2,I77=\"QPLL\"),AND(Y77<>1,M77=\"QPLL\")),OFFSET(GTXE1_DATA,9,$AA$1),0))*1/MAX(IF(E77>H77,H77,4),1)","v":0},{"$f":"OFFSET(GTXE1_DATA,13,$AA$1)","v":25.6},{"$f":"OFFSET(GTXE1_DATA,14,$AA$1)","v":1.55},{"$f":"IF(OR($Y77=2,$I77=\"CPLL\"),0,IF(OR(AND($J77*2>=$AE$2,$J77*2<=$AE$3),AND($J77*2>=$AF$2,$J77*2<=$AF$3)),$J77*2,IF(OR(AND($J77*4>=$AE$2,$J77*4<=$AE$3),AND($J77*4>=$AF$2,$J77*4<=$AF$3)),$J77*4,IF(OR(AND($J77*8>=$AE$2,$J77*8<=$AE$3),AND($J77*8>=$AF$2,$J77*8<=$AF$3)),$J77*8,IF(OR(AND($J77*16>=$AE$2,$J77*16<=$AE$3),AND($J77*16>=$AF$2,$J77*16<=$AF$3)),$J77*16,$J77)))))","v":{"$error":"#VALUE!"}},{"$f":"IF(OR($Y77=1,$M77=\"CPLL\"),0,IF(OR(AND($N77*2>=$AE$2,$N77*2<=$AE$3),AND($N77*2>=$AF$2,$N77*2<=$AF$3)),$N77*2,IF(OR(AND($N77*4>=$AE$2,$N77*4<=$AE$3),AND($N77*4>=$AF$2,$N77*4<=$AF$3)),$N77*4,IF(OR(AND($N77*8>=$AE$2,$N77*8<=$AE$3),AND($N77*8>=$AF$2,$N77*8<=$AF$3)),$N77*8,IF(OR(AND($N77*16>=$AE$2,$N77*16<=$AE$3),AND($N77*16>=$AF$2,$N77*16<=$AF$3)),$N77*16,$N77)))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND(E77>0,S77=\"PCIe\"),OFFSET(PCIE_DATA,IF(J77<=2.5,0,4)+IF(E77=1,1,IF(E77=2,2,IF(E77<5,3,4))),1),0)","v":0}]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$f":"IF($F78=\"Receiver\",1,IF($F78=\"Transmitter\",2,3))","v":3},{"$f":"INT((E78+3)/4)","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF($Y78=2,0,1000*IF($J78>$AB$104,$J78/2,IF($J78*4<$AB$103,$J78*8,IF($J78*2<$AB$103,$J78*4,IF($J78<$AB$103,$J78*2,IF($J78/2>=$AB$103,$J78/2,$J78))))))","v":{"$error":"#VALUE!"}},{"$f":"IF($Y78=1,0,1000*IF($N78>$AB$104,$N78/2,IF($N78*4<$AB$103,$N78*8,IF($N78*2<$AB$103,$N78*4,IF($N78<$AB$103,$N78*2,IF($N78/2>=$AB$103,$N78/2,$N78))))))","v":{"$error":"#VALUE!"}},{"$f":" IF(AND($Y78<>2,$K78 > 0), $J78*1000/IF(AND($K78=64,LEFT($L78,3)=\"64b\"),32,IF(OR($L78=\"8b/10b\",INT($K78/10)*10=$K78),IF($K78>=32,40,20),IF($K78>=32,32,16))),0)","v":{"$error":"#VALUE!"}},{"$f":" IF(AND($Y78<>1,$O78 > 0), $N78*1000/IF(AND($O78=64,LEFT($P78,3)=\"64b\"),32,IF(OR($P78=\"8b/10b\",INT($O78/10)*10=$O78),IF($O78>=32,40,20),IF($O78>=32,32,16))),0)","v":{"$error":"#VALUE!"}},1,{"$error":"#VALUE!"},0,{"$f":"(IF(AND(Y78>1,M78=\"QPLL\"),AB78,IF(AND(Y78<>2,I78=\"QPLL\"),AA78,0))*OFFSET(GTXE1_DATA,8,2+$AA$1) + IF(AND(OR(Y78=2,I78=\"CPLL\"),OR(Y78=1,M78=\"CPLL\")),0,OFFSET(GTXE1_DATA,8,$AA$1)))*1/MAX(IF(E78>H78,H78,4),1)","v":6.9181749999999997},{"$f":"IF(Y78=2,0,J78*1000*OFFSET(GTXE1_DATA,3+$AG78,2+$AA$1)+OFFSET(GTXE1_DATA,3+$AG78,$AA$1))","v":{"$error":"#VALUE!"}},{"$f":"IF(Y78=1,0,N78*1000*OFFSET(GTXE1_DATA,2,2+$AA$1)+OFFSET(GTXE1_DATA,2,$AA$1))","v":{"$error":"#VALUE!"}},{"$f":" IF(AND(Y78>1,M78=\"CPLL\"),AD78,IF(I78=\"CPLL\",AC78,0))*OFFSET(GTXE1_DATA,6,2+$AA$1) + IF(OR(I78=\"CPLL\",M78=\"CPLL\"),OFFSET(GTXE1_DATA,6,$AA$1),0)","v":0},0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",269,"No",null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,3,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,{"$error":"#VALUE!"},0,6.9181749999999997,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,25.6,1.55,{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,{"$f":"ROW(GTXROWS)-13","v":88}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VCO MIN",{"$f":"1.6","v":1.6}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VCO MAX",{"$f":"3.3","v":3.3}]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,3]
[null,null,null,null,null,null,null,null,null,null,null,null,"Power Planes",0,4]
[null,null,null,null,null,null,null,null,null,null,null,null,"Used Quad",{"$f":"INT((O4+3)/4)","v":0},5,null,null,null,null,"FactorCol",{"$f":"IF(PROCESS<>\"Maximum\",1,IF(OR(NUM_DICE>2,GRADE=\"Commercial\"),16,IF(OR(LEFT(GRADE,1)=\"Q\",LEFT(GRADE,1)=\"M\",LEFT(SPEEDGRADE,3)=\"-2L\"),46,31)))","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Used Pl",{"$f":"IF(GTX_PLANES>0,MAX(IF($O4>0,1,0),INT((N116+N118/2)/N118),GTXPOWERPLANE),0)","v":0},6]
[null,null,null,null,null,null,null,null,null,null,null,null,"Avg Quad",{"$f":"IF(GTX_PLANES>0,NUM_GTS/GTX_PLANES/4,0)","v":0},{"$f":"\"O111:O11\" & TEXT(GTX_PLANES + 1,\"#\")","v":"O111:O111"}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Quads",null,{"$f":"IF(GTX_PLANES>0,MAX(MIN($N117,IF($O4*2<=NUM_GTS,NUM_GTS/8,NUM_GTS/4),INT((N116+N118/2)/N118*N118)),INT(GTXPOWERPLANE*N118)),0)","v":0},"MMF",null,"x^4","x^3","x^2","x","c"]
[null,null,null,null,null,null,null,null,null,null,null,null,"AVCCQ",{"$f":"O119*Y120*($R$120*390625+$S$120*15625+$T$120*625+$U$120*25+$V$120)/1000","v":0},{"$f":"O119*Y120*($R$120*TemperatureEstimate^4+$S$120*TemperatureEstimate^3+$T$120*TemperatureEstimate^2+$U$120*TemperatureEstimate+$V$120)/1000*P120","v":0},1,null,{"$f":"OFFSET(BLOCK_LEAKAGE,6,$U116)","v":3.8743880687599882E-9},{"$f":"OFFSET(BLOCK_LEAKAGE,6,$U116+1)","v":6.6997220269763771E-6},{"$f":"OFFSET(BLOCK_LEAKAGE,6,$U116+2)","v":1.1091806104240854E-3},{"$f":"OFFSET(BLOCK_LEAKAGE,6,$U116+3)","v":8.7707208420573238E-2},{"$f":"OFFSET(BLOCK_LEAKAGE,6,$U116+4)","v":2.854548824691669},{"$f":"OFFSET(BLOCK_LEAKAGE,10,1)","v":0.90615000000000001},{"$f":"OFFSET(BLOCK_LEAKAGE,10,2)","v":2.4011360000000002},{"$f":"(W120*EXP(X120*AVCC))/(W120*EXP(X120))","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,null,"AVTTQ",{"$f":"O119*Y121*($R$121*390625+$S$121*15625+$T$121*625+$U$121*25+$V$121)/1000","v":0},{"$f":"O119*Y121*($R$121*TemperatureEstimate^4+$S$121*TemperatureEstimate^3+$T$121*TemperatureEstimate^2+$U$121*TemperatureEstimate+$V$121)/1000","v":0},1,null,{"$f":"OFFSET(BLOCK_LEAKAGE,6,$U116+5)","v":2.9566926386627962E-9},{"$f":"OFFSET(BLOCK_LEAKAGE,6,$U116+6)","v":6.8619488188000005E-8},{"$f":"OFFSET(BLOCK_LEAKAGE,6,$U116+7)","v":3.0651708042157973E-5},{"$f":"OFFSET(BLOCK_LEAKAGE,6,$U116+8)","v":4.0665640160207992E-3},{"$f":"OFFSET(BLOCK_LEAKAGE,6,$U116+9)","v":2.6746258995502563},{"$f":"OFFSET(BLOCK_LEAKAGE,10,3)","v":1.0000709999999999},{"$f":"OFFSET(BLOCK_LEAKAGE,10,4)","v":-0.20008500000000001},{"$f":"W121*AVTT+X121","v":1.0000001999999999}]
[null,null,null,null,null,null,null,null,null,null,null,null,"AUXQ",{"$f":"O119*($R$122*390625+$S$122*15625+$T$122*625+$U$122*25+$V$122)/1000","v":0},{"$f":"O119*($R$122*TemperatureEstimate^4+$S$122*TemperatureEstimate^3+$T$122*TemperatureEstimate^2+$U$122*TemperatureEstimate+$V$122)/1000","v":0},1,null,{"$f":"OFFSET(BLOCK_LEAKAGE,6,$U116+10)","v":6.4860950108070533E-9},{"$f":"OFFSET(BLOCK_LEAKAGE,6,$U116+11)","v":-2.8492648783160272E-7},{"$f":"OFFSET(BLOCK_LEAKAGE,6,$U116+12)","v":-3.2614893996764716E-6},{"$f":"OFFSET(BLOCK_LEAKAGE,6,$U116+13)","v":6.0933950674031689E-4},{"$f":"OFFSET(BLOCK_LEAKAGE,6,$U116+14)","v":-4.5971262032672988E-3}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(O120:O121)","v":0},{"$f":"IF(NUM_GTS>0,AVCCQ*AVCC + AVTTQ*AVTT + GTXAUXQ*GTVCCAUX,0)","v":0}]

{"sheet":"GTH","index":15,"n_rows":123,"n_cols":55,"rows_kept":123,"cut":false,"hidden":false,"merged":[[11,1,11,3],[12,1,12,3],[13,1,13,3],[14,1,14,3],[16,1,16,3],[3,1,3,2],[10,1,10,3],[0,1,0,23],[2,5,2,9],[3,12,3,13],[6,12,6,13],[2,12,2,15],[2,19,2,21],[10,13,10,17],[2,1,2,3],[8,7,8,10],[4,19,4,21],[4,12,4,13],[10,9,10,12],[6,19,6,21],[8,12,8,13],[5,12,5,13],[25,1,25,3],[26,1,26,3],[21,1,21,3],[22,1,22,3],[15,1,15,3],[19,1,19,3],[23,1,23,3],[20,1,20,3],[18,1,18,3],[24,1,24,3],[17,1,17,3],[27,1,27,3],[28,1,28,3],[31,1,31,3],[34,1,34,3],[32,1,32,3],[41,1,41,3],[44,1,44,3],[39,1,39,3],[40,1,40,3],[38,1,38,3],[29,1,29,3],[37,1,37,3],[30,1,30,3],[36,1,36,3],[33,1,33,3],[74,1,74,3],[52,1,52,3],[53,1,53,3],[56,1,56,3],[35,1,35,3],[51,1,51,3],[42,1,42,3],[43,1,43,3],[45,1,45,3],[50,1,50,3],[47,1,47,3],[48,1,48,3],[46,1,46,3],[49,1,49,3],[67,1,67,3],[73,1,73,3],[54,1,54,3],[55,1,55,3],[58,1,58,3],[57,1,57,3],[59,1,59,3],[60,1,60,3],[68,1,68,3],[72,1,72,3],[64,1,64,3],[65,1,65,3],[63,1,63,3],[66,1,66,3],[69,1,69,3],[70,1,70,3],[62,1,62,3],[71,1,71,3],[61,1,61,3],[88,1,88,3],[86,1,86,3],[87,1,87,3],[83,1,83,3],[82,1,82,3],[78,1,78,3],[75,1,75,3],[84,1,84,3],[85,1,85,3],[76,1,76,3],[79,1,79,3],[80,1,80,3],[81,1,81,3],[77,1,77,3],[105,1,105,21],[98,1,98,3],[89,1,89,3],[90,1,90,3],[97,1,97,3],[92,1,92,3],[93,1,93,3],[94,1,94,3],[95,1,95,3],[96,1,96,3],[99,1,99,3],[91,1,91,3]]}
[null,"GTH Transceiver Power",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(PROCESS<>\"Maximum\",1,1)","v":1},{"$f":"IF(PROCESS<>\"Maximum\",1,1)","v":1},{"$f":"IF(RIGHT(SPEEDGRADE,3)=\"9V)\",10.3125,IF(OR(LEFT(PACKAGE,3)=\"FBV\",AND(LEFT(SPEEDGRADE,2)=\"-1\",LEFT(SPEEDGRADE,3)<>\"-1H\")),12.5,16.375))","v":16.375},null,"CPLL VCO range (MHz)","LC VCO range (MHz)",null,null,null,"Raised Voltage",null,null,null,null,null,null,null,{"$f":"IF(AND(NUM_CMACS>0,NUM_ILMACS>0),\"AR1:AR9\",IF(NUM_CMACS>0,\"AR1:AR6\",\"AR1:AR3\"))","v":"AR1:AR9"},null,{"$f":"\"AT2:AT17\"","v":"AT2:AT17"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,8,9.8000000000000007,{"$f":"IF(LEFT(SPEEDGRADE,2)=\"-1\",8.5,12.5)","v":12.5},null,{"$f":"IF(K3>0,COUNTIF(K13:K100,\">10.3125\")+COUNTIF(O13:O100,\">10.3125\"),0)","v":0},null,null,null,null,null,null,null,null,"PCIe",null,269]
[null,"Active Current",null,null,null,"Transceiver Power",null,null,null,null,{"$f":"SUM(G6:G9)-I6","v":17.663842814539279},null,"Utilization",null,null,null,null,null,null,"Transceivers User Guide",null,null,null,null,null,null,null,null,null,6.25,13,16.375,null,null,null,null,null,null,null,null,null,null,null,"PCIe500",null,336]
[null,"Source",null,"Active",null,null,null,null,null,null,null,null,"GTH Channels",null,{"$f":"SUM(E13:E100)","v":60},{"$f":"IF(NUM_GTHS>0,O4/NUM_GTHS,\"N/A\")","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CMAC",null,407]
[null,"VCCINT",{"$f":"VCCINT","v":0.95},{"$f":"IF(GTH_INTPOWER>0,GTH_INTPOWER/VCCINT,0)","v":2.035839445509688},null,"Source","Power",null,"Hard IP","PCS","PMA",null,"PCIe Blocks",null,{"$f":"COUNTIF(AR13:AR100,\">0\")","v":0},{"$f":"IF(NUM_PCIES>0,O5/NUM_PCIES,\"N/A\")","v":0},null,null,null,"XPE User Guide",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CMAC-Low",null,474]
[null,"MGTVCCAUX",{"$f":"GTVCCAUX","v":1.8},{"$f":"IF(GTH_AUXPOWER>0,GTH_AUXPOWER/GTVCCAUX,0)","v":0.2144323232323232},null,"VCCINT",{"$f":"IF(NUM_GTHS>0,SUM(U13:U100),0)","v":1.9340474732342037},null,{"$f":"IF(NUM_GTHS>0,(VCCINT/1000)*VCCINT_N*(SUM(AR13:AR100)+SUM(AV13:AV100)+SUM(AW13:AW100)),0)*PL_POWERED","v":0},{"$f":"GTH_INTPOWER-I6-((VCCINT/1000)*VCCINT_N*SUM(AS13:AS100))","v":1.9340474732342037},{"$f":"SUM(G7:G9)+((VCCINT/1000)*VCCINT_N*SUM(AS13:AS100))","v":15.729795341305078},null,"CMAC Blocks",null,{"$f":"COUNTIF(AV13:AV100,\">0\")","v":0},{"$f":"IF(NUM_CMACS>0,O6/NUM_CMACS,\"N/A\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CMAC-High",null,543]
[null,"MGTAVCC",{"$f":"AVCC","v":1},{"$f":"IF(NUM_GTHS>1,GTH_AVDD/AVCC,0)","v":10.696823639486896},null,"VCCAUX",{"$f":"IF(NUM_GTHS>0,SUM(V13:V100),0)","v":0.38597818181818178},null,null,null,null,null,"ILKN Blocks",null,{"$f":"COUNTIF(AW13:AW100,\">0\")","v":0},{"$f":"IF(NUM_ILMACS>0,O7/NUM_ILMACS,\"N/A\")","v":0},null,null,null,"Introduction to XPE (video)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ILKN",null,609]
[null,"MGTAVTT",{"$f":"AVTT","v":1.2},{"$f":"IF(NUM_GTHS>1,GTH_VTTX/AVTT,0)","v":3.8724946},null,"MGTAVCC",{"$f":"IF(NUM_GTHS>0,SUM(W13:W100),0)","v":10.696823639486896},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ILKN-Low",null,677]
[null,null,null,null,null,"MGTAVTT",{"$f":"IF(NUM_GTHS>0,SUM(X13:X100),0)","v":4.6469935199999997},{"$f":"TEXT(GTH_POWER/TOTAL_POWER,\"0%\")&\" of total on-chip power \"&TEXT(TOTAL_POWER,\"0.000\")&\"W\"","v":"21% of total on-chip power 0.084W"},null,null,null,null,"Power Planes",null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ILKN-High",null,741]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,807]
[null,null,null,null,null,null,null,null,null,"RX",null,null,null,"TX",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,866]
[null,"Name",null,null,"GTH Channels","Operational Mode","EyeScan","Power Mode","Channels Sharing QPLL","Clock Source","Data Rate (Gb/s)","Data Path","Data Mode","Clock Source","Data Rate (Gb/s)","Data Path","Data Mode","O/P (mV)","OOB Used","Hard IP Block","VCCINT Power (W)","MGTVCCAUX Power (W)","MGTAVCC Power (W)","MGTAVTT Power (W)",null,"Operate Mode","Quads","RX VCO LC (MHz)","TX VCO LC (MHz)","RX VCO CPLL (MHz)","TX VCO CPLL (MHz)","RX USERCLK","TX USERCLK","Power Mode (LPM=0, DFE=1)","TX Voltage Swing Current","AVTT Current (CPLL)","AVTT Current (LC)","AVCC Current (RX)","AVCC Current (TX)","AVCC Current (CPLL)","AVCC Current (LC)","AVCC CLK","AVTT CLK","PCIe","Vccint RX",924,"LPM","cmac","ilkn","QPLL1 RX","QPLL1 TX","QPLL0RX","QPLL0TX","QPLL rx","QPLL tx"]
[null,null,null,null,58,"Transceiver","Off","DFE",4,"QPLL1",12.8,32,"8b/10b","QPLL1",12.8,32,"8b/10b",1092,"No",null,{"$f":"(VCCINT/1000)*VCCINT_N*($E13*(OFFSET(GTHE1_DATA,1,$AA$1)+OFFSET(GTHE1_DATA,1,2+$AA$1)*MAX($AF13,$AG13))+AR13+AV13+AW13)","v":1.9266152382174542},{"$f":"IF(AND(OR(Z13=2,J13=\"CPLL\"),OR(Z13=1,N13=\"CPLL\")),0,(IF(AND(Z13>1,LEFT(N13,4)=\"QPLL\"),AC13,IF(LEFT(J13,4)=\"QPLL\",AB13,0))*OFFSET(GTHE1_DATA,7,$AA$1+2)+OFFSET(GTHE1_DATA,7,$AA$1))/1000*AA13*GTVCCAUX)","v":0.3619854545454545},{"$f":"(AVCC/1000)*$E13*(SUM($AL13:$AP13)+IF($G13=\"On\",OFFSET(GTHE1_DATA,18,$AA$1),0))*OFFSET(POWER_SCALE,6,OFFSET(POWER_SCALE,1,1))","v":10.538142184941441},{"$f":"(AVTT/1000)*$E13*(($AQ13+$AJ13+$AK13+IF(Z13<>1,OFFSET(GTHE1_DATA,10,$Z$1)+$AI13+OFFSET(GTHE1_DATA,15,$Z$1),0)+IF(Z13<>2,OFFSET(GTHE1_DATA,11+$AH13,$Z$1)+OFFSET(GTHE1_DATA,11+$AH13,2+$Z$1)*$O13*1000,0)*OFFSET(POWER_SCALE,6,OFFSET(POWER_SCALE,1,1)))+IF($S13=\"Yes\",OFFSET(GTHE1_DATA,16,$AA$1),0))","v":4.5775061599999995},null,{"$f":"IF($F13=\"Receiver\",1,IF($F13=\"Transmitter\",2,3))","v":3},{"$f":"INT((E13+3)/4)","v":15},{"$f":"IF(OR($Z13=2,$J13=\"CPLL\"),0,1000*IF(AND($J13=\"QPLL1\",$AX13>=0),$AX13,IF($AZ13>=0,$AZ13,IF($AX13>=0,$AX13,MIN(MAX($J13,$AE$2),$AF$3)))))","v":12800},{"$f":"IF(OR($Z13=1,$N13=\"CPLL\"),0,1000*IF(AND($N13=\"QPLL1\",$AY13>=0),$AY13,IF($BA13>=0,$BA13,IF($AY13>=0,$AY13,MIN(MAX($N13,$AE$2),$AF$3)))))","v":12800},{"$f":"IF($Z13=2,0,1000*IF($K13/2 >= $AD$2,$K13/2,IF($K13 >=$AD$2,$K13,IF($K13*2>$AD$2,$K13*2,IF($K13*4>$AD$2,$K13*4)))))","v":6400},{"$f":"IF($Z13=1,0,IF($O13/2 >= $AD$2,$O13/2,IF($O13 >= $AD$2,$O13,IF($O13*2>$AD$2,$O13*2,IF($O13*4>$AD$2,$O13*4)))))*1000","v":6400},{"$f":" IF(AND($Z13<>2,$L13 > 0), $K13*1000/IF(AND($L13=64,LEFT($M13,3)=\"64b\"),32,IF(OR($M13=\"8b/10b\",INT($L13/10)*10=$L13),IF($L13>=32,40,20),IF($L13>=32,32,16))),0)","v":320},{"$f":" IF(AND($Z13<>1,$P13 > 0), $O13*1000/IF(AND($P13=64,LEFT($Q13,3)=\"64b\"),32,IF(OR($Q13=\"8b/10b\",INT($P13/10)*10=$P13),IF($P13>=32,40,20),IF($P13>=32,32,16))),0)","v":320},{"$f":"IF($H13=\"Low Power\",0,1)","v":1},{"$f":"IF($Z13>1,$R13^2*OFFSET(GTHE1_DATA,1,12)+$R13*OFFSET(GTHE1_DATA,2,12)+OFFSET(GTHE1_DATA,3,12),0)","v":29.263299999999997},{"$f":"IF(AND(Z13>1,N13=\"CPLL\"),AE13,IF(J13=\"CPLL\",AD13,0))*(OFFSET(GTHE1_DATA,5,2+$Z$1))+IF(AND(LEFT(J13,4)=\"QPLL\",LEFT(N13,4)=\"QPLL\"),0,OFFSET(GTHE1_DATA,5,$Z$1))","v":0},{"$f":"(IF(AND(Z13>2,LEFT(N13,4)=\"QPLL\",LEFT(J13,4)=\"QPLL\",N13<>J13),(AB13+AC13)/2,IF(AND(Z13>1,LEFT(N13,4)=\"QPLL\"),AC13,IF(AND(Z13<>2,LEFT(J13,4)=\"QPLL\"),AB13,0)))*OFFSET(GTHE1_DATA,8,2+$Z$1) + IF(AND(OR(Z13=2,J13=\"CPLL\"),OR(Z13=1,N13=\"CPLL\")),0,OFFSET(GTHE1_DATA,8,$Z$1)))*1/MAX(IF(E13>I13,I13,4),1)","v":15},{"$f":"IF(Z13=2,0,K13*1000*(OFFSET(GTHE1_DATA,3+$AH13+IF(J13=\"CPLL\",19,IF(K13<9,16,0)),2+$Z$1+IF($AH13=0,IF(AU13=4,7,IF(AU13=2,5,IF(AU13=1.5,3,0))))))+OFFSET(GTHE1_DATA,3+$AH13+IF(J13=\"CPLL\",19,IF(K13<9,16,0)),$Z$1+IF($AH13=0,IF(AU13=4,8,IF(AU13=2,6,IF(AU13=1.5,4,0)))))+IF(AND($AU13>1,K13>($AF$3/2)),OFFSET(GTHE1_DATA,3+$AH13+IF(J13=\"CPLL\",19,0),IF(K13<9,11,1)),0))","v":108.55079754601229},{"$f":"IF(Z13=1,0,O13*1000*OFFSET(GTHE1_DATA,2,2+$Z$1)+OFFSET(GTHE1_DATA,2,$Z$1))","v":49.241309090909091},{"$f":" IF(AND(Z13>1,N13=\"CPLL\"),AE13,IF(J13=\"CPLL\",AD13,0))*OFFSET(GTHE1_DATA,6,2+$Z$1) + IF(OR(AND(Z13<>2,J13=\"CPLL\"),AND(Z13<>1,N13=\"CPLL\")),OFFSET(GTHE1_DATA,6,$Z$1),0)","v":0},{"$f":"(IF(AND(Z13>2,LEFT(N13,4)=\"QPLL\",LEFT(J13,4)=\"QPLL\",N13<>J13),(AB13+AC13)/2,IF(AND(Z13>1,LEFT(N13,4)=\"QPLL\"),AC13,IF(AND(Z13<>2,LEFT(J13,4)=\"QPLL\"),AB13,0)))*OFFSET(GTHE1_DATA,9+IF(MAX(K13,O13)<9,12,0),2+$Z$1) + IF(AND(OR(Z13=2,J13=\"CPLL\"),OR(Z13=1,N13=\"CPLL\")),0,OFFSET(GTHE1_DATA,9+IF(MAX(K13,O13)<9,12,0),$Z$1)))*1/MAX(IF(E13>I13,I13,4),1)","v":11.4},{"$f":"OFFSET(GTHE1_DATA,13,$Z$1)","v":12.5},{"$f":"OFFSET(GTHE1_DATA,14,$Z$1)","v":1.6666666666666667},{"$f":"IF(AND(E13>0,LEFT(T13,4)=\"PCIe\"),OFFSET(PCIE_DATA,IF(K13<=2.5,9,IF(K13<=5,13,17))+IF(E13=1,1,IF(E13=2,2,IF(E13<5,3,4))),IF(RIGHT(T13,3)=\"500\",2,1)),0)","v":0},{"$f":"IF($Z13<>2,$E13*OFFSET(GTHE1_DATA,17,$AA$1),0)","v":0},973,{"$f":"IF(AND($AH13=0),IF(OR(K13>12.5,AB13>12500),4,IF(OR(K13>10.4,AB13>10400),2,IF(OR(K13>=9,AB13>=9000),1.5,1.5))),1)","v":1},{"$f":"IF(AND(E13>0,LEFT(T13,4)=\"CMAC\"),OFFSET(CMAC_DATA,1+IF(MAX(K13,Q14)>=25,1,0),1+(IF(MID(T13,6,1)=\"H\",0,IF(MID(T13,6,1)=\"L\",2,1)))),0)","v":0},{"$f":"IF(AND(E13>0,LEFT(T13,4)=\"ILKN\"),OFFSET(ILMAC_DATA,IF(K13<=16.4,2,1),1+IF(MID(T13,6,1)=\"H\",0,IF(MID(T13,6,1)=\"L\",2,1))),0)","v":0},{"$f":"IF(AND($K13>=$AE$2,$K13<=$AE$3),$K13,IF(AND($K13*2>=$AE$2,$K13*2<=$AE$3),$K13*2,IF(AND($K13*4>=$AE$2,$K13*4<=$AE$3),$K13*4,IF(AND($K13*8>=$AE$2,$K13*8<=$AE$3),$K13*8,IF(AND($K13*16>=$AE$2,$K13*16<=$AE$3),$K13*16,-1)))))","v":12.8},{"$f":"IF(AND($O13>=$AE$2,$O13<=$AE$3),$O13,IF(AND($O13*2>=$AE$2,$O13*2<=$AE$3),$O13*2,IF(AND($O13*4>=$AE$2,$O13*4<=$AE$3),$O13*4,IF(AND($O13*8>=$AE$2,$O13*8<=$AE$3),$O13*8,IF(AND($O13*16>=$AE$2,$O13*16<=$AE$3),$O13*16,-1)))))","v":12.8},{"$f":"IF(AND($K13>=$AF$2,$K13<=$AF$3),$K13,IF(AND($K13*2>=$AF$2,$K13*2<=$AF$3),$K13*2,IF(AND($K13*4>=$AF$2,$K13*4<=$AF$3),$K13*4,IF(AND($K13*8>=$AF$2,$K13*8<=$AF$3),$K13*8,IF(AND($K13*16>=$AF$2,$K13*16<=$AF$3),$K13*16,-1)))))","v":12.8},{"$f":"IF(AND($O13>=$AF$2,$O13<=$AF$3),$O13,IF(AND($O13*2>=$AF$2,$O13*2<=$AF$3),$O13*2,IF(AND($O13*4>=$AF$2,$O13*4<=$AF$3),$O13*4,IF(AND($O13*8>=$AF$2,$O13*8<=$AF$3),$O13*8,IF(AND($O13*16>=$AF$2,$O13*16<=$AF$3),$O13*16,-1)))))","v":12.8},{"$f":"IF($J13=\"QPLL1\",$AX13,$AZ13)","v":12.8},{"$f":"IF($N13=\"QPLL1\",$AY13,$BA13)","v":12.8}]
[null,null,null,null,2,"Transceiver","Off","Low Power",2,"QPLL1",1,32,"8b/10b","QPLL1",1,32,"8b/10b",269,"No",null,7.4322350167496058E-3,2.3992727272727273E-2,0.15868145454545454,6.9487359999999998E-2,null,{"$f":"IF($F14=\"Receiver\",1,IF($F14=\"Transmitter\",2,3))","v":3},1,{"$f":"IF(OR($Z14=2,$J14=\"CPLL\"),0,1000*IF(AND($J14=\"QPLL1\",$AX14>=0),$AX14,IF($AZ14>=0,$AZ14,IF($AX14>=0,$AX14,MIN(MAX($J14,$AE$2),$AF$3)))))","v":8000},{"$f":"IF(OR($Z14=1,$N14=\"CPLL\"),0,1000*IF(AND($N14=\"QPLL1\",$AY14>=0),$AY14,IF($BA14>=0,$BA14,IF($AY14>=0,$AY14,MIN(MAX($N14,$AE$2),$AF$3)))))","v":8000},{"$f":"IF($Z14=2,0,1000*IF($K14/2 >= $AD$2,$K14/2,IF($K14 >=$AD$2,$K14,IF($K14*2>$AD$2,$K14*2,IF($K14*4>$AD$2,$K14*4)))))","v":4000},{"$f":"IF($Z14=1,0,IF($O14/2 >= $AD$2,$O14/2,IF($O14 >= $AD$2,$O14,IF($O14*2>$AD$2,$O14*2,IF($O14*4>$AD$2,$O14*4)))))*1000","v":4000},25,25,0,7.9475999999999996,0,15,18.399999999999999,{"$f":"IF(Z14=1,0,O14*1000*OFFSET(GTHE1_DATA,2,2+$Z$1)+OFFSET(GTHE1_DATA,2,$Z$1))","v":20.440727272727273},{"$f":" IF(AND(Z14>1,N14=\"CPLL\"),AE14,IF(J14=\"CPLL\",AD14,0))*OFFSET(GTHE1_DATA,6,2+$Z$1) + IF(OR(J14=\"CPLL\",N14=\"CPLL\"),OFFSET(GTHE1_DATA,6,$Z$1),0)","v":0},28,12.5,1.6666666666666667,0,0,1018,{"$f":"IF(AND($AH14=0),IF(OR(K14>12.5,AB14>12500),4,IF(OR(K14>10.4,AB14>10400),2,IF(OR(K14>=9,AB14>=9000),1.5,1.5))),1)","v":1.5},0,0,{"$f":"IF(AND($K14>=$AE$2,$K14<=$AE$3),$K14,IF(AND($K14*2>=$AE$2,$K14*2<=$AE$3),$K14*2,IF(AND($K14*4>=$AE$2,$K14*4<=$AE$3),$K14*4,IF(AND($K14*8>=$AE$2,$K14*8<=$AE$3),$K14*8,IF(AND($K14*16>=$AE$2,$K14*16<=$AE$3),$K14*16,-1)))))","v":8},{"$f":"IF(AND($O14>=$AE$2,$O14<=$AE$3),$O14,IF(AND($O14*2>=$AE$2,$O14*2<=$AE$3),$O14*2,IF(AND($O14*4>=$AE$2,$O14*4<=$AE$3),$O14*4,IF(AND($O14*8>=$AE$2,$O14*8<=$AE$3),$O14*8,IF(AND($O14*16>=$AE$2,$O14*16<=$AE$3),$O14*16,-1)))))","v":8},{"$f":"IF(AND($K14>=$AF$2,$K14<=$AF$3),$K14,IF(AND($K14*2>=$AF$2,$K14*2<=$AF$3),$K14*2,IF(AND($K14*4>=$AF$2,$K14*4<=$AF$3),$K14*4,IF(AND($K14*8>=$AF$2,$K14*8<=$AF$3),$K14*8,IF(AND($K14*16>=$AF$2,$K14*16<=$AF$3),$K14*16,-1)))))","v":16},{"$f":"IF(AND($O14>=$AF$2,$O14<=$AF$3),$O14,IF(AND($O14*2>=$AF$2,$O14*2<=$AF$3),$O14*2,IF(AND($O14*4>=$AF$2,$O14*4<=$AF$3),$O14*4,IF(AND($O14*8>=$AF$2,$O14*8<=$AF$3),$O14*8,IF(AND($O14*16>=$AF$2,$O14*16<=$AF$3),$O14*16,-1)))))","v":16},{"$f":"IF($J14=\"QPLL1\",$AX14,$AZ14)","v":8},{"$f":"IF($N14=\"QPLL1\",$AY14,$BA14)","v":8}]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b",{"$f":"$J15","v":"QPLL1"},{"$f":"$K15","v":8},{"$f":"$L15","v":32},{"$f":"$M15","v":"8b/10b"},269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,1056,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,1092,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,1119,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b",{"$f":"$J45","v":"QPLL1"},{"$f":"$K45","v":8},{"$f":"$L45","v":32},{"$f":"$M45","v":"8b/10b"},269,"No",null,{"$f":"(VCCINT/1000)*VCCINT_N*($E45*(OFFSET(GTHE1_DATA,1,$AA$1)+OFFSET(GTHE1_DATA,1,2+$AA$1)*MAX($AF45,$AG45))+AR45+AV45+AW45)","v":0},{"$f":"IF(AND(OR(Z45=2,J45=\"CPLL\"),OR(Z45=1,N45=\"CPLL\")),0,(IF(AND(Z45>1,LEFT(N45,4)=\"QPLL\"),AC45,IF(LEFT(J45,4)=\"QPLL\",AB45,0))*OFFSET(GTHE1_DATA,7,$AA$1+2)+OFFSET(GTHE1_DATA,7,$AA$1))/1000*AA45*GTVCCAUX)","v":0},{"$f":"(AVCC/1000)*$E45*(SUM($AL45:$AP45)+IF($G45=\"On\",OFFSET(GTHE1_DATA,18,$AA$1),0))*OFFSET(POWER_SCALE,6,OFFSET(POWER_SCALE,1,1))","v":0},{"$f":"(AVTT/1000)*$E45*(($AQ45+$AJ45+$AK45+IF(Z45<>1,OFFSET(GTHE1_DATA,10,$Z$1)+$AI45+OFFSET(GTHE1_DATA,15,$Z$1),0)+IF(Z45<>2,OFFSET(GTHE1_DATA,11+$AH45,$Z$1)+OFFSET(GTHE1_DATA,11+$AH45,2+$Z$1)*$O45*1000,0)*OFFSET(POWER_SCALE,6,OFFSET(POWER_SCALE,1,1)))+IF($S45=\"Yes\",OFFSET(GTHE1_DATA,16,$AA$1),0))","v":0},null,3,{"$f":"INT((E45+3)/4)","v":0},8000,8000,4000,4000,{"$f":" IF(AND($Z45<>2,$L45 > 0), $K45*1000/IF(AND($L45=64,LEFT($M45,3)=\"64b\"),32,IF(OR($M45=\"8b/10b\",INT($L45/10)*10=$L45),IF($L45>=32,40,20),IF($L45>=32,32,16))),0)","v":200},{"$f":" IF(AND($Z45<>1,$P45 > 0), $O45*1000/IF(AND($P45=64,LEFT($Q45,3)=\"64b\"),32,IF(OR($Q45=\"8b/10b\",INT($P45/10)*10=$P45),IF($P45>=32,40,20),IF($P45>=32,32,16))),0)","v":200},{"$f":"IF($H45=\"Low Power\",0,1)","v":0},{"$f":"IF($Z45>1,$R45^2*OFFSET(GTHE1_DATA,1,12)+$R45*OFFSET(GTHE1_DATA,2,12)+OFFSET(GTHE1_DATA,3,12),0)","v":7.9475999999999996},{"$f":"IF(AND(Z45>1,N45=\"CPLL\"),AE45,IF(J45=\"CPLL\",AD45,0))*(OFFSET(GTHE1_DATA,5,2+$Z$1))+IF(AND(LEFT(J45,4)=\"QPLL\",LEFT(N45,4)=\"QPLL\"),0,OFFSET(GTHE1_DATA,5,$Z$1))","v":0},{"$f":"(IF(AND(Z45>2,LEFT(N45,4)=\"QPLL\",LEFT(J45,4)=\"QPLL\",N45<>J45),(AB45+AC45)/2,IF(AND(Z45>1,LEFT(N45,4)=\"QPLL\"),AC45,IF(AND(Z45<>2,LEFT(J45,4)=\"QPLL\"),AB45,0)))*OFFSET(GTHE1_DATA,8,2+$Z$1) + IF(AND(OR(Z45=2,J45=\"CPLL\"),OR(Z45=1,N45=\"CPLL\")),0,OFFSET(GTHE1_DATA,8,$Z$1)))*1/MAX(IF(E45>I45,I45,4),1)","v":15},{"$f":"IF(Z45=2,0,K45*1000*(OFFSET(GTHE1_DATA,3+$AH45+IF(J45=\"CPLL\",19,IF(K45<9,16,0)),2+$Z$1+IF($AH45=0,IF(AU45=4,7,IF(AU45=2,5,IF(AU45=1.5,3,0))))))+OFFSET(GTHE1_DATA,3+$AH45+IF(J45=\"CPLL\",19,IF(K45<9,16,0)),$Z$1+IF($AH45=0,IF(AU45=4,8,IF(AU45=2,6,IF(AU45=1.5,4,0)))))+IF(AND($AU45>1,K45>($AF$3/2)),OFFSET(GTHE1_DATA,3+$AH45+IF(J45=\"CPLL\",19,0),IF(K45<9,11,1)),0))","v":35.200000000000003},37.525818181818181,0,{"$f":"(IF(AND(Z45>2,LEFT(N45,4)=\"QPLL\",LEFT(J45,4)=\"QPLL\",N45<>J45),(AB45+AC45)/2,IF(AND(Z45>1,LEFT(N45,4)=\"QPLL\"),AC45,IF(AND(Z45<>2,LEFT(J45,4)=\"QPLL\"),AB45,0)))*OFFSET(GTHE1_DATA,9+IF(MAX(K45,O45)<9,12,0),2+$Z$1) + IF(AND(OR(Z45=2,J45=\"CPLL\"),OR(Z45=1,N45=\"CPLL\")),0,OFFSET(GTHE1_DATA,9+IF(MAX(K45,O45)<9,12,0),$Z$1)))*1/MAX(IF(E45>I45,I45,4),1)","v":28},12.5,{"$f":"OFFSET(GTHE1_DATA,14,$Z$1)","v":1.6666666666666667},{"$f":"IF(AND(E45>0,LEFT(T45,4)=\"PCIe\"),OFFSET(PCIE_DATA,IF(K45<=2.5,9,IF(K45<=5,13,17))+IF(E45=1,1,IF(E45=2,2,IF(E45<5,3,4))),IF(RIGHT(T45,3)=\"500\",2,1)),0)","v":0},{"$f":"IF($Z45<>2,$E45*OFFSET(GTHE1_DATA,17,$AA$1),0)","v":0},null,1.5,{"$f":"IF(AND(E45>0,LEFT(T45,4)=\"CMAC\"),OFFSET(CMAC_DATA,1+IF(MAX(K45,Q46)>=25,1,0),1+(IF(MID(T45,6,1)=\"H\",0,IF(MID(T45,6,1)=\"L\",2,1)))),0)","v":0},{"$f":"IF(AND(E45>0,LEFT(T45,4)=\"ILKN\"),OFFSET(ILMAC_DATA,IF(K45<=16.4,2,1),1+IF(MID(T45,6,1)=\"H\",0,IF(MID(T45,6,1)=\"L\",2,1))),0)","v":0},8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b",{"$f":"$J77","v":"QPLL1"},{"$f":"$K77","v":8},{"$f":"$L77","v":32},{"$f":"$M77","v":"8b/10b"},269,"No",null,{"$f":"(VCCINT/1000)*VCCINT_N*($E77*(OFFSET(GTHE1_DATA,1,$AA$1)+OFFSET(GTHE1_DATA,1,2+$AA$1)*MAX($AF77,$AG77))+AR77+AV77+AW77)","v":0},{"$f":"IF(AND(OR(Z77=2,J77=\"CPLL\"),OR(Z77=1,N77=\"CPLL\")),0,(IF(AND(Z77>1,LEFT(N77,4)=\"QPLL\"),AC77,IF(LEFT(J77,4)=\"QPLL\",AB77,0))*OFFSET(GTHE1_DATA,7,$AA$1+2)+OFFSET(GTHE1_DATA,7,$AA$1))/1000*AA77*GTVCCAUX)","v":0},{"$f":"(AVCC/1000)*$E77*(SUM($AL77:$AP77)+IF($G77=\"On\",OFFSET(GTHE1_DATA,18,$AA$1),0))*OFFSET(POWER_SCALE,6,OFFSET(POWER_SCALE,1,1))","v":0},{"$f":"(AVTT/1000)*$E77*(($AQ77+$AJ77+$AK77+IF(Z77<>1,OFFSET(GTHE1_DATA,10,$Z$1)+$AI77+OFFSET(GTHE1_DATA,15,$Z$1),0)+IF(Z77<>2,OFFSET(GTHE1_DATA,11+$AH77,$Z$1)+OFFSET(GTHE1_DATA,11+$AH77,2+$Z$1)*$O77*1000,0)*OFFSET(POWER_SCALE,6,OFFSET(POWER_SCALE,1,1)))+IF($S77=\"Yes\",OFFSET(GTHE1_DATA,16,$AA$1),0))","v":0},null,3,{"$f":"INT((E77+3)/4)","v":0},8000,8000,4000,4000,{"$f":" IF(AND($Z77<>2,$L77 > 0), $K77*1000/IF(AND($L77=64,LEFT($M77,3)=\"64b\"),32,IF(OR($M77=\"8b/10b\",INT($L77/10)*10=$L77),IF($L77>=32,40,20),IF($L77>=32,32,16))),0)","v":200},{"$f":" IF(AND($Z77<>1,$P77 > 0), $O77*1000/IF(AND($P77=64,LEFT($Q77,3)=\"64b\"),32,IF(OR($Q77=\"8b/10b\",INT($P77/10)*10=$P77),IF($P77>=32,40,20),IF($P77>=32,32,16))),0)","v":200},{"$f":"IF($H77=\"Low Power\",0,1)","v":0},{"$f":"IF($Z77>1,$R77^2*OFFSET(GTHE1_DATA,1,12)+$R77*OFFSET(GTHE1_DATA,2,12)+OFFSET(GTHE1_DATA,3,12),0)","v":7.9475999999999996},{"$f":"IF(AND(Z77>1,N77=\"CPLL\"),AE77,IF(J77=\"CPLL\",AD77,0))*(OFFSET(GTHE1_DATA,5,2+$Z$1))+IF(AND(LEFT(J77,4)=\"QPLL\",LEFT(N77,4)=\"QPLL\"),0,OFFSET(GTHE1_DATA,5,$Z$1))","v":0},{"$f":"(IF(AND(Z77>2,LEFT(N77,4)=\"QPLL\",LEFT(J77,4)=\"QPLL\",N77<>J77),(AB77+AC77)/2,IF(AND(Z77>1,LEFT(N77,4)=\"QPLL\"),AC77,IF(AND(Z77<>2,LEFT(J77,4)=\"QPLL\"),AB77,0)))*OFFSET(GTHE1_DATA,8,2+$Z$1) + IF(AND(OR(Z77=2,J77=\"CPLL\"),OR(Z77=1,N77=\"CPLL\")),0,OFFSET(GTHE1_DATA,8,$Z$1)))*1/MAX(IF(E77>I77,I77,4),1)","v":15},{"$f":"IF(Z77=2,0,K77*1000*(OFFSET(GTHE1_DATA,3+$AH77+IF(J77=\"CPLL\",19,IF(K77<9,16,0)),2+$Z$1+IF($AH77=0,IF(AU77=4,7,IF(AU77=2,5,IF(AU77=1.5,3,0))))))+OFFSET(GTHE1_DATA,3+$AH77+IF(J77=\"CPLL\",19,IF(K77<9,16,0)),$Z$1+IF($AH77=0,IF(AU77=4,8,IF(AU77=2,6,IF(AU77=1.5,4,0)))))+IF(AND($AU77>1,K77>($AF$3/2)),OFFSET(GTHE1_DATA,3+$AH77+IF(J77=\"CPLL\",19,0),IF(K77<9,11,1)),0))","v":35.200000000000003},37.525818181818181,0,{"$f":"(IF(AND(Z77>2,LEFT(N77,4)=\"QPLL\",LEFT(J77,4)=\"QPLL\",N77<>J77),(AB77+AC77)/2,IF(AND(Z77>1,LEFT(N77,4)=\"QPLL\"),AC77,IF(AND(Z77<>2,LEFT(J77,4)=\"QPLL\"),AB77,0)))*OFFSET(GTHE1_DATA,9+IF(MAX(K77,O77)<9,12,0),2+$Z$1) + IF(AND(OR(Z77=2,J77=\"CPLL\"),OR(Z77=1,N77=\"CPLL\")),0,OFFSET(GTHE1_DATA,9+IF(MAX(K77,O77)<9,12,0),$Z$1)))*1/MAX(IF(E77>I77,I77,4),1)","v":28},{"$f":"OFFSET(GTHE1_DATA,13,$Z$1)","v":12.5},{"$f":"OFFSET(GTHE1_DATA,14,$Z$1)","v":1.6666666666666667},{"$f":"IF(AND(E77>0,LEFT(T77,4)=\"PCIe\"),OFFSET(PCIE_DATA,IF(K77<=2.5,9,IF(K77<=5,13,17))+IF(E77=1,1,IF(E77=2,2,IF(E77<5,3,4))),IF(RIGHT(T77,3)=\"500\",2,1)),0)","v":0},{"$f":"IF($Z77<>2,$E77*OFFSET(GTHE1_DATA,17,$AA$1),0)","v":0},null,1.5,{"$f":"IF(AND(E77>0,LEFT(T77,4)=\"CMAC\"),OFFSET(CMAC_DATA,1+IF(MAX(K77,Q78)>=25,1,0),1+(IF(MID(T77,6,1)=\"H\",0,IF(MID(T77,6,1)=\"L\",2,1)))),0)","v":0},{"$f":"IF(AND(E77>0,LEFT(T77,4)=\"ILKN\"),OFFSET(ILMAC_DATA,IF(K77<=16.4,2,1),1+IF(MID(T77,6,1)=\"H\",0,IF(MID(T77,6,1)=\"L\",2,1))),0)","v":0},8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,{"$f":"IF($F78=\"Receiver\",1,IF($F78=\"Transmitter\",2,3))","v":3},0,{"$f":"IF(OR($Z78=2,$J78=\"CPLL\"),0,1000*IF(AND($J78=\"QPLL1\",$AX78>=0),$AX78,IF($AZ78>=0,$AZ78,IF($AX78>=0,$AX78,MIN(MAX($J78,$AE$2),$AF$3)))))","v":8000},{"$f":"IF(OR($Z78=1,$N78=\"CPLL\"),0,1000*IF(AND($N78=\"QPLL1\",$AY78>=0),$AY78,IF($BA78>=0,$BA78,IF($AY78>=0,$AY78,MIN(MAX($N78,$AE$2),$AF$3)))))","v":8000},{"$f":"IF($Z78=2,0,1000*IF($K78/2 >= $AD$2,$K78/2,IF($K78 >=$AD$2,$K78,IF($K78*2>$AD$2,$K78*2,IF($K78*4>$AD$2,$K78*4)))))","v":4000},{"$f":"IF($Z78=1,0,IF($O78/2 >= $AD$2,$O78/2,IF($O78 >= $AD$2,$O78,IF($O78*2>$AD$2,$O78*2,IF($O78*4>$AD$2,$O78*4)))))*1000","v":4000},200,200,0,7.9475999999999996,0,15,35.200000000000003,{"$f":"IF(Z78=1,0,O78*1000*OFFSET(GTHE1_DATA,2,2+$Z$1)+OFFSET(GTHE1_DATA,2,$Z$1))","v":37.525818181818181},{"$f":" IF(AND(Z78>1,N78=\"CPLL\"),AE78,IF(J78=\"CPLL\",AD78,0))*OFFSET(GTHE1_DATA,6,2+$Z$1) + IF(OR(J78=\"CPLL\",N78=\"CPLL\"),OFFSET(GTHE1_DATA,6,$Z$1),0)","v":0},28,12.5,1.6666666666666667,0,0,null,{"$f":"IF(AND($AH78=0),IF(OR(K78>12.5,AB78>12500),4,IF(OR(K78>10.4,AB78>10400),2,IF(OR(K78>=9,AB78>=9000),1.5,1.5))),1)","v":1.5},0,0,{"$f":"IF(AND($K78>=$AE$2,$K78<=$AE$3),$K78,IF(AND($K78*2>=$AE$2,$K78*2<=$AE$3),$K78*2,IF(AND($K78*4>=$AE$2,$K78*4<=$AE$3),$K78*4,IF(AND($K78*8>=$AE$2,$K78*8<=$AE$3),$K78*8,IF(AND($K78*16>=$AE$2,$K78*16<=$AE$3),$K78*16,-1)))))","v":8},{"$f":"IF(AND($O78>=$AE$2,$O78<=$AE$3),$O78,IF(AND($O78*2>=$AE$2,$O78*2<=$AE$3),$O78*2,IF(AND($O78*4>=$AE$2,$O78*4<=$AE$3),$O78*4,IF(AND($O78*8>=$AE$2,$O78*8<=$AE$3),$O78*8,IF(AND($O78*16>=$AE$2,$O78*16<=$AE$3),$O78*16,-1)))))","v":8},{"$f":"IF(AND($K78>=$AF$2,$K78<=$AF$3),$K78,IF(AND($K78*2>=$AF$2,$K78*2<=$AF$3),$K78*2,IF(AND($K78*4>=$AF$2,$K78*4<=$AF$3),$K78*4,IF(AND($K78*8>=$AF$2,$K78*8<=$AF$3),$K78*8,IF(AND($K78*16>=$AF$2,$K78*16<=$AF$3),$K78*16,-1)))))","v":16},{"$f":"IF(AND($O78>=$AF$2,$O78<=$AF$3),$O78,IF(AND($O78*2>=$AF$2,$O78*2<=$AF$3),$O78*2,IF(AND($O78*4>=$AF$2,$O78*4<=$AF$3),$O78*4,IF(AND($O78*8>=$AF$2,$O78*8<=$AF$3),$O78*8,IF(AND($O78*16>=$AF$2,$O78*16<=$AF$3),$O78*16,-1)))))","v":16},{"$f":"IF($J78=\"QPLL1\",$AX78,$AZ78)","v":8},{"$f":"IF($N78=\"QPLL1\",$AY78,$BA78)","v":8}]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,1.5,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",269,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,7.9475999999999996,0,15,35.200000000000003,37.525818181818181,0,28,12.5,1.6666666666666667,0,0,null,{"$f":"IF(AND($AH100=0),IF(OR(K100>12.5,AB100>12500),4,IF(OR(K100>10.4,AB100>10400),2,IF(OR(K100>=9,AB100>=9000),1.5,1.5))),1)","v":1.5},0,0,8,8,16,16,8,8]
[null,{"$f":"ROW(GTHROWS)-13","v":88},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AR13:AR100)","v":0},null,null,null,{"$f":"SUM(AV13:AV100)","v":0},{"$f":"SUM(AW13:AW100)","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VCO MIN",null,null,null,{"$f":"1.6","v":1.6}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VCO MAX",null,null,null,{"$f":" 4","v":4}]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,null,2]
[null,null,null,null,null,null,null,null,3]
[null,null,null,null,null,null,null,null,4,null,null,null,60]
[null,null,null,null,null,null,null,null,5,null,null,"Power Planes",3]
[null,null,null,null,null,null,null,null,6,null,null,"Used Quad",{"$f":"INT((O4+3)/4)","v":15},null,null,null,null,null,null,null,{"$f":"IF(PROCESS<>\"Maximum\",1,IF(OR(NUM_DICE>5, GRADE=\"Commercial\",ISOLY),16,IF(OR(LEFT(GRADE,1)=\"Q\",LEFT(GRADE,1)=\"M\",LEFT(SPEEDGRADE,3)=\"-2L\"),46,31)))","v":1}]
[null,null,null,null,null,null,null,null,7,null,null,"Used Pl",{"$f":"IF(GTH_PLANES>0,MAX(INT((M116+M118/2)/M118),GTHPOWERPLANE),0)","v":3}]
[null,null,null,null,null,null,null,null,8,null,null,"Avg Quad",{"$f":"IF(GTH_PLANES>0,M114/GTH_PLANES/4,0)","v":5},{"$f":"\"I110:I1\" & TEXT(10+GTH_PLANES,\"#\")","v":"I110:I113"}]
[null,null,null,null,null,null,null,null,9,null,null,"Quads",null,{"$f":"IF(GTH_PLANES>0,MAX(MIN(IF(O4>0,1,0),IF($O4*2<=M114,M114/8,M114/4),INT((M116+M118/2)/M118*M118)),INT(GTHPOWERPLANE*M118)),0)","v":15},null,"MMF",null,null,"x^4","x^3","x^2","x","c"]
[null,null,null,null,null,null,null,null,10,null,null,"AVCCQ",{"$f":"N119*O120*Z120*($S$120*390625+$T$120*15625+$U$120*625+$V$120*25+$W$120)/1000","v":8.7699952593478778E-2},{"$f":"N119*Z120*($S$120*TemperatureEstimate^4+$T$120*TemperatureEstimate^3+$U$120*TemperatureEstimate^2+$V$120*TemperatureEstimate+$W$120)/1000*O120","v":0.3308571672145097},1,null,null,null,{"$f":"OFFSET(BLOCK_LEAKAGE,7,$U116)","v":3.8743880687599882E-9},{"$f":"OFFSET(BLOCK_LEAKAGE,7,$U116+1)","v":6.6997220269763771E-6},{"$f":"OFFSET(BLOCK_LEAKAGE,7,$U116+2)","v":1.1091806104240854E-3},{"$f":"OFFSET(BLOCK_LEAKAGE,7,$U116+3)","v":8.7707208420573238E-2},{"$f":"OFFSET(BLOCK_LEAKAGE,7,$U116+4)","v":2.854548824691669},{"$f":"OFFSET(BLOCK_LEAKAGE,10,1)","v":0.90615000000000001},{"$f":"OFFSET(BLOCK_LEAKAGE,10,2)","v":2.4011360000000002},{"$f":"(X120*EXP(Y120*AVCC))/(X120*EXP(Y120))","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,"AVTTQ",{"$f":"N119*O121*Z121*($S$121*390625+$T$121*15625+$U$121*625+$V$121*25+$W$121)/1000","v":0.15446514771865402},{"$f":"N119*Z121*($S$121*TemperatureEstimate^4+$T$121*TemperatureEstimate^3+$U$121*TemperatureEstimate^2+$V$121*TemperatureEstimate+$W$121)/1000*O121","v":0.16370899246771675},1,null,null,null,{"$f":"OFFSET(BLOCK_LEAKAGE,7,$U116+5)","v":2.9566926386627962E-9},{"$f":"OFFSET(BLOCK_LEAKAGE,7,$U116+6)","v":6.8619488188000005E-8},{"$f":"OFFSET(BLOCK_LEAKAGE,7,$U116+7)","v":3.0651708042157973E-5},{"$f":"OFFSET(BLOCK_LEAKAGE,7,$U116+8)","v":4.0665640160207992E-3},{"$f":"OFFSET(BLOCK_LEAKAGE,7,$U116+9)","v":10.174625899550261},{"$f":"OFFSET(BLOCK_LEAKAGE,10,3)","v":1.0000709999999999},{"$f":"OFFSET(BLOCK_LEAKAGE,10,4)","v":-0.20008500000000001},{"$f":"X121*AVTT+Y121","v":1.0000001999999999}]
[null,null,null,null,null,null,null,null,null,null,null,"AUXQ",{"$f":"N119*O122*($S$122*390625+$T$122*15625+$U$122*625+$V$122*25+$W$122)/1000","v":1.0019377622505813E-4},{"$f":"N119*($S$122*TemperatureEstimate^4+$T$122*TemperatureEstimate^3+$U$122*TemperatureEstimate^2+$V$122*TemperatureEstimate+$W$122)/1000*O122","v":2.6131185913682684E-3},1,null,null,null,{"$f":"OFFSET(BLOCK_LEAKAGE,7,$U116+10)","v":6.4860950108070533E-9},{"$f":"OFFSET(BLOCK_LEAKAGE,7,$U116+11)","v":-2.8492648783160272E-7},{"$f":"OFFSET(BLOCK_LEAKAGE,7,$U116+12)","v":-3.2614893996764716E-6},{"$f":"OFFSET(BLOCK_LEAKAGE,7,$U116+13)","v":6.0933950674031689E-4},{"$f":"OFFSET(BLOCK_LEAKAGE,7,$U116+14)","v":-4.5971262032672988E-3}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N120:N121)","v":0.49456615968222645},{"$f":"IF(NUM_GTHS>0,GTHAVCCQ*AVCC +GTHVTTXQ*AVTT +GTHAUXQ*GTVCCAUX,0)","v":0.53201157164023272}]

{"sheet":"PS","index":16,"n_rows":48,"n_cols":27,"rows_kept":48,"cut":false,"hidden":true,"merged":[[0,1,0,15],[19,1,19,3],[32,2,32,3],[33,2,33,3],[29,2,29,3],[31,2,31,3],[30,2,30,3],[20,2,20,3],[21,2,21,3],[22,2,22,3],[23,2,23,3],[25,2,25,3],[27,2,27,3],[28,2,28,3],[24,2,24,3],[26,2,26,3],[4,12,4,14],[2,1,2,3],[2,12,2,15],[3,1,3,2],[11,9,11,10],[7,8,7,10],[11,1,11,3],[8,8,8,10],[9,8,9,10],[12,9,12,10],[14,9,14,10],[13,9,13,10],[2,5,2,9],[16,1,16,3],[38,1,38,3],[35,2,35,3],[17,1,17,3],[12,1,12,3],[44,1,44,3],[34,2,34,3],[36,2,36,3],[45,1,45,3],[46,1,46,3],[47,1,47,3],[39,1,39,3],[40,1,40,3],[41,1,41,3],[42,1,42,3],[43,1,43,3]]}
[null,"PS Power",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Leakage",{"$f":"(S3*C6+S5*C8)/1000","v":0},null,null,null,null,null,null,{"$f":"IF(E18=\"LPDDR2\",\"Z2\",IF(E18=\"DDR3\",\"Z2:Z5\",\"Z2:Z6\"))","v":"Z2:Z6"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pint",{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",OFFSET(PS_DATA,1,5)*IF(PROCESS=\"Typical\",0.805,OFFSET(PS_DATA,PSFACTOROW,8)*OFFSET(PS_DATA,1,19)),0)*Vcc_c1*EXP(Vcc_c2*VCCPINT)","v":0},null,null,null,null,null,null,"None"]
[null,"Supply Current",null,null,null,"On-Chip Power",null,null,null,null,{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",SUM(G6:G10),0)","v":0},null,"Zynq-7000 AP SoC Technical Reference Manual",null,null,null,null,"Pauxq",{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",OFFSET(PS_DATA,1,IF(PROCESS=\"Typical\",11,12)),0)","v":0},null,null,null,null,null,null,"40Ω"]
[null,"Source",null,"Total",null,null,null,null,null,null,null,null,null,null,null,null,"Static","Pllq",{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",OFFSET(PS_DATA,1,IF(PROCESS=\"Typical\",13,14)),0)","v":0},null,null,null,null,null,null,"50Ω"]
[null,"VCCPINT",{"$f":"VCCPINT","v":1.8},{"$f":"IF(G6>0,G6/C5,0)","v":0},null,"Source","Power",null,"Logic","DDR","I/O",null,"XPE User Guide",null,null,null,{"$f":"Summary!$G$50*VCCPINT","v":0},"Pddroq",{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",OFFSET(PS_DATA,1,IF(PROCESS=\"Typical\",15,16)),0)","v":0},null,null,null,null,null,null,"60Ω"]
[null,"VCCPAUX",{"$f":"VCCPAUX","v":1},{"$f":"IF(G7>0,G7/C6,0)","v":0},null,"VCCPINT",{"$f":"H13+J18+SUM(J21:J37)+SUM(I40:I48)","v":0},null,{"$f":"H13+M13","v":0},{"$f":"SUM(J18:P18)+M14","v":0},{"$f":"SUM(J21:M37)+M15","v":0},null,null,null,null,null,{"$f":"(S3+S4)/1000*C6","v":0},"Pccoq",{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",OFFSET(PS_DATA,1,IF(PROCESS=\"Typical\",17,18)),0)","v":0},null,null,null,null,null,null,"75Ω"]
[null,"VCCPLL",{"$f":"VCCPLL","v":1.2},{"$f":"SUM(M13:M15)/VCCPAUX","v":0},null,"VCCPAUX",{"$f":"K18+SUM(K21:K37)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"S5/1000*C8","v":0}]
[null,"VCCO_DDR",{"$f":"VCCO_DDR","v":0},{"$f":"IF(G9>0,(L18+M18)/C8,0)","v":0},null,"VCCPLL",{"$f":"SUM(M13:M15)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"S6/1000*C9","v":0},null,null,"Addr/CE/CS_B","Clk","DQ","DQS","DQM","Term"]
[null,"VCCO_MIO0",{"$f":"IF(ISERR(Q41),1.8,Q41)","v":0},{"$f":"IF(C9>0,SUM(L21:L37)/C9,0)","v":0},null,"VCCO_DDR",{"$f":"L18","v":0},null,null,null,null,null,null,null,null,null,{"$f":"S6/1000*C10","v":0},null,"Pins",{"$f":"IF(LEFT(E18,2)=\"LP\",21,29)","v":29},2,{"$f":"F18","v":0},{"$f":"F18/IF(LEFT(E18,2)=\"LP\",4,8)","v":0},{"$f":"IF(LEFT(E18,4)=\"DDR3\",F18/8,0)","v":0},{"$f":"IF(E18=\"DDR2\",50, IF(LEFT(E18,4)=\"DDR3\",40,0))","v":0}]
[null,"VCCO_MIO1",{"$f":"IF(ISERR(R41),1.8,R41)","v":0},{"$f":"IF(C10>0,SUM(M21:M37)/C10,0)","v":0},null,"VCCO_MIO",{"$f":"SUM(L21:M37)","v":0},null,{"$f":"TEXT(PS_POWER/TOTAL_POWER,\"0%\")&\" of total on-chip power \"&TEXT(TOTAL_POWER,\"0.000\")&\"W\"","v":"0% of total on-chip power 0.084W"},null,null,null,null,null,null,null,{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",SUM(Q5:Q9),0)","v":0},null,"Freq",{"$f":"G18*0.2/2","v":0},{"$f":"G18","v":0},{"$f":"G18*0.35/2","v":0},{"$f":"G18*0.35/2","v":0},{"$f":"G18*0.35/2","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Swing",{"$f":"IF(OFFSET(VIO_STANDARD,T18,8)=0,VCCO_DDR,OFFSET(VIO_STANDARD,T18,8)-OFFSET(VIO_STANDARD,T18,9))","v":0.72},{"$f":"IF(OFFSET(VIO_STANDARD,U18,8)=0,VCCO_DDR,OFFSET(VIO_STANDARD,U18,8)-OFFSET(VIO_STANDARD,U18,9))","v":0.72},{"$f":"IF(OFFSET(VIO_STANDARD,V18,8)=0,VCCO_DDR,OFFSET(VIO_STANDARD,V18,8)-OFFSET(VIO_STANDARD,V18,9))","v":0.72},{"$f":"IF(OFFSET(VIO_STANDARD,W18,8)=0,VCCO_DDR,OFFSET(VIO_STANDARD,W18,8)-OFFSET(VIO_STANDARD,W18,9))","v":0.72},{"$f":"IF(OFFSET(VIO_STANDARD,X18,8)=0,VCCO_DDR,OFFSET(VIO_STANDARD,X18,8)-OFFSET(VIO_STANDARD,X18,9))","v":0.72}]
[null,"Processor",null,null,"A9 Cores","Clock (MHz)","Load","VCCPINT Power (W)",null,"PLLs",null,"(MHz)","VCCPLL Power (W)",null,null,null,null,null,"Pint",{"$f":"T9*T10*(OFFSET(FANOUT,3,6)+OFFSET(IODELAY_DATA,16,2)*($H$18+$I$18))","v":0},{"$f":"U9*U10*(OFFSET(FANOUT,3,6)+OFFSET(IODELAY_DATA,16,2)*$H$18)","v":0},{"$f":"V9*V10*(OFFSET(FANOUT,3,6)+OFFSET(IODELAY_DATA,16,2)*($H$18+$I$18))","v":0},{"$f":"W9*W10*(OFFSET(FANOUT,3,6)+OFFSET(IODELAY_DATA,16,2)*($H$18+$I$18))","v":0},{"$f":"$I$18*X9*X10*OFFSET(FANOUT,3,6)","v":0},"Read","Write","Power"]
[null,null,null,null,1,null,0.5,{"$f":"(VCCPINT/1000)*(IF($E13>0,IF($G13<0.5,(0.5-$G13)*$E13*$F13*OFFSET(PS_DATA,1,1),0),0)+($E13*$F13*$G13*OFFSET(PS_DATA,2,1)))","v":0},null,"Processor",null,{"$f":"2*F13","v":0},{"$f":"(IF($L13>0,OFFSET(PS_DATA,5,1),0)+$L13*OFFSET(PS_DATA,5,2))*VCCPAUX/1000","v":0},null,null,null,null,null,"Paux",{"$f":"OFFSET(VIO_STANDARD,T18,4)*T10*$I$18*T9","v":0},{"$f":"(OFFSET(VIO_STANDARD,U18,4)*U10*$I$18+IF(LEFT($E$18,2)=\"LP\",0,(OFFSET(IODELAY_DATA,16,5)*$H$18+OFFSET(IODELAY_DATA,16,6)*U10*$H$18)))*U9","v":0.9},{"$f":"(OFFSET(VIO_STANDARD,V18,4)*V10*$I$18+(OFFSET(IODELAY_DATA,16,5)*0.8*$H$18+OFFSET(IODELAY_DATA,16,6)*V10*$H$18))*V9","v":0},{"$f":"(OFFSET(VIO_STANDARD,W18,4)*W10*$I$18+(OFFSET(IODELAY_DATA,16,5)*$H$18+OFFSET(IODELAY_DATA,16,6)*W10*$H$18))*W9","v":0},{"$f":"(OFFSET(VIO_STANDARD,X18,4)*X10*$I$18+IF(LEFT($E$18,2)=\"LP\",0,(OFFSET(IODELAY_DATA,16,5)*$H$18+OFFSET(IODELAY_DATA,16,6)*X10*$H$18)))*X9","v":0},{"$f":"OFFSET(PS_DATA,7,4)*$H18^2+OFFSET(PS_DATA,7,5)*$H18+OFFSET(PS_DATA,7,6)","v":333.625},{"$f":"OFFSET(PS_DATA,7,1)*$I18^2+OFFSET(PS_DATA,7,2)*$I18+OFFSET(PS_DATA,7,3)","v":187.1875},{"$f":"(Y13+Z13-OFFSET(PS_DATA,7,3))*IF(F18=16,0.66,IF(F18<16,0,1))*VCCO_DDR/1000-M18","v":0}]
[null,null,null,null,null,null,null,null,null,"Memory",null,{"$f":"IF(G18<800,2*G18,G18)","v":0},{"$f":"(IF($L14>0,OFFSET(PS_DATA,5,1),0)+$L14*OFFSET(PS_DATA,5,2))*VCCPAUX/1000","v":0},null,null,null,null,null,"Pddr",{"$f":"((OFFSET(VIO_STANDARD,T18,3)*T11+IF(OFFSET(VIO_STANDARD,T18,11)=0,VCCO_DDR*5,(OFFSET(VIO_STANDARD,T18,8)-OFFSET(VIO_STANDARD,T18,9))*2.5))*T11*T10/1000+OFFSET(VIO_STANDARD,T18,13))*T9*MIN(1,H18+I18)","v":0},{"$f":"((OFFSET(VIO_STANDARD,U18,3)*U11+IF(OFFSET(VIO_STANDARD,U18,12)=0,VCCO_DDR*5,(OFFSET(VIO_STANDARD,U18,8)-OFFSET(VIO_STANDARD,U18,9))*2.5))*U11*U10/1000+OFFSET(VIO_STANDARD,U18,13))*U9","v":0},{"$f":"(((OFFSET(VIO_STANDARD,V18,3)+IF($Y9<=0,5,0))*V11+IF(OFFSET(VIO_STANDARD,V18,12)=0,VCCO_DDR*150,(OFFSET(VIO_STANDARD,V18,8)-OFFSET(VIO_STANDARD,V18,9))*2.5))*$I$18*V11*V10/1000+IF(OFFSET(VIO_STANDARD,V18,6)=0,0,OFFSET(VIO_STANDARD,V18,11)/IF(Y9>0,Y9*0.02,1)*VCCO_DDR*$H$18)+OFFSET(VIO_STANDARD,V18,13)*$I$18)*V9+OFFSET(VIO_STANDARD,V18,6)","v":0},{"$f":"((OFFSET(VIO_STANDARD,W18,3)*W11+IF(OFFSET(VIO_STANDARD,W18,12)=0,VCCO_DDR*5,(OFFSET(VIO_STANDARD,W18,8)-OFFSET(VIO_STANDARD,W18,9))*2.5))*$I$18*W11*W10/1000+IF(OFFSET(VIO_STANDARD,W18,6)=0,0,OFFSET(VIO_STANDARD,W18,11)/IF(E18=\"DDR3\",0.8,1)*VCCO_DDR*$H$18)+OFFSET(VIO_STANDARD,W18,13)*$I$18)*W9+OFFSET(VIO_STANDARD,W18,6)","v":0},{"$f":"((OFFSET(VIO_STANDARD,X18,3)*X11+IF(OFFSET(VIO_STANDARD,X18,11)=0,5,(OFFSET(VIO_STANDARD,X18,8)-OFFSET(VIO_STANDARD,X18,9))*2.5))*X11*X10/1000+OFFSET(VIO_STANDARD,X18,13))*$I$18*X9","v":0}]
[null,null,null,null,null,null,null,null,null,"I/O",null,null,{"$f":"(IF($L15>0,OFFSET(PS_DATA,5,1),0)+$L15*OFFSET(PS_DATA,5,2))*VCCPAUX/1000","v":0}]
[]
[null,"Memory Interface",null,null,"Memory Type","Data Width","Clock (MHz)","Read Rate","Write Rate","VCCPINT Power (W)","VCCPAUX Power (W)","VCCO_DDR Power (W)","VCCO_DDR Off-Chip (W)",null,null,null,null,null,"DDR",{"$f":"IF(OR(LEN(E18)<4,F18<=0),0,(SUM(T14:X14)+IF(E18=\"LPDDR2\",95))/1000)","v":0},null,{"$f":"IF(V14<=0,0,MAX(0,V19*OFFSET(VIO_STANDARD,V18,10)/OFFSET(VIO_STANDARD,V18,13)-V19))*I18","v":0}]
[null,null,null,null,null,null,null,0.25,0.25,{"$f":"IF(LEN(E18)<4,0,(VCCPINT/1000)*(OFFSET(PS_DATA,3,1)*$G18*MAX($H18*0.8,$I18)*F18/5+SUM(T12:X12)))","v":0},{"$f":"IF(OR(LEN(E18)<4,F18<=0),0,SUM(T13:X13))*VCCPAUX/1000","v":0},{"$f":"IF(E18=\"DDR3\",AA13,T17)","v":0},{"$f":"V19/1000","v":0},null,null,null,null,null,null,{"$f":"MATCH(IF(LEFT($E18,5)=\"DDR3L\",\"SSTL 1.35V\",IF($E18=\"DDR3\",\"SSTL 1.5V\",IF($E18=\"DDR2\",\"SSTL Class I 1.8V\",\"HSUL 1.2V\"))),VIOSTD_LIST,FALSE)","v":29},{"$f":"MATCH(IF(LEFT($E18,5)=\"DDR3L\",\"Diff SSTL 1.35V (pair)\",IF($E18=\"DDR3\",\"Diff SSTL 1.5V (pair)\",IF($E18=\"DDR2\",\"Diff HSTL Class I 1.8V (pair)\",\"Diff HSUL 1.2V (pair)\"))),VIOSTD_LIST,FALSE)","v":7},{"$f":"MATCH(IF(LEFT($E18,5)=\"DDR3L\",\"SSTL T DCI 1.35V\",IF($E18=\"DDR3\",\"SSTL T DCI 1.5V\",IF($E18=\"DDR2\",\"SSTL Class II T DCI 1.8V\",\"HSUL 1.2V\"))),VIOSTD_LIST,FALSE)","v":29},{"$f":"MATCH(IF(LEFT($E18,5)=\"DDR3L\",\"Diff SSTL T DCI 1.35V (pair)\",IF($E18=\"DDR3\",\"Diff SSTL T DCI 1.5V (pair)\",IF($E18=\"DDR2\",\"Diff SSTL Class II T DCI 1.8V (pair)\",\"HSUL 1.2V\"))),VIOSTD_LIST,FALSE)","v":29},{"$f":"MATCH(IF(LEFT($E18,5)=\"DDR3L\",\"SSTL 1.35V\",IF($E18=\"DDR3\",\"SSTL 1.5V\",IF($E18=\"DDR2\",\"SSTL Class II 1.8V\",\"HSUL 1.2V\"))),VIOSTD_LIST,FALSE)","v":29}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y9<=0,0,((VCCO_DDR-OFFSET(VIO_STANDARD,V18,8))*(ABS(VCCO_DDR/2-OFFSET(VIO_STANDARD,V18,8))/$Y9)+OFFSET(VIO_STANDARD,V18,9)*(VCCO_DDR/2-OFFSET(VIO_STANDARD,V18,9))/$Y9)*V9*I18*1000*VCCO_DDR)","v":0}]
[null,"I/O Interfaces",null,null,"I/O Standard","Number of Interfaces","I/O Bank","Clock (MHz)","Usage Rate","VCCPINT Power (W)","VCCPAUX Power (W)","VCCO_MIO0 Power (W)","VCCO_MIO1 Power (W)",null,null,null,"Bank 0 Pins","Bank 1 Pins","Standard Index","Vcco","Rate",null,null,"Iccint","Iccaux","Vcco"]
[null,"QSPI 4-bit",null,null,null,null,null,null,0.5,{"$f":"X21*VCCPINT","v":0},{"$f":"Y21*VCCPAUX","v":0},{"$f":"Q21*T21*Z21","v":0},{"$f":"R21*T21*Z21","v":0},null,null,null,{"$f":"F21*5","v":0},0,{"$f":"MATCH(IF(LEFT($E21,2)=\"LV\",$E21 & \" 8mA (slow)\",IF(ISBLANK($E21),\"LVCMOS 1.8V 8mA (slow)\",$E21)),SIOSTD_LIST,FALSE)","v":35},{"$f":"OFFSET(IO_STANDARDS,$S21,1)","v":1.8},{"$f":"H21*I21/2","v":0},null,null,{"$f":"($U21*2*OFFSET(FANOUT,3,6)*(Q21+R21))/1000","v":0},{"$f":"(OFFSET(IO_STANDARDS,$S21,4)*U21/2+OFFSET(IO_STANDARDS,$S21,5))/1000*(Q21+R21)","v":0},{"$f":"OFFSET(IO_STANDARDS,$S21,3)*U21/2000000","v":0}]
[null,"QSPI 8-bit",null,null,null,null,null,null,0.5,0,0,{"$f":"Q22*T22*Z22","v":0},{"$f":"R22*T22*Z22","v":0},null,null,null,{"$f":"F22*10","v":0},0,35,1.8,{"$f":"H22*I22/2","v":0},null,null,0,0,0]
[null,"NAND",null,null,null,null,null,null,0.5,0,0,0,0,null,null,null,{"$f":"F23*15","v":0},0,35,1.8,0,null,null,0,0,0]
[null,"SRAM/NOR",null,null,null,null,null,null,0.5,0,0,0,0,null,null,null,{"$f":"F24*16","v":0},{"$f":"F24*24","v":0},35,1.8,0,null,null,0,0,0]
[null,"USB",null,null,null,null,null,null,0.5,0,0,0,0,null,null,null,0,{"$f":"F25*12","v":0},35,1.8,0,null,null,0,0,0]
[null,"GigE",null,null,null,null,null,null,0.5,0,0,0,0,null,null,null,0,{"$f":"F26*12","v":0},35,1.8,0,null,null,0,0,0]
[null,"UART",null,null,null,null,null,null,0.5,0,0,0,0,null,null,null,{"$f":"IF(G27=\"Vcco_p0\",F27,IF(G27=\"Vcco_p0/1\",F27/2,0))*2","v":0},{"$f":"IF(G27=\"Vcco_p1\",F27,IF(G27=\"Vcco_p0/1\",F27/2,0))*2","v":0},35,1.8,0,null,null,0,0,0]
[null,"I2C",null,null,null,null,null,null,0.5,0,0,0,0,null,null,null,{"$f":"IF(G28=\"Vcco_p0\",F28,IF(G28=\"Vcco_p0/1\",F28/2,0))*2","v":0},{"$f":"IF(G28=\"Vcco_p1\",F28,IF(G28=\"Vcco_p0/1\",F28/2,0))*2","v":0},35,1.8,0,null,null,0,0,0]
[null,"SPI",null,null,null,null,null,null,0.5,0,0,0,0,null,null,null,{"$f":"IF(G29=\"Vcco_p0\",F29,IF(G29=\"Vcco_p0/1\",F29/2,0))*2","v":0},{"$f":"IF(G29=\"Vcco_p1\",F29,IF(G29=\"Vcco_p0/1\",F29/2,0))*2","v":0},35,1.8,0,null,null,0,0,0]
[null,"CAN",null,null,null,null,null,null,0.5,{"$f":"X30*VCCPINT","v":0},{"$f":"Y30*VCCPAUX","v":0},{"$f":"Q30*T30*Z30","v":0},{"$f":"R30*T30*Z30","v":0},null,null,null,{"$f":"IF(G30=\"Vcco_p0\",F30,IF(G30=\"Vcco_p0/1\",F30/2,0))*2","v":0},{"$f":"IF(G30=\"Vcco_p1\",F30,IF(G30=\"Vcco_p0/1\",F30/2,0))*2","v":0},35,1.8,{"$f":"H30*I30/2","v":0},null,null,{"$f":"($U30*2*OFFSET(FANOUT,3,6)*(Q30+R30))/1000","v":0},{"$f":"(OFFSET(IO_STANDARDS,$S30,4)*U30/2+OFFSET(IO_STANDARDS,$S30,5))/1000*(Q30+R30)","v":0},{"$f":"OFFSET(IO_STANDARDS,$S30,3)*U30/2000000","v":0}]
[null,"SD",null,null,null,null,null,null,0.5,0,0,0,0,null,null,null,{"$f":"IF(G31=\"Vcco_p0\",F31,IF(G31=\"Vcco_p0/1\",F31/2,0))*5","v":0},{"$f":"IF(G31=\"Vcco_p1\",F31,IF(G31=\"Vcco_p0/1\",F31/2,0))*5","v":0},35,1.8,0,null,null,0,0,0]
[null,"Trace",null,null,null,null,null,null,0.5,{"$f":"X32*VCCPINT","v":0},{"$f":"Y32*VCCPAUX","v":0},{"$f":"Q32*T32*Z32","v":0},{"$f":"R32*T32*Z32","v":0},null,null,null,{"$f":"IF(G32=\"Vcco_p0\",F32,IF(G32=\"Vcco_p0/1\",F32/2,0))*5","v":0},{"$f":"IF(G32=\"Vcco_p1\",F32,IF(G32=\"Vcco_p0/1\",F32/2,0))*5","v":0},35,1.8,{"$f":"H32*I32/2","v":0},null,null,{"$f":"($U32*2*OFFSET(FANOUT,3,6)*(Q32+R32))/1000","v":0},{"$f":"(OFFSET(IO_STANDARDS,$S32,4)*U32/2+OFFSET(IO_STANDARDS,$S32,5))/1000*(Q32+R32)","v":0},{"$f":"OFFSET(IO_STANDARDS,$S32,3)*U32/2000000","v":0}]
[null,"Timer",null,null,null,null,null,null,0.5,0,0,0,0,null,null,null,0,0,35,1.8,0,null,null,0,0,0]
[null,"Watchdog",null,null,null,null,null,null,0.5,0,0,0,0,null,null,null,0,0,35,1.8,0,null,null,0,0,0]
[null,"PJTAG",null,null,null,null,null,null,0.5,0,0,0,0,null,null,null,0,0,35,1.8,0,null,null,0,0,0]
[null,"GPIO Bank 0",null,null,null,null,null,null,0.5,0,0,0,0,null,null,null,{"$f":"F36","v":0},0,35,1.8,0,null,null,0,0,0]
[null,"GPIO Bank 1",null,null,null,null,null,null,0.5,0,0,0,0,null,null,null,0,{"$f":"F37","v":0},35,1.8,0,null,null,0,0,0]
[]
[null,"AXI Interfaces",null,null,"PS-PL Interface","Width","Clock (MHz)","Usage Rate","VCCPINT Power (W)"]
[null,null,null,null,"AXI_ACP",64,null,0.5,{"$f":"(VCCPINT/1000)*$G40*$H40*OFFSET(PS_DATA,4,1)*IF($F40>=8,$F40/8,0)","v":0}]
[null,null,null,null,"AXI_HP",null,null,0.5,0,null,null,null,null,null,null,null,{"$f":"IF(SUM(Q11:Q37)=0,0,MEDIAN(IF(Q21:Q37>0,T21:T37)))","v":0},{"$f":"IF(SUM(R21:R37)=0,0,MEDIAN(IF(R21:R37>0,T21:T37)))","v":0}]
[null,null,null,null,"AXI_HP",null,null,0.5,0]
[null,null,null,null,"AXI_HP",null,null,0.5,0]
[null,null,null,null,"AXI_HP",null,null,0.5,0]
[null,null,null,null,"AXI_GP",32,null,0.5,0]
[null,null,null,null,"AXI_GP",32,null,0.5,0]
[null,null,null,null,"AXI_GP",32,null,0.5,0]
[null,null,null,null,"AXI_GP",32,null,0.5,0]

{"sheet":"GTZ","index":17,"n_rows":39,"n_cols":29,"rows_kept":39,"cut":false,"hidden":true,"merged":[[19,1,19,3],[2,1,2,3],[2,5,2,9],[11,1,11,3],[12,1,12,3],[15,1,15,3],[16,1,16,3],[17,1,17,3],[2,17,2,19],[4,17,4,19],[0,1,0,19],[18,1,18,3],[13,1,13,3],[14,1,14,3],[2,12,2,15],[3,1,3,2],[3,12,3,13],[8,7,8,10],[5,12,5,13]]}
[null,"GTZ Transceiver Power",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(PROCESS<>\"Maximum\",2,1)","v":2},{"$f":"IF(RIGHT(SPEEDGRADE,1)=\"G\",28.6,25.78125)","v":25.78125},9.8000000000000007,null,{"$f":"\"AC2:AC6\"","v":"AC2:AC6"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14.3,null,800]
[null,"Active Current",null,null,null,"Power",null,null,null,null,{"$f":"IF(NUM_GTZS>1,SUM(G6:G9),0)","v":0},null,"Utilization",null,null,null,null,"Transceivers User Guide",null,null,null,null,null,null,null,null,null,null,900]
[null,"Source",null,"Active",null,null,null,null,null,null,null,null,"GTZ Channels",null,{"$f":"SUM(E13:E100)","v":0},{"$f":"IF(NUM_GTZS>0,O4/NUM_GTZS,\"N/A\")","v":"N/A"},null,null,null,null,null,null,null,null,null,null,null,null,1000]
[null,"VCCINT",{"$f":"VCCINT","v":0.95},{"$f":"IF(GTZ_INTPOWER>0,GTZ_INTPOWER/VCCINT,0)","v":0},null,"Source","Power",null,null,"PMA","PCS",null,null,null,null,null,null,"XPE User Guide",null,null,null,null,null,null,null,null,null,null,1100]
[null,"MGTZVCCH",{"$f":"Summary!O30","v":1.8},{"$f":"IF(NUM_GTZS>0,SUM(L13:L20),0)/Summary!O30","v":0},null,"VCCINT",{"$f":"IF(NUM_GTZS>0,SUM(K13:K20),0)","v":0},null,null,{"$f":"IF(NUM_GTZS>1,SUM(G7:G9),0)","v":0},{"$f":"GTZ_INTPOWER","v":0},null,"Power Planes",null,{"$f":"INT(($O4+7)/8)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,1200]
[null,"MGTZAVCC",{"$f":"Summary!O31","v":1},{"$f":"IF(NUM_GTZS>0,SUM(M13:M20),0)/Summary!O31","v":0},null,"MGTZVCCH",{"$f":"IF(NUM_GTZS>0,SUM(L13:L20),0)","v":0}]
[null,"MGTZVCCL",{"$f":"Summary!O32","v":1.2},{"$f":"IF(NUM_GTZS>0,SUM(N13:N20),0)/Summary!O32","v":0},null,"MGTZAVCC",{"$f":"IF(NUM_GTZS>0,SUM(M13:M20),0)","v":0}]
[null,null,null,null,null,"MGTZVCCL",{"$f":"IF(NUM_GTZS>0,SUM(N13:N20),0)","v":0},{"$f":"TEXT(GTZ_POWER/TOTAL_POWER,\"0%\")&\" of total on-chip power \"&TEXT(TOTAL_POWER,\"0.000\")&\"W\"","v":"0% of total on-chip power 0.084W"}]
[]
[]
[null,"Name",null,null,"GTZ Channels","Operational Mode","Power Mode","Data Rate (Gb/s)","Data Path","O/P (mV)","VCCINT Power (W)","MGTZVCCH Power (W)","MGTZAVCC Power (W)","MGTZVCCL Power (W)",null,null,null,null,null,null,null,null,"RX","TX","VCO","USRCLK"]
[null,null,null,null,null,"Transceiver","Functional",25.78125,80,800,{"$f":"(VCCINT_N/1000)*$E13*(OFFSET(GTZ_DATA,1,$Y$1)+OFFSET(GTZ_DATA,1,2+$Y$1)*$H13)","v":0},{"$f":"(Summary!O$30/1000)*$E13*(OFFSET(GTZ_DATA,2,$Y$1)+OFFSET(GTZ_DATA,2,2+$Y$1)*$H13)","v":0},{"$f":"(Summary!O$31/1000)*(IF($E13>0,OFFSET(GTZ_DATA,9,$Y$1),0)+IF($G13=\"Functional\",$E13,MAX($E13-1,0))*(OFFSET(GTZ_DATA,3,$Y$1)+IF($H13/2<$AA$1,OFFSET(GTZ_DATA,5,$Y$1),0)+OFFSET(GTZ_DATA,3,2+$Y$1)*$H13)+IF(OR($E13<1,$G13=\"Functional\"),0,OFFSET(GTZ_DATA,4,$Y$1)+OFFSET(GTZ_DATA,4,2+$Y$1)*$H13))","v":0},{"$f":"(Summary!O$32/1000)*$E13*(MAX(0,OFFSET(GTZ_DATA,6,$Y$1)+OFFSET(GTZ_DATA,7,$Y$1)*$W13+OFFSET(GTZ_DATA,8,$Y$1)*$X13)+(OFFSET(GTZ_DATA,6,2+$Y$1)+OFFSET(GTZ_DATA,7,2+$Y$1)*$W13+OFFSET(GTZ_DATA,8,2+$Y$1)*$X13)*$H13)","v":0},null,null,null,null,null,null,null,null,{"$f":"IF(LEFT($F13,6)<>\"Transm\",1,0)","v":1},{"$f":"IF(LEFT($F13,1)=\"T\",1,0)","v":1},{"$f":"IF($H13/2>=$AA$1,$H13/2,IF($H13>=$AA$1,$H13,IF($H13*2>=$AA$1,$H13*2,$H13*4)))","v":12.890625},{"$f":"IF($H13/2>=$AA$1,$H13/$I13,IF($H13>=$AA$1,$H13/$I13,IF($H13*2>=$AA$1,$H13/$I13,$H13*2/$I13)))*1000","v":322.265625}]
[null,null,null,null,null,"Transceiver","Functional",25.78125,80,800,0,{"$f":"(Summary!O$30/1000)*$E14*(OFFSET(GTZ_DATA,2,$Y$1)+OFFSET(GTZ_DATA,2,2+$Y$1)*$H14)","v":0},{"$f":"(Summary!O$31/1000)*(IF($E14>0,OFFSET(GTZ_DATA,9,$Y$1),0)+IF($G14=\"Functional\",$E14,MAX($E14-1,0))*(OFFSET(GTZ_DATA,3,$Y$1)+IF($H14/2<$AA$1,OFFSET(GTZ_DATA,5,$Y$1),0)+OFFSET(GTZ_DATA,3,2+$Y$1)*$H14)+IF(OR($E14<1,$G14=\"Functional\"),0,OFFSET(GTZ_DATA,4,$Y$1)+OFFSET(GTZ_DATA,4,2+$Y$1)*$H14))","v":0},{"$f":"(Summary!O$32/1000)*$E14*(MAX(0,OFFSET(GTZ_DATA,6,$Y$1)+OFFSET(GTZ_DATA,7,$Y$1)*$W14+OFFSET(GTZ_DATA,8,$Y$1)*$X14)+(OFFSET(GTZ_DATA,6,2+$Y$1)+OFFSET(GTZ_DATA,7,2+$Y$1)*$W14+OFFSET(GTZ_DATA,8,2+$Y$1)*$X14)*$H14)","v":0},null,null,null,null,null,null,null,null,{"$f":"IF(LEFT($F14,6)<>\"Transm\",1,0)","v":1},{"$f":"IF(LEFT($F14,1)=\"T\",1,0)","v":1},{"$f":"IF($H14/2>=$AA$1,$H14/2,IF($H14>=$AA$1,$H14,IF($H14*2>=$AA$1,$H14*2,$H14*4)))","v":12.890625},{"$f":"IF($H14/2>=$AA$1,$H14/$I14,IF($H14>=$AA$1,$H14/$I14,IF($H14*2>=$AA$1,$H14/$I14,$H14*2/$I14)))*1000","v":322.265625}]
[null,null,null,null,null,"Transceiver","Functional",25.78125,80,800,0,{"$f":"(Summary!O$30/1000)*$E15*(OFFSET(GTZ_DATA,2,$Y$1)+OFFSET(GTZ_DATA,2,2+$Y$1)*$H15)","v":0},{"$f":"(Summary!O$31/1000)*(IF($E15>0,OFFSET(GTZ_DATA,9,$Y$1),0)+IF($G15=\"Functional\",$E15,MAX($E15-1,0))*(OFFSET(GTZ_DATA,3,$Y$1)+IF($H15/2<$AA$1,OFFSET(GTZ_DATA,5,$Y$1),0)+OFFSET(GTZ_DATA,3,2+$Y$1)*$H15)+IF(OR($E15<1,$G15=\"Functional\"),0,OFFSET(GTZ_DATA,4,$Y$1)+OFFSET(GTZ_DATA,4,2+$Y$1)*$H15))","v":0},{"$f":"(Summary!O$32/1000)*$E15*(MAX(0,OFFSET(GTZ_DATA,6,$Y$1)+OFFSET(GTZ_DATA,7,$Y$1)*$W15+OFFSET(GTZ_DATA,8,$Y$1)*$X15)+(OFFSET(GTZ_DATA,6,2+$Y$1)+OFFSET(GTZ_DATA,7,2+$Y$1)*$W15+OFFSET(GTZ_DATA,8,2+$Y$1)*$X15)*$H15)","v":0},null,null,null,null,null,null,null,null,1,1,12.890625,322.265625]
[null,null,null,null,null,"Transceiver","Functional",25.78125,80,800,0,{"$f":"(Summary!O$30/1000)*$E16*(OFFSET(GTZ_DATA,2,$Y$1)+OFFSET(GTZ_DATA,2,2+$Y$1)*$H16)","v":0},{"$f":"(Summary!O$31/1000)*(IF($E16>0,OFFSET(GTZ_DATA,9,$Y$1),0)+IF($G16=\"Functional\",$E16,MAX($E16-1,0))*(OFFSET(GTZ_DATA,3,$Y$1)+IF($H16/2<$AA$1,OFFSET(GTZ_DATA,5,$Y$1),0)+OFFSET(GTZ_DATA,3,2+$Y$1)*$H16)+IF(OR($E16<1,$G16=\"Functional\"),0,OFFSET(GTZ_DATA,4,$Y$1)+OFFSET(GTZ_DATA,4,2+$Y$1)*$H16))","v":0},{"$f":"(Summary!O$32/1000)*$E16*(MAX(0,OFFSET(GTZ_DATA,6,$Y$1)+OFFSET(GTZ_DATA,7,$Y$1)*$W16+OFFSET(GTZ_DATA,8,$Y$1)*$X16)+(OFFSET(GTZ_DATA,6,2+$Y$1)+OFFSET(GTZ_DATA,7,2+$Y$1)*$W16+OFFSET(GTZ_DATA,8,2+$Y$1)*$X16)*$H16)","v":0},null,null,null,null,null,null,null,null,1,1,12.890625,322.265625]
[null,null,null,null,null,"Transceiver","Functional",25.78125,80,800,0,{"$f":"(Summary!O$30/1000)*$E17*(OFFSET(GTZ_DATA,2,$Y$1)+OFFSET(GTZ_DATA,2,2+$Y$1)*$H17)","v":0},{"$f":"(Summary!O$31/1000)*(IF($E17>0,OFFSET(GTZ_DATA,9,$Y$1),0)+IF($G17=\"Functional\",$E17,MAX($E17-1,0))*(OFFSET(GTZ_DATA,3,$Y$1)+IF($H17/2<$AA$1,OFFSET(GTZ_DATA,5,$Y$1),0)+OFFSET(GTZ_DATA,3,2+$Y$1)*$H17)+IF(OR($E17<1,$G17=\"Functional\"),0,OFFSET(GTZ_DATA,4,$Y$1)+OFFSET(GTZ_DATA,4,2+$Y$1)*$H17))","v":0},{"$f":"(Summary!O$32/1000)*$E17*(MAX(0,OFFSET(GTZ_DATA,6,$Y$1)+OFFSET(GTZ_DATA,7,$Y$1)*$W17+OFFSET(GTZ_DATA,8,$Y$1)*$X17)+(OFFSET(GTZ_DATA,6,2+$Y$1)+OFFSET(GTZ_DATA,7,2+$Y$1)*$W17+OFFSET(GTZ_DATA,8,2+$Y$1)*$X17)*$H17)","v":0},null,null,null,null,null,null,null,null,1,1,12.890625,322.265625]
[null,null,null,null,null,"Transceiver","Functional",25.78125,80,800,0,{"$f":"(Summary!O$30/1000)*$E18*(OFFSET(GTZ_DATA,2,$Y$1)+OFFSET(GTZ_DATA,2,2+$Y$1)*$H18)","v":0},{"$f":"(Summary!O$31/1000)*(IF($E18>0,OFFSET(GTZ_DATA,9,$Y$1),0)+IF($G18=\"Functional\",$E18,MAX($E18-1,0))*(OFFSET(GTZ_DATA,3,$Y$1)+IF($H18/2<$AA$1,OFFSET(GTZ_DATA,5,$Y$1),0)+OFFSET(GTZ_DATA,3,2+$Y$1)*$H18)+IF(OR($E18<1,$G18=\"Functional\"),0,OFFSET(GTZ_DATA,4,$Y$1)+OFFSET(GTZ_DATA,4,2+$Y$1)*$H18))","v":0},{"$f":"(Summary!O$32/1000)*$E18*(MAX(0,OFFSET(GTZ_DATA,6,$Y$1)+OFFSET(GTZ_DATA,7,$Y$1)*$W18+OFFSET(GTZ_DATA,8,$Y$1)*$X18)+(OFFSET(GTZ_DATA,6,2+$Y$1)+OFFSET(GTZ_DATA,7,2+$Y$1)*$W18+OFFSET(GTZ_DATA,8,2+$Y$1)*$X18)*$H18)","v":0},null,null,null,null,null,null,null,null,1,1,12.890625,322.265625]
[null,null,null,null,null,"Transceiver","Functional",25.78125,80,800,0,{"$f":"(Summary!O$30/1000)*$E19*(OFFSET(GTZ_DATA,2,$Y$1)+OFFSET(GTZ_DATA,2,2+$Y$1)*$H19)","v":0},{"$f":"(Summary!O$31/1000)*(IF($E19>0,OFFSET(GTZ_DATA,9,$Y$1),0)+IF($G19=\"Functional\",$E19,MAX($E19-1,0))*(OFFSET(GTZ_DATA,3,$Y$1)+IF($H19/2<$AA$1,OFFSET(GTZ_DATA,5,$Y$1),0)+OFFSET(GTZ_DATA,3,2+$Y$1)*$H19)+IF(OR($E19<1,$G19=\"Functional\"),0,OFFSET(GTZ_DATA,4,$Y$1)+OFFSET(GTZ_DATA,4,2+$Y$1)*$H19))","v":0},{"$f":"(Summary!O$32/1000)*$E19*(MAX(0,OFFSET(GTZ_DATA,6,$Y$1)+OFFSET(GTZ_DATA,7,$Y$1)*$W19+OFFSET(GTZ_DATA,8,$Y$1)*$X19)+(OFFSET(GTZ_DATA,6,2+$Y$1)+OFFSET(GTZ_DATA,7,2+$Y$1)*$W19+OFFSET(GTZ_DATA,8,2+$Y$1)*$X19)*$H19)","v":0},null,null,null,null,null,null,null,null,1,1,12.890625,322.265625]
[null,null,null,null,null,"Transceiver","Functional",25.78125,80,800,0,{"$f":"(Summary!O$30/1000)*$E20*(OFFSET(GTZ_DATA,2,$Y$1)+OFFSET(GTZ_DATA,2,2+$Y$1)*$H20)","v":0},{"$f":"(Summary!O$31/1000)*(IF($E20>0,OFFSET(GTZ_DATA,9,$Y$1),0)+IF($G20=\"Functional\",$E20,MAX($E20-1,0))*(OFFSET(GTZ_DATA,3,$Y$1)+IF($H20/2<$AA$1,OFFSET(GTZ_DATA,5,$Y$1),0)+OFFSET(GTZ_DATA,3,2+$Y$1)*$H20)+IF(OR($E20<1,$G20=\"Functional\"),0,OFFSET(GTZ_DATA,4,$Y$1)+OFFSET(GTZ_DATA,4,2+$Y$1)*$H20))","v":0},{"$f":"(Summary!O$32/1000)*$E20*(MAX(0,OFFSET(GTZ_DATA,6,$Y$1)+OFFSET(GTZ_DATA,7,$Y$1)*$W20+OFFSET(GTZ_DATA,8,$Y$1)*$X20)+(OFFSET(GTZ_DATA,6,2+$Y$1)+OFFSET(GTZ_DATA,7,2+$Y$1)*$W20+OFFSET(GTZ_DATA,8,2+$Y$1)*$X20)*$H20)","v":0},null,null,null,null,null,null,null,null,1,1,12.890625,322.265625]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,null,null,null,null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"M30:M3\"&M34","v":"M30:M30"}]
[null,null,null,null,null,null,null,null,null,null,null,"Dice",{"$f":"IF(NUM_GTZS=16,2,IF(NUM_GTZS=8,1,0))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,"Planes",{"$f":"IF(NUM_GTZS>0,MIN(NUM_GTZS/8,MAX(INT(($O4+7)/8),GTZPOWERPLANE)),0)","v":0},null,"x^4","x^3","x^2","x","c"]
[null,null,null,null,null,null,null,null,null,null,null,"MGTZVCCHQ",{"$f":"M35*($O36*TemperatureEstimate^4+$P36*TemperatureEstimate^3+$Q36*TemperatureEstimate^2+$R36*TemperatureEstimate+$S36)/1000","v":0},null,{"$f":"OFFSET(BLOCK_LEAKAGE,8,FACTORCOL+5)","v":2.4649305786499833E-8},{"$f":"OFFSET(BLOCK_LEAKAGE,8,FACTORCOL+6)","v":-1.1541480970309239E-7},{"$f":"OFFSET(BLOCK_LEAKAGE,8,FACTORCOL+7)","v":9.2331847762599305E-6},{"$f":"OFFSET(BLOCK_LEAKAGE,8,FACTORCOL+8)","v":1.0898455601923847E-2},{"$f":"OFFSET(BLOCK_LEAKAGE,8,FACTORCOL+9)","v":13.780528278499251}]
[null,null,null,null,null,null,null,null,null,null,null,"MGTZAVCCQ",{"$f":"S37*M35/1000","v":0},null,{"$f":"OFFSET(BLOCK_LEAKAGE,8,FACTORCOL)","v":1.4965611218380669E-8},{"$f":"OFFSET(BLOCK_LEAKAGE,8,FACTORCOL+1)","v":1.1042825965039589E-5},{"$f":"OFFSET(BLOCK_LEAKAGE,8,FACTORCOL+2)","v":1.8008324024245675E-3},{"$f":"OFFSET(BLOCK_LEAKAGE,8,FACTORCOL+3)","v":0.13986641471177225},{"$f":"OFFSET(BLOCK_LEAKAGE,8,FACTORCOL+4)","v":4.4173599107819443}]
[null,null,null,null,null,null,null,null,null,null,null,"MGTZVCCLQ",{"$f":"M35*($O38*TemperatureEstimate^4+$P38*TemperatureEstimate^3+$Q38*TemperatureEstimate^2+$R38*TemperatureEstimate+$S38)/1000","v":0},null,{"$f":"OFFSET(BLOCK_LEAKAGE,8,FACTORCOL+10)","v":6.4860950108070533E-9},{"$f":"OFFSET(BLOCK_LEAKAGE,8,FACTORCOL+11)","v":-2.8492648783160272E-7},{"$f":"OFFSET(BLOCK_LEAKAGE,8,FACTORCOL+12)","v":-3.2614893996764716E-6},{"$f":"OFFSET(BLOCK_LEAKAGE,8,FACTORCOL+13)","v":6.0933950674031689E-4},{"$f":"OFFSET(BLOCK_LEAKAGE,8,FACTORCOL+14)","v":-4.5971262032672988E-3}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"M36*C6+M37*C7+M38*C8","v":0}]

{"sheet":"GTY","index":18,"n_rows":123,"n_cols":56,"rows_kept":123,"cut":false,"hidden":false,"merged":[[95,1,95,3],[96,1,96,3],[97,1,97,3],[98,1,98,3],[99,1,99,3],[105,1,105,21],[89,1,89,3],[90,1,90,3],[91,1,91,3],[92,1,92,3],[93,1,93,3],[94,1,94,3],[83,1,83,3],[84,1,84,3],[85,1,85,3],[86,1,86,3],[87,1,87,3],[88,1,88,3],[77,1,77,3],[78,1,78,3],[79,1,79,3],[80,1,80,3],[81,1,81,3],[82,1,82,3],[71,1,71,3],[72,1,72,3],[73,1,73,3],[74,1,74,3],[75,1,75,3],[76,1,76,3],[65,1,65,3],[66,1,66,3],[67,1,67,3],[68,1,68,3],[69,1,69,3],[70,1,70,3],[59,1,59,3],[60,1,60,3],[61,1,61,3],[62,1,62,3],[63,1,63,3],[64,1,64,3],[53,1,53,3],[54,1,54,3],[55,1,55,3],[56,1,56,3],[57,1,57,3],[58,1,58,3],[47,1,47,3],[48,1,48,3],[49,1,49,3],[50,1,50,3],[51,1,51,3],[52,1,52,3],[41,1,41,3],[42,1,42,3],[43,1,43,3],[44,1,44,3],[45,1,45,3],[46,1,46,3],[35,1,35,3],[36,1,36,3],[37,1,37,3],[38,1,38,3],[39,1,39,3],[40,1,40,3],[29,1,29,3],[30,1,30,3],[31,1,31,3],[32,1,32,3],[33,1,33,3],[34,1,34,3],[23,1,23,3],[24,1,24,3],[25,1,25,3],[26,1,26,3],[27,1,27,3],[28,1,28,3],[17,1,17,3],[18,1,18,3],[19,1,19,3],[20,1,20,3],[21,1,21,3],[22,1,22,3],[13,1,13,3],[14,1,14,3],[15,1,15,3],[16,1,16,3],[4,12,4,13],[4,19,4,21],[6,12,6,13],[8,7,8,10],[10,1,10,3],[10,9,10,12],[10,13,10,17],[8,12,8,13],[5,12,5,13],[2,1,2,3],[2,5,2,9],[2,12,2,15],[2,19,2,21],[3,1,3,2],[3,12,3,13],[11,1,11,3],[12,1,12,3],[0,1,0,23]]}
[null,"GTY Transceiver Power",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(PROCESS<>\"Maximum\",1,1)","v":1},{"$f":"IF(PROCESS<>\"Maximum\",1,1)","v":1},{"$f":"IF(LEFT(SPEEDGRADE,3)=\"-1H\",25.7,IF(LEFT(SPEEDGRADE,2)=\"-1\",12.5,IF(PART=\"XCKU095\",16.3,IF(SPEEDGRADE=\"-2\",28.21,30.5))))","v":30.5},null,"CPLL VCO range (MHz)","LC VCO range (MHz)",null,1,null,"Raised Voltage",null,null,null,null,null,null,null,{"$f":"IF(AND(NUM_CMACS>0,NUM_ILMACS>0),\"AR1:AR9\",IF(NUM_CMACS>0,\"AR1:AR6\",\"AR1:AR3\"))","v":"AR1:AR9"},null,{"$f":"\"AT2:AT33\"","v":"AT2:AT33"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,8,9.8000000000000007,{"$f":"IF(LEFT(SPEEDGRADE,2)=\"-1\",8.5,12.5)","v":12.5},null,{"$f":"IF(K3>0,COUNTIF(K13:K100,\">10.3125\")+COUNTIF(O13:O100,\">10.3125\"),0)","v":0},null,null,null,null,null,null,null,null,"PCIe",null,166]
[null,"Active Current",null,null,null,"Transceiver Power",null,null,null,null,{"$f":"SUM(G6:G9)-I6","v":27.879543583288999},null,"Utilization",null,null,null,null,null,null,"Transceivers User Guide",null,null,null,null,null,null,null,null,null,6.25,13,{"$f":"32.75/2","v":16.375},null,null,null,null,null,null,null,null,null,null,null,"PCIe500",null,196]
[null,"Source",null,"Active",null,null,null,null,null,null,null,null,"GTY Channels",null,{"$f":"SUM(E13:E100)","v":60},{"$f":"IF(NUM_GTYS>0,O4/NUM_GTYS,\"N/A\")","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CMAC",null,226]
[null,"VCCINT",{"$f":"VCCINT","v":0.95},{"$f":"IF(GTY_INTPOWER>0,GTY_INTPOWER/VCCINT,0)","v":2.9346032986199999},null,"Source","Power",null,"Hard IP","PCS","PMA",null,"PCIe Blocks",null,{"$f":"COUNTIF(AR13:AR100,\">0\")","v":0},{"$f":"IF(NUM_PCIES>0,O5/NUM_PCIES,\"N/A\")","v":0},null,null,null,"XPE User Guide",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CMAC-Low",null,255]
[null,"MGTYVCCAUX",{"$f":"VCCPINT","v":1.8},{"$f":"IF(GTY_AUXPOWER>0,GTY_AUXPOWER/VCCPINT,0)","v":0.30576000000000003},null,"VCCINT",{"$f":"IF(NUM_GTYS>0,SUM(U13:U100),0)","v":2.7878731336889997},null,{"$f":"IF(NUM_GTYS>0,(VCCINT/1000)*VCCINT_N*(SUM(AR13:AR100)+SUM(AW13:AW100)+SUM(AX13:AX100)),0)*PL_POWERED","v":0},{"$f":"GTY_INTPOWER-I6-((VCCINT/1000)*VCCINT_N*SUM(AS13:AS100))","v":2.7878731336889997},{"$f":"SUM(G7:G9)+((VCCINT/1000)*VCCINT_N*SUM(AS13:AS100))","v":25.091670449599999},null,"CMAC Blocks",null,{"$f":"COUNTIF(AW13:AW100,\">0\")","v":0},{"$f":"IF(NUM_CMACS>0,O6/NUM_CMACS,\"N/A\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CMAC-High",null,285]
[null,"MGTYAVCC",{"$f":"VCCPAUX","v":1},{"$f":"IF(NUM_GTHS>1,GTY_AVDD/VCCPAUX,0)","v":3.6819757999999996},null,"MGTYVCCAUX",{"$f":"IF(NUM_GTYS>0,SUM(V13:V100),0)","v":0.55036800000000008},null,null,null,null,null,"ILKN Blocks",null,{"$f":"COUNTIF(AX13:AX100,\">0\")","v":0},{"$f":"IF(NUM_ILMACS>0,O7/NUM_ILMACS,\"N/A\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ILKN",null,315]
[null,"MGTYAVTT",{"$f":"VCCPLL","v":1.2},{"$f":"IF(NUM_GTYS>1,GTY_VTTX/VCCPLL,0)","v":17.382772208000002},null,"MGTYAVCC",{"$f":"IF(NUM_GTYS>0,SUM(W13:W100),0)","v":3.6819757999999996},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ILKN-Low",null,344]
[null,null,null,null,null,"MGTYAVTT",{"$f":"IF(NUM_GTYS>0,SUM(X13:X100),0)","v":20.8593266496},{"$f":"TEXT(GTH_POWER/TOTAL_POWER,\"0%\")&\" of total on-chip power \"&TEXT(TOTAL_POWER,\"0.000\")&\"W\"","v":"21% of total on-chip power 0.084W"},null,null,null,null,"Power Planes",null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ILKN-High",null,374]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,404]
[null,null,null,null,null,null,null,null,null,"RX",null,null,null,"TX",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,433]
[null,"Name",null,null,"GTY Channels","Operational Mode","EyeScan","Power Mode","Channels Sharing QPLL","Clock Source","Data Rate (Gb/s)","Data Path","Data Mode","Clock Source","Data Rate (Gb/s)","Data Path","Data Mode","O/P (mV)","OOB Used","Hard IP Block","VCCINT Power (W)","MGTYVCCAUX Power (W)","MGTYAVCC Power (W)","MGTYAVTT Power (W)",null,"Operate Mode","Quads","RX VCO LC (MHz)","TX VCO LC (MHz)","RX VCO CPLL (MHz)","TX VCO CPLL (MHz)","RX USERCLK","TX USERCLK","Power Mode (LPM=0, DFE=1)","TX Voltage Swing Current","AVTT Current (CPLL)","AVTT Current (LC)","AVCC Current (RX)","AVCC Current (TX)","AVCC Current (CPLL)","AVCC Current (LC)","AVCC CLK","AVTT CLK","PCIe",null,463,"mA col","mA/MHz col","cmac","ilkn","QPLL1 RX","QPLL1 TX","QPLL0RX","QPLL0TX","QPLL rx","QPLL tx"]
[null,"In",null,null,44,"Receiver","Off","Low Power",4,"QPLL0",12.8,32,"8b/10b","QPLL1",0,20,"Raw",166,"No",null,{"$f":"(VCCINT/1000)*VCCINT_N*($E13*(OFFSET(GTY_DATA,1,$AA$1)+OFFSET(GTY_DATA,1,2+$AA$1)*MAX(IF($Z13<>2,$K13,0),IF($Z13>1,$O13,0))+IF(MAX(IF($Z13<>2,$K13,0),IF($Z13>1,$O13,0))>20.6,IF($AH13>0,-20,-40),0))+$AS13+AR13+AW13+AX13)","v":2.100945273152},{"$f":"(IF(AND(OR(Z13=2,J13=\"CPLL\"),OR(Z13=1,N13=\"CPLL\")),0,(IF(AND(Z13>1,LEFT(N13,4)=\"QPLL\"),AC13,IF(LEFT(J13,4)=\"QPLL\",AB13,0))*OFFSET(GTY_DATA,7,$AA$1+2)+OFFSET(GTY_DATA,7,$AA$1))/1000*AA13*$C$6))*$AG$1","v":0.37837799999999999},{"$f":"(($C$7/1000)*$E13*(SUM($AL13:$AP13)+IF($G13=\"On\",OFFSET(GTY_DATA,18,$AA$1),0))*OFFSET(POWER_SCALE,6,OFFSET(POWER_SCALE,1,1)))*$AG$1","v":2.2388722399999996},{"$f":"(($C$8/1000)*$E13*(($AQ13+$AJ13+IF($AJ13>0,-50,0)+$AK13+IF(Z13<>1,OFFSET(GTY_DATA,10,$AU13)+OFFSET(GTY_DATA,10,$AV13)*O13*1000+$AI13+OFFSET(GTY_DATA,15,$Z$1),0)+IF(Z13<>2,OFFSET(GTY_DATA,11+$AH13,$AU13)+OFFSET(GTY_DATA,11+$AH13,$AV13)*K13*1000,0)*OFFSET(POWER_SCALE,6,OFFSET(POWER_SCALE,1,1)))+IF($S13=\"Yes\",OFFSET(GTY_DATA,16,$AA$1),0)))*$AG$1","v":13.349623372799998},null,{"$f":"IF($F13=\"Receiver\",1,IF($F13=\"Transmitter\",2,3))","v":1},{"$f":"INT((E13+3)/4)","v":11},{"$f":"IF(OR($Z13=2,$J13=\"CPLL\"),0,1000*IF(AND($J13=\"QPLL1\",$AY13>=0),$AY13,IF($BA13>=0,$BA13,MIN(MAX($J13,$AE$2),$AF$3))))","v":12800},{"$f":"IF(OR($Z13=1,$N13=\"CPLL\"),0,1000*IF(AND($N13=\"QPLL1\",$AZ13>=0),$AZ13,IF($BB13>=0,$BB13,MIN(MAX($N13,$AE$2),$AF$3))))","v":0},{"$f":"IF($Z13=2,0,1000*IF($K13/2 >= $AB$103,$K13/2,IF($K13 >= $AB$103,$K13,$K13*2)))","v":6400},{"$f":"IF($Z13=1,0,IF($O13/2 >= $AB$103,$O13/2,IF($O13 >= $AB$103,$O13,$O13*2))) * 1000","v":0},{"$f":" IF(AND($Z13<>2,$L13 > 0), $K13*1000/IF(AND($L13=64,LEFT($M13,3)=\"64b\"),32,IF(OR($M13=\"8b/10b\",INT($L13/10)*10=$L13),IF($L13>=32,40,20),IF($L13>=32,32,16))),0)","v":320},{"$f":" IF(AND($Z13<>1,$P13 > 0), $O13*1000/IF(AND($P13=64,LEFT($Q13,3)=\"64b\"),32,IF(OR($Q13=\"8b/10b\",INT($P13/10)*10=$P13),IF($P13>=32,40,20),IF($P13>=32,32,16))),0)","v":0},{"$f":"IF($H13=\"Low Power\",0,1)","v":0},{"$f":"IF($Z13>1,$R13^2*OFFSET(GTY_DATA,1,15)+$R13*OFFSET(GTY_DATA,2,15)+OFFSET(GTY_DATA,3,15),0)","v":0},{"$f":"IF(AND(Z13>1,N13=\"CPLL\"),O13,IF(AND(Z13<>2,J13=\"CPLL\"),K13,0))*1000*OFFSET(GTY_DATA,5,2+$Z$1)+IF(OR(AND(Z13<>2,J13=\"CPLL\"),AND(Z13<>1,N13=\"CPLL\")),OFFSET(GTY_DATA,5,$Z$1),0)","v":0},{"$f":"(IF(AND(Z13>2,LEFT(N13,4)=\"QPLL\",LEFT(J13,4)=\"QPLL\",N13<>J13),(AB13+AC13)/2,IF(AND(Z13>1,LEFT(N13,4)=\"QPLL\"),AC13*IF($K13<9.8,IF(AB13=K13*1000,0.14*(9.8-K13),IF($K13<9,1,0))),IF(AND(Z13<>2,LEFT(J13,4)=\"QPLL\"),AB13*IF($O13<9.8,IF(AB13=$O13*1000,0.14*(9.8-$O13),IF($O13<9,1,0))),0)))*OFFSET(GTY_DATA,8,2+$Z$1) + IF(AND(OR(Z13=2,J13=\"CPLL\"),OR(Z13=1,N13=\"CPLL\")),0,OFFSET(GTY_DATA,8,$Z$1)))*1/MAX(IF(E13>I13,I13,4),1)","v":64},{"$f":"IF(Z13=2,0,K13*1000*OFFSET(GTY_DATA,3+$AH13,$AV13)+OFFSET(GTY_DATA,3+$AH13,$AU13))","v":50.320959999999999},{"$f":"IF(Z13=1,0,O13*1000*OFFSET(GTY_DATA,2,2+$Z$1)+OFFSET(GTY_DATA,2,$Z$1))","v":0},{"$f":" IF(AND(Z13>1,N13=\"CPLL\"),AE13,IF(J13=\"CPLL\",AD13,0))*OFFSET(GTY_DATA,6,2+$Z$1) + IF(OR(AND(Z13<>2,J13=\"CPLL\"),AND(Z13<>1,N13=\"CPLL\")),OFFSET(GTY_DATA,6,$Z$1),0)","v":0},{"$f":"(IF(AND(Z13>2,LEFT(N13,4)=\"QPLL\",LEFT(J13,4)=\"QPLL\",N13<>J13),(AB13+AC13)/2,IF(AND(Z13>1,LEFT(N13,4)=\"QPLL\"),AC13,IF(AND(Z13<>2,LEFT(J13,4)=\"QPLL\"),AB13,0)))*OFFSET(GTY_DATA,9,2+$Z$1) + IF(AND(OR(Z13=2,J13=\"CPLL\"),OR(Z13=1,N13=\"CPLL\")),0,OFFSET(GTY_DATA,9,$Z$1)))*1/MAX(IF(E13>I13,I13,4),1)","v":0.5625},{"$f":"OFFSET(GTY_DATA,13,$Z$1)","v":0},{"$f":"OFFSET(GTY_DATA,14,$AU13)+MAX($K13,O13)*1000*OFFSET(GTY_DATA,14,$AV13)","v":51.640176000000004},{"$f":"IF(AND(E13>0,LEFT(T13,4)=\"PCIe\"),OFFSET(PCIE_DATA,IF(K13<=2.5,9,IF(K13<=5,13,17))+IF(E13=1,1,IF(E13=2,2,IF(E13<5,3,4))),IF(RIGHT(T13,3)=\"500\",2,1)),0)","v":0},{"$f":"IF($Z13<>2,$E13*OFFSET(GTY_DATA,17,$AA$1),0)","v":0},493,{"$f":"IF(K13>29,17,IF(K13>26,13,IF(K13>22,11,IF(K13>15,9,IF(K13>12.5,7,IF(K13>11,5,$Z$1+0))))))","v":7},{"$f":"IF(K13>29,18,IF(K13>26,14,IF(K13>22,12,IF(K13>15,10,IF(K13>12.5,8,IF(K13>11,6,$Z$1+2))))))","v":8},{"$f":"IF(AND(E13>0,LEFT(T13,4)=\"CMAC\"),OFFSET(CMAC_DATA,1+IF(MAX(K13,Q14)>=25,1,0),1+(IF(MID(T13,6,1)=\"H\",0,IF(MID(T13,6,1)=\"L\",2,1)))),0)","v":0},{"$f":"IF(AND(E13>0,LEFT(T13,4)=\"ILKN\"),OFFSET(ILMAC_DATA,IF(K13<=16.4,2,1),1+IF(MID(T13,6,1)=\"H\",0,IF(MID(T13,6,1)=\"L\",2,1))),0)","v":0},{"$f":"IF(AND($K13/2>=$AE$2,$K13/2<=$AE$3),$K13/2,IF(AND($K13>=$AE$2,$K13<=$AE$3),$K13,IF(AND($K13*2>=$AE$2,$K13*2<=$AE$3),$K13*2,IF(AND($K13*4>=$AE$2,$K13*4<=$AE$3),$K13*4,IF(AND($K13*8>=$AE$2,$K13*8<=$AE$3),$K13*8,IF(AND($K13*16>=$AE$2,$K13*16<=$AE$3),$K13*16,-1))))))","v":12.8},{"$f":"IF(AND($O13/2>=$AE$2,$O13/2<=$AE$3),$O13/2,IF(AND($O13>=$AE$2,$O13<=$AE$3),$O13,IF(AND($O13*2>=$AE$2,$O13*2<=$AE$3),$O13*2,IF(AND($O13*4>=$AE$2,$O13*4<=$AE$3),$O13*4,IF(AND($O13*8>=$AE$2,$O13*8<=$AE$3),$O13*8,IF(AND($O13*16>=$AE$2,$O13*16<=$AE$3),$O13*16,-1))))))","v":-1},{"$f":"IF(AND($K13/2>=$AF$2,$K13/2<=$AF$3),$K13/2,IF(AND($K13>=$AF$2,$K13<=$AF$3),$K13,IF(AND($K13*2>=$AF$2,$K13*2<=$AF$3),$K13*2,IF(AND($K13*4>=$AF$2,$K13*4<=$AF$3),$K13*4,IF(AND($K13*8>=$AF$2,$K13*8<=$AF$3),$K13*8,IF(AND($K13*16>=$AF$2,$K13*16<=$AF$3),$K13*16,-1))))))","v":12.8},{"$f":"IF(AND($O13/2>=$AF$2,$O13/2<=$AF$3),$O13/2,IF(AND($O13>=$AF$2,$O13<=$AF$3),$O13,IF(AND($O13*2>=$AF$2,$O13*2<=$AF$3),$O13*2,IF(AND($O13*4>=$AF$2,$O13*4<=$AF$3),$O13*4,IF(AND($O13*8>=$AF$2,$O13*8<=$AF$3),$O13*8,IF(AND($O13*16>=$AF$2,$O13*16<=$AF$3),$O13*16,-1))))))","v":-1},{"$f":"IF($J13=\"QPLL1\",$AY13,$BA13)","v":12.8},{"$f":"IF($N13=\"QPLL1\",$AZ13,$BB13)","v":-1}]
[null,"Out",null,null,12,"Transceiver","Off","Low Power",4,"QPLL1",12.8,32,"8b/10b","QPLL0",12.8,32,"8b/10b",998,"No",null,0.572985074496,0.10319399999999999,1.17747048,5.9179172543999998,null,{"$f":"IF($F14=\"Receiver\",1,IF($F14=\"Transmitter\",2,3))","v":3},3,{"$f":"IF(OR($Z14=2,$J14=\"CPLL\"),0,1000*IF(AND($J14=\"QPLL1\",$AY14>=0),$AY14,IF($BA14>=0,$BA14,MIN(MAX($J14,$AE$2),$AF$3))))","v":12800},{"$f":"IF(OR($Z14=1,$N14=\"CPLL\"),0,1000*IF(AND($N14=\"QPLL1\",$AZ14>=0),$AZ14,IF($BB14>=0,$BB14,MIN(MAX($N14,$AE$2),$AF$3))))","v":12800},6400,6400,320,320,0,22.093900000000001,0,64,50.320959999999999,47.239080000000001,0,0.5625,0,51.640176000000004,0,0,523,{"$f":"IF(K14>29,17,IF(K14>26,13,IF(K14>22,11,IF(K14>15,9,IF(K14>12.5,7,IF(K14>11,5,$Z$1+0))))))","v":7},{"$f":"IF(K14>29,18,IF(K14>26,14,IF(K14>22,12,IF(K14>15,10,IF(K14>12.5,8,IF(K14>11,6,$Z$1+2))))))","v":8},0,0,{"$f":"IF(AND($K14/2>=$AE$2,$K14/2<=$AE$3),$K14/2,IF(AND($K14>=$AE$2,$K14<=$AE$3),$K14,IF(AND($K14*2>=$AE$2,$K14*2<=$AE$3),$K14*2,IF(AND($K14*4>=$AE$2,$K14*4<=$AE$3),$K14*4,IF(AND($K14*8>=$AE$2,$K14*8<=$AE$3),$K14*8,IF(AND($K14*16>=$AE$2,$K14*16<=$AE$3),$K14*16,-1))))))","v":12.8},{"$f":"IF(AND($O14/2>=$AE$2,$O14/2<=$AE$3),$O14/2,IF(AND($O14>=$AE$2,$O14<=$AE$3),$O14,IF(AND($O14*2>=$AE$2,$O14*2<=$AE$3),$O14*2,IF(AND($O14*4>=$AE$2,$O14*4<=$AE$3),$O14*4,IF(AND($O14*8>=$AE$2,$O14*8<=$AE$3),$O14*8,IF(AND($O14*16>=$AE$2,$O14*16<=$AE$3),$O14*16,-1))))))","v":12.8},{"$f":"IF(AND($K14/2>=$AF$2,$K14/2<=$AF$3),$K14/2,IF(AND($K14>=$AF$2,$K14<=$AF$3),$K14,IF(AND($K14*2>=$AF$2,$K14*2<=$AF$3),$K14*2,IF(AND($K14*4>=$AF$2,$K14*4<=$AF$3),$K14*4,IF(AND($K14*8>=$AF$2,$K14*8<=$AF$3),$K14*8,IF(AND($K14*16>=$AF$2,$K14*16<=$AF$3),$K14*16,-1))))))","v":12.8},{"$f":"IF(AND($O14/2>=$AF$2,$O14/2<=$AF$3),$O14/2,IF(AND($O14>=$AF$2,$O14<=$AF$3),$O14,IF(AND($O14*2>=$AF$2,$O14*2<=$AF$3),$O14*2,IF(AND($O14*4>=$AF$2,$O14*4<=$AF$3),$O14*4,IF(AND($O14*8>=$AF$2,$O14*8<=$AF$3),$O14*8,IF(AND($O14*16>=$AF$2,$O14*16<=$AF$3),$O14*16,-1))))))","v":12.8},{"$f":"IF($J14=\"QPLL1\",$AY14,$BA14)","v":12.8},{"$f":"IF($N14=\"QPLL1\",$AZ14,$BB14)","v":12.8}]
[null,"IPBus",null,null,2,"Transceiver","Off","Low Power",2,"QPLL1",1,32,"8b/10b","QPLL1",1,32,"8b/10b",166,"No",null,1.8445273625000001E-2,3.4397999999999998E-2,6.9388000000000005E-2,0.6529903199999999,null,3,1,8000,8000,2000,2000,25,25,0,2.2923,0,40,22.5532,11.5783,0,0.5625,0,35.014000000000003,0,0,552,1,3,0,0,8,8,16,16,8,8]
[null,"ROD",null,null,2,"Transceiver","Off","Low Power",2,"QPLL1",12.8,32,"8b/10b","QPLL0",12.8,32,"8b/10b",166,"No",null,9.5497512415999991E-2,3.4397999999999998E-2,0.19624508000000002,0.93879570239999999,null,3,1,12800,12800,6400,6400,320,320,0,2.2923,0,64,50.320959999999999,47.239080000000001,0,0.5625,0,51.640176000000004,0,0,582,7,8,0,0,12.8,12.8,12.8,12.8,12.8,12.8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b",{"$f":"$J17","v":"QPLL1"},{"$f":"$K17","v":8},{"$f":"$L17","v":32},{"$f":"$M17","v":"8b/10b"},166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,612,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,641,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,671,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,701,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,730,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,760,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,790,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,819,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,849,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,879,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,908,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,938,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,968,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,998,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,1027,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,1057,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,1087,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b",{"$f":"$J45","v":"QPLL1"},{"$f":"$K45","v":8},{"$f":"$L45","v":32},{"$f":"$M45","v":"8b/10b"},166,"No",null,{"$f":"(VCCINT/1000)*VCCINT_N*($E45*(OFFSET(GTY_DATA,1,$AA$1)+OFFSET(GTY_DATA,1,2+$AA$1)*MAX(IF($Z45<>2,$K45,0),IF($Z45>1,$O45,0))+IF(MAX(IF($Z45<>2,$K45,0),IF($Z45>1,$O45,0))>20.6,IF($AH45>0,-20,-40),0))+$AS45+AR45+AW45+AX45)","v":0},{"$f":"(IF(AND(OR(Z45=2,J45=\"CPLL\"),OR(Z45=1,N45=\"CPLL\")),0,(IF(AND(Z45>1,LEFT(N45,4)=\"QPLL\"),AC45,IF(LEFT(J45,4)=\"QPLL\",AB45,0))*OFFSET(GTY_DATA,7,$AA$1+2)+OFFSET(GTY_DATA,7,$AA$1))/1000*AA45*$C$6))*$AG$1","v":0},{"$f":"(($C$7/1000)*$E45*(SUM($AL45:$AP45)+IF($G45=\"On\",OFFSET(GTY_DATA,18,$AA$1),0))*OFFSET(POWER_SCALE,6,OFFSET(POWER_SCALE,1,1)))*$AG$1","v":0},{"$f":"(($C$8/1000)*$E45*(($AQ45+$AJ45+IF($AJ45>0,-50,0)+$AK45+IF(Z45<>1,OFFSET(GTY_DATA,10,$AU45)+OFFSET(GTY_DATA,10,$AV45)*O45*1000+$AI45+OFFSET(GTY_DATA,15,$Z$1),0)+IF(Z45<>2,OFFSET(GTY_DATA,11+$AH45,$AU45)+OFFSET(GTY_DATA,11+$AH45,$AV45)*K45*1000,0)*OFFSET(POWER_SCALE,6,OFFSET(POWER_SCALE,1,1)))+IF($S45=\"Yes\",OFFSET(GTY_DATA,16,$AA$1),0)))*$AG$1","v":0},null,3,{"$f":"INT((E45+3)/4)","v":0},8000,8000,{"$f":"IF($Z45=2,0,1000*IF($K45/2 >= $AB$103,$K45/2,IF($K45 >= $AB$103,$K45,$K45*2)))","v":4000},{"$f":"IF($Z45=1,0,IF($O45/2 >= $AB$103,$O45/2,IF($O45 >= $AB$103,$O45,$O45*2))) * 1000","v":4000},{"$f":" IF(AND($Z45<>2,$L45 > 0), $K45*1000/IF(AND($L45=64,LEFT($M45,3)=\"64b\"),32,IF(OR($M45=\"8b/10b\",INT($L45/10)*10=$L45),IF($L45>=32,40,20),IF($L45>=32,32,16))),0)","v":200},{"$f":" IF(AND($Z45<>1,$P45 > 0), $O45*1000/IF(AND($P45=64,LEFT($Q45,3)=\"64b\"),32,IF(OR($Q45=\"8b/10b\",INT($P45/10)*10=$P45),IF($P45>=32,40,20),IF($P45>=32,32,16))),0)","v":200},{"$f":"IF($H45=\"Low Power\",0,1)","v":0},{"$f":"IF($Z45>1,$R45^2*OFFSET(GTY_DATA,1,15)+$R45*OFFSET(GTY_DATA,2,15)+OFFSET(GTY_DATA,3,15),0)","v":2.2923},{"$f":"IF(AND(Z45>1,N45=\"CPLL\"),O45,IF(AND(Z45<>2,J45=\"CPLL\"),K45,0))*1000*OFFSET(GTY_DATA,5,2+$Z$1)+IF(OR(AND(Z45<>2,J45=\"CPLL\"),AND(Z45<>1,N45=\"CPLL\")),OFFSET(GTY_DATA,5,$Z$1),0)","v":0},{"$f":"(IF(AND(Z45>2,LEFT(N45,4)=\"QPLL\",LEFT(J45,4)=\"QPLL\",N45<>J45),(AB45+AC45)/2,IF(AND(Z45>1,LEFT(N45,4)=\"QPLL\"),AC45*IF($K45<9.8,IF(AB45=K45*1000,0.14*(9.8-K45),IF($K45<9,1,0))),IF(AND(Z45<>2,LEFT(J45,4)=\"QPLL\"),AB45*IF($O45<9.8,IF(AB45=$O45*1000,0.14*(9.8-$O45),IF($O45<9,1,0))),0)))*OFFSET(GTY_DATA,8,2+$Z$1) + IF(AND(OR(Z45=2,J45=\"CPLL\"),OR(Z45=1,N45=\"CPLL\")),0,OFFSET(GTY_DATA,8,$Z$1)))*1/MAX(IF(E45>I45,I45,4),1)","v":10.080000000000005},{"$f":"IF(Z45=2,0,K45*1000*OFFSET(GTY_DATA,3+$AH45,$AV45)+OFFSET(GTY_DATA,3+$AH45,$AU45))","v":39.025599999999997},{"$f":"IF(Z45=1,0,O45*1000*OFFSET(GTY_DATA,2,2+$Z$1)+OFFSET(GTY_DATA,2,$Z$1))","v":32.733000000000004},{"$f":" IF(AND(Z45>1,N45=\"CPLL\"),AE45,IF(J45=\"CPLL\",AD45,0))*OFFSET(GTY_DATA,6,2+$Z$1) + IF(OR(AND(Z45<>2,J45=\"CPLL\"),AND(Z45<>1,N45=\"CPLL\")),OFFSET(GTY_DATA,6,$Z$1),0)","v":0},{"$f":"(IF(AND(Z45>2,LEFT(N45,4)=\"QPLL\",LEFT(J45,4)=\"QPLL\",N45<>J45),(AB45+AC45)/2,IF(AND(Z45>1,LEFT(N45,4)=\"QPLL\"),AC45,IF(AND(Z45<>2,LEFT(J45,4)=\"QPLL\"),AB45,0)))*OFFSET(GTY_DATA,9,2+$Z$1) + IF(AND(OR(Z45=2,J45=\"CPLL\"),OR(Z45=1,N45=\"CPLL\")),0,OFFSET(GTY_DATA,9,$Z$1)))*1/MAX(IF(E45>I45,I45,4),1)","v":0.5625},{"$f":"OFFSET(GTY_DATA,13,$Z$1)","v":0},{"$f":"OFFSET(GTY_DATA,14,$AU45)+MAX($K45,O45)*1000*OFFSET(GTY_DATA,14,$AV45)","v":35.112000000000002},{"$f":"IF(AND(E45>0,LEFT(T45,4)=\"PCIe\"),OFFSET(PCIE_DATA,IF(K45<=2.5,9,IF(K45<=5,13,17))+IF(E45=1,1,IF(E45=2,2,IF(E45<5,3,4))),IF(RIGHT(T45,3)=\"500\",2,1)),0)","v":0},{"$f":"IF($Z45<>2,$E45*OFFSET(GTY_DATA,17,$AA$1),0)","v":0},null,1,3,{"$f":"IF(AND(E45>0,LEFT(T45,4)=\"CMAC\"),OFFSET(CMAC_DATA,1+IF(MAX(K45,Q46)>=25,1,0),1+(IF(MID(T45,6,1)=\"H\",0,IF(MID(T45,6,1)=\"L\",2,1)))),0)","v":0},{"$f":"IF(AND(E45>0,LEFT(T45,4)=\"ILKN\"),OFFSET(ILMAC_DATA,IF(K45<=16.4,2,1),1+IF(MID(T45,6,1)=\"H\",0,IF(MID(T45,6,1)=\"L\",2,1))),0)","v":0},8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b",{"$f":"$J77","v":"QPLL1"},{"$f":"$K77","v":8},{"$f":"$L77","v":32},{"$f":"$M77","v":"8b/10b"},166,"No",null,{"$f":"(VCCINT/1000)*VCCINT_N*($E77*(OFFSET(GTY_DATA,1,$AA$1)+OFFSET(GTY_DATA,1,2+$AA$1)*MAX(IF($Z77<>2,$K77,0),IF($Z77>1,$O77,0))+IF(MAX(IF($Z77<>2,$K77,0),IF($Z77>1,$O77,0))>20.6,IF($AH77>0,-20,-40),0))+$AS77+AR77+AW77+AX77)","v":0},{"$f":"(IF(AND(OR(Z77=2,J77=\"CPLL\"),OR(Z77=1,N77=\"CPLL\")),0,(IF(AND(Z77>1,LEFT(N77,4)=\"QPLL\"),AC77,IF(LEFT(J77,4)=\"QPLL\",AB77,0))*OFFSET(GTY_DATA,7,$AA$1+2)+OFFSET(GTY_DATA,7,$AA$1))/1000*AA77*$C$6))*$AG$1","v":0},{"$f":"(($C$7/1000)*$E77*(SUM($AL77:$AP77)+IF($G77=\"On\",OFFSET(GTY_DATA,18,$AA$1),0))*OFFSET(POWER_SCALE,6,OFFSET(POWER_SCALE,1,1)))*$AG$1","v":0},{"$f":"(($C$8/1000)*$E77*(($AQ77+$AJ77+IF($AJ77>0,-50,0)+$AK77+IF(Z77<>1,OFFSET(GTY_DATA,10,$AU77)+OFFSET(GTY_DATA,10,$AV77)*O77*1000+$AI77+OFFSET(GTY_DATA,15,$Z$1),0)+IF(Z77<>2,OFFSET(GTY_DATA,11+$AH77,$AU77)+OFFSET(GTY_DATA,11+$AH77,$AV77)*K77*1000,0)*OFFSET(POWER_SCALE,6,OFFSET(POWER_SCALE,1,1)))+IF($S77=\"Yes\",OFFSET(GTY_DATA,16,$AA$1),0)))*$AG$1","v":0},null,3,{"$f":"INT((E77+3)/4)","v":0},8000,8000,{"$f":"IF($Z77=2,0,1000*IF($K77/2 >= $AB$103,$K77/2,IF($K77 >= $AB$103,$K77,$K77*2)))","v":4000},{"$f":"IF($Z77=1,0,IF($O77/2 >= $AB$103,$O77/2,IF($O77 >= $AB$103,$O77,$O77*2))) * 1000","v":4000},{"$f":" IF(AND($Z77<>2,$L77 > 0), $K77*1000/IF(AND($L77=64,LEFT($M77,3)=\"64b\"),32,IF(OR($M77=\"8b/10b\",INT($L77/10)*10=$L77),IF($L77>=32,40,20),IF($L77>=32,32,16))),0)","v":200},{"$f":" IF(AND($Z77<>1,$P77 > 0), $O77*1000/IF(AND($P77=64,LEFT($Q77,3)=\"64b\"),32,IF(OR($Q77=\"8b/10b\",INT($P77/10)*10=$P77),IF($P77>=32,40,20),IF($P77>=32,32,16))),0)","v":200},{"$f":"IF($H77=\"Low Power\",0,1)","v":0},{"$f":"IF($Z77>1,$R77^2*OFFSET(GTY_DATA,1,15)+$R77*OFFSET(GTY_DATA,2,15)+OFFSET(GTY_DATA,3,15),0)","v":2.2923},{"$f":"IF(AND(Z77>1,N77=\"CPLL\"),O77,IF(AND(Z77<>2,J77=\"CPLL\"),K77,0))*1000*OFFSET(GTY_DATA,5,2+$Z$1)+IF(OR(AND(Z77<>2,J77=\"CPLL\"),AND(Z77<>1,N77=\"CPLL\")),OFFSET(GTY_DATA,5,$Z$1),0)","v":0},{"$f":"(IF(AND(Z77>2,LEFT(N77,4)=\"QPLL\",LEFT(J77,4)=\"QPLL\",N77<>J77),(AB77+AC77)/2,IF(AND(Z77>1,LEFT(N77,4)=\"QPLL\"),AC77*IF($K77<9.8,IF(AB77=K77*1000,0.14*(9.8-K77),IF($K77<9,1,0))),IF(AND(Z77<>2,LEFT(J77,4)=\"QPLL\"),AB77*IF($O77<9.8,IF(AB77=$O77*1000,0.14*(9.8-$O77),IF($O77<9,1,0))),0)))*OFFSET(GTY_DATA,8,2+$Z$1) + IF(AND(OR(Z77=2,J77=\"CPLL\"),OR(Z77=1,N77=\"CPLL\")),0,OFFSET(GTY_DATA,8,$Z$1)))*1/MAX(IF(E77>I77,I77,4),1)","v":10.080000000000005},{"$f":"IF(Z77=2,0,K77*1000*OFFSET(GTY_DATA,3+$AH77,$AV77)+OFFSET(GTY_DATA,3+$AH77,$AU77))","v":39.025599999999997},{"$f":"IF(Z77=1,0,O77*1000*OFFSET(GTY_DATA,2,2+$Z$1)+OFFSET(GTY_DATA,2,$Z$1))","v":32.733000000000004},{"$f":" IF(AND(Z77>1,N77=\"CPLL\"),AE77,IF(J77=\"CPLL\",AD77,0))*OFFSET(GTY_DATA,6,2+$Z$1) + IF(OR(AND(Z77<>2,J77=\"CPLL\"),AND(Z77<>1,N77=\"CPLL\")),OFFSET(GTY_DATA,6,$Z$1),0)","v":0},{"$f":"(IF(AND(Z77>2,LEFT(N77,4)=\"QPLL\",LEFT(J77,4)=\"QPLL\",N77<>J77),(AB77+AC77)/2,IF(AND(Z77>1,LEFT(N77,4)=\"QPLL\"),AC77,IF(AND(Z77<>2,LEFT(J77,4)=\"QPLL\"),AB77,0)))*OFFSET(GTY_DATA,9,2+$Z$1) + IF(AND(OR(Z77=2,J77=\"CPLL\"),OR(Z77=1,N77=\"CPLL\")),0,OFFSET(GTY_DATA,9,$Z$1)))*1/MAX(IF(E77>I77,I77,4),1)","v":0.5625},{"$f":"OFFSET(GTY_DATA,13,$Z$1)","v":0},{"$f":"OFFSET(GTY_DATA,14,$AU77)+MAX($K77,O77)*1000*OFFSET(GTY_DATA,14,$AV77)","v":35.112000000000002},{"$f":"IF(AND(E77>0,LEFT(T77,4)=\"PCIe\"),OFFSET(PCIE_DATA,IF(K77<=2.5,9,IF(K77<=5,13,17))+IF(E77=1,1,IF(E77=2,2,IF(E77<5,3,4))),IF(RIGHT(T77,3)=\"500\",2,1)),0)","v":0},{"$f":"IF($Z77<>2,$E77*OFFSET(GTY_DATA,17,$AA$1),0)","v":0},null,1,3,{"$f":"IF(AND(E77>0,LEFT(T77,4)=\"CMAC\"),OFFSET(CMAC_DATA,1+IF(MAX(K77,Q78)>=25,1,0),1+(IF(MID(T77,6,1)=\"H\",0,IF(MID(T77,6,1)=\"L\",2,1)))),0)","v":0},{"$f":"IF(AND(E77>0,LEFT(T77,4)=\"ILKN\"),OFFSET(ILMAC_DATA,IF(K77<=16.4,2,1),1+IF(MID(T77,6,1)=\"H\",0,IF(MID(T77,6,1)=\"L\",2,1))),0)","v":0},8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,{"$f":"IF($F78=\"Receiver\",1,IF($F78=\"Transmitter\",2,3))","v":3},0,{"$f":"IF(OR($Z78=2,$J78=\"CPLL\"),0,1000*IF(AND($J78=\"QPLL1\",$AY78>=0),$AY78,IF($BA78>=0,$BA78,MIN(MAX($J78,$AE$2),$AF$3))))","v":8000},{"$f":"IF(OR($Z78=1,$N78=\"CPLL\"),0,1000*IF(AND($N78=\"QPLL1\",$AZ78>=0),$AZ78,IF($BB78>=0,$BB78,MIN(MAX($N78,$AE$2),$AF$3))))","v":8000},4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,{"$f":"IF(K78>29,17,IF(K78>26,13,IF(K78>22,11,IF(K78>15,9,IF(K78>12.5,7,IF(K78>11,5,$Z$1+0))))))","v":1},{"$f":"IF(K78>29,18,IF(K78>26,14,IF(K78>22,12,IF(K78>15,10,IF(K78>12.5,8,IF(K78>11,6,$Z$1+2))))))","v":3},0,0,{"$f":"IF(AND($K78/2>=$AE$2,$K78/2<=$AE$3),$K78/2,IF(AND($K78>=$AE$2,$K78<=$AE$3),$K78,IF(AND($K78*2>=$AE$2,$K78*2<=$AE$3),$K78*2,IF(AND($K78*4>=$AE$2,$K78*4<=$AE$3),$K78*4,IF(AND($K78*8>=$AE$2,$K78*8<=$AE$3),$K78*8,IF(AND($K78*16>=$AE$2,$K78*16<=$AE$3),$K78*16,-1))))))","v":8},{"$f":"IF(AND($O78/2>=$AE$2,$O78/2<=$AE$3),$O78/2,IF(AND($O78>=$AE$2,$O78<=$AE$3),$O78,IF(AND($O78*2>=$AE$2,$O78*2<=$AE$3),$O78*2,IF(AND($O78*4>=$AE$2,$O78*4<=$AE$3),$O78*4,IF(AND($O78*8>=$AE$2,$O78*8<=$AE$3),$O78*8,IF(AND($O78*16>=$AE$2,$O78*16<=$AE$3),$O78*16,-1))))))","v":8},{"$f":"IF(AND($K78/2>=$AF$2,$K78/2<=$AF$3),$K78/2,IF(AND($K78>=$AF$2,$K78<=$AF$3),$K78,IF(AND($K78*2>=$AF$2,$K78*2<=$AF$3),$K78*2,IF(AND($K78*4>=$AF$2,$K78*4<=$AF$3),$K78*4,IF(AND($K78*8>=$AF$2,$K78*8<=$AF$3),$K78*8,IF(AND($K78*16>=$AF$2,$K78*16<=$AF$3),$K78*16,-1))))))","v":16},{"$f":"IF(AND($O78/2>=$AF$2,$O78/2<=$AF$3),$O78/2,IF(AND($O78>=$AF$2,$O78<=$AF$3),$O78,IF(AND($O78*2>=$AF$2,$O78*2<=$AF$3),$O78*2,IF(AND($O78*4>=$AF$2,$O78*4<=$AF$3),$O78*4,IF(AND($O78*8>=$AF$2,$O78*8<=$AF$3),$O78*8,IF(AND($O78*16>=$AF$2,$O78*16<=$AF$3),$O78*16,-1))))))","v":16},{"$f":"IF($J78=\"QPLL1\",$AY78,$BA78)","v":8},{"$f":"IF($N78=\"QPLL1\",$AZ78,$BB78)","v":8}]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,null,null,null,null,"Transceiver","Off","Low Power",4,"QPLL1",8,32,"8b/10b","QPLL1",8,32,"8b/10b",166,"No",null,0,0,0,0,null,3,0,8000,8000,4000,4000,200,200,0,2.2923,0,10.080000000000005,39.025599999999997,32.733000000000004,0,0.5625,0,35.112000000000002,0,0,null,1,3,0,0,8,8,16,16,8,8]
[null,{"$f":"ROW(GTHROWS)-13","v":88},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AR13:AR100)","v":0},null,null,null,null,{"$f":"SUM(AW13:AW100)","v":0},{"$f":"SUM(AX13:AX100)","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VCO MIN",null,null,null,{"$f":"1.6","v":1.6}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VCO MAX",null,null,null,{"$f":" 4","v":4}]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,3]
[null,null,null,null,null,null,null,null,null,null,null,"Power Planes",3,4]
[null,null,null,null,null,null,null,null,null,null,null,"Used Quad",{"$f":"INT((O4+3)/4)","v":15},5,null,null,null,null,null,null,{"$f":"IF(PROCESS<>\"Maximum\",1,IF(OR(NUM_DICE>5, GRADE=\"Commercial\",ISOLY),16,IF(OR(LEFT(GRADE,1)=\"Q\",LEFT(GRADE,1)=\"M\",LEFT(SPEEDGRADE,3)=\"-2L\"),46,31)))","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,"Used Pl",{"$f":"IF(GTY_PLANES>0,MAX(INT((M116+M118/2)/M118),GTYPOWERPLANE),0)","v":3},6]
[null,null,null,null,null,null,null,null,null,null,null,"Avg Quad",{"$f":"IF(GTY_PLANES>0,NUM_GTYS/GTY_PLANES/4,0)","v":5},{"$f":"\"N111:N11\" & TEXT(GTY_PLANES + 1,\"#\")","v":"N111:N114"}]
[null,null,null,null,null,null,null,null,null,null,null,"Quads",null,{"$f":"IF(GTY_PLANES>0,MAX(MIN(IF(O4>0,1,0),IF($O4*2<=NUM_GTYS,NUM_GTYS/8,NUM_GTYS/4),INT((M116+M118/2)/M118*M118)),INT(GTYPOWERPLANE*M118)),0)","v":15},null,"MMF",null,null,"x^4","x^3","x^2","x","c"]
[null,null,null,null,null,null,null,null,null,null,null,"AVCCQ",{"$f":"N119*O120*Z120*($S$120*390625+$T$120*15625+$U$120*625+$V$120*25+$W$120)/1000","v":0.13826895941516293},{"$f":"N119*Z120*($S$120*TemperatureEstimate^4+$T$120*TemperatureEstimate^3+$U$120*TemperatureEstimate^2+$V$120*TemperatureEstimate+$W$120)/1000*O120","v":0.53855255604232821},1,null,null,null,{"$f":"OFFSET(BLOCK_LEAKAGE,8,$U116)","v":1.4965611218380669E-8},{"$f":"OFFSET(BLOCK_LEAKAGE,8,$U116+1)","v":1.1042825965039589E-5},{"$f":"OFFSET(BLOCK_LEAKAGE,8,$U116+2)","v":1.8008324024245675E-3},{"$f":"OFFSET(BLOCK_LEAKAGE,8,$U116+3)","v":0.13986641471177225},{"$f":"OFFSET(BLOCK_LEAKAGE,8,$U116+4)","v":4.4173599107819443},{"$f":"OFFSET(BLOCK_LEAKAGE,10,5)","v":9.5627000000000004E-2},{"$f":"OFFSET(BLOCK_LEAKAGE,10,6)","v":2.347296},{"$f":"(X120*EXP(Y120*VCCPAUX))/(X120*EXP(Y120))","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,"AVTTQ",{"$f":"N119*O121*Z121*($S$121*390625+$T$121*15625+$U$121*625+$V$121*25+$W$121)/1000","v":0.21098190541273099},{"$f":"N119*Z121*($S$121*TemperatureEstimate^4+$T$121*TemperatureEstimate^3+$U$121*TemperatureEstimate^2+$V$121*TemperatureEstimate+$W$121)/1000*O121","v":0.23840693556877182},1,null,null,null,{"$f":"OFFSET(BLOCK_LEAKAGE,8,$U116+5)","v":2.4649305786499833E-8},{"$f":"OFFSET(BLOCK_LEAKAGE,8,$U116+6)","v":-1.1541480970309239E-7},{"$f":"OFFSET(BLOCK_LEAKAGE,8,$U116+7)","v":9.2331847762599305E-6},{"$f":"OFFSET(BLOCK_LEAKAGE,8,$U116+8)","v":1.0898455601923847E-2},{"$f":"OFFSET(BLOCK_LEAKAGE,8,$U116+9)","v":13.780528278499251},{"$f":"OFFSET(BLOCK_LEAKAGE,10,7)","v":2.2246000000000001},{"$f":"OFFSET(BLOCK_LEAKAGE,10,8)","v":-1.6696},{"$f":"X121*VCCPLL+Y121","v":0.99991999999999992}]
[null,null,null,null,null,null,null,null,null,null,null,"AUXQ",{"$f":"N119*O122*($S$122*390625+$T$122*15625+$U$122*625+$V$122*25+$W$122)/1000","v":1.0019377622505813E-4},{"$f":"N119*($S$122*TemperatureEstimate^4+$T$122*TemperatureEstimate^3+$U$122*TemperatureEstimate^2+$V$122*TemperatureEstimate+$W$122)/1000*O122","v":2.6131185913682684E-3},1,null,null,null,{"$f":"OFFSET(BLOCK_LEAKAGE,7,$U116+10)","v":6.4860950108070533E-9},{"$f":"OFFSET(BLOCK_LEAKAGE,8,$U116+11)","v":-2.8492648783160272E-7},{"$f":"OFFSET(BLOCK_LEAKAGE,7,$U116+12)","v":-3.2614893996764716E-6},{"$f":"OFFSET(BLOCK_LEAKAGE,8,$U116+13)","v":6.0933950674031689E-4},{"$f":"OFFSET(BLOCK_LEAKAGE,8,$U116+14)","v":-4.5971262032672988E-3}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N120:N121)","v":0.77695949161110001},{"$f":"IF(NUM_GTYS>0,GTYAVCCQ*C7 +GTYVTTXQ*C8 +GTYAUXQ*C6,0)","v":0.82934449218931727}]

{"sheet":"HardIP","index":19,"n_rows":24,"n_cols":19,"rows_kept":24,"cut":false,"hidden":true,"merged":[[9,1,9,3],[10,1,10,3],[2,1,2,3],[2,5,2,7],[2,9,2,11],[4,1,4,3],[4,9,4,11],[11,1,11,3],[12,1,12,3],[0,1,0,13],[22,1,22,3],[18,1,18,3],[19,1,19,3],[14,1,14,3],[15,1,15,3],[16,1,16,3],[17,1,17,3],[13,1,13,3],[6,1,6,3],[7,1,7,3],[20,1,20,3],[21,1,21,3],[8,1,8,3]]}
[null,"                                                  Hard IP Block Power",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(NUM_CMACS>0,NUM_ILMACS>0),\"N1:N3\",IF(NUM_CMACS>0,\"N1:N2\",\"N1\"))","v":"N1:N3"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"CMAC"]
[null,"Power",null,null,null,"Utilization",null,null,null,null,null,null,null,"ILKN"]
[null,"VCCINT",{"$f":"VCCINT","v":0.95},{"$f":"IF(OR(NUM_CMACS>0,NUM_ILMACS>0),SUM(F8:F23),0)*PL_POWERED","v":0},null,"CMAC",{"$f":"IF(NUM_CMACS>0,COUNTIF(E8:E23,\"=CMAC\"),\"N/A\")","v":0},{"$f":"IF(NUM_CMACS>0,G4/NUM_CMACS,\"N/A\")","v":0}]
[null,{"$f":"TEXT((CMAC_POWER+ILMAC_POWER)/TOTAL_POWER,\"0%\")&\" of total on-chip power \"&TEXT(TOTAL_POWER,\"0.000\")&\"W\"","v":"0% of total on-chip power 0.084W"},null,null,null,"ILKN",{"$f":"IF(NUM_ILMACS>0,COUNTIF(E8:E23,\"=ILKN\"),\"N/A\")","v":0},{"$f":"IF(NUM_ILMACS>0,G5/NUM_ILMACS,\"N/A\")","v":0},null,"XPE User Guide"]
[]
[null,"Name",null,null,"CMAC or ILKN","Power (W)"]
[null,null,null,null,null,{"$f":"IF(E8=\"CMAC\",OFFSET(CMAC_DATA,1,1),IF(E8=\"ILKN\",OFFSET(ILMAC_DATA,1,1),0))*(VCCINT/1000)*VCCINT_N","v":0}]
[null,null,null,null,null,0]
[null,null,null,null,null,0]
[null,null,null,null,null,0]
[null,null,null,null,null,0]
[null,null,null,null,null,0]
[null,null,null,null,null,0]
[null,null,null,null,null,0]
[null,null,null,null,null,0]
[null,null,null,null,null,0]
[null,null,null,null,null,0]
[null,null,null,null,null,0]
[null,null,null,null,null,0]
[null,null,null,null,null,0]
[null,null,null,null,null,0]
[null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,{"$f":"(VCCINT/1000)*VCCINT_N*(GTH!$AV101+GTY!$AW101)","v":0},{"$f":"(VCCINT/1000)*VCCINT_N*(GTH!$AW101+GTY!$AX101)","v":0}]

{"sheet":"Data","index":20,"n_rows":1006,"n_cols":167,"rows_kept":1006,"cut":false,"hidden":true,"merged":[[13,39,13,41],[227,133,227,135],[227,136,227,138],[226,118,226,132],[227,113,227,117],[227,118,227,122],[227,123,227,127],[227,128,227,132],[227,93,227,97],[227,98,227,102],[227,103,227,107],[227,108,227,112],[226,88,226,102],[226,103,226,117],[227,73,227,77],[227,78,227,82],[226,73,226,87],[227,83,227,87],[227,88,227,92],[396,39,396,40],[396,43,396,44],[396,49,396,50],[396,51,396,52],[227,41,227,45],[227,46,227,50],[227,51,227,55],[396,45,396,46],[226,46,226,60],[227,36,227,40],[396,31,396,32],[385,2,385,3],[396,23,396,24],[396,41,396,42],[396,35,396,36],[396,33,396,34],[396,37,396,38],[396,27,396,28],[396,29,396,30],[396,21,396,22],[396,25,396,26],[396,11,396,12],[396,15,396,16],[396,1,396,2],[812,3,812,6],[396,7,396,8],[396,3,396,4],[396,5,396,6],[227,1,227,5],[227,6,227,10],[282,5,282,7],[282,8,282,10],[39,5,39,8],[226,1,226,15],[226,16,226,30],[62,15,62,17],[556,18,556,20],[227,11,227,15],[282,15,282,16],[396,13,396,14],[396,19,396,20],[396,17,396,18],[282,11,282,12],[282,17,282,18],[282,13,282,14],[227,16,227,20],[227,21,227,25],[227,26,227,30],[33,36,33,40],[33,1,33,5],[33,6,33,10],[33,11,33,15],[33,16,33,20],[33,31,33,35],[227,31,227,35],[226,31,226,45],[227,153,227,166],[227,139,227,152],[13,25,13,32],[227,61,227,63],[227,67,227,69],[227,70,227,72],[227,64,227,66],[33,41,33,45],[33,46,33,50],[33,51,33,55],[33,56,33,60],[227,56,227,60],[33,21,33,25],[33,26,33,30]]}
["FAMILIES","Supply","Min","Max",null,"Grade","Factor","WireBond","Process","Speed","Heatsink","Board",null,null,"GT OpMode","DataMode","RawWidth","8b/10b","PwrMode","PLL","Channels","int1"]
["Artix-7","Vccint",{"$f":"IF(SPEEDGRADE=\"-2L (0.85V)\",0.82,IF(SPEEDGRADE=\"-1L (0.9V)\",0.88,IF(OR(SPEEDGRADE=\"-3\",SPEEDGRADE=\"-1H\"),0.97,0.92)))","v":0.92},{"$f":"IF(SPEEDGRADE=\"-1L (0.9V)\",0.92,IF(OR(SPEEDGRADE=\"-3\",SPEEDGRADE=-3,SPEEDGRADE=\"-1H\"),1.03,0.979))","v":0.97899999999999998},null,"Extended",1,{"$f":"OR(LEFT(PACKAGE,1)=\"C\",LEFT(PACKAGE,2)=\"FT\",LEFT(PACKAGE,2)=\"FG\")","v":false},"Typical","-1","None","JEDEC (2S2P)",null,null,"Transceiver","Raw",16,16,"Low Power","CPLL",1,4]
["Kintex UltraScale","Vbram",{"$f":"IF(OR(SPEEDGRADE=\"-3\",SPEEDGRADE=\"-1H\"),0.97,0.922)","v":0.92200000000000004},{"$f":"IF(OR(SPEEDGRADE=\"-3\",SPEEDGRADE=-3,SPEEDGRADE=\"-1H\"),1.03,0.979)","v":0.97899999999999998},null,"Industrial",2,{"$f":"IF(OR(EXACT(SPEEDGRADE,\"-1\"),LEFT(SPEEDGRADE,5)=\"-2L (\"),-1,IF(EXACT(SPEEDGRADE,\"-3\"),-3,-2))","v":-2},"Maximum","-2","Custom","Small (4\"x4\")",null,null,"Receiver","8b/10b",20,32,"DFE","QPLL0",2,8]
["Virtex UltraScale",null,null,null,null,null,null,null,null,"","Low Profile","Medium (10\"x10\")",null,null,"Transmitter","64b/66b",32,64,"Functional","QPLL1",4,12]
["Zynq-7000","VID ok?",{"$f":"IF(AND(FAMILY=\"Virtex-7\",NUM_DICE=1,EXACT(SPEEDGRADE,\"-1\"),GRADE=\"Commercial\"),1,0)","v":0},null,null,null,null,null,null,"","Medium Profile","Large (20\"x20\")",null,null,null,"64b/67b",40,null,"CTLE Tuning",null,8]
["Artix-7 Automotive",null,null,null,null,null,null,null,null,null,"High Profile","Custom",null,null,null,"128b/130b",64,"GTZ",null,null,16]
["Zynq-7000 Automotive","Junction",-40,100,null,"Quick Temp",{"$f":"TemperatureEstimate","v":83.634328072469927},null,null,null,null,null,null,null,null,null,80,40]
["Artix-7 Defense",null,null,null,null,"LVDS scale",{"$f":"IF(TRUE,1,8/IF(PROCESS_FACTOR>1,-0.0131*G7+8.9271,-0.0052*G7+5.7614))","v":1},null,null,null,null,null,null,null,null,null,null,80]
["Kintex-7 Defense","Status",{"$f":"IF(OR(PART=\"XCKU025\",AND(OR(PART=\"XCVU080\",PART=\"XCVU095\"),LEFT(SPEEDGRADE,3)<>\"-1H\"),PART=\"XCKU060\",PART=\"XCKU040\",PART=\"XCKU035\",PART=\"XCKU095\",AND(OR(PART=\"XCKU085\",PART=\"XCKU115\",PART=\"XCVU190\",PART=\"XCVU160\"),OR(SPEEDGRADE=-1,SPEEDGRADE=\"-1\",SPEEDGRADE=-2,SPEEDGRADE=\"-2\",SPEEDGRADE=-3,SPEEDGRADE=\"-3\")),AND(PART=\"XCVU440\",OR(SPEEDGRADE=-1,SPEEDGRADE=\"-1\",SPEEDGRADE=-2,SPEEDGRADE=\"-2\"))),\"Production\",\"Advance\")","v":"Production"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,160]
["Virtex-7 Defense"]
["Zynq-7000 Defense"]
["Kintex-7 SCD",{"$f":"IF(FALSE,0.87,1)","v":1}]
[]
[{"$f":"MATCH(PART,PARTLIST,FALSE)","v":13},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Power Up Current (adder to Iccq)",null,null,null,null,null,null,null,null,null,null,null,null,null,"Power Up current "]
["PARTS","CLKROWS","CLKCOLS","BUFG","BUFR","BUFIO","LUT","LUTRAM","FF","BRAM","DSP","MMCM","PCIE","Die","Packages",null,null,null,null,null,null,null,null,null,null,"Int","Int_io","Aux","I/O","Aux_io","Bram","Avcc","Avtt","GTaux",null,"CMAC","ILMAC","CFG",null,"YAvcc","YAvtt","YGTaux"]
["XCKU025",5,4,240,40,40,145440,135360,290880,360,1152,6,1,1,"FFVA1156",null,null,null,null,null,null,null,null,null,null,2400,null,380,100,null,50,9.5,4.5,2,null,0,0,5]
["XCKU035",5,4,240,40,40,203128,189056,406256,540,1700,10,2,1,"SFVA784","FBVA676","FBVA900","FFVA1156",null,null,null,null,null,null,null,2400,null,380,100,null,50,9.5,4.5,2,null,0,0,5]
["XCKU040",5,4,240,40,40,242400,225600,484800,600,1920,10,3,1,"SFVA784","FBVA676","FBVA900","FFVA1156",null,null,null,null,null,null,null,2400,null,380,100,null,50,9.5,4.5,2,null,0,0,5]
["XCKU060",5,5,288,40,40,331680,293760,663360,1080,2760,12,3,1,"FFVA1156","FFVA1517",null,null,null,null,null,null,null,null,null,3284,null,520,137,null,100,9.5,4.5,2,null,0,0,5]
["XCKU085",10,5,432,80,80,497520,428800,995040,1620,4100,18,4,2,"FLVA1517","FLVB1760","FLVF1924",null,null,null,null,null,null,null,null,6568,null,1040,274,null,137,9.5,4.5,2,null,0,0,10]
["XCKU095",8,5,384,64,64,537600,150400,1075200,1680,768,16,4,1,"FFVA1156","FFVC1517","FFVB1760","FFVB2104",null,null,null,null,null,null,null,5323,null,843,222,null,111,9.5,4.5,2,null,2,2,8,null,20.833333333333332,116.66666666666667,1.6666666666666667]
["XCKU115",10,5,576,80,80,663360,587520,1326720,2160,5520,24,6,2,"FLVA1517","FLVD1517","FLVB1760","FLVD1924","FLVF1924","FLVA2104","FLVB2104",null,null,null,null,6568,null,1040,274,null,137,9.5,4.5,2,null,0,0,10]
["XCVU065",5,6,240,40,40,358080,135360,716160,1260,600,10,2,1,"FFVC1517",null,null,null,null,null,null,null,null,null,null,2199,null,267,40,null,100,9.5,4.5,2,null,3,3,5,null,20.833333333333332,116.66666666666667,1.6666666666666667]
["XCVU080",8,5,384,64,64,445712,127360,891429,1421,672,16,4,1,"FFVC1517","FFVD1517","FFVB1760","FFVA2104","FFVB2104",null,null,null,null,null,null,3300,null,400,40,null,150,9.5,4.5,2,null,4,6,8,null,20.833333333333332,116.66666666666667,1.6666666666666667]
["XCVU095",8,5,384,64,64,537600,153600,1075200,1728,768,16,4,1,"FFVC1517","FFVD1517","FFVB1760","FFVA2104","FFVB2104","FFVC2104",null,null,null,null,null,3300,null,400,40,null,150,9.5,4.5,2,null,4,6,8,null,20.833333333333332,116.66666666666667,1.6666666666666667]
["XCVU125",10,6,480,80,80,716160,270720,1432320,2520,1200,20,4,2,"FLVD1517","FLVB1760","FLVA2104","FLVB2104","FLVC2104",null,null,null,null,null,null,4397,null,533,54,null,200,9.5,4.5,2,null,6,6,10,null,20.833333333333332,116.66666666666667,1.6666666666666667]
["XCVU160",15,6,720,80,80,926400,351936,1852800,3276,1560,28,4,3,"FLGB2104","FLGC2104",null,null,null,null,null,null,null,null,null,6595,null,800,80,null,300,9.5,4.5,2,null,7,9,13,null,20.833333333333332,116.66666666666667,1.6666666666666667]
["XCVU190",15,6,720,80,80,1074240,406080,2148480,3780,1800,30,6,3,"FLGB2104","FLGC2104","FLGA2577",null,null,null,null,null,null,null,null,6595,null,800,80,null,300,9.5,4.5,2,null,9,9,13,null,20.833333333333332,116.66666666666667,1.6666666666666667]
["XCVU440",15,9,720,80,80,2532960,702720,5065920,2520,2880,30,6,3,"FLGB2377","FLGA2892",null,null,null,null,null,null,null,null,null,15549,null,1885,189,null,707,9.5,4.5,2,null,3,0,15]
[]
["Block Leakage (mA)","TYP (25)","MAX (25)","c1","c2",0,null,"TT VX865","FF1.5","FF2","FF3"]
["BRAM_LEAKAGE_VCC",5.291549536697095E-4,{"$f":"L279*B32","v":0},null,null,0,null,2.4475058260749207E-3,3.4557185495351459,3.4557185495351459,3.4557185495351459]
["BRAM_LEAKAGE_VBRAM",6.5600000000000007E-3,{"$f":"L279*B33","v":0},2.2240887874227853,31.275516990856477,0,null,null,3.4557185495351459,3.4557185495351459,3.4557185495351459,"Process factors for bins (used BRAM)"]
[null,"MGTAVcc",null,null,null,null,"MGTAVtt/MGTZVddh",null,null,null,null,"MGTVccaux/MGTZVddl",null,null,null,null,"MGTAVcc",null,null,null,null,"MGTAVtt",null,null,null,null,"MGTVccaux",null,null,null,null,"MGTAVcc",null,null,null,null,"MGTAVtt",null,null,null,null,"MGTVccaux",null,null,null,null,"MGTAVcc",null,null,null,null,"MGTAVtt",null,null,null,null,"MGTVccaux"]
["Per Quad/Octal","x^4","x^3","x^2","x","c","x^4","x^3","x^2","x","c","x^4","x^3","x^2","x","c","x^4","x^3","x^2","x","c","x^4","x^3","x^2","x","c","x^4","x^3","x^2","x","c","x^4","x^3","x^2","x","c","x^4","x^3","x^2","x","c","x^4","x^3","x^2","x","c","x^4","x^3","x^2","x","c","x^4","x^3","x^2","x","c","x^4","x^3","x^2","x","c"]
["GTP",3.8743880687599882E-9,6.6997220269763771E-6,1.1091806104240854E-3,8.7707208420573238E-2,2.854548824691669,2.9566926386627962E-9,6.8619488188000005E-8,3.0651708042157973E-5,4.0665640160207992E-3,2.6746258995502563,6.4860950108070533E-9,-2.8492648783160272E-7,-3.2614893996764716E-6,6.0933950674031689E-4,-4.5971262032672988E-3,-1.1038515983955029E-8,8.2049223180657948E-6,2.9552193974106806E-3,0.36335466583659953,15.904089928263121,5.7636469910955334E-9,5.806343384694148E-7,7.7667553885472522E-5,6.7667391643963289E-3,2.7489500261629849,1.6345576944232936E-8,-5.0674260397845944E-7,-4.451102486799763E-6,1.564790088094578E-3,-3.9971402847061022E-3,-1.1038515983955029E-8,8.2049223180657948E-6,2.9552193974106806E-3,0.36335466583659953,15.904089928263121,5.7636469910955334E-9,5.806343384694148E-7,7.7667553885472522E-5,6.7667391643963289E-3,2.7489500261629849,1.3325554748688251E-8,-6.679285550839844E-7,4.7645970576657197E-7,1.7731134197627768E-3,-5.8681549595853699E-3,-1.1038515983955029E-8,8.2049223180657948E-6,2.9552193974106806E-3,0.36335466583659953,15.904089928263121,5.7636469910955334E-9,5.806343384694148E-7,7.7667553885472522E-5,6.7667391643963289E-3,2.7489500261629849,1.1994589834308496E-8,-6.4043082370666259E-7,-3.1289947882372655E-6,1.5824405851657133E-3,-2.969455075443328E-3]
["GTX",3.8743880687599882E-9,6.6997220269763771E-6,1.1091806104240854E-3,8.7707208420573238E-2,2.854548824691669,2.9566926386627962E-9,6.8619488188000005E-8,3.0651708042157973E-5,4.0665640160207992E-3,2.6746258995502563,6.4860950108070533E-9,-2.8492648783160272E-7,-3.2614893996764716E-6,6.0933950674031689E-4,-4.5971262032672988E-3,-1.1038515983955029E-8,8.2049223180657948E-6,2.9552193974106806E-3,0.36335466583659953,15.904089928263121,5.7636469910955334E-9,5.806343384694148E-7,7.7667553885472522E-5,6.7667391643963289E-3,2.7489500261629849,1.6345576944232936E-8,-5.0674260397845944E-7,-4.451102486799763E-6,1.564790088094578E-3,-3.9971402847061022E-3,-1.1038515983955029E-8,8.2049223180657948E-6,2.9552193974106806E-3,0.36335466583659953,15.904089928263121,5.7636469910955334E-9,5.806343384694148E-7,7.7667553885472522E-5,6.7667391643963289E-3,2.7489500261629849,1.3325554748688251E-8,-6.679285550839844E-7,4.7645970576657197E-7,1.7731134197627768E-3,-5.8681549595853699E-3,-1.1038515983955029E-8,8.2049223180657948E-6,2.9552193974106806E-3,0.36335466583659953,15.904089928263121,5.7636469910955334E-9,5.806343384694148E-7,7.7667553885472522E-5,6.7667391643963289E-3,2.7489500261629849,1.1994589834308496E-8,-6.4043082370666259E-7,-3.1289947882372655E-6,1.5824405851657133E-3,-2.969455075443328E-3]
["GTH",3.8743880687599882E-9,6.6997220269763771E-6,1.1091806104240854E-3,8.7707208420573238E-2,2.854548824691669,2.9566926386627962E-9,6.8619488188000005E-8,3.0651708042157973E-5,4.0665640160207992E-3,{"$f":"2.67462589955026+IF(OR(PART=\"XCKU035\",PART=\"XCKU040\",PART=\"XCKU025\"),0,7.5)","v":10.174625899550261},6.4860950108070533E-9,-2.8492648783160272E-7,-3.2614893996764716E-6,6.0933950674031689E-4,-4.5971262032672988E-3,-1.1038515983955029E-8,8.2049223180657948E-6,2.9552193974106806E-3,0.36335466583659953,15.904089928263121,5.7636469910955334E-9,5.806343384694148E-7,7.7667553885472522E-5,6.7667391643963289E-3,{"$f":"2.74895002616298+IF(OR(PART=\"XCKU035\",PART=\"XCKU040\",PART=\"XCKU025\"),0,7.5)","v":10.24895002616298},1.6345576944232936E-8,-5.0674260397845944E-7,-4.451102486799763E-6,1.564790088094578E-3,-3.9971402847061022E-3,-1.1038515983955029E-8,8.2049223180657948E-6,2.9552193974106806E-3,0.36335466583659953,15.904089928263121,5.7636469910955334E-9,5.806343384694148E-7,7.7667553885472522E-5,6.7667391643963289E-3,{"$f":"2.74895002616298+IF(OR(PART=\"XCKU035\",PART=\"XCKU040\",PART=\"XCKU025\"),0,7.5)","v":10.24895002616298},1.3325554748688251E-8,-6.679285550839844E-7,4.7645970576657197E-7,1.7731134197627768E-3,-5.8681549595853699E-3,-1.1038515983955029E-8,8.2049223180657948E-6,2.9552193974106806E-3,0.36335466583659953,15.904089928263121,5.7636469910955334E-9,5.806343384694148E-7,7.7667553885472522E-5,6.7667391643963289E-3,2.74895002616298,1.1994589834308496E-8,-6.4043082370666259E-7,-3.1289947882372655E-6,1.5824405851657133E-3,-2.969455075443328E-3]
["GTY",1.4965611218380669E-8,1.1042825965039589E-5,1.8008324024245675E-3,0.13986641471177225,4.4173599107819443,2.4649305786499833E-8,-1.1541480970309239E-7,9.2331847762599305E-6,1.0898455601923847E-2,13.780528278499251,6.4860950108070533E-9,-2.8492648783160272E-7,-3.2614893996764716E-6,6.0933950674031689E-4,-4.5971262032672988E-3,-1.1269536117357983E-8,1.5034064123875886E-5,4.8956600198582223E-3,0.58745346596263059,25.451371560043384,4.3116055424107181E-8,-2.0188119596570959E-7,1.615049567727258E-5,1.9063352933335137E-2,24.104614798307871,1.6345576944232936E-8,-5.0674260397845944E-7,-4.451102486799763E-6,1.564790088094578E-3,-3.9971402847061022E-3,-1.1269536117357983E-8,1.5034064123875886E-5,4.8956600198582223E-3,0.58745346596263059,25.451371560043384,4.3116055424107181E-8,-2.0188119596570959E-7,1.615049567727258E-5,1.9063352933335137E-2,24.104614798307871,1.3325554748688251E-8,-6.679285550839844E-7,4.7645970576657197E-7,1.7731134197627768E-3,-5.8681549595853699E-3,-1.1269536117357983E-8,1.5034064123875886E-5,4.8956600198582223E-3,0.58745346596263059,25.451371560043384,4.3116055424107181E-8,-2.0188119596570959E-7,1.615049567727258E-5,1.9063352933335137E-2,24.104614798307871,1.1994589834308496E-8,-6.4043082370666259E-7,-3.1289947882372655E-6,1.5824405851657133E-3,-2.969455075443328E-3]
[null,"GTH AVCC = (c1*e^c2*v)",null,"AVTT = mx + b",null,"GTY"]
["Voltage Scaling",0.90615000000000001,2.4011360000000002,1.0000709999999999,-0.20008500000000001,9.5627000000000004E-2,2.347296,2.2246000000000001,-1.6696]
[]
[]
["Power Scaling Factors","Scaling factors for architecture evaluations",null,null,null,"Olympus"]
["Column (1=Fuji,5=Olympus)",{"$f":"IF(ISOLY,5,1)","v":5}]
["Clock Power Factor",1,null,null,null,1]
["Logic Power Factor",1,null,null,null,1]
["BRAM Power Factor",1,null,null,null,1]
["DSP Power Factor",1,null,null,null,1]
["GTH Power Factor",1,null,null,null,1,1]
["PCIe Power Factor",1,null,null,null,1]
["IOI Power Factor",1,null,null,null,1]
["IOB Power Factor (Aux)",1,null,null,null,1]
["Iccintq Power Factor",1,null,null,null,1]
["Iccauxq Power Factor",1,null,null,null,1]
[]
["Power Optimization Factors","Clock","Logic","BRAM TDP","BRAM SDP","DSP"]
["Default",1,1,0.97499999999999998,0.97499999999999998,1]
["Power Optimization",0.98,0.98,0.93,0.93,1]
["Off",1,1,1,1,1]
[]
[]
[{"$f":"MATCH(RIGHT(PART,LEN(PART)-2)&\":\"&PACKAGE,FUJI_PARTLIST,FALSE)","v":60},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AVCC MMF"]
["PACKAGES","JA","JB","JC","JA (250)","JA (500)","JA (750)","Total I/Os","3.3 Pins","GTs","GTHs","GT Power","GTH Power","GTZs","GTY","Comm","Indust","-2LE",null,"GTY Power",null,"Bonded GTH","Bonded GTY"]
["KU025:FFVA1156",9.5,2.5,0.21,5.9,5,4.5999999999999996,312,104,0,12,0,1,null,null,1,1,1,null,null,null,20,0]
["KU035:SFVA784",13.1,2,0.21,9.4,7.9,7.3,468,104,0,8,0,1,null,null,1,1,1,null,null,null,8,0]
["KU035:FBVA676",11.7,2.4,0.03,7.9,6.6,6.2,312,104,0,16,0,1,null,null,1,1,1,null,null,null,16,0]
["KU035:FBVA900",10.5,2.5,0.03,6.8,5.7,5.3,468,104,0,16,0,1,null,null,1,1,1,null,null,null,16,0]
["KU035:FFVA1156",9.5,2.5,0.21,5.9,5,4.5999999999999996,520,104,0,16,0,1,null,null,1,1,1,null,null,null,20,0]
["KU040:SFVA784",13.1,2,0.21,9.4,7.9,7.3,468,104,0,8,0,1,null,null,1,1,1,null,null,null,8,0]
["KU040:FBVA676",11.7,2.4,0.03,7.9,6.6,6.2,312,104,0,16,0,1,null,null,1,1,1,null,null,null,16,0]
["KU040:FBVA900",10.5,2.5,0.03,6.8,5.7,5.3,468,104,0,16,0,1,null,null,1,1,1,null,null,null,16,0]
["KU040:FFVA1156",9.5,2.5,0.21,5.9,5,4.5999999999999996,520,104,0,20,0,1,null,null,1,1,1,null,null,null,20,0]
["KU060:FFVA1156",8.9,1.9,0.15,5.7,4.7,4.5,520,104,0,28,0,2,null,null,1,1,1,null,null,null,28,0]
["KU060:FFVA1517",7.9,1.9,0.15,4.8,4.0999999999999996,3.8,624,104,0,32,0,2,null,null,1,1,1,null,null,null,32,0]
["KU085:FLVA1517",7.8,1.7,0.1,4.8,4,3.8,624,104,0,48,0,3,null,null,1,1,1,null,null,null,48,0]
["KU085:FLVB1760",7.4,1.7,0.1,4.4000000000000004,3.7,3.5,676,104,0,44,0,3,null,null,1,1,1,null,null,null,52,0]
["KU085:FLVF1924",7,1.7,0.1,4.2,3.5,3.3,624,104,0,56,0,4,null,null,1,1,1,null,null,null,64,0]
["KU095:FFVC1517",7.8,1.7,0.1,4.8,4,3.8,520,52,0,20,0,1,null,20,1,1,1,null,1,null,20,20]
["KU095:FFVB1760",7.4,1.7,0.1,4.5,3.7,3.5,702,52,0,32,0,2,null,16,1,1,1,null,1,null,32,16]
["KU095:FFVB2104",6.7,1.7,0.1,3.9,3.3,3.1,702,52,0,32,0,2,null,32,1,1,1,null,2,null,32,32]
["KU095:FFVA1156",8.9,1.9,0.15,5.7,4.7,4.5,520,52,0,20,0,1,null,8,1,1,1,null,1,null,20,8]
["KU100:FLVD1924",7.1,1.7,0.12,4.2,3.6,3.2,832,156,0,52,0,4,null,null,1,1,1,null,null,null,52,0]
["KU100:FLVF1924",7.1,1.7,0.12,4.2,3.6,3.2,728,104,0,64,0,4,null,null,1,1,1,null,null,null,64,0]
["KU115:FLVA1517",7.8,1.7,0.1,4.8,4,3.8,624,104,0,48,0,3,null,null,1,1,1,null,null,null,48,0]
["KU115:FLVB1517",8.1,2.1,0.18,5,4.3,3.9,364,104,0,64,0,4,null,null,1,1,1,null,null,null,64,0]
["KU115:FLVD1517",7.8,1.7,0.1,4.8,4,3.8,338,104,0,64,0,4,null,null,1,1,1,null,null,null,64,0]
["KU115:FLVB1760",7.4,1.7,0.1,4.4000000000000004,3.7,3.5,702,104,0,52,0,3,null,null,1,1,1,null,null,null,52,0]
["KU115:FLVD1924",7,1.7,0.1,4.2,3.5,3.3,832,156,0,52,0,4,null,null,1,1,1,null,null,null,52,0]
["KU115:FLVF1924",7,1.7,0.1,4.2,3.5,3.3,728,104,0,64,0,4,null,null,1,1,1,null,null,null,64,0]
["KU115:FLVA2104",6.7,1.7,0.1,3.9,3.3,3.1,832,156,0,52,0,4,null,null,1,1,1,null,null,null,52,0]
["KU115:FLVB2104",6.7,1.7,0.1,3.9,3.3,3.1,702,104,0,64,0,4,null,null,1,1,1,null,null,null,64,0]
["VU065:FFVC1517",7.8,1.7,0.18,4.8,4,3.8,520,52,0,20,0,1,null,20,1,1,1,null,1,null,20,20]
["VU080:FFVA1760",8.1,2.1,0.18,5,4.3,3.9,728,52,0,32,0,2,null,16,1,1,1,null,2,null,32,16]
["VU080:FFVB1517",8.1,2.1,0.18,5,4.3,3.9,364,52,0,32,0,2,null,32,1,1,1,null,2,null,32,32]
["VU080:FFVC1517",7.8,1.7,0.1,4.8,4,3.8,520,52,0,20,0,1,null,20,1,1,1,null,1,null,20,20]
["VU080:FFVD1517",7.8,1.7,0.1,4.8,4,3.8,338,52,0,32,0,2,null,32,1,1,1,null,2,null,32,32]
["VU080:FFVB1760",7.4,1.7,0.1,4.5,3.7,3.5,702,52,0,32,0,2,null,16,1,1,1,null,1,null,32,16]
["VU080:FFVA2104",6.7,1.7,0.1,3.9,3.3,3.1,832,52,0,28,0,2,null,24,1,1,1,null,2,null,28,24]
["VU080:FFVB2104",6.7,1.7,0.1,3.9,3.3,3.1,702,52,0,32,0,2,null,32,1,1,1,null,2,null,32,32]
["VU095-ES1:FFVA1760",8.1,2.1,0.18,5,4.3,3.9,728,52,0,32,0,2,null,16,1,1,1,null,2,null,32,16]
["VU095-ES1:FFVB1517",8.1,2.1,0.18,5,4.3,3.9,364,52,0,32,0,2,null,32,1,1,1,null,2,null,32,32]
["VU095-ES1:FFVD1924",7.1,1.7,0.12,4.2,3.6,3.2,832,52,0,28,0,2,null,24,1,1,1,null,2,null,28,24]
["VU095-ES1:FFVE1924",7.1,1.7,0.12,4.2,3.6,3.2,676,52,0,32,0,2,null,32,1,1,1,null,2,null,32,32]
["VU095-ES1:FFVJ1924",7.1,1.7,0.12,4.2,3.6,3.2,364,52,0,32,0,2,null,32,1,1,1,null,2,null,32,32]
["VU095:FFVC1517",7.8,1.7,0.1,4.8,4,3.8,520,52,0,20,0,1,null,20,1,1,1,null,1,null,20,20]
["VU095:FFVD1517",7.8,1.7,0.1,4.8,4,3.8,338,52,0,32,0,2,null,32,1,1,1,null,2,null,32,32]
["VU095:FFVB1760",7.4,1.7,0.1,4.5,3.7,3.5,702,52,0,32,0,2,null,16,1,1,1,null,1,null,32,16]
["VU095:FFVA2104",6.7,1.7,0.1,3.9,3.3,3.1,832,52,0,28,0,2,null,24,1,1,1,null,2,null,28,24]
["VU095:FFVB2104",6.7,1.7,0.1,3.9,3.3,3.1,702,52,0,32,0,2,null,32,1,1,1,null,2,null,32,32]
["VU095:FFVC2104",6.7,1.7,0.1,3.9,3.3,3.1,416,52,0,32,0,2,null,32,1,1,1,null,2,null,32,32]
["VU125:FLVB1517",8.1,2.1,0.18,5,4.3,3.9,338,52,0,40,0,2,null,32,1,1,1,null,2,null,40,32]
["VU125:FLVD1517",7.7,1.6,0.09,4.7,4,3.7,338,52,0,40,0,2,null,32,1,1,1,null,2,null,40,32]
["VU125:FLVB1760",7.4,1.7,0.09,4.4000000000000004,3.7,3.5,702,52,0,36,0,2,null,16,1,1,1,null,1,null,36,16]
["VU125:FLVD1924",7.1,1.7,0.12,4.2,3.6,3.2,832,52,0,28,0,2,null,24,1,1,1,null,2,null,28,24]
["VU125:FLVJ1924",7.1,1.7,0.12,4.2,3.6,3.2,572,52,0,40,0,2,null,40,1,1,1,null,2,null,40,40]
["VU125:FLVA2104",6.8,1.8,0.09,3.9,3.3,3.1,832,52,0,28,0,2,null,24,1,1,1,null,2,null,28,24]
["VU125:FLVB2104",6.8,1.8,0.09,3.9,3.3,3.1,702,52,0,40,0,2,null,36,1,1,1,null,2,null,40,36]
["VU125:FLVC2104",6.8,1.8,0.09,3.9,3.3,3.1,416,52,0,40,0,2,null,40,1,1,1,null,2,null,40,40]
["VU160:FLGB2104",6.5,1.5,0.06,3.8,3.2,3,702,52,0,40,0,2,null,36,1,1,1,null,2,null,40,36]
["VU160:FLGC2104",6.5,1.5,0.06,3.8,3.2,3,416,52,0,52,0,3,null,52,1,1,1,null,3,null,52,52]
["VU190:FLGB2104",6.5,1.5,0.06,3.8,3.2,3,702,52,0,40,0,2,null,36,1,1,1,null,2,null,40,36]
["VU190:FLGC2104",6.5,1.5,0.06,3.8,3.2,3,416,52,0,52,0,3,null,52,1,1,1,null,3,null,52,52]
["VU190:FLGA2577",5.9,1.4,0.06,3.4,2.8,2.7,448,0,0,60,0,3,null,60,1,1,1,null,3,null,60,60]
["VU440:FLGB2377",6.2,1.4,0.05,3.6,3,2.8,1300,52,0,36,0,3,null,0,1,1,1,null,0,null,36,0]
["VU440:FLGA2892",5.7,1.5,0.04,3.2,2.7,2.5,1456,52,0,48,0,3,null,0,1,1,1,null,0,null,48,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,50,51,52,53,54,55,56,57,58,59,60,61,62,63,64,65,66,67,68,69,70,71,72,73,74,75,76,77,78,79,80,81,82,83,84,85,86,87,88,89,90,91,92,93,94,95,96,97,98,99,100,101,102,103,104,105,106,107,108,109,110,111,112]
[null,"TYP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAX (TT+FF)/2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAX (FF2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAX (FF1.5)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TYP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAX (TT+FF)/2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAX (FF2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAX (FF1.5)"]
[null,"Vccint",null,null,null,null,"Vccaux",null,null,null,null,"Vccbram",null,null,null,null,"Vccint",null,null,null,null,"Vccaux",null,null,null,null,"Vccbram",null,null,null,null,"Vccint",null,null,null,null,"Vccaux",null,null,null,null,"Vccbram",null,null,null,null,"Vccint",null,null,null,null,"Vccaux",null,null,null,null,"Vccbram",null,null,null,null,"Vcco",null,null,"Vccint MMF",null,null,"Vccaux MMF",null,null,"Vccbram MMF",null,null,"Vccint_io",null,null,null,null,"Vccaux_io",null,null,null,null,null,null,null,null,null,"Vccint_io",null,null,null,null,"Vccaux_io",null,null,null,null,null,null,null,null,null,"Vccint_io",null,null,null,null,"Vccaux_io",null,null,null,null,null,null,null,null,null,"Vccint_io",null,null,null,null,"Vccaux_io",null,null,null,null,null,null,null,null,null,"Vccint_io MMF",null,null,"Vccaux_io MMF",null,null,"Max Total Power Factors C/E",null,null,null,null,null,null,null,null,null,null,null,null,null,"Max Total Power Factors I"]
["Quiescent Data","x^4","x^3","x^2","X","c","x^4","x^3","x^2","X","c","x^4","x^3","x^2","X","c","x^4","x^3","x^2","X","c","x^4","x^3","x^2","X","c","x^4","x^3","x^2","X","c","x^4","x^3","x^2","X","c","x^4","x^3","x^2","X","c","x^4","x^3","x^2","X","c","x^4","x^3","x^2","X","c","x^4","x^3","x^2","X","c","x^4","x^3","x^2","X","c","25C","Max Com","Max Ind","(TT+FF)/2","FF2","FF1.5","(TT+FF)/2","FF2","FF1.5","(TT+FF)/2","FF2","FF1.5","x^4","x^3","x^2","X","c","x^4","x^3","x^2","X","c","x^4","x^3","x^2","X","c","x^4","x^3","x^2","X","c","x^4","x^3","x^2","X","c","x^4","x^3","x^2","X","c","x^4","x^3","x^2","X","c","x^4","x^3","x^2","X","c",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(TT+FF)/2","FF2","FF1.5","(TT+FF)/2","FF2","FF1.5","core","Iccio","bram","aux","auxio","io18","io33","mgthaux","mgthavcc","mgthavtt","mgtyaux","mgtyavcc","mgtyavtt","vccadc","core","Iccio","bram","aux","auxio","io18","io33","mgthaux","mgthavcc","mgthavtt","mgtyaux","mgtyavcc","mgtyavtt","vccadc"]
["KU025",6.5899272036754265E-6,4.1359231750767879E-4,2.3087567404711268E-2,1.8710180014129252,74.476772584978789,5.325856607899323E-7,3.0796499288025103E-6,1.5500306470576516E-3,0.15541183240422771,90.53205458904938,2.0480044721900343E-7,2.1899197025088924E-6,1.1325484890850241E-3,0.14700898908624055,5.8850703757927683,1.4281792955032954E-5,1.0273847762295996E-3,0.10742746580402027,6.6495068231783687,161.90011087672406,1.0648206183856056E-6,5.3619931114654647E-5,7.8394831100246087E-3,0.53603627740694137,119.39998174278014,3.7921377590602202E-7,1.7261797184194572E-5,2.4864639231143809E-3,0.21661122205569117,7.1631647773613807,1.4281792955032954E-5,1.0273847762295996E-3,0.10742746580402027,6.6495068231783687,161.90011087672406,1.0648206183856056E-6,5.3619931114654647E-5,7.8394831100246087E-3,0.53603627740694137,119.39998174278014,3.7921377590602202E-7,1.7261797184194572E-5,2.4864639231143809E-3,0.21661122205569117,7.1631647773613807,1.4281792955032954E-5,1.0273847762295996E-3,0.10742746580402027,6.6495068231783687,161.90011087672406,1.0648206183856056E-6,5.3619931114654647E-5,7.8394831100246087E-3,0.53603627740694137,119.39998174278014,3.7921377590602202E-7,1.7261797184194572E-5,2.4864639231143809E-3,0.21661122205569117,7.1631647773613807,4.0150304503314999E-2,2.0033799932031675,3.3026787868737126,0.8,0.6,0.6,0.9,0.63749999999999996,0.63749999999999996,0.8,0.6,0.6,3.1086423097900821E-7,3.0371133139514859E-5,3.571562346255277E-3,0.23544541675608618,6.402199302880752,2.8065607544161585E-8,-6.5161211445461745E-7,4.8361863220367999E-6,3.2782908484008904E-3,64.831728620534719,null,null,null,null,null,4.3321809036020173E-7,9.6737945992926401E-5,1.4657914537218935E-2,1.1367614372972745,36.046100717094831,7.6659501857478851E-8,2.5970110294105398E-7,1.1000776500116274E-4,1.1234569242054498E-2,155.65119899099193,null,null,null,null,null,4.3321809036020173E-7,9.6737945992926401E-5,1.4657914537218935E-2,1.1367614372972745,36.046100717094831,7.6659501857478851E-8,2.5970110294105398E-7,1.1000776500116274E-4,1.1234569242054498E-2,155.65119899099193,null,null,null,null,null,4.3321809036020173E-7,9.6737945992926401E-5,1.4657914537218935E-2,1.1367614372972745,36.046100717094831,7.6659501857478851E-8,2.5970110294105398E-7,1.1000776500116274E-4,1.1234569242054498E-2,155.65119899099193,null,null,null,null,null,0.8,0.6,0.6,1,1,1,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,null,null,null,1.2,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,null,null,null,1.2]
["KU035",6.5899272036754265E-6,4.1359231750767879E-4,2.3087567404711268E-2,1.8710180014129252,74.476772584978789,5.325856607899323E-7,3.0796499288025103E-6,1.5500306470576516E-3,0.15541183240422771,90.53205458904938,2.0480044721900343E-7,2.1899197025088924E-6,1.1325484890850241E-3,0.14700898908624055,5.8850703757927683,1.4281792955032954E-5,1.0273847762295996E-3,0.10742746580402027,6.6495068231783687,161.90011087672406,1.0648206183856056E-6,5.3619931114654647E-5,7.8394831100246087E-3,0.53603627740694137,119.39998174278014,3.7921377590602202E-7,1.7261797184194572E-5,2.4864639231143809E-3,0.21661122205569117,7.1631647773613807,1.4281792955032954E-5,1.0273847762295996E-3,0.10742746580402027,6.6495068231783687,161.90011087672406,1.0648206183856056E-6,5.3619931114654647E-5,7.8394831100246087E-3,0.53603627740694137,119.39998174278014,3.7921377590602202E-7,1.7261797184194572E-5,2.4864639231143809E-3,0.21661122205569117,7.1631647773613807,1.4281792955032954E-5,1.0273847762295996E-3,0.10742746580402027,6.6495068231783687,161.90011087672406,1.0648206183856056E-6,5.3619931114654647E-5,7.8394831100246087E-3,0.53603627740694137,119.39998174278014,3.7921377590602202E-7,1.7261797184194572E-5,2.4864639231143809E-3,0.21661122205569117,7.1631647773613807,4.0150304503314999E-2,2.0033799932031675,3.3026787868737126,0.8,0.6,0.6,0.9,0.63749999999999996,0.63749999999999996,0.8,0.6,0.6,3.1086423097900821E-7,3.0371133139514859E-5,3.571562346255277E-3,0.23544541675608618,6.402199302880752,2.8065607544161585E-8,-6.5161211445461745E-7,4.8361863220367999E-6,3.2782908484008904E-3,64.831728620534719,null,null,null,null,null,4.3321809036020173E-7,9.6737945992926401E-5,1.4657914537218935E-2,1.1367614372972745,36.046100717094831,7.6659501857478851E-8,2.5970110294105398E-7,1.1000776500116274E-4,1.1234569242054498E-2,155.65119899099193,null,null,null,null,null,4.3321809036020173E-7,9.6737945992926401E-5,1.4657914537218935E-2,1.1367614372972745,36.046100717094831,7.6659501857478851E-8,2.5970110294105398E-7,1.1000776500116274E-4,1.1234569242054498E-2,155.65119899099193,null,null,null,null,null,4.3321809036020173E-7,9.6737945992926401E-5,1.4657914537218935E-2,1.1367614372972745,36.046100717094831,7.6659501857478851E-8,2.5970110294105398E-7,1.1000776500116274E-4,1.1234569242054498E-2,155.65119899099193,null,null,null,null,null,0.8,0.6,0.6,1,1,1,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,null,null,null,1.2,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,null,null,null,1.2]
["KU040",6.5899272036754265E-6,4.1359231750767879E-4,2.3087567404711268E-2,1.8710180014129252,74.476772584978789,5.325856607899323E-7,3.0796499288025103E-6,1.5500306470576516E-3,0.15541183240422771,90.53205458904938,2.0480044721900343E-7,2.1899197025088924E-6,1.1325484890850241E-3,0.14700898908624055,5.8850703757927683,1.4281792955032954E-5,1.0273847762295996E-3,0.10742746580402027,6.6495068231783687,161.90011087672406,1.0648206183856056E-6,5.3619931114654647E-5,7.8394831100246087E-3,0.53603627740694137,119.39998174278014,3.7921377590602202E-7,1.7261797184194572E-5,2.4864639231143809E-3,0.21661122205569117,7.1631647773613807,1.4281792955032954E-5,1.0273847762295996E-3,0.10742746580402027,6.6495068231783687,161.90011087672406,1.0648206183856056E-6,5.3619931114654647E-5,7.8394831100246087E-3,0.53603627740694137,119.39998174278014,3.7921377590602202E-7,1.7261797184194572E-5,2.4864639231143809E-3,0.21661122205569117,7.1631647773613807,1.4281792955032954E-5,1.0273847762295996E-3,0.10742746580402027,6.6495068231783687,161.90011087672406,1.0648206183856056E-6,5.3619931114654647E-5,7.8394831100246087E-3,0.53603627740694137,119.39998174278014,3.7921377590602202E-7,1.7261797184194572E-5,2.4864639231143809E-3,0.21661122205569117,7.1631647773613807,4.0150304503314999E-2,2.0033799932031675,3.3026787868737126,0.8,0.6,0.6,0.9,0.63749999999999996,0.63749999999999996,0.8,0.6,0.6,3.1086423097900821E-7,3.0371133139514859E-5,3.571562346255277E-3,0.23544541675608618,6.402199302880752,2.8065607544161585E-8,-6.5161211445461745E-7,4.8361863220367999E-6,3.2782908484008904E-3,64.831728620534719,null,null,null,null,null,4.3321809036020173E-7,9.6737945992926401E-5,1.4657914537218935E-2,1.1367614372972745,36.046100717094831,7.6659501857478851E-8,2.5970110294105398E-7,1.1000776500116274E-4,1.1234569242054498E-2,155.65119899099193,null,null,null,null,null,4.3321809036020173E-7,9.6737945992926401E-5,1.4657914537218935E-2,1.1367614372972745,36.046100717094831,7.6659501857478851E-8,2.5970110294105398E-7,1.1000776500116274E-4,1.1234569242054498E-2,155.65119899099193,null,null,null,null,null,4.3321809036020173E-7,9.6737945992926401E-5,1.4657914537218935E-2,1.1367614372972745,36.046100717094831,7.6659501857478851E-8,2.5970110294105398E-7,1.1000776500116274E-4,1.1234569242054498E-2,155.65119899099193,null,null,null,null,null,0.8,0.6,0.6,1,1,1,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,null,null,null,1.2,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,null,null,null,1.2]
["KU060",1.1463060749819721E-5,2.9215577242147384E-4,3.980049944392814E-2,3.3704061175856239,95.182504774669908,7.6385369660268656E-7,4.4147823800373039E-6,2.2229963438100782E-3,0.22290189782731928,110.63856271454799,3.6864080499420551E-7,3.9418554645160876E-6,2.0385872803530387E-3,0.26461618035523327,10.593126676426984,2.0782936776487834E-5,1.4891920809600369E-3,0.15553770698539354,9.6188845967059748,232.3632276875569,1.527168650562397E-6,7.6891650193510597E-5,1.1242238838301121E-2,0.76873051574027318,149.90421440814944,6.825847966308398E-7,3.107123493155012E-5,4.4756350616058996E-3,0.38990019970024398,12.893696599250482,2.0782936776487834E-5,1.4891920809600369E-3,0.15553770698539354,9.6188845967059748,232.3632276875569,1.527168650562397E-6,7.6891650193510597E-5,1.1242238838301121E-2,0.76873051574027318,149.90421440814944,6.825847966308398E-7,3.107123493155012E-5,4.4756350616058996E-3,0.38990019970024398,12.893696599250482,2.0782936776487834E-5,1.4891920809600369E-3,0.15553770698539354,9.6188845967059748,232.3632276875569,1.527168650562397E-6,7.6891650193510597E-5,1.1242238838301121E-2,0.76873051574027318,149.90421440814944,6.825847966308398E-7,3.107123493155012E-5,4.4756350616058996E-3,0.38990019970024398,12.893696599250482,4.2588191248434999E-2,2.1500147795153599,3.5596822029308011,0.8,0.6,0.6,0.9,0.63749999999999996,0.63749999999999996,0.8,0.6,0.6,3.7402652374931992E-7,3.6708052011980587E-5,4.3182862003896226E-3,0.28462706773923102,7.7405820918453347,3.3377026312612693E-8,-7.97130586302531E-7,4.512360143801129E-6,3.8629312544758792E-3,81.036688990606891,null,null,null,null,null,5.2031661318055178E-7,1.1678080050784376E-4,1.7725922208609871E-2,1.376024666855608,43.660901751799145,9.1373897697532405E-8,2.20803066676525E-7,1.2502587682009821E-4,1.3165386355957848E-2,194.55059512025593,null,null,null,null,null,5.2031661318055178E-7,1.1678080050784376E-4,1.7725922208609871E-2,1.376024666855608,43.660901751799145,9.1373897697532405E-8,2.20803066676525E-7,1.2502587682009821E-4,1.3165386355957848E-2,194.55059512025593,null,null,null,null,null,5.2031661318055178E-7,1.1678080050784376E-4,1.7725922208609871E-2,1.376024666855608,43.660901751799145,9.1373897697532405E-8,2.20803066676525E-7,1.2502587682009821E-4,1.3165386355957848E-2,194.55059512025593,null,null,null,null,null,0.8,0.6,0.6,1,1,1,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,null,null,null,1.2,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,null,null,null,1.2]
["KU085",2.2926121499639512E-5,5.8431154484293857E-4,7.9600998887856045E-2,6.740812235171262,190.36500954934093,1.527707393205371E-6,8.8295647600753514E-6,4.4459926876201069E-3,0.44580379565463679,220.37712542909611,7.3728160998841101E-7,7.8837109290321751E-6,4.0771745607060773E-3,0.52923236071046653,21.186253352853967,4.156587355297594E-5,2.978384161920014E-3,0.31107541397078947,19.23776919341206,464.72645537511016,3.054337301124797E-6,1.5378330038702065E-4,2.2484477676602256E-2,1.5374610314805479,298.80842881629894,1.3651695932616796E-6,6.2142469863100239E-5,8.9512701232117992E-3,0.77980039940048795,25.787393198500965,4.156587355297594E-5,2.978384161920014E-3,0.31107541397078947,19.23776919341206,464.72645537511016,3.054337301124797E-6,1.5378330038702065E-4,2.2484477676602256E-2,1.5374610314805479,298.80842881629894,1.3651695932616796E-6,6.2142469863100239E-5,8.9512701232117992E-3,0.77980039940048795,25.787393198500965,4.156587355297594E-5,2.978384161920014E-3,0.31107541397078947,19.23776919341206,464.72645537511016,3.054337301124797E-6,1.5378330038702065E-4,2.2484477676602256E-2,1.5374610314805479,298.80842881629894,1.3651695932616796E-6,6.2142469863100239E-5,8.9512701232117992E-3,0.77980039940048795,25.787393198500965,8.5176382496869998E-2,4.3000295590307198,7.1193644058616012,0.624,0.58499999999999996,0.58499999999999996,0.70199999999999996,0.66299999999999992,0.66299999999999992,0.624,0.58499999999999996,0.58499999999999996,7.4805304749863985E-7,7.3416104023961174E-5,8.6365724007792452E-3,0.56925413547846204,15.481164183690669,6.6754052625221852E-8,-1.594261172604472E-6,9.0247202875949853E-6,7.7258625089503298E-3,162.07337798121378,null,null,null,null,null,1.0406332263610887E-6,2.3356160101569039E-4,3.5451844417219588E-2,2.752049333711216,87.321803503598304,1.8274779539506206E-7,4.4160613335336097E-7,2.5005175364021376E-4,2.6330772711914495E-2,389.1011902405117,null,null,null,null,null,1.0406332263610887E-6,2.3356160101569039E-4,3.5451844417219588E-2,2.752049333711216,87.321803503598304,1.8274779539506206E-7,4.4160613335336097E-7,2.5005175364021376E-4,2.6330772711914495E-2,389.1011902405117,null,null,null,null,null,1.0406332263610887E-6,2.3356160101569039E-4,3.5451844417219588E-2,2.752049333711216,87.321803503598304,1.8274779539506206E-7,4.4160613335336097E-7,2.5005175364021376E-4,2.6330772711914495E-2,389.1011902405117,null,null,null,null,null,0.624,0.58499999999999996,0.58499999999999996,1,1,1,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,null,null,null,1.2,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,null,null,null,1.2]
["KU095",1.6306866951953694E-5,4.36968482686214E-4,5.8780515047016341E-2,4.9108712219142721,139.23319213145115,1.101905988862775E-6,6.3752494256171232E-6,3.2069459719309165E-3,0.32152854240760764,160.96968796748584,5.8982528799072858E-7,6.3069687432257975E-6,3.2617396485648655E-3,0.42338588856837273,16.949002682283162,2.936928882464829E-5,2.1720747047510917E-3,0.23002872685366099,14.344334932992528,352.45156660499742,2.2030896739876043E-6,1.1095532943490867E-4,1.6219421971813905E-2,1.1089505165781424,217.76077883012951,1.0921356746093442E-6,4.971397589048011E-5,7.1610160985694409E-3,0.62384031952039021,20.629914558800763,2.936928882464829E-5,2.1720747047510917E-3,0.23002872685366099,14.344334932992528,352.45156660499742,2.2030896739876043E-6,1.1095532943490867E-4,1.6219421971813905E-2,1.1089505165781424,217.76077883012951,1.0921356746093442E-6,4.971397589048011E-5,7.1610160985694409E-3,0.62384031952039021,20.629914558800763,2.936928882464829E-5,2.1720747047510917E-3,0.23002872685366099,14.344334932992528,352.45156660499742,2.2030896739876043E-6,1.1095532943490867E-4,1.6219421971813905E-2,1.1089505165781424,217.76077883012951,1.0921356746093442E-6,4.971397589048011E-5,7.1610160985694409E-3,0.62384031952039021,20.629914558800763,3.4475803792135003E-2,1.8556678685590402,3.1409300715074409,0.8,0.6,0.6,0.9,0.63749999999999996,0.63749999999999996,0.8,0.6,0.6,5.0290701289947329E-7,5.0038503128647236E-5,5.8929159961001003E-3,0.38824316229533379,10.563366953620449,4.3322820808241471E-8,-1.1288898129187154E-6,6.0430701280474822E-7,4.8625559637142709E-3,121.54319784799451,null,null,null,null,null,6.9581785273244086E-7,1.586092988001951E-4,2.4203606813080272E-2,1.8843736351610572,59.90629232101864,1.194579035606257E-7,-8.7114536505479862E-8,1.3766532052441032E-4,1.6258667242125557E-2,291.77244161451364,null,null,null,null,null,6.9581785273244086E-7,1.586092988001951E-4,2.4203606813080272E-2,1.8843736351610572,59.90629232101864,1.194579035606257E-7,-8.7114536505479862E-8,1.3766532052441032E-4,1.6258667242125557E-2,291.77244161451364,null,null,null,null,null,6.9581785273244086E-7,1.586092988001951E-4,2.4203606813080272E-2,1.8843736351610572,59.90629232101864,1.194579035606257E-7,-8.7114536505479862E-8,1.3766532052441032E-4,1.6258667242125557E-2,291.77244161451364,null,null,null,null,null,0.8,0.6,0.6,1,1,1,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,1,1,1,1.2,1.1000000000000001,1.1000000000000001,1.25,1.2,1.2,1,1,1,1,1,1,1,1,1.2]
["KU115",2.2926121499639512E-5,5.8431154484293857E-4,7.9600998887856045E-2,6.740812235171262,190.36500954934093,1.527707393205371E-6,8.8295647600753514E-6,4.4459926876201069E-3,0.44580379565463679,220.37712542909611,7.3728160998841101E-7,7.8837109290321751E-6,4.0771745607060773E-3,0.52923236071046653,21.186253352853967,4.156587355297594E-5,2.978384161920014E-3,0.31107541397078947,19.23776919341206,464.72645537511016,3.054337301124797E-6,1.5378330038702065E-4,2.2484477676602256E-2,1.5374610314805479,298.80842881629894,1.3651695932616796E-6,6.2142469863100239E-5,8.9512701232117992E-3,0.77980039940048795,25.787393198500965,4.156587355297594E-5,2.978384161920014E-3,0.31107541397078947,19.23776919341206,464.72645537511016,3.054337301124797E-6,1.5378330038702065E-4,2.2484477676602256E-2,1.5374610314805479,298.80842881629894,1.3651695932616796E-6,6.2142469863100239E-5,8.9512701232117992E-3,0.77980039940048795,25.787393198500965,4.156587355297594E-5,2.978384161920014E-3,0.31107541397078947,19.23776919341206,464.72645537511016,3.054337301124797E-6,1.5378330038702065E-4,2.2484477676602256E-2,1.5374610314805479,298.80842881629894,1.3651695932616796E-6,6.2142469863100239E-5,8.9512701232117992E-3,0.77980039940048795,25.787393198500965,8.5176382496869998E-2,4.3000295590307198,7.1193644058616012,0.624,0.58499999999999996,0.58499999999999996,0.70199999999999996,0.66299999999999992,0.66299999999999992,0.624,0.58499999999999996,0.58499999999999996,7.4805304749863985E-7,7.3416104023961174E-5,8.6365724007792452E-3,0.56925413547846204,15.481164183690669,6.6754052625221852E-8,-1.594261172604472E-6,9.0247202875949853E-6,7.7258625089503298E-3,162.07337798121378,null,null,null,null,null,1.0406332263610887E-6,2.3356160101569039E-4,3.5451844417219588E-2,2.752049333711216,87.321803503598304,1.8274779539506206E-7,4.4160613335336097E-7,2.5005175364021376E-4,2.6330772711914495E-2,389.1011902405117,null,null,null,null,null,1.0406332263610887E-6,2.3356160101569039E-4,3.5451844417219588E-2,2.752049333711216,87.321803503598304,1.8274779539506206E-7,4.4160613335336097E-7,2.5005175364021376E-4,2.6330772711914495E-2,389.1011902405117,null,null,null,null,null,1.0406332263610887E-6,2.3356160101569039E-4,3.5451844417219588E-2,2.752049333711216,87.321803503598304,1.8274779539506206E-7,4.4160613335336097E-7,2.5005175364021376E-4,2.6330772711914495E-2,389.1011902405117,null,null,null,null,null,0.624,0.58499999999999996,0.58499999999999996,1,1,1,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,null,null,null,1.2,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,null,null,null,1.2]
["VU080",1.6306866951953694E-5,4.36968482686214E-4,5.8780515047016341E-2,4.9108712219142721,139.23319213145115,1.101905988862775E-6,6.3752494256171232E-6,3.2069459719309165E-3,0.32152854240760764,160.96968796748584,5.8982528799072858E-7,6.3069687432257975E-6,3.2617396485648655E-3,0.42338588856837273,16.949002682283162,2.936928882464829E-5,2.1720747047510917E-3,0.23002872685366099,14.344334932992528,352.45156660499742,2.2030896739876043E-6,1.1095532943490867E-4,1.6219421971813905E-2,1.1089505165781424,217.76077883012951,1.0921356746093442E-6,4.971397589048011E-5,7.1610160985694409E-3,0.62384031952039021,20.629914558800763,2.936928882464829E-5,2.1720747047510917E-3,0.23002872685366099,14.344334932992528,352.45156660499742,2.2030896739876043E-6,1.1095532943490867E-4,1.6219421971813905E-2,1.1089505165781424,217.76077883012951,1.0921356746093442E-6,4.971397589048011E-5,7.1610160985694409E-3,0.62384031952039021,20.629914558800763,2.936928882464829E-5,2.1720747047510917E-3,0.23002872685366099,14.344334932992528,352.45156660499742,2.2030896739876043E-6,1.1095532943490867E-4,1.6219421971813905E-2,1.1089505165781424,217.76077883012951,1.0921356746093442E-6,4.971397589048011E-5,7.1610160985694409E-3,0.62384031952039021,20.629914558800763,3.4475803792135003E-2,1.8556678685590402,3.1409300715074409,0.8,0.6,0.6,0.9,0.63749999999999996,0.63749999999999996,0.8,0.6,0.6,5.0290701289947329E-7,5.0038503128647236E-5,5.8929159961001003E-3,0.38824316229533379,10.563366953620449,4.3322820808241471E-8,-1.1288898129187154E-6,6.0430701280474822E-7,4.8625559637142709E-3,121.54319784799451,null,null,null,null,null,6.9581785273244086E-7,1.586092988001951E-4,2.4203606813080272E-2,1.8843736351610572,59.90629232101864,1.194579035606257E-7,-8.7114536505479862E-8,1.3766532052441032E-4,1.6258667242125557E-2,291.77244161451364,null,null,null,null,null,6.9581785273244086E-7,1.586092988001951E-4,2.4203606813080272E-2,1.8843736351610572,59.90629232101864,1.194579035606257E-7,-8.7114536505479862E-8,1.3766532052441032E-4,1.6258667242125557E-2,291.77244161451364,null,null,null,null,null,6.9581785273244086E-7,1.586092988001951E-4,2.4203606813080272E-2,1.8843736351610572,59.90629232101864,1.194579035606257E-7,-8.7114536505479862E-8,1.3766532052441032E-4,1.6258667242125557E-2,291.77244161451364,null,null,null,null,null,0.8,0.6,0.6,1,1,1,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,1,1,1,1.2,1.1000000000000001,1.1000000000000001,1.25,1.2,1.2,1,1,1,1,1,1,1,1,1.2]
["VU095-ES1",1.6306866951953694E-5,4.36968482686214E-4,5.8780515047016341E-2,4.9108712219142721,139.23319213145115,1.101905988862775E-6,6.3752494256171232E-6,3.2069459719309165E-3,0.32152854240760764,160.96968796748584,5.8982528799072858E-7,6.3069687432257975E-6,3.2617396485648655E-3,0.42338588856837273,16.949002682283162,2.936928882464829E-5,2.1720747047510917E-3,0.23002872685366099,14.344334932992528,352.45156660499742,2.2030896739876043E-6,1.1095532943490867E-4,1.6219421971813905E-2,1.1089505165781424,217.76077883012951,1.0921356746093442E-6,4.971397589048011E-5,7.1610160985694409E-3,0.62384031952039021,20.629914558800763,2.936928882464829E-5,2.1720747047510917E-3,0.23002872685366099,14.344334932992528,352.45156660499742,2.2030896739876043E-6,1.1095532943490867E-4,1.6219421971813905E-2,1.1089505165781424,217.76077883012951,1.0921356746093442E-6,4.971397589048011E-5,7.1610160985694409E-3,0.62384031952039021,20.629914558800763,2.936928882464829E-5,2.1720747047510917E-3,0.23002872685366099,14.344334932992528,352.45156660499742,2.2030896739876043E-6,1.1095532943490867E-4,1.6219421971813905E-2,1.1089505165781424,217.76077883012951,1.0921356746093442E-6,4.971397589048011E-5,7.1610160985694409E-3,0.62384031952039021,20.629914558800763,3.4475803792135003E-2,1.8556678685590402,3.1409300715074409,0.8,0.6,0.6,0.9,0.63749999999999996,0.63749999999999996,0.8,0.6,0.6,5.0290701289947329E-7,5.0038503128647236E-5,5.8929159961001003E-3,0.38824316229533379,10.563366953620449,4.3322820808241471E-8,-1.1288898129187154E-6,6.0430701280474822E-7,4.8625559637142709E-3,121.54319784799451,null,null,null,null,null,6.9581785273244086E-7,1.586092988001951E-4,2.4203606813080272E-2,1.8843736351610572,59.90629232101864,1.194579035606257E-7,-8.7114536505479862E-8,1.3766532052441032E-4,1.6258667242125557E-2,291.77244161451364,null,null,null,null,null,6.9581785273244086E-7,1.586092988001951E-4,2.4203606813080272E-2,1.8843736351610572,59.90629232101864,1.194579035606257E-7,-8.7114536505479862E-8,1.3766532052441032E-4,1.6258667242125557E-2,291.77244161451364,null,null,null,null,null,6.9581785273244086E-7,1.586092988001951E-4,2.4203606813080272E-2,1.8843736351610572,59.90629232101864,1.194579035606257E-7,-8.7114536505479862E-8,1.3766532052441032E-4,1.6258667242125557E-2,291.77244161451364,null,null,null,null,null,0.8,0.6,0.6,1,1,1,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,1,1,1,1.2,1.1000000000000001,1.1000000000000001,1.25,1.2,1.2,1,1,1,1,1,1,1,1,1.2]
["VU095",1.6306866951953694E-5,4.36968482686214E-4,5.8780515047016341E-2,4.9108712219142721,139.23319213145115,1.101905988862775E-6,6.3752494256171232E-6,3.2069459719309165E-3,0.32152854240760764,160.96968796748584,5.8982528799072858E-7,6.3069687432257975E-6,3.2617396485648655E-3,0.42338588856837273,16.949002682283162,2.936928882464829E-5,2.1720747047510917E-3,0.23002872685366099,14.344334932992528,352.45156660499742,2.2030896739876043E-6,1.1095532943490867E-4,1.6219421971813905E-2,1.1089505165781424,217.76077883012951,1.0921356746093442E-6,4.971397589048011E-5,7.1610160985694409E-3,0.62384031952039021,20.629914558800763,2.936928882464829E-5,2.1720747047510917E-3,0.23002872685366099,14.344334932992528,352.45156660499742,2.2030896739876043E-6,1.1095532943490867E-4,1.6219421971813905E-2,1.1089505165781424,217.76077883012951,1.0921356746093442E-6,4.971397589048011E-5,7.1610160985694409E-3,0.62384031952039021,20.629914558800763,2.936928882464829E-5,2.1720747047510917E-3,0.23002872685366099,14.344334932992528,352.45156660499742,2.2030896739876043E-6,1.1095532943490867E-4,1.6219421971813905E-2,1.1089505165781424,217.76077883012951,1.0921356746093442E-6,4.971397589048011E-5,7.1610160985694409E-3,0.62384031952039021,20.629914558800763,3.4475803792135003E-2,1.8556678685590402,3.1409300715074409,0.8,0.6,0.6,0.9,0.63749999999999996,0.63749999999999996,0.8,0.6,0.6,5.0290701289947329E-7,5.0038503128647236E-5,5.8929159961001003E-3,0.38824316229533379,10.563366953620449,4.3322820808241471E-8,-1.1288898129187154E-6,6.0430701280474822E-7,4.8625559637142709E-3,121.54319784799451,null,null,null,null,null,6.9581785273244086E-7,1.586092988001951E-4,2.4203606813080272E-2,1.8843736351610572,59.90629232101864,1.194579035606257E-7,-8.7114536505479862E-8,1.3766532052441032E-4,1.6258667242125557E-2,291.77244161451364,null,null,null,null,null,6.9581785273244086E-7,1.586092988001951E-4,2.4203606813080272E-2,1.8843736351610572,59.90629232101864,1.194579035606257E-7,-8.7114536505479862E-8,1.3766532052441032E-4,1.6258667242125557E-2,291.77244161451364,null,null,null,null,null,6.9581785273244086E-7,1.586092988001951E-4,2.4203606813080272E-2,1.8843736351610572,59.90629232101864,1.194579035606257E-7,-8.7114536505479862E-8,1.3766532052441032E-4,1.6258667242125557E-2,291.77244161451364,null,null,null,null,null,0.8,0.6,0.6,1,1,1,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,1,1,1,1.2,1.1000000000000001,1.1000000000000001,1.25,1.2,1.2,1,1,1,1,1,1,1,1,1.2]
["VU065",1.1247746814735684E-5,2.9545927699861922E-4,3.9968536611685743E-2,3.3588515919202706,95.214507904010958,7.5911308303996152E-7,4.389808278286816E-6,2.2091879911130701E-3,0.22150770868610153,110.00053003390452,4.3008093915990517E-7,4.5988313752690184E-6,2.3783518270785384E-3,0.3087188770811049,12.358647789164838,2.0302321783785466E-5,1.4824822643461741E-3,0.15616692578033162,9.7088365849844358,237.17050902455117,1.5176982761513019E-6,7.6426706184785429E-5,1.1172488617202641E-2,0.76390905088673022,149.02251424417994,7.9634892940264499E-7,3.6249774086808485E-5,5.2215742385402332E-3,0.45488356631695082,15.042646032458912,2.0302321783785466E-5,1.4824822643461741E-3,0.15616692578033162,9.7088365849844358,237.17050902455117,1.5176982761513019E-6,7.6426706184785429E-5,1.1172488617202641E-2,0.76390905088673022,149.02251424417994,7.9634892940264499E-7,3.6249774086808485E-5,5.2215742385402332E-3,0.45488356631695082,15.042646032458912,2.0302321783785466E-5,1.4824822643461741E-3,0.15616692578033162,9.7088365849844358,237.17050902455117,1.5176982761513019E-6,7.6426706184785429E-5,1.1172488617202641E-2,0.76390905088673022,149.02251424417994,7.9634892940264499E-7,3.6249774086808485E-5,5.2215742385402332E-3,0.45488356631695082,15.042646032458912,2.7162143556775001E-2,1.4157635096224641,2.3699198233361765,0.8,0.6,0.6,0.9,0.63749999999999996,0.63749999999999996,0.8,0.6,0.6,3.1342013458853863E-7,3.1027746511249592E-5,3.6527444336971063E-3,0.24069820934590022,6.5482185867266596,2.7388564502892607E-8,-6.923343973757008E-7,1.5757855475050699E-6,3.1086347454926098E-3,72.928316737778061,null,null,null,null,null,4.3452228427140246E-7,9.8480735255439844E-5,1.4999583798907644E-2,1.166583946486059,37.061889216905712,7.531471604047564E-8,2.9579572286059768E-8,9.2610985067669615E-5,1.0466215900419774E-2,175.07425322672151,null,null,null,null,null,4.3452228427140246E-7,9.8480735255439844E-5,1.4999583798907644E-2,1.166583946486059,37.061889216905712,7.531471604047564E-8,2.9579572286059768E-8,9.2610985067669615E-5,1.0466215900419774E-2,175.07425322672151,null,null,null,null,null,4.3452228427140246E-7,9.8480735255439844E-5,1.4999583798907644E-2,1.166583946486059,37.061889216905712,7.531471604047564E-8,2.9579572286059768E-8,9.2610985067669615E-5,1.0466215900419774E-2,175.07425322672151,null,null,null,null,null,0.8,0.6,0.6,1,1,1,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,1,1,1,1.2,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,1,1,1,1.2]
["VU125",2.2495493629471368E-5,5.9091855399723845E-4,7.9937073223371485E-2,6.7177031838405412,190.42901580802192,1.518226166079923E-6,8.779616556573632E-6,4.4183759822261403E-3,0.44301541737220307,219.10106006780904,8.6016187831981034E-7,9.1976627505380368E-6,4.7567036541570767E-3,0.61743775416220981,24.717295578329676,4.0604643567570932E-5,2.9649645286923482E-3,0.31233385156066323,19.417673169968872,474.34101804910233,3.0353965523026063E-6,1.5285341236957018E-4,2.234497723440532E-2,1.5278181017734593,297.04502848835978,1.59269785880529E-6,7.2499548173616971E-5,1.0443148477080466E-2,0.90976713263390163,30.085292064917823,4.0604643567570932E-5,2.9649645286923482E-3,0.31233385156066323,19.417673169968872,474.34101804910233,3.0353965523026063E-6,1.5285341236957018E-4,2.234497723440532E-2,1.5278181017734593,297.04502848835978,1.59269785880529E-6,7.2499548173616971E-5,1.0443148477080466E-2,0.90976713263390163,30.085292064917823,4.0604643567570932E-5,2.9649645286923482E-3,0.31233385156066323,19.417673169968872,474.34101804910233,3.0353965523026063E-6,1.5285341236957018E-4,2.234497723440532E-2,1.5278181017734593,297.04502848835978,1.59269785880529E-6,7.2499548173616971E-5,1.0443148477080466E-2,0.90976713263390163,30.085292064917823,5.4324287113550002E-2,2.8315270192449282,4.7398396466723529,0.624,0.58499999999999996,0.58499999999999996,0.70199999999999996,0.66299999999999992,0.66299999999999992,0.624,0.58499999999999996,0.58499999999999996,6.2684026917707726E-7,6.2055493022499184E-5,7.3054888673942126E-3,0.48139641869180044,13.096437173453319,5.4777129005785215E-8,-1.3846687947514016E-6,3.1515710950101397E-6,6.2172694909852196E-3,145.85663347555612,null,null,null,null,null,8.6904456854280492E-7,1.9696147051087969E-4,2.9999167597815287E-2,2.333167892972118,74.123778433811424,1.5062943208095128E-7,5.9159144572119537E-8,1.8522197013533923E-4,2.0932431800839549E-2,350.14850645344302,null,null,null,null,null,8.6904456854280492E-7,1.9696147051087969E-4,2.9999167597815287E-2,2.333167892972118,74.123778433811424,1.5062943208095128E-7,5.9159144572119537E-8,1.8522197013533923E-4,2.0932431800839549E-2,350.14850645344302,null,null,null,null,null,8.6904456854280492E-7,1.9696147051087969E-4,2.9999167597815287E-2,2.333167892972118,74.123778433811424,1.5062943208095128E-7,5.9159144572119537E-8,1.8522197013533923E-4,2.0932431800839549E-2,350.14850645344302,null,null,null,null,null,0.624,0.58499999999999996,0.58499999999999996,1,1,1,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,1,1,1,1.2,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,1,1,1,1.2]
["VU160",3.3743240444207193E-5,8.8637783099584423E-4,0.11990560983505652,10.076554775760851,285.64352371203353,2.2773392491199095E-6,1.3169424834856415E-5,6.6275639733392637E-3,0.66452312605831276,328.20159010171352,1.2902428174797283E-6,1.3796494125804877E-5,7.1350554812356862E-3,0.92615663124331837,37.075943367494304,6.0906965351356418E-5,4.4474467930385583E-3,0.46850077734099077,29.126509754953268,711.51152707365782,4.5530948284538834E-6,2.2928011855436012E-4,3.3517465851607919E-2,2.2917271526601803,445.06754273253938,2.3890467882079455E-6,1.087493222604243E-4,1.566472271562068E-2,1.3646506989508564,45.127938097376557,6.0906965351356418E-5,4.4474467930385583E-3,0.46850077734099077,29.126509754953268,711.51152707365782,4.5530948284538834E-6,2.2928011855436012E-4,3.3517465851607919E-2,2.2917271526601803,445.06754273253938,2.3890467882079455E-6,1.087493222604243E-4,1.566472271562068E-2,1.3646506989508564,45.127938097376557,6.0906965351356418E-5,4.4474467930385583E-3,0.46850077734099077,29.126509754953268,711.51152707365782,4.5530948284538834E-6,2.2928011855436012E-4,3.3517465851607919E-2,2.2917271526601803,445.06754273253938,2.3890467882079455E-6,1.087493222604243E-4,1.566472271562068E-2,1.3646506989508564,45.127938097376557,8.1486430670325002E-2,4.2472905288673921,7.1097594700085285,0.58400000000000007,0.54700000000000004,0.54700000000000004,0.65700000000000003,0.62049999999999994,0.62049999999999994,0.58400000000000007,0.54700000000000004,0.54700000000000004,9.4026040376562139E-7,9.3083239533747874E-5,1.0958233301091337E-2,0.72209462803770252,19.644655760179944,8.2165693508678828E-8,-2.0770031921271607E-6,4.727356642507581E-6,9.3259042364777864E-3,218.78495021333421,null,null,null,null,null,1.3035668528142084E-6,2.9544220576631976E-4,4.4998751396722894E-2,3.4997518394581757,111.18566765071714,2.2594414812142999E-7,8.8738716858162127E-8,2.7783295520296435E-4,3.1398647701259587E-2,525.22275968016459,null,null,null,null,null,1.3035668528142084E-6,2.9544220576631976E-4,4.4998751396722894E-2,3.4997518394581757,111.18566765071714,2.2594414812142999E-7,8.8738716858162127E-8,2.7783295520296435E-4,3.1398647701259587E-2,525.22275968016459,null,null,null,null,null,1.3035668528142084E-6,2.9544220576631976E-4,4.4998751396722894E-2,3.4997518394581757,111.18566765071714,2.2594414812142999E-7,8.8738716858162127E-8,2.7783295520296435E-4,3.1398647701259587E-2,525.22275968016459,null,null,null,null,null,0.58400000000000007,0.54700000000000004,0.54700000000000004,1,1,1,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,1,1,1,1.2,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,1,1,1,1.2]
["VU190",3.3743240444207193E-5,8.8637783099584423E-4,0.11990560983505652,10.076554775760851,285.64352371203353,2.2773392491199095E-6,1.3169424834856415E-5,6.6275639733392637E-3,0.66452312605831276,328.20159010171352,1.2902428174797283E-6,1.3796494125804877E-5,7.1350554812356862E-3,0.92615663124331837,37.075943367494304,6.0906965351356418E-5,4.4474467930385583E-3,0.46850077734099077,29.126509754953268,711.51152707365782,4.5530948284538834E-6,2.2928011855436012E-4,3.3517465851607919E-2,2.2917271526601803,445.06754273253938,2.3890467882079455E-6,1.087493222604243E-4,1.566472271562068E-2,1.3646506989508564,45.127938097376557,6.0906965351356418E-5,4.4474467930385583E-3,0.46850077734099077,29.126509754953268,711.51152707365782,4.5530948284538834E-6,2.2928011855436012E-4,3.3517465851607919E-2,2.2917271526601803,445.06754273253938,2.3890467882079455E-6,1.087493222604243E-4,1.566472271562068E-2,1.3646506989508564,45.127938097376557,6.0906965351356418E-5,4.4474467930385583E-3,0.46850077734099077,29.126509754953268,711.51152707365782,4.5530948284538834E-6,2.2928011855436012E-4,3.3517465851607919E-2,2.2917271526601803,445.06754273253938,2.3890467882079455E-6,1.087493222604243E-4,1.566472271562068E-2,1.3646506989508564,45.127938097376557,8.1486430670325002E-2,4.2472905288673921,7.1097594700085285,0.58400000000000007,0.54700000000000004,0.54700000000000004,0.65700000000000003,0.62049999999999994,0.62049999999999994,0.58400000000000007,0.54700000000000004,0.54700000000000004,9.4026040376562139E-7,9.3083239533747874E-5,1.0958233301091337E-2,0.72209462803770252,19.644655760179944,8.2165693508678828E-8,-2.0770031921271607E-6,4.727356642507581E-6,9.3259042364777864E-3,218.78495021333421,null,null,null,null,null,1.3035668528142084E-6,2.9544220576631976E-4,4.4998751396722894E-2,3.4997518394581757,111.18566765071714,2.2594414812142999E-7,8.8738716858162127E-8,2.7783295520296435E-4,3.1398647701259587E-2,525.22275968016459,null,null,null,null,null,1.3035668528142084E-6,2.9544220576631976E-4,4.4998751396722894E-2,3.4997518394581757,111.18566765071714,2.2594414812142999E-7,8.8738716858162127E-8,2.7783295520296435E-4,3.1398647701259587E-2,525.22275968016459,null,null,null,null,null,1.3035668528142084E-6,2.9544220576631976E-4,4.4998751396722894E-2,3.4997518394581757,111.18566765071714,2.2594414812142999E-7,8.8738716858162127E-8,2.7783295520296435E-4,3.1398647701259587E-2,525.22275968016459,null,null,null,null,null,0.58400000000000007,0.54700000000000004,0.54700000000000004,1,1,1,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,1,1,1,1.2,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,1,1,1,1.2]
["VU440",5.9552391617082806E-5,1.4070029350840378E-3,0.19313966292041757,16.752752422307701,475.59500282726731,4.6862007541915846E-6,2.7137454149634157E-5,1.3640081681116389E-2,1.3674077285815538,533.2050484686481,8.6016187831981034E-7,9.1976627505380368E-6,4.7567036541570767E-3,0.61743775416220981,24.717295578329676,1.0838033465807769E-4,7.380246096801552E-3,0.74517916090865288,45.272366315246501,1063.7057639830809,9.3694918492907824E-6,4.7199391160226159E-4,6.8991657591272071E-2,4.7168312114506934,757.94133940647509,1.59269785880529E-6,7.2499548173616971E-5,1.0443148477080466E-2,0.90976713263390163,30.085292064917823,1.0838033465807769E-4,7.380246096801552E-3,0.74517916090865288,45.272366315246501,1063.7057639830809,9.3694918492907824E-6,4.7199391160226159E-4,6.8991657591272071E-2,4.7168312114506934,757.94133940647509,1.59269785880529E-6,7.2499548173616971E-5,1.0443148477080466E-2,0.90976713263390163,30.085292064917823,1.0838033465807769E-4,7.380246096801552E-3,0.74517916090865288,45.272366315246501,1063.7057639830809,9.3694918492907824E-6,4.7199391160226159E-4,6.8991657591272071E-2,4.7168312114506934,757.94133940647509,1.59269785880529E-6,7.2499548173616971E-5,1.0443148477080466E-2,0.90976713263390163,30.085292064917823,8.1486430670325016E-2,4.2472905288673921,7.1097594700085285,0.58400000000000007,0.54700000000000004,0.54700000000000004,0.65700000000000003,0.62049999999999994,0.62049999999999994,0.58400000000000007,0.54700000000000004,0.54700000000000004,9.4026040376562139E-7,9.3083239533747874E-5,1.0958233301091337E-2,0.72209462803770252,19.644655760179944,8.2165693508680059E-8,-2.0770031921275101E-6,4.7273566425283164E-6,9.3259042364785254E-3,218.78495021333416,null,null,null,null,null,1.3035668528142341E-6,2.9544220576631532E-4,4.4998751396722998E-2,3.4997518394581841,111.18566765071699,2.2594414812143555E-7,8.8738716857019492E-8,2.7783295520301867E-4,3.1398647701260655E-2,525.22275968016447,null,null,null,null,null,1.3035668528142341E-6,2.9544220576631532E-4,4.4998751396722998E-2,3.4997518394581841,111.18566765071699,2.2594414812143555E-7,8.8738716857019492E-8,2.7783295520301867E-4,3.1398647701260655E-2,525.22275968016447,null,null,null,null,null,1.3035668528142341E-6,2.9544220576631532E-4,4.4998751396722998E-2,3.4997518394581841,111.18566765071699,2.2594414812143555E-7,8.8738716857019492E-8,2.7783295520301867E-4,3.1398647701260655E-2,525.22275968016447,null,null,null,null,null,0.58400000000000007,0.54700000000000004,0.54700000000000004,1,1,1,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,null,null,null,1.2,1.1000000000000001,1.1000000000000001,1.2,1.2,1.2,1,1,1,1,1,null,null,null,1.2]
[null,5.9552391617082806E-5,1.4070029350840378E-3,0.19313966292041757,16.752752422307701,475.59500282726731,4.6862007541915846E-6,2.7137454149634157E-5,1.3640081681116389E-2,1.3674077285815538,533.2050484686481,8.6016187831981034E-7,9.1976627505380368E-6,4.7567036541570767E-3,0.61743775416220981,24.717295578329676,1.0838033465807769E-4,7.380246096801552E-3,0.74517916090865288,45.272366315246501,1063.7057639830809,9.3694918492907824E-6,4.7199391160226159E-4,6.8991657591272071E-2,4.7168312114506934,757.94133940647509,1.59269785880529E-6,7.2499548173616971E-5,1.0443148477080466E-2,0.90976713263390163,30.085292064917823,1.0838033465807769E-4,7.380246096801552E-3,0.74517916090865288,45.272366315246501,1063.7057639830809,9.3694918492907824E-6,4.7199391160226159E-4,6.8991657591272071E-2,4.7168312114506934,757.94133940647509,1.59269785880529E-6,7.2499548173616971E-5,1.0443148477080466E-2,0.90976713263390163,30.085292064917823,1.0838033465807769E-4,7.380246096801552E-3,0.74517916090865288,45.272366315246501,1063.7057639830809,9.3694918492907824E-6,4.7199391160226159E-4,6.8991657591272071E-2,4.7168312114506934,757.94133940647509,1.59269785880529E-6,7.2499548173616971E-5,1.0443148477080466E-2,0.90976713263390163,30.085292064917823,8.1486430670325016E-2,4.2472905288673921,7.1097594700085285,0.58400000000000007,0.54700000000000004,0.54700000000000004,0.65700000000000003,0.62049999999999994,0.62049999999999994,0.58400000000000007,0.54700000000000004,0.54700000000000004,9.4026040376562139E-7,9.3083239533747874E-5,1.0958233301091337E-2,0.72209462803770252,19.644655760179944,8.2165693508680059E-8,-2.0770031921275101E-6,4.7273566425283164E-6,9.3259042364785254E-3,218.78495021333416,null,null,null,null,null,1.3035668528142341E-6,2.9544220576631532E-4,4.4998751396722998E-2,3.4997518394581841,111.18566765071699,2.2594414812143555E-7,8.8738716857019492E-8,2.7783295520301867E-4,3.1398647701260655E-2,525.22275968016447,null,null,null,null,null,1.3035668528142341E-6,2.9544220576631532E-4,4.4998751396722998E-2,3.4997518394581841,111.18566765071699,2.2594414812143555E-7,8.8738716857019492E-8,2.7783295520301867E-4,3.1398647701260655E-2,525.22275968016447,null,null,null,null,null,1.3035668528142341E-6,2.9544220576631532E-4,4.4998751396722998E-2,3.4997518394581841,111.18566765071699,2.2594414812143555E-7,8.8738716857019492E-8,2.7783295520301867E-4,3.1398647701260655E-2,525.22275968016447,null,null,null,null,null,0.58400000000000007,0.54700000000000004,0.54700000000000004,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.65700000000000003]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Vcc Voltage Scaling","vcc","vccio"]
["c1",0.16438900000000001,0.10756300000000001]
["c2",1.900045,2.346295]
[null,null,null,null,null,"TYP",null,null,"MAX",null,null,"Pauxq",null,"Pllq",null,"PDDRoq",null,"Pccoq"]
["PSS","mA/MHz",null,null,null,"Pintq","Pint_c1","Pint_c2","process","Pint_c1","Pint_c2","TYP","MAX","TYP","MAX","TYP","MAX","TYP","MAX","Pint-MMF"]
["Clock (WFE)",{"$f":"0.303/2","v":0.1515},null,null,null,19.899999999999999,2.3306724258038045,29.545350682264591,{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",IF(INT(RIGHT(PART,3))>20,4.763,3.4),1)","v":1},1.9,33.549999999999997,10.33,20.66,3,6,2,5.55,1,2,1]
["A9",0.41499999999999998,null,null,null,19.899999999999999,2.3306724258038045,29.545350682264591,{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",IF(INT(RIGHT(PART,3))>20,2.75,1.927),1)","v":1},2.1822612551669605,32.036429789211681]
["DDR Switch",6.2778E-2,null,null,null,19.899999999999999,2.3306724258038045,29.545350682264591,{"$f":"IF(LEFT(FAMILY,4)=\"Zynq\",IF(INT(RIGHT(PART,3))>20,1.836,1.435),1)","v":1},2.1502422282397071,32.654959206810467]
["AXI",1.0416999999999999E-2]
["PLL (Vccpaux)",15,0.02,null,null,null,null,null,null,2.4122459607069375,29.545350682264591]
[null,"x^2","x","read"]
["DDR3",-65,125,160,-398,814,155]
[]
[]
[]
["XADC","mA (int)","mA/MHz","mA (Vccadc)","mA/MHz","Leakage"]
["Typical",0,2.06E-2,0,1.1999999999999999E-3,13.8]
["Max",0,2.06E-2,0,1.1999999999999999E-3,16.96]
["Leakage (Vccadc)"]
[]
["Config","mA (int)","mA/MHz","mA (Aux)","mA/MHz"]
["Center",0,0.125,0,0]
["Cframe",0,0,8,0]
["eFUSE (Vccaux mA)",115]
[]
["DSP48","mA/MHz"]
["DSP_mA_MHz",2.4489574736842101E-2]
["Pre-Adder",2.2704052631578979E-3]
["ACC only (no mult)",1.808268E-2]
["DSP No MREG",2.7573179999999996E-2]
["PCIE-GEN2"]
["x1 GEN1 - 31.25MHZ",25]
["x2 GEN1 - 62.5MHZ",28]
["x4 GEN1 - 125MHZ",35]
["x8 GEN1 - 250MHZ",45]
["x1 GEN2 - 62.5MHZ",42]
["x2 GEN2 - 125MHZ",48]
["x4 GEN2 - 250MHZ",58]
["x8 GEN2 - 500MHZ",82]
["PCIE-GEN3",100,"500MHz core"]
["x1 GEN1 - 62.5MHZ",109.21416600000001,109.21416600000001]
["x2 GEN1 - 62.5MHZ",118.08723249999998,118.08723249999998]
["x4 GEN1 - 125MHZ",123.04456049999999,123.04456049999999]
["x8 GEN1 - 250MHZ",136.41719749999999,136.41719749999999]
["x1 GEN2 - 62.5MHZ",129.91288949999998,129.91288949999998]
["x2 GEN2 - 125MHZ",140.73191699999998,140.73191699999998]
["x4 GEN2 - 250MHZ",151.6274195,151.6274195]
["x8 GEN2 - 500MHZ",174.147559,174.147559]
["x1 GEN3 - 125MHZ",150.86246999999997,237.61019999999999]
["x2 GEN3 - 125MHZ",146.35909000000001,235.49930000000001]
["x4 GEN3 - 250MHZ",172.88822000000002,265.67700000000002]
["x8 GEN3 - 500MHZ",314.06619999999998,314.06619999999998]
[]
["CMAC","High (mA)","Med (mA)","Low (mA)","x2","x1","x"]
["caui10",{"$f":"E334*0.5349^2+F334*0.5349+G334","v":302.76326419180003},{"$f":"E334*0.2959^2+F334*0.2959+G334","v":290.14751917580003},{"$f":"E334*0.0928^2+F334*0.0928+G334","v":261.03588293120004},-204.82,222.95,242.11]
["cau4",{"$f":"E335*0.5349^2+F335*0.5349+G335","v":305.6744946394},{"$f":"E335*0.2959^2+F335*0.2959+G335","v":292.08788191140002},{"$f":"E335*0.0928^2+F335*0.0928+G335","v":260.06447976959998},-228.06,246.32,239.17]
["ILMAC","High (mA)","Med (mA)","Low (mA)","x2","x1","x"]
["6x25",{"$f":"E337*0.7137^2+F337*0.7137+G337","v":526.91238400890006},{"$f":"E337*0.3938^2+F337*0.3938+G337","v":461.89844321639998},{"$f":"E337*0.1239^2+F337*0.1239+G337","v":362.92105610009997},-277.19,510.22,303.95999999999998]
["12x12",{"$f":"E338*0.7413^2+F338*0.7413+G338","v":432.7927279662},{"$f":"E338*0.409^2+F338*0.409+G338","v":377.47986637999998},{"$f":"E338*0.1284^2+F338*0.1284+G338","v":294.99748178880003},-208.02,405.74,246.33]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["PLL","I (mA)","mA/MHz","Comments","Supply"]
["Avdd regulator",8.1,null,"regulator static current","Aux"]
["Dvdd Regulator",7.45,null,"regulator static current","Aux"]
["charge Pump",7.58,null,"Charge Pump Static Current","Aux"]
["VCO Ring",null,7.9865016872890885E-3,"mA/MHz","Aux"]
["ouput counters",null,1.5625E-4,"mA/MHz","Aux"]
["Input counters",null,1.5625E-4,"mA/MHz","Aux"]
["Lock/PFD",null,1.475E-3,"mA/MHz","Aux"]
["Output Drivers",null,9.5E-4,"mA/MHz","VccInt"]
["Control Logic",5.1999999999999995E-4,null,"mA  ","VccInt"]
["Perf Path Center IO",{"$f":"B363/3","v":1.2999999999999999E-4},{"$f":"C363/3","v":1.5666666666666667E-3},"mA/MHz","Aux"]
["Perf Path Outter IO",3.8999999999999999E-4,4.7000000000000002E-3,"mA/MHz","Aux"]
["Interpolator",0]
["misc",2.355,null,"mA","Aux"]
["xiphy_mux",null,4.6874999999999998E-4,"mA/MHz","Aux"]
[]
["MMCM","I(mA)","mA/Mhz","Comments","Supply"]
["Avdd Regulator ",10.3,null,"regulator static current","Aux"]
["Dvdd Regulator",9.3000000000000007,null,"regulator static current","Aux"]
["Charge Pump",7.58,null,"Charge Pump Static Current","Aux"]
["VCO Ring",null,2.1575E-2,"mA/MHz","Aux"]
["Ouput counters (non-fract)",null,1.5625E-4,"mA/MHz","Aux"]
["Input counters",null,1.5625E-4,"mA/MHz","Aux"]
["Lock/PFD",null,1.475E-3,"mA/MHz","Aux"]
["Output Drivers",null,9.5E-4,"mA/MHz","VccInt"]
["Control Logic",5.1999999999999995E-4,null,"mA  ","VccInt"]
["Perf Path Center IO",{"$f":"B379/3","v":1.2999999999999999E-4},{"$f":"C379/3","v":1.5666666666666667E-3},"mA/MHz","Aux"]
["Perf Path Outter IO",3.8999999999999999E-4,4.7000000000000002E-3,"mA/MHz","Aux"]
["Interpolator",null,5.8312499999999996E-3,"mA/MHz","Aux"]
["misc",3.14,null,"mA","Aux"]
["ouput counters (fract)",null,4.3749999999999995E-4,"mA/MHz","Aux"]
["spread spectrum",null,4.3749999999999995E-4,"mA/MHz","Aux"]
["VCO output phases",null,1.3375000000000001E-3,"mA/MHz","Aux"]
[]
[null,"Vccint","Vccaux"]
["PHASER","mA/MHz","I(mA)","mA/MHz","Comments"]
["FIFO",0]
["PHASER_IN",1.8518518518518517E-3,null,0,"In/Out  Aux current is per pair of IN/OUT"]
["PHASER_OUT",0,null,0]
["PHY Control",0,null,null,"One per CMT"]
["PHASER_REF",0,0,0,"One per CMT"]
["PHASER_IN (bypass)",0,null,null,"PHASER_IN_EN attribute is set to false"]
[]
["BRAMCLK","vccint * BRAMS * (PortA_clock  * {1,0} + PortB_clock * {1,0}) * clock_mA "]
["BRAM","vccint * BRAMS * (PortA_clock * ((read_rate * bit_mA) + (write_rate * bit_mA)) + PortB_clock * ((read_rate * bit_mA) + (write_rate * bit_mA)))"]
[null,"RAMB18READ_FIRST",null,"RAMB18WRITE_FIRST",null,"RAMB18NO_CHANGE",null,"RAMB36READ_FIRST",null,"RAMB36WRITE_FIRST",null,"RAMB36NO_CHANGE",null,"RAMB18SDPREAD_FIRST",null,"RAMB18SDPWRITE_FIRST",null,"RAMB18SDPNO_CHANGE",null,"RAMB36SDPREAD_FIRST",null,"RAMB36SDPWRITE_FIRST",null,"RAMB36SDPNO_CHANGE",null,"RAMB36SDP_ECCREAD_FIRST",null,"RAMB36SDP_ECCWRITE_FIRST",null,"RAMB36SDP_ECCNO_CHANGE",null,"RAMB36SDP_ECC_ENCODE_ONLYREAD_FIRST",null,"RAMB36SDP_ECC_ENCODE_ONLYWRITE_FIRST",null,"RAMB36SDP_ECC_ENCODE_ONLYNO_CHANGE",null,"RAMB36SDP_ECC_DECODE_ONLYREAD_FIRST",null,"RAMB36SDP_ECC_DECODE_ONLYWRITE_FIRST",null,"RAMB36SDP_ECC_DECODE_ONLYNO_CHANGE",null,"FIFO18",null,"FIFO36",null,"FIFO18_36",null,"FIFO36_72",null,"FIFO36_ECC",null,"CASC (pair)READ_FIRST",null,"CASC (pair)WRITE_FIRST",null,"CASC (pair)NO_CHANGE",null,null,null,"ASYNC_FIFO18",null,"ASYNC_FIFO36",null,null,null,"Vccint Standby CLK",null,null,"uA/MHz"]
["Bit Width","Read","Write","Read","Write","Read","Write","Read","Write","Read","Write","Read","Write","Read","Write","Read","Write","Read","Write","Read","Write","Read","Write","Read","Write","Read","Write","Read","Write","Read","Write","Read","Write","Read","Write","Read","Write","Read","Write","Read","Write","Read","Write","PortA - R","PortB -W","PortA - R","PortB -W","PortA - R","PortB -W","PortA - R","PortB -W","PortA - R","PortB -W","Read","Write","Read","Write","Read","Write",null,null,"Read","Write","Read","Write",null,null,"mode","x","c"]
[0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,0,0,0,0,null,null,"TDP18",{"$f":"BS399*1.2","v":0.73914000000000002},0,0.61595]
[1,14.437235699999999,14.724600599999999,12.331906199999995,12.025534725,12.623500147499998,10.242702,28.874471399999997,29.449201199999997,24.663812399999991,24.05106945,25.247000294999996,20.485403999999999,13.883452799999997,13.43987667,11.941544174999997,11.31555105,11.662654589999999,9.9091840149999992,27.766905599999994,26.879753340000001,23.883088349999994,22.6311021,23.325309179999998,19.818368029999998,54.715910399999991,50.575016999999995,46.690000500000004,42.790338800000001,46.569583500000007,36.58671408,53.108447999999996,50.295032099999993,45.231466499999989,42.469226799999994,45.021074999999996,36.344015400000004,54.664742399999994,50.066904000000001,46.538464500000003,42.104457999999987,46.538464500000003,36.250682999999995,13.178310199999999,13.178310199999999,22.5833412,22.5833412,21.376930959999999,21.376930959999999,41.204876999999989,41.204876999999989,41.686864799999988,41.686864799999988,41.609054999999991,44.519849999999991,41.152768049999999,44.454249999999988,40.816996499999988,42.611094999999992,null,null,13.018385599999998,13.018385599999998,22.252028399999993,22.252028399999993,null,null,"TDP36",{"$f":"BS400*1.2","v":1.4317200000000001},0,1.1931]
[2,14.031598612499998,14.274002400000001,12.019327222499996,11.696971999999999,12.375035534999997,10.113294725000001,28.063197224999996,28.548004800000001,24.038654444999992,23.393943999999998,24.750071069999994,20.226589450000002,13.918758719999996,13.429100025,12.229902299999999,11.273365125,11.671056719999997,9.9274144600000014,27.837517439999992,26.858200050000001,24.459804599999998,22.54673025,23.342113439999995,19.854828920000003,54.715910399999991,50.575016999999995,46.690000500000004,42.790338800000001,46.569583500000007,36.58671408,53.108447999999996,50.295032099999993,45.231466499999989,42.469226799999994,45.021074999999996,36.344015400000004,54.664742399999994,50.066904000000001,46.538464500000003,42.104457999999987,46.538464500000003,36.250682999999995,13.178310199999999,13.178310199999999,22.5833412,22.5833412,21.376930959999999,21.376930959999999,41.204876999999989,41.204876999999989,41.686864799999988,41.686864799999988,41.609054999999991,44.519849999999991,41.152768049999999,44.454249999999988,40.816996499999988,42.611094999999992,null,null,13.018385599999998,13.018385599999998,22.252028399999993,22.252028399999993,null,null,"SDP18",0.73914000000000002,0,0.61595]
[4,13.869521819999999,14.473203975000001,11.848169339999998,11.819528174999999,12.083118712499999,10.0321342,27.739043639999998,28.946407950000001,23.696338679999997,23.639056349999997,24.166237424999998,20.0642684,14.5387968,13.4519319,11.947328250000002,11.1738578590125,11.747472929999997,9.8221620070000011,29.0775936,26.9038638,23.894656500000004,22.347715718025,23.494945859999994,19.644324014000002,54.715910399999991,50.575016999999995,46.690000500000004,42.790338800000001,46.569583500000007,36.58671408,53.108447999999996,50.295032099999993,45.231466499999989,42.469226799999994,45.021074999999996,36.344015400000004,54.664742399999994,50.066904000000001,46.538464500000003,42.104457999999987,46.538464500000003,36.250682999999995,13.178310199999999,13.178310199999999,22.5833412,22.5833412,21.376930959999999,21.376930959999999,41.204876999999989,41.204876999999989,41.686864799999988,41.686864799999988,41.609054999999991,44.519849999999991,41.152768049999999,44.454249999999988,40.816996499999988,42.611094999999992,null,null,13.018385599999998,13.018385599999998,22.252028399999993,22.252028399999993,null,null,"SDP36",1.43754,0,1.1979500000000001]
[9,13.52830752,13.987043399999999,11.556308789999999,11.516582249999999,11.7867456,9.6783232649999995,27.056615040000001,27.974086799999998,23.112617579999998,23.033164499999998,23.573491199999999,19.356646529999999,14.564380800000002,13.441885875000001,12.3319185,11.417644125000001,11.695466069999998,9.8882303500000006,29.128761600000004,26.883771750000001,24.663837000000001,22.835288250000001,23.390932139999997,19.776460700000001,54.715910399999991,50.575016999999995,46.690000500000004,42.790338800000001,46.569583500000007,36.58671408,53.108447999999996,50.295032099999993,45.231466499999989,42.469226799999994,45.021074999999996,36.344015400000004,54.664742399999994,50.066904000000001,46.538464500000003,42.104457999999987,46.538464500000003,36.250682999999995,13.123522719999999,13.123522719999999,22.738321200000001,22.738321200000001,21.376930959999999,21.376930959999999,41.204876999999989,41.204876999999989,41.686864799999988,41.686864799999988,41.609054999999991,44.519849999999991,41.152768049999999,44.454249999999988,40.816996499999988,42.611094999999992,null,null,13.586645599999997,13.586645599999997,22.34110746,22.34110746,null,null,"FIFO18",1.2804,0,1.0669999999999999]
[18,13.391255999999998,14.136117350000001,11.495309399999998,11.799132725,11.512255724999999,9.7668437000000008,26.782511999999997,28.272234700000002,22.990618799999996,23.59826545,23.024511449999999,19.533687400000002,14.5324992,13.583443499999998,12.402037725,11.487431249999998,12.1634946,9.8920882450000001,29.0649984,27.166886999999996,24.804075449999999,22.974862499999997,24.3269892,19.78417649,54.715910399999991,50.575016999999995,46.690000500000004,42.790338800000001,46.569583500000007,36.58671408,53.108447999999996,50.295032099999993,45.231466499999989,42.469226799999994,45.021074999999996,36.344015400000004,54.664742399999994,50.066904000000001,46.538464500000003,42.104457999999987,46.538464500000003,36.250682999999995,14.214798399999999,14.214798399999999,22.264237379999994,22.264237379999994,21.376930959999999,21.376930959999999,41.204876999999989,41.204876999999989,41.686864799999988,41.686864799999988,41.609054999999991,44.519849999999991,41.152768049999999,44.454249999999988,40.816996499999988,42.611094999999992,null,null,13.456757599999996,13.456757599999996,21.834873900000002,21.834873900000002,null,null,"FIFO36",1.8449399999999998,0,1.53745]
[36,13.391255999999998,14.136117350000001,11.495309399999998,11.799132725,11.512255724999999,9.7668437000000008,27.461988599999998,28.71,22.895379899999998,24.02,23.010929174999998,19.420238349999998,26.60736,24.3154395,22.710104999999995,20.483087499999996,22.237416,17.705132499999998,29.123959679999999,27.221683500000001,25.146316799999994,22.774474999999999,24.699605399999996,20.089631000000004,54.715910399999991,50.575016999999995,46.690000500000004,42.790338800000001,46.569583500000007,36.58671408,53.108447999999996,50.295032099999993,45.231466499999989,42.469226799999994,45.021074999999996,36.344015400000004,54.664742399999994,50.066904000000001,46.538464500000003,42.104457999999987,46.538464500000003,36.250682999999995,21.376930959999999,21.376930959999999,23.993314799999997,23.993314799999997,21.376930959999999,21.376930959999999,41.204876999999989,41.204876999999989,41.686864799999988,41.686864799999988,41.609054999999991,44.519849999999991,41.152768049999999,44.454249999999988,40.816996499999988,42.611094999999992,null,null,23.244720399999999,23.244720399999999,21.981433319999997,21.981433319999997]
[72,13.391255999999998,14.136117350000001,11.495309399999998,11.799132725,11.512255724999999,9.7668437000000008,27.461988599999998,28.71,22.895379899999998,24.02,23.010929174999998,19.420238349999998,26.60736,24.3154395,22.710104999999995,20.483087499999996,22.237416,17.705132499999998,53.21472,48.630879,45.42020999999999,40.966174999999993,44.474831999999999,35.410264999999995,54.715910399999991,50.575016999999995,46.690000500000004,42.790338800000001,46.569583500000007,36.58671408,53.108447999999996,50.295032099999993,45.231466499999989,42.469226799999994,45.021074999999996,36.344015400000004,54.664742399999994,50.066904000000001,46.538464500000003,42.104457999999987,46.538464500000003,36.250682999999995,21.376930959999999,21.376930959999999,41.204876999999989,41.204876999999989,21.376930959999999,21.376930959999999,41.204876999999989,41.204876999999989,41.686864799999988,41.686864799999988,41.609054999999991,44.519849999999991,41.152768049999999,44.454249999999988,40.816996499999988,42.611094999999992,null,null,23.244720399999999,23.244720399999999,40.901116200000004,40.901116200000004]
[]
[0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,0,0,0,0]
[1,0.55600000000000005,0.57399999999999995,0.54900000000000004,0.57399999999999995,0.54900000000000004,0.57899999999999996,1.1120000000000001,1.1479999999999999,1.0980000000000001,1.1479999999999999,1.0980000000000001,1.1579999999999999,0.56000000000000005,0.53700000000000003,0.56000000000000005,0.53700000000000003,0.56000000000000005,0.53700000000000003,1.1200000000000001,1.0740000000000001,1.1200000000000001,1.0740000000000001,1.1200000000000001,1.0740000000000001,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,0.35499999999999998,0.35499999999999998,0.7,0.7,0.71,0.71,1.4259999999999999,1.4259999999999999,1.44,1.44,2.2736899383983569,2.5354507658643324,2.2620523504273504,2.6404577464788734,2.2473507462686562,2.582603864734299,null,null,0.37,0.37,0.73,0.73]
[2,0.55600000000000005,0.57399999999999995,0.54900000000000004,0.57399999999999995,0.54900000000000004,0.57899999999999996,1.1120000000000001,1.1479999999999999,1.0980000000000001,1.1479999999999999,1.0980000000000001,1.1579999999999999,0.56000000000000005,0.53700000000000003,0.56000000000000005,0.53700000000000003,0.56000000000000005,0.53700000000000003,1.1200000000000001,1.0740000000000001,1.1200000000000001,1.0740000000000001,1.1200000000000001,1.0740000000000001,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,0.35499999999999998,0.35499999999999998,0.7,0.7,0.71,0.71,1.4259999999999999,1.4259999999999999,1.44,1.44,2.2736899383983569,2.5354507658643324,2.2620523504273504,2.6404577464788734,2.2473507462686562,2.582603864734299,null,null,0.37,0.37,0.73,0.73]
[4,0.55600000000000005,0.57399999999999995,0.54900000000000004,0.57399999999999995,0.54900000000000004,0.57899999999999996,1.1120000000000001,1.1479999999999999,1.0980000000000001,1.1479999999999999,1.0980000000000001,1.1579999999999999,0.56000000000000005,0.53700000000000003,0.56000000000000005,0.53700000000000003,0.56000000000000005,0.53700000000000003,1.1200000000000001,1.0740000000000001,1.1200000000000001,1.0740000000000001,1.1200000000000001,1.0740000000000001,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,0.35499999999999998,0.35499999999999998,0.7,0.7,0.71,0.71,1.4259999999999999,1.4259999999999999,1.44,1.44,2.2736899383983569,2.5354507658643324,2.2620523504273504,2.6404577464788734,2.2473507462686562,2.582603864734299,null,null,0.37,0.37,0.73,0.73]
[9,0.55600000000000005,0.57399999999999995,0.54900000000000004,0.57399999999999995,0.54900000000000004,0.57899999999999996,1.1120000000000001,1.1479999999999999,1.0980000000000001,1.1479999999999999,1.0980000000000001,1.1579999999999999,0.56000000000000005,0.53700000000000003,0.56000000000000005,0.53700000000000003,0.56000000000000005,0.53700000000000003,1.1200000000000001,1.0740000000000001,1.1200000000000001,1.0740000000000001,1.1200000000000001,1.0740000000000001,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,0.35499999999999998,0.35499999999999998,0.7,0.7,0.71,0.71,1.4259999999999999,1.4259999999999999,1.44,1.44,2.2736899383983569,2.5354507658643324,2.2620523504273504,2.6404577464788734,2.2473507462686562,2.582603864734299,null,null,0.37,0.37,0.73,0.73]
[18,0.56699999999999995,0.57399999999999995,0.55900000000000005,0.57399999999999995,0.55900000000000005,0.57899999999999996,1.1339999999999999,1.1479999999999999,1.1180000000000001,1.1479999999999999,1.1180000000000001,1.1579999999999999,0.56000000000000005,0.53700000000000003,0.56000000000000005,0.53700000000000003,0.56000000000000005,0.53700000000000003,1.1200000000000001,1.0740000000000001,1.1200000000000001,1.0740000000000001,1.1200000000000001,1.0740000000000001,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,0.35499999999999998,0.35499999999999998,0.7,0.7,0.71,0.71,1.4259999999999999,1.4259999999999999,1.44,1.44,2.2736899383983569,2.5354507658643324,2.2620523504273504,2.6404577464788734,2.2473507462686562,2.582603864734299,null,null,0.37,0.37,0.73,0.73]
[36,0.56699999999999995,0.57399999999999995,0.55900000000000005,0.57399999999999995,0.55900000000000005,0.57899999999999996,1.1599999999999999,1.18,1.1599999999999999,1.18,1.1399999999999999,1.19,0.748,0.75600000000000001,0.748,0.752,0.747,0.753,1.1200000000000001,1.0740000000000001,1.1200000000000001,1.0740000000000001,1.1200000000000001,1.0740000000000001,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,0.71,0.71,0.7,0.7,0.71,0.71,1.4259999999999999,1.4259999999999999,1.44,1.44,2.2736899383983569,2.5354507658643324,2.2620523504273504,2.6404577464788734,2.2473507462686562,2.582603864734299,null,null,0.72,0.72,0.73,0.73]
[72,0.56699999999999995,0.57399999999999995,0.55900000000000005,0.57399999999999995,0.55900000000000005,0.57899999999999996,1.1599999999999999,1.18,1.1599999999999999,1.18,1.1399999999999999,1.19,0.748,0.75600000000000001,0.748,0.752,0.747,0.753,1.4890000000000001,1.506,1.492,1.5069999999999999,1.49,1.502,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,1.4990000000000001,1.5049999999999999,1.5049999999999999,1.52,1.502,1.5129999999999999,0.71,0.71,1.4259999999999999,1.4259999999999999,0.71,0.71,1.4259999999999999,1.4259999999999999,1.44,1.44,2.2736899383983569,2.5354507658643324,2.2620523504273504,2.6404577464788734,2.2473507462686562,2.582603864734299,null,null,0.72,0.72,1.4259999999999999,1.4259999999999999]
[]
[]
[null,"BUFG","HROW","LEAF","BSW_CLK","D_FF_CTRL","Intra-BRAM","CMT","Other",null,"VDIST","SSIT"]
["CLOCK","mA","mA","mA","mA/MHz"]
[null,6.9999999999999998E-9,2.0000000000000001E-10,-7.0000000000000005E-8,8.2000000000000001E-5]
[null,-2.0000000000000002E-5,-4.9999999999999998E-7,2.9999999999999997E-4,5.0000000000000002E-5,null,"HROW number is per CLOCK_COL"]
[null,2.01E-2,5.0000000000000001E-4,0.1188]
[null,2.7999999999999998E-4,8.0000000000000007E-5]
["V7 Clock",3.70405E-3,3.1872499999999995E-3,6.7164999999999998E-4,3.7771428571428564E-5,6.5739999999999991E-5,1.2800000000000001E-3,9.5999999999999991E-7,6.7164999999999998E-4,null,1.2511499999999999E-3,2.109E-4]
[]
["SLICE","clock * toggle_rate * ( LUTs * lut_routing + SRs * sr_routing + RAM * ram_routing) "]
["Fanout","LUT","SR","RAM","FFs",null,null,null,null,"fF","usage"]
[1,{"$f":"G428 + N431","v":5.2892961282499998E-4},{"$f":"G428 + N428","v":7.4077961282499995E-4},{"$f":"G428+N429","v":5.0137961282499988E-4},{"$f":"G428 + N430","v":3.2372961282499992E-4},null,{"$f":"$G430*0.7","v":2.5532961282499994E-4},null,"SGL/DBL",51,4.1539999999999999,"SRLUT",511,{"$f":"M428*0.95/1000000","v":4.8545000000000001E-4},null,null,{"$f":"$G430*0.7*1000000","v":255.32961282499994}]
["Low",{"$f":"G429 + N431","v":5.8364310128749988E-4},{"$f":"G429+N428","v":7.9549310128749985E-4},{"$f":"G429+N429","v":5.5609310128749989E-4},{"$f":"G429 + N430","v":3.7844310128749988E-4},null,{"$f":"$G430*0.85","v":3.100431012874999E-4},null,"QUAD",76,1.855,"SRAM",259,{"$f":"M429*0.95/1000000","v":2.4604999999999999E-4},null,null,{"$f":"$G430*0.85*1000000","v":310.04310128749989}]
["Medium",{"$f":"G430 + N431","v":6.3835658974999989E-4},{"$f":"G430+N428","v":8.5020658974999997E-4},{"$f":"G430+N429","v":6.108065897499999E-4},{"$f":"G430 + N430","v":4.3315658974999989E-4},null,{"$f":"(K428*$J428 + K429*$J429 + K430*$J430 + (NUM_DICE-1)*K431*J431)*0.95/1000000","v":3.6475658974999991E-4},null,"LONG",179,8.7950000000000007E-3,"FF+OMUX",72,{"$f":"M430*0.95/1000000","v":6.8399999999999996E-5},null,null,{"$f":"(3.56*$J428 + 1.29*$J429 + 0.11*$J430)*1","v":299.29000000000002}]
["High",{"$f":"G431 + N431","v":6.930700782124999E-4},{"$f":"G431+N428","v":9.0492007821249987E-4},{"$f":"G431+N429","v":6.655200782124998E-4},{"$f":"G431 + N430","v":4.8787007821249985E-4},null,{"$f":"$G430*1.15","v":4.1947007821249987E-4},null,"BALI",935,1.5800000000000002E-2,"LUT",288,{"$f":"M431*0.95/1000000","v":2.7359999999999998E-4},null,null,{"$f":"$G430*1.15*1000000","v":419.47007821249986}]
[5,{"$f":"G432 + N431","v":7.477835666749998E-4},{"$f":"G432+N428","v":9.5963356667499989E-4},{"$f":"G432+N429","v":7.2023356667499992E-4},{"$f":"G432 + N430","v":5.4258356667499991E-4},null,{"$f":"$G430*1.3","v":4.7418356667499988E-4},null,"IMUX",69,null,"Per Pin",{"$f":"144*0.95","v":136.79999999999998},{"$f":"M432*1*0.95/1000000","v":1.2995999999999998E-4},null,null,{"$f":"$G430*1.3*1000000","v":474.18356667499989}]
[]
[null,"Net","LUT","FF","SRLUT","SRAM",{"$f":"G428*(1+5*0.14)","v":4.3406034180249993E-4},null,null,null,null,null,null,"LUT","FF","SRLUT","SRAM"]
[null,{"$f":"G430","v":3.6475658974999991E-4},{"$f":"N431","v":2.7359999999999998E-4},{"$f":"N430","v":6.8399999999999996E-5},{"$f":"N428","v":4.8545000000000001E-4},{"$f":"N429","v":2.4604999999999999E-4},null,null,null,null,null,"LogicPerBel","slope",3.5259700000000001E-4,5.94E-5,5.2695400000000005E-4,6.7626199999999996E-4]
[null,{"$f":"(J428*0.5+J432)*0.95/1000000","v":8.9774999999999987E-5},null,null,null,null,null,null,null,null,null,"SignalPerFanout","slope",3.1083E-5,3.18987E-5,3.4967800000000001E-5,3.3969E-5]
[null,null,null,null,null,null,null,null,null,null,null,null,"const",0,0,0,0]
[null,null,null,null,null,null,null,"Leakage/Quad"]
["GTP","Typ (DC) mA","Max (DC)","Typ mA/MHZ","Max mA/MHZ",null,null,"Typ","Max"]
["Vccint",1.2,1.2,0.08,0.08,null,"AVCC"]
["AVCC TX",13,13,3.0000000000000001E-3,3.0000000000000001E-3,null,"AVTT"]
["AVCC RX (LP)",20,20,2.7799999999999999E-3,2.7799999999999999E-3]
["AVTT Ring",0,0,8.9999999999999998E-4,8.9999999999999998E-4]
["AVCC Ring",0,0,3.7000000000000002E-3,3.4146341463414634E-3]
["AVTTTX",15,15,1.4999999999999999E-2,2.23E-2,"mA/mV"]
["AVTTRX (LP)",12,12]
["CLK AVCC",10,10]
["CLK AVTT",1.55,1.55]
["BIAS",3.05,3.05]
["OOB",12.5,12.5]
[]
["GTXE2","Typ (DC) mA","Max (DC)","Typ mA/MHZ","Max mA/MHZ"]
["Vccint",1.2,1.2,0.14000000000000001,0.14000000000000001]
["AVCC TX",27.228999999999999,27.228999999999999,3.2616666666666649E-3,3.2616666666666649E-3]
["AVCC RX (LP)",40,40,2.7750000000000001E-3,2.7750000000000001E-3]
["AVCC RX (DFE)",25.5,25.5,9.6399999999999993E-3,9.6399999999999993E-3]
["AVTT Ring",0,0,8.5000000000000006E-3,8.5000000000000006E-3]
["AVCC Ring",0,0,3.4146341463414634E-3,3.4146341463414634E-3]
["VCCAUX LC",7.6726999999999999,7.6726999999999999,2.6446280991735506E-4,2.6446280991735506E-4]
["AVTT LC",{"$f":"27.6727","v":27.672699999999999},{"$f":"27.6727","v":27.672699999999999},2.6446280991735506E-4,2.6446280991735506E-4]
["AVCC LC",50,50,1.5867768595041326E-3,1.5867768595041326E-3]
["AVTTTX",0,0,2.23E-2,2.23E-2,"mA/mV"]
["AVTTRX (LP)",58,58]
["AVTTRX (DFE)",{"$f":"50.64","v":50.64},{"$f":"50.64","v":50.64}]
["CLK AVCC",25.6,25.6]
["CLK AVTT",1.55,1.55]
["BIAS",3.05,3.05]
["OOB",12.5,12.5]
[null,null,null,null,null,"lpm1.5",null,"lpm2",null,"lpm4"]
["GTHE3","Typ (DC) mA","Max (DC)","Typ mA/MHZ","Max mA/MHZ","mA ","mA/MHz ","mA ","mA/MHz ","mA ","mA/MHz ","mA","AVTT TX/OP"]
["Vccint",1.28,1.28,0.10526810561578119,0.10526810561578119,null,null,null,null,null,null,null,0,"x^2"]
["AVCC TX",18,18,2.4407272727272728E-3,2.4407272727272728E-3,null,null,null,null,null,null,null,2.5899999999999999E-2,"x"]
["AVCC RX (LP)",28,28,2.3999999999999998E-3,2.3999999999999998E-3,11,2.3999999999999998E-3,18,2.3999999999999998E-3,16,4.5000000000000005E-3,25,0.98050000000000004,"c"]
["AVCC RX (DFE)",41.5,41.5,5.2383435582822099E-3,5.2383435582822099E-3]
["AVTT Ring",19.100000000000001,19.100000000000001,2.0999999999999999E-3,2.0999999999999999E-3]
["AVCC Ring",10,10,6.0000000000000001E-3,6.0000000000000001E-3]
["VCCAUX LC",13.2,13.2,1.6161616161616192E-5,1.6161616161616192E-5]
["AVTT LC",60,60,0,0]
["AVCC LC",20,20,2E-3,2E-3]
["AVTTTX",1.3388,1.3388,0,0]
["AVTTRX (LP)",3,3,0,0]
["AVTTRX (DFE)",18.5,18.5]
["CLK AVCC",12.5,12.5]
["CLK AVTT",1.6666666666666667,1.6666666666666667]
["BIAS",0,0]
["OOB",15,15]
["Vccint RX ",0,0]
["Eye Scan",23,23]
["AVCC RX (LP) < 9G",28,28,2.3999999999999998E-3,2.3999999999999998E-3,16,2.3999999999999998E-3,21,2.3999999999999998E-3,47,2E-3,0]
["AVCC RX (DFE) < 9G",37,37,2.5000000000000001E-3,2.5000000000000001E-3]
["AVCC LC < 9G",0,0,1.4E-2,1.4E-2]
["AVCC RX (LPM) - CPLL",0,0,2.0999999999999999E-3,2.0999999999999999E-3,23,2E-3,33,1.1999999999999999E-3,18,2E-3,0]
["AVCC RX (DFE) - CPLL",29,29,3.79E-3,3.79E-3]
[null,null,null,null,null,">10.4Gb",null,12.5,null,15,null,22,null,26,null,null,null,29]
["GTY","Typ (DC) mA","Max (DC)","Typ mA/MHZ","Max mA/MHZ","mA","mA/MHz ","mA","mA/MHz ","mA","mA/MHz ","mA","mA/MHz ","mA","mA/MHz ",null,null,"mA","mA/MHz "]
["Vccint",6.2712751999999998,6.2712751999999998,3.4367635499999998,3.4367635499999998,null,null,null,null,null,null,null,null,null,null,0,"x^2"]
["AVCC TX",8.5562000000000005,8.5562000000000005,3.0220999999999998E-3,3.0220999999999998E-3,null,null,null,null,null,null,null,null,null,null,2.3800000000000002E-2,"x"]
["AVCC RX (LP)",20.2,20.2,2.3532000000000002E-3,2.3532000000000002E-3,20.2,2.3532000000000002E-3,20.2,2.3532000000000002E-3,20.2,2.8999999999999998E-3,26,2.9499999999999999E-3,27,2.99E-3,-1.6585000000000001,"c",103,4.4999999999999999E-4]
["AVCC RX (DFE)",17.5,17.5,3.6946000000000001E-3,3.6946000000000001E-3,17.5,3.6946000000000001E-3,17.5,3.6946000000000001E-3,17.5,4.5690000000000001E-3,17.5,4.5690000000000001E-3,17.5,4.5690000000000001E-3,null,null,17.5,4.5690000000000001E-3]
["AVTT Ring",14.308299999999999,14.308299999999999,1.2953000000000001E-3,1.2953000000000001E-3]
["AVCC Ring",1,1,1.75E-3,1.75E-3]
["VCCAUX LC",19.11,19.11,0,0]
["AVTT LC",0,0,0.02,0.02]
["AVCC LC",2.25,2.25,0,0]
["AVTTTX",110,110,1.73E-4,1.73E-4,118.81,1.346E-3,118.81,1.346E-3,110,1.6999999999999999E-3,118.81,1.346E-3,118.81,1.346E-3,null,null,118.81,1.346E-3]
["AVTTRX (LP)",80,80,4.5999999999999999E-3,4.5999999999999999E-3,65,4.5999999999999999E-3,66,5.5620000000000001E-3,160,1.2999999999999999E-4,110,1.4499999999999999E-3,60,3.5000000000000001E-3,null,null,60,4.0000000000000001E-3]
["AVTTRX (DFE)",100,100,4.5999999999999999E-3,4.5999999999999999E-3,100,3.8E-3,100,4.5999999999999999E-3,148,2E-3,148,1.1999999999999999E-3,148,2E-3,null,null,148,2E-3]
["CLK AVCC",0,0,0,0]
["CLK AVTT",35,35,1.4E-5,1.4E-5,50.63,7.8919999999999997E-5,50.63,7.8919999999999997E-5,52,7.7837000000000002E-4,98.4,0,98.4,0,null,null,98.4,0]
["BIAS",0,0]
["OOB",15,15]
["Vccint RX ",0,0]
["Eye Scan",23,23]
[]
["GTZ","Typ (DC) mA","Max (DC)","Typ mA/Gbps","Max mA/Gbps"]
["Vccint",0,0,6.4335699999999996,6.4335699999999996]
["VCCH",2.302,2.302,0,0]
["AVCC",0.52700000000000002,0.52700000000000002,11.635,11.635]
["AVCC (Tuning)",26.844000000000001,26.844000000000001,13.222,13.222]
["AVCC (Divided Rates)",19.05,19.05,11.635,11.635]
["AVCCLSB",-0.6,-0.6,1.8542000000000001,1.8542000000000001]
["AVCCLSB (RX)",{"$f":"B521*0.67","v":-0.40200000000000002},{"$f":"C521*0.67","v":-0.40200000000000002},{"$f":"D521*0.67","v":1.2423140000000001},{"$f":"E521*0.67","v":1.2423140000000001}]
["AVCCLSB (TX)",{"$f":"B522*0.67","v":-0.26934000000000002},{"$f":"C522*0.67","v":-0.26934000000000002},{"$f":"D521*0.33","v":0.61188600000000004},{"$f":"E521*0.33","v":0.61188600000000004}]
["AVCC HCSL",13.333,13.333,null,null,"Per Yosemite die"]
[]
["IOI","RX/TX ma/MHz","RX ma/MHz","TX mA/MHz"]
["I/ODDR",{"$f":"MAX(C527:D527)","v":1.0949614500000001E-3},1.0949614500000001E-3,1.0949614500000001E-3]
["I/ODELAY",{"$f":"MAX(C528:D528)","v":2.02893856E-3},2.02893856E-3,1.7502718933333334E-3]
["I/OSERDES",1.05798935E-3,1.05798935E-3,1.05798935E-3]
["Bitslice RX/TX",1.4752746206533193E-3,1.4752746206533193E-3,1.0066117212855635E-3]
["Bitslice TRI",1.7028890547945204E-3,1.7028890547945204E-3,1.7028890547945204E-3]
["Bitslice Control",3.7570493125E-3,3.7570493125E-3,3.7570493125E-3]
["IDELAYCTRL",7.2135346799999988E-3,7.2135346799999988E-3,7.2135346799999988E-3]
["Internal VREF",0.25]
["IO Clock",null,null,3.2159531249999998E-4,"Iccint"]
["LVCMOS25",null,null,2.0999999999999999E-3,"Icco for inputs"]
["LVCMOS18",null,null,3.6499999999999998E-4]
["LVCMOS15",null,null,2.3499999999999999E-4]
["LVCMOS12",null,null,1.05E-4]
["IOB18 IBUF","LP Iccint (mA)","LP Vccint Dynamic (mA/MHZ)","HP Iccint (mA)","HP Vccint Dynamic (mA/MHZ)","LP Vccaux Static (mA)","LP Vccaux Dynamic (mA/MHZ)","HP Vccaux Static (mA)","HP Vccaux (mA/MHZ)"]
["LVCMOS",0,6.4459999999999995E-4,0,6.4459999999999995E-4,0,0,0,0]
["SSTL",0.373,6.8999999999999997E-4,0.373,6.8999999999999997E-4,1.8,0,3,0]
["LVDS",{"$f":"0.37*2","v":0.74},{"$f":"0.000672*2","v":1.3439999999999999E-3},{"$f":"0.37*2","v":0.74},{"$f":"0.000677*2","v":1.354E-3},3.6,0,6,0,null,"All the LVDS numbers are multiplied by 2, as the simulation is for a single pin"]
["POD",0.373,6.8999999999999997E-4,0.373,6.8999999999999997E-4,1.8,0,3,0]
["DIFF POD",0.746,1.3799999999999999E-3,0.746,1.3799999999999999E-3,3.6,0,6,0,null,"All the LVDS numbers are multiplied by 2, as the simulation is for a single pin"]
[]
["IOB33 IBUF"]
["LVCMOS",0,6.9999999999999994E-5,0,6.9999999999999994E-5,0,0,0,0,null,null,"`"]
["SSTL",0.315,4.5399999999999998E-4,0.315,4.5399999999999998E-4,1.754,2.2000000000000001E-3,2.93,3.5999999999999999E-3]
["LVDS",{"$f":"2*0.315","v":0.63},{"$f":"2*0.000454","v":9.0799999999999995E-4},{"$f":"2*0.315","v":0.63},{"$f":"2*0.000454","v":9.0799999999999995E-4},{"$f":"2*1.754","v":3.508},{"$f":"2*0.0022","v":4.4000000000000003E-3},{"$f":"2*2.93","v":5.86},{"$f":"2*0.0036","v":7.1999999999999998E-3}]
[]
["LVDS Bias (IOB18 bank)",0]
["LVDS Bias (IOB33 bank)",0]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,10,11,12,13,14,null,null,null,"On-Chip Termination (W)",null,null,"IBUF LP","IBUF LP",null,"IBUF LP","IBUF LP","LP","IBUF HP","IBUF HP",null,"IBUF HP","IBUF HP","HP","OBUF","OBUF","OBUF","OBUF","OBUF"]
["HR Bank",1,2,3,"Output","Input","DCI",7,8,9,"Static Output Current","Static Input Current","Static Power","Output on-chip static power","Input on-chip static power",15,null,null,"Diff Term","In Term(50)",null,"Vccint","Vccaux","Vcco","Vccint","Vccaux","Vcco","Vccint","Vccaux","Vcco","Vccint","Vccaux","Vcco","Vccint_io","Vccaux_io","Vcco","Vccint_io","Vccaux_io"]
["IO_STANDARD","Vcco","Type","Internal","Iccaux","Iccauxq","Bank mA","DIFFAMP","Voh","Vol","mA","mA","mW","mW",null,"IBUF","MAP Name",null,null,null,0," (mA/MHZ)"," (mA/MHZ)","mA/MHz","(mA)","(mA)","mA"," (mA/MHZ)"," (mA/MHZ)","mA/MHz","(mA)","(mA)","mA","(mA/Mhz)","(mA/Mhz)","(mA/Mhz*pF)","(mA)","(mA)"]
["BLVDS 2.5V (pair)",{"$f":"VCCO25","v":2.5},2,13,0,0,0,0,0,0,14.9,1.6059E-2,{"$f":"B560*K560","v":37.25},15.055,0,"LVDS","BLVDS_25",null,null,null,0,8.0424000000000012E-4,4.3839999999999971E-4,3.1999999999998698E-7,0.39779999999999999,1.2719,1.6059E-2,8.0103999999999993E-4,5.7600000000000056E-4,3.2000000000001472E-7,0.44026999999999999,1.6996,1.6059E-2,1.1000000000000001E-3,3.5000000000000001E-3,2.1935483870967744E-3,6.0299999999999999E-2,1.7100000000000001E-2]
["Diff HSTL Class I 1.5V (pair)",{"$f":"VCCO15","v":1.5},1,13,0,0,0,0.73,1.1000000000000001,0.4,9.6,0,10.5,15.602999999999998,0,"LVDS","DIFF_HSTL_I",null,null,15,0,3.6899999999999997E-4,5.1875000000000116E-5,3.750000000000142E-6,0.48144999999999999,1.6612,15.625,1.8786250000000005E-4,8.9000000000000185E-5,3.750000000000142E-6,0.63144,2.2328000000000001,15.625,7.2559999999999996E-4,5.0619999999999997E-3,4.5690322580645154E-4,0.12510000000000002,2.722E-3]
["Diff HSTL Class I 1.8V (pair)",{"$f":"VCCO18","v":1.8},1,13,0,0,0,0.73,1.4,0.4,11.6,0,18,23.666399999999999,0,"LVDS","DIFF_HSTL_I_18",null,null,18,0,3.8858749999999998E-4,2.8374999999999927E-5,3.750000000000142E-6,0.46128999999999998,1.6232,18.75,3.3686250000000001E-4,8.712499999999957E-5,2.4999999999986145E-6,0.50839000000000001,2.1545999999999998,18.75,7.275999999999999E-4,5.4000000000000003E-3,6.8129032258064512E-4,0.12510000000000002,2.7039999999999994E-3]
["Diff HSTL Class II 1.5V (pair)",{"$f":"VCCO15","v":1.5},1,13,0,0,0,0.73,1.1000000000000001,0.4,18.600000000000001,0,21,15.602999999999998,0,"LVDS","DIFF_HSTL_II",null,null,15,0,3.6899999999999997E-4,5.1875000000000116E-5,3.750000000000142E-6,0.48144999999999999,1.6612,15.625,3.3686250000000001E-4,8.712499999999957E-5,2.4999999999986145E-6,0.50839000000000001,2.1545999999999998,15.625,9.2299999999999999E-4,9.6179999999999998E-3,4.0619354838709681E-4,0.12510000000000002,2.7359999999999997E-3]
["Diff HSTL Class II 1.8V (pair)",{"$f":"VCCO18","v":1.8},1,13,0,0,0,0.73,1.4,0.4,24.4,0,36,23.666399999999999,0,"LVDS","DIFF_HSTL_II_18",null,null,18,0,3.8858749999999998E-4,2.8374999999999927E-5,3.750000000000142E-6,0.46128999999999998,1.6232,18.75,3.3686250000000001E-4,8.712499999999957E-5,2.4999999999986145E-6,0.50839000000000001,2.1545999999999998,18.75,1.2018E-3,1.4387999999999998E-2,7.0851612903225793E-4,0.12510000000000002,2.7279999999999995E-3]
["Diff HSUL 1.2V (pair)",{"$f":"VCCO12","v":1.2},1,13,0,0,{"$f":"2*G577","v":0},0.9,0.96,0.24,7.4,0,0,0,0,"LVDS","DIFF_HSUL_12",null,null,null,0,3.5260000000000001E-4,5.874999999999991E-5,1.2145000000000017E-6,0.50060000000000004,1.6188,0,6.8187499999999984E-5,6.9000000000000173E-5,1.0285000000000004E-6,0.84031,2.2016,0,7.3700000000000002E-4,5.0359999999999997E-3,1.2618064516129032E-3,0.12510000000000002,2.722E-3]
["Diff SSTL 1.2V (pair)",1.2,1,13,0,0,0,1,0.85,0.5,7.62,0,10.5,11.618400000000003,0,"LVDS","DIFF_SSTL12",null,null,13.5,0,3.3136249999999993E-4,5.88749999999999E-5,6.2500000000009769E-6,0.51765000000000005,1.6191,12.5,1.8786250000000005E-4,8.9000000000000185E-5,3.750000000000142E-6,0.63144,2.2328000000000001,12.5,1.1205999999999998E-3,1.223E-2,6.1703225806451615E-4,0.12515999999999999,2.7299999999999998E-3]
["Diff SSTL 1.35V (pair)",{"$f":"VCCO135","v":1.35},1,13,0,0,0,1,0.85,0.5,7.62,0,10.5,13.224600000000001,0,"LVDS","DIFF_SSTL135",null,null,13.5,0,3.7580000000000003E-4,6.0125000000000038E-5,3.750000000000142E-6,0.47960000000000003,1.6471,14.0625,6.8237500000000039E-5,6.9125000000000433E-5,6.2500000000009769E-6,0.84025000000000005,2.2019000000000002,14.0625,1.0208000000000001E-3,1.0774000000000001E-2,3.7238709677419354E-4,0.12514,2.7419999999999996E-3]
["Diff SSTL 1.35V R (pair)",{"$f":"VCCO135","v":1.35},1,13,0,0,0,1,0.75,0.6,7.62,0,10.5,13.224600000000001,0,"LVDS","DIFF_SSTL135_R",null,null,13.5,0,3.7580000000000003E-4,6.0125000000000038E-5,3.750000000000142E-6,0.47960000000000003,1.6471,14.0625,9.6374999999999937E-6,8.0999999999999963E-5,3.750000000000142E-6,0.77600000000000002,2.2267000000000001,14.0625,7.3079999999999998E-4,5.1680000000000007E-3,5.1483870967741925E-4,0.12510000000000002,2.7060000000000001E-3]
["Diff SSTL 1.5V (pair)",{"$f":"VCCO15","v":1.5},1,13,0,0,0,1,0.92500000000000004,0.57499999999999996,7.62,0,10.5,15.864000000000001,0,"LVDS","DIFF_SSTL15",null,null,15,0,3.6899999999999997E-4,5.1875000000000116E-5,3.750000000000142E-6,0.48144999999999999,1.6612,15.625,9.6374999999999937E-6,8.0999999999999963E-5,3.750000000000142E-6,0.77600000000000002,2.2267000000000001,15.625,1.1068E-3,1.2133999999999999E-2,4.7122580645161288E-4,0.12512000000000001,2.722E-3]
["Diff SSTL 1.5V R (pair)",{"$f":"VCCO15","v":1.5},1,13,0,0,0,1,0.82499999999999996,0.67500000000000004,7.62,0,10.5,15.864000000000001,0,"LVDS","DIFF_SSTL15_R",null,null,15,0,3.6899999999999997E-4,5.1875000000000116E-5,3.750000000000142E-6,0.48144999999999999,1.6612,15.625,1.8786250000000005E-4,8.9000000000000185E-5,3.750000000000142E-6,0.63144,2.2328000000000001,15.625,6.3019999999999992E-4,3.65E-3,5.206451612903226E-4,0.12506000000000003,2.6899999999999997E-3]
["Diff SSTL Class I 1.8V (pair)",{"$f":"VCCO18","v":1.8},1,13,0,0,0,0.73,1.3,0.54,9.4,0,13.68,20.491200000000003,0,"LVDS","DIFF_SSTL18_I",null,null,18,0,3.8858749999999998E-4,2.8374999999999927E-5,3.750000000000142E-6,0.46128999999999998,1.6232,18.75,3.3686250000000001E-4,8.712499999999957E-5,2.4999999999986145E-6,0.50839000000000001,2.1545999999999998,18.75,6.3659999999999997E-4,3.552E-3,4.2606451612903223E-4,0.12508,2.7080000000000003E-3]
["Diff SSTL Class II 1.8V (pair)",{"$f":"VCCO18","v":1.8},1,13,0,0,0,0.73,1.4,0.4,16.2,0,36,20.491200000000003,0,"LVDS","DIFF_SSTL18_II",null,null,18,0,3.8858749999999998E-4,2.8374999999999927E-5,3.750000000000142E-6,0.46128999999999998,1.6232,18.75,1.8786250000000005E-4,8.9000000000000185E-5,3.750000000000142E-6,0.63144,2.2328000000000001,18.75,1.0118E-3,1.1188E-2,5.8619354838709674E-4,0.12510000000000002,2.722E-3]
["HSTL Class I 1.5V",{"$f":"VCCO15","v":1.5},3,6.5,0,0,0,0.45,1.1000000000000001,0.4,4.8,0,{"$f":"B573*(I573-J573)/200*1000","v":5.25},7.801499999999999,0,"HSTL","HSTL_I",null,null,7.5,0,2.0825000000000002E-4,3.4750000000000059E-5,4.1249999999992685E-6,0.35666999999999999,1.52,7.8125,1.153499999999999E-4,5.8124999999999983E-5,2.874999999999961E-6,0.62117999999999995,2.0926999999999998,7.8125,3.6279999999999998E-4,2.5309999999999998E-3,3.9344444444444436E-4,6.2550000000000008E-2,1.361E-3]
["HSTL Class I 1.8V",{"$f":"VCCO18","v":1.8},3,6.5,0,0,0,0.45,1.4,0.4,5.8,0,9,11.8332,0,"HSTL","HSTL_I_18",null,null,9,0,2.4403749999999996E-4,2.2625000000000008E-5,2.500000000000835E-6,0.32558999999999999,1.4825999999999999,9.375,1.5841249999999995E-4,4.8875000000000172E-5,2.500000000000835E-6,0.39582000000000001,2.0152000000000001,9.375,3.6379999999999995E-4,2.7000000000000001E-3,5.8666666666666665E-4,6.2550000000000008E-2,1.3519999999999997E-3]
["HSTL Class II 1.5V",{"$f":"VCCO15","v":1.5},3,6.5,0,0,0,0.45,1.1000000000000001,0.4,9.3000000000000007,0,{"$f":"B575*(I575-J575)/100*1000","v":10.5},7.801499999999999,0,"HSTL","HSTL_II",null,null,7.5,0,2.0825000000000002E-4,3.4750000000000059E-5,4.1249999999992685E-6,0.35666999999999999,1.52,7.8125,1.153499999999999E-4,5.8124999999999983E-5,2.874999999999961E-6,0.62117999999999995,2.0926999999999998,7.8125,4.615E-4,4.8089999999999999E-3,3.4977777777777779E-4,6.2550000000000008E-2,1.3679999999999999E-3]
["HSTL Class II 1.8V",{"$f":"VCCO18","v":1.8},3,6.5,0,0,0,0.45,1.4,0.4,12.2,0,{"$f":"B576*(I576-J576)/100*1000","v":18},11.8332,0,"HSTL","HSTL_II_18",null,null,9,0,2.4403749999999996E-4,2.2625000000000008E-5,2.500000000000835E-6,0.32558999999999999,1.4825999999999999,9.375,1.5841249999999995E-4,4.8875000000000172E-5,2.500000000000835E-6,0.39582000000000001,2.0152000000000001,9.375,6.0090000000000002E-4,7.193999999999999E-3,6.1011111111111108E-4,6.2550000000000008E-2,1.3639999999999998E-3]
["HSUL 1.2V",{"$f":"VCCO12","v":1.2},1,6.5,0,0,0,0.45,0.96,0.24,3.7,0,0,0,0,"HSTL","HSUL_12",null,null,null,0,1.5268749999999996E-4,5.5499999999999994E-5,1.4112499999999996E-7,0.40827999999999998,1.4778,0,4.8642499999999997E-4,1.2262500000000009E-4,1.5625000000000446E-8,0.39021,1.9632000000000001,0,3.6850000000000001E-4,2.5179999999999998E-3,1.0865555555555555E-3,6.2550000000000008E-2,1.361E-3]
["LVCMOS 1.2V 4mA (Slow)",{"$f":"VCCO12","v":1.2},1,6.5,0,0,0,0,0,0,0,3.1970000000000002E-3,0,0,0,"LVCMOS12","LVCMOS12_4_SLOW",null,null,null,0,1.7646666666666663E-4,0,1.0128666666666666E-4,8.523E-2,1.64E-3,3.1970000000000002E-3,1.7646666666666663E-4,0,1.0128666666666666E-4,8.523E-2,1.64E-3,3.1970000000000002E-3,3.4900000000000003E-4,1.7149999999999999E-3,9.0000000000000008E-4,6.2539999999999998E-2,1.34E-3]
["LVCMOS 1.2V 4mA (Fast)",1.2,1,6.5,0,0,0,0,0,0,0,3.1970000000000002E-3,0,0,0,"LVCMOS12","LVCMOS12_4_FAST",null,null,null,0,1.7646666666666663E-4,0,1.0128666666666666E-4,8.523E-2,1.64E-3,3.1970000000000002E-3,1.7646666666666663E-4,0,1.0128666666666666E-4,8.523E-2,1.64E-3,3.1970000000000002E-3,3.4900000000000003E-4,1.7149999999999999E-3,9.0000000000000008E-4,6.2539999999999998E-2,1.34E-3]
["LVCMOS 1.2V 8mA (Slow)",1.2,1,6.5,0,0,0,0,0,0,0,3.1970000000000002E-3,0,0,0,"LVCMOS12","LVCMOS12_8_SLOW",null,null,null,0,1.7646666666666663E-4,0,1.0128666666666666E-4,8.523E-2,1.64E-3,3.1970000000000002E-3,1.7646666666666663E-4,0,1.0128666666666666E-4,8.523E-2,1.64E-3,3.1970000000000002E-3,4.529E-4,3.4910000000000002E-3,9.0956521739130459E-4,6.2560000000000004E-2,1.3649999999999999E-3]
["LVCMOS 1.2V 8mA (Fast)",1.2,1,6.5,0,0,0,0,0,0,0,3.1970000000000002E-3,0,0,0,"LVCMOS12","LVCMOS12_8_FAST",null,null,null,0,1.7646666666666663E-4,0,1.0128666666666666E-4,8.523E-2,1.64E-3,3.1970000000000002E-3,1.7646666666666663E-4,0,1.0128666666666666E-4,8.523E-2,1.64E-3,3.1970000000000002E-3,4.529E-4,3.4910000000000002E-3,9.0956521739130459E-4,6.2560000000000004E-2,1.3649999999999999E-3]
["LVCMOS 1.2V 12mA (Slow)",1.2,1,6.5,0,0,0,0,0,0,0,3.1970000000000002E-3,0,0,0,"LVCMOS12","LVCMOS12_12_SLOW",null,null,null,0,1.7646666666666663E-4,0,1.0128666666666666E-4,8.523E-2,1.64E-3,3.1970000000000002E-3,1.7646666666666663E-4,0,1.0128666666666666E-4,8.523E-2,1.64E-3,3.1970000000000002E-3,5.9219999999999987E-4,6.2220000000000001E-3,9.2695652173913057E-4,6.2590000000000007E-2,1.3620000000000001E-3]
["LVCMOS 1.2V 12mA (Fast)",1.2,1,6.5,0,0,0,0,0,0,0,3.1970000000000002E-3,0,0,0,"LVCMOS12","LVCMOS12_12_FAST",null,null,null,0,1.7646666666666663E-4,0,1.0128666666666666E-4,8.523E-2,1.64E-3,3.1970000000000002E-3,1.7646666666666663E-4,0,1.0128666666666666E-4,8.523E-2,1.64E-3,3.1970000000000002E-3,5.9219999999999987E-4,6.2220000000000001E-3,9.2695652173913057E-4,6.2590000000000007E-2,1.3620000000000001E-3]
["LVCMOS 1.5V 4mA (Slow)",{"$f":"VCCO15","v":1.5},1,6.5,0,0,0,0,0,0,0,3.6449999999999998E-3,0,0,0,"LVCMOS15","LVCMOS15_4_SLOW",null,null,null,0,1.7639999999999998E-4,0,2.0623333333333335E-4,8.5239999999999996E-2,1.7240000000000001E-3,3.6449999999999998E-3,1.7639999999999998E-4,0,2.0623333333333335E-4,8.5239999999999996E-2,1.7240000000000001E-3,3.6449999999999998E-3,3.4809999999999995E-4,1.6859999999999998E-3,1.1113043478260872E-3,6.2539999999999998E-2,1.3389999999999999E-3]
["LVCMOS 1.5V 4mA (Fast)",1.5,1,6.5,0,0,0,0,0,0,0,3.6449999999999998E-3,0,0,0,"LVCMOS15","LVCMOS15_4_FAST",null,null,null,0,1.7639999999999998E-4,0,2.0623333333333335E-4,8.5239999999999996E-2,1.7240000000000001E-3,3.6449999999999998E-3,1.7639999999999998E-4,0,2.0623333333333335E-4,8.5239999999999996E-2,1.7240000000000001E-3,3.6449999999999998E-3,3.4809999999999995E-4,1.6859999999999998E-3,1.1113043478260872E-3,6.2539999999999998E-2,1.3389999999999999E-3]
["LVCMOS 1.5V 8mA (Slow)",1.5,1,6.5,0,0,0,0,0,0,0,3.6449999999999998E-3,0,0,0,"LVCMOS15","LVCMOS15_8_SLOW",null,null,null,0,1.7639999999999998E-4,0,2.0623333333333335E-4,8.5239999999999996E-2,1.7240000000000001E-3,3.6449999999999998E-3,1.7639999999999998E-4,0,2.0623333333333335E-4,8.5239999999999996E-2,1.7240000000000001E-3,3.6449999999999998E-3,4.0149999999999995E-4,2.5349999999999999E-3,1.1208695652173914E-3,6.2550000000000008E-2,1.3460000000000002E-3]
["LVCMOS 1.5V 8mA (Fast)",1.5,1,6.5,0,0,0,0,0,0,0,3.6449999999999998E-3,0,0,0,"LVCMOS15","LVCMOS15_8_FAST",null,null,null,0,1.7639999999999998E-4,0,2.0623333333333335E-4,8.5239999999999996E-2,1.7240000000000001E-3,3.6449999999999998E-3,1.7639999999999998E-4,0,2.0623333333333335E-4,8.5239999999999996E-2,1.7240000000000001E-3,3.6449999999999998E-3,4.0149999999999995E-4,2.5349999999999999E-3,1.1208695652173914E-3,6.2550000000000008E-2,1.3460000000000002E-3]
["LVCMOS 1.5V 12mA (Slow)",1.5,1,6.5,0,0,0,0,0,0,0,3.6449999999999998E-3,0,0,0,"LVCMOS15","LVCMOS15_12_SLOW",null,null,null,0,1.7639999999999998E-4,0,2.0623333333333335E-4,8.5239999999999996E-2,1.7240000000000001E-3,3.6449999999999998E-3,1.7639999999999998E-4,0,2.0623333333333335E-4,8.5239999999999996E-2,1.7240000000000001E-3,3.6449999999999998E-3,4.9209999999999998E-4,4.3689999999999988E-3,1.1304347826086958E-3,6.2550000000000008E-2,1.3429999999999998E-3]
["LVCMOS 1.5V 12mA (Fast)",1.5,1,6.5,0,0,0,0,0,0,0,3.6449999999999998E-3,0,0,0,"LVCMOS15","LVCMOS15_12_FAST",null,null,null,0,1.7639999999999998E-4,0,2.0623333333333335E-4,8.5239999999999996E-2,1.7240000000000001E-3,3.6449999999999998E-3,1.7639999999999998E-4,0,2.0623333333333335E-4,8.5239999999999996E-2,1.7240000000000001E-3,3.6449999999999998E-3,4.9209999999999998E-4,4.3689999999999988E-3,1.1304347826086958E-3,6.2550000000000008E-2,1.3429999999999998E-3]
["LVCMOS 1.5V 16mA (Slow)",1.5,1,6.5,0,0,0,0,0,0,0,3.6449999999999998E-3,0,0,0,"LVCMOS15","LVCMOS15_16_SLOW",null,null,null,0,1.7639999999999998E-4,0,2.0623333333333335E-4,8.5239999999999996E-2,1.7240000000000001E-3,3.6449999999999998E-3,1.7639999999999998E-4,0,2.0623333333333335E-4,8.5239999999999996E-2,1.7240000000000001E-3,3.6449999999999998E-3,5.886E-4,6.5949999999999993E-3,1.1434782608695654E-3,6.2560000000000004E-2,1.3629999999999998E-3]
["LVCMOS 1.5V 16mA (Fast)",1.5,1,6.5,0,0,0,0,0,0,0,3.6449999999999998E-3,0,0,0,"LVCMOS15","LVCMOS15_16_FAST",null,null,null,0,1.7639999999999998E-4,0,2.0623333333333335E-4,8.5239999999999996E-2,1.7240000000000001E-3,3.6449999999999998E-3,1.7639999999999998E-4,0,2.0623333333333335E-4,8.5239999999999996E-2,1.7240000000000001E-3,3.6449999999999998E-3,5.886E-4,6.5949999999999993E-3,1.1434782608695654E-3,6.2560000000000004E-2,1.3629999999999998E-3]
["LVCMOS 1.8V 4mA (Slow)",{"$f":"VCCO18","v":1.8},1,6.5,0,0,0,0,0,0,0,4.6800000000000001E-3,0,0,0,"LVCMOS18","LVCMOS18_4_SLOW",null,null,null,0,1.664666666666666E-4,0,2.9546666666666667E-4,7.5130000000000002E-2,1.7619999999999999E-3,4.6800000000000001E-3,1.664666666666666E-4,0,2.9546666666666667E-4,7.5130000000000002E-2,1.7619999999999999E-3,4.6800000000000001E-3,3.5090000000000002E-4,1.5769999999999998E-3,1.3000000000000004E-3,6.2539999999999998E-2,1.3260000000000001E-3]
["LVCMOS 1.8V 4mA (Fast)",1.8,1,6.5,0,0,0,0,0,0,0,4.6800000000000001E-3,0,0,0,"LVCMOS18","LVCMOS18_4_FAST",null,null,null,0,1.664666666666666E-4,0,2.9546666666666667E-4,7.5130000000000002E-2,1.7619999999999999E-3,4.6800000000000001E-3,1.664666666666666E-4,0,2.9546666666666667E-4,7.5130000000000002E-2,1.7619999999999999E-3,4.6800000000000001E-3,3.5090000000000002E-4,1.5769999999999998E-3,1.3000000000000004E-3,6.2539999999999998E-2,1.3260000000000001E-3]
["LVCMOS 1.8V 8mA (Slow)",1.8,1,6.5,0,0,0,0,0,0,0,4.6800000000000001E-3,0,0,0,"LVCMOS18","LVCMOS18_8_SLOW",null,null,null,0,1.664666666666666E-4,0,2.9546666666666667E-4,7.5130000000000002E-2,1.7619999999999999E-3,4.6800000000000001E-3,1.664666666666666E-4,0,2.9546666666666667E-4,7.5130000000000002E-2,1.7619999999999999E-3,4.6800000000000001E-3,3.4739999999999999E-4,1.8290000000000001E-3,1.3043478260869568E-3,6.2539999999999998E-2,1.3449999999999998E-3]
["LVCMOS 1.8V 8mA (Fast)",1.8,1,6.5,0,0,0,0,0,0,0,4.6800000000000001E-3,0,0,0,"LVCMOS18","LVCMOS18_8_FAST",null,null,null,0,1.664666666666666E-4,0,2.9546666666666667E-4,7.5130000000000002E-2,1.7619999999999999E-3,4.6800000000000001E-3,1.664666666666666E-4,0,2.9546666666666667E-4,7.5130000000000002E-2,1.7619999999999999E-3,4.6800000000000001E-3,3.4739999999999999E-4,1.8290000000000001E-3,1.3043478260869568E-3,6.2539999999999998E-2,1.3449999999999998E-3]
["LVCMOS 1.8V 12mA (Slow)",1.8,1,6.5,0,0,0,0,0,0,0,4.6800000000000001E-3,0,0,0,"LVCMOS18","LVCMOS18_12_SLOW",null,null,null,0,1.664666666666666E-4,0,2.9546666666666667E-4,7.5130000000000002E-2,1.7619999999999999E-3,4.6800000000000001E-3,1.664666666666666E-4,0,2.9546666666666667E-4,7.5130000000000002E-2,1.7619999999999999E-3,4.6800000000000001E-3,4.4699999999999997E-4,3.3909999999999999E-3,1.310434782608696E-3,6.2539999999999998E-2,1.3439999999999999E-3]
["LVCMOS 1.8V 12mA (Fast)",1.8,1,6.5,0,0,0,0,0,0,0,4.6800000000000001E-3,0,0,0,"LVCMOS18","LVCMOS18_12_FAST",null,null,null,0,1.664666666666666E-4,0,2.9546666666666667E-4,7.5130000000000002E-2,1.7619999999999999E-3,4.6800000000000001E-3,1.664666666666666E-4,0,2.9546666666666667E-4,7.5130000000000002E-2,1.7619999999999999E-3,4.6800000000000001E-3,4.4699999999999997E-4,3.3909999999999999E-3,1.310434782608696E-3,6.2539999999999998E-2,1.3439999999999999E-3]
["LVCMOS 1.8V 16mA (Slow)",1.8,1,6.5,0,0,0,0,0,0,0,4.6800000000000001E-3,0,0,0,"LVCMOS18","LVCMOS18_16_SLOW",null,null,null,0,1.664666666666666E-4,0,2.9546666666666667E-4,7.5130000000000002E-2,1.7619999999999999E-3,4.6800000000000001E-3,1.664666666666666E-4,0,2.9546666666666667E-4,7.5130000000000002E-2,1.7619999999999999E-3,4.6800000000000001E-3,4.44E-4,3.7420000000000001E-3,1.3165217391304348E-3,6.2539999999999998E-2,1.341E-3]
["LVCMOS 1.8V 16mA (Fast)",1.8,1,6.5,0,0,0,0,0,0,0,4.6800000000000001E-3,0,0,0,"LVCMOS18","LVCMOS18_16_FAST",null,null,null,0,1.664666666666666E-4,0,2.9546666666666667E-4,7.5130000000000002E-2,1.7619999999999999E-3,4.6800000000000001E-3,1.664666666666666E-4,0,2.9546666666666667E-4,7.5130000000000002E-2,1.7619999999999999E-3,4.6800000000000001E-3,4.44E-4,3.7420000000000001E-3,1.3165217391304348E-3,6.2539999999999998E-2,1.341E-3]
["LVCMOS 2.5V 4mA (Slow)",{"$f":"VCCO25","v":2.5},1,6.5,0,0,0,0,0,0,0,1.504E-2,0,0,0,"LVCMOS25","LVCMOS25_4_SLOW",null,null,null,0,1.5586666666666664E-4,6.9653333333333331E-4,1.3524000000000001E-3,7.5370000000000006E-2,1.6920000000000001E-2,1.504E-2,1.5586666666666664E-4,6.9653333333333331E-4,1.3524000000000001E-3,7.5370000000000006E-2,1.6920000000000001E-2,1.504E-2,4.1879999999999999E-4,1.0332E-3,1.9713043478260871E-3,6.2770000000000006E-2,1.7210000000000003E-2]
["LVCMOS 2.5V 4mA (Fast)",2.5,1,6.5,0,0,0,0,0,0,0,1.504E-2,0,0,0,"LVCMOS25","LVCMOS25_4_FAST",null,null,null,0,1.5586666666666664E-4,6.9653333333333331E-4,1.3524000000000001E-3,7.5370000000000006E-2,1.6920000000000001E-2,1.504E-2,1.5586666666666664E-4,6.9653333333333331E-4,1.3524000000000001E-3,7.5370000000000006E-2,1.6920000000000001E-2,1.504E-2,4.1879999999999999E-4,1.0332E-3,1.9713043478260871E-3,6.2770000000000006E-2,1.7210000000000003E-2]
["LVCMOS 2.5V 8mA (Slow)",2.5,1,6.5,0,0,0,0,0,0,0,1.504E-2,0,0,0,"LVCMOS25","LVCMOS25_8_SLOW",null,null,null,0,1.5586666666666664E-4,6.9653333333333331E-4,1.3524000000000001E-3,7.5370000000000006E-2,1.6920000000000001E-2,1.504E-2,1.5586666666666664E-4,6.9653333333333331E-4,1.3524000000000001E-3,7.5370000000000006E-2,1.6920000000000001E-2,1.504E-2,5.334999999999999E-4,1.1843999999999999E-3,2.0913043478260874E-3,6.2750000000000014E-2,1.7220000000000003E-2]
["LVCMOS 2.5V 8mA (Fast)",2.5,1,6.5,0,0,0,0,0,0,0,1.504E-2,0,0,0,"LVCMOS25","LVCMOS25_8_FAST",null,null,null,0,1.5586666666666664E-4,6.9653333333333331E-4,1.3524000000000001E-3,7.5370000000000006E-2,1.6920000000000001E-2,1.504E-2,1.5586666666666664E-4,6.9653333333333331E-4,1.3524000000000001E-3,7.5370000000000006E-2,1.6920000000000001E-2,1.504E-2,5.334999999999999E-4,1.1843999999999999E-3,2.0913043478260874E-3,6.2750000000000014E-2,1.7220000000000003E-2]
["LVCMOS 2.5V 12mA (Slow)",2.5,1,6.5,0,0,0,0,0,0,0,1.504E-2,0,0,0,"LVCMOS25","LVCMOS25_12_SLOW",null,null,null,0,1.5586666666666664E-4,6.9653333333333331E-4,1.3524000000000001E-3,7.5370000000000006E-2,1.6920000000000001E-2,1.504E-2,1.5586666666666664E-4,6.9653333333333331E-4,1.3524000000000001E-3,7.5370000000000006E-2,1.6920000000000001E-2,1.504E-2,5.3680000000000004E-4,1.2859E-3,2.1252173913043483E-3,6.2750000000000014E-2,1.7210000000000003E-2]
["LVCMOS 2.5V 12mA (Fast)",2.5,1,6.5,0,0,0,0,0,0,0,1.504E-2,0,0,0,"LVCMOS25","LVCMOS25_12_FAST",null,null,null,0,1.5586666666666664E-4,6.9653333333333331E-4,1.3524000000000001E-3,7.5370000000000006E-2,1.6920000000000001E-2,1.504E-2,1.5586666666666664E-4,6.9653333333333331E-4,1.3524000000000001E-3,7.5370000000000006E-2,1.6920000000000001E-2,1.504E-2,5.3680000000000004E-4,1.2859E-3,2.1252173913043483E-3,6.2750000000000014E-2,1.7210000000000003E-2]
["LVCMOS 2.5V 16mA (Slow)",2.5,1,6.5,0,0,0,0,0,0,0,1.504E-2,0,0,0,"LVCMOS25","LVCMOS25_16_SLOW",null,null,null,0,1.5586666666666664E-4,6.9653333333333331E-4,1.3524000000000001E-3,7.5370000000000006E-2,1.6920000000000001E-2,1.504E-2,1.5586666666666664E-4,6.9653333333333331E-4,1.3524000000000001E-3,7.5370000000000006E-2,1.6920000000000001E-2,1.504E-2,7.0209999999999988E-4,1.9292000000000001E-3,2.2443478260869569E-3,6.2720000000000012E-2,1.7210000000000003E-2]
["LVCMOS 2.5V 16mA (Fast)",2.5,1,6.5,0,0,0,0,0,0,0,1.504E-2,0,0,0,"LVCMOS25","LVCMOS25_16_FAST",null,null,null,0,1.5586666666666664E-4,6.9653333333333331E-4,1.3524000000000001E-3,7.5370000000000006E-2,1.6920000000000001E-2,1.504E-2,1.5586666666666664E-4,6.9653333333333331E-4,1.3524000000000001E-3,7.5370000000000006E-2,1.6920000000000001E-2,1.504E-2,7.0209999999999988E-4,1.9292000000000001E-3,2.2443478260869569E-3,6.2720000000000012E-2,1.7210000000000003E-2]
["LVCMOS 3.3V 4mA (Slow)",{"$f":"VCCO33","v":3.3},1,6.5,0,0,0,0,0,0,0,1.5779999999999999E-2,0,0,0,"LVCMOS33","LVCMOS33_4_SLOW",null,null,null,0,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,7.405999999999999E-4,1.1930000000000001E-2,2.9913043478260871E-3,6.2740000000000004E-2,2.2679999999999999E-2]
["LVCMOS 3.3V 4mA (Fast)",3.3,1,6.5,0,0,0,0,0,0,0,1.5779999999999999E-2,0,0,0,"LVCMOS33","LVCMOS33_4_FAST",null,null,null,0,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,7.405999999999999E-4,1.1930000000000001E-2,2.9913043478260871E-3,6.2740000000000004E-2,2.2679999999999999E-2]
["LVCMOS 3.3V 8mA (Slow)",3.3,1,6.5,0,0,0,0,0,0,0,1.5779999999999999E-2,0,0,0,"LVCMOS33","LVCMOS33_8_SLOW",null,null,null,0,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,6.9439999999999997E-4,1.1670000000000002E-2,2.9965217391304351E-3,6.2750000000000014E-2,2.2679999999999999E-2]
["LVCMOS 3.3V 8mA (Fast)",3.3,1,6.5,0,0,0,0,0,0,0,1.5779999999999999E-2,0,0,0,"LVCMOS33","LVCMOS33_8_FAST",null,null,null,0,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,6.9439999999999997E-4,1.1670000000000002E-2,2.9965217391304351E-3,6.2750000000000014E-2,2.2679999999999999E-2]
["LVCMOS 3.3V 12mA (Slow)",3.3,1,6.5,0,0,0,0,0,0,0,1.5779999999999999E-2,0,0,0,"LVCMOS33","LVCMOS33_12_SLOW",null,null,null,0,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,5.7679999999999993E-4,1.2440000000000001E-2,2.9321739130434782E-3,6.2770000000000006E-2,2.2690000000000005E-2]
["LVCMOS 3.3V 12mA (Fast)",3.3,1,6.5,0,0,0,0,0,0,0,1.5779999999999999E-2,0,0,0,"LVCMOS33","LVCMOS33_12_FAST",null,null,null,0,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,5.7679999999999993E-4,1.2440000000000001E-2,2.9321739130434782E-3,6.2770000000000006E-2,2.2690000000000005E-2]
["LVCMOS 3.3V 16mA (Slow)",3.3,1,6.5,0,0,0,0,0,0,0,1.5779999999999999E-2,0,0,0,"LVCMOS33","LVCMOS33_16_SLOW",null,null,null,0,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,5.8120000000000003E-4,1.5689999999999999E-2,3.001739130434783E-3,6.2770000000000006E-2,2.2679999999999999E-2]
["LVCMOS 3.3V 16mA (Fast)",3.3,1,6.5,0,0,0,0,0,0,0,1.5779999999999999E-2,0,0,0,"LVCMOS33","LVCMOS33_16_FAST",null,null,null,0,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,5.8120000000000003E-4,1.5689999999999999E-2,3.001739130434783E-3,6.2770000000000006E-2,2.2679999999999999E-2]
["LVDS 2.5V (pair)",{"$f":"VCCO25","v":2.5},2,13,0,0,0,0.28999999999999998,0,0,14.3,1.6059E-2,{"$f":"B616*K616","v":35.75},26.65,0,"LVDS","LVDS_25",null,{"$f":"3.5*0.35","v":1.2249999999999999},null,0,4.742875E-4,2.637500000000015E-5,6.0499999999999791E-7,0.39779999999999999,1.2719,1.6059E-2,4.2725000000000006E-4,5.4124999999999865E-5,1.0037499999999978E-6,0.44026999999999999,1.6996,1.6059E-2,4.0999999999999999E-4,5.7999999999999996E-3,8.3870967741935505E-5,0,0]
["MINI LVDS 2.5V (pair)",{"$f":"VCCO25","v":2.5},2,13,0,0,0,0.28999999999999998,0,0,14.3,1.6059E-2,{"$f":"B617*K617","v":35.75},31.349999999999998,0,"LVDS","MINI_LVDS_25",null,{"$f":"3.5*0.45","v":1.575},null,0,4.7397500000000001E-4,2.5000000000000022E-5,7.8374999999999885E-7,0.39779999999999999,1.2719,1.6059E-2,4.2333749999999998E-4,6.9875000000000072E-5,5.8499999999999959E-7,0.44026999999999999,1.6996,1.6059E-2,4.0999999999999999E-4,5.7999999999999996E-3,8.3870967741935505E-5,0,0]
["LVPECL",2.5,2,6.5,0,0,0,0.28999999999999998,0,0,14.3,1.6059E-2,35.75,0,0,"LVDS","LVPECL",null,1.2249999999999999,null,0,4.742875E-4,2.637500000000015E-5,6.0499999999999791E-7,0.39779999999999999,1.2719,1.6059E-2,4.2725000000000006E-4,5.4124999999999865E-5,1.0037499999999978E-6,0.44026999999999999,1.6996,1.6059E-2,null,null,0]
["LVTTL 3.3V 4mA (Slow)",{"$f":"VCCO33","v":3.3},1,6.5,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS33","LVTTL_4_SLOW",null,null,null,0,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,6.2599999999999993E-4,1.2610000000000003E-2,2.8800000000000002E-3,6.2759999999999996E-2,2.2679999999999999E-2]
["LVTTL 3.3V 4mA (Fast)",3.3,1,6.5,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS33","LVTTL_4_FAST",null,null,null,0,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,6.2599999999999993E-4,1.2610000000000003E-2,2.8800000000000002E-3,6.2759999999999996E-2,2.2679999999999999E-2]
["LVTTL 3.3V 8mA (Slow)",3.3,1,6.5,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS33","LVTTL_8_SLOW",null,null,null,0,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,5.7919999999999998E-4,1.2580000000000001E-2,2.8956521739130435E-3,6.2770000000000006E-2,2.2679999999999999E-2]
["LVTTL 3.3V 8mA (Fast)",3.3,1,6.5,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS33","LVTTL_8_FAST",null,null,null,0,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,5.7919999999999998E-4,1.2580000000000001E-2,2.8956521739130435E-3,6.2770000000000006E-2,2.2679999999999999E-2]
["LVTTL 3.3V 12mA (Slow)",3.3,1,6.5,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS33","LVTTL_12_SLOW",null,null,null,0,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,5.8E-4,1.4520000000000002E-2,2.9217391304347832E-3,6.2770000000000006E-2,2.2679999999999999E-2]
["LVTTL 3.3V 12mA (Fast)",3.3,1,6.5,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS33","LVTTL_12_FAST",null,null,null,0,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,5.8E-4,1.4520000000000002E-2,2.9217391304347832E-3,6.2770000000000006E-2,2.2679999999999999E-2]
["LVTTL 3.3V 16mA (Slow)",3.3,1,6.5,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS33","LVTTL_16_SLOW",null,null,null,0,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,5.8120000000000003E-4,1.5689999999999999E-2,3.001739130434783E-3,6.2770000000000006E-2,2.2679999999999999E-2]
["LVTTL 3.3V 16mA (Fast)",3.3,1,6.5,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS33","LVTTL_16_FAST",null,null,null,0,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,1.5586666666666664E-4,8.0513333333333324E-4,2.7767999999999998E-3,7.5370000000000006E-2,2.0930000000000001E-2,1.5779999999999999E-2,5.8120000000000003E-4,1.5689999999999999E-2,3.001739130434783E-3,6.2770000000000006E-2,2.2679999999999999E-2]
["PPDS 2.5V (pair)",{"$f":"VCCO25","v":2.5},2,13,0,0,0,0.28999999999999998,0,0,14.3,3.4542000000000003E-2,{"$f":"B627*K627","v":35.75},15.824999999999999,0,"LVDS","PPDS_25",null,{"$f":"3.5*0.25","v":0.875},null,0,4.6906250000000002E-4,2.8249999999999941E-5,3.1250000000000892E-8,0.39779999999999999,1.6129,3.4542000000000003E-2,3.3684999999999992E-4,1.3299999999999979E-4,2.3133750000000002E-5,0.50934000000000001,2.1812,3.4542000000000003E-2,4.0999999999999999E-4,5.7999999999999996E-3,8.3870967741935505E-5,0,0]
["RSDS 2.5V (pair)",{"$f":"VCCO25","v":2.5},2,13,0,0,0,0.28999999999999998,0,0,14.3,3.4542000000000003E-2,{"$f":"B628*K628","v":35.75},31.349999999999998,0,"LVDS","RSDS_25",null,{"$f":"3.5*0.35","v":1.2249999999999999},null,0,4.6906250000000002E-4,2.8249999999999941E-5,3.1250000000000892E-8,0.39779999999999999,1.6129,3.4542000000000003E-2,3.3684999999999992E-4,1.3299999999999979E-4,2.3133750000000002E-5,0.50934000000000001,2.1812,3.4542000000000003E-2,4.0999999999999999E-4,5.7999999999999996E-3,8.3870967741935505E-5,0,0]
["SSTL 1.2V",1.2,1,6.5,0,0,0,1,0.77500000000000002,0.42499999999999999,3.7,0,2.1,5.8092000000000015,0,"HSTL","SSTL12",null,null,null,0,1.5052500000000004E-4,4.2125000000000082E-5,6.7499999999998117E-6,0.40894000000000003,1.4779,6.25,2.8171249999999994E-4,5.0250000000000015E-5,7.0000000000003396E-6,0.76141999999999999,2.0613999999999999,6.25,5.602999999999999E-4,6.1149999999999998E-3,5.3133333333333331E-4,6.2579999999999997E-2,1.3649999999999999E-3]
["SSTL 1.35V",{"$f":"VCCO135","v":1.35},3,6.5,0,0,0,1,0.85,0.5,2.07E-2,0,{"$f":"B630*(I630-J630)/200*1000","v":2.3624999999999998},6.6123000000000003,0,"HSTL","SSTL135",null,null,6.75,0,1.8487500000000003E-4,3.762500000000002E-5,3.5000000000007246E-6,0.37861,1.5058,7.03125,2.3621249999999998E-4,4.8374999999999943E-5,3.5000000000007246E-6,0.72119,2.0863999999999998,7.03125,5.1040000000000005E-4,5.3870000000000003E-3,3.2066666666666669E-4,6.2570000000000001E-2,1.3709999999999998E-3]
["SSTL 1.35V R",{"$f":"VCCO135","v":1.35},3,6.5,0,0,0,1,0.75,0.6,1.6799999999999999E-2,0,{"$f":"B631*(I631-J631)/200*1000","v":1.0125000000000002},6.6123000000000003,0,"HSTL","SSTL135_R",null,null,6.75,0,1.8487500000000003E-4,3.762500000000002E-5,3.5000000000007246E-6,0.37861,1.5058,7.03125,2.3621249999999998E-4,4.8374999999999943E-5,3.5000000000007246E-6,0.72119,2.0863999999999998,7.03125,3.6539999999999999E-4,2.5840000000000004E-3,4.4333333333333329E-4,6.2550000000000008E-2,1.353E-3]
["SSTL 1.5V",{"$f":"VCCO15","v":1.5},3,6.5,0,0,0,1,0.92500000000000004,0.57499999999999996,2.07E-2,0,{"$f":"B632*(I632-J632)/200*1000","v":2.6250000000000004},7.9320000000000004,0,"HSTL","SSTL15",null,null,7.5,0,2.0825000000000002E-4,3.4750000000000059E-5,4.1249999999992685E-6,0.35666999999999999,1.52,7.8125,1.153499999999999E-4,5.8124999999999983E-5,2.874999999999961E-6,0.62117999999999995,2.0926999999999998,7.8125,5.5340000000000001E-4,6.0669999999999995E-3,4.0577777777777774E-4,6.2560000000000004E-2,1.361E-3]
["SSTL 1.5V R",{"$f":"VCCO15","v":1.5},3,6.5,0,0,0,1,0.82499999999999996,0.67500000000000004,1.6799999999999999E-2,0,{"$f":"B633*(I633-J633)/200*1000","v":1.1249999999999993},7.9320000000000004,0,"HSTL","SSTL15_R",null,null,7.5,0,2.0825000000000002E-4,3.4750000000000059E-5,4.1249999999992685E-6,0.35666999999999999,1.52,7.8125,1.153499999999999E-4,5.8124999999999983E-5,2.874999999999961E-6,0.62117999999999995,2.0926999999999998,7.8125,3.1509999999999996E-4,1.825E-3,4.4833333333333335E-4,6.2530000000000016E-2,1.3449999999999998E-3]
["SSTL Class I 1.8V",{"$f":"VCCO18","v":1.8},3,6.5,0,0,0,0.45,1.37,0.43,4.7,0,{"$f":"B634*(I634-J634)/200*1000","v":8.4600000000000026},10.245600000000001,0,"HSTL","SSTL18_I",null,null,9,0,2.4548749999999992E-4,2.8249999999999941E-5,2.500000000000835E-6,0.32567000000000002,1.4826999999999999,9.375,1.5999999999999993E-4,6.4250000000000139E-5,2.500000000000835E-6,0.39582000000000001,2.0152000000000001,9.375,3.1829999999999998E-4,1.776E-3,3.6688888888888887E-4,6.2539999999999998E-2,1.3540000000000002E-3]
["SSTL Class II 1.8V",{"$f":"VCCO18","v":1.8},3,6.5,0,0,0,0.45,1.5,0.3,8.1,0,{"$f":"B635*(I635-J635)/100*1000","v":21.6},10.245600000000001,0,"HSTL","SSTL18_II",null,null,9,0,2.4548749999999992E-4,2.8249999999999941E-5,2.500000000000835E-6,0.32567000000000002,1.4826999999999999,9.375,1.5999999999999993E-4,6.4250000000000139E-5,2.500000000000835E-6,0.39582000000000001,2.0152000000000001,9.375,5.0589999999999999E-4,5.594E-3,5.0477777777777771E-4,6.2550000000000008E-2,1.361E-3]
["SLVS 400 2.5V",2.5,2,6.5,0,0,0,0.28999999999999998,0,0,14.3,1.6126999999999999E-2,35.75,0,0,"LVDS","SLVS_400_25",null,null,null,0,2.7884999999999992E-4,3.3749999999999614E-5,2.4999999999938268E-9,0.75727,1.5407999999999999,1.6126999999999999E-2,3.9917499999999993E-4,3.7249999999999781E-5,3.7500000000002811E-8,0.81859999999999999,2.1526999999999998,1.6126999999999999E-2,null,null,0]
["SUB_LVDS (pair)",1.8,2,13,0,0,0,0.28999999999999998,0,0,14.3,1.6080000000000001E-2,35.75,10.720800000000001,0,"LVDS","SUB_LVDS",null,1.2249999999999999,null,0,4.687375E-4,1.2500000000000011E-5,1.1999999999999989E-6,0.39779999999999999,1.6129,1.6080000000000001E-2,3.549375E-4,4.4750000000000065E-5,1.3487500000000002E-6,0.49259999999999998,2.1442999999999999,1.6080000000000001E-2,4.0999999999999999E-4,5.7999999999999996E-3,8.3870967741935505E-5,0,0]
["TMDS 3.3V (pair)",{"$f":"VCCO33","v":3.3},2,13,0,0,0,0.28999999999999998,0,0,14.3,6.5533000000000001,{"$f":"B638*K638","v":47.19},0,0,"LVDS","TMDS_33",null,{"$f":"3.5*0.6","v":2.1},null,0,3.3167500000000019E-4,0,0,0.75931000000000004,0.16965,6.5533000000000001,3.3167500000000019E-4,0,0,0.75931000000000004,0.16965,6.5533000000000001,4.0999999999999999E-4,3.2599999999999999E-3,0,0,0]
[]
["HP Bank",1,2,3,"Output","Input","DCI",7,8,9,"Static Output Current","Static Input Current","Static Power","Output on-chip static power","Input on-chip static power",15]
["IO_STANDARD","Vcco","Type","Internal","Iccaux","Iccauxq","Bank mA","DIFFAMP","Voh","Vol","mA","mA","mW","mW",null,"IBUF","MAP Name",null,null,null,"DCI InTerm mA"]
["Diff HSTL Class I 1.5V (pair)",{"$f":"VCCO15","v":1.5},1,6.2,0,0,0,1,1.1000000000000001,0.4,9.6,0,10.5,14.0625,0,"LVDS","DIFF_HSTL_I",null,null,null,0,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,18.75,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,18.75,1.5602437880918893E-3,2.1340834505391468E-2,4.5373468914862783E-4,0,0.31900000000000001]
["Diff HSTL Class I DCI 1.5V (pair)",{"$f":"VCCO15","v":1.5},1,6.2,0,0,0,1,1.1000000000000001,0.4,9.4,9.375,{"$f":"B643*K643","v":14.100000000000001},14.0625,0,"LVDS","DIFF_HSTL_I_DCI",null,null,null,18.75,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,18.75,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,18.75,1.5602437880918893E-3,2.0590717299578058E-2,4.3756837005782162E-4,0,0.31900000000000001]
["Diff HSTL Class I 1.2V (pair)",1.5,1,6.2,0,0,0,1,1.1000000000000001,0.4,9.6,0,10.5,11.25,0,"LVDS","DIFF_HSTL_I_12",null,null,null,0,4.7899999999999999E-4,1.9800000000000001E-6,0,0.51800000000000002,1.7,15,3.9599999999999998E-4,1.2549E-5,0,0.73816899999999996,2.919,15,1.5459662288930586E-3,2.1388367729831145E-2,4.0758232516012157E-4,0,0.31900000000000001]
["Diff HSTL Class I DCI 1.2V (pair)",1.5,1,6.2,0,0,0,1,1.1000000000000001,0.4,9.4,7.5,14.100000000000001,11.25,0,"LVDS","DIFF_HSTL_I_DCI_12",null,null,null,15,4.7899999999999999E-4,1.9800000000000001E-6,0,0.51800000000000002,1.7,15,3.9599999999999998E-4,1.2549E-5,0,0.73816899999999996,2.919,15,1.5459662288930586E-3,2.2626641651031894E-2,3.9679972396540941E-4,0,0.31900000000000001]
["Diff HSTL Class I 1.8V (pair)",{"$f":"VCCO18","v":1.8},1,6.2,0,0,0,1,1.4,0.4,11.6,0,18,20.25,0,"LVDS","DIFF_HSTL_I_18",null,null,null,0,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,22.5,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,22.5,1.5399999999999993E-3,2.2099999999999998E-2,6.2931034482758609E-4,0,0.31900000000000001]
["Diff HSTL Class I DCI 1.8V (pair)",{"$f":"VCCO18","v":1.8},1,6.2,0,0,0,1,1.4,0.4,10.8,11.25,19.440000000000001,20.25,0,"LVDS","DIFF_HSTL_I_DCI_18",null,null,null,22.5,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,22.5,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,22.5,1.5399999999999993E-3,2.1350000000000001E-2,6.0919540229885047E-4,0,0.31900000000000001]
["Diff HSUL 1.2V (pair)",{"$f":"VCCO12","v":1.2},1,6.2,0,0,0,1,0.96,0.24,0,0,{"$f":"2*M670","v":0},0,0,"LVDS","DIFF_HSUL_12",null,null,null,0,4.7899999999999999E-4,1.9800000000000001E-6,0,0.51800000000000002,1.7,0,3.9599999999999998E-4,1.2549E-5,0,0.73816899999999996,2.919,0,1.5459662288930586E-3,2.1388367729831145E-2,4.0758232516012157E-4,0,0.31900000000000001]
["Diff HSUL DCI 1.2V (pair)",{"$f":"VCCO12","v":1.2},1,6.2,0,0,0,1,0.96,0.24,3.7,0,{"$f":"2*M671","v":10.8},0,0,"LVDS","DIFF_HSUL_12_DCI",null,null,null,0,4.7899999999999999E-4,1.9800000000000001E-6,0,0.51800000000000002,1.7,0,3.9599999999999998E-4,1.2549E-5,0,0.73816899999999996,2.919,0,1.5459662288930586E-3,2.2626641651031894E-2,3.9679972396540941E-4,0,0.31900000000000001]
["Diff POD 1.0V (pair)",{"$f":"VCCO10","v":1},1,6.2,0,0,0,1,0.77500000000000002,0.42499999999999999,11.86,0,10.5,0,0,"LVDS","DIFF_POD10",null,null,null,0,5.1999999999999995E-4,4.2000000000000004E-6,0,0.51700000000000002,1.6579999999999999,12.5,4.5800000000000002E-4,3.5480000000000002E-6,0,0.73882999999999999,2.8530000000000002,12.5,1.2133333333333334E-3,2.1466666666666669E-2,3.0651340996168587E-4,0,0.31900000000000001]
["Diff POD DCI 1.0V (pair)",{"$f":"VCCO10","v":1},3,6.2,0,0,0,1,0.77500000000000002,0.42499999999999999,11.86,6.25,10.5,0,0,"LVDS","DIFF_POD10_DCI",null,null,10,12.5,5.1999999999999995E-4,4.2000000000000004E-6,0,0.51700000000000002,1.6579999999999999,12.5,4.5800000000000002E-4,3.5480000000000002E-6,0,0.73882999999999999,2.8530000000000002,12.5,1.2133333333333334E-3,2.23E-2,2.9118773946360156E-4,0,0.31900000000000001]
["Diff POD 1.2V (pair)",{"$f":"VCCO12","v":1.2},1,6.2,0,0,0,1,0.77500000000000002,0.42499999999999999,11.86,0,10.5,0,0,"LVDS","DIFF_POD12",null,null,null,0,5.2899999999999996E-4,2.2000000000000001E-6,0,0.51600000000000001,1.617,15,4.5800000000000002E-4,1.0900000000000001E-5,0,0.74446000000000001,2.7549999999999999,15,1.5358080239970006E-3,2.1717285339332586E-2,3.6374763499390163E-4,0,0.31900000000000001]
["Diff POD DCI 1.2V (pair)",1.2,3,6.2,0,0,0,1,0.77500000000000002,0.42499999999999999,11.86,7.5,10.5,0,0,"LVDS","DIFF_POD12_DCI",null,null,12,15,5.2899999999999996E-4,2.2000000000000001E-6,0,0.51600000000000001,1.617,15,4.5800000000000002E-4,1.0900000000000001E-5,0,0.74446000000000001,2.7549999999999999,15,1.5358080239970006E-3,2.2617172853393326E-2,3.4478448814587837E-4,0,0.31900000000000001]
["Diff SSTL 1.2V (pair)",{"$f":"VCCO12","v":1.2},1,6.2,0,0,0,1,0.77500000000000002,0.42499999999999999,11.86,0,10.5,9,0,"LVDS","DIFF_SSTL12",null,null,null,0,4.7899999999999999E-4,1.9800000000000001E-6,0,0.51800000000000002,1.7,15,3.9599999999999998E-4,1.2549E-5,0,0.73816899999999996,2.919,15,1.5459662288930586E-3,2.1388367729831145E-2,4.0758232516012157E-4,0,0.31900000000000001]
["Diff SSTL DCI 1.2V (pair)",{"$f":"VCCO12","v":1.2},3,6.2,0,0,0,1,0.77500000000000002,0.42499999999999999,11.86,7.5,10.5,9,0,"LVDS","DIFF_SSTL12_DCI",null,null,12,15,4.7899999999999999E-4,1.9800000000000001E-6,0,0.51800000000000002,1.7,15,3.9599999999999998E-4,1.2549E-5,0,0.73816899999999996,2.919,15,1.5459662288930586E-3,2.2626641651031894E-2,3.9679972396540941E-4,0,0.31900000000000001]
["Diff SSTL 1.35V (pair)",{"$f":"VCCO135","v":1.35},1,6.2,0,0,0,1,0.85,0.5,11.86,0,10.5,11.390625,0,"LVDS","DIFF_SSTL135",null,null,null,0,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,16.875,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,16.875,1.5605573419078245E-3,2.1178992497320474E-2,4.3365241280752972E-4,0,0.31900000000000001]
["Diff SSTL DCI 1.35V (pair)",{"$f":"VCCO135","v":1.35},3,6.2,0,0,0,1,0.85,0.5,11.86,8.4375,10.5,11.390625,0,"LVDS","DIFF_SSTL135_DCI",null,null,13.5,16.875,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,16.875,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,16.875,1.5605573419078245E-3,2.2465166130760987E-2,4.1517290657993623E-4,0,0.31900000000000001]
["Diff SSTL 1.5V (pair)",{"$f":"VCCO15","v":1.5},1,6.2,0,0,0,1,0.92500000000000004,0.57499999999999996,11.86,0,10.5,14.0625,0,"LVDS","DIFF_SSTL15",null,null,null,0,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,18.75,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,18.75,1.5602437880918893E-3,2.1340834505391468E-2,4.5373468914862783E-4,0,0.31900000000000001]
["Diff SSTL DCI 1.5V (pair)",{"$f":"VCCO15","v":1.5},3,6.2,0,0,0,1,0.92500000000000004,0.57499999999999996,11.86,9.375,10.5,14.0625,0,"LVDS","DIFF_SSTL15_DCI",null,null,15,18.75,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,18.75,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,18.75,1.5602437880918893E-3,2.0590717299578058E-2,4.3756837005782162E-4,0,0.31900000000000001]
["Diff SSTL Class I 1.8V (pair)",{"$f":"VCCO18","v":1.8},1,6.2,0,0,0,1,1.37,0.43,9.4,0,13.68,20.25,0,"LVDS","DIFF_SSTL18_I",null,null,null,0,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,22.5,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,22.5,1.5399999999999993E-3,2.2099999999999998E-2,6.2931034482758609E-4,0,0.31900000000000001]
["Diff SSTL Class I DCI 1.8V (pair)",{"$f":"VCCO18","v":1.8},1,6.2,0,0,0,1,1.37,0.43,9.4,11.25,{"$f":"B661*K661","v":16.920000000000002},20.25,0,"LVDS","DIFF_SSTL18_I_DCI",null,null,null,22.5,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,22.5,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,22.5,1.5399999999999993E-3,2.1350000000000001E-2,6.0919540229885047E-4,0,0.31900000000000001]
["HSLV DCI 1.5V",{"$f":"VCCO15","v":1.5},1,3.1,0,0,0,0,0.92500000000000004,0.57499999999999996,4.8,0,{"$f":"B662*(I662-J662)/200*1000","v":2.6250000000000004},0,0,"HSTL","HSLVDCI_15",null,null,null,0,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,0,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,0,7.8012189404594464E-4,1.0295358649789029E-2,3.398968588842007E-4,0,0.1595]
["HSLV DCI 1.8V",{"$f":"VCCO18","v":1.8},1,3.1,0,0,0,0,1.37,0.43,5.8,0,{"$f":"B663*(I663-J663)/200*1000","v":8.4600000000000026},0,0,"HSTL","HSLVDCI_18",null,null,null,0,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,11.25,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,0,7.6999999999999963E-4,1.0675E-2,4.7321428571428558E-4,0,0.1595]
["HSTL Class I 1.5V",{"$f":"VCCO15","v":1.5},1,3.1,0,0,0,1,1.1000000000000001,0.4,4.8,0,{"$f":"B664*(I664-J664)/200*1000","v":5.25},7.03125,0,"HSTL","HSTL_I",null,null,null,0,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,9.375,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,9.375,7.8012189404594464E-4,1.0670417252695734E-2,3.5245462460652339E-4,0,0.1595]
["HSTL Class I 1.2V",{"$f":"VCCO12","v":1.2},1,3.1,0,0,0,1,0.9,0.32,3.7,0,{"$f":"B665*(I665-J665)/200*1000","v":3.4800000000000004},4.5,0,"HSTL","HSTL_I_12",null,null,null,0,4.7899999999999999E-4,1.9800000000000001E-6,0,0.51800000000000002,1.7,7.5,3.9599999999999998E-4,1.2549E-5,0,0.73816899999999996,2.919,7.5,7.7298311444652928E-4,1.0694183864915573E-2,3.1660412757973731E-4,0,0.1595]
["HSTL Class I 1.8V",{"$f":"VCCO18","v":1.8},1,3.1,0,0,0,1,1.4,0.4,5.8,0,{"$f":"B666*(I666-J666)/200*1000","v":9},10.125,0,"HSTL","HSTL_I_18",null,null,null,0,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,11.25,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,11.25,7.6999999999999963E-4,1.1049999999999999E-2,4.888392857142857E-4,0,0.1595]
["HSTL Class I DCI 1.5V",{"$f":"VCCO15","v":1.5},1,3.1,0,0,0,1,1.1000000000000001,0.4,4.7,9.375,{"$f":"(B667^2/200 +B667/200*(I667-J667))*1000","v":16.5},7.03125,0,"HSTL","HSTL_I_DCI",null,null,null,9.375,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,9.375,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,9.375,7.8012189404594464E-4,1.0295358649789029E-2,3.398968588842007E-4,0,0.1595]
["HSTL Class I DCI 1.2V",{"$f":"VCCO15","v":1.5},1,3.1,0,0,0,1,1.1000000000000001,0.4,4.7,7.5,{"$f":"(B668^2/200 +B668/200*(I668-J668))*1000","v":16.5},5.625,0,"HSTL","HSTL_I_DCI_12",null,null,null,7.5,4.7899999999999999E-4,1.9800000000000001E-6,0,0.51800000000000002,1.7,7.5,3.9599999999999998E-4,1.2549E-5,0,0.73816899999999996,2.919,7.5,7.7298311444652928E-4,1.1313320825515947E-2,3.0822835700884481E-4,0,0.1595]
["HSTL Class I DCI 1.8V",{"$f":"VCCO18","v":1.8},1,3.1,0,0,0,1,1.4,0.4,5.4,11.25,{"$f":"(B669^2/200 +B669/200*(I669-J669))*1000","v":25.2},10.125,0,"HSTL","HSTL_I_DCI_18",null,null,null,11.25,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,11.25,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,11.25,7.6999999999999963E-4,1.0675E-2,4.7321428571428558E-4,0,0.1595]
["HSUL 1.2V",{"$f":"VCCO12","v":1.2},1,3.1,0,0,0,1,0.96,0.24,null,0,0,0,0,"HSTL","HSUL_12",null,null,null,0,4.7899999999999999E-4,1.9800000000000001E-6,0,0.51800000000000002,1.7,0,3.9599999999999998E-4,1.2549E-5,0,0.73816899999999996,2.919,0,7.7298311444652928E-4,1.0694183864915573E-2,3.1660412757973731E-4,0,0.1595]
["HSUL DCI 1.2V",{"$f":"VCCO12","v":1.2},1,3.1,0,0,0,1,0.96,0.24,3.7,0,{"$f":"B671*(I671-J671)/160*1000","v":5.4},0,0,"HSTL","HSUL_12_DCI",null,null,null,0,4.7899999999999999E-4,1.9800000000000001E-6,0,0.51800000000000002,1.7,0,3.9599999999999998E-4,1.2549E-5,0,0.73816899999999996,2.919,0,7.7298311444652928E-4,1.1313320825515947E-2,3.0822835700884481E-4,0,0.1595]
["LVCMOS 1.2V 2mA (Slow)",{"$f":"VCCO12","v":1.2},1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS12","LVCMOS12_2_SLOW",null,null,null,0,1.493E-3,0,1.2899999999999999E-4,0,0,0,1.493E-3,0,1.2899999999999999E-4,0,0,0,6.3999999999999767E-4,4.2671999999999996E-3,9.9753086419753097E-4,0,0.1595]
["LVCMOS 1.2V 2mA (Fast)",1.2,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS12","LVCMOS12_2_FAST",null,null,null,0,1.493E-3,0,1.2899999999999999E-4,0,0,0,1.493E-3,0,1.2899999999999999E-4,0,0,0,6.3999999999999767E-4,4.2671999999999996E-3,9.9753086419753097E-4,0,0.1595]
["LVCMOS 1.2V 4mA (Slow)",1.2,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS12","LVCMOS12_4_SLOW",null,null,null,0,1.493E-3,0,1.2899999999999999E-4,0,0,0,1.493E-3,0,1.2899999999999999E-4,0,0,0,6.4000000000000341E-4,6.8319999999999995E-3,1.0567901234567901E-3,0,0.1595]
["LVCMOS 1.2V 4mA (Fast)",1.2,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS12","LVCMOS12_4_FAST",null,null,null,0,1.493E-3,0,1.2899999999999999E-4,0,0,0,1.493E-3,0,1.2899999999999999E-4,0,0,0,6.4000000000000341E-4,6.8319999999999995E-3,1.0567901234567901E-3,0,0.1595]
["LVCMOS 1.2V 6mA (Slow)",1.2,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS12","LVCMOS12_6_SLOW",null,null,null,0,1.493E-3,0,1.2899999999999999E-4,0,0,0,1.493E-3,0,1.2899999999999999E-4,0,0,0,6.3999999999999767E-4,1.0303999999999999E-2,1.0567901234567901E-3,0,0.1595]
["LVCMOS 1.2V 6mA (Fast)",1.2,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS12","LVCMOS12_6_FAST",null,null,null,0,1.493E-3,0,1.2899999999999999E-4,0,0,0,1.493E-3,0,1.2899999999999999E-4,0,0,0,6.3999999999999767E-4,1.0303999999999999E-2,1.0567901234567901E-3,0,0.1595]
["LVCMOS 1.2V 8mA (Slow)",1.2,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS12","LVCMOS12_8_SLOW",null,null,null,0,1.493E-3,0,1.2899999999999999E-4,0,0,0,1.493E-3,0,1.2899999999999999E-4,0,0,0,6.7199999999999985E-4,1.2655999999999999E-2,1.0666666666666667E-3,0,0.1595]
["LVCMOS 1.2V 8mA (Fast)",1.2,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS12","LVCMOS12_8_FAST",null,null,null,0,1.493E-3,0,1.2899999999999999E-4,0,0,0,1.493E-3,0,1.2899999999999999E-4,0,0,0,6.7199999999999985E-4,1.2655999999999999E-2,1.0666666666666667E-3,0,0.1595]
["LVCMOS 1.5V 2mA (Slow)",{"$f":"VCCO15","v":1.5},1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS15","LVCMOS15_2_SLOW",null,null,null,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,6.3999999999999767E-4,4.3568000000000001E-3,1.2444444444444445E-3,0,0.1595]
["LVCMOS 1.5V 2mA (Fast)",1.5,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS15","LVCMOS15_2_FAST",null,null,null,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,6.3999999999999767E-4,4.3568000000000001E-3,1.2444444444444445E-3,0,0.1595]
["LVCMOS 1.5V 4mA (Slow)",1.5,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS15","LVCMOS15_4_SLOW",null,null,null,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,6.4000000000000341E-4,7.0559999999999998E-3,1.3135802469135802E-3,0,0.1595]
["LVCMOS 1.5V 4mA (Fast)",1.5,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS15","LVCMOS15_4_FAST",null,null,null,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,6.4000000000000341E-4,7.0559999999999998E-3,1.3135802469135802E-3,0,0.1595]
["LVCMOS 1.5V 6mA (Slow)",1.5,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS15","LVCMOS15_6_SLOW",null,null,null,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,6.3999999999999767E-4,1.064E-2,1.3234567901234569E-3,0,0.1595]
["LVCMOS 1.5V 6mA (Fast)",1.5,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS15","LVCMOS15_6_FAST",null,null,null,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,6.3999999999999767E-4,1.064E-2,1.3234567901234569E-3,0,0.1595]
["LVCMOS 1.5V 8mA (Slow)",1.5,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS15","LVCMOS15_8_SLOW",null,null,null,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,6.7199999999999985E-4,1.3551999999999998E-2,1.3234567901234569E-3,0,0.1595]
["LVCMOS 1.5V 8mA (Fast)",1.5,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS15","LVCMOS15_8_FAST",null,null,null,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,6.7199999999999985E-4,1.3551999999999998E-2,1.3234567901234569E-3,0,0.1595]
["LVCMOS 1.5V 12mA (Slow)",1.5,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS15","LVCMOS15_12_SLOW",null,null,null,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,7.0399999999999998E-4,1.848E-2,1.3333333333333335E-3,0,0.1595]
["LVCMOS 1.5V 12mA (Fast)",1.5,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS15","LVCMOS15_12_FAST",null,null,null,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,1.493E-3,0,2.7300000000000002E-4,0,0,0,7.0399999999999998E-4,1.848E-2,1.3333333333333335E-3,0,0.1595]
["LVCMOS 1.8V 2mA (Slow)",{"$f":"VCCO18","v":1.8},1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS18","LVCMOS18_2_SLOW",null,null,null,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,6.3999999999999767E-4,4.3568000000000001E-3,1.4913580246913583E-3,0,0.1595]
["LVCMOS 1.8V 2mA (Fast)",1.8,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS18","LVCMOS18_2_FAST",null,null,null,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,6.3999999999999767E-4,4.3568000000000001E-3,1.4913580246913583E-3,0,0.1595]
["LVCMOS 1.8V 4mA (Slow)",1.8,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS18","LVCMOS18_4_SLOW",null,null,null,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,6.4000000000000341E-4,7.0559999999999998E-3,1.5703703703703704E-3,0,0.1595]
["LVCMOS 1.8V 4mA (Fast)",1.8,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS18","LVCMOS18_4_FAST",null,null,null,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,6.4000000000000341E-4,7.0559999999999998E-3,1.5703703703703704E-3,0,0.1595]
["LVCMOS 1.8V 6mA (Slow)",1.8,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS18","LVCMOS18_6_SLOW",null,null,null,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,6.3999999999999767E-4,1.0864E-2,1.580246913580247E-3,0,0.1595]
["LVCMOS 1.8V 6mA (Fast)",1.8,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS18","LVCMOS18_6_FAST",null,null,null,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,6.3999999999999767E-4,1.0864E-2,1.580246913580247E-3,0,0.1595]
["LVCMOS 1.8V 8mA (Slow)",1.8,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS18","LVCMOS18_8_SLOW",null,null,null,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,6.7199999999999985E-4,1.3103999999999999E-2,1.580246913580247E-3,0,0.1595]
["LVCMOS 1.8V 8mA (Fast)",1.8,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS18","LVCMOS18_8_FAST",null,null,null,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,6.7199999999999985E-4,1.3103999999999999E-2,1.580246913580247E-3,0,0.1595]
["LVCMOS 1.8V 12mA (Slow)",1.8,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS18","LVCMOS18_12_SLOW",null,null,null,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,7.0399999999999998E-4,1.8815999999999999E-2,1.5901234567901237E-3,0,0.1595]
["LVCMOS 1.8V 12mA (Fast)",1.8,1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS18","LVCMOS18_12_FAST",null,null,null,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,1.493E-3,0,5.6099999999999998E-4,0,0,0,7.0399999999999998E-4,1.8815999999999999E-2,1.5901234567901237E-3,0,0.1595]
["LVDCI 1.5V",{"$f":"VCCO15","v":1.5},1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS15","LVDCI_15",null,null,null,0,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,0,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,0,7.8012189404594464E-4,1.0295358649789029E-2,3.398968588842007E-4,0,0.1595]
["LVDCI 1.8V",{"$f":"VCCO18","v":1.8},1,3.1,0,0,0,0,0,0,0,0,0,0,0,"LVCMOS18","LVDCI_18",null,null,null,0,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,11.25,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,0,7.6999999999999963E-4,1.1049999999999999E-2,4.888392857142857E-4,0,0.1595]
["LVDS 1.8V (pair)",{"$f":"VCCO18","v":1.8},2,6.2,0,0,0,1,0,0,{"$f":"9.2/LVDS_SCALE","v":9.1999999999999993},0,{"$f":"B702*K702","v":16.559999999999999},16.920000000000002,0,"LVDS","LVDS",null,{"$f":"3.5*0.35","v":1.2249999999999999},null,0,1.3929999999999999E-3,5.9757999999999999E-5,0,0.35320200000000002,1.2370000000000001,0,1.3940000000000001E-3,9.5084999999999988E-5,0,0.35317300000000001,2.3370000000000002,0,7.5000000000000002E-4,2.6099999999999999E-3,1.4942528735632186E-4,0,0.31]
["POD 1.0V",{"$f":"VCCO10","v":1},1,3.1,0,0,0,1,0.77500000000000002,0.42499999999999999,5.93,0,{"$f":"B703*(I703-J703)/200*1000","v":1.7500000000000002},0,0,"SSTL15","POD10",null,null,null,0,5.1999999999999995E-4,4.2000000000000004E-6,0,0.51700000000000002,1.6579999999999999,6.25,4.5800000000000002E-4,3.5480000000000002E-6,0,0.73882999999999999,2.8530000000000002,6.25,6.066666666666667E-4,1.0733333333333334E-2,2.3809523809523815E-4,0,0.1595]
["POD DCI 1.0V",{"$f":"VCCO10","v":1},3,3.1,0,0,0,1,0.77500000000000002,0.42499999999999999,5.93,6.25,1.7500000000000002,0,0,"SSTL15","POD10_DCI",null,null,5,6.25,5.1999999999999995E-4,4.2000000000000004E-6,0,0.51700000000000002,1.6579999999999999,6.25,4.5800000000000002E-4,3.5480000000000002E-6,0,0.73882999999999999,2.8530000000000002,6.25,6.066666666666667E-4,1.115E-2,2.2619047619047618E-4,0,0.1595]
["POD 1.2V",{"$f":"VCCO12","v":1.2},1,3.1,0,0,0,1,0.77500000000000002,0.42499999999999999,5.93,0,2.1,0,0,"SSTL15","POD12",null,null,null,0,5.2899999999999996E-4,2.2000000000000001E-6,0,0.51600000000000001,1.617,7.5,4.5800000000000002E-4,1.0900000000000001E-5,0,0.74446000000000001,2.7549999999999999,7.5,7.6790401199850031E-4,1.0858642669666293E-2,2.8255396646847714E-4,0,0.1595]
["POD DCI 1.2V",1.2,3,3.1,0,0,0,1,0.77500000000000002,0.42499999999999999,5.93,7.5,2.1,0,0,"SSTL15","POD12_DCI",null,null,6,7.5,5.2899999999999996E-4,2.2000000000000001E-6,0,0.51600000000000001,1.617,7.5,4.5800000000000002E-4,1.0900000000000001E-5,0,0.74446000000000001,2.7549999999999999,7.5,7.6790401199850031E-4,1.1308586426696663E-2,2.6782366489903051E-4,0,0.1595]
["SSTL 1.2V",1.2,1,3.1,0,0,0,1,0.77500000000000002,0.42499999999999999,3.7,0,2.1,4.5,0,"HSTL","SSTL12",null,null,null,0,4.7899999999999999E-4,1.9800000000000001E-6,0,0.51800000000000002,1.7,7.5,3.9599999999999998E-4,1.2549E-5,0,0.73816899999999996,2.919,7.5,7.7298311444652928E-4,1.0694183864915573E-2,3.1660412757973731E-4,0,0.1595]
["SSTL DCI 1.2V",1.2,3,3.1,0,0,0,1,0.77500000000000002,0.42499999999999999,3.7,7.5,2.1,4.5,0,"HSTL","SSTL12_DCI",null,null,6,7.5,4.7899999999999999E-4,1.9800000000000001E-6,0,0.51800000000000002,1.7,7.5,3.9599999999999998E-4,1.2549E-5,0,0.73816899999999996,2.919,7.5,7.7298311444652928E-4,1.1313320825515947E-2,3.0822835700884481E-4,0,0.1595]
["SSTL 1.35V",{"$f":"VCCO135","v":1.35},1,3.1,0,0,0,1,0.85,0.5,5.93,0,2.3624999999999998,5.6953125,0,"SSTL15","SSTL135",null,null,null,0,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,8.4375,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,8.4375,7.8027867095391225E-4,1.0589496248660237E-2,3.368549992344204E-4,0,0.1595]
["SSTL DCI 1.35V",{"$f":"VCCO135","v":1.35},3,3.1,0,0,0,1,0.85,0.5,5.93,8.4375,2.3624999999999998,5.6953125,0,"SSTL15","SSTL135_DCI",null,null,6.75,8.4375,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,8.4375,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,8.4375,7.8027867095391225E-4,1.1232583065380494E-2,3.2250038278977186E-4,0,0.1595]
["SSTL 1.5V",{"$f":"VCCO15","v":1.5},1,3.1,0,0,0,1,0.92500000000000004,0.57499999999999996,5.93,0,2.6250000000000004,7.03125,0,"SSTL15","SSTL15",null,null,null,0,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,9.375,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,9.375,7.8012189404594464E-4,1.0670417252695734E-2,3.5245462460652339E-4,0,0.1595]
["SSTL DCI 1.5V",{"$f":"VCCO15","v":1.5},3,3.1,0,0,0,1,0.92500000000000004,0.57499999999999996,5.93,9.375,2.6250000000000004,7.03125,0,"SSTL15","SSTL15_DCI",null,null,7.5,9.375,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,9.375,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,9.375,7.8012189404594464E-4,1.0295358649789029E-2,3.398968588842007E-4,0,0.1595]
["SSTL Class I 1.8V",{"$f":"VCCO18","v":1.8},1,3.1,0,0,0,1,1.37,0.43,4.7,0,8.4600000000000026,10.125,0,"HSTL","SSTL18_I",null,null,null,0,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,11.25,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,11.25,7.6999999999999963E-4,1.1049999999999999E-2,4.888392857142857E-4,0,0.1595]
["SSTL Class I DCI 1.8V",{"$f":"VCCO18","v":1.8},1,3.1,0,0,0,1,1.37,0.43,4.7,11.25,{"$f":"(B714^2/200 +B714/200*(I714-J714))*1000","v":24.660000000000004},10.125,0,"HSTL","SSTL18_I_DCI",null,null,null,11.25,5.0100000000000003E-4,8.4000000000000009E-6,0,0.51800000000000002,1.6870000000000001,11.25,4.2700000000000002E-4,2.5000000000000001E-5,0,0.74331899999999995,2.839,11.25,7.6999999999999963E-4,1.0675E-2,4.7321428571428558E-4,0,0.1595]
["SUB_LVDS 1.8V (pair)",1.8,2,6.2,0,0,0,1,0,0,9.1999999999999993,0,16.559999999999999,6.9300000000000006,0,"LVDS","SUB_LVDS",null,1.2249999999999999,null,0,1.3979999999999999E-3,5.8275E-5,0,0.35223500000000002,1.425,0,1.4E-3,9.1590000000000009E-5,0,0.35217000000000004,2.6930000000000001,0,6.4999999999999997E-4,2.7899999999999999E-3,1.3793103448275863E-4,0,0.31]
["SLVS 400 2.5V",2.5,2,3.1,0,0,0,0.28999999999999998,0,0,14.3,0,35.75,0,0,"LVDS","SLVS_400_25",null,null,null,0,1.4109999999999999E-3,4.4651000000000003E-5,0,0.35292800000000002,1.129,0,1.4109999999999999E-3,6.6799999999999997E-5,0,0.352995,2.13,0]
[]
["Package","Board Index","Sink Index","Size mm2"]
["CPG196",0,0,{"$f":"8*8","v":64}]
["CPG236",0,0,{"$f":"10*10","v":100}]
["CLG225",0,0,{"$f":"12*12","v":144}]
["CSG225",0,0,{"$f":"12*12","v":144}]
["CS324",0,0,{"$f":"15*15","v":225}]
["CSG324",0,0,{"$f":"15*15","v":225}]
["SB324",0,0,{"$f":"15*15","v":225}]
["SBG324",0,0,{"$f":"15*15","v":225}]
["CL400",0,0,{"$f":"17*17","v":289}]
["CLG400",0,0,{"$f":"17*17","v":289}]
["CS400",0,0,{"$f":"17*17","v":289}]
["CSG400",0,0,{"$f":"17*17","v":289}]
["FTG256",0,0,{"$f":"17*17","v":289}]
["CL484",0,0,{"$f":"19*19","v":361}]
["CLG484",0,0,{"$f":"19*19","v":361}]
["CSG484",0,0,{"$f":"19*19","v":361}]
["SB484",0,0,{"$f":"19*19","v":361}]
["SBG484",0,0,{"$f":"19*19","v":361}]
["FB484",17,6,{"$f":"23*23","v":529}]
["FBG484",17,6,{"$f":"23*23","v":529}]
["FFG484",34,6,{"$f":"23*23","v":529}]
["FG484",34,0,{"$f":"23*23","v":529}]
["SFVA784",34,0,{"$f":"23*23","v":529}]
["FB676",34,12,{"$f":"27*27","v":729}]
["FBVA676",34,12,729]
["FFG676",51,12,729]
["FG676",51,0,729]
["FGG676",51,0,729]
["RF676",51,12,729]
["FFG784",51,18,{"$f":"29*29","v":841}]
["FGG784",51,0,{"$f":"29*29","v":841}]
["FB900",51,18,{"$f":"31*31","v":961}]
["FBVA900",51,18,{"$f":"31*31","v":961}]
["FFG900",68,18,{"$f":"31*31","v":961}]
["FFG901",68,18,{"$f":"31*31","v":961}]
["RF900",68,18,{"$f":"31*31","v":961}]
["FFVA1156",85,24,{"$f":"35*35","v":1225}]
["FFVA1157",85,24,1225]
["FFG1158",85,24,1225]
["FFG1159",85,24,1225]
["FLG1157",85,24,1225]
["HCG1155",85,24,1225]
["FFVA1517",102,30,1600]
["FFVB1517",102,30,1600]
["FFVC1517",102,30,1600]
["FFVD1517",102,30,1600]
["FLVA1517",102,30,1600]
["FLVB1517",102,30,1600]
["FLVC1517",102,30,1600]
["FLVD1517",102,30,1600]
["FFG1761",102,30,1806.25]
["FFVA1760",102,30,{"$f":"42.5*42.5","v":1806.25}]
["FFVB1760",102,30,1806.25]
["FLVA1760",102,30,{"$f":"42.5*42.5","v":1806.25}]
["FLVB1760",102,30,{"$f":"42.5*42.5","v":1806.25}]
["FLG1761",102,30,{"$f":"42.5*42.5","v":1806.25}]
["RF1761",102,30,{"$f":"42.5*42.5","v":1806.25}]
["FFG1924",119,36,{"$f":"45*45","v":2025}]
["FFVD1924",119,36,2025]
["HCG1924",119,36,2025]
["FFVE1924",119,36,2025]
["FFVF1924",119,36,2025]
["FFVJ1924",119,36,2025]
["FLVJ1924",119,36,2025]
["FLVD1924",119,36,2025]
["FLVE1924",119,36,2025]
["FLVF1924",119,36,2025]
["FFG1926",119,36,{"$f":"45*45","v":2025}]
["FFG1927",119,36,2025]
["FFG1928",119,36,2025]
["FFG1929",119,36,2025]
["FFG1930",119,36,2025]
["FFG1933",119,36,2025]
["FLG1925",119,36,2025]
["FLG1926",119,36,2025]
["FLG1928",119,36,2025]
["FLG1930",119,36,2025]
["FLG1933",119,36,2025]
["FHGE1924",119,36,2256.25]
["FHGJ1924",119,36,2256.25]
["FFVA2104",119,36,2256.25]
["FFVB2104",119,36,2256.25]
["FFVC2104",119,36,2256.25]
["FLVA2104",119,36,2256.25]
["FLVB2104",119,36,2256.25]
["FLVC2104",119,36,2256.25]
["FLGB2104",119,36,2256.25]
["FLGC2104",119,36,2256.25]
["FLVA2377",119,42,2500]
["FLGA2377",119,42,2500]
["FLGB2377",119,42,2500]
["FLGA2577",119,42,2756.25]
["FLGA2892",119,48,3025]
[]
[null,null,null,"Board Type"]
["Package","Air Flow\n(LFM)","# Board\nLayers","JEDEC (2S2P)","Small (4\"x4\")","Medium (10\"x10\")","Large (20\"x20\")"]
["CS324 (Estimated)",0,"4 to 7",21.9,18.86,17.260000000000002,19.34]
[null,null,"8 to 11",null,17.32,14.38,14.28]
[null,null,"12 to 15",null,16.62,13.14,12.84]
[null,null,"16+",null,16.68,12.94,12.5]
[null,250,"4 to 7",16.8,15.06,13.800425531914801,15.4378723404255]
[null,null,"8 to 11",null,13.847659574468,11.5331914893617,11.454468085106299]
[null,null,"12 to 15",null,13.296595744680801,10.5570212765957,10.3208510638297]
[null,null,"16+",null,13.343829787234,10.399574468085101,10.0531914893617]
[null,500,"4 to 7",15.6,14.1009523809523,12.9272948328267,14.453049645389999]
[null,null,"8 to 11",null,12.9713069908814,10.8147112462006,10.741357649442699]
[null,null,"12 to 15",null,12.4578318135764,9.9051266464032395,9.6850658561296896]
[null,null,"16+",null,12.5018439716312,9.7584194528875408,9.4356636271529908]
[null,750,"4 to 7",15,13.5761904761904,12.449544072948299,13.914184397163099]
[null,null,"8 to 11",null,12.4917933130699,10.4215805471124,10.3511651469098]
[null,null,"12 to 15",null,11.9988855116514,9.5484295845998002,9.3371833839918903]
[null,null,"16+",null,12.041134751773001,9.4075987841945299,9.0977710233029399]
[]
["FB484",0,"4 to 7",15.74,13.86,12.26,14.34]
[null,null,"8 to 11",null,12.32,9.3800000000000008,9.2799999999999994]
[null,null,"12 to 15",null,11.62,8.14,7.84]
[null,null,"16+",null,11.68,7.94,7.5]
[null,250,"4 to 7",11.54,10.06,8.8004255319148932,10.437872340425534]
[null,null,"8 to 11",null,8.8476595744680857,6.5331914893617036,6.4544680851063845]
[null,null,"12 to 15",null,8.2965957446808503,5.5570212765957452,5.3208510638297879]
[null,null,"16+",null,8.3438297872340446,5.3995744680851079,5.0531914893617031]
[null,500,"4 to 7",10.48,9.100952380952382,7.9272948328267487,9.4530496453900721]
[null,null,"8 to 11",null,7.9713069908814607,5.814711246200611,5.7413576494427572]
[null,null,"12 to 15",null,7.4578318135764947,4.9051266464032439,4.685065856129687]
[null,null,"16+",null,7.5018439716312075,4.7584194528875399,4.435663627152989]
[null,750,"4 to 7",9.9,8.5761904761904759,7.4495440729483278,8.9141843971631207]
[null,null,"8 to 11",null,7.4917933130699081,5.4215805471124643,5.3511651469098283]
[null,null,"12 to 15",null,6.9988855116514683,4.5484295845997975,4.3371833839918947]
[null,null,"16+",null,7.0411347517730505,4.4075987841945308,4.0977710233029381]
[]
["FF484 (FB676) - index34",0,"4 to 7",12.54,11.52,9.84,10.119999999999999]
[null,null,"8 to 11",null,10.32,7.36,7.26]
[null,null,"12 to 15",null,9.8800000000000008,6.4,6.08]
[null,null,"16+",null,9.8800000000000008,6.12,5.68]
[null,250,"4 to 7",8.48,7.7103748488512682,6.442756952841596,6.6540266021765389]
[null,null,"8 to 11",null,6.8049334945586439,4.5715114873035052,4.4960580411124536]
[null,null,"12 to 15",null,6.4729383313180167,3.8471584038694062,3.6057073760580396]
[null,null,"16+",null,6.4729383313180167,3.6358887545344616,3.303893591293833]
[null,500,"4 to 7",7.5,6.7908101571946791,5.6227327690447408,5.817412333736395]
[null,null,"8 to 11",null,5.9564691656590067,3.8984280532043512,3.8288996372430475]
[null,null,"12 to 15",null,5.6505441354292625,3.2309552599758149,3.008464328899636]
[null,null,"16+",null,5.6505441354292625,3.0362756952841594,2.7303506650544138]
[null,750,"4 to 7",6.94,6.265344619105198,5.154147521160823,5.3393470374848846]
[null,null,"8 to 11",null,5.4716324062877861,3.5138089480048351,3.4476662636033866]
[null,null,"12 to 15",null,5.1806045949214035,2.8788391777509061,2.6671825876662623]
[null,null,"16+",null,5.1806045949214035,2.6936396614268432,2.4026118500604596]
[]
["FF676 (FB900) - index51",0,"4 to 7",12.38,11.38,9.6999999999999993,9.98]
[null,null,"8 to 11",null,10.199999999999999,7.24,7.14]
[null,null,"12 to 15",null,9.74,6.26,5.96]
[null,null,"16+",null,9.6,6,5.56]
[null,250,"4 to 7",8.34,7.5866422466422474,6.3210012210012207,6.5319413919413929]
[null,null,"8 to 11",null,6.697680097680097,4.4677411477411484,4.3924053724053724]
[null,null,"12 to 15",null,6.3511355311355313,3.7294505494505485,3.5034432234432229]
[null,null,"16+",null,6.2456654456654466,3.5335775335775339,3.2021001221001213]
[null,500,"4 to 7",7.32,6.628913308913309,5.467887667887668,5.6613919413919422]
[null,null,"8 to 11",null,5.8134310134310123,3.7678144078144071,3.6987057387057378]
[null,null,"12 to 15",null,5.4955311355311354,3.0905494505494486,2.8832234432234429]
[null,null,"16+",null,5.3987789987789991,2.9108669108669103,2.6067887667887661]
[null,750,"4 to 7",6.8,6.1406593406593402,5.032967032967032,5.2175824175824177]
[null,null,"8 to 11",null,5.3626373626373622,3.4109890109890104,3.3450549450549447]
[null,null,"12 to 15",null,5.0593406593406582,2.7648351648351635,2.5670329670329664]
[null,null,"16+",null,4.967032967032968,2.5934065934065926,2.3032967032967031]
[]
["FF900 (estimated) id68",0,"4 to 7",10.64,{"$f":"(E849+E900)/2","v":10.79},9.0300000000000011,9.2100000000000009]
[null,null,"8 to 11",null,9.81,6.8100000000000005,6.66]
[null,null,"12 to 15",null,9.4400000000000013,5.93,5.59]
[null,null,"16+",null,9.4400000000000013,5.66,5.1999999999999993]
[null,250,"4 to 7",6.72,6.9983890593030171,5.6915010922246125,5.8264002220691955]
[null,null,"8 to 11",null,6.2676574829741449,4.0389028826163305,3.9280153965780249]
[null,null,"12 to 15",null,5.9919187569396621,3.3840832891281636,3.1316684019254772]
[null,null,"16+",null,5.9919187569396621,3.1833394726350783,2.8417560599520937]
[null,500,"4 to 7",5.8,6.1076121630660047,4.9068977196722336,5.0310494911188783]
[null,null,"8 to 11",null,5.435727770840403,3.3878516287820117,3.2860574480493163]
[null,null,"12 to 15",null,5.1822202965974657,2.7859953411595697,2.5540959246678017]
[null,null,"16+",null,5.1822202965974657,2.6015165942360854,2.2876821445163076]
[null,750,"4 to 7",5.36,5.6341709471547787,4.4894715807438992,4.6076844179250029]
[null,null,"8 to 11",null,4.9939905900648736,3.0417818581986027,2.9446778184501938]
[null,null,"12 to 15",null,4.7524276380601567,2.4681661828809025,2.2470790322527496]
[null,null,"16+",null,4.7524276380601567,2.2923239179068817,1.9931315381092489]
[]
["FF1100 - index85",0,"4 to 7",9.1,10.06,8.2200000000000006,8.3000000000000007]
[null,null,"8 to 11",null,9.3000000000000007,6.26,6.06]
[null,null,"12 to 15",null,9,5.46,5.0999999999999996]
[null,null,"16+",null,9,5.2,4.72]
[null,250,"4 to 7",5.9,6.2864032697547669,4.9402452316076291,4.9987738419618521]
[null,null,"8 to 11",null,5.7303814713896459,3.5062942779291548,3.3599727520435962]
[null,null,"12 to 15",null,5.5108991825613076,2.921008174386921,2.6576294277929149]
[null,null,"16+",null,5.5108991825613076,2.7307901907356951,2.3796185286103544]
[null,500,"4 to 7",5,5.4244141689373295,4.1910626702997273,4.2446866485013617]
[null,null,"8 to 11",null,4.9149863760217984,2.8772752043596723,2.7432152588555851]
[null,null,"12 to 15",null,4.7138964577656681,2.3410354223433245,2.0997275204359673]
[null,null,"16+",null,4.7138964577656681,2.1667574931880109,1.8450136239782018]
[null,750,"4 to 7",4.5,5.0029972752043594,3.8247956403269754,3.8760217983651217]
[null,null,"8 to 11",null,4.5163487738419601,2.5697547683923703,2.4416893732970011]
[null,null,"12 to 15",null,4.3242506811989099,2.0574931880108993,1.8269754768392368]
[null,null,"16+",null,4.3242506811989099,1.8910081743869207,1.5836512261580382]
[]
["FF1700 - index102",0,"4 to 7",9.2799999999999994,8.8800000000000008,6.94,7.18]
[null,null,"8 to 11",null,8.34,5.26,5.12]
[null,null,"12 to 15",null,8.14,4.58,4.24]
[null,null,"16+",null,8.14,4.32,3.88]
[null,250,"4 to 7",5.46,5.1750602409638544,3.7931024096385526,3.9640662650602394]
[null,null,"8 to 11",null,4.7903915662650594,2.596355421686745,2.4966265060240955]
[null,null,"12 to 15",null,4.6479216867469875,2.1119578313253,1.8697590361445777]
[null,null,"16+",null,4.6479216867469875,1.926746987951806,1.6133132530120471]
[null,500,"4 to 7",4.62,4.3603614457831323,3.1011144578313248,3.2568975903614459]
[null,null,"8 to 11",null,4.0098493975903606,2.0106325301204806,1.9197590361445784]
[null,null,"12 to 15",null,3.8800301204819276,1.5692469879518072,1.3485542168674698]
[null,null,"16+",null,3.8800301204819276,1.4004819277108431,1.1148795180722886]
[null,750,"4 to 7",4.18,3.9336144578313252,2.7386445783132514,2.8864759036144578]
[null,null,"8 to 11",null,3.6009939759036129,1.7038253012048172,1.6175903614457829]
[null,null,"12 to 15",null,3.4778012048192766,1.2849698795180722,1.0755421686746984]
[null,null,"16+",null,3.4778012048192766,1.1248192771084333,0.85379518072289073]
[]
["FF1900 - index 119",0,"4 to 7",7.887999999999999,7.8144000000000009,6.1072000000000006,6.3183999999999996]
[null,null,"8 to 11",null,7.3391999999999999,4.6288,4.5056000000000003]
[null,null,"12 to 15",null,7.1632000000000007,4.0304000000000002,3.7312000000000003]
[null,null,"16+",null,7.1632000000000007,3.8016000000000001,3.4144000000000001]
[null,250,"4 to 7",4.641,4.5540530120481924,3.3379301204819263,3.4883783132530106]
[null,null,"8 to 11",null,4.2155445783132519,2.2847927710843359,2.1970313253012042]
[null,null,"12 to 15",null,4.0901710843373493,1.8585228915662639,1.6453879518072283]
[null,null,"16+",null,4.0901710843373493,1.6955373493975894,1.4197156626506013]
[null,500,"4 to 7",3.927,3.8371180722891567,2.7289807228915657,2.8660698795180726]
[null,null,"8 to 11",null,3.5286674698795175,1.769356626506023,1.689387951807229]
[null,null,"12 to 15",null,3.4144265060240961,1.3809373493975903,1.1867277108433734]
[null,null,"16+",null,3.4144265060240961,1.232424096385542,0.98109397590361391]
[null,750,"4 to 7",3.5529999999999995,3.4615807228915663,2.4100072289156613,2.540098795180723]
[null,null,"8 to 11",null,3.1688746987951792,1.4993662650602391,1.423479518072289]
[null,null,"12 to 15",null,3.0604650602409635,1.1307734939759035,0.94647710843373467]
[null,null,"16+",null,3.0604650602409635,0.98984096385542131,0.75133975903614381]
[]
[null,"Radian Heatsink Data"]
["Package","Height (mm)","Airflow (LFM)","ThetaSA"]
["FF324 (19mm)",6.3,250,5.2]
[null,null,500,4.3]
[null,9.5,250,4.5999999999999996]
[null,null,500,3.6]
[null,12.7,250,3.9]
[null,null,500,3.1]
["FF484 (23mm)",6.3,250,4.9000000000000004]
[null,null,500,3.8]
[null,9.5,250,4.2]
[null,null,500,3.2]
[null,12.7,250,3.5]
[null,null,500,2.8]
["FF665-676 (27mm)",6.3,250,4.2]
[null,null,500,3.2]
[null,9.5,250,3.4]
[null,null,500,2.4]
[null,12.7,250,2.8]
[null,null,500,2]
["FF784 (29mm)",6.3,250,4.0999999999999996]
[null,null,500,3]
[null,9.5,250,3.3]
[null,null,500,2.2999999999999998]
[null,12.7,250,2.6]
[null,null,500,1.8]
["FF1136-1158 (35mm)",6.3,250,3.5]
[null,null,500,2.2999999999999998]
[null,9.5,250,2.4]
[null,null,500,1.5]
[null,12.7,250,2]
[null,null,500,1.2]
["FF1738-1760 (42.5mm)",12.7,250,3.1]
[null,null,500,2]
[null,14.6,250,2.2000000000000002]
[null,null,500,1.4]
[null,17.600000000000001,250,1.6]
[null,null,500,1.1000000000000001]
["FF1923-1933 (45mm)",14.6,250,1.7]
[null,null,500,1.2]
[null,20.6,250,1.2]
[null,null,500,0.8]
[null,27.6,250,1]
[null,null,500,0.6]
["FF2377(50mm)",14.6,250,1.3]
[null,null,500,0.9]
[null,20.6,250,0.9]
[null,null,500,0.6]
[null,27.6,250,0.8]
[null,null,500,0.5]
["FF2892(55mm)",14.6,250,1.1000000000000001]
[null,null,500,0.8]
[null,20.6,250,0.8]
[null,null,500,0.5]
[null,27.6,250,0.7]
[null,null,500,0.4]

{"sheet":"Test","index":21,"n_rows":707,"n_cols":85,"rows_kept":707,"cut":false,"hidden":true,"merged":[[258,1,258,3],[258,4,258,6],[258,7,258,9],[622,38,622,45],[632,38,632,45],[598,20,598,21],[605,9,605,11],[605,12,605,15],[605,0,605,3],[499,11,506,12],[559,5,559,8],[470,11,477,12],[478,11,489,12],[490,11,498,12],[570,9,570,11],[570,12,570,14],[622,56,622,63],[632,56,632,63],[654,56,654,63],[654,38,654,45],[685,50,685,60],[685,38,685,48],[632,29,632,36],[654,29,654,36],[622,47,622,54],[632,47,632,54],[654,47,654,54],[538,0,538,4],[559,0,559,4],[654,2,654,9],[632,11,632,18],[654,20,654,27],[654,11,654,18],[622,20,622,27],[632,20,632,27],[622,11,622,18],[622,2,622,9],[632,2,632,9],[605,5,605,8],[538,5,538,8],[538,9,538,11],[538,12,538,14],[559,9,559,11],[509,36,509,40],[509,41,509,45],[509,46,509,50],[509,1,509,5],[509,6,509,10],[509,11,509,15],[509,16,509,20],[509,31,509,35],[559,12,559,14],[570,0,570,4],[570,5,570,8],[685,74,685,84],[693,74,693,84],[685,2,685,12],[685,14,685,24],[685,26,685,36],[693,2,693,12],[693,14,693,24],[693,26,693,36],[685,62,685,72],[693,62,693,72],[693,50,693,60],[693,38,693,48],[622,29,622,36]]}
["Each test section consists of a named range with parameters and expected results."]
[]
["CLOCK","MHz","Type","Fan","CE","SliceCE","Vccint"]
["GCLK_Test_200k",500,"Global",200000,1,1,4.5728819999999999,3.7658696799999998]
["GCLK_Test_20k",500,"Global",20000,1,1,0.64393299999999998,0.53722873999999998]
["GCLK_Test_2k",500,"Global",2000,1,1,8.6134000000000002E-2,7.5231719999999988E-2]
["GCLK_Test_200",500,"Global",200,1,1,1.68115E-2,1.7236809999999998E-2]
["GCLK_Test_20",500,"Global",20,1,1,5.4674999999999993E-3,6.7842699999999994E-3]
["GCLK_Test_2",500,"Global",2,1,1,2.3574999999999998E-3,3.0836099999999996E-3]
["GCLK_Test_40k",500,"Global",40000,1,1,1.22305,1.0132551399999998]
["GCLK_Test_40k_100_50",500,"Global",40000,1,0.5,0.78754000000000002,0.65613693999999989]
["GCLK_Test_40k_50_100",500,"Global",40000,0.5,1,0.68918149999999989,0.50662756999999992]
["GCLK_Test_40k_50_50",500,"Global",40000,0.5,0.5,0.68918149999999989,0.32806846999999995]
["RCLK_Test_4k",500,"Regional",4000,1,1,0.1539845,0.13201959000000002]
["RCLK_Test_400",500,"Regional",400,1,1,2.5589500000000001E-2,2.4434769999999998E-2]
["RCLK_Test_40",500,"Regional",40,1,1,6.7644999999999997E-3,7.8478099999999985E-3]
["IOCLK_Test_2k",500,"I/O",2000,1,1,5.1822000000000007E-2,4.2494040000000004E-2]
["IOCLK_Test_200",500,"I/O",200,1,1,5.6325000000000004E-3,4.6186500000000002E-3]
["IOCLK_Test_20",500,"I/O",20,1,1,1.0215000000000001E-3,8.3763000000000002E-4]
["MMCM_Test",800,"CMT",1,1,1,1.2815999999999999E-4,1.0509119999999999E-4]
["PHASER_TEST",800,"CMT",8,1,1,3.8256000000000005E-4,3.1369920000000003E-4]
["Other_Test_100",500,"Other",100,1,1,2.8235000000000001E-3,2.3152699999999999E-3]
["Other_Test_10",500,"Other",10,1,1,5.1800000000000001E-4,4.2475999999999999E-4]
["Other_Test_1",500,"Other",1,1,1,2.7950000000000002E-4,2.2918999999999999E-4]
[]
["LOGIC","Clk","LUTs","SREGs","SRAM","FF","Toggle","Fan","Signal Rate","Vccint"]
["LOGIC_Test1",100,10000,0,0,10000,0.5,3,50,0.19597327250000005,0.19102191514469297]
["LOGIC_Test2",100,10000,0,0,10000,1,3,100,0.39194654500000009,0.38204383028938593]
["LOGIC_Test3",400,10000,0,0,10000,0.5,3,200,0.78389309000000018,0.76408766057877187]
["LOGIC_Test4",400,10000,0,0,10000,1,3,400,1.5677861800000004,1.5281753211575437]
["LOGIC_Test5",100,40000,0,0,40000,0.5,3,50,0.78389309000000018,0.76408763389469303]
["LOGIC_Test6",100,40000,0,0,40000,1,3,100,1.5677861800000004,1.5281752677893861]
["LOGIC_Test7",400,40000,0,0,40000,0.5,3,200,3.1355723600000007,3.0563505355787721]
["LOGIC_Test8",400,40000,0,0,40000,1,3,400,6.2711447200000014,6.1127010711575442]
["LOGIC_Test9",100,1000,1000,1000,1000,0.2,3,20,2.4694332900000001E-2,2.8710132307877174E-2]
["LOGIC_Test10",100,1000,1000,1000,1000,0.2,4,20,2.69128909E-2,3.1578958444928508E-2]
["LOGIC_Test11",100,1000,1000,1000,1000,0.2,5,20,2.9131448899999999E-2,3.444778472829374E-2]
["LOGIC_Test12",200,40000,1000,1000,65000,0.2,2,40,0.73019407850000007,0.65566529053832578]
["LOGIC_Test13",200,40000,1000,1000,65000,0.2,3,40,0.80554854849999991,0.81239926836575438]
["LOGIC_Test14",200,40000,1000,1000,65000,0.2,4,40,0.88090301850000008,0.91663324563985715]
["LOGIC_Test15",200,40000,1000,1000,65000,0.2,5,40,0.95625748850000014,1.0208672232065876]
["LOGIC_Test16",200,40000,1000,1000,65000,0.2,15,40,1.7098021885000003,2.0632070149684214]
[]
["BRAM","BRAMs","Cascade Group Size","Mode","Toggle Rate","Clock","Enable","Width","Mode","Write Rate","Clock","Enable","Width","Mode","Write Rate","Signal Rate","Vccint","Vbram",null,"KC705"]
["18x18_WRITE_FIRST_1",500,0,"RAMB18",0.25,250,0.5,18,"WRITE_FIRST",0.5,250,0.5,18,"WRITE_FIRST",0.5,31.25,1.5615000000000001,9.4062500000000007E-2,null,1.69,{"$f":"(SUM(Q45:R45)-T45)/T45","v":-2.0377218934911182E-2}]
["18x18_WRITE_FIRST_2",500,0,"RAMB18",0.125,250,1,18,"WRITE_FIRST",0.5,250,1,18,"WRITE_FIRST",0.5,31.25,2.9489999999999998,0.18812500000000001,null,3.24,{"$f":"(SUM(Q46:R46)-T46)/T46","v":-3.1751543209876693E-2}]
["18x18_WRITE_FIRST_3",500,0,"RAMB18",0.5,250,0.25,18,"WRITE_FIRST",0.5,250,0.25,18,"WRITE_FIRST",0.5,31.25,0.86775000000000002,4.7031250000000004E-2,null,0.92,-5.6725543478261409E-3]
["18x18_NO_CHANGE_1",500,0,"RAMB18",0.25,250,0.5,18,"NO_CHANGE",0.5,250,0.5,18,"NO_CHANGE",0.5,31.25,1.25875,9.1874999999999998E-2,null,1.29,4.6996124031007697E-2]
["18x18_NO_CHANGE_2",500,0,"RAMB18",0.125,250,1,18,"NO_CHANGE",0.5,250,1,18,"NO_CHANGE",0.5,31.25,2.4649999999999999,0.18375,null,2.57,3.0642023346303456E-2]
["18x18_NO_CHANGE_3",500,0,"RAMB18",0.5,250,0.25,18,"NO_CHANGE",0.5,250,0.25,18,"NO_CHANGE",0.5,31.25,0.65562500000000001,4.5937499999999999E-2,null,0.67,4.7108208955223788E-2]
["18x1_WRITE_FIRST_1",500,0,"RAMB18",0.25,250,0.5,1,"WRITE_FIRST",0.5,250,0.5,1,"WRITE_FIRST",0.5,31.25,1.3147500000000001,9.6250000000000002E-2,null,1.36,3.749999999999995E-2]
["18x1_WRITE_FIRST_2",500,0,"RAMB18",0.125,250,1,1,"WRITE_FIRST",0.5,250,1,1,"WRITE_FIRST",0.5,31.25,2.6085000000000003,0.1925,null,2.77,1.1191335740072252E-2]
["18x1_WRITE_FIRST_3",500,0,"RAMB18",0.5,250,0.25,1,"WRITE_FIRST",0.5,250,0.25,1,"WRITE_FIRST",0.5,31.25,0.667875,4.8125000000000001E-2,null,0.66,8.4848484848484756E-2]
["No activity1",500,0,"RAMB18",0,250,0.5,18,"WRITE_FIRST",0.5,250,0.5,18,"WRITE_FIRST",0.5,0,1.1856422212639328,9.4062500000000007E-2,null,1.27,7.6415128062462491E-3]
["No activity2",500,0,"RAMB18",0,250,1,18,"WRITE_FIRST",0.5,250,1,18,"WRITE_FIRST",0.5,0,2.3592844425278656,0.18812500000000001,null,2.5299999999999998,6.8812025801840686E-3]
["No activity3",500,0,"RAMB18",0,250,0.25,18,"WRITE_FIRST",0.5,250,0.25,18,"WRITE_FIRST",0.5,0,0.59882111063196641,4.7031250000000004E-2,null,0.62,4.16973558580103E-2]
["18SDP_1",500,0,"RAMB18SDP",0.25,250,0.5,36,"WRITE_FIRST",0.5,250,0.5,36,"WRITE_FIRST",0.5,31.25,1.9759687500000001,7.1093749999999997E-2,null,1.98,3.3869949494949508E-2]
["18SDP_2",500,0,"RAMB18SDP",0.125,250,1,36,"WRITE_FIRST",0.5,250,1,36,"WRITE_FIRST",0.5,31.25,3.8589375000000001,0.14218749999999999,null,4,2.8125000000001066E-4]
["18SDP_3",500,0,"RAMB18SDP",0.5,250,0.25,36,"WRITE_FIRST",0.5,250,0.25,36,"WRITE_FIRST",0.5,31.25,1.0344843750000001,3.5546874999999999E-2,null,0.98,9.1868622448979823E-2]
["36SDP_1",250,0,"RAMB36SDP",0.25,250,0.5,72,"WRITE_FIRST",0.5,250,0.5,72,"WRITE_FIRST",0.5,31.25,1.9759687500000001,7.4484375000000005E-2,null,2.17,-5.5090725806451482E-2]
["36SDP_2",250,0,"RAMB36SDP",0.125,250,1,72,"WRITE_FIRST",0.5,250,1,72,"WRITE_FIRST",0.5,31.25,3.8589375000000001,0.14896875000000001,null,4.24,-5.473909198113202E-2]
["36SDP_3",250,0,"RAMB36SDP",0.5,250,0.25,72,"WRITE_FIRST",0.5,250,0.25,72,"WRITE_FIRST",0.5,31.25,1.0344843750000001,3.7242187500000003E-2,null,1.1100000000000001,-3.4480574324324324E-2]
["BRAM_Test1",1,0,"RAMB18",0.5,166,1,18,"WRITE_FIRST",0.5,166,1,18,"WRITE_FIRST",0.5,83,4.5776159999999996E-3,2.4983000000000004E-4]
["BRAM_Test2",1,0,"RAMB36",0.5,166,1,36,"READ_FIRST",0.5,166,1,36,"READ_FIRST",0.5,83,9.72926E-3,5.4846399999999992E-4]
["BRAM_Test3",1,0,"RAMB18SDP",0.5,166,1,36,"WRITE_FIRST",0.5,166,1,36,"WRITE_FIRST",0.25,83,4.8507689999999996E-3,1.583225E-4]
["BRAM_Test4",1,0,"RAMB18SDP",0.5,166,1,36,"READ_FIRST",0.5,166,1,36,"READ_FIRST",0.5,83,5.784519000000001E-3,1.8592000000000004E-4]
["BRAM_Test5",1,0,"RAMB36SDP",0.5,166,1,72,"WRITE_FIRST",0.5,166,1,72,"WRITE_FIRST",0.5,83,1.0894746000000002E-2,3.9566100000000006E-4]
["BRAM_Test6",1,0,"RAMB36SDP",0.5,166,1,72,"READ_FIRST",0.5,166,1,72,"READ_FIRST",0.5,83,1.1537166000000003E-2,4.0118050000000007E-4]
["BRAM_Test7",1,0,"RAMB36SDP_ECC",0.5,166,1,64,"WRITE_FIRST",0.5,166,1,64,"WRITE_FIRST",0.5,83,1.0299013499999999E-2,2.93405E-4]
["BRAM_Test8",1,0,"FIFO18",0.5,166,0,18,null,0.5,166,1,18,null,0.25,83,2.5716719999999997E-3,1.978305E-4]
["BRAM_Test9",1,0,"FIFO36",0.5,166,0,36,null,0.5,166,1,36,null,0.25,83,4.8251219999999994E-3,3.4772850000000001E-4]
["BRAM_Test10",1,0,"FIFO18",0.5,166,0,36,null,0.5,166,1,36,null,0.25,83,3.9536219999999995E-3,3.05025E-4]
["BRAM_Test11",1,0,"FIFO36",0.5,166,0,72,null,0.5,166,1,72,null,0.25,83,7.1781719999999992E-3,5.2290000000000008E-4]
["BRAM_Test12",1,0,"FIFO36_72_ECC",0.5,166,0,64,null,0.5,166,1,64,null,0.25,83,6.9910485000000003E-3,4.7177199999999997E-4]
["BRAM_Test13",1,0,"RAMB36",0.5,166,1,1,"READ_FIRST",0.25,166,1,1,"READ_FIRST",0.75,83,1.5300552E-2,1.3897520000000002E-3]
["BRAM_Test14",1,0,"RAMB36",0.5,166,1,1,"WRITE_FIRST",0.25,166,1,1,"WRITE_FIRST",0.75,83,1.4022351999999998E-2,1.3368810000000001E-3]
["BRAM_Test15",1,0,"RAMB36",0.5,166,1,36,"READ_FIRST",0.5,166,1,1,"READ_FIRST",0.5,83,8.7017199999999996E-3,5.5224049999999991E-4]
["BRAM_Test16",1,0,"RAMB36",0.5,166,1,18,"READ_FIRST",0.75,166,1,2,"READ_FIRST",0.25,83,8.280827000000001E-3,4.1250999999999994E-4]
["BRAM_Test17",1,0,"RAMB36",0.5,166,1,9,"READ_FIRST",0.5,166,1,4,"READ_FIRST",0.5,83,8.0906740000000008E-3,5.5863149999999992E-4]
["BRAM_Test18",1,0,"RAMB36",0.5,166,1,4,"READ_FIRST",0.5,166,1,9,"READ_FIRST",0.5,83,8.0906740000000008E-3,5.5863149999999992E-4]
["BRAM_Test19",1,0,"RAMB36",0.5,300,0,36,"READ_FIRST",0.5,300,0,36,"READ_FIRST",0.5,0,5.7599999999999997E-5,0]
["BRAM_Test20",1,0,"RAMB36",0,300,1,36,"READ_FIRST",0.5,300,1,36,"READ_FIRST",0.5,0,1.2250791077131238E-2,9.9120000000000002E-4]
["BRAM_Test21",1,0,"RAMB36",0.25,300,1,36,"READ_FIRST",0.5,300,1,36,"READ_FIRST",0.5,75,1.6027799999999998E-2,9.9120000000000002E-4]
["BRAM_Test22",1,0,"RAMB36",0.5,300,1,36,"READ_FIRST",0.5,300,1,36,"READ_FIRST",0.5,150,1.7582999999999998E-2,9.9120000000000002E-4]
["BRAM_Test23",1,0,"RAMB36",0.75,300,1,36,"READ_FIRST",0.5,300,1,36,"READ_FIRST",0.5,225,1.9138200000000001E-2,9.9120000000000002E-4]
["BRAM_Test24",1,0,"RAMB36",1,300,1,36,"READ_FIRST",0.5,300,1,36,"READ_FIRST",0.5,300,2.0693400000000001E-2,9.9120000000000002E-4]
[]
["ClkMgr",null,"Clock","Mode","Divide","Mult","Clock0","Clock1","Clock2","Clock3","Clock4","Clock5","Clock6","PowerDown","Vccint","Vccaux"]
["MMCM_Test1","MMCM",200,"None",1,1,1,1,1,1,1,1,1,0,3.3445720000000001E-3,6.5972486250000004E-2]
["MMCM_Test2","MMCM",400,"Fixed",10,32,2,"off",2,"off",2,"off","off",0,4.0969720000000008E-3,0.12920588999999996]
["MMCM_Test3","MMCM",600,"Dynamic",36,64,4,8,16,32,64,128,"off",0,1.1326553333333336E-3,0.132214005]
["MMCM_Test4","MMCM",400,"Fixed",36,64,4,8,16,32,64,128,128,0.1,6.9021480000000014E-4,8.4365622000000015E-2]
["PLL_Test1","PLL",200,"None",1,1,1,1,1,1,1,1,"off",0,2.9265719999999997E-3,5.859760499999999E-2]
["PLL_Test2","PLL",200,"None",10,32,2,"off",2,"off",2,"off","off",0,2.0487719999999999E-3,7.623000000000002E-2]
["PLL_Test3","PLL",400,"None",36,64,4,8,16,32,64,128,"off",0.1,6.7976480000000008E-4,7.0758566999999981E-2]
[]
["Phaser","FIFOin","FIFOout","Phsrin","PhsrOut","FIFOClk","MemClk","Vccint","Vccaux"]
["PHASER_Test1",4,4,4,4,400,1066,8.5314086000000011E-2,0.236376]
["PHASER_Test2",0,0,1,1,0,533,1.7177524000000003E-2,5.2171200000000008E-2]
["PHASER_Test3",4,4,0,0,500,0,4.2588000000000001E-2,0]
["PHASER_Test4",0,0,1,0,0,400,1.2426400000000001E-2,4.0680000000000008E-2]
[]
["XADC","Clock","Vccint","Vccaux"]
["XADC_Test",50,2.5000000000000001E-4,2.8265399999999996E-2]
[]
["Config","Clock","Bank","Vccint","Vccaux"]
["CFG_Test",25,2.5,6.5000000000000006E-3,3.0001499999999996E-3]
[]
["DSP","Num","Clock","Toggle","MULT?","MREG?","PreAdd?","Signal Rate","Vccint"]
["DSP_Test1",100,400,0.2,"Yes","Yes","Yes",80,0.20372591999999998,0.18104591999999994]
["DSP_Test1",100,400,0.2,"No","Yes","No",80,0.1387776,0.1160976]
["DSP_Test2",100,400,0.2,"Yes","No","Yes",92,0.23041624799999999,0.20514424799999997]
["DSP_Test3",100,400,0.2,"No","No","No",80,0.1387776,0.1160976]
["DSP_Test4",100,400,0,"Yes","Yes","Yes",0,6.3600000000000002E-3,9.6000000000000002E-4]
["DSP_Test5",100,400,0.5,"Yes","Yes","Yes",200,0.49977479999999991,0.45117479999999993]
["DSP_Test6",100,400,1,"Yes","Yes","Yes",400,0.99318959999999989,0.90138959999999979]
[]
["PS7","A9","Clock","Usage","Memory","Width","Clock","Read","Write","AXI","Usage","I/O","Clock","Vccpint","Vccpaux","Vccpll","Vcco_ddr","Vcc_mio"]
["PS7_DDR3_QSPI4",2,500,0.5,"DDR3",32,533,0.25,0.25,200,0.5,"QSPI 4-bit",100,0.27376369119503746,3.0275895516068758E-2,0.12837599999999999,0.48084374999999996,1.1250000000000001E-3]
["PS7_DDR3_QSPI8",2,500,0.5,"DDR3",32,533,0.5,0,200,0.5,"QSPI 8-bit",100,0.30623201300395997,5.6277959098206258E-2,0.12837599999999999,0.69374999999999998,3.3750000000000004E-3]
["PS7_DDR3_NAND",2,500,0.5,"DDR3",32,533,0,0.5,200,0.5,"NAND",100,0.32765254250111503,5.7332259964125E-3,0.12837599999999999,0.18112499999999998,6.7500000000000008E-3]
["PS7_DDR3_SRAM",1,250,0.25,"DDR3",16,533,0.25,0.25,200,0.35,"SRAM/NOR",100,7.2429974370103747E-2,1.9283332499962506E-2,0.110376,0.32701687499999998,1.575E-2]
["PS7_DDR3_USB",1,250,0.5,"DDR3",16,533,0.5,0,200,0.5,"USB",60,0.107768772485565,3.2647759082101505E-2,0.110376,0.45787499999999998,1.737E-2]
["PS7_DDR3_GigE",1,250,0.5,"DDR3",16,533,0,0.5,200,0.5,"GigE",250,0.1187437685966425,7.7702515285139996E-3,0.110376,0.1388625,2.4120000000000003E-2]
["PS7_LPDDR2_UART",2,500,0.5,"LPDDR2",32,400,0.25,0.25,200,0.3,"UART",10,0.25797982697999999,3.791547868565686E-2,0.1188,0.1917966046208,2.4120000000000003E-2]
["PS7_LPDDR2_I2C",2,500,0.5,"LPDDR2",32,400,0.5,0,200,0.5,"I2C",2,0.28556200668100001,5.6834054923156754E-2,0.1188,0.11353548462079999,2.4165000000000002E-2]
["PS7_LPDDR2_SPI",2,500,0.5,"LPDDR2",32,400,0,0.5,200,0.5,"SPI",50,0.30135797222119998,1.9015249116371015E-2,0.1188,0.27005772462080002,2.4174000000000001E-2]
["PS7_LPDDR2_CAN",1,250,0.25,"LPDDR2",16,400,0.25,0.25,200,0.25,"CAN",2,6.39472025862E-2,2.3169437432441903E-2,0.1008,0.1526660446208,2.4399000000000001E-2]
["PS7_LPDDR2_SD",1,250,0.5,"LPDDR2",16,400,0.5,0,200,0.5,"SD",50,9.6774926126400013E-2,3.0701187654227604E-2,0.1008,0.11353548462079999,2.4407999999999999E-2]
["PS7_LPDDR2_Trace",1,250,0.5,"LPDDR2",16,400,0,0.5,200,0.5,"Trace",109,0.10458435638890001,1.5745265401547689E-2,0.1008,0.1917966046208,2.49705E-2]
["PS7_DDR2_Timer",2,500,0.5,"DDR2",32,400,0.25,0.25,200,0.2,"Timer",50,0.25652689018515007,4.0712965148419773E-2,0.1188,0.31378925030137139,2.6196750000000001E-2]
["PS7_DDR2_Watchdog",2,500,0.5,"DDR2",32,400,0.5,0,200,0.5,"Watchdog",50,0.28582164844765001,5.4266041024311297E-2,0.1188,0.40421725030137146,2.6759250000000002E-2]
["PS7_DDR2_PJTAG",2,500,0.5,"DDR2",32,400,0,0.5,200,0.5,"PJTAG",20,0.30166666271015002,2.7472616571631372E-2,0.1188,0.22336125030137144,2.7321750000000002E-2]
["PS7_DDR3_GPIO0",2,500,0.5,"DDR3",32,400,0.25,0.25,250,0.15,"GPIO Bank 0",60,0.25647805822515002,3.4579198614487661E-2,0.1188,0.48084374999999996,2.7681750000000001E-2]
["PS7_DDR3_GPIO1",2,500,0.5,"DDR3",32,400,0.5,0,200,0.5,"GPIO Bank 1",60,0.28591535942114998,6.0689596798415922E-2,0.1188,0.69374999999999998,2.7816750000000001E-2]
[]
["GTH","Num","Mode","Mode","Share LC","RX","RX Rate","RX Data","Data Mode","TX","TX Rate","TX Data","Data Mode","TX/OP","OOB","PCIe","Vccint","Vccaux","AVcc","AVtt","mW/Channel",null,"PMA"]
["13.1 LP",4,"Transceiver","Low Power",4,"QPLL",13.1,64,"8b/10b","QPLL",13.1,64,"8b/10b",250,"No",null,0.18820000000000003,2.0046893057851234E-2,0.73356366942148765,0.18640079999999998,{"$f":"SUM(Q138:T138)/B138*1000","v":282.05284061983468},null,{"$f":"SUM(R138:T138)/B138*1000","v":235.00284061983473}]
["13.1 DFE",1,"Transceiver","DFE",1,"QPLL",13.1,64,"8b/10b","QPLL",13.1,64,"8b/10b",600,"Yes",null,4.7050000000000008E-2,2.0046893057851234E-2,0.2122449173553719,8.1307199999999996E-2,360.64901041322315,null,313.59901041322314]
["12.5 DFE",1,"Transceiver","DFE",1,"QPLL",12.5,64,"8b/10b","QPLL",12.5,64,"8b/10b",600,"No",null,4.4950000000000011E-2,1.9761273223140488E-2,0.20629896694214878,6.6307199999999997E-2,337.31744016528933,null,292.36744016528928]
["12.5 LP",1,"Transceiver","Low Power",1,"QPLL",12.5,64,"8b/10b","QPLL",12.5,64,"8b/10b",600,"No",null,4.4950000000000011E-2,1.9761273223140488E-2,0.17794896694214876,5.4307199999999993E-2,296.96744016528925,null,252.01744016528926]
["10.3125 DFE",1,"Transceiver","DFE",1,"QPLL",10.3125,64,"8b/10b","QPLL",10.3125,64,"8b/10b",600,"No",null,3.7293750000000001E-2,1.8719950909090902E-2,0.18462102272727274,6.6307199999999997E-2,306.94192363636364,null,269.64817363636359]
["10.3125 LP",1,"Transceiver","Low Power",1,"QPLL",10.3125,64,"8b/10b","QPLL",10.3125,64,"8b/10b",600,"No",null,3.7293750000000001E-2,1.8719950909090902E-2,0.15810852272727274,5.4307199999999993E-2,268.42942363636365,null,231.13567363636363]
["10.3125 LP (64b/66b)",1,"Transceiver","Low Power",1,"QPLL",10.3125,64,"64b/66b","QPLL",10.3125,64,"64b/66b",600,"No",null,4.6317187500000009E-2,1.8719950909090902E-2,0.15810852272727274,5.4307199999999993E-2,277.45286113636365,null,231.13567363636363]
["6.5 DFE",1,"Transceiver","DFE",1,"QPLL",6.5,40,"Raw","QPLL",6.5,40,"Raw",600,"No",null,2.3950000000000003E-2,1.9999289752066111E-2,0.14846392561983474,6.6307199999999997E-2,258.7204153719008,null,234.77041537190087]
["6.5 LP",1,"Transceiver","Low Power",1,"QPLL",6.5,40,"Raw","QPLL",6.5,40,"Raw",600,"No",null,2.3950000000000003E-2,1.9999289752066111E-2,0.12515392561983471,5.4307199999999993E-2,223.41041537190083,null,199.46041537190081]
["6.5 Ring DFE",1,"Transceiver","DFE",0,"CPLL",6.5,40,"Raw","CPLL",6.5,40,"Raw",600,"No",null,2.3950000000000003E-2,0,0.17590125000000004,0.10686719999999998,306.71845000000002,null,282.76845000000003]
["6.5 Ring LP",1,"Transceiver","Low Power",0,"CPLL",6.5,40,"Raw","CPLL",6.5,40,"Raw",600,"No",null,2.3950000000000003E-2,0,0.15259125000000001,9.4867199999999985E-2,271.40845000000002,null,247.45845]
["6.5 Ring+LC DFE",1,"Transceiver","DFE",1,"CPLL",6.5,40,"Raw","QPLL",6.5,40,"Raw",600,"No",null,2.3950000000000003E-2,1.9999289752066111E-2,0.18912517561983475,0.11286719999999999,345.94166537190085,null,321.99166537190081]
["6.5 Ring+LC LP",1,"Transceiver","Low Power",1,"CPLL",6.5,40,"Raw","QPLL",6.5,40,"Raw",600,"No",null,2.3950000000000003E-2,1.9999289752066111E-2,0.16581517561983472,0.10086719999999999,310.63166537190079,null,286.68166537190081]
["3.125 LC",1,"Transceiver","Low Power",1,"QPLL",3.125,20,"Raw","QPLL",3.125,20,"Raw",600,"No",null,2.3075000000000002E-2,1.9761273223140488E-2,9.5261466942148765E-2,5.4307199999999993E-2,192.40494016528925,null,169.32994016528923]
["3.125 Ring",1,"Transceiver","Low Power",0,"CPLL",3.125,20,"Raw","CPLL",3.125,20,"Raw",600,"No",null,2.3075000000000002E-2,0,0.12239062500000002,7.3807199999999989E-2,219.27282500000001,null,196.19782499999999]
["PCIe GEN2",1,"Transceiver","Low Power",1,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",600,"Yes","PCIe",0.1447,1.8571190578512392E-2,0.11117417355371903,6.9307199999999999E-2,343.75256413223144,null,199.05256413223142]
["PCIe GEN2 x8",8,"Transceiver","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",600,"Yes","PCIe",0.31860000000000005,3.7142381157024784E-2,0.88939338842975224,0.55445759999999999,224.94917119834713,null,185.12417119834711]
["PCIe GEN3 x2",2,"Transceiver","DFE",2,"QPLL",8,64,"8b/10b","QPLL",8,64,"8b/10b",600,"Yes","PCIe",0.29139999999999999,1.7619124462809915E-2,0.32340867768595044,0.16261439999999999,397.52110107438023,null,251.82110107438015]
["Mixed rate",1,"Transceiver","Low Power",1,"QPLL",6.25,64,"8b/10b","QPLL",3.125,32,"8b/10b",600,"No",null,2.3075000000000002E-2,1.9761273223140488E-2,0.10904271694214877,5.4307199999999993E-2,206.18619016528928,null,183.11119016528926]
["Transmit min TX/OP",1,"Transmitter","Low Power",1,"QPLL",2.488,16,"8b/10b","QPLL",2.488,16,"8b/10b",250,"No",null,1.8616000000000004E-2,1.8548340991735534E-2,5.7034257520661165E-2,1.1800199999999999E-2,105.9987985123967,null,87.38279851239669]
["Transmit max TX/OP",1,"Transmitter","Low Power",1,"QPLL",2.488,16,"8b/10b","QPLL",2.488,16,"8b/10b",1000,"No",null,1.8616000000000004E-2,1.8548340991735534E-2,5.7034257520661165E-2,3.1555199999999999E-2,125.75379851239671,null,107.13779851239669]
["Transmit (Ring)",1,"Transmitter","Low Power",0,"CPLL",2.488,16,"8b/10b","CPLL",2.488,16,"8b/10b",1000,"No",null,1.8616000000000004E-2,0,8.2593000000000014E-2,4.7080319999999988E-2,148.28932,null,129.67332000000002]
["Receive (Ring)",1,"Receiver","Low Power",0,"CPLL",1.244,16,"8b/10b","CPLL",1.244,16,"8b/10b",600,"No",null,9.9080000000000019E-3,0,8.7606960000000025E-2,5.0422559999999991E-2,147.93752000000001,null,138.02952000000002]
["Receive (LC)",1,"Receiver","Low Power",1,"QPLL",1.244,16,"8b/10b","QPLL",1.244,16,"8b/10b",600,"No",null,9.9080000000000019E-3,1.8548340991735534E-2,6.204821752066117E-2,4.265999999999999E-2,133.1645585123967,null,123.25655851239669]
[]
[]
["GTX","Num","Mode","Mode","Share QPLL","RX","RX Rate","RX Data","Data Mode","TX","TX Rate","TX Data","Data Mode","TX/OP","OOB","PCIe","Vccint","Vccaux","AVcc","AVtt","mW/Channel",null,"PMA"]
["12.5 DFE",1,"Transceiver","DFE",1,"QPLL",12.5,64,"8b/10b","QPLL",12.5,64,"8b/10b",600,"Yes",null,4.4950000000000011E-2,1.9761273223140488E-2,0.26991143657024796,0.10663754553719008,{"$f":"SUM(Q165:T165)/B165*1000","v":441.26025533057856},null,{"$f":"SUM(R165:T165)/B165*1000","v":396.31025533057851}]
["12.5 LP",1,"Transceiver","Low Power",1,"QPLL",12.5,64,"8b/10b","QPLL",12.5,64,"8b/10b",600,"No",null,4.4950000000000011E-2,1.6786066611570245E-2,0.19243000578512395,9.9973677768595032E-2,354.13975016528923,null,309.18975016528924]
["10.3125 DFE",1,"Transceiver","DFE",1,"QPLL",10.3125,64,"8b/10b","QPLL",10.3125,64,"8b/10b",600,"Yes",null,3.7293750000000001E-2,1.8719950909090902E-2,0.23936676392045453,0.10646399181818181,401.84445664772727,null,364.55070664772728]
["10.3125 LP",1,"Transceiver","Low Power",1,"QPLL",10.3125,64,"8b/10b","QPLL",10.3125,64,"8b/10b",600,"No",null,3.7293750000000001E-2,1.8719950909090902E-2,0.18025668579545456,0.10029599181818181,336.56637852272729,null,299.2726285227273]
["10.3125 LP (64b/66b)",1,"Transceiver","Low Power",1,"QPLL",10.3125,64,"64b/66b","QPLL",10.3125,64,"64b/66b",600,"No",null,4.6317187500000009E-2,1.8719950909090902E-2,0.18025668579545456,0.10029599181818181,345.58981602272729,null,299.2726285227273]
["6.5 DFE",1,"Transceiver","DFE",1,"QPLL",6.5,40,"Raw","QPLL",6.5,40,"Raw",600,"No",null,2.3950000000000003E-2,1.6905074876033054E-2,0.18613176301652895,9.1161512479338833E-2,318.14835037190085,null,294.19835037190086]
["6.5 LP",1,"Transceiver","Low Power",1,"QPLL",6.5,40,"Raw","QPLL",6.5,40,"Raw",600,"No",null,2.3950000000000003E-2,1.6905074876033054E-2,0.15450313801652893,9.9993512479338839E-2,295.35172537190084,null,271.40172537190085]
["6.5 Ring DFE",1,"Transceiver","DFE",0,"CPLL",6.5,40,"Raw","CPLL",6.5,40,"Raw",600,"No",null,2.3950000000000003E-2,0,0.18195176402439026,0.115494,321.39576402439025,null,297.44576402439026]
["6.5 Ring LP",1,"Transceiver","Low Power",0,"CPLL",6.5,40,"Raw","CPLL",6.5,40,"Raw",600,"No",null,2.3950000000000003E-2,0,0.15032313902439026,0.12432599999999999,298.5991390243903,null,274.64913902439025]
["6.5 Ring+LC DFE",1,"Transceiver","DFE",1,"CPLL",6.5,40,"Raw","QPLL",6.5,40,"Raw",600,"No",null,2.3950000000000003E-2,1.6905074876033054E-2,0.19778420204091918,0.12431151247933883,362.9507893962911,null,339.00078939629105]
["6.5 Ring+LC LP",1,"Transceiver","Low Power",1,"CPLL",6.5,40,"Raw","QPLL",6.5,40,"Raw",600,"No",null,2.3950000000000003E-2,1.6905074876033054E-2,0.16615557704091918,0.13314351247933884,340.15416439629109,null,316.20416439629105]
["3.125 LC",1,"Transceiver","Low Power",1,"QPLL",3.125,20,"Raw","QPLL",3.125,20,"Raw",600,"No",null,2.3075000000000002E-2,1.6786066611570245E-2,0.13300656828512397,9.9973677768595032E-2,272.84131266528919,null,249.76631266528926]
["3.125 Ring",1,"Transceiver","Low Power",0,"CPLL",3.125,20,"Raw","CPLL",3.125,20,"Raw",600,"No",null,2.3075000000000002E-2,0,0.12848253079268296,0.12305099999999999,274.60853079268298,null,251.53353079268294]
["PCIe GEN1",1,"Transceiver","Low Power",1,"CPLL",2.5,32,"8b/10b","CPLL",2.5,32,"8b/10b",600,"Yes","PCIe",3.4950000000000002E-2,0,0.12228011463414633,0.13167599999999999,288.90611463414626,null,253.9561146341463]
["PCIe GEN2x8",8,"Transceiver","Low Power",4,"QPLL",5,32,"8b/10b","QPLL",5,32,"8b/10b",600,"Yes","PCIe",0.2316,3.7142381157024784E-2,1.1716259140495868,0.92216958743801647,295.31723533057851,null,266.36723533057847]
["Mixed rate",1,"Transceiver","Low Power",1,"QPLL",6.25,64,"8b/10b","QPLL",3.125,32,"8b/10b",600,"No",null,2.3075000000000002E-2,1.6786066611570245E-2,0.14211203703512398,9.9973677768595032E-2,281.94678141528931,null,258.87178141528926]
["Transmit min TX/OP",1,"Transmitter","Low Power",1,"QPLL",2.488,16,"8b/10b","QPLL",2.488,16,"8b/10b",250,"No",null,1.8616000000000004E-2,1.8548340991735534E-2,8.1261523867768609E-2,2.1301390165289254E-2,139.72725502479341,null,121.11125502479341]
["Transmit max TX/OP",1,"Transmitter","Low Power",1,"QPLL",2.488,16,"8b/10b","QPLL",2.488,16,"8b/10b",1000,"No",null,1.8616000000000004E-2,1.8548340991735534E-2,8.1261523867768609E-2,4.1371390165289255E-2,159.79725502479343,null,141.18125502479339]
["Transmit (Ring)",1,"Transmitter","Low Power",0,"CPLL",2.488,16,"8b/10b","CPLL",2.488,16,"8b/10b",1000,"No",null,1.8616000000000004E-2,0,7.2911618243902465E-2,5.7657599999999996E-2,149.18521824390245,null,130.56921824390247]
["Receive (Ring)",1,"Receiver","Low Power",0,"CPLL",1.244,16,"8b/10b","CPLL",1.244,16,"8b/10b",600,"No",null,9.9080000000000019E-3,0,8.1425095243902457E-2,9.6837599999999996E-2,188.17069524390246,null,178.26269524390244]
["Receive (LC)",1,"Receiver","Low Power",1,"QPLL",1.244,16,"8b/10b","QPLL",1.244,16,"8b/10b",600,"No",null,9.9080000000000019E-3,1.8548340991735534E-2,8.9775000867768628E-2,8.0551390165289241E-2,198.7827320247934,null,188.87473202479342]
[]
["GTP","Num","Mode","RX Rate","RX Data","Data Mode","TX Rate","TX Data","Data Mode","TX/OP","OOB","PCIe","Vccint","AVcc","AVtt",null,null,null,null,null,"mW/Channel",null,"PMA"]
["3G-SDI",1,"Transceiver",2.97,40,"Raw",2.97,40,"Raw",600,null,null,1.308E-2,7.1155600000000013E-2,5.192759999999999E-2,null,null,null,null,null,{"$f":"SUM(M188:O188)/B188*1000","v":136.16319999999999},null,{"$f":"SUM(N188:O188)/B188*1000","v":123.08320000000001}]
["3G-SDI",1,"Transceiver",1.4850000000000001,20,"Raw",1.4850000000000001,20,"Raw",600,null,null,7.1400000000000005E-3,6.2572299999999997E-2,5.0323799999999995E-2,null,null,null,null,null,120.0361,null,112.8961]
["Aurora",1,"Transceiver",6.25,64,"8b/10b",6.25,64,"8b/10b",1000,null,null,2.6200000000000001E-2,9.0687500000000004E-2,6.266999999999999E-2,null,null,null,null,null,179.55749999999998,null,153.35749999999999]
["Aurora",1,"Transceiver",3.125,32,"8b/10b",3.125,32,"8b/10b",600,null,null,1.37E-2,7.2624999999999995E-2,5.2094999999999995E-2,null,null,null,null,null,138.41999999999999,null,124.72]
["Aurora",1,"Transceiver",2.5,16,"8b/10b",2.5,16,"8b/10b",600,null,null,1.12E-2,6.6700000000000009E-2,5.142E-2,null,null,null,null,null,129.32000000000002,null,118.12]
["Aurora",1,"Transceiver",1.25,16,"8b/10b",1.25,16,"8b/10b",600,null,null,6.2000000000000006E-3,5.9475E-2,5.0069999999999996E-2,null,null,null,null,null,115.74499999999999,null,109.545]
["CPRI/OBSAI",1,"Transceiver",0.61439999999999995,16,"Raw",0.61439999999999995,16,"Raw",250,null,null,4.2720000000000006E-3,4.6551231999999998E-2,4.3083551999999997E-2,null,null,null,null,null,93.906783999999988,null,89.634783999999996]
["PCIe Gen1",1,"Transceiver",2.5,20,"8b/10b",2.5,20,"8b/10b",600,"Yes","PCIe",3.6200000000000003E-2,6.6700000000000009E-2,6.6419999999999993E-2,null,null,null,null,null,169.32000000000002,null,133.12]
["PCIe Gen2x4",4,"Transceiver",5,32,"8b/10b",5,32,"8b/10b",600,"Yes","PCIe",0.31680000000000003,0.32460000000000006,0.27648,null,null,null,null,null,229.47,null,150.27000000000001]
["GPON",1,"Transceiver",2.488,16,"Raw",1.244,16,"Raw",600,null,null,1.3639999999999999E-2,6.2854240000000006E-2,5.1407040000000001E-2,null,null,null,null,null,127.90128,null,114.26128000000001]
["DisplayPort",1,"Transceiver",2.7,32,"Raw",2.7,32,"Raw",600,null,null,1.47E-2,6.8596000000000004E-2,5.1635999999999994E-2,null,null,null,null,null,134.93199999999999,null,120.232]
["DisplayPort",1,"Transceiver",1.62,16,"Raw",1.62,16,"Raw",600,null,null,9.2999999999999992E-3,5.8357600000000003E-2,5.0469599999999996E-2,null,null,null,null,null,118.12719999999999,null,108.8272]
["SMPTE",1,"Transceiver",1.4850000000000001,20,"Raw",1.4850000000000001,20,"Raw",600,null,null,7.1400000000000005E-3,6.2572299999999997E-2,5.0323799999999995E-2,null,null,null,null,null,120.0361,null,112.8961]
["SRIO",1,"Transceiver",3.125,40,"Raw",3.125,40,"Raw",600,null,null,1.37E-2,7.2624999999999995E-2,5.2094999999999995E-2,null,null,null,null,null,138.41999999999999,null,124.72]
["SRIO",1,"Transmitter",3.125,40,"Raw",3.125,40,"Raw",600,null,null,1.37E-2,4.3937500000000004E-2,3.7694999999999999E-2,null,null,null,null,null,95.33250000000001,null,81.632499999999993]
["SRIO",1,"Receiver",3.125,40,"Raw",3.125,40,"Raw",600,null,null,1.37E-2,5.0250000000000003E-2,1.9635E-2,null,null,null,null,null,83.585000000000008,null,69.885000000000005]
[]
["GTZ","Num","Mode","Power","DataRate","DataPath","TX/OP","Vccint","Avcch","Avcc","Avcclsb"]
["Fibre Channel",1,"Transceiver","Functional",28.05,40,1000,0.18046163849999999,4.1435999999999999E-3,0.34872729375,0.10662113549999999,null,null,null,null,null,null,null,null,null,{"$f":"SUM(H206:K206)/B206*1000","v":639.95366774999991},null,{"$f":"SUM(I206:K206)/B206*1000","v":459.49202924999997}]
["Fibre Channel (CTLE)",1,"Transceiver","CTLE Tuning",28.05,40,1000,0.18046163849999999,4.1435999999999999E-3,0.42133045249999995,0.10662113549999999,null,null,null,null,null,null,null,null,null,{"$f":"SUM(H207:K207)/B207*1000","v":712.55682649999994},null,{"$f":"SUM(I207:K207)/B207*1000","v":532.09518800000001}]
["100GE-R4",1,"Transceiver","Functional",25.78125,80,1000,0.1658654765625,4.1435999999999999E-3,0.32167046484374995,9.7997367187500004E-2,null,null,null,null,null,null,null,null,null,{"$f":"SUM(H208:K208)/B208*1000","v":589.67690859374989},null,{"$f":"SUM(I208:K208)/B208*1000","v":423.81143203124998}]
["OUT-4",1,"Transceiver","Functional",27.952493400000002,80,1000,0.17983432296343801,4.1435999999999999E-3,0.347564442226725,0.106250502187674,null,null,null,null,null,null,null,null,null,{"$f":"SUM(H209:K209)/B209*1000","v":637.79286737783696},null,{"$f":"SUM(I209:K209)/B209*1000","v":457.95854441439906}]
[]
["IOB18 Tests","Bank","Std","Input","Output","Bidir","SERDES","DELAY","IBUF_LP","ODT","Clock","Toggle","Rate","Enable","Term","IBUF","Load","Rate","Vccint","Vccaux","Vccauxpd","Vcco"]
["LVDS 1.8V (input)","HP","LVDS 1.8V (Pair)",10,0,0,"No",null,"Low Power",null,800,0.35,"SDR",0,0,0,0,280,1.1514712559999999E-2,2.9001599999999995E-2,0,0]
["LVDS 1.8V (input 2v)","HP","LVDS 1.8V (Pair)",10,0,0,"No",null,"Low Power",null,800,0.35,"SDR",0,0,0,0,280,1.1514712559999999E-2,0,4.5369599999999996E-2,0]
["LVDS 1.8V (input HP)","HP","LVDS 1.8V (Pair)",10,0,0,"No",null,"High Perf",null,800,0.35,"SDR",0,0,0,0,280,1.1528712560000001E-2,5.7555599999999998E-2,0,0]
["LVDS 1.8V (input 2v HP)","HP","LVDS 1.8V (Pair)",10,0,0,"No",null,"High Perf",null,800,0.35,"SDR",0,0,0,0,280,1.1528712560000001E-2,0,9.0472000000000011E-2,0]
["LVDS 1.8V (input 2v HP)","HP","LVDS 1.8V (Pair)",10,0,0,"No",null,"High Perf","DIFF_TERM",800,0.35,"SDR",0,0,0,0,280,1.1528712560000001E-2,0,9.0472000000000011E-2,2.2049999999999997E-2]
["SSTL 1.5V (input)","HP","SSTL 1.5V",10,0,0,"No",null,"Low Power",null,1066,0.35,"DDR",0,0,0,0,746.19999999999993,1.9923189673700003E-2,3.1735007000000003E-2,0,0]
["SSTL 1.5V (input 2v)","HP","SSTL 1.5V",10,0,0,"No",null,"Low Power",null,1066,0.35,"DDR",0,0,0,0,746.19999999999993,1.9923189673700003E-2,0,4.629544E-2,0]
["SSTL 1.5V (input HP)","HP","SSTL 1.5V",10,0,0,"No",null,"High Perf",null,1066,0.35,"DDR",0,0,0,0,746.19999999999993,1.9923189673700003E-2,6.3220774000000007E-2,0,0]
["SSTL 1.5V (input 2v HP)","HP","SSTL 1.5V",10,0,0,"No",null,"High Perf",null,1066,0.35,"DDR",0,0,0,0,746.19999999999993,1.9923189673700003E-2,0,9.1630447000000004E-2,0]
["SSTL 1.8V (input)","HP","SSTL Class II 1.8V",10,0,0,"No",null,"Low Power",null,500,0.35,"DDR",0,0,0,0,350,1.1080304725000002E-2,3.1344750000000005E-2,0,0]
["SSTL 1.8V (input 2v)","HP","SSTL Class II 1.8V",10,0,0,"No",null,"Low Power",null,500,0.35,"DDR",0,0,0,0,350,1.1080304725000002E-2,0,4.582E-2,0]
["SSTL 1.8V (input HP)","HP","SSTL Class II 1.8V",10,0,0,"No",null,"High Perf",null,500,0.35,"DDR",0,0,0,0,350,1.1080304725000002E-2,6.2519500000000006E-2,0,0]
["SSTL 1.8V (input 2v HP)","HP","SSTL Class II 1.8V",10,0,0,"No",null,"High Perf",null,500,0.35,"DDR",0,0,0,0,350,1.1080304725000002E-2,0,9.0764750000000005E-2,0]
["SSTL DCI 1.5V (input)","HP","SSTL DCI 1.5V",10,0,0,"No",null,"Low Power",null,1066,0.35,"SDR",0,0,0,0,373.09999999999997,1.4275313430600001E-2,3.1367503499999998E-2,0,0.11249999999999999]
["SSTL DCI 1.5V (input 50% idle)","HP","SSTL DCI 1.5V",10,0,0,"No",null,"Low Power",null,1066,0.35,"SDR",0,0.5,0.5,0,373.09999999999997,1.2410313430599999E-2,1.5867503500000001E-2,0,5.6249999999999994E-2]
["SSTL DCI 1.5V (bidi)","HP","SSTL DCI 1.5V",0,0,10,"No",null,"High Perf",null,1066,0.35,"DDR",0.5,0,0,0,746.19999999999993,1.9162565673699998E-2,7.5051659000000007E-2,0,0.13529453749999998]
["SSTL DCI 1.5V (bidi 50% idle)","HP","SSTL DCI 1.5V",0,0,10,"No",null,"High Perf",null,1066,0.35,"DDR",0.5,0,0,0,746.19999999999993,1.8230065673699999E-2,3.1910659000000001E-2,0,7.9044537499999998E-2]
["POD DCI 1.2V","HP","POD DCI 1.2V",10,0,0,"No",null,"High Perf",null,1066,0.35,"DDR",0.5,0,0,0,746.19999999999993,1.8230065673699999E-2,5.957665899999999E-2,0,7.9044537499999998E-2]
["POD DCI 1.2V (50% idle)","HP","POD DCI 1.2V",10,0,0,"No",null,"High Perf",null,1066,0.35,"DDR",0.5,0.5,0.5,0,746.19999999999993,1.7763815673699997E-2,2.4173159E-2,0,5.0919537500000001E-2]
["POD DCI 1.2V (40 Ohm)","HP","POD DCI 1.2V",0,0,10,"No",null,"High Perf","DCI 60Ω",1066,0.35,"DDR",0.5,0,0,0,746.19999999999993,1.8230065673699999E-2,5.957665899999999E-2,0,6.9669537500000003E-2]
["POD DCI 1.2V (60 Ohm)","HP","POD DCI 1.2V",0,0,10,"No",null,"High Perf","DCI 40Ω",1066,0.35,"DDR",0.5,0,0,0,746.19999999999993,1.8230065673699999E-2,5.957665899999999E-2,0,9.3107037500000003E-2]
["LVCMOS 1.2V 8mA (Fast)","HP","LVCMOS 1.2V 8mA (Fast)",0,10,0,"No",null,"Low Power",null,400,0.35,"DDR",1,0,0,5,280,1.1165562800000003E-3,4.1659139999999989E-3,0,3.024E-2]
["LVCMOS 1.5V 8mA (Fast)","HP","LVCMOS 1.5V 8mA (Fast)",0,10,0,"No",null,"Low Power",null,400,0.35,"DDR",1,0,0,5,280,1.1165562800000003E-3,4.1659139999999989E-3,0,4.725E-2]
["LVCMOS 1.8V 8mA (Fast)","HP","LVCMOS 1.8V 8mA (Fast)",0,10,0,"No",null,"Low Power",null,400,0.35,"DDR",1,0,0,5,280,1.1165562800000003E-3,4.6700609999399999E-3,0,6.8040000000000003E-2]
["LVCMOS 1.8V 12mA (Slow)","HP","LVCMOS 1.8V 12mA (Slow)",10,0,0,"No",null,"High Perf",null,500,0.35,"SDR",0,0,0,0,175,1.2618726750000002E-3,0,0,4.1387499999999996E-4]
[]
["IOB33 Tests","Bank","Std","Input","Output","Bidir","SERDES","DELAY","IBUF_LP","ODT","Clock","Toggle","Rate","Enable","Term","IBUF","Load","Rate","Vccint","Vccaux","Vccauxpd","Vcco"]
["LVDS 2.5V ","HR","LVDS 2.5V (Pair)",10,0,0,"No","Off","Low Power","None",600,0.35,"SDR",0,0,0,0,210,6.7948344200000014E-3,1.85472E-2,0,0]
["LVDS 2.5V (DIFF_TERM)","HR","LVDS 2.5V (Pair)",10,0,0,"No","Off","Low Power","DIFF_TERM",600,0.35,"SDR",0,0,0,0,210,6.7948344200000014E-3,1.85472E-2,0,3.0624999999999996E-2]
["LVDS 2.5V (output)","HR","LVDS 2.5V (Pair)",0,10,0,"No","Off","High Perf","None",600,0.35,"SDR",1,0,0,0,210,1.6748344200000003E-3,4.7250000000000009E-3,0,0.36021427187499999]
["SSTL 1.35V","HR","SSTL 1.35V",0,0,10,"DDR3","High Perf","High Perf","None",600,0.35,"DDR",0.5,0,0,0,420,1.2181465670000001E-2,6.5260800000000008E-2,0,1.4021328125000003E-2]
["SSTL 1.35V R","HR","SSTL 1.35V R",0,0,10,"DDR3","Low Power","Low Power","None",1066,0.35,"DDR",0.5,0,0,0,746.19999999999993,2.1137570673699996E-2,3.4086978000000004E-2,0,8.5137398437500015E-3]
["SSTL 1.5V","HR","SSTL 1.5V",0,0,10,"DDR3","High Perf","High Perf","None",1066,0.35,"DDR",0.5,0,0,0,746.19999999999993,2.1137570673699996E-2,8.0996688000000011E-2,0,2.0468492187499999E-2]
["SSTL 1.5V R","HR","SSTL 1.5V R",0,0,10,"DDR3","Low Power","Low Power","None",1066,0.35,"DDR",0.5,0,0,0,746.19999999999993,2.1137570673699996E-2,3.4086978000000004E-2,0,9.522210937499994E-3]
["HSUL 1.2V","HR","HSUL 1.2V",0,0,10,"Yes","Low Power","Low Power","None",533,0.35,"DDR",0.5,0,0,0,373.09999999999997,1.128261533685E-2,2.6059944007499995E-2,0,2.6058959999999999E-2]
["SSTL 1.5V","HR","SSTL 1.5V",0,0,10,"DDR3","High Perf","High Perf","UNTUNED_SPLIT_40",1066,0.35,"DDR",0.5,0,0,0,746.19999999999993,2.1137570673699996E-2,8.0996688000000011E-2,0,9.0780992187499993E-2]
["SSTL 1.5V","HR","SSTL 1.5V",0,0,10,"DDR3","High Perf","High Perf","UNTUNED_SPLIT_50",1066,0.35,"DDR",0.5,0,0,0,746.19999999999993,2.1137570673699996E-2,8.0996688000000011E-2,0,7.6718492187499987E-2]
["SSTL 1.5V","HR","SSTL 1.5V",0,0,10,"DDR3","High Perf","High Perf","UNTUNED_SPLIT_60",1066,0.35,"DDR",0.5,0,0,0,746.19999999999993,2.1137570673699996E-2,8.0996688000000011E-2,0,6.7343492187499993E-2]
["Diff SSTL 1.5V (pair)","HR","Diff SSTL 1.5V (pair)",0,10,0,"Yes","Low Power","Low Power","None",533,0.35,"DDR",1,0,0,0,373.09999999999997,1.28763306737E-2,8.5545575999999998E-2,0,6.1061984375000003E-2]
["Diff SSTL 1.5V R (pair)","HR","Diff SSTL 1.5V R (pair)",0,10,0,"Yes","Low Power","Low Power","None",533,0.35,"DDR",1,0,0,0,373.09999999999997,1.28763306737E-2,5.2638155999999998E-2,0,2.9169421874999983E-2]
["HDMI","HR","TMDS 3.3V (pair)",0,19,0,"No","Off","Low Power","None",200,0.35,"DDR",1,0,0,0,140,2.1214569320000005E-3,5.9850000000000007E-3,0,0.88973674659899993]
["LVCMOS 1.2V 8mA (Fast)","HR","LVCMOS 1.2V 8mA (Fast)",0,10,0,"No","Off","Low Power","None",400,0.35,"DDR",1,0,0,5,280,1.1165562800000003E-3,4.1659139999999989E-3,0,3.024E-2]
["LVCMOS 1.5V 8mA (Fast)","HR","LVCMOS 1.5V 8mA (Fast)",0,10,0,"No","Off","Low Power","None",400,0.35,"DDR",1,0,0,5,280,1.1165562800000003E-3,4.1659139999999989E-3,0,4.725E-2]
["LVCMOS 1.8V 8mA (Fast)","HR","LVCMOS 1.8V 8mA (Fast)",0,10,0,"No","Off","Low Power","None",400,0.35,"DDR",1,0,0,5,280,1.1165562800000003E-3,4.6700609999399999E-3,0,6.8040000000000003E-2]
["LVCMOS 2.5V 8mA (Fast)","HR","LVCMOS 2.5V 8mA (Fast)",0,10,0,"No","Off","Low Power","None",400,0.35,"DDR",1,0,0,5,280,1.1165562800000003E-3,7.0641509999999994E-3,0,0.13125000000000001]
["LVCMOS 3.3V 8mA (Fast)","HR","LVCMOS 3.3V 8mA (Fast)",0,10,0,"No","Off","Low Power","None",400,0.35,"DDR",1,0,0,5,280,1.1165562800000003E-3,4.1563260000000001E-3,0,0.22869]
[]
[null,"Output (10)",null,null,"Input (10)",null,null,"Bidi (10)"]
["IO Tests","Vccint","Vccaux","Vcco","Vccint","Vccaux","Vcco","Vccint","Vccaux","Vcco"]
["BLVDS 2.5V (pair)",1.5950804000000006E-3,4.4999999999999997E-3,0.35978331250000001,10]
["Diff HSTL Class I 1.5V (pair)",1.5950804000000006E-3,3.3119999999999997E-2,6.8920009000000004E-2,10]
["Diff HSTL Class I 1.8V (pair)",1.5950804000000006E-3,3.3119999999999997E-2,0.12880001599999999,10]
["Diff HSTL Class II 1.5V (pair)",1.5950804000000006E-3,3.3119999999999997E-2,0.11410000000000001,10]
["Diff HSTL Class II 1.8V (pair)",1.5950804000000006E-3,3.3119999999999997E-2,0.16519998399999999,10]
["Diff HSUL 1.2V (pair)",1.5950804000000006E-3,3.3119999999999997E-2,8.9279999999999998E-2,10]
["Diff SSTL 1.35V (pair)",1.5950804000000006E-3,3.3119999999999997E-2,4.5040625000000008E-2,10]
["Diff SSTL 1.35V R (pair)",1.5950804000000006E-3,1.5480000000000001E-2,2.2303125000000004E-2,10]
["Diff SSTL 1.5V (pair)",1.5950804000000006E-3,3.3119999999999997E-2,5.1406250000000001E-2,10]
["Diff SSTL 1.5V R (pair)",1.5950804000000006E-3,1.5480000000000001E-2,2.5031249999999988E-2,10]
["Diff SSTL Class I 1.8V (pair)",1.5950804000000006E-3,3.3119999999999997E-2,9.2142858742857145E-2,10]
["Diff SSTL Class II 1.8V (pair)",1.5950804000000006E-3,3.3119999999999997E-2,0.1268,10]
["HSTL Class I 1.5V",7.975402000000003E-4,1.6559999999999998E-2,4.4500004500000002E-2,10]
["HSTL Class I 1.2V",7.975402000000003E-4,1.6559999999999998E-2,2.726400272E-2,10]
["HSTL Class I 1.8V",7.975402000000003E-4,1.6559999999999998E-2,6.4400007999999995E-2,10]
["HSTL Class II 1.5V",7.975402000000003E-4,1.6559999999999998E-2,5.7050000000000003E-2,10]
["HSTL Class II 1.8V",7.975402000000003E-4,1.6559999999999998E-2,8.2599991999999997E-2,10]
["HSUL 1.2V",7.975402000000003E-4,4.8822728571428567E-3,4.4639999999999999E-2,10]
["LVCMOS 1.2V 2mA (Slow)",7.975402000000003E-4,2.216745E-3,1.44E-2,10]
["LVCMOS 1.2V 2mA (Fast)",7.975402000000003E-4,2.216745E-3,1.44E-2,10]
["LVCMOS 1.2V 4mA (Slow)",7.975402000000003E-4,2.7939964285714288E-3,1.44E-2,10]
["LVCMOS 1.2V 4mA (Fast)",7.975402000000003E-4,2.7939964285714288E-3,1.44E-2,10]
["LVCMOS 1.2V 6mA (Slow)",7.975402000000003E-4,4.8822728571428567E-3,1.44E-2,10]
["LVCMOS 1.2V 6mA (Fast)",7.975402000000003E-4,4.8822728571428567E-3,1.44E-2,10]
["LVCMOS 1.2V 8mA (Slow)",7.975402000000003E-4,2.9756528571428563E-3,1.44E-2,10]
["LVCMOS 1.2V 8mA (Fast)",7.975402000000003E-4,2.9756528571428563E-3,1.44E-2,10]
["LVCMOS 1.5V 2mA (Slow)",7.975402000000003E-4,2.216745E-3,2.2499999999999999E-2,10]
["LVCMOS 1.5V 2mA (Fast)",7.975402000000003E-4,2.216745E-3,2.2499999999999999E-2,10]
["LVCMOS 1.5V 4mA (Slow)",7.975402000000003E-4,2.7939964285714288E-3,2.2499999999999999E-2,10]
["LVCMOS 1.5V 4mA (Fast)",7.975402000000003E-4,2.7939964285714288E-3,2.2499999999999999E-2,10]
["LVCMOS 1.5V 6mA (Slow)",7.975402000000003E-4,4.8822728571428567E-3,2.2499999999999999E-2,10]
["LVCMOS 1.5V 6mA (Fast)",7.975402000000003E-4,4.8822728571428567E-3,2.2499999999999999E-2,10]
["LVCMOS 1.5V 8mA (Slow)",7.975402000000003E-4,2.9756528571428563E-3,2.2499999999999999E-2,10]
["LVCMOS 1.5V 8mA (Fast)",7.975402000000003E-4,2.9756528571428563E-3,2.2499999999999999E-2,10]
["LVCMOS 1.5V 12mA (Slow)",7.975402000000003E-4,5.5982914285714275E-3,2.2499999999999999E-2,10]
["LVCMOS 1.5V 12mA (Fast)",7.975402000000003E-4,5.5982914285714275E-3,2.2499999999999999E-2,10]
["LVCMOS 1.5V 16mA (Slow)",7.975402000000003E-4,5.9655364285714288E-3,2.2499999999999999E-2,10]
["LVCMOS 1.5V 16mA (Fast)",7.975402000000003E-4,5.9655364285714288E-3,2.2499999999999999E-2,10]
["LVCMOS 1.8V 2mA (Slow)",7.975402000000003E-4,2.2161942857142855E-3,3.2399999999999998E-2,10]
["LVCMOS 1.8V 2mA (Fast)",7.975402000000003E-4,2.2161942857142855E-3,3.2399999999999998E-2,10]
["LVCMOS 1.8V 4mA (Slow)",7.975402000000003E-4,2.7885642857142855E-3,3.2399999999999998E-2,10]
["LVCMOS 1.8V 4mA (Fast)",7.975402000000003E-4,2.7885642857142855E-3,3.2399999999999998E-2,10]
["LVCMOS 1.8V 6mA (Slow)",7.975402000000003E-4,4.8802414285714279E-3,3.2399999999999998E-2,10]
["LVCMOS 1.8V 6mA (Fast)",7.975402000000003E-4,4.8802414285714279E-3,3.2399999999999998E-2,10]
["LVCMOS 1.8V 8mA (Slow)",7.975402000000003E-4,3.3357578570999999E-3,3.2399999999999998E-2,10]
["LVCMOS 1.8V 8mA (Fast)",7.975402000000003E-4,3.3357578570999999E-3,3.2399999999999998E-2,10]
["LVCMOS 1.8V 12mA (Slow)",7.975402000000003E-4,5.5992342857142871E-3,3.2399999999999998E-2,10]
["LVCMOS 1.8V 12mA (Fast)",7.975402000000003E-4,5.5992342857142871E-3,3.2399999999999998E-2,10]
["LVCMOS 1.8V 16mA (Slow)",7.975402000000003E-4,5.9126528571428567E-3,3.2399999999999998E-2,10]
["LVCMOS 1.8V 16mA (Fast)",7.975402000000003E-4,5.9126528571428567E-3,3.2399999999999998E-2,10]
["LVCMOS 1.8V 24mA (Slow)",7.975402000000003E-4,6.4404968946262919E-3,3.2399999999999998E-2,10]
["LVCMOS 1.8V 24mA (Fast)",7.975402000000003E-4,6.4404968946262919E-3,3.2399999999999998E-2,10]
["LVCMOS 2.5V 2mA (Slow)",7.975402000000003E-4,2.2181464285714286E-3,6.25E-2,10]
["LVCMOS 2.5V 2mA (Fast)",7.975402000000003E-4,2.2181464285714286E-3,6.25E-2,10]
["LVCMOS 2.5V 4mA (Slow)",7.975402000000003E-4,2.7798300000000001E-3,6.25E-2,10]
["LVCMOS 2.5V 4mA (Fast)",7.975402000000003E-4,2.7798300000000001E-3,6.25E-2,10]
["LVCMOS 2.5V 6mA (Slow)",7.975402000000003E-4,4.872321428571429E-3,6.25E-2,10]
["LVCMOS 2.5V 6mA (Fast)",7.975402000000003E-4,4.872321428571429E-3,6.25E-2,10]
["LVCMOS 2.5V 8mA (Slow)",7.975402000000003E-4,5.0458221428571421E-3,6.25E-2,10]
["LVCMOS 2.5V 8mA (Fast)",7.975402000000003E-4,5.0458221428571421E-3,6.25E-2,10]
["LVCMOS 2.5V 12mA (Slow)",7.975402000000003E-4,5.0458221428571421E-3,6.25E-2,10]
["LVCMOS 2.5V 12mA (Fast)",7.975402000000003E-4,5.0458221428571421E-3,6.25E-2,10]
["LVCMOS 2.5V 16mA (Slow)",7.975402000000003E-4,5.0458221428571421E-3,6.25E-2,10]
["LVCMOS 2.5V 16mA (Fast)",7.975402000000003E-4,5.0458221428571421E-3,6.25E-2,10]
["LVCMOS 3.3V 2mA (Slow)",7.975402000000003E-4,2.2024971428571427E-3,0.1089,10]
["LVCMOS 3.3V 2mA (Fast)",7.975402000000003E-4,2.2024971428571427E-3,0.1089,10]
["LVCMOS 3.3V 4mA (Slow)",7.975402000000003E-4,2.7946135714285716E-3,0.1089,10]
["LVCMOS 3.3V 4mA (Fast)",7.975402000000003E-4,2.7946135714285716E-3,0.1089,10]
["LVCMOS 3.3V 6mA (Slow)",7.975402000000003E-4,4.8779164285714287E-3,0.1089,10]
["LVCMOS 3.3V 6mA (Fast)",7.975402000000003E-4,4.8779164285714287E-3,0.1089,10]
["LVCMOS 3.3V 8mA (Slow)",7.975402000000003E-4,2.9688042857142858E-3,0.1089,10]
["LVCMOS 3.3V 8mA (Fast)",7.975402000000003E-4,2.9688042857142858E-3,0.1089,10]
["LVCMOS 3.3V 12mA (Slow)",7.975402000000003E-4,7.690251428571427E-3,0.1089,10]
["LVCMOS 3.3V 12mA (Fast)",7.975402000000003E-4,7.690251428571427E-3,0.1089,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
["LVCMOS 3.3V 16mA (Slow)",7.975402000000003E-4,6.6371549999999988E-3,0.1089,10]
["LVCMOS 3.3V 16mA (Fast)",7.975402000000003E-4,6.6371549999999988E-3,0.1089,10]
["LVDS 2.5V (pair)",1.5950804000000006E-3,4.4999999999999997E-3,0.3595016875,10]
["MINI LVDS 2.5V (pair)",1.5950804000000006E-3,4.4999999999999997E-3,0.3560016875,10]
["LVTTL 3.3V 2mA (Slow)",7.975402000000003E-4,2.2094292857142862E-3,0.1089,10]
["LVTTL 3.3V 2mA (Fast)",7.975402000000003E-4,2.2094292857142862E-3,0.1089,10]
["LVTTL 3.3V 4mA (Slow)",7.975402000000003E-4,2.7832457142857145E-3,0.1089,10]
["LVTTL 3.3V 4mA (Fast)",7.975402000000003E-4,2.7832457142857145E-3,0.1089,10]
["LVTTL 3.3V 6mA (Slow)",7.975402000000003E-4,4.8773335714285713E-3,0.1089,10]
["LVTTL 3.3V 6mA (Fast)",7.975402000000003E-4,4.8773335714285713E-3,0.1089,10]
["LVTTL 3.3V 8mA (Slow)",7.975402000000003E-4,2.9582699999999998E-3,0.1089,10]
["LVTTL 3.3V 8mA (Fast)",7.975402000000003E-4,2.9582699999999998E-3,0.1089,10]
["LVTTL 3.3V 12mA (Slow)",7.975402000000003E-4,7.690251428571427E-3,0.1089,10]
["LVTTL 3.3V 12mA (Fast)",7.975402000000003E-4,7.690251428571427E-3,0.1089,10]
["LVTTL 3.3V 16mA (Slow)",7.975402000000003E-4,6.6371549999999988E-3,0.1089,10]
["LVTTL 3.3V 16mA (Fast)",7.975402000000003E-4,6.6371549999999988E-3,0.1089,10]
["LVTTL 3.3V 24mA (Slow)",7.975402000000003E-4,9.6364221428571449E-3,0.1089,10]
["LVTTL 3.3V 24mA (Fast)",7.975402000000003E-4,9.6364221428571449E-3,0.1089,10]
["PPDS 2.5V (pair)",7.975402000000003E-4,1.0136117142857141E-2,0.16390005389999998,10]
["RSDS 2.5V (pair)",7.975402000000003E-4,1.0132161428571431E-2,0.16276335569999997,10]
["SSTL 1.35V",7.975402000000003E-4,8.6256492857142847E-3,0.16811666189999994,10]
["SSTL 1.35V R",1.5950804000000006E-3,4.4999999999999997E-3,0.3630016875,10]
["SSTL 1.5V",1.5950804000000006E-3,4.4999999999999997E-3,0.3595016875,10]
["SSTL 1.5V R",7.975402000000003E-4,1.6559999999999998E-2,2.2520312500000004E-2,10]
["SSTL Class I 1.8V",7.975402000000003E-4,7.7400000000000004E-3,1.1151562500000002E-2,10]
["SSTL Class II 1.8V",7.975402000000003E-4,1.6559999999999998E-2,2.5703125E-2,10]
["TMDS 3.3V (pair)",7.975402000000003E-4,7.7400000000000004E-3,1.2515624999999994E-2,10]
["Diff HSTL Class I 1.5V (pair)"]
["Diff HSTL Class I DCI 1.5V (pair)"]
["Diff HSTL Class I 1.8V (pair)"]
["Diff HSTL Class I DCI 1.8V (pair)",1.5950804000000006E-3,1.2666561428571445E-2,8.9000009000000005E-2,10]
["Diff HSUL 1.2V (pair)",1.5950804000000006E-3,1.2666561428571445E-2,8.9000009000000005E-2,10]
["Diff HSUL DCI 1.2V (pair)",1.5950804000000006E-3,1.4123974285714285E-2,0.12880001599999999,10]
["Diff POD 1.0V (pair)",1.5950804000000006E-3,1.4123974285714285E-2,0.13320000799999998,10]
["Diff POD DCI 1.0V (pair)",1.5950804000000006E-3,1.4742531428571432E-2,0.11410000000000001,10]
["Diff POD 1.2V (pair)",1.5950804000000006E-3,1.4742531428571432E-2,0.37074333300000001,10]
["Diff POD DCI 1.2V (pair)",1.5950804000000006E-3,1.4742531428571432E-2,0.11410000000000001,10]
["Diff SSTL 1.2V (pair)",1.5950804000000006E-3,2.1834702857142865E-2,0.16519998399999999,10]
["Diff SSTL DCI 1.2V (pair)",1.5950804000000006E-3,2.1834702857142865E-2,0.600800004,10]
["Diff SSTL 1.35V (pair)",1.5950804000000006E-3,2.1834702857142865E-2,0.16519998399999999,10]
["Diff SSTL DCI 1.35V (pair)",1.5950804000000006E-3,1.4123974285714285E-2,2.3099592959999998E-2,10]
["Diff SSTL 1.5V (pair)",1.5950804000000006E-3,1.4123974285714285E-2,9.5099592959999993E-2,10]
["Diff SSTL DCI 1.5V (pair)",1.5950804000000006E-3,2.3040000000000001E-3,4.5920000000000002E-2,10]
["Diff SSTL Class I 1.8V (pair)",1.5950804000000006E-3,2.3040000000000001E-3,4.5920000000000002E-2,10]
["Diff SSTL Class I DCI 1.8V (pair)",1.5950804000000006E-3,2.3040000000000001E-3,4.5920000000000002E-2,10]
["HSLV DCI 1.5V",1.5950804000000006E-3,2.3040000000000001E-3,5.2534999999999998E-2,10]
["HSLV DCI 1.8V",1.5950804000000006E-3,2.3040000000000001E-3,5.2534999999999998E-2,10]
["HSTL Class I 1.5V",1.5950804000000006E-3,2.3040000000000001E-3,5.2534999999999998E-2,10]
["HSTL Class I 1.2V",1.5950804000000006E-3,2.3040000000000001E-3,5.3900000000000003E-2,10]
["HSTL Class I 1.8V",1.5950804000000006E-3,2.3040000000000001E-3,5.3900000000000003E-2,10]
["HSTL Class I DCI 1.5V",1.5950804000000006E-3,2.3040000000000001E-3,5.3900000000000003E-2,10]
["HSTL Class I DCI 1.8V",1.5950804000000006E-3,7.7625600000000121E-3,0.10029022754285716,10]
["HSUL 1.2V",1.5950804000000006E-3,7.7625600000000121E-3,8.8990442422857141E-2,10]
["HSUL DCI 1.2V",1.5950804000000006E-3,2.0726601428571408E-2,0.13616,10]
["LVCMOS 1.2V 2mA (Slow)",1.5950804000000006E-3,2.0726601428571408E-2,0.52991999999999995,10]
["LVCMOS 1.2V 2mA (Fast)",1.5950804000000006E-3,2.0726601428571408E-2,0.13616,10]
["LVCMOS 1.2V 4mA (Slow)",7.975402000000003E-4,5.7600000000000004E-3,3.0436000000000005E-2,10]
["LVCMOS 1.2V 4mA (Fast)",7.975402000000003E-4,6.8399999999999997E-3,7.3650880000000002E-2,10]
["LVCMOS 1.2V 6mA (Slow)",7.975402000000003E-4,6.3332807142857149E-3,4.4500004500000002E-2,10]
["LVCMOS 1.2V 6mA (Fast)",7.975402000000003E-4,7.0619871428571424E-3,2.726400272E-2,10]
["LVCMOS 1.2V 8mA (Slow)",7.975402000000003E-4,7.0619871428571424E-3,6.4400007999999995E-2,10]
["LVCMOS 1.2V 8mA (Fast)",7.975402000000003E-4,6.3332807142857149E-3,4.4500004500000002E-2,10]
["LVCMOS 1.5V 2mA (Slow)",7.975402000000003E-4,7.0619871428571424E-3,6.660000399999999E-2,10]
["LVCMOS 1.5V 2mA (Fast)",7.975402000000003E-4,7.3712657142857149E-3,5.7050000000000003E-2,10]
["LVCMOS 1.5V 4mA (Slow)",7.975402000000003E-4,1.0917351428571431E-2,8.2599991999999997E-2,10]
["LVCMOS 1.5V 4mA (Fast)",7.975402000000003E-4,7.3712657142857149E-3,0.1853716665,10]
["LVCMOS 1.5V 6mA (Slow)",7.975402000000003E-4,1.0917351428571431E-2,0.300400002,10]
["LVCMOS 1.5V 6mA (Fast)",7.975402000000003E-4,7.3712657142857149E-3,5.7050000000000003E-2,10]
["LVCMOS 1.5V 8mA (Slow)",7.975402000000003E-4,1.0917351428571431E-2,8.2599991999999997E-2,10]
["LVCMOS 1.5V 8mA (Fast)",7.975402000000003E-4,1.3841365714285715E-2,8.3300003999999983E-2,10]
["LVCMOS 1.5V 12mA (Slow)",7.975402000000003E-4,1.0183180714285717E-2,0.10799999999999998,10]
["LVCMOS 1.5V 12mA (Fast)",7.975402000000003E-4,1.3841365714285715E-2,8.3933332499999985E-2,10]
["LVCMOS 1.8V 2mA (Slow)",7.975402000000003E-4,1.0183180714285717E-2,0.10826999999999998,10]
["LVCMOS 1.8V 2mA (Fast)",7.975402000000003E-4,4.8822728571428567E-3,8.6400000000000001E-3,10]
["LVCMOS 1.8V 4mA (Slow)",7.975402000000003E-4,4.8822728571428567E-3,4.4639999999999999E-2,10]
["LVCMOS 1.8V 4mA (Fast)",7.975402000000003E-4,2.216745E-3,1.44E-2,10]
["LVCMOS 1.8V 6mA (Slow)",7.975402000000003E-4,2.216745E-3,1.44E-2,10]
["LVCMOS 1.8V 6mA (Fast)",7.975402000000003E-4,2.7939964285714288E-3,1.44E-2,10]
["LVCMOS 1.8V 8mA (Slow)",7.975402000000003E-4,2.7939964285714288E-3,1.44E-2,10]
["LVCMOS 1.8V 8mA (Fast)",7.975402000000003E-4,4.8822728571428567E-3,1.44E-2,10]
["LVCMOS 1.8V 12mA (Slow)",7.975402000000003E-4,4.8822728571428567E-3,1.44E-2,10]
["LVCMOS 1.8V 12mA (Fast)",7.975402000000003E-4,2.9756528571428563E-3,1.44E-2,10]
["LVDCI 1.5V",7.975402000000003E-4,2.9756528571428563E-3,1.44E-2,10]
["LVDCI 1.8V",7.975402000000003E-4,2.216745E-3,2.2499999999999999E-2,10]
["LVDCI DV2 1.5V",7.975402000000003E-4,2.216745E-3,2.2499999999999999E-2,10]
["LVDCI DV2 1.8V",7.975402000000003E-4,2.7939964285714288E-3,2.2499999999999999E-2,10]
["LVDS 1.8V (pair)",7.975402000000003E-4,2.7939964285714288E-3,2.2499999999999999E-2,10]
["POD 1.0V",7.975402000000003E-4,4.8822728571428567E-3,2.2499999999999999E-2,10]
["POD DCI 1.0V",7.975402000000003E-4,4.8822728571428567E-3,2.2499999999999999E-2,10]
["POD 1.2V",7.975402000000003E-4,2.9756528571428563E-3,2.2499999999999999E-2,10]
["POD DCI 1.2V",7.975402000000003E-4,2.9756528571428563E-3,2.2499999999999999E-2,10]
["SSTL 1.2V",7.975402000000003E-4,5.5982914285714275E-3,2.2499999999999999E-2,10]
["SSTL DCI 1.2V",7.975402000000003E-4,5.5982914285714275E-3,2.2499999999999999E-2,10]
["SSTL 1.35V",7.975402000000003E-4,5.9655364285714288E-3,2.2499999999999999E-2,10]
["SSTL DCI 1.35V",7.975402000000003E-4,5.9655364285714288E-3,2.2499999999999999E-2]
["SSTL 1.5V",7.975402000000003E-4,2.2161942857142855E-3,3.2399999999999998E-2]
["SSTL DCI 1.5V",7.975402000000003E-4,2.2161942857142855E-3,3.2399999999999998E-2]
["SSTL Class I 1.8V",7.975402000000003E-4,2.7885642857142855E-3,3.2399999999999998E-2]
["SSTL Class I DCI 1.8V",7.975402000000003E-4,2.7885642857142855E-3,3.2399999999999998E-2]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Thermal Models","Ambient","Airflow","Heat sink","CustomSA","Board","Layers","CustomJB","Board temp","TJA","Junction"]
["JEDEC_0",50,0,"None",0,"JEDEC (2S2P)","8 to 11",0,50,4.9000000000000004,54.542047584284127,"Airflow",null,null,10.6,58.803239111693728]
["JEDEC_250",50,250,"None",0,"JEDEC (2S2P)","8 to 11",0,50,3.8,53.409168153055219,null,null,null,6.4,55.162820328576899]
["JEDEC_500",50,500,"None",0,"JEDEC (2S2P)","8 to 11",0,50,3.2,52.822959322607097,null,null,null,5.3,54.24319482892529]
["JEDEC_750",50,750,"None",0,"JEDEC (2S2P)","8 to 11",0,50,2.9,52.537467665097985,null,null,null,4.8,53.829705551334087]
["Medium_0",50,0,"None",0,"Medium (10\"x10\")","8 to 11",0,50,4.9000000000000004,54.542047584284127,null,null,null,6.12,54.927428317847749]
["Medium_250",50,250,"None",0,"Medium (10\"x10\")","8 to 11",0,50,2.596355421686745,52.253395421238793,null,null,null,3.3953846153846157,52.683041292593586]
["Medium_500",50,500,"None",0,"Medium (10\"x10\")","8 to 11",0,50,2.0106325301204806,51.718604343713601,null,null,null,2.7698351648351647,52.179375749448681]
["Medium_750",50,750,"None",0,"Medium (10\"x10\")","8 to 11",0,50,1.7038253012048172,51.445053840446917,null,null,null,2.4501098901098901,51.923596299210232]
["Small_250_4",50,250,"None",0,"Small (4\"x4\")","4 to 7",0,50,3.8,53.409168153055219,"Standard Board",null,null,6.1723076923076929,54.971334666042779]
["Medium_250_4",50,250,"None",0,"Medium (10\"x10\")","4 to 7",0,50,3.7931024096385526,53.402308794154806,null,null,null,4.8276923076923079,53.852533074932026]
["Large_250_4",50,250,"None",0,"Large (20\"x20\")","4 to 7",0,50,3.8,53.409168153055219,null,null,null,4.8861538461538476,53.900752735291782]
["Small_250_8",50,250,"None",0,"Small (4\"x4\")","8 to 11",0,50,3.8,53.409168153055219,null,null,null,5.6169230769230776,54.506741873680468]
["Medium_250_8",50,250,"None",0,"Medium (10\"x10\")","8 to 11",0,50,2.596355421686745,52.253395421238793,null,null,null,3.3953846153846157,52.683041292593586]
["Large_250_8",50,250,"None",0,"Large (20\"x20\")","8 to 11",0,50,2.4966265060240955,52.161134126649486,null,null,null,3.2492307692307705,52.564980704244356]
["Small_250_12",50,250,"None",0,"Small (4\"x4\")","12 to 15",0,50,3.8,53.409168153055219,null,null,null,5.3976923076923082,54.324312876850144]
["Medium_250_12",50,250,"None",0,"Medium (10\"x10\")","12 to 15",0,50,2.1119578313253,51.809919329755189,null,null,null,2.8107692307692318,52.212203273845496]
["Large_250_12",50,250,"None",0,"Large (20\"x20\")","12 to 15",0,50,1.8697590361445777,51.59245659786388,null,null,null,2.5476923076923086,52.001544127230829]
["Small_250_16",50,250,"None",0,"Small (4\"x4\")","16 or more",0,50,3.8,53.409168153055219,null,null,null,5.3976923076923082,54.324312876850144]
["Medium_250_16",50,250,"None",0,"Medium (10\"x10\")","16 or more",0,50,1.926746987951806,51.643375129492902,null,null,null,2.6207692307692314,52.05998498727611]
["Large_250_16",50,250,"None",0,"Large (20\"x20\")","16 or more",0,50,1.6133132530120471,51.365181623573719,null,null,null,2.27,51.779997732789802]
["Medium_250_Low",50,250,"Low Profile",0,"Medium (10\"x10\")","8 to 11",0,50,1.1015946026511969,50.920458460185309,"Heatsink",null,null,3.4468987059348506,52.724709442705702]
["Medium_500_Low",50,500,"Low Profile",0,"Medium (10\"x10\")","8 to 11",0,50,0.82294823669661732,50.683013507623876,null,null,null,2.4830014995457579,51.949858222190237]
["Medium_250_Med",50,250,"Medium Profile",0,"Medium (10\"x10\")","8 to 11",0,50,0.90666548633888278,50.754012015178439,null,null,null,2.9767400432625015,52.34549277703379]
["Medium_500_Med",50,500,"Medium Profile",0,"Medium (10\"x10\")","8 to 11",0,50,0.6595679200964204,50.545281723368944,null,null,null,2.1068874383842853,51.65025399059725]
["Medium_250_High",50,250,"High Profile",0,"Medium (10\"x10\")","8 to 11",0,50,0.81452031703595607,50.675882003082123,null,null,null,2.2656400966183576,51.776526013680737]
["Medium_500_High",50,500,"High Profile",0,"Medium (10\"x10\")","8 to 11",0,50,0.56056402458750143,50.462345204886965,null,null,null,1.522749960443607,51.187970473629505]
["Medium_250_12_Med",50,250,"Medium Profile",0,"Medium (10\"x10\")","12 to 15",0,50,0.83943206296644957,50.696970168307722,null,null,null,2.1068874383842853,51.65025399059725]
["Medium_250_12_High",50,250,"High Profile",0,"Medium (10\"x10\")","12 to 15",0,50,0.75984638472486365,50.629688918654374,null,null,null,1.522749960443607,51.187970473629505]
["Medium_250_12_Custom",50,250,"Custom",5.5,"Medium (10\"x10\")","12 to 15",0,50,1.5680826923931186,51.325406892440192,null,null,null,3.0388033546125923,52.395412522082133]
["Custom_250_Low",50,250,"Low Profile",0,"Custom","8 to 11",4.4000000000000004,50,1.2622366288492777,51.058838864817922,"Custom Board",null,null,2.7310344827586235,52.148275979023339]
["Custom_250_Med",50,250,"Medium Profile",0,"Custom","8 to 11",4.4000000000000004,50,0.98553791887125786,50.821167785015476,null,null,null,2.4444444444444398,51.919073975747395]
["Custom_250_High",50,250,"High Profile",0,"Custom","8 to 11",4.4000000000000004,50,0.86069469835465873,50.71498951582813,null,null,null,1.98,51.549523435500696]
["Custom_500_High",50,500,"High Profile",0,"Custom","8 to 11",4.4000000000000004,50,0.58145956607495497,50.479816915180763,null,null,null,1.5104477611940337,51.178274007365459]
["Custom_250_Cust_44",50,250,"Custom",3.3,"Custom","8 to 11",4.4000000000000004,50,1.908365508365516,51.626934733340541,null,null,null,1.9493670886075942,51.525231302649971]
["Custom_250_Cust_88",50,250,"Custom",3.3,"Custom","8 to 11",8.8000000000000007,50,2.4368118323746915,52.106039860146602,null,null,null,2.5040650406504086,51.966682332200094]
["Custom_250_Cust_50",50,250,"Custom",5.5,"Custom","8 to 11",4.4000000000000004,50,2.4581745235707113,52.125696002657399,null,null,null,2.4831683168316836,51.949991445451523]
["Custom_250_Cust_52",50,250,"Custom",5.5,"Custom","8 to 11",4.4000000000000004,52,4.0462742897814978,53.655987654376624,null,null,null,4.1523170086179562,53.101129619446283]
[]
["XPE Comparison Table for Automated Tests - Static Power (Vccint, Vccbram, Vccaux), Nominal Voltages",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"XPE Comparison Table for Automated Tests - Static Power (Vccint, Vccbram, Vccaux), Nominal Voltages"]
[null,"TT",null,null,null,null,"(TT+FF)/2",null,null,null,null,"FF2",null,null,null,null,"FF1.5",null,null,null,null,null,"TT","TT","FF3","FF2 (E/I)","FF1.5 (-2L)",null,null,null,null,"TT",null,null,null,null,"(TT+FF)/2",null,null,null,null,"FF2",null,null,null,null,"FF1.5"]
[null,0,25,85,100,125,0,25,85,100,125,0,25,85,100,125,0,25,85,100,125,null,25,85,85,100,85,100,125,null,null,0,25,85,100,125,0,25,85,100,125,0,25,85,100,125,0,25,85,100,125]
["XC7A100T",22.761414322633179,37.598935218740486,210.29110944572187,342.32796225536708,748.01377604951961,42.133518970357514,86.029032014548847,555.65683541428439,858.64707367036397,1694.1033217930963,31.14916666054582,59.294882102757178,368.39540330674566,579.85290887954056,1185.3629599427511,27.746818950330162,50.322802182622873,301.43353932414288,478.33212953515147,994.27320205036062,null,{"$f":"(C512-AG512)/AG512","v":-3.7378055447672446E-3},{"$f":"(D512-AH512)/AH512","v":-7.7799875166468125E-3},{"$f":"(I512-AM512)/AM512","v":-7.89737999163629E-3},{"$f":"(O512-AS512)/AS512","v":-8.1202379754694801E-3},{"$f":"(S512-AW512)/AW512","v":-7.9201575693032197E-3},{"$f":"(T512-AX512)/AX512","v":-8.1447154332694501E-3},{"$f":"(U512-AY512)/AY512","v":4.1540781796483954E-3},null,"7A100T",null,37.74,211.94,345.12,743.54,null,86.54,560.08000000000004,865.6,1691.3,null,59.6,371.34,584.6,1181.74,null,50.56,303.83999999999997,482.26,990.16]
["XC7A200T",34.827004200291512,63.878915361786582,432.60458175948781,717.09841396001673,1600.8574670206933,75.872815090845563,163.56865971034696,1163.8718142854816,1815.5180614580336,3630.6838874635787,53.076339248432205,108.86558450829185,767.51837424610926,1223.0605137097377,2540.1156916728437,45.885309430320902,90.543514516634517,625.71002726910217,1006.6940431327711,2128.918315499312,null,-4.3809949846230437E-3,-7.9696804267844652E-3,-7.9341496739788082E-3,-8.1577513058438411E-3,-8.0376244188113174E-3,-8.2027515391114563E-3,7.1045534317195408E-3,null,"7A200T",null,64.16,436.08,723.02,1584.96,null,164.6,1173.18,1830.24,3615.86,null,109.48,773.72,1233.1199999999999,2524.8000000000002,null,91.02,630.78,1015.02,2113.9]
["XC7K70T",62.658816104080472,99.156867370585317,317.55547908044559,481.90252021897243,955.07785143398348,86.029449878819364,161.83917674757976,762.41061124280532,1141.6049681432651,2135.8416070027306,71.998179743003348,127.06835713398739,522.74346499218848,788.40112403337878,1504.3442468710173,68.080742141487136,115.61890212417372,437.13733642726436,659.14024365938883,1266.7616890387005,null,2.394534680401491E-3,2.6379107111820094E-3,2.644149451348421E-3,2.6721658824606686E-3,2.6545631158868301E-3,2.6776653676546811E-3,-9.7235076307844916E-3,null,"7K70T",null,98.92,316.72000000000003,480.62,965.16,null,161.44,760.4,1138.58,2145.94,null,126.76,521.36,786.3,1516.64,null,115.34,435.98,657.38,1279.2]
["XC7K160T",70.813540421734388,128.27025457587283,594.35436541371166,947.96674406435545,1984.3981779990131,124.74360587134356,258.31978249816393,1545.6728817603287,2365.743347795978,4564.6992010773383,93.993942926474816,186.25568868682811,1033.0104745488998,1606.0433623512888,3185.5249023028723,84.625285091070623,162.5158581981438,849.63305793150255,1328.5804873187774,2667.1431349825048,null,2.2679682440445562E-3,2.6220739097700869E-3,2.6159685531826913E-3,2.6491212081963117E-3,2.6351875519265654E-3,2.6568512510961322E-3,-1.705605052024949E-3,null,"7K160T",null,127.98,592.79999999999995,945.46,1992.76,null,257.7,1541.64,2359.54,4546.82,null,185.82,1030.3,1601.8,3184.96,null,162.13999999999999,847.4,1325.06,2671.7]
["XC7K325T",126.8859708986385,229.80430403551605,1020.6440877692762,1621.8213519018598,3381.5940685122118,217.98498424086199,450.21413088537224,2640.471301508107,4039.0799278412378,7780.9321858141275,165.96462423995015,328.16700104346023,1766.8776299305646,2742.9222505379489,5426.2951332067169,150.13307354601963,287.94697673930131,1454.7509922138963,2269.7383335155851,4542.0817253692958,null,2.3741779443254966E-3,2.6367320614524882E-3,2.6090907913529316E-3,2.6473310248088504E-3,2.6403883149286327E-3,2.6586033235494032E-3,-3.4573996960631272E-3,null,"7K325T",null,229.26,1017.96,1617.52,3399.78,null,449.12,2633.6,4028.52,7762.06,null,327.38,1762.24,2735.68,5434.36,null,287.26,1450.92,2263.7199999999998,4557.84]
["XC7K410T",134.72306005779757,258.40505499325695,1339.3195668497212,2164.6105335238631,4600.1739117925908,259.03873889704477,553.90327117671302,3543.9760430184883,5461.8832816792747,10644.616205611885,188.72564394176231,390.15090103932124,2355.6575746623885,3694.5800967347573,7414.5641877020307,166.81702798711706,336.05681938006495,1930.4600687238112,3049.1715931580165,6200.1011989122708,null,2.3469937674823211E-3,2.6348007558925635E-3,2.6072613185868653E-3,2.6432889174990274E-3,2.638475897646755E-3,2.6541689382186184E-3,5.6178996166795505E-4,null,"7K410T",null,257.8,1335.8,2158.88,4610.5200000000004,null,552.55999999999995,3534.76,5447.62,10579.86,null,389.22,2349.48,3684.84,7396.3,null,335.26,1925.38,3041.1,6196.62]
["XC7K355T",168.78373747573016,301.48030744081677,1258.6206890297067,1990.9428222355264,4139.3598985107128,273.71866279780556,561.3283176567187,3205.7913592474756,4906.6085207391607,9460.1321316677095,213.17586037927151,417.48688014046246,2156.5888055932915,3344.0693895109098,6610.953001934362,194.91759910254834,369.98906010120754,1781.0592448535904,2773.2335707900343,5541.7627470476991,null,2.5282902394810646E-3,2.6613098509549338E-3,2.6181606568657038E-3,2.6533150769394486E-3,2.6567238555628165E-3,2.6659233620046339E-3,-4.8479828457863323E-3,null,"7K355T",null,300.72000000000003,1255.28,1985.64,4163.54,null,559.91999999999996,3197.42,4893.76,9451.2800000000007,null,416.44,2150.9,3335.22,6631.56,null,369.06,1776.34,2765.86,5568.76]
["XC7K420T",196.53647616174487,351.58702534761971,1471.8470843225834,2328.783654618996,4842.5209693703227,319.5650041933572,655.80579867334109,3750.7750180551348,5741.2352483948098,11070.414262432956,248.73398524502934,487.5426897302886,2522.655298102808,3912.5546632415994,7736.0364336148941,227.4070313303657,431.96461937178651,2083.1206665789391,3244.3872496452309,6484.9247201206663,null,2.5292995369823961E-3,2.6616103673061478E-3,2.6183027054768357E-3,2.6535449852902494E-3,2.6572326621771272E-3,2.6662205000465657E-3,-4.7660182933853823E-3,null,"7K420T",null,350.7,1467.94,2322.58,4871.4799999999996,null,654.16,3740.98,5726.2,11059.76,null,486.32,2516,3902.2,7759.92,null,430.88,2077.6,3235.76,6515.98]
["XC7K480T",224.32585581973876,400.39006137819536,1666.7403992331897,2635.3936673888734,5477.2238196922181,363.03818904535126,744.12609760090766,4242.987719937506,6493.685722325914,12518.706551288607,282.90811010126822,553.74868098350942,2854.5429936002361,4426.0210026484992,8748.7027207073425,258.88388636188409,490.99281488991198,2357.6420074963576,3670.6505287173977,7334.1378586847659,null,2.529073509428013E-3,2.659174667446554E-3,2.6152951703968647E-3,2.6506919861948217E-3,2.6545919436750331E-3,2.6634239442207184E-3,-4.8686626786948401E-3,null,"7K480T",null,399.38,1662.32,2628.38,5510.6,null,742.26,4231.92,6476.7,12508.18,null,552.36,2847.02,4414.32,8776.74,null,489.76,2351.4,3660.9,7370.02]
["XC7VX330T",62.655539141549923,130.07047029489931,1144.5492394597366,1915.9447101380908,4320.9862702458759,176.84126714428601,404.11675390965854,3184.1432918008391,4961.6236770734795,9888.6663028697385,112.34444234707551,252.00814887061358,2086.0312300565274,3331.0315547135624,6922.3493649201982,92.133596187357668,201.94888603458332,1692.2578604225223,2733.892064308498,5798.8638215483534,null,1.9293660060030475E-3,2.8821122791796469E-3,2.8860943378663908E-3,2.9240045263817507E-3,2.9026766205921674E-3,2.9318993024314544E-3,2.5164557280510442E-2,null,"7VX330T",null,129.82,1141.26,1910.36,4194.8599999999997,null,403.1,3174.98,4947.26,9692.1,null,251.42,2080,3321.32,6762.9,null,201.5,1687.36,2725.9,5656.52]
["XC7V585T",253.57079572020396,452.30199527631953,1871.9686354641801,2951.3954767451714,6101.9442980034682,415.04466158769088,847.37027222017321,4773.7202766127111,7280.86029006835,13958.945580633355,321.96449457538847,628.53860443220424,3209.2740884550353,4959.5706849089984,9750.2408739497823,293.92147851015307,556.35911296615177,2649.646497451894,4112.0553662088196,8172.3541805080458,null,2.5312423005574643E-3,2.6720347642610561E-3,2.6254356263123477E-3,2.6626809212758245E-3,2.6665017225058971E-3,2.6762136336817744E-3,-5.3026099927889082E-3,null,"7V585T",null,451.16,1866.98,2943.5,6142.2,null,845.24,4761.22,7261.74,13953.52,null,626.96,3200.78,4946.3999999999996,9785.9599999999991,null,554.96,2642.6,4101.08,8215.92]
["XC7V2000T",401.35669837428384,809.28746220468486,4599.193873424384,7488.8540412182274,16024.152829840104,598.64753703306576,1308.1594099093504,8738.5797445765147,13497.343803920921,26378.648057463761,598.64753703306576,1308.1594099093504,8738.5797445765147,13497.343803920921,26378.648057463761,509.3855212654563,1113.495498422948,7448.1327828900367,11506.942233332782,22498.881479351261,null,2.3873640069917304E-3,2.6496113886916341E-3,7.2833285239280749E-3,7.713873285647533E-3,1.0041636880263858E-2,1.0717846857566347E-2,1.6931250047968308E-2,null,"7V2000T",null,807.36,4587.04,7468.94,16040.86,null,1301.8879999999999,8675.3940000000002,13394.023999999999,26028.575999999997,null,1301.8879999999999,8675.3940000000002,13394.023999999999,26028.575999999997,null,1106.6047999999998,7374.0848999999998,11384.920399999999,22124.289599999996]
["XC7VX485T",357.19769085782184,593.14069568956438,2034.2271663661088,3136.1962927199365,6350.0473109598197,504.51303013416407,985.54897263341888,4960.5812864029549,7516.5922567838861,14295.571517928467,416.5483847994297,768.47853213752501,3384.3014042169657,5170.3823204973542,10041.780331418908,391.5584744934406,696.9190406714722,2820.1341765406182,4312.7695693888709,8445.6290163890517,null,{"$f":"(C524-AG524)/AG524","v":2.7059804739568215E-3},{"$f":"(D524-AH524)/AH524","v":2.7146015054363226E-3},{"$f":"(I524-AM524)/AM524","v":2.6521258186938076E-3},{"$f":"(O524-AS524)/AS524","v":2.6844202696680707E-3},{"$f":"(S524-AW524)/AW524","v":2.7001132572757238E-3},{"$f":"(T524-AX524)/AX524","v":2.6991717092298413E-3},{"$f":"(U524-AY524)/AY524","v":-8.482273008183671E-3},null,"7VX485T",null,591.54,2028.72,3127.72,6405.44,null,982.96,4947.46,7496.7,14347.78,null,766.44,3375.24,5156.54,10114.299999999999,null,695.06,2812.54,4301.16,8517.8799999999992]
["XC7VX415T",70.514476462932109,154.53638353039906,1456.8055454204252,2451.875697217024,5566.4949782752019,214.47122861976106,499.45601263595785,4068.8704707983543,6364.2851133834756,12756.447134108417,133.45864263638273,308.1999183205595,2662.6592278974535,4269.6235717660156,8925.4021310626522,107.90924736735222,245.16516374233672,2158.1667706003109,3502.7522672191467,7475.4568213764169,null,2.0515077836795823E-3,2.9089932536764279E-3,2.8962591193640807E-3,2.9370963858232181E-3,2.9215247134183942E-3,2.9469964492497129E-3,2.6152146946497472E-2,null,"7VX415T",null,154.22,1452.58,2444.6799999999998,5399.24,null,498.18,4057.12,6345.8,12490.46,null,307.45999999999998,2654.92,4257.12,8712.1200000000008,null,244.6,2151.88,3492.46,7284.94]
["XC7VX550T",93.578488244024456,205.42116867401404,1943.278454776266,3271.2420373376558,7429.2718849089706,285.98652435448219,666.18258957544856,5429.6412657502915,8492.7084509065444,17022.67410951951,177.66410449214266,410.66667043294331,3552.7677589613354,5697.3458510626269,11910.694836262654,143.5733568519654,326.5534389842515,2879.5295718210496,4673.7146281951982,9975.2821672429891,null,2.0544813366538575E-3,2.9099599390319752E-3,2.8964502416514823E-3,2.9373085279927121E-3,2.9220350874738558E-3,2.9473577558699051E-3,2.6208697399212041E-2,null,"7VX550T",null,205,1937.64,3261.64,7204.28,null,664.48,5413.96,8468.0400000000009,16667.3,null,409.68,3542.44,5680.66,11625.18,null,325.8,2871.14,4659.9799999999996,9720.52]
["XC7VX690T",116.79858478440875,256.78662985081382,2435.3452228123942,4099.8930526695249,9313.3526472222256,357.78908726792838,833.99187064767841,6805.4712706269365,10645.776349598736,21341.469962890169,222.12144536092708,513.91545064488128,4452.641979286238,7141.27139648305,14932.038044626473,179.41478881082384,408.5230662925357,3608.7729920539227,5858.1124809134408,12505.806146143308,null,2.0550606837346189E-3,2.909558540363566E-3,2.8959316084035272E-3,2.9368453958859299E-3,2.921687719598505E-3,2.9468884783922242E-3,2.6295950240641564E-2,null,"7VX690T",null,256.26,2428.2800000000002,4087.86,9030.74,null,831.86,6785.82,10614.86,20894.759999999998,null,512.67999999999995,4439.7,7120.36,14573.22,null,407.58,3598.26,5840.9,12185.38]
["XC7VX980T",151.48735979444078,332.68261880605797,3146.6587896561127,5295.2409684703835,11934.150364411462,463.91265104525013,1080.6494318419823,8800.8526518150193,13761.689254478362,27405.953770638309,288.01420256752095,665.84008583834589,5756.36457307211,9228.5128154279682,19160.505928296847,232.65409007636543,529.27998618029653,4664.7048896700999,7569.1362251874734,16040.960236274896,null,0.15868841880070342,0.12766493562120135,0.12372732995247848,0.12350199723741595,0.12583203156634495,0.1240846241516385,0.14038883483088535,null,"7VX850T",null,287.12,2790.42,4705.58,10413.200000000001,null,951.84,7831.84,12260.26,24155.66,null,583.22,5116.5600000000004,8214.06,16831.28,null,461.88,4143.34,6733.6,14066.22]
["XC7VX1140T",169.71153820005557,382.72245139013637,3730.3060524394518,6291.1754819654598,14319.367570678411,381.32382234433521,895.64751629519753,7403.7543314737795,11599.282778949706,23309.353308168218,381.32382234433521,895.64751629519753,7403.7543314737795,11599.282778949706,23309.353308168218,325.09579482311506,764.13538885091816,6330.3311817527119,9921.8503621072523,19953.714735584115,null,2.1010981099087631E-3,2.9052432959945779E-3,1.3048332858141543E-2,1.3818924847573208E-2,1.9026955467199531E-2,2.0241546096991705E-2,4.1369364427394285E-2,null,"7VX1140T",null,381.92,3719.5,6272.76,13882.06,null,887.69799999999998,7308.3920000000007,11441.177999999998,22542.393999999997,null,887.69799999999998,7308.3920000000007,11441.177999999998,22542.393999999997,null,754.54329999999993,6212.1332000000002,9725.0012999999981,19161.034899999995]
["XCVH580T"]
["XCVH870T"]
["XC7Z010",10.863566257456057,16.127753784718699,70.25753784718691,111.48330850757968,235.91596092389969,16.818398126931822,31.78549764096044,180.12830726309903,275.17729956374018,535.28761779321223,13.244341132068518,22.894462645131764,120.42374782215889,186.84157854573215,375.01344426794907,12.386348926313143,20.176406055549911,99.255115408281668,154.70176469783306,314.6399987267913,null,-3.2290615130593685E-3,-7.3814941058645243E-3,-7.7762076506607929E-3,-7.9559384850156935E-3,-7.6473164538925021E-3,-7.9404598061237758E-3,-7.6219916542394144E-4,null,"7Z010",null,16.18,70.78,112.36,236.88,null,31.96,181.54,277.38,536.34,null,23,121.36,188.34,375.3,null,20.260000000000002,100.02,155.94,314.88]
["XC7Z020",17.515217779887404,28.916552493743023,156.42132538325382,254.4810598033373,555.75415973340773,32.0341704142823,65.092186644419613,415.45925041367417,642.84749810591154,1271.6000216330351,23.882214357099212,45.15952097151289,274.72716305402383,432.76623229351941,886.41952536076565,21.364661065378545,38.527587489571694,224.43482997141129,356.39870437480948,741.64677624403544,null,-3.5646969764637098E-3,-7.4788998524503722E-3,-7.5978157517815233E-3,-7.8265113175308328E-3,-7.6280952802825737E-3,-7.853949182090484E-3,2.4421175443817642E-3,null,"7Z020",null,29.02,157.6,256.48,554.04,null,65.459999999999994,418.64,647.86,1270.1199999999999,null,45.38,276.83999999999997,436.18,884.5,null,38.700000000000003,226.16,359.22,739.84]
["XC7Z030",44.959544289681951,83.293355005674528,437.51156329367734,706.69413150317007,1501.1816099221617,85.93076077902407,181.50157482795888,1160.0680928772265,1783.9941983735864,3470.5888306231195,62.6627620052477,127.00289082341936,770.80692936657874,1206.609481785164,2419.2533743779381,55.525499824024074,109.07778783964207,631.24518502730348,995.82210951945888,2023.9369074301635,null,2.0855992020515279E-3,2.5930686412698688E-3,2.5997725936654499E-3,2.6336849241872904E-3,2.6130638934298844E-3,2.6400619406552876E-3,2.8425861808361189E-3,null,"7Z030",null,83.12,436.38,704.84,1502.04,null,181.08,1157.06,1779.34,3444.16,null,126.72,768.8,1203.44,2408.6,null,108.84,629.6,993.2,2018.2]
["XC7Z045",98.608582658230517,179.21789295173207,816.15763597262685,1301.2185655727333,2724.0936612137025,171.16179922575398,354.81818398384382,2113.5776548525246,3238.7224856840867,6258.2997425166395,129.71207985332137,257.51241874571048,1414.4055015991705,2200.239261880095,4367.7794234699977,117.24460632610212,225.6123379377793,1164.2181050293061,1820.8968145736003,3657.3924322192242,null,2.3372089023045686E-3,2.6260238969888546E-3,2.6078966891790859E-3,2.6427069685637091E-3,2.6336637752816445E-3,2.6523140905689003E-3,-2.5329638203430869E-3,null,"7Z040",null,178.8,814.02,1297.78,2736.6,null,353.96,2108.08,3230.26,6237.3,null,256.89999999999998,1410.7,2194.44,4370.4799999999996,null,225.08,1161.1600000000001,1816.08,3666.68]
[]
[]
["Max Power Comparisons for package analysis"]
[null,null,null,null,null,"Total Power (W) @ Tj=",null,null,null,"Static Power (W) @ Tj=",null,null,"Design Power (W)",null,null,null,"Fabric","IO","GT","GTHs"]
["PART","Process","Voltages","Pkg","Q-Grade","55'C","85'C","100'C","125'C","85'C","100'C","125'C","Core","I/O","GTX","Util","MHz","MHz","Gbps"]
["KU040","Max","Vmax","FBVA676",null,18.620640838351882,20.511325089108144,20.219224163862219,null,3.1427949347954938,3.4261044101711415,null,8.3975044942398434,3.3071873454033884,5.6638383146694204,0.75,250,400,16.3,20,null,null,null,null,588.83472335838258,32.440486295375791,50.460669768929108,1.6,0.63889683254248275,66.53097146862315,5.3977763981648055,null,615.50986632828199,35.384353786736931,47.029206493911474,3,0.84083470385919878,63.990553324175607,5.5204332173029647]
["KU040","Max","Vmax","FBVA900",null,18.620640838351882,20.511325089108144,20.219224163862219,null,3.1427949347954938,3.4261044101711415,null,8.3975044942398434,3.3071873454033884,5.6638383146694204,0.75,250,400,16.3,20,null,null,null,null,588.83472335838258,32.440486295375791,50.460669768929108,1.6,1.2777936650849655,133.0619429372463,10.795552796329611,null,615.50986632828199,35.384353786736931,47.029206493911474,3,1.6816694077183976,127.98110664835121,11.040866434605929]
["KU040","Max","Vmax","FFVA1156",null,18.620640838351882,20.511325089108144,20.219224163862219,null,3.1427949347954938,3.4261044101711415,null,8.3975044942398434,3.3071873454033884,5.6638383146694204,0.75,250,400,16.3,20,null,null,null,null,1257.6832419289758,59.294247926260326,149.03126142055586,2.1,0.63889683254248275,66.949405251444674,5.3977763981648055,null,1320.1919867326606,63.817654884585657,146.1670478006923,3.9,0.84083470385919878,63.990553324175607,5.5204332173029647]
["7K160T","Max","Vmax","FBG676",null,10.081778871730371,11.162939671722192,11.224358095224298,null,1.7950216216736126,1.8564400451757181,null,5.1180645526328821,1.9709726472338795,2.2788808501818183,0.75,250,400,6.6,8,null,null,null,null,1257.6832419289758,59.294247926260326,149.03126142055586,2.1,1.2777936650849655,133.89881050288935,10.795552796329611,null,1320.1919867326606,63.817654884585657,146.1670478006923,3.9,1.6816694077183976,127.98110664835121,11.040866434605929]
["7K160T","Max","Vmax","FFG676",null,11.941000557068675,13.048228445724428,13.266110139177801,null,1.8418072363802103,1.9011579535939154,null,5.1180645526328821,3.4276750951658794,2.6606815615454549,0.75,250,400,10.3125,8,null,null,null,null,1257.6832419289758,59.294247926260326,149.03126142055586,2.1,1.2777936650849655,171.01980511534617,10.795552796329611,null,1320.1919867326606,63.817654884585657,146.1670478006923,3.9,1.6816694077183976,163.46152617222137,11.040866434605929]
["7K325T","Max","Vmax","FBG676",null,14.836101167748057,16.677631389887864,16.781444401631692,null,3.0292973610381138,3.1331103727819416,null,7.9417780835020508,3.4276750951658794,2.2788808501818183,0.75,250,400,6.6,8,null,null,null,null,2216.4985519497709,81.244685803334264,268.05189243765011,2.1,1.2777936650849655,133.0619429372463,10.795552796329611,null,2323.2117131341861,87.461705685116158,262.14939546635651,3.9,1.6816694077183976,127.98110664835121,11.040866434605929]
["7K325T","Max","Vmax","FBG900",null,17.114982017929876,18.956512240069681,19.060325251813509,null,3.0292973610381138,3.1331103727819416,null,7.9417780835020508,3.4276750951658794,4.5577617003636366,0.75,250,400,6.6,16,null,null,null,null,2216.4985519497709,81.244685803334264,268.05189243765011,2.1,1.2777936650849655,133.0619429372463,10.795552796329611,null,2323.2117131341861,87.461705685116158,262.14939546635651,3.9,1.6816694077183976,127.98110664835121,11.040866434605929]
["7K325T","Max","Vmax","FFG676","RF676",15.238490914366592,17.10592530586618,17.366493997653194,21.646240370074576,3.0757905656527953,3.177828281200139,5.3574222645967273,7.9417780835020508,3.4276750951658794,2.6606815615454549,0.75,250,400,10.3125,8,null,null,null,null,2216.4985519497709,81.244685803334264,268.05189243765011,2.1,1.2777936650849655,169.95093133337525,10.795552796329611,null,2323.2117131341861,87.461705685116158,262.14939546635651,3.9,1.6816694077183976,163.46152617222137,11.040866434605929]
["7K325T","Max","Vmax","FFG900","RF900",17.741245013384422,19.582775235524227,19.994375289279073,21.453516246507334,3.0292973610381138,3.1331103727819416,5.2901348506713557,7.9417780835020508,3.4276750951658794,5.1840246958181826,0.75,250,400,10.3125,16,null,null,null,null,2216.4985519497709,81.244685803334264,268.05189243765011,2.1,1.2777936650849655,133.0619429372463,10.795552796329611,null,2323.2117131341861,87.461705685116158,262.14939546635651,3.9,1.6816694077183976,127.98110664835121,11.040866434605929]
["7K355T","Max","Vmax","FFG901",null,22.094523554309141,24.403192789051456,24.983880718340199,null,3.8131760161212158,3.9321833823934296,null,11.499997964380382,1.3139817648225864,7.776037043727273,0.75,250,400,10.3125,24,null,null,null,null,2567.3170462085395,128.94659640268182,304.03609306660769,2.1,3.8333809952548963,399.18582881173887,32.386658388988835,null,2696.0292383674737,140.68078110596252,295.60522774383702,3.9,5.0450082231551931,383.94331994505359,33.122599303817786]
["7K410T","Max","Vmax","FBG676",null,19.866904176012721,22.098286885428095,22.231978453754692,null,3.6492092905364157,3.7829008588630137,null,12.742521649543981,3.4276750951658794,2.2788808501818183,0.75,250,400,6.6,8,null,null,null,null,2613.5527345668588,143.38642942969915,345.38132390196034,2.6,1.2777936650849655,133.0619429372463,10.795552796329611,null,2746.2892770912049,156.40439130421595,337.06586584607641,4.8,1.6816694077183976,127.98110664835121,11.040866434605929]
["7K410T","Max","Vmax","FBG900",null,22.145785026194538,24.377167735609913,24.51085930393651,null,3.6492092905364157,3.7829008588630137,null,12.742521649543981,3.4276750951658794,4.5577617003636366,0.75,250,400,6.6,16,null,null,null,null,2613.5527345668588,143.38642942969915,345.38132390196034,2.6,1.2777936650849655,133.0619429372463,10.795552796329611,null,2746.2892770912049,156.40439130421595,337.06586584607641,4.8,1.6816694077183976,127.98110664835121,11.040866434605929]
["7K410T","Max","Vmax","FFG676","RF676",20.269293922631256,22.526580801406414,22.817028049776198,27.622217399242622,3.6957024951510973,3.8276187672812112,6.5326557277228394,12.742521649543981,3.4276750951658794,2.6606815615454549,0.75,250,400,10.3125,8,null,null,null,null,2613.5527345668588,143.38642942969915,345.38132390196034,2.6,1.2777936650849655,169.95093133337525,10.795552796329611,null,2746.2892770912049,156.40439130421595,337.06586584607641,4.8,1.6816694077183976,163.46152617222137,11.040866434605929]
["7K410T","Max","Vmax","FFG900","RF900",22.772048021649084,25.003430731064459,25.444909341402077,27.429493275675377,3.6492092905364157,3.7829008588630137,6.4653683137974678,12.742521649543981,3.4276750951658794,5.1840246958181826,0.75,250,400,10.3125,16,null,null,null,null,2613.5527345668588,143.38642942969915,345.38132390196034,2.6,1.2777936650849655,133.0619429372463,10.795552796329611,null,2746.2892770912049,156.40439130421595,337.06586584607641,4.8,1.6816694077183976,127.98110664835121,11.040866434605929]
["7K420T","Max","Vmax","FFG901",null,25.812659449059993,28.902655322572578,29.599992247369123,null,5.0864742670406633,5.2451838683179277,null,13.430156073027508,1.3139817648225864,9.07204321768182,0.75,250,400,10.3125,28,null,null,null,null,3513.4381948174987,160.73199594389135,404.74317327938331,1.7,4.4722778277973791,465.71680028036195,37.784434787153636,null,3684.7225665482692,176.47818125790792,393.4552747059804,3,5.8858429270143917,447.93387326922925,38.643032521120752]
["7K420T","Max","Vmax","FFG1156",null,28.023503581667072,31.095537722921886,31.888117344145229,null,5.0500110291321114,5.208466745396775,null,13.431827800374077,1.9709726472338795,10.64272624618182,0.75,250,400,10.3125,32,null,null,null,null,3513.4381948174987,160.73199594389135,404.74317327938331,1.7,3.1944841627124139,424.87732833343819,26.98888199082403,null,3684.7225665482692,176.47818125790792,393.4552747059804,3,4.2041735192959937,408.65381543055349,27.602166086514824]
["7K480T","Max","Vmax","FFG901",null,28.064905172920575,31.257531972802113,31.964685455600417,null,5.2712730614689312,5.4235681274283944,null,15.359891681101503,1.3139817648225864,9.3123854654090898,0.75,250,400,10.3125,28,null,null,null,null,3523.3490642661013,172.25081414274797,404.74317327938331,1.7,4.4722778277973791,594.82825966681344,37.784434787153636,null,3694.5284686935079,187.9068224590543,393.4552747059804,3,5.8858429270143917,572.11534160277483,38.643032521120752]
["7K480T","Max","Vmax","FFG1156",null,29.963345434408239,33.047345909272764,33.839724531865997,null,5.0720836074089934,5.2303383250435509,null,15.361563408448074,1.9709726472338795,10.64272624618182,0.75,250,400,10.3125,32,null,null,null,null,3523.3490642661013,172.25081414274797,404.74317327938331,1.7,3.1944841627124139,424.87732833343819,26.98888199082403,null,3694.5284686935079,187.9068224590543,393.4552747059804,3,4.2041735192959937,408.65381543055349,27.602166086514824]
[]
[null,null,null,null,null,"Total Power (W) @ Tj=",null,null,null,"Static Power (W) @ Tj=",null,null,"Design Power (W)",null,null,null,"Fabric","IO","GT","GTPs"]
["PART","Process","Voltages","Pkg","Q-Grade","55'C","85'C","100'C","125'C","85'C","100'C","125'C","Core","I/O","GTP","Util","MHz","MHz","Gbps"]
["7A100T","Max","Vmax","FTG256","FTG256",2.201167016501218,2.5689997506430564,2.5938870146494346,3.0339839661046342,0.62919934565233648,0.65408660965871468,1.0941835611139141,1.49875682044826,0.44104358454246007,0,0.75,150,150,null,null,null,null,null,null,412.91363109727041,33.966522374694435,83.309621432155225,1.6,0,0,0,null,442.42369760386981,37.048872623793727,77.203921121517439,3,0,0,0]
["7A100T","Max","Vmax","CSG324","CSG324",2.201167016501218,2.5689997506430564,2.5938870146494346,3.0339839661046342,0.62919934565233648,0.65408660965871468,1.0941835611139141,1.49875682044826,0.44104358454246007,0,0.75,150,150,null,null,null,null,null,null,412.91363109727041,33.966522374694435,83.309621432155225,1.6,0,0,0,null,442.42369760386981,37.048872623793727,77.203921121517439,3,0,0,0]
["7A100T","Max","Vmax","FGG484","FGG484",3.320162051471784,3.7108363799425939,3.7343320304256413,4.0611519084524259,0.67264239887295718,0.69613804935600465,1.1567571623827893,1.4994239519847166,0.88208716908492013,0.65668285999999998,0.75,150,150,6.6,4,null,null,null,null,412.91363109727041,33.966522374694435,83.309621432155225,1.6,0,36.129747604609406,5.0645635673764096,null,442.42369760386981,37.048872623793727,77.203921121517439,3,0,34.641234876499674,5.1796485971506332]
["7A100T","Max","Vmax","FGG676",null,3.9974463703634338,4.4109622931632151,4.4330663301229318,null,0.71608545209357788,0.73818948905329451,null,1.4994239519847166,0.88208716908492013,1.31336572,0.75,150,150,6.6,8,null,null,null,null,412.91363109727041,33.966522374694435,83.309621432155225,1.6,0,72.259495209218812,10.129127134752819,null,442.42369760386981,37.048872623793727,77.203921121517439,3,0,69.282469752999347,10.359297194301266]
["7A200T","Max","Vmax","SBG484","SB484",5.8605244296157402,6.7100880086418284,6.762835667636339,7.6984106185907466,1.4238477187525891,1.4765953777471001,2.4896330437015068,3.8038067808043188,0.88208716908492013,0.60034633999999998,null,null,null,5.4,4,null,null,null,null,912.8268685131618,91.773253073088796,170.09499358010856,2.6,0,36.129747604609406,5.0645635673764096,null,976.47700103377065,100.08876891676918,156.92586222314458,4.8,0,34.641234876499674,5.1796485971506332]
["7A200T","Max","Vmax","FBG484","FB484",5.8605244296157402,6.7100880086418284,6.762835667636339,7.6984106185907466,1.4238477187525891,1.4765953777471001,2.4896330437015068,3.8038067808043188,0.88208716908492013,0.60034633999999998,0.75,150,150,5.4,4,null,null,null,null,912.8268685131618,91.773253073088796,170.09499358010856,2.6,0,36.129747604609406,5.0645635673764096,null,976.47700103377065,100.08876891676918,156.92586222314458,4.8,0,34.641234876499674,5.1796485971506332]
["7A200T","Max","Vmax","FBG676","FB676",6.9231672927131997,7.7955724660682586,7.8469285115394385,7.6984106185907466,1.4672907719732098,1.5186468174443901,2.4896330437015068,3.8044582604676682,1.3231307536273802,1.20069268,0.75,150,150,5.4,8,null,null,null,null,912.8268685131618,91.773253073088796,170.09499358010856,2.6,0,72.259495209218812,10.129127134752819,null,976.47700103377065,100.08876891676918,156.92586222314458,4.8,0,69.282469752999347,10.359297194301266]
["7A200T","Max","Vmax","FFG1156",null,8.3904089704964981,9.3084973325094982,9.3570701509340175,null,1.5541768784144512,1.6027496968389698,null,3.8044582604676682,1.3231307536273802,2.6267314399999999,0.75,150,150,6.6,16,null,null,null,null,912.8268685131618,91.773253073088796,170.09499358010856,2.6,0,144.51899041843762,20.258254269505638,null,976.47700103377065,100.08876891676918,156.92586222314458,4.8,0,138.56493950599869,20.718594388602533]
[]
[null,null,null,null,null,"Total Power (W) @ Tj=",null,null,null,"Static Power (W) @ Tj=",null,null,"Design Power (W)",null,null,null,"Fabric","IO","GT","GTs"]
["PART","Process","Voltages","Pkg","Q-Grade","55'C","85'C","100'C","125'C","85'C","100'C","125'C","Core","I/O","GTX/GTH","Util","MHz","MHz","Gbps","GTX/H"]
["7V585T","Max","Vmax","FFG1157","RF1157",26.977131035376065,30.418708924340638,31.028344681810925,39.201762522882504,5.6742015104798575,5.8875098273509678,10.040181515563047,13.631115072900972,4.4616884370961731,6.6517039038636359,0.75,250,400,10.3125,20,null,null,null,null,4005.1067842785815,162.50462002032569,469.19813002509233,5.3,3.1944841627124139,414.18859051372903,26.98888199082403,null,4200.3479780250118,177.25831014477808,453.1988528433651,9.8000000000000007,4.2041735192959937,430.43160496760493,27.602166086514824]
["7V585T","Max","Vmax","FFG1761","RF1761",32.076405887629264,35.616454797599985,36.530417299383117,39.058821669283162,5.8593893100119301,6.0808309672702769,10.179473258657922,13.631115072900972,4.461894849096173,11.66405556559091,0.75,250,400,10.3125,36,null,null,null,null,4005.1067842785815,162.50462002032569,469.19813002509233,5.3,5.7500714928823449,583.71512703603321,48.579987583483245,null,4200.3479780250118,177.25831014477808,453.1988528433651,9.8000000000000007,7.5675123347327888,606.60637383168353,49.683898955726683]
["7V2000T","Max","Vmax","FHG1761",null,51.805000048582755,58.072812866621831,64.185055365584006,null,10.191249648039758,15.610971302477143,null,31.747918075237383,4.4695895777537853,11.66405556559091,0.75,250,400,10.3125,36,null,null,null,null,7271.6662150045586,184.92302351641985,967.8651505431319,6.4,5.7500714928823449,583.71512703603321,48.579987583483245,null,11387.978226175612,292.14680539017462,1514.3382864460057,11.7,7.5675123347327888,606.60637383168353,49.683898955726683]
["7V2000T","Max","Vmax","FLG1925",null,45.243122993311957,51.253384363607033,56.969935797921977,null,9.7142039695249505,15.113693451360559,null,31.747918075237383,4.4698991957537855,5.3213631230909098,0.75,250,400,10.3125,16,null,null,null,null,7271.6662150045586,184.92302351641985,967.8651505431319,6.4,1.2777936650849655,165.67543620549159,10.795552796329611,null,11387.978226175612,292.14680539017462,1514.3382864460057,11.7,1.6816694077183976,172.17264198704197,11.040866434605929]
["7VX330T","Max","Vmax","FFG1157","RF1157",21.637331409301787,23.694946786401367,24.22646743729381,27.467184748610968,3.3868444252875265,3.5095964277832792,6.0215506153649008,10.777324311860639,4.4616884370961731,5.0690896121570255,0.75,250,400,11.3,20,null,null,null,null,2515.1957776805425,153.24897104000573,291.9125688446062,3.6,0.63889683254248275,68.031633531662223,5.1263866948433741,null,2635.5664597326345,167.19701306324106,282.48871583233523,6.6,0.84083470385919878,65.228792129773851,5.2428765675760518]
["7VX330T","Max","Vmax","FFG1761","RF1761",23.486131057153752,25.570757026455937,26.24698670223599,27.248083055518542,3.4373049721982998,3.5588033883552077,5.9775462940080102,10.777324311860639,4.4617916430961726,6.8943360993008271,0.75,250,400,11.3,28,null,null,null,null,2515.1957776805425,153.24897104000573,291.9125688446062,3.6,1.2777936650849655,113.05562752437632,10.252773389686748,null,2635.5664597326345,167.19701306324106,282.48871583233523,6.6,1.6816694077183976,108.39783853575362,10.485753135152104]
["7VX415T","Max","Vmax","FFG1157",null,26.010605721300848,28.884595594023992,29.437083322432613,null,4.6981814298937499,4.8544325442858414,null,14.800199941819193,4.4616884370961731,4.9245257852148763,0.75,250,400,11.3,20,null,null,null,null,3638.8966125315919,179.90760566439369,367.31191650897841,3.1,0.63889683254248275,56.52781376218816,5.1263866948433741,null,3795.8618302581472,196.24530911333576,354.36800079737748,5.7,0.84083470385919878,54.198919267876811,5.2428765675760518]
["7VX415T","Max","Vmax","FFG1158",null,31.209268674805575,34.311778317064338,35.435894874680386,null,5.1182398408781715,5.2613116423421529,null,14.796879188461224,2.2308442185480866,12.165815069176858,0.75,250,400,11.3,48,null,null,null,null,3638.8966125315919,179.90760566439369,367.31191650897841,3.1,3.8333809952548963,408.18980118997337,30.758320169060244,null,3795.8618302581472,196.24530911333576,354.36800079737748,5.7,5.0450082231551931,391.37275277864308,31.457259405456309]
["7VX415T","Max","Vmax","FFG1927",null,33.443433646711625,36.545943288970392,37.67005984658644,null,5.1182398408781715,5.2613116423421529,null,14.800199941819193,4.4616884370961731,12.165815069176858,0.75,250,400,11.3,48,null,null,null,null,3638.8966125315919,179.90760566439369,367.31191650897841,3.1,3.8333809952548963,408.18980118997337,30.758320169060244,null,3795.8618302581472,196.24530911333576,354.36800079737748,5.7,5.0450082231551931,391.37275277864308,31.457259405456309]
["7VX485T","Max","Vmax","FFG1157","RF1157",31.339749578032791,34.847332524532483,35.441667649347309,40.07396443903265,5.7810195948494254,5.9790272790650718,10.280204816998351,17.952920588723252,4.4616884370961731,6.6517039038636359,0.75,250,400,10.3125,20,null,null,null,null,4100.4761443840844,210.55108226530265,448.9744725375653,3.6,3.1944841627124139,414.18859051372903,26.98888199082403,null,4299.8991471908394,228.30618105407848,422.21495889454127,6.6,4.2041735192959937,430.43160496760493,27.602166086514824]
["7VX485T","Max","Vmax","FFG1158",null,38.195342412332707,41.922598068361623,43.061532905912493,null,6.1900799269937075,6.4056536385115264,null,17.949599835365284,2.2308442185480866,15.552074087454546,0.75,250,400,10.3125,48,null,null,null,null,4100.4761443840844,210.55108226530265,448.9744725375653,3.6,7.6667619905097926,778.28683604804428,64.773316777977669,null,4299.8991471908394,228.30618105407848,422.21495889454127,6.6,10.090016446310386,808.80849844224451,66.245198607635572]
["7VX485T","Max","Vmax","FFG1761","RF1761",34.089052647074837,37.702689211399765,38.463621200597274,40.07396443903265,5.9755915141712492,6.1816650865299216,10.280204816998351,17.952920588723252,4.4617916430961726,9.3123854654090898,0.75,250,400,10.3125,28,null,null,null,null,4100.4761443840844,210.55108226530265,448.9744725375653,3.6,4.4722778277973791,579.86402671922053,37.784434787153636,null,4299.8991471908394,228.30618105407848,422.21495889454127,6.6,5.8858429270143917,602.6042469546469,38.643032521120752]
["7VX485T","Max","Vmax","FFG1927",null,42.984956862755631,46.660894807923924,47.918292596461917,null,6.1021993467408571,6.2823424882402907,null,17.952920588723252,4.4616884370961731,18.14408643536364,0.75,250,400,10.3125,56,null,null,null,null,4100.4761443840844,210.55108226530265,448.9744725375653,3.6,8.9445556555947583,677.77904141431293,75.568869574307271,null,4299.8991471908394,228.30618105407848,422.21495889454127,6.6,11.771685854028783,672.88373689847845,77.286065042241503]
["7VX485T","Max","Vmax","FFG1930",null,32.714452715553819,36.275062470966127,36.952696027972294,null,5.8783055545103373,6.0803461827974967,null,17.952920588723252,4.4617916430961726,7.9820446846363629,0.75,250,400,10.3125,24,null,null,null,null,4100.4761443840844,210.55108226530265,448.9744725375653,3.6,3.8333809952548963,497.02630861647486,32.386658388988835,null,4299.8991471908394,228.30618105407848,422.21495889454127,6.6,5.0450082231551931,516.51792596112591,33.122599303817786]
["7VX550T","Max","Vmax","FFG1158",null,37.368613411230434,42.304798899053267,43.518794661424955,null,8.102886577303817,8.3358375835234426,null,19.805253034024503,2.2308442185480866,12.165815069176858,0.75,250,400,11.3,48,null,null,null,null,5989.8794629862632,268.98121194635991,615.05720009993536,5.0999999999999996,3.8333809952548963,408.18980118997337,30.758320169060244,null,6236.2677035051429,296.54017072660832,593.40328348267496,9.4,5.0450082231551931,391.37275277864308,31.457259405456309]
["7VX550T","Max","Vmax","FFG1927",null,48.082891978592961,53.459123040301122,55.302046629021099,null,8.9125023671943779,9.1203513623275807,null,19.808573787382471,4.4616884370961731,20.276358448628102,0.75,250,400,11.3,80,null,null,null,null,5989.8794629862632,268.98121194635991,615.05720009993536,5.0999999999999996,10.222349320679724,1088.5061365065956,82.022187117493985,null,6236.2677035051429,296.54017072660832,593.40328348267496,9.4,13.453355261747181,1043.6606740763816,83.886025081216829]
["7VX690T","Max","Vmax","FFG1157","RF1157",37.250347936261115,41.997613495196418,42.651327163937502,49.033758808142835,7.7554496609262467,8.0003946812706435,13.777467433441259,24.711385785016972,4.4616884370961731,5.0690896121570255,0.75,250,400,11.3,20,null,null,null,null,6014.103204892599,300.4574492319764,615.05720009993536,5.0999999999999996,0.63889683254248275,68.031633531662223,5.1263866948433741,null,6260.1970940400251,327.76999101625944,593.40328348267496,9.4,0.84083470385919878,65.228792129773851,5.2428765675760518]
["7VX690T","Max","Vmax","FFG1761","RF1761",41.129468080507714,45.974759381236765,46.927912933024587,48.912644844670496,7.9373323337368493,8.1772599802949131,13.829830062299502,24.711385785016972,4.461894849096173,8.8641464133867771,0.75,250,400,11.3,36,null,null,null,null,6014.103204892599,300.4574492319764,615.05720009993536,5.0999999999999996,2.555587330169931,226.11125504875264,20.505546779373496,null,6260.1970940400251,327.76999101625944,593.40328348267496,9.4,3.3633388154367951,216.79567707150724,20.971506270304207]
["7VX690T","Max","Vmax","FFG1926",null,48.204921902734611,53.263258652237084,54.759852101305583,null,8.3315987114363388,8.5602349956519408,null,24.711385785016972,4.4617916430961726,15.758482512687603,0.75,250,400,11.3,64,null,null,null,null,6014.103204892599,300.4574492319764,615.05720009993536,5.0999999999999996,6.3889683254248277,565.27813762188168,51.263866948433737,null,6260.1970940400251,327.76999101625944,593.40328348267496,9.4,8.4083470385919874,541.98919267876818,52.428765675760516]
["7VX690T","Max","Vmax","FFG1927",null,53.011972096740038,58.419306016503334,60.261672613804869,null,8.9698733457620889,9.1771653494768497,null,24.711385785016972,4.4616884370961731,20.276358448628102,0.75,250,400,11.3,80,null,null,null,null,6014.103204892599,300.4574492319764,615.05720009993536,5.0999999999999996,10.222349320679724,1088.5061365065956,82.022187117493985,null,6260.1970940400251,327.76999101625944,593.40328348267496,9.4,13.453355261747181,1043.6606740763816,83.886025081216829]
["7VX690T","Max","Vmax","FFG1930","RF1930",38.301432498293039,43.092702614616876,43.825659811928666,49.033758808142835,7.8364112399153028,8.078846059151056,13.777467433441259,24.711385785016972,4.4619980550961724,6.0829075345884291,0.75,250,400,11.3,24,null,null,null,null,6014.103204892599,300.4574492319764,615.05720009993536,5.0999999999999996,1.2777936650849655,136.06326706332445,10.252773389686748,null,6260.1970940400251,327.76999101625944,593.40328348267496,9.4,1.6816694077183976,130.4575842595477,10.485753135152104]
["7VX980T","Max","Vmax","FFG1926",null,51.659516494443537,58.058290396502521,59.699757500422542,null,10.44410255110941,10.817612490176536,null,27.393913689609334,4.4617916430961726,15.758482512687603,0.75,250,400,11.3,64,null,null,null,null,7737.0353390300415,306.67517325257364,790.85983807363425,4.5999999999999996,6.3889683254248277,565.27813762188168,51.263866948433737,null,8137.9822926448496,334.53336469664316,761.58712743549438,8.4,8.4083470385919874,541.98919267876818,52.428765675760516]
["7VX980T","Max","Vmax","FFG1928",null,53.284902686700178,59.988669201631453,61.814912195534475,null,11.001415606446104,11.356091466121033,null,27.392264663597935,3.3462663278221298,18.248722603765287,0.75,250,400,11.3,72,null,null,null,null,7737.0353390300415,306.67517325257364,790.85983807363425,4.5999999999999996,9.583452488137242,1020.4745029749331,76.895800422650609,null,8137.9822926448496,334.53336469664316,761.58712743549438,8.4,12.612520557887981,978.43188194660775,78.643148513640767]
["7VX980T","Max","Vmax","FFG1930","RF1930",41.755923884001959,47.887631152882307,48.76546200504562,54.809355891186456,9.9489150795883745,10.336223553675651,17.633674628233013,27.393913689609334,4.461894849096173,6.0829075345884291,0.75,250,400,11.3,24,null,null,null,null,7737.0353390300415,306.67517325257364,790.85983807363425,4.5999999999999996,1.2777936650849655,136.06326706332445,10.252773389686748,null,8137.9822926448496,334.53336469664316,761.58712743549438,8.4,1.6816694077183976,130.4575842595477,10.485753135152104]
["7VX1140T","Max","Vmax","FLG1926",null,55.15970900733209,60.642360410215289,66.538039259367125,null,8.986092489690332,13.613814173989278,null,31.428299036083558,4.4694863717537858,15.758482512687603,0.75,250,400,11.3,64,null,null,null,null,6417.0373286566755,269.06224185501151,757.78799077468057,6.4,6.3889683254248277,565.27813762188168,51.263866948433737,null,9983.7507326408104,425.07603215821609,1183.0705894098253,11.7,8.4083470385919874,541.98919267876818,52.428765675760516]
["7VX1140T","Max","Vmax","FLG1928",null,63.198692246417465,69.38237727866975,75.930762585902841,null,10.272059755928533,14.858355550857498,null,31.426650010072159,3.3520373743153393,24.331630138353717,0.75,250,400,11.3,96,null,null,null,null,6417.0373286566755,269.06224185501151,757.78799077468057,6.4,15.333523981019585,1632.7592047598935,123.03328067624098,null,9983.7507326408104,425.07603215821609,1183.0705894098253,11.7,20.180032892620773,1565.4910111145723,125.82903762182524]
["7VX1140T","Max","Vmax","FLG1930",null,45.256322808890509,50.471907578595065,55.603950175990192,null,8.4909050181692969,13.132425237488393,null,31.428299036083558,4.469795989753786,6.0829075345884291,0.75,250,400,11.3,24,"GTZ Total (lkg+dyn)",null,null,null,6417.0373286566755,269.06224185501151,757.78799077468057,6.4,1.2777936650849655,136.06326706332445,10.252773389686748,null,9983.7507326408104,425.07603215821609,1183.0705894098253,11.7,1.6816694077183976,130.4575842595477,10.485753135152104]
["7VH580T","Max","Vmax","HCG1155",null,32.628364823142107,36.449011289509883,37.746370193707797,null,6.5804355585172107,6.8745494175340873,null,15.693051467042714,3.3481900099865332,6.0829075345884291,0.75,250,400,11.3,24,5.2423962581249999,8,null,null,4556.6909261288902,192.16576506971074,541.89442849446505,3.2,1.2777936650849655,136.06326706332445,10.252773389686748,null,4795.8258567985094,209.64360456696974,521.91831881842165,5.9,1.6816694077183976,130.4575842595477,10.485753135152104]
["7VH580T","Max","Vmax","HCG1931",null,39.976812806806208,43.973477502728116,45.751317980567492,null,6.9042818744734351,7.188354929055742,null,15.694700493054114,4.4642533466487109,12.165815069176858,0.75,250,400,11.3,48,5.2423962581249999,8,null,null,4556.6909261288902,192.16576506971074,541.89442849446505,3.2,3.8333809952548963,408.18980118997337,30.758320169060244,null,4795.8258567985094,209.64360456696974,521.91831881842165,5.9,5.0450082231551931,391.37275277864308,31.457259405456309]
["7VH580T","Max","Vmax","HCG1932",null,36.623590152675249,40.620254848597156,42.398095326436533,null,6.9042818744734351,7.188354929055742,null,15.689667848909686,1.1160633366621777,12.165815069176858,0.75,250,400,11.3,48,5.2423962581249999,8,null,null,4556.6909261288902,192.16576506971074,541.89442849446505,3.2,3.8333809952548963,408.18980118997337,30.758320169060244,null,4795.8258567985094,209.64360456696974,521.91831881842165,5.9,5.0450082231551931,391.37275277864308,31.457259405456309]
["7VH870T","Max","Vmax","HCG1931",null,48.111806569259699,52.367464852155472,57.431161198437266,null,7.323665366636952,10.893594289661676,null,23.666636234765413,4.4669214622012481,12.165815069176858,0.75,250,400,11.3,48,5.2423962581249999,8,null,null,4902.8390291599389,201.71906165388856,568.60927006051497,4.8,3.8333809952548963,408.18980118997337,30.758320169060244,null,7608.6428070644442,318.72737487910359,887.58716453827503,8.8000000000000007,5.0450082231551931,391.37275277864308,31.457259405456309]
["7VH870T","Max","Vmax","HCG1932",null,56.31276689358247,61.052173663475031,67.164848700210086,null,8.5502891162884573,12.165951684585401,null,23.661603590620985,1.1167045640503119,18.248722603765287,0.75,250,400,11.3,72,10.470792866250001,16,null,null,4902.8390291599389,201.71906165388856,568.60927006051497,4.8,9.583452488137242,1020.4745029749331,76.895800422650609,null,7608.6428070644442,318.72737487910359,887.58716453827503,8.8000000000000007,12.612520557887981,978.43188194660775,78.643148513640767]
[]
[null,null,null,null,null,"Total Power (W) @ Tj=",null,null,null,"Static Power (W) @ Tj=",null,null,"Design Power (W)",null,null,null,null,"Fabric","IO","GT","GTs"]
["PART","Process","Voltages","Pkg","Q-Grade","55'C","85'C","100'C","125'C","85'C","100'C","125'C","Core","I/O","GTX","PS","Util","MHz","MHz","Gbps","GTX"]
["7Z010","Max","Vmax","CLG225","CLG225",2.6370571659742312,3.0836310037672368,3.0322659426214278,3.4369787887221248,0.82762069164896901,0.77625563050315982,1.1809684766038568,0.53392767785190576,0.21242930440713217,0,1.5096533298592301,0.75,150,150,null,null,null,null,157.81533518697347,149.92456842762479,15.124535165593274,27.84843118260779,2,0,0,0,167.8905049368166,159.49597968997577,16.504195266622958,26.009310221283389,2,0,0,0]
["7Z010","Max","Vmax","CLG400","CLG400",2.6370571659742312,3.0836310037672368,3.0322659426214278,3.4369787887221248,0.82762069164896901,0.77625563050315982,1.1809684766038568,0.53392767785190576,0.21242930440713217,0,1.5096533298592301,0.75,150,150,null,null,null,null,157.81533518697347,149.92456842762479,15.124535165593274,27.84843118260779,2,0,0,0,167.8905049368166,159.49597968997577,16.504195266622958,26.009310221283389,2,0,0,0]
["7Z020","Max","Vmax","CLG400","CLG400",3.6251632464445693,4.2543195053667313,4.2183558136578023,4.838556943586652,1.1246329356937417,1.0886692439848131,1.7088703739136619,1.4076039354066274,0.21242930440713217,0,1.5096533298592301,0.75,150,150,null,null,null,null,356.45007785399781,338.62757396129791,35.256145869691856,68.978535412826034,2,0,0,0,383.34532696761249,364.17806061923187,38.470750556144935,63.891609402202121,3.8,0,0,0]
["7Z020","Max","Vmax","CLG484","CLG484",3.8557108915619316,4.484867150484094,4.4503209587751646,5.0705220887040143,1.1262079356937418,1.0916617439848131,1.7118628739136619,1.4079623003886621,0.44104358454246007,0,1.5096533298592301,0.75,150,150,null,null,null,null,356.45007785399781,338.62757396129791,35.256145869691856,68.978535412826034,3,0,0,0,383.34532696761249,364.17806061923187,38.470750556144935,63.891609402202121,5.7,0,0,0]
["7Z030","Max","Vmax","FBG484","FGB484",8.5949446514522592,9.8989242180146952,10.051266997933853,11.098883983416037,2.2384254227265612,2.2162973224804281,3.4383851881279011,3.9226243960816016,1.0681396150552933,1.160081454292011,1.5096533298592301,0.75,250,400,8,4,null,null,1095.7602867769556,1038.3421321672492,63.456926795465328,114.84357807726826,4.2,0.63889683254248275,58.580729595014084,5.3977763981648055,1152.9845764660615,1092.567852595861,69.211952513843187,106.20307777088765,7.5,0.84083470385919878,56.167256836266986,5.5204332173029647]
["7Z030","Max","Vmax","FBG676",null,8.5949446514522592,9.8989242180146952,10.051266997933853,null,2.2384254227265612,2.2162973224804281,null,3.9226243960816016,1.0681396150552933,1.160081454292011,1.5096533298592301,0.75,250,400,8,4,null,null,1095.7602867769556,1038.3421321672492,63.456926795465328,114.84357807726826,4.2,0.63889683254248275,58.580729595014084,5.3977763981648055,1152.9845764660615,1092.567852595861,69.211952513843187,106.20307777088765,7.5,0.84083470385919878,56.167256836266986,5.5204332173029647]
["7Z030","Max","Vmax","FFG676","RF676",8.6353681840063956,9.950752101859301,10.107545746721927,11.159773687314127,2.2588941291606979,2.2359227368332419,3.4679157146155246,3.9226243960816016,1.0681396150552933,1.1914406317024793,1.5096533298592301,0.75,250,400,8,4,null,null,1095.7602867769556,1038.3421321672492,63.456926795465328,114.84357807726826,4.2,0.63889683254248275,74.82116473796394,5.3977763981648055,1152.9845764660615,1092.567852595861,69.211952513843187,106.20307777088765,7.5,0.84083470385919878,71.73860082793415,5.5204332173029647]
["7Z045","Max","Vmax","FBG676",null,15.630459321424127,18.134743064353099,18.578763863940523,null,4.1977031319402034,4.2927821711970484,null,9.0390840789143496,1.0681396150552933,2.3201629085840221,1.5096533298592301,0.75,250,400,8,8,null,null,2710.3300114922308,2487.2034770963496,130.64864594672923,287.47647628787968,6.3000000000000007,1.2777936650849655,117.16145919002817,10.795552796329611,2851.5607097649449,2673.6945482899664,142.45950285367124,264.75674110469254,11.7,1.6816694077183976,112.33451367253397,11.040866434605929]
["7Z045","Max","Vmax","FFG676","RF676",15.630459321424127,18.134743064353099,18.578763863940523,20.833341472287486,4.1977031319402034,4.2927821711970484,6.8963015398745897,9.0390840789143496,1.0681396150552933,2.3201629085840221,1.5096533298592301,0.75,250,400,8,8,null,null,2710.3300114922308,2487.2034770963496,130.64864594672923,287.47647628787968,6.3000000000000007,1.2777936650849655,117.16145919002817,10.795552796329611,2851.5607097649449,2673.6945482899664,142.45950285367124,264.75674110469254,11.7,1.6816694077183976,112.33451367253397,11.040866434605929]
["7Z045","Max","Vmax","FFG900",null,19.089810223760377,21.667691229964497,22.462400941898427,null,4.3406368831258249,4.437463074398603,null,9.0407959697008096,2.1362792301105866,4.6403258171680442,1.5096533298592301,0.75,250,400,8,16,null,null,null,2487.2034770963496,130.64864594672923,287.47647628787968,10.500000000000002,2.555587330169931,234.32291838005634,21.591105592659222,null,2673.6945482899664,142.45950285367124,264.75674110469254,19.5,3.3633388154367951,224.66902734506795,22.081732869211859]
["7Z100","Max","Vmax","FFG900",null,24.285804966991005,27.492563242686742,28.350639023003616,null,5.3342948878271823,5.4944871474829009,null,13.872009977721699,2.1362792301105866,4.6403258171680442,1.5096533298592301,0.75,250,400,8,16,null,null,null,3240.9177672694755,181.08118109044207,374.98270624820395,10.500000000000002,2.555587330169931,234.32291838005634,21.591105592659222,null,3498.2882521563492,197.55994153522468,344.61870208877929,19.5,3.3633388154367951,224.66902734506795,22.081732869211859]
["7Z100","Max","Vmax","FFG1156",null,25.527232939609405,28.77960862046702,29.663992860557777,null,5.4260922135637282,5.5914163048941568,null,13.873681705068268,3.2044188451658799,4.7657625268099171,1.5096533298592301,0.75,250,400,8,16,null,null,2710.3300114922308,3240.9177672694755,181.08118109044207,374.98270624820395,16.8,2.555587330169931,299.28465895185576,21.591105592659222,2851.5607097649449,3498.2882521563492,197.55994153522468,344.61870208877929,31.2,3.3633388154367951,286.9544033117366,22.081732869211859]
[]
[]
["XPE Generated Datasheet (F/T) Tables"]
[null,null,"Commercial (nominal voltages, TT, 85C)",null,null,null,null,null,null,null,null,"Industrial (nominal voltages, TT, 100C)",null,null,null,null,null,null,null,null,"Commercial (max voltages, (TT+FF/2), 85C)",null,null,null,null,null,null,null,null,"Commercial (max voltages, (TT+FF/2), 100C)",null,null,null,null,null,null,null,null,"Industrial (max voltages, FF2, 100C)",null,null,null,null,null,null,null,null,"Extended -2L (max voltages, FF1.5, 100C)",null,null,null,null,null,null,null,null,"Q-Grade (max voltages, FF1.5, 125C)"]
["PART","Pkg","Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW"]
["KU040","FFG1165",154.89082023684637,4.0686338010645455,36.19714665329689,4,0,0,0,267.31431801384531,null,260.49143588219158,7.4812966282471853,50.740086108225888,4,0,0,0,402.50488750524539,null,402.70165567528983,15.920177471702445,83.309621432155225,1.6,0,0,0,645.03210931111528,null,621.40655768476665,26.981179511397023,119.81351060876349,1.6,0,0,0,955.27865910653497,null,432.0566643498633,19.143806554697836,77.203921121517439,3,0,0,0,670.34590536945711,null,368.27998994502298,16.128207870782681,62.687028789547405,3,0,0,0,572.77709211884053,null,751.6738582029983,36.676479637107306,113.23815814017732,3,0,0,0,1092.457973617046]
["KU060","FFG1166",154.89082023684637,4.0686338010645455,36.19714665329689,4,0,0,0,267.31431801384531,null,260.49143588219158,7.4812966282471853,50.740086108225888,4,0,0,0,402.50488750524539,null,402.70165567528983,15.920177471702445,83.309621432155225,1.6,0,0,0,645.03210931111528,null,621.40655768476665,26.981179511397023,119.81351060876349,1.6,0,0,0,955.27865910653497,null,432.0566643498633,19.143806554697836,77.203921121517439,3,0,0,0,670.34590536945711,null,368.27998994502298,16.128207870782681,62.687028789547405,3,0,0,0,572.77709211884053,null,751.6738582029983,36.676479637107306,113.23815814017732,3,0,0,0,1092.457973617046]
["KU075","FFG1167",154.89082023684637,4.0686338010645455,36.19714665329689,4,0,12.511680808782703,3.1225316981949502,283.57303686046197,null,260.49143588219158,7.4812966282471853,50.740086108225888,4,0,19.712938642896805,3.6273977788963325,426.57070348281781,null,402.70165567528983,15.920177471702445,83.309621432155225,1.6,0,36.129747604609406,5.0645635673764096,688.47516253173603,null,621.40655768476665,26.981179511397023,119.81351060876349,1.6,0,51.695388041236583,6.6601382488343432,1016.7168788350749,null,432.0566643498633,19.143806554697836,77.203921121517439,3,0,34.641234876499674,5.1796485971506332,712.39734506674711,null,368.27998994502298,16.128207870782681,62.687028789547405,3,0,28.400218609043684,4.6579029001213108,607.75853785330469,null,751.6738582029983,36.676479637107306,113.23815814017732,3,0,52.124958265546205,7.2234912645222948,1155.0315748859211]
["VU095","FFGA1760",154.89082023684637,4.0686338010645455,36.19714665329689,4,0,25.023361617565406,6.2450633963899005,299.83175570707863,null,260.49143588219158,7.4812966282471853,50.740086108225888,4,0,39.425877285793611,7.2547955577926651,450.63651946039016,null,402.70165567528983,15.920177471702445,83.309621432155225,1.6,0,72.259495209218812,10.129127134752819,731.91821575235667,null,621.40655768476665,26.981179511397023,119.81351060876349,1.6,0,103.39077608247317,13.320276497668686,1078.1550985636147,null,432.0566643498633,19.143806554697836,77.203921121517439,3,0,69.282469752999347,10.359297194301266,754.44878476403699,null,368.27998994502298,16.128207870782681,62.687028789547405,3,0,56.800437218087367,9.3158058002426216,642.73998358776896,null,751.6738582029983,36.676479637107306,113.23815814017732,3,0,104.24991653109241,14.44698252904459,1217.605176154796]
["7A200T","FBG484",327.76418781269888,11.035118025584048,72.857953715399134,5,0,12.511680808782703,3.1225316981949502,531.20234137261809,null,555.3797493394967,20.254732442530411,106.98227353361229,5,0,19.712938642896805,3.6273977788963325,837.26839012010169,null,884.10838872774809,42.994518830348071,170.09499358010856,2.6,0,36.129747604609406,5.0645635673764096,1388.2946440230271,null,1374.6153873675987,72.953629007307313,249.15057766503739,2.6,0,51.695388041236583,6.6601382488343432,2102.194278709112,null,947.60222339150823,51.691907165648608,156.92586222314458,4.8,0,34.641234876499674,5.1796485971506332,1441.9721563840478,null,804.87917574292737,43.573104733190867,125.52861050931205,4.8,0,28.400218609043684,4.6579029001213108,1217.1774140969881,null,1658.5453640847545,99.316551154218331,234.72067435731316,4.8,0,52.124958265546205,7.2234912645222948,2406.0226868051191]
["7A200T","FBG676",327.76418781269888,11.035118025584048,72.857953715399134,5,0,25.023361617565406,6.2450633963899005,547.4610602192347,null,555.3797493394967,20.254732442530411,106.98227353361229,5,0,39.425877285793611,7.2547955577926651,861.33420609767404,null,884.10838872774809,42.994518830348071,170.09499358010856,2.6,0,72.259495209218812,10.129127134752819,1431.7376972436477,null,1374.6153873675987,72.953629007307313,249.15057766503739,2.6,0,103.39077608247317,13.320276497668686,2163.6324984376524,null,947.60222339150823,51.691907165648608,156.92586222314458,4.8,0,69.282469752999347,10.359297194301266,1484.0235960813377,null,804.87917574292737,43.573104733190867,125.52861050931205,4.8,0,56.800437218087367,9.3158058002426216,1252.1588598314522,null,1658.5453640847545,99.316551154218331,234.72067435731316,4.8,0,104.24991653109241,14.44698252904459,2468.5962880739939]
["7A200T","FFG1156",327.76418781269888,11.035118025584048,72.857953715399134,5,0,50.046723235130813,12.490126792779801,579.97849791246801,null,555.3797493394967,20.254732442530411,106.98227353361229,5,0,78.851754571587222,14.50959111558533,909.46583805281887,null,884.10838872774809,42.994518830348071,170.09499358010856,2.6,0,144.51899041843762,20.258254269505638,1518.623803684889,null,1374.6153873675987,72.953629007307313,249.15057766503739,2.6,0,206.78155216494633,26.640552995337373,2286.5089378947323,null,947.60222339150823,51.691907165648608,156.92586222314458,4.8,0,138.56493950599869,20.718594388602533,1568.1264754759177,null,804.87917574292737,43.573104733190867,125.52861050931205,4.8,0,113.60087443617473,18.631611600485243,1322.1217513003808,null,1658.5453640847545,99.316551154218331,234.72067435731316,4.8,0,208.49983306218482,28.893965058089179,2593.7434906117442]
[]
[null,null,"Commercial (nominal voltages, TT, 85C)",null,null,null,null,null,null,null,null,"Industrial (nominal voltages, TT, 100C)",null,null,null,null,null,null,null,null,"Commercial (max voltages, (TT+FF/2), 85C)",null,null,null,null,null,null,null,null,"Commercial (max voltages, (TT+FF/2), 100C)",null,null,null,null,null,null,null,null,"Industrial (max voltages, FF2, 100C)",null,null,null,null,null,null,null,null,"Extended -2L (max voltages, FF1.5, 100C)",null,null,null,null,null,null,null,null,"Q-Grade (max voltages, FF1.5, 125C)"]
["PART","Pkg","Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW"]
["7K70T","SB324",241.28225634399141,5.808242491061284,21.32577661417605,1,0.37446040998184815,39.787144971928996,6.2626744751677199,371.25327982066727,null,405.81774254048588,10.680043250156706,28.972102717657556,1,0.7748098874462046,62.884274270840812,7.2752540812656408,579.45680764818894,null,578.6673161426412,15.204921286716202,50.460669768929108,1.6,1.2777936650849655,133.0619429372463,10.795552796329611,907.77931986077056,null,890.32945551018975,25.768978481725515,71.638206510183124,1.6,2.4715718682031764,190.38850890794069,14.196657449279803,1345.1360581098877,null,605.33978328811315,18.283720285762318,47.029206493911474,3,1.6816694077183976,127.98110664835121,11.040866434605929,930.3993029212304,null,514.67042864159043,15.403605368528819,38.645013108340464,3,1.3660256305658847,99.003373112724262,9.9287206112579849,786.39827787968636,null,1045.1169679146803,35.028691542370836,67.991406588407727,3,3.6469405614374213,181.70799185347619,15.39749285057802,1504.5687755468039]
["7K70T","FBG484",241.28225634399141,5.808242491061284,21.32577661417605,1,0.18723020499092408,19.893572485964498,3.13133723758386,347.26508828061844,null,405.81774254048588,10.680043250156706,28.972102717657556,1,0.3874049437231023,31.442137135420406,3.6376270406328204,542.95218916530757,null,578.6673161426412,15.204921286716202,50.460669768929108,1.6,0.63889683254248275,66.53097146862315,5.3977763981648055,831.43119513814247,null,890.32945551018975,25.768978481725515,71.638206510183124,1.6,1.2357859341015882,95.194254453970345,7.0983287246399014,1236.0688277129032,null,605.33978328811315,18.283720285762318,47.029206493911474,3,0.84083470385919878,63.990553324175607,5.5204332173029647,856.14335593790736,null,514.67042864159043,15.403605368528819,38.645013108340464,3,0.68301281528294233,49.501686556362131,4.9643603056289924,728.04180384243637,null,1045.1169679146803,35.028691542370836,67.991406588407727,3,1.8234702807187106,90.853995926738094,7.6987464252890101,1398.1462816198284]
["7K70T","FBG676",241.28225634399141,5.808242491061284,21.32577661417605,1,0.37446040998184815,39.787144971928996,6.2626744751677199,371.25327982066727,null,405.81774254048588,10.680043250156706,28.972102717657556,1,0.7748098874462046,62.884274270840812,7.2752540812656408,579.45680764818894,null,578.6673161426412,15.204921286716202,50.460669768929108,1.6,1.2777936650849655,133.0619429372463,10.795552796329611,907.77931986077056,null,890.32945551018975,25.768978481725515,71.638206510183124,1.6,2.4715718682031764,190.38850890794069,14.196657449279803,1345.1360581098877,null,605.33978328811315,18.283720285762318,47.029206493911474,3,1.6816694077183976,127.98110664835121,11.040866434605929,930.3993029212304,null,514.67042864159043,15.403605368528819,38.645013108340464,3,1.3660256305658847,99.003373112724262,9.9287206112579849,786.39827787968636,null,1045.1169679146803,35.028691542370836,67.991406588407727,3,3.6469405614374213,181.70799185347619,15.39749285057802,1504.5687755468039]
["7K160T","FBG484",473.73915093689925,13.989817736383044,39.855262805190513,1,0.18723020499092408,20.018689294052326,3.13133723758386,621.38175007076188,null,806.2593215006292,25.682299739202207,57.340601846386349,1,0.3874049437231023,31.442137135420406,3.6376270406328204,1009.4593230462081,null,1231.1853525443262,27.778761334188516,149.03126142055586,2.1,0.63889683254248275,66.949405251444674,5.3977763981648055,1704.1502328986548,null,1917.2123046663855,47.122356706035376,216.67443176288853,2.1,1.2357859341015882,95.792960456825512,7.0983287246399014,2591.432274825378,null,1293.8861118479219,32.960323641490383,146.1670478006923,3.9,0.84083470385919878,63.990553324175607,5.5204332173029647,1769.5344958807261,null,1086.8353866145312,37.088302050602607,111.68525703850027,3.9,0.68301281528294233,49.337229125942322,4.9643603056289924,1479.2846180117708,null,2241.1398822054475,84.502057955334223,205.77990547446811,3.9,1.8234702807187106,90.552155408709055,7.6987464252890101,2942.817817905755]
["7K160T","FBG676",473.73915093689925,13.989817736383044,39.855262805190513,1,0.37446040998184815,40.037378588104652,6.2626744751677199,645.49505841889857,null,806.2593215006292,25.682299739202207,57.340601846386349,1,0.7748098874462046,62.884274270840812,7.2752540812656408,1045.9639415290897,null,1231.1853525443262,27.778761334188516,149.03126142055586,2.1,1.2777936650849655,133.89881050288935,10.795552796329611,1780.9293444175894,null,1917.2123046663855,47.122356706035376,216.67443176288853,2.1,2.4715718682031764,191.58592091365102,14.196657449279803,2701.1161724053031,null,1293.8861118479219,32.960323641490383,146.1670478006923,3.9,1.6816694077183976,127.98110664835121,11.040866434605929,1843.7904428640493,null,1086.8353866145312,37.088302050602607,111.68525703850027,3.9,1.3660256305658847,98.674458251884644,9.9287206112579849,1537.4717008956886,null,2241.1398822054475,84.502057955334223,205.77990547446811,3.9,3.6469405614374213,181.10431081741811,15.39749285057802,3048.9294160991608]
["7K160T","FFG676",473.73915093689925,13.989817736383044,39.855262805190513,1,0.37446040998184815,40.037378588104652,6.2626744751677199,645.49505841889857,null,806.2593215006292,25.682299739202207,57.340601846386349,1,0.7748098874462046,62.884274270840812,7.2752540812656408,1045.9639415290897,null,1231.1853525443262,27.778761334188516,149.03126142055586,2.1,1.2777936650849655,133.89881050288935,10.795552796329611,1780.9293444175894,null,1917.2123046663855,47.122356706035376,216.67443176288853,2.1,2.4715718682031764,191.58592091365102,14.196657449279803,2701.1161724053031,null,1293.8861118479219,32.960323641490383,146.1670478006923,3.9,1.6816694077183976,127.98110664835121,11.040866434605929,1843.7904428640493,null,1086.8353866145312,37.088302050602607,111.68525703850027,3.9,1.3660256305658847,98.674458251884644,9.9287206112579849,1537.4717008956886,null,2241.1398822054475,84.502057955334223,205.77990547446811,3.9,3.6469405614374213,181.10431081741811,15.39749285057802,3048.9294160991608]
["7K325T","FBG676",809.90559200209577,19.178923562926332,68.425687437088442,1,0.37446040998184815,39.787144971928996,6.2626744751677199,1038.0271360318791,null,1379.6220330465596,35.181925507879882,100.66647506111411,1,0.7748098874462046,62.884274270840812,7.2752540812656408,1706.8128506302075,null,2178.9165645650892,38.056796769754378,268.05189243765011,2.1,1.2777936650849655,133.0619429372463,10.795552796329611,2991.7658883273039,null,3395.6195052930148,64.543378261520644,392.74787591771116,2.1,2.4715718682031764,190.38850890794069,14.196657449279803,4573.3647163396154,null,2285.995828786009,45.175733240874493,262.14939546635651,3.9,1.6816694077183976,127.98110664835121,11.040866434605929,3097.4519602857499,null,1920.7599006364303,50.760694630776925,198.89914738369879,3.9,1.3660256305658847,99.003373112724262,9.9287206112579849,2575.6695497549144,null,3964.3491278000206,115.64984056426488,372.07434459038467,3.9,3.6469405614374213,181.70799185347619,15.39749285057802,5170.8354365449923]
["7K325T","FBG900",809.90559200209577,19.178923562926332,68.425687437088442,1,0.7489208199636963,79.574289943857991,12.52534895033544,1086.0035191119766,null,1379.6220330465596,35.181925507879882,100.66647506111411,1,1.5496197748924092,125.76854854168162,14.550508162531282,1779.8220875959705,null,2178.9165645650892,38.056796769754378,268.05189243765011,2.1,2.555587330169931,266.1238858744926,21.591105592659222,3144.4621377725603,null,3395.6195052930148,64.543378261520644,392.74787591771116,2.1,4.9431437364063529,380.77701781588138,28.393314898559606,4791.4991771335835,null,2285.995828786009,45.175733240874493,262.14939546635651,3.9,3.3633388154367951,255.96221329670243,22.081732869211859,3245.9638542523962,null,1920.7599006364303,50.760694630776925,198.89914738369879,3.9,2.7320512611317693,198.00674622544852,19.85744122251597,2692.3824978294142,null,3964.3491278000206,115.64984056426488,372.07434459038467,3.9,7.2938811228748426,363.41598370695237,30.79498570115604,5383.6804243989427]
["7K325T","FFG676",809.90559200209577,19.178923562926332,68.425687437088442,1,0.37446040998184815,39.787144971928996,6.2626744751677199,1038.0271360318791,null,1379.6220330465596,35.181925507879882,100.66647506111411,1,0.7748098874462046,62.884274270840812,7.2752540812656408,1706.8128506302075,null,2178.9165645650892,38.056796769754378,268.05189243765011,2.1,1.2777936650849655,133.0619429372463,10.795552796329611,2991.7658883273039,null,3395.6195052930148,64.543378261520644,392.74787591771116,2.1,2.4715718682031764,190.38850890794069,14.196657449279803,4573.3647163396154,null,2285.995828786009,45.175733240874493,262.14939546635651,3.9,1.6816694077183976,127.98110664835121,11.040866434605929,3097.4519602857499,null,1920.7599006364303,50.760694630776925,198.89914738369879,3.9,1.3660256305658847,99.003373112724262,9.9287206112579849,2575.6695497549144,null,3964.3491278000206,115.64984056426488,372.07434459038467,3.9,3.6469405614374213,181.70799185347619,15.39749285057802,5170.8354365449923]
["7K325T","FFG900",809.90559200209577,19.178923562926332,68.425687437088442,1,0.7489208199636963,79.574289943857991,12.52534895033544,1086.0035191119766,null,1379.6220330465596,35.181925507879882,100.66647506111411,1,1.5496197748924092,125.76854854168162,14.550508162531282,1779.8220875959705,null,2178.9165645650892,38.056796769754378,268.05189243765011,2.1,2.555587330169931,266.1238858744926,21.591105592659222,3144.4621377725603,null,3395.6195052930148,64.543378261520644,392.74787591771116,2.1,4.9431437364063529,380.77701781588138,28.393314898559606,4791.4991771335835,null,2285.995828786009,45.175733240874493,262.14939546635651,3.9,3.3633388154367951,255.96221329670243,22.081732869211859,3245.9638542523962,null,1920.7599006364303,50.760694630776925,198.89914738369879,3.9,2.7320512611317693,198.00674622544852,19.85744122251597,2692.3824978294142,null,3964.3491278000206,115.64984056426488,372.07434459038467,3.9,7.2938811228748426,363.41598370695237,30.79498570115604,5383.6804243989427]
["7K355T","FFG901",993.04316840436024,30.809563431967877,74.850258145311443,1,1.1233812299455446,119.361434915787,18.788023425503162,1340.3123457381816,null,1693.7685679735905,56.528261546614885,112.04260637312595,1,2.3244296623386136,188.65282281252243,21.825762243796923,2208.8012318891201,null,2510.4279528554607,60.345634685046605,304.03609306660769,2.1,3.8333809952548963,399.18582881173887,32.386658388988835,3729.5827593983799,null,3917.4431007332728,102.36718995052374,448.08619530672399,2.1,7.4147156046095297,571.16552672382204,42.589972347839407,5690.6598909159247,null,2639.6583052779242,72.616873508023986,295.60522774383702,3.9,5.0450082231551931,383.94331994505359,33.122599303817786,3850.243996485317,null,2223.5487334881118,81.522707428137039,223.8757688358057,3.9,4.0980768916976542,297.01011933817284,29.786161833773949,3199.8586314669096,null,4597.0469705900377,185.82368648327832,423.72353504043701,3.9,10.940821684312263,545.12397556042856,46.192478551734055,6418.1002215737926]
["7K410T","FBG676",1080.0448519277747,34.284830260849482,85.181018298547883,1,0.37446040998184815,39.787144971928996,6.2626744751677199,1353.4318982061079,null,1847.211516652045,62.846887525575696,127.40986793855343,1,0.7748098874462046,62.884274270840812,7.2752540812656408,2250.2054034327798,null,2554.3898317286385,67.106255579492824,345.38132390196034,2.6,1.2777936650849655,133.0619429372463,10.795552796329611,3555.5219215473358,null,3997.4580334894436,113.80263877398664,508.90377106666705,2.6,2.4715718682031764,190.38850890794069,14.196657449279803,5464.4750805413041,null,2687.7863167523406,80.721389572179802,337.06586584607641,4.8,1.6816694077183976,127.98110664835121,11.040866434605929,3691.2013179299865,null,2267.0291274634865,90.689139341453966,255.31513759708668,4.8,1.3660256305658847,99.003373112724262,9.9287206112579849,3081.7803729420825,null,4703.6748705004793,206.63557362703904,483.1207691860107,4.8,3.6469405614374213,181.70799185347619,15.39749285057802,6237.6349990668541]
["7K410T","FBG900",1080.0448519277747,34.284830260849482,85.181018298547883,1,0.7489208199636963,79.574289943857991,12.52534895033544,1401.4082812862055,null,1847.211516652045,62.846887525575696,127.40986793855343,1,1.5496197748924092,125.76854854168162,14.550508162531282,2323.2146403985421,null,2554.3898317286385,67.106255579492824,345.38132390196034,2.6,2.555587330169931,266.1238858744926,21.591105592659222,3708.2181709925926,null,3997.4580334894436,113.80263877398664,508.90377106666705,2.6,4.9431437364063529,380.77701781588138,28.393314898559606,5682.6095413352732,null,2687.7863167523406,80.721389572179802,337.06586584607641,4.8,3.3633388154367951,255.96221329670243,22.081732869211859,3839.7132118966329,null,2267.0291274634865,90.689139341453966,255.31513759708668,4.8,2.7320512611317693,198.00674622544852,19.85744122251597,3198.4933210165827,null,4703.6748705004793,206.63557362703904,483.1207691860107,4.8,7.2938811228748426,363.41598370695237,30.79498570115604,6450.4799869208055]
["7K410T","FFG676",1080.0448519277747,34.284830260849482,85.181018298547883,1,0.37446040998184815,39.787144971928996,6.2626744751677199,1353.4318982061079,null,1847.211516652045,62.846887525575696,127.40986793855343,1,0.7748098874462046,62.884274270840812,7.2752540812656408,2250.2054034327798,null,2554.3898317286385,67.106255579492824,345.38132390196034,2.6,1.2777936650849655,133.0619429372463,10.795552796329611,3555.5219215473358,null,3997.4580334894436,113.80263877398664,508.90377106666705,2.6,2.4715718682031764,190.38850890794069,14.196657449279803,5464.4750805413041,null,2687.7863167523406,80.721389572179802,337.06586584607641,4.8,1.6816694077183976,127.98110664835121,11.040866434605929,3691.2013179299865,null,2267.0291274634865,90.689139341453966,255.31513759708668,4.8,1.3660256305658847,99.003373112724262,9.9287206112579849,3081.7803729420825,null,4703.6748705004793,206.63557362703904,483.1207691860107,4.8,3.6469405614374213,181.70799185347619,15.39749285057802,6237.6349990668541]
["7K410T","FFG900",1080.0448519277747,34.284830260849482,85.181018298547883,1,0.7489208199636963,79.574289943857991,12.52534895033544,1401.4082812862055,null,1847.211516652045,62.846887525575696,127.40986793855343,1,1.5496197748924092,125.76854854168162,14.550508162531282,2323.2146403985421,null,2554.3898317286385,67.106255579492824,345.38132390196034,2.6,2.555587330169931,266.1238858744926,21.591105592659222,3708.2181709925926,null,3997.4580334894436,113.80263877398664,508.90377106666705,2.6,4.9431437364063529,380.77701781588138,28.393314898559606,5682.6095413352732,null,2687.7863167523406,80.721389572179802,337.06586584607641,4.8,3.3633388154367951,255.96221329670243,22.081732869211859,3839.7132118966329,null,2267.0291274634865,90.689139341453966,255.31513759708668,4.8,2.7320512611317693,198.00674622544852,19.85744122251597,3198.4933210165827,null,4703.6748705004793,206.63557362703904,483.1207691860107,4.8,7.2938811228748426,363.41598370695237,30.79498570115604,6450.4799869208055]
["7K420T","FFG901",1313.0217661397098,41.194549460674565,99.486223775371457,1,1.3106114349364686,139.25500740175147,21.919360663087023,1739.0088591763945,null,2239.8462869087962,75.523787814065898,149.00195404678203,1,2.711834606061716,220.09495994794281,25.463389284429745,2876.9059213872392,null,3444.5025917638841,80.612216027399484,404.74317327938331,1.7,4.4722778277973791,465.71680028036195,37.784434787153636,4978.4827225814533,null,5375.3017534930277,136.6883811521557,596.60417452859917,1.7,8.6505015387111168,666.35978117779234,49.688301072479305,7616.6153413224829,null,3616.5170694047179,96.985632458822963,393.4552747059804,3,5.8858429270143917,447.93387326922925,38.643032521120752,5138.999880997012,null,3047.6022558589257,108.90451661965275,297.85195714075718,3,4.7810897069805964,346.51180589453497,34.750522139402946,4273.3074929097174,null,6301.181344829215,248.13276999401288,563.99280818221882,3,12.764291965030974,635.97797148716666,53.891224977023072,8607.3674032211457]
["7K420T","FFG1156",1313.0217661397098,41.194549460674565,99.486223775371457,1,1.4978416399273926,159.14857988771598,25.05069790067088,1762.9970507164435,null,2239.8462869087962,75.523787814065898,149.00195404678203,1,3.0992395497848184,251.53709708336325,29.101016325062563,2913.4105398701208,null,3444.5025917638841,80.612216027399484,404.74317327938331,1.7,5.111174660339862,532.2477717489852,43.182211185318444,5054.8308473040815,null,5375.3017534930277,136.6883811521557,596.60417452859917,1.7,9.8862874728127057,761.55403563176276,56.786629797119211,7725.682571719467,null,3616.5170694047179,96.985632458822963,393.4552747059804,3,6.7266776308735903,511.92442659340486,44.163465738423717,5213.2558279803352,null,3047.6022558589257,108.90451661965275,297.85195714075718,3,5.4641025222635387,396.01349245089705,39.71488244503194,4331.6639669469678,null,6301.181344829215,248.13276999401288,563.99280818221882,3,14.587762245749685,726.83196741390475,61.589971402312081,8713.7898971481209]
["7K480T","FFG901",1313.0217661397098,41.194549460674565,99.486223775371457,1,1.3106114349364686,139.25500740175147,21.919360663087023,1739.0088591763945,null,2239.8462869087962,75.523787814065898,149.00195404678203,1,2.711834606061716,220.09495994794281,25.463389284429745,2876.9059213872392,null,3444.5025917638841,80.612216027399484,404.74317327938331,1.7,4.4722778277973791,465.71680028036195,37.784434787153636,4978.4827225814533,null,5375.3017534930277,136.6883811521557,596.60417452859917,1.7,8.6505015387111168,666.35978117779234,49.688301072479305,7616.6153413224829,null,3616.5170694047179,96.985632458822963,393.4552747059804,3,5.8858429270143917,447.93387326922925,38.643032521120752,5138.999880997012,null,3047.6022558589257,108.90451661965275,297.85195714075718,3,4.7810897069805964,346.51180589453497,34.750522139402946,4273.3074929097174,null,6301.181344829215,248.13276999401288,563.99280818221882,3,12.764291965030974,635.97797148716666,53.891224977023072,8607.3674032211457]
["7K480T","FFG1156",1313.0217661397098,41.194549460674565,99.486223775371457,1,1.4978416399273926,159.14857988771598,25.05069790067088,1762.9970507164435,null,2239.8462869087962,75.523787814065898,149.00195404678203,1,3.0992395497848184,251.53709708336325,29.101016325062563,2913.4105398701208,null,3444.5025917638841,80.612216027399484,404.74317327938331,1.7,5.111174660339862,532.2477717489852,43.182211185318444,5054.8308473040815,null,5375.3017534930277,136.6883811521557,596.60417452859917,1.7,9.8862874728127057,761.55403563176276,56.786629797119211,7725.682571719467,null,3616.5170694047179,96.985632458822963,393.4552747059804,3,6.7266776308735903,511.92442659340486,44.163465738423717,5213.2558279803352,null,3047.6022558589257,108.90451661965275,297.85195714075718,3,5.4641025222635387,396.01349245089705,39.71488244503194,4331.6639669469678,null,6301.181344829215,248.13276999401288,563.99280818221882,3,14.587762245749685,726.83196741390475,61.589971402312081,8713.7898971481209]
[]
[null,null,"Commercial (nominal voltages, TT, 85C)",null,null,null,null,null,null,null,null,"Industrial (nominal voltages, TT, 100C)",null,null,null,null,null,null,null,null,"Commercial (max voltages, (TT+FF/2), 85C)",null,null,null,null,null,null,null,null,"Commercial (max voltages, (TT+FF/2), 100C)",null,null,null,null,null,null,null,null,"Industrial (max voltages, FF2, 100C)",null,null,null,null,null,null,null,null,"Extended -2L (max voltages, FF1.5, 100C)",null,null,null,null,null,null,null,null,"Q-Grade (max voltages, FF1.5, 125C)"]
["PART","Pkg","Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Static mW"]
["7V585T","FFG1157",1482.6591197105056,34.284830260849482,114.14562461087685,1,0.93615102495462033,96.965526268065943,15.656686187919302,1877.6446958094209,null,2521.1357903285148,62.846887525575696,171.44139323514821,1,1.9370247186155116,165.58868460033315,18.188135203164101,3121.2782770149952,null,3938.6583411807705,76.053756323425205,469.19813002509233,5.3,3.1944841627124139,324.28618168668515,26.98888199082403,5450.075813863763,null,6125.5948944863285,128.97632394385153,692.37153083276746,5.3,6.1789296705079408,463.99715221274846,35.491643623199508,8338.8103565831207,null,4134.3906993647124,91.484241515137114,453.1988528433651,9.8000000000000007,4.2041735192959937,337.00354101760195,27.602166086514824,5661.5610535254455,null,3485.1850236820787,90.689139341453966,342.8874569696502,9.8000000000000007,3.4150640764147115,246.68614562971169,24.821801528144963,4685.6650960064662,null,7174.7753179417105,206.63557362703904,650.77457639670297,9.8000000000000007,9.1173514035935526,452.76077704354532,38.493732126445053,9426.8971586726093]
["7V585T","FFG1761",1482.6591197105056,34.284830260849482,114.14562461087685,1,1.6850718449183166,174.5379472825187,28.18203513825474,1971.5955930402108,null,2521.1357903285148,62.846887525575696,171.44139323514821,1,3.4866444935079208,298.05963228059966,32.738643365695381,3273.9991500851056,null,3938.6583411807705,76.053756323425205,469.19813002509233,5.3,5.7500714928823449,583.71512703603321,48.579987583483245,5748.572524013377,null,6125.5948944863285,128.97632394385153,692.37153083276746,5.3,11.122073406914295,835.19487398294723,63.884958521759103,8765.2126032440065,null,4134.3906993647124,91.484241515137114,453.1988528433651,9.8000000000000007,7.5675123347327888,606.60637383168353,49.683898955726683,5972.6346795616382,null,3485.1850236820787,90.689139341453966,342.8874569696502,9.8000000000000007,6.1471153375464809,444.03506213348101,44.679242750660926,4918.4134275421366,null,7174.7753179417105,206.63557362703904,650.77457639670297,9.8000000000000007,16.411232526468396,814.96939867838148,69.28871782760109,9851.3435514462308]
["7V2000T","FHG1761",3755.9095848651928,55.669954036290832,314.91243052062964,1,1.6850718449183166,152.01692182670988,28.18203513825474,4713.0904071520854,null,6432.2664124975527,102.11931740513785,488.64792463710251,1,3.4866444935079208,248.38302690049971,32.738643365695381,7853.6973532771235,null,7193.8165104369518,86.534397936541339,967.8651505431319,6.4,5.7500714928823449,508.39704612815797,48.579987583483245,10114.162544652736,null,11272.927703083988,146.74274891876303,1442.2269394723862,6.4,11.122073406914295,727.42779346901852,63.884958521759103,15528.570443223287,null,11272.927703083988,146.74274891876303,1514.3382864460057,11.7,11.122073406914295,754.36956359750059,63.884958521759103,15702.627912235765,null,9561.3380748723648,146.74274891876303,1225.8928985515283,11.7,11.122073406914295,808.25310385446505,63.884958521759103,13450.028858521904,null,18728.630344388479,318.47405494103049,2272.8029166401625,11.7,28.106467804134546,1384.8765436339008,105.73474499857325,25724.701585488114]
["7V2000T","FLG1925",3755.9095848651928,55.669954036290832,314.91243052062964,1,0.7489208199636963,67.563076367426603,12.52534895033544,4608.1634664223811,null,6432.2664124975527,102.11931740513785,488.64792463710251,1,1.5496197748924092,110.39245640022209,14.550508162531282,7690.3943760395414,null,7193.8165104369518,86.534397936541339,967.8651505431319,6.4,2.555587330169931,225.95424272362578,21.591105592659222,9784.1403365963361,null,11272.927703083988,146.74274891876303,1442.2269394723862,6.4,4.9431437364063529,323.30124154178606,28.393314898559606,15057.234353191263,null,11272.927703083988,146.74274891876303,1514.3382864460057,11.7,4.9431437364063529,335.27536159888922,28.393314898559606,15215.875142630219,null,9561.3380748723648,146.74274891876303,1225.8928985515283,11.7,4.9431437364063529,359.2236017130956,28.393314898559606,12932.442729769318,null,18728.630344388479,318.47405494103049,2272.8029166401625,11.7,12.491763468504242,615.50068605951162,46.993219999365891,24831.105173416548]
["7VX330T","FFG1157",1011.831565186405,32.328981396793779,73.228788529339269,1,0.93615102495462033,62.558404043913512,15.625304744352441,1296.7662075180642,null,1717.2651546193583,59.30702819230472,108.36346257149899,1,1.9370247186155116,98.564693214484024,18.15167985548619,2133.2597689749364,null,2457.8542815706733,71.729868023800933,291.9125688446062,3.6,3.1944841627124139,201.88504915067205,25.631933474216869,3454.3691036981104,null,3815.0174594629111,121.65906248634128,428.65979026523951,3.6,6.1789296705079408,288.8624097179308,33.707192782189324,5267.1669702310337,null,2578.5810959603805,86.316095999720574,282.48871583233523,6.6,4.2041735192959937,193.56756881384578,26.214382837880258,3575.617788421569,null,2156.3129820216855,85.517502926056736,214.59229909917184,6.6,3.4150640764147115,158.69414844860773,23.573809604115461,2970.9074720501048,null,4428.0979294016006,194.88081231781635,403.43183380833989,6.6,9.1173514035935526,291.26275324641284,36.558342111941599,5943.4627666069027]
["7VX330T","FFG1761",1011.831565186405,32.328981396793779,73.228788529339269,1,1.3106114349364686,87.581765661478926,21.875426642093419,1329.963744150886,null,1717.2651546193583,59.30702819230472,108.36346257149899,1,2.711834606061716,137.99057050027764,25.412351797680671,2182.7931103887668,null,2457.8542815706733,71.729868023800933,291.9125688446062,3.6,4.4722778277973791,282.63906881094084,35.884706863903617,3552.520573497909,null,3815.0174594629111,121.65906248634128,428.65979026523951,3.6,8.6505015387111168,404.40737360510309,47.190069895065051,5407.3346298398337,null,2578.5810959603805,86.316095999720574,282.48871583233523,6.6,5.8858429270143917,270.99459633938409,36.70013597303236,3671.3761915333898,null,2156.3129820216855,85.517502926056736,214.59229909917184,6.6,4.7810897069805964,222.17180782805082,33.003333445761648,3050.4149229527029,null,4428.0979294016006,194.88081231781635,403.43183380833989,6.6,12.764291965030974,407.76785454497792,51.181678956718237,6088.1965653021598]
["7VX415T","FFG1157",1324.277091249792,37.952319415652006,88.029206590233983,1,0.93615102495462033,62.558404043913512,15.625304744352441,1641.4758241099198,null,2246.5941212841735,69.572738087407458,133.16019931234416,1,1.9370247186155116,98.564693214484024,18.15167985548619,2717.4885716683757,null,3564.3645257009598,84.17342774500726,367.31191650897841,3.1,3.1944841627124139,201.88504915067205,25.631933474216869,4748.4512887508126,null,5529.9062154791691,142.76207221950833,543.23870967699247,3.1,6.1789296705079408,288.8624097179308,33.707192782189324,7270.8476466411548,null,3722.0721855747893,101.26060224158572,354.36800079737748,5.7,4.2041735192959937,193.56756881384578,26.214382837880258,4902.9573007374611,null,3098.1767641779743,100.36673642370859,267.56369314902889,5.7,3.4150640764147115,158.69414844860773,23.573809604115461,4054.736812927893,null,6359.0065308729108,228.72623040143168,510.10202221700342,5.7,9.1173514035935526,291.26275324641284,36.558342111941599,8167.0650628408521]
["7VX415T","FFG1158",1324.277091249792,37.952319415652006,88.029206590233983,1,2.2467624598910891,150.14016970539245,37.500731386445857,1757.6672023247966,null,2246.5941212841735,69.572738087407458,133.16019931234416,1,4.6488593246772272,236.55526371476168,43.564031653166865,2890.8552666167811,null,3564.3645257009598,84.17342774500726,367.31191650897841,3.1,7.6667619905097926,484.52411796161283,61.516640338120489,5091.9814330501085,null,5529.9062154791691,142.76207221950833,543.23870967699247,3.1,14.829431209219059,693.26978332303383,80.897262677254375,7761.4344552719567,null,3722.0721855747893,101.26060224158572,354.36800079737748,5.7,10.090016446310386,464.56216515322984,62.914518810912618,5238.1117116288333,null,3098.1767641779743,100.36673642370859,267.56369314902889,5.7,8.1961537833953084,380.86595627665849,56.577143049877101,4333.0128910869862,null,6359.0065308729108,228.72623040143168,510.10202221700342,5.7,21.881643368624527,699.03060779139071,87.740021068659829,8673.63335827425]
["7VX415T","FFG1927",1324.277091249792,37.952319415652006,88.029206590233983,1,2.2467624598910891,150.14016970539245,37.500731386445857,1757.6672023247966,null,2246.5941212841735,69.572738087407458,133.16019931234416,1,4.6488593246772272,236.55526371476168,43.564031653166865,2890.8552666167811,null,3564.3645257009598,84.17342774500726,367.31191650897841,3.1,7.6667619905097926,484.52411796161283,61.516640338120489,5091.9814330501085,null,5529.9062154791691,142.76207221950833,543.23870967699247,3.1,14.829431209219059,693.26978332303383,80.897262677254375,7761.4344552719567,null,3722.0721855747893,101.26060224158572,354.36800079737748,5.7,10.090016446310386,464.56216515322984,62.914518810912618,5238.1117116288333,null,3098.1767641779743,100.36673642370859,267.56369314902889,5.7,8.1961537833953084,380.86595627665849,56.577143049877101,4333.0128910869862,null,6359.0065308729108,228.72623040143168,510.10202221700342,5.7,21.881643368624527,699.03060779139071,87.740021068659829,8673.63335827425]
["7VX485T","FFG1157",1578.061942906234,44.393853458150232,104.48573430567565,1,0.93615102495462033,96.965526268065943,15.656686187919302,1965.7687396530878,null,2678.5794284039962,81.419448357464788,158.3024295316294,1,1.9370247186155116,165.58868460033315,18.188135203164101,3273.644341256032,null,4018.0522936593361,98.571104456565806,448.9744725375653,3.6,3.1944841627124139,324.28618168668515,26.98888199082403,5513.6087408423946,null,6237.1151914704978,167.13374656036987,664.2587009635082,3.6,6.1789296705079408,463.99715221274846,35.491643623199508,8436.6321593189314,null,4217.8950909953519,117.85640622214011,422.21495889454127,6.6,4.2041735192959937,337.00354101760195,27.602166086514824,5710.1263469899404,null,3581.4893241167324,117.47856930356626,318.47234241369978,6.6,3.4150640764147115,246.68614562971169,24.821801528144963,4760.2590718043884,null,7356.4077384813263,267.64021897558399,607.6650982664753,6.6,9.1173514035935526,452.76077704354532,38.493732126445053,9589.2884228712828]
["7VX485T","FFG1158",1578.061942906234,44.393853458150232,104.48573430567565,1,2.2467624598910891,232.71726304335832,37.576046851006325,2130.1828098069705,null,2678.5794284039962,81.419448357464788,158.3024295316294,1,4.6488593246772272,397.4128430407996,43.651524487593846,3540.905869128725,null,4018.0522936593361,98.571104456565806,448.9744725375653,3.6,7.6667619905097926,778.28683604804428,64.773316777977669,6035.9779836042171,null,6237.1151914704978,167.13374656036987,664.2587009635082,3.6,14.829431209219059,1113.5931653105963,85.179944695678813,9182.8360909754792,null,4217.8950909953519,117.85640622214011,422.21495889454127,6.6,10.090016446310386,808.80849844224451,66.245198607635572,6254.505192553278,null,3581.4893241167324,117.47856930356626,318.47234241369978,6.6,8.1961537833953084,592.04674951130801,59.572323667547899,5167.5686519918127,null,7356.4077384813263,267.64021897558399,607.6650982664753,6.6,21.881643368624527,1086.6258649045089,92.384957103468111,10332.06961022512]
["7VX485T","FFG1761",1578.061942906234,44.393853458150232,104.48573430567565,1,1.3106114349364686,135.75173677529233,21.919360663087023,2012.7441882684827,null,2678.5794284039962,81.419448357464788,158.3024295316294,1,2.711834606061716,231.82415844046642,25.463389284429745,3350.0047777910868,null,4018.0522936593361,98.571104456565806,448.9744725375653,3.6,4.4722778277973791,454.00065436135912,37.784434787153636,5662.8570959172011,null,6237.1151914704978,167.13374656036987,664.2587009635082,3.6,8.6505015387111168,649.59601309784784,49.688301072479305,8649.8332826493734,null,4217.8950909953519,117.85640622214011,422.21495889454127,6.6,5.8858429270143917,471.80495742464268,38.643032521120752,5865.6631600080364,null,3581.4893241167324,117.47856930356626,318.47234241369978,6.6,4.7810897069805964,345.36060388159626,34.750522139402946,4876.6332375722241,null,7356.4077384813263,267.64021897558399,607.6650982664753,6.6,12.764291965030974,633.8650878609634,53.891224977023072,9801.5116192580936]
["7VX485T","FFG1927",1578.061942906234,44.393853458150232,104.48573430567565,1,2.6212228698729372,271.50347355058466,43.838721326174046,2177.1582584223652,null,2678.5794284039962,81.419448357464788,158.3024295316294,1,5.423669212123432,463.64831688093284,50.92677856885949,3617.2663056637798,null,4018.0522936593361,98.571104456565806,448.9744725375653,3.6,8.9445556555947583,908.00130872271825,75.568869574307271,6185.2263386790246,null,6237.1151914704978,167.13374656036987,664.2587009635082,3.6,17.301003077422234,1299.1920261956957,99.376602144958611,9396.0372143059212,null,4217.8950909953519,117.85640622214011,422.21495889454127,6.6,11.771685854028783,943.60991484928536,77.286065042241503,6410.0420055713739,null,3581.4893241167324,117.47856930356626,318.47234241369978,6.6,9.5621794139611929,690.72120776319252,69.501044278805892,5283.9428177596483,null,7356.4077384813263,267.64021897558399,607.6650982664753,6.6,25.528583930061949,1267.7301757219268,107.78244995404614,10544.292806611931]
["7VX485T","FFG1930",1578.061942906234,44.393853458150232,104.48573430567565,1,1.1233812299455446,116.35863152167916,18.788023425503162,1989.2564639607854,null,2678.5794284039962,81.419448357464788,158.3024295316294,1,2.3244296623386136,198.7064215203998,21.825762243796923,3311.8245595235589,null,4018.0522936593361,98.571104456565806,448.9744725375653,3.6,3.8333809952548963,389.14341802402214,32.386658388988835,5588.2329183797974,null,6237.1151914704978,167.13374656036987,664.2587009635082,3.6,7.4147156046095297,556.79658265529815,42.589972347839407,8543.2327209841515,null,4217.8950909953519,117.85640622214011,422.21495889454127,6.6,5.0450082231551931,404.40424922112226,33.122599303817786,5787.8947534989893,null,3581.4893241167324,117.47856930356626,318.47234241369978,6.6,4.0980768916976542,296.023374755654,29.786161833773949,4818.4461546883067,null,7356.4077384813263,267.64021897558399,607.6650982664753,6.6,10.940821684312263,543.31293245225447,46.192478551734055,9695.4000210646864]
["7VX550T","FFG1158",2213.7578851375638,63.37158161262073,146.99847191664387,1,2.2467624598910891,150.14016970539245,37.500731386445857,2778.7119359970748,null,3756.3161361503171,116.20286599122203,222.68434156668877,1,4.6488593246772272,236.55526371476168,43.564031653166865,4608.3508654445604,null,5891.0867828613427,140.6103824635463,615.05720009993536,5.0999999999999996,7.6667619905097926,484.52411796161283,61.516640338120489,8018.6540072723055,null,9140.6623709969554,238.47051362353136,910.08786276006276,5.0999999999999996,14.829431209219059,693.26978332303383,80.897262677254375,12276.217889428421,null,6169.0719702275928,169.17431378494342,593.40328348267496,9.4,10.090016446310386,464.56216515322984,62.914518810912618,8287.2422969860909,null,5206.0472651120699,167.63996629473428,447.8397013557115,9.4,8.1961537833953084,380.86595627665849,56.577143049877101,6921.1255893268917,null,10687.032302149266,382.00752868206706,854.45696610481866,9.4,21.881643368624527,699.03060779139071,87.740021068659829,13947.20348386592]
["7VX550T","FFG1927",2213.7578851375638,63.37158161262073,146.99847191664387,1,3.7446040998184813,250.23361617565405,62.501218977409764,2911.5020825283627,null,3756.3161361503171,116.20286599122203,222.68434156668877,1,7.7480988744620465,394.25877285793609,72.60671942194476,4806.4842310998811,null,5891.0867828613427,140.6103824635463,615.05720009993536,5.0999999999999996,12.777936650849655,807.54019660268818,102.52773389686747,8411.2598864715001,null,9140.6623709969554,238.47051362353136,910.08786276006276,5.0999999999999996,24.715718682031763,1155.4496388717232,134.8287711287573,12836.888527863624,null,6169.0719702275928,169.17431378494342,593.40328348267496,9.4,16.816694077183975,774.27027525538313,104.85753135152103,8670.2759094333742,null,5206.0472651120699,167.63996629473428,447.8397013557115,9.4,13.660256305658846,634.77659379443094,94.295238416461842,7239.155392937284,null,10687.032302149266,382.00752868206706,854.45696610481866,9.4,36.46940561437421,1165.0510129856514,146.2333684477664,14526.138678646947]
["7VX690T","FFG1157",2213.7578851375638,63.37158161262073,146.99847191664387,1,0.93615102495462033,62.558404043913512,15.625304744352441,2662.5205577821985,null,3756.3161361503171,116.20286599122203,222.68434156668877,1,1.9370247186155116,98.564693214484024,18.15167985548619,4434.9841704961545,null,5891.0867828613427,140.6103824635463,615.05720009993536,5.0999999999999996,3.1944841627124139,201.88504915067205,25.631933474216869,7675.1238629730096,null,9140.6623709969554,238.47051362353136,910.08786276006276,5.0999999999999996,6.1789296705079408,288.8624097179308,33.707192782189324,11785.631080797619,null,6169.0719702275928,169.17431378494342,593.40328348267496,9.4,4.2041735192959937,193.56756881384578,26.214382837880258,7952.0878860947196,null,5206.0472651120699,167.63996629473428,447.8397013557115,9.4,3.4150640764147115,158.69414844860773,23.573809604115461,6642.8495111677976,null,10687.032302149266,382.00752868206706,854.45696610481866,9.4,9.1173514035935526,291.26275324641284,36.558342111941599,13440.635188432523]
["7VX690T","FFG1158",2213.7578851375638,63.37158161262073,146.99847191664387,1,2.2467624598910891,150.14016970539245,37.500731386445857,2778.7119359970748,null,3756.3161361503171,116.20286599122203,222.68434156668877,1,4.6488593246772272,236.55526371476168,43.564031653166865,4608.3508654445604,null,5891.0867828613427,140.6103824635463,615.05720009993536,5.0999999999999996,7.6667619905097926,484.52411796161283,61.516640338120489,8018.6540072723055,null,9140.6623709969554,238.47051362353136,910.08786276006276,5.0999999999999996,14.829431209219059,693.26978332303383,80.897262677254375,12276.217889428421,null,6169.0719702275928,169.17431378494342,593.40328348267496,9.4,10.090016446310386,464.56216515322984,62.914518810912618,8287.2422969860909,null,5206.0472651120699,167.63996629473428,447.8397013557115,9.4,8.1961537833953084,380.86595627665849,56.577143049877101,6921.1255893268917,null,10687.032302149266,382.00752868206706,854.45696610481866,9.4,21.881643368624527,699.03060779139071,87.740021068659829,13947.20348386592]
["7VX690T","FFG1761",2213.7578851375638,63.37158161262073,146.99847191664387,1,1.6850718449183166,112.60512727904432,28.125548539834391,2728.915631047842,null,3756.3161361503171,116.20286599122203,222.68434156668877,1,3.4866444935079208,177.41644778607125,32.673023739875141,4534.0508533238144,null,5891.0867828613427,140.6103824635463,615.05720009993536,5.0999999999999996,5.7500714928823449,363.39308847120964,46.137480253590361,7871.4268025726069,null,9140.6623709969554,238.47051362353136,910.08786276006276,5.0999999999999996,11.122073406914295,519.95233749227543,60.672947007940785,12065.966400015222,null,6169.0719702275928,169.17431378494342,593.40328348267496,9.4,7.5675123347327888,348.42162386492242,47.185889108184462,8143.6046923183603,null,5206.0472651120699,167.63996629473428,447.8397013557115,9.4,6.1471153375464809,285.6494672074939,42.432857287407828,6801.8644129729946,null,10687.032302149266,382.00752868206706,854.45696610481866,9.4,16.411232526468396,524.27295584354306,65.805015801494875,13730.102785823035]
["7VX690T","FFG1926",2213.7578851375638,63.37158161262073,146.99847191664387,1,2.9956832798547852,200.18689294052325,50.000975181927807,2845.1070092627187,null,3756.3161361503171,116.20286599122203,222.68434156668877,1,6.1984790995696368,315.40701828634889,58.085375537555812,4707.4175482722203,null,5891.0867828613427,140.6103824635463,615.05720009993536,5.0999999999999996,10.222349320679724,646.03215728215048,82.022187117493985,8214.9569468719019,null,9140.6623709969554,238.47051362353136,910.08786276006276,5.0999999999999996,19.772574945625411,924.35971109737852,107.86301690300583,12556.553208646024,null,6169.0719702275928,169.17431378494342,593.40328348267496,9.4,13.453355261747181,619.41622020430646,83.886025081216829,8478.7591032097316,null,5206.0472651120699,167.63996629473428,447.8397013557115,9.4,10.928205044527077,507.82127503554477,75.436190733169468,7080.1404911320869,null,10687.032302149266,382.00752868206706,854.45696610481866,9.4,29.17552449149937,932.04081038852098,116.9866947582131,14236.671081256434]
["7VX690T","FFG1927",2213.7578851375638,63.37158161262073,146.99847191664387,1,3.7446040998184813,250.23361617565405,62.501218977409764,2911.5020825283627,null,3756.3161361503171,116.20286599122203,222.68434156668877,1,7.7480988744620465,394.25877285793609,72.60671942194476,4806.4842310998811,null,5891.0867828613427,140.6103824635463,615.05720009993536,5.0999999999999996,12.777936650849655,807.54019660268818,102.52773389686747,8411.2598864715001,null,9140.6623709969554,238.47051362353136,910.08786276006276,5.0999999999999996,24.715718682031763,1155.4496388717232,134.8287711287573,12836.888527863624,null,6169.0719702275928,169.17431378494342,593.40328348267496,9.4,16.816694077183975,774.27027525538313,104.85753135152103,8670.2759094333742,null,5206.0472651120699,167.63996629473428,447.8397013557115,9.4,13.660256305658846,634.77659379443094,94.295238416461842,7239.155392937284,null,10687.032302149266,382.00752868206706,854.45696610481866,9.4,36.46940561437421,1165.0510129856514,146.2333684477664,14526.138678646947]
["7VX690T","FFG1930",2213.7578851375638,63.37158161262073,146.99847191664387,1,1.1233812299455446,75.070084852696226,18.750365693222928,2679.1193260986097,null,3756.3161361503171,116.20286599122203,222.68434156668877,1,2.3244296623386136,118.27763185738084,21.782015826583432,4459.7508412030693,null,5891.0867828613427,140.6103824635463,615.05720009993536,5.0999999999999996,3.8333809952548963,242.26205898080642,30.758320169060244,7724.1995978729092,null,9140.6623709969554,238.47051362353136,910.08786276006276,5.0999999999999996,7.4147156046095297,346.63489166151692,40.448631338627187,11855.714910602021,null,6169.0719702275928,169.17431378494342,593.40328348267496,9.4,5.0450082231551931,232.28108257661492,31.457259405456309,7999.9670876506307,null,5206.0472651120699,167.63996629473428,447.8397013557115,9.4,4.0980768916976542,190.43297813832925,28.288571524938551,6682.6032366190966,null,10687.032302149266,382.00752868206706,854.45696610481866,9.4,10.940821684312263,349.51530389569535,43.870010534329914,13513.002087780151]
["7VX980T","FFG1926",2579.6485624646634,64.666935876122523,183.32121683611885,1,2.9956832798547852,200.18689294052325,50.000975181927807,3277.6739817083753,null,4394.5773516136105,118.60533967586117,281.95653221634171,1,6.1984790995696368,315.40701828634889,58.085375537555812,5454.7711805895269,null,7598.0463989380878,143.49191543543773,790.85983807363425,4.5999999999999996,10.222349320679724,646.03215728215048,82.022187117493985,10307.415316162291,null,11839.274939541789,243.37852401211694,1175.4201572998982,4.5999999999999996,19.772574945625411,924.35971109737852,107.86301690300583,15841.712441627733,null,7999.8381967806581,172.62761434706914,761.58712743549438,8.4,13.453355261747181,619.41622020430646,83.886025081216829,10683.982681209209,null,6753.9396018174848,171.09298704762747,572.36090276886944,8.4,10.928205044527077,507.82127503554477,75.436190733169468,8911.4812799850151,null,13937.931761357444,389.77114201531242,1102.0785549259431,8.4,29.17552449149937,932.04081038852098,116.9866947582131,18059.208848846021]
["7VX980T","FFG1928",2579.6485624646634,64.666935876122523,183.32121683611885,1,3.3701436898366333,225.21025455808865,56.251097079668781,3310.8715183411973,null,4394.5773516136105,118.60533967586117,281.95653221634171,1,6.9732889870158417,354.83289557214249,65.346047479750283,5504.3045220033573,null,7598.0463989380878,143.49191543543773,790.85983807363425,4.5999999999999996,11.50014298576469,726.78617694241927,92.274960507180722,10405.566785962088,null,11839.274939541789,243.37852401211694,1175.4201572998982,4.5999999999999996,22.244146813828589,1039.9046749845509,121.34589401588157,15981.880101236535,null,7999.8381967806581,172.62761434706914,761.58712743549438,8.4,15.135024669465578,696.84324772984485,94.371778216368924,10779.741084321029,null,6753.9396018174848,171.09298704762747,572.36090276886944,8.4,12.294230675092962,571.2989344149878,84.865714574815655,8990.9887308876132,null,13937.931761357444,389.77114201531242,1102.0785549259431,8.4,32.822465052936792,1048.5459116870861,131.61003160298975,18203.94264754128]
["7VX980T","FFG1930",2579.6485624646634,64.666935876122523,183.32121683611885,1,1.1233812299455446,75.070084852696226,18.750365693222928,3111.6862985442658,null,4394.5773516136105,118.60533967586117,281.95653221634171,1,2.3244296623386136,118.27763185738084,21.782015826583432,5207.1044735203768,null,7598.0463989380878,143.49191543543773,790.85983807363425,4.5999999999999996,3.8333809952548963,242.26205898080642,30.758320169060244,9816.6579671632971,null,11839.274939541789,243.37852401211694,1175.4201572998982,4.5999999999999996,7.4147156046095297,346.63489166151692,40.448631338627187,15140.874143583731,null,7999.8381967806581,172.62761434706914,761.58712743549438,8.4,5.0450082231551931,232.28108257661492,31.457259405456309,10205.190665650105,null,6753.9396018174848,171.09298704762747,572.36090276886944,8.4,4.0980768916976542,190.43297813832925,28.288571524938551,8513.944025472023,null,13937.931761357444,389.77114201531242,1102.0785549259431,8.4,10.940821684312263,349.51530389569535,43.870010534329914,17335.539855369738]
["7VX1140T","FLG1926",3447.8930208947281,81.03572553700738,250.35818051513769,1,2.9956832798547852,200.18689294052325,50.000975181927807,4390.9537644215588,null,5869.8710489424566,148.60437460286056,385.51205321386624,1,6.1984790995696368,315.40701828634889,58.085375537555812,7254.4638506409174,null,6308.7328249096236,125.89613033011082,757.78799077468057,6.4,10.222349320679724,646.03215728215048,82.022187117493985,9037.194884859462,null,9823.6924526706371,213.49737413479983,1126.733894676024,6.4,19.772574945625411,924.35971109737852,107.86301690300583,13781.269859417687,null,9823.6924526706371,213.49737413479983,1183.0705894098253,11.7,19.772574945625411,924.35971109737852,107.86301690300583,13897.763212464572,null,8523.1297136397443,213.49737413479983,957.72381047462045,11.7,19.772574945625411,924.35971109737852,107.86301690300583,12132.278179075214,null,16557.297583741572,463.43674352824388,1772.1075570912083,11.7,49.967053874016969,1583.8158562883407,178.5219690348807,23026.104043547122]
["7VX1140T","FLG1928",3447.8930208947281,81.03572553700738,250.35818051513769,1,4.4935249197821783,300.2803394107849,75.001462772891713,4523.7439109528459,null,5869.8710489424566,148.60437460286056,385.51205321386624,1,9.2977186493544544,473.11052742952336,87.128063306333729,7452.597216296238,null,6308.7328249096236,125.89613033011082,757.78799077468057,6.4,15.333523981019585,969.04823592322566,123.03328067624098,9429.8007640586566,null,9823.6924526706371,213.49737413479983,1126.733894676024,6.4,29.658862418438119,1386.5395666460677,161.79452535450875,14341.940497852891,null,9823.6924526706371,213.49737413479983,1183.0705894098253,11.7,29.658862418438119,1386.5395666460677,161.79452535450875,14458.433850899775,null,8523.1297136397443,213.49737413479983,957.72381047462045,11.7,29.658862418438119,1386.5395666460677,161.79452535450875,12692.948817510418,null,16557.297583741572,463.43674352824388,1772.1075570912083,11.7,74.950580811025446,2375.7237844325109,267.78295355232103,23997.779745325533]
["7VX1140T","FLG1930",3447.8930208947281,81.03572553700738,250.35818051513769,1,1.1233812299455446,75.070084852696226,18.750365693222928,4224.9660812574493,null,5869.8710489424566,148.60437460286056,385.51205321386624,1,2.3244296623386136,118.27763185738084,21.782015826583432,7006.7971435717664,null,6308.7328249096236,125.89613033011082,757.78799077468057,6.4,3.8333809952548963,242.26205898080642,30.758320169060244,8546.4375358604684,null,9823.6924526706371,213.49737413479983,1126.733894676024,6.4,7.4147156046095297,346.63489166151692,40.448631338627187,13080.431561373685,null,9823.6924526706371,213.49737413479983,1183.0705894098253,11.7,7.4147156046095297,346.63489166151692,40.448631338627187,13196.92491442057,null,8523.1297136397443,213.49737413479983,957.72381047462045,11.7,7.4147156046095297,346.63489166151692,40.448631338627187,11431.439881031214,null,16557.297583741572,463.43674352824388,1772.1075570912083,11.7,18.737645202756362,593.93094610812773,66.945738388080258,21811.509416324108]
[]
[null,null,"Commercial (nominal voltages, TT, 85C)",null,null,null,null,null,null,null,null,null,null,null,"Extended (nominal voltages, TT, 100C)",null,null,null,null,null,null,null,null,null,null,null,"Commercial (max voltages, (TT+FF/2), 85C)",null,null,null,null,null,null,null,null,null,null,null,"Commercial (max voltages, (TT+FF/2), 100C)",null,null,null,null,null,null,null,null,null,null,null,"Extended (max voltages, FF2, 100C)",null,null,null,null,null,null,null,null,null,null,null,"Extended -2L (max voltages, FF1.5, 100C)",null,null,null,null,null,null,null,null,null,null,null,"Q-Grade (max voltages, FF1.5, 125C)"]
["PART","Pkg","Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Iccmax_mgtzvcch","Iccmax_mgtzavcc","Iccmax_mgtzvccl","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Iccmax_mgtzvcch","Iccmax_mgtzavcc","Iccmax_mgtzvccl","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Iccmax_mgtzvcch","Iccmax_mgtzavcc","Iccmax_mgtzvccl","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Iccmax_mgtzvcch","Iccmax_mgtzavcc","Iccmax_mgtzvccl","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Iccmax_mgtzvcch","Iccmax_mgtzavcc","Iccmax_mgtzvccl","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Iccmax_mgtzvcch","Iccmax_mgtzavcc","Iccmax_mgtzvccl","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Iccmax_mgtzvcch","Iccmax_mgtzavcc","Iccmax_mgtzvccl","Static mW"]
["7VH580T","HCG1155",1724.9520962994322,40.503238788397709,125.58071455940187,1,1.1233812299455446,75.070084852696226,18.750365693222928,3.5358000000000005,152,171.58919500000002,2502.9365960682189,null,2936.3287779085995,74.316393453533266,193.20444871372388,1,2.3244296623386136,118.27763185738084,21.782015826583432,4.1583000000000006,152,235.48720000000003,3985.4725232883261,null,4479.8143334697215,89.90425683763884,541.89442849446505,3.2,3.8333809952548963,242.26205898080642,30.758320169060244,3.5358000000000005,296,171.58919500000002,6619.4625660205165,null,6975.6517083345498,152.52036860778543,805.45226946251955,3.2,7.4147156046095297,346.63489166151692,40.448631338627187,4.1583000000000006,296,235.48720000000003,9947.1680013611694,null,4719.3461436140515,108.18266768123672,521.91831881842165,5.9,5.0450082231551931,232.28108257661492,31.457259405456309,4.1583000000000006,296,235.48720000000003,6913.5015015364252,null,3924.7873599735663,107.18046982942977,392.17371480618567,5.9,4.0980768916976542,190.43297813832925,28.288571524938551,4.1583000000000006,296,235.48720000000003,5800.1035323885708,null,8091.7129993464696,244.25049300638392,755.21338171881894,5.9,10.940821684312263,349.51530389569535,43.870010534329914,5.1958000000000002,296,386.94187499999998,11276.124737407778]
["7VH580T","HCG1931",1724.9520962994322,40.503238788397709,125.58071455940187,1,2.2467624598910891,150.14016970539245,37.500731386445857,3.5358000000000005,152,171.58919500000002,2602.5292059666849,null,2936.3287779085995,74.316393453533266,193.20444871372388,1,4.6488593246772272,236.55526371476168,43.564031653166865,4.1583000000000006,152,235.48720000000003,4134.0725475298168,null,4479.8143334697215,89.90425683763884,541.89442849446505,3.2,7.6667619905097926,484.52411796161283,61.516640338120489,3.5358000000000005,296,171.58919500000002,6913.916975419912,null,6975.6517083345498,152.52036860778543,805.45226946251955,3.2,14.829431209219059,693.26978332303383,80.897262677254375,4.1583000000000006,296,235.48720000000003,10367.670980187571,null,4719.3461436140515,108.18266768123672,521.91831881842165,5.9,10.090016446310386,464.56216515322984,62.914518810912618,4.1583000000000006,296,235.48720000000003,7200.7767108718863,null,3924.7873599735663,107.18046982942977,392.17371480618567,5.9,8.1961537833953084,380.86595627665849,56.577143049877101,4.1583000000000006,296,235.48720000000003,6038.625885096365,null,8091.7129993464696,244.25049300638392,755.21338171881894,5.9,21.881643368624527,699.03060779139071,87.740021068659829,5.1958000000000002,296,386.94187499999998,11710.326133493545]
["7VH580T","HCG1932",1724.9520962994322,40.503238788397709,125.58071455940187,1,2.2467624598910891,150.14016970539245,37.500731386445857,3.5358000000000005,152,171.58919500000002,2602.5292059666849,null,2936.3287779085995,74.316393453533266,193.20444871372388,1,4.6488593246772272,236.55526371476168,43.564031653166865,4.1583000000000006,152,235.48720000000003,4134.0725475298168,null,4479.8143334697215,89.90425683763884,541.89442849446505,3.2,7.6667619905097926,484.52411796161283,61.516640338120489,3.5358000000000005,296,171.58919500000002,6913.916975419912,null,6975.6517083345498,152.52036860778543,805.45226946251955,3.2,14.829431209219059,693.26978332303383,80.897262677254375,4.1583000000000006,296,235.48720000000003,10367.670980187571,null,4719.3461436140515,108.18266768123672,521.91831881842165,5.9,10.090016446310386,464.56216515322984,62.914518810912618,4.1583000000000006,296,235.48720000000003,7200.7767108718863,null,3924.7873599735663,107.18046982942977,392.17371480618567,5.9,8.1961537833953084,380.86595627665849,56.577143049877101,4.1583000000000006,296,235.48720000000003,6038.625885096365,null,8091.7129993464696,244.25049300638392,755.21338171881894,5.9,21.881643368624527,699.03060779139071,87.740021068659829,5.1958000000000002,296,386.94187499999998,11710.326133493545]
["7VH870T","HCG1931",2586.4197390119607,60.791414279663037,187.99847325792473,1,2.2467624598910891,150.14016970539245,37.500731386445857,3.5358000000000005,152,171.58919500000002,3632.6369898278194,null,4403.1026524510744,111.48762292930215,289.37862597801603,1,4.6488593246772272,236.55526371476168,43.564031653166865,4.1583000000000006,152,235.48720000000003,5847.1311706237875,null,4820.1397161369141,94.395246134867307,568.60927006051497,4.8,7.6667619905097926,484.52411796161283,61.516640338120489,3.5358000000000005,296,171.58919500000002,7367.5928891031008,null,7505.641219261357,160.11840925445753,845.3211090840714,4.8,14.829431209219059,693.26978332303383,80.897262677254375,4.1583000000000006,296,235.48720000000003,11044.762265192987,null,7486.7331571035938,160.11840925445753,887.58716453827503,8.8000000000000007,14.829431209219059,693.26978332303383,80.897262677254375,4.1583000000000006,296,235.48720000000003,11112.729805978935,null,6505.4477039842013,160.11840925445753,718.52294272146071,8.8000000000000007,14.829431209219059,693.26978332303383,80.897262677254375,4.1583000000000006,296,235.48720000000003,9782.4744100321786,null,12637.679295480038,347.59754247550677,1329.3095500259033,8.8000000000000007,37.475290405512723,1187.8618922162555,133.89147677616052,5.1958000000000002,296,386.94187499999998,18223.752398060788]
["7VH870T","HCG1932",2586.4197390119607,60.791414279663037,187.99847325792473,1,3.3701436898366333,225.21025455808865,56.251097079668781,7.071600000000001,304,343.17839000000004,4070.2729646012854,null,4403.1026524510744,111.48762292930215,289.37862597801603,1,6.9732889870158417,354.83289557214249,65.346047479750283,8.3166000000000011,304,470.97440000000006,6400.3905148652766,null,4820.1397161369141,94.395246134867307,568.60927006051497,4.8,11.50014298576469,726.78617694241927,92.274960507180722,7.071600000000001,592,343.17839000000004,8160.0168372524977,null,7505.641219261357,160.11840925445753,845.3211090840714,4.8,22.244146813828589,1039.9046749845509,121.34589401588157,8.3166000000000011,592,470.97440000000006,12031.560238019389,null,7486.7331571035938,160.11840925445753,887.58716453827503,8.8000000000000007,22.244146813828589,1039.9046749845509,121.34589401588157,8.3166000000000011,592,470.97440000000006,12099.527778805337,null,6505.4477039842013,160.11840925445753,718.52294272146071,8.8000000000000007,22.244146813828589,1039.9046749845509,121.34589401588157,8.3166000000000011,592,470.97440000000006,10769.27238285858,null,12637.679295480038,347.59754247550677,1329.3095500259033,8.8000000000000007,56.212935608269092,1781.7928383243832,200.8372151642408,10.3916,592,773.88374999999996,19679.885827144597]
[]
[null,null,"Commercial (nominal voltages, TT, 85C)",null,null,null,null,null,null,null,null,null,null,null,"Industrial (nominal voltages, TT, 100C)",null,null,null,null,null,null,null,null,null,null,null,"Commercial (max voltages, (TT+FF/2), 100C)",null,null,null,null,null,null,null,null,null,null,null,"Commercial (max voltages, (TT+FF/2), 100C)",null,null,null,null,null,null,null,null,null,null,null,"Industrial (max voltages, FF2, 100C)",null,null,null,null,null,null,null,null,null,null,null,"Q-Grade (max voltages, FF1.5, 100C)",null,null,null,null,null,null,null,null,null,null,null,"Q-Grade (max voltages, FF1.5, 125C)"]
["PART","Pkg","Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Iccmax_pint","Iccmax_paux","Iccmax_ddr","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Iccmax_pint","Iccmax_paux","Iccmax_pddr","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Iccmax_pint","Iccmax_paux","Iccmax_ddr","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Iccmax_pint","Iccmax_paux","Iccmax_ddr","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Iccmax_pint","Iccmax_paux","Iccmax_ddr","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Iccmax_pint","Iccmax_paux","Iccmax_ddr","Static mW",null,"Iccmax_core","Iccmax_bram","Iccmax_aux","Iccmax_io","Iccmax_mgtaux","Iccmax_mgtavcc","Iccmax_mgtavtt","Iccmax_pint","Iccmax_paux","Iccmax_ddr","Static mW"]
["7Z010","CLG225",34.607214196035819,2.5819848847638136,18.117451807433888,1,0,0,0,122.08656873518918,10.33,3,256.68118106936981,null,58.779170026110677,4.7185646288717544,23.820761101349941,1,0,0,0,202.841414691214,10.33,3,374.01051932862629,null,144.1957473043359,7.0840844662404061,27.84843118260779,1,0,0,0,506.52090280091556,20.66,6,851.59295623519517,null,225.95224306189345,11.996330364760443,38.900809708323855,1,0,0,0,792.07769096601419,20.66,6,1263.3187579610337,null,153.81200760244721,8.5266905823723143,26.009310221283389,1,0,0,0,449.96114331476707,20.66,6,800.34107989279164,null,127.12733086249573,7.1593550171555957,21.638489032891343,1,0,0,0,320.54361592996042,20.66,6,626.73721117225705,null,264.33370229430312,16.362656652585066,36.997424820993459,1,0,0,0,689.24641896525088,20.66,6,1196.6336997194237]
["7Z010","CLG400",34.607214196035819,2.5819848847638136,18.117451807433888,1,0,0,0,122.08656873518918,10.33,3,256.68118106936981,null,58.779170026110677,4.7185646288717544,23.820761101349941,1,0,0,0,202.841414691214,10.33,3,374.01051932862629,null,144.1957473043359,7.0840844662404061,27.84843118260779,1,0,0,0,506.52090280091556,20.66,6,851.59295623519517,null,225.95224306189345,11.996330364760443,38.900809708323855,1,0,0,0,792.07769096601419,20.66,6,1263.3187579610337,null,153.81200760244721,8.5266905823723143,26.009310221283389,1,0,0,0,449.96114331476707,20.66,6,800.34107989279164,null,127.12733086249573,7.1593550171555957,21.638489032891343,1,0,0,0,320.54361592996042,20.66,6,626.73721117225705,null,264.33370229430312,16.362656652585066,36.997424820993459,1,0,0,0,689.24641896525088,20.66,6,1196.6336997194237]
["7Z020","CLG400",78.163486475838496,6.0356166931691915,38.401740768961112,1,0,0,0,122.08656873518918,10.33,3,340.20280528832694,null,134.36872508113868,11.065036668598681,54.294880395866358,1,0,0,0,202.841414691214,10.33,3,510.79996115351076,null,325.26032467362376,16.495094237868503,68.978535412826034,1,0,0,0,506.52090280091556,20.66,6,1129.3282197282695,null,514.89215515581941,27.987254219236021,99.520851313254724,1,0,0,0,792.07769096601419,20.66,6,1698.0680143401746,null,350.91545908166523,19.856572959560097,63.891609402202121,1.9,0,0,0,449.96114331476707,20.66,6,1092.494625893954,null,290.15284607028406,16.710717171213389,51.779430802259832,1.9,0,0,0,320.54361592996042,20.66,6,866.61031234630195,null,611.11705964584576,38.140836009740305,93.994381392295821,1.9,0,0,0,689.24641896525088,20.66,6,1693.048561183318]
["7Z020","CLG484",78.163486475838496,6.0356166931691915,38.401740768961112,1,0,0,0,122.08656873518918,10.33,3,340.20280528832694,null,134.36872508113868,11.065036668598681,54.294880395866358,1,0,0,0,202.841414691214,10.33,3,510.79996115351076,null,325.26032467362376,16.495094237868503,68.978535412826034,1,0,0,0,506.52090280091556,20.66,6,1129.3282197282695,null,514.89215515581941,27.987254219236021,99.520851313254724,1,0,0,0,792.07769096601419,20.66,6,1698.0680143401746,null,350.91545908166523,19.856572959560097,63.891609402202121,1.9,0,0,0,449.96114331476707,20.66,6,1092.494625893954,null,290.15284607028406,16.710717171213389,51.779430802259832,1.9,0,0,0,320.54361592996042,20.66,6,866.61031234630195,null,611.11705964584576,38.140836009740305,93.994381392295821,1.9,0,0,0,689.24641896525088,20.66,6,1693.048561183318]
["7Z030","FBG484",246.22615020949993,11.439633278256384,55.812218169608101,1,0.18723020499092408,17.516353132295784,3.13133723758386,122.08656873518918,10.33,3,566.61931711462023,null,420.01395863519866,20.960507998936396,79.902988063809275,1,0.3874049437231023,27.598114100055522,3.6376270406328204,202.841414691214,10.33,3,885.09585528772243,null,1014.3286287901361,29.753764160920404,114.84357807726826,1.4,0.63889683254248275,58.580729595014084,5.3977763981648055,709.5761941296355,20.66,6,2214.6982567345535,null,1583.8456067807433,50.483010287152631,166.62829558208227,1.4,1.2357859341015882,83.818840399722305,7.0983287246399014,1109.6076594326839,20.66,6,3369.7492005554955,null,1068.7423429522776,35.77264073337507,106.20307777088765,2.5,0.84083470385919878,56.167256836266986,5.5204332173029647,642.13448059969346,20.66,6,2189.9170564136552,null,878.85591815564419,30.13033688559182,85.590661819402172,2.5,0.68301281528294233,46.048080517546168,4.9643603056289924,410.11712811666024,20.66,6,1694.5480878709066,null,1818.2978200203459,68.708885143349434,157.04982819811408,2.5,1.8234702807187106,84.515345048128452,7.6987464252890101,881.85116740083674,20.66,6,3377.3821409059283]
["7Z030","FBG676",246.22615020949993,11.439633278256384,55.812218169608101,1,0.18723020499092408,17.516353132295784,3.13133723758386,122.08656873518918,10.33,3,566.61931711462023,null,420.01395863519866,20.960507998936396,79.902988063809275,1,0.3874049437231023,27.598114100055522,3.6376270406328204,202.841414691214,10.33,3,885.09585528772243,null,1014.3286287901361,29.753764160920404,114.84357807726826,1.4,0.63889683254248275,58.580729595014084,5.3977763981648055,709.5761941296355,20.66,6,2214.6982567345535,null,1583.8456067807433,50.483010287152631,166.62829558208227,1.4,1.2357859341015882,83.818840399722305,7.0983287246399014,1109.6076594326839,20.66,6,3369.7492005554955,null,1068.7423429522776,35.77264073337507,106.20307777088765,2.5,0.84083470385919878,56.167256836266986,5.5204332173029647,642.13448059969346,20.66,6,2189.9170564136552,null,878.85591815564419,30.13033688559182,85.590661819402172,2.5,0.68301281528294233,46.048080517546168,4.9643603056289924,410.11712811666024,20.66,6,1694.5480878709066,null,1818.2978200203459,68.708885143349434,157.04982819811408,2.5,1.8234702807187106,84.515345048128452,7.6987464252890101,881.85116740083674,20.66,6,3377.3821409059283]
["7Z030","FFG676",246.22615020949993,11.439633278256384,55.812218169608101,1,0.18723020499092408,17.516353132295784,3.13133723758386,122.08656873518918,10.33,3,566.61931711462023,null,420.01395863519866,20.960507998936396,79.902988063809275,1,0.3874049437231023,27.598114100055522,3.6376270406328204,202.841414691214,10.33,3,885.09585528772243,null,1014.3286287901361,29.753764160920404,114.84357807726826,1.4,0.63889683254248275,58.580729595014084,5.3977763981648055,709.5761941296355,20.66,6,2214.6982567345535,null,1583.8456067807433,50.483010287152631,166.62829558208227,1.4,1.2357859341015882,83.818840399722305,7.0983287246399014,1109.6076594326839,20.66,6,3369.7492005554955,null,1068.7423429522776,35.77264073337507,106.20307777088765,2.5,0.84083470385919878,56.167256836266986,5.5204332173029647,642.13448059969346,20.66,6,2189.9170564136552,null,878.85591815564419,30.13033688559182,85.590661819402172,2.5,0.68301281528294233,46.048080517546168,4.9643603056289924,410.11712811666024,20.66,6,1694.5480878709066,null,1818.2978200203459,68.708885143349434,157.04982819811408,2.5,1.8234702807187106,84.515345048128452,7.6987464252890101,881.85116740083674,20.66,6,3377.3821409059283]
["7Z045","FBG676",610.79643360315356,23.488921109837175,130.7432729436926,1,0.37446040998184815,35.032706264591567,6.2626744751677199,122.08656873518918,10.33,3,1099.7257591195869,null,1042.169742565821,43.111899875041132,193.24310628327012,1,0.7748098874462046,55.196228200111044,7.2752540812656408,202.841414691214,10.33,3,1766.0758393369954,null,2439.2837076777787,61.199704760394233,287.47647628787968,2.1,1.2777936650849655,117.16145919002817,10.795552796329611,709.5761941296355,20.66,6,4110.5498600171495,null,3808.0366423191845,103.79061157849524,421.83328017748835,2.1,2.4715718682031764,167.63768079944461,14.196657449279803,1109.6076594326839,20.66,6,6296.5837712965986,null,2625.1163480852497,73.554254336342964,264.75674110469254,3.9,1.6816694077183976,112.33451367253397,11.040866434605929,642.13448059969346,20.66,6,4200.4077190133412,null,2158.3849211057923,62.033577029091468,211.254674390243,3.9,1.3660256305658847,92.096161035092337,9.9287206112579849,410.11712811666024,20.66,6,3340.2735418335224,null,4464.5397523492584,141.28007949411358,396.5187621618627,3.9,3.6469405614374213,169.0306900962569,15.39749285057802,881.85116740083674,20.66,6,6732.8956300994869]
["7Z045","FFG676",610.79643360315356,23.488921109837175,130.7432729436926,1,0.37446040998184815,35.032706264591567,6.2626744751677199,122.08656873518918,10.33,3,1099.7257591195869,null,1042.169742565821,43.111899875041132,193.24310628327012,1,0.7748098874462046,55.196228200111044,7.2752540812656408,202.841414691214,10.33,3,1766.0758393369954,null,2439.2837076777787,61.199704760394233,287.47647628787968,2.1,1.2777936650849655,117.16145919002817,10.795552796329611,709.5761941296355,20.66,6,4110.5498600171495,null,3808.0366423191845,103.79061157849524,421.83328017748835,2.1,2.4715718682031764,167.63768079944461,14.196657449279803,1109.6076594326839,20.66,6,6296.5837712965986,null,2625.1163480852497,73.554254336342964,264.75674110469254,3.9,1.6816694077183976,112.33451367253397,11.040866434605929,642.13448059969346,20.66,6,4200.4077190133412,null,2158.3849211057923,62.033577029091468,211.254674390243,3.9,1.3660256305658847,92.096161035092337,9.9287206112579849,410.11712811666024,20.66,6,3340.2735418335224,null,4464.5397523492584,141.28007949411358,396.5187621618627,3.9,3.6469405614374213,169.0306900962569,15.39749285057802,881.85116740083674,20.66,6,6732.8956300994869]
["7Z045","FFG900",610.79643360315356,23.488921109837175,130.7432729436926,1,0.7489208199636963,70.065412529183135,12.52534895033544,122.08656873518918,10.33,3,1142.947703492347,null,1042.169742565821,43.111899875041132,193.24310628327012,1,1.5496197748924092,110.39245640022209,14.550508162531282,202.841414691214,10.33,3,1831.3970302320281,null,2439.2837076777787,61.199704760394233,287.47647628787968,2.1,2.555587330169931,234.32291838005634,21.591105592659222,709.5761941296355,20.66,6,4246.8686112027708,null,3808.0366423191845,103.79061157849524,421.83328017748835,2.1,4.9431437364063529,335.27536159888922,28.393314898559606,1109.6076594326839,20.66,6,6491.284879138816,null,2625.1163480852497,73.554254336342964,264.75674110469254,3.9,3.3633388154367951,224.66902734506795,22.081732869211859,642.13448059969346,20.66,6,4332.8036222148958,null,2158.3849211057923,62.033577029091468,211.254674390243,3.9,1.3660256305658847,92.096161035092337,9.9287206112579849,410.11712811666024,20.66,6,3340.2735418335224,null,4464.5397523492584,141.28007949411358,396.5187621618627,3.9,3.6469405614374213,169.0306900962569,15.39749285057802,881.85116740083674,20.66,6,6732.8956300994869]
["7Z100","FFG900",795.03366737073054,32.560872791518889,164.91253109565682,1,0.7489208199636963,70.065412529183135,12.52534895033544,122.08656873518918,10.33,3,1397.7615536151413,null,1361.963879348765,59.740036150997476,247.80782693564763,1,1.5496197748924092,110.39245640022209,14.550508162531282,202.841414691214,10.33,3,2266.035800465208,null,3174.4408322427321,84.737796993712635,374.98270624820395,2.1,2.555587330169931,234.32291838005634,21.591105592659222,709.5761941296355,20.66,6,5193.7114591300033,null,4976.6633382702712,143.71032601448857,553.25022821603022,2.1,4.9431437364063529,335.27536159888922,28.393314898559606,1109.6076594326839,20.66,6,7984.465713630354,null,3430.8979057939241,101.97079775873502,344.61870208877929,3.9,3.3633388154367951,224.66902734506795,22.081732869211859,642.13448059969346,20.66,6,5342.9667726398175]
["7Z100","FFG1156",795.03366737073054,32.560872791518889,164.91253109565682,1,0.7489208199636963,70.065412529183135,12.52534895033544,122.08656873518918,10.33,3,1397.7615536151413,null,1361.963879348765,59.740036150997476,247.80782693564763,1,1.5496197748924092,110.39245640022209,14.550508162531282,202.841414691214,10.33,3,2266.035800465208,null,3174.4408322427321,84.737796993712635,374.98270624820395,2.1,2.555587330169931,234.32291838005634,21.591105592659222,709.5761941296355,20.66,6,5193.7114591300033,null,4976.6633382702712,143.71032601448857,553.25022821603022,2.1,4.9431437364063529,335.27536159888922,28.393314898559606,1109.6076594326839,20.66,6,7984.465713630354,null,3430.8979057939241,101.97079775873502,344.61870208877929,3.9,3.3633388154367951,224.66902734506795,22.081732869211859,642.13448059969346,20.66,6,5342.9667726398175]

{"sheet":"Template","index":22,"n_rows":107,"n_cols":54,"rows_kept":107,"cut":false,"hidden":true,"merged":[[105,6,105,19],[19,8,19,14],[44,8,44,14]]}
[null,null,null,null,null,null,null,null,8,8,18,"mode","Rate Row Source",null,null,null,null,"Memory Row Source",null,null,null,null,null,null,null,null,null,null,null,"64b",null,null,null,null,null,"8b",null,null,null,null,null,null,"PCIe","Lanes","Type","GEN1","GEN2","GEN3",null,"JESD204","Lane Type","Number of Lane","FF count","LUT count"]
["Memory",{"$f":"ADDRESS(MATCH(MIG_PROTOCOL,MIG_PROTOCOLS,0)+ROW()+1,1)","v":"$A$4"},null,"Limit (HP)","Limit (HR)",null,null,null,16,12,36,"x4","GTP","GTX/H","GTZ",null,null,"BRAM","Mode","Algorithm","LUT",null,null,null,null,null,"Aurora",null,null,"Streaming",null,null,"Framing",null,null,"Streaming",null,null,"Framing",null,null,null,null,1,"LUTs",400,400,832,null,null,null,4,5267,5045]
["DDR3","Standard","Voltage",null,null,null,"LUTs","FFs",24,16,72,"x8",1.62,6.25,null,null,null,"Single Port RAM","READ_FIRST","Minimum Area","Single Port RAM",null,null,null,null,null,"Modes",null,null,"Duplex","Simplex",null,"Duplex","Simplex",null,"Duplex","Simplex",null,"Duplex","Simplex",null,null,null,null,"FFs",575,575,566,null,null,"RX",8,10030,9456]
["DDR3","SSTL","1.5V",{"$f":"IF(GRADE=\"Extended\",2133,1866)","v":1866},1333,null,172.31818181818181,120.39772727272727,32,20,null,"x16",2.7,10.3125,null,null,null,"Simple Dual Port RAM","WRITE_FIRST","Low Power","Simple Dual Port RAM",null,null,null,null,null,"N/A","Lanes","Type","Full‐Duplex","TX‐Only","RX‐Only","Full‐Duplex","TX‐Only","RX‐Only","Full‐Duplex","TX‐Only","RX‐Only","Full‐Duplex","TX‐Only","RX‐Only",null,null,2,"LUTs",525,525,1384,null,null,null,12,14670,12442]
["DDR3L","SSTL","1.35V",{"$f":"IF(LEFT(SPEEDGRADE,2)=\"-1\",1600,1866)","v":1866},1333,null,172.31818181818181,120.39772727272727,40,24,null,"x32",5.4,12.5,null,null,null,"True Dual Port RAM","NO_CHANGE",null,"Single Port ROM",null,null,null,null,null,"Framing - Duplex",1,"LUTs",549,315,377,873,315,597,379,166,236,388,163,244,null,null,null,"FFs",750,750,957,null,null,null,4,3060,2836]
["DDR4","SSTL","1.2V",{"$f":"IF(LEFT(SPEEDGRADE,2)=\"-1\",1233,2400)","v":2400},0,null,172.31818181818181,120.39772727272727,48,28,null,"x18",3.0720000000000001,3.0720000000000001,null,null,null,"Single Port ROM",null,null,"Dual Port ROM",null,null,null,null,null,"Framing - Simplex_Tx_only",null,"FFs",1359,476,957,1398,499,975,582,275,355,596,273,371,null,null,4,"LUTs",800,800,2500,null,null,"TX",8,5360,4749]
["RLDRAM3","SSTL","1.2V",{"$f":"IF(GRADE=\"Extended\",1066,933)","v":933},0,null,99.215909090909093,59.761363636363633,56,32,null,"x36",4.9000000000000004,4.9000000000000004,null,null,null,"Dual Port ROM",null,null,null,null,null,null,null,null,"Framing - Simplex_Rx_only",2,"LUTs",1044,467,686,1475,471,1106,520,210,324,553,213,356,null,null,null,"FFs",1100,1300,1740,null,null,null,12,7678,6639]
["LPDDR3","HSUL","1.2V",667,667,null,109.02083333333333,80.645833333333329,64,36,null,"1x18",6.1440000000000001,6.1440000000000001,null,null,null,null,null,null,null,null,null,null,null,null,"Streaming - Duplex",null,"FFs",2379,761,1721,2442,799,1748,798,329,526,843,329,572,null,null,8,"LUTs",1350,1450,4818]
["QDRII+ (1.5V)","HSTL Class I","1.5V",714,667,null,48.769230769230766,40.71153846153846,72,40,null,"1x36",null,9.8303999999999991,null,null,null,null,null,null,null,null,null,null,null,null,"Streaming - Simplex_Tx_only",4,"LUTs",1971,711,1452,2628,764,2012,760,316,470,827,297,530,null,null,null,"FFs",2275,2600,3399]
["QDRII+ (1.8V)","HSTL Class I","1.8V",714,667,null,48.769230769230766,40.71153846153846,80,44,null,"2x18",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Streaming - Simplex_Rx_only",null,"FFs",4347,1380,3139,4444,1425,3182,1189,433,805,1271,438,885]
["QDRIV (HSTL)","HSTL Class I","1.2V",714,667,null,48.769230769230766,40.71153846153846,null,48,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,"LUTs",3610,1256,2805,4997,1566,3896,1258,478,757,1374,475,867]
["QDRIV (SSTL)","SSTL","1.2V",714,667,null,48.769230769230766,40.71153846153846,null,52,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FFs",8219,2539,5973,8391,2623,6046,1970,656,1361,2145,662,1507]
["QDRIV (POD)","POD","1.2V",714,667,null,48.769230769230766,40.71153846153846,null,56,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,"LUTs",6656,1949,5496,9418,2874,7560,2229,841,1345,2448,903,1545]
[null,null,null,null,null,null,null,null,null,60]
[null,null,null,null,null,null,null,null,null,64]
[null,null,null,null,null,null,null,null,null,68]
[null,null,null,null,null,null,null,null,null,72]
[null,null,null,null,null,null,null,null,null,76,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FFs",15966,4825,11641,16273,5018,11771,3534,1092,2473,3907,1153,2785]
["GTP",{"$f":"ADDRESS(MATCH(GTP_PROTOCOL,GTP_PROTOCOLS,0)+ROW()+1,1)","v":"$A$24"},null,null,null,null,null,null,null,80]
["DisplayPort","Rate","Channels","OpMode","Fabric","DataMode",null,"TX/OP","Rate list",null,null,null,null,null,null,"Clock","LUTs","FFs","SREG","SRAM","BRAM"]
["Aurora",3.125,4,null,16,"8b/10b",null,800,3.125,6.25]
["CEI 6G-SR",6.6,4,null,16,"8b/10b",null,800,5,6.6]
["CPRI",6.1440000000000001,4,null,32,"8b/10b",null,800,0.6,1.2,2.4,3.0720000000000001,4.9000000000000004,6.1440000000000001]
["DisplayPort",2.7,"1,2,4","Transmitter",16,"8b/10b",null,800,1.62,2.7,5.4]
["Fibre Channel",4.25,4,null,16,"8b/10b",null,800,1.0625,2.125,4.25]
["GigE",1.25,4,null,16,"8b/10b",null,650,1.25,2.5]
["GPON",2.488,4,"Receiver",20,"Raw",null,800,1.244,2.488]
["Interlaken",5,4,null,16,"8b/10b",null,800,4.25,5,6.25]
["PCIe Gen1",2.5,"1,2,4,8",null,16,"8b/10b",null,800,2.5]
["PCIe Gen2",5,"1,2,4,8",null,32,"8b/10b",null,800,5]
["QPI",6.4,4,null,32,"8b/10b",null,800,4.8,6.4]
["RXAUI",6.25,4,null,32,"8b/10b",null,800,6.25]
["SAS",3,4,null,16,"8b/10b",null,800,1.5,3]
["SATA",6,4,null,16,"8b/10b",null,800,1.5,3,6]
["SDI",2.97,4,null,20,"Raw",null,800,1.4850000000000001,2.97]
["SMPTE",2.97,4,null,20,"Raw",null,800,1.4850000000000001,2.97]
["SRIO",6.25,4,null,20,"Raw",null,800,1.25,2.5,3.125,5,6.25]
["OBSAI",6.1440000000000001,4,null,20,"Raw",null,800,3.0720000000000001,6.1440000000000001]
["OC-12",0.622,4,null,20,"Raw",null,800,0.622]
["OTU-1",2.6659999999999999,4,null,32,"8b/10b",null,600,2.6659999999999999]
["TI-5",2.488,4,null,20,"Raw",null,800,2.488]
["XAUI",3.125,4,null,32,"8b/10b",null,900,3.125,6.25]
[]
["GTX",{"$f":"ADDRESS(MATCH(GTX_PROTOCOL,GTX_PROTOCOLS,0)+ROW()+1,1)","v":"$A$65"}]
["PCIe Gen3","Default Rate","Channels","OpMode","Fabric","DataMode","PowerMode","TX/OP","Rate list",null,null,null,null,null,null,"Clock","LUTs","FFs","SREG","SRAM","BRAM","CMAC","ILKN"]
["10GBASE-KR",10.3125,1,null,32,"64b/66b","Low Power",973,10.3125,null,null,null,null,null,null,null,2878,2747]
["10GBASE-R + MAC",10.3125,1,null,64,"64b/66b","DFE",973,10.3125,null,null,null,null,null,null,null,6818,7107]
["100GbE MAC + CAUI-10",10.3125,10,null,32,"Raw","Low Power",973,10.3125,null,null,null,null,null,null,null,null,null,null,null,null,1]
["Aurora",3.125,4,null,16,"8b/10b","Low Power",973,3.125,6.25]
["Aurora 64b66b",12.5,4,null,64,"64b/66b","DFE",973,12.5,6.6]
["CEI-11 SR",11.1,4,null,32,"8b/10b","Low Power",973,11.1]
["CPRI",9.8303999999999991,4,null,32,"8b/10b","Low Power",1119,0.6,1.2,2.4,3.0720000000000001,4.9000000000000004,6.1440000000000001,9.8303999999999991,153.6]
["DisplayPort",2.7,"1,2,4","Transmitter",16,"8b/10b","Low Power",973,1.62,2.7,5.4]
["Fibre Channel",10,1,null,64,"64b/66b","DFE",973,1.0625,2.125,4.25,8.5,10]
["1000Base-X or SGMII",1.25,4,null,16,"8b/10b","DFE",807,1.25,2.5,null,null,null,null,null,null,604,896]
["GPON",2.488,4,"Receiver",20,"Raw","Low Power",973,1.244,2.488]
["Interlaken",10.3125,12,null,64,"Raw","DFE",973,10.3125,12.5,null,null,null,null,null,null,null,null,null,null,null,null,1]
["JESD204B",6.6,"4,8,12",null,16,"8b/10b","Low Power",269,1.25,6.6,12.5,null,null,null,null,null,5045,5267]
["OC-192",9.9559999999999995,4,null,32,"8b/10b","Low Power",973,9.9559999999999995]
["OTU-1",2.6659999999999999,4,null,32,"8b/10b","Low Power",741,2.6659999999999999]
["OTU-2",10.709,4,null,64,"8b/10b","Low Power",973,10.709,11.1,11.3]
["OTU-3",10.7546,4,null,64,"8b/10b","Low Power",973,2.7,10.7546]
["PCIe Gen1",2.5,"1,2,4,8",null,16,"8b/10b","Low Power",973,2.5,null,null,null,null,null,null,null,null,null,null,null,8]
["PCIe Gen2",5,"1,2,4,8",null,16,"8b/10b","Low Power",973,5,null,null,null,null,null,null,null,null,null,null,null,8]
["PCIe Gen3",8,"1,2,4,8",null,32,"64b/66b","DFE",973,8,null,null,null,null,null,null,null,null,null,null,null,8]
["QPI",8,4,null,32,"8b/10b","Low Power",973,4.8,6.4,8,9.8000000000000007]
["RXAUI",6.25,4,null,32,"8b/10b","Low Power",973,6.25]
["SAS",3,4,null,16,"8b/10b","Low Power",973,1.5,3]
["SATA",6,4,null,16,"8b/10b","Low Power",973,1.5,3,6]
["SFI",11.18,4,null,64,"64b/66b","DFE",973,11.18]
["SMPTE",2.97,4,null,20,"Raw","Low Power",973,1.4850000000000001,2.97]
["SRIO",6.25,4,null,20,"Raw","Low Power",973,1.25,2.5,3.125,5,6.25]
["SDI",10.692,4,null,20,"Raw","Low Power",973,1.4850000000000001,2.97,10.680999999999999,10.692]
["XAUI",3.125,4,null,32,"8b/10b","Low Power",1056,3.125,6.25]
["XLAUI",10.3125,4,null,64,"8b/10b","Low Power",973,10.3125]
[]
["GTZ",{"$f":"ADDRESS(MATCH(GTZ_PROTOCOL,GTZ_PROTOCOLS,0)+ROW()+1,1)","v":"$A$79"}]
["100GE-R4","Rate","Channels","OpMode","Fabric","DataMode",null,"TX/OP","Rate list",null,null,null,null,null,null,"Clock","LUTs","FFs","SREG","SRAM","BRAM"]
["100GE-R4",25.78125,4,null,80,"64b/66b",null,1000,25.78125]
["Fibre Channel",28.05,4,null,80,"64b/66b",null,1000,28.05]
["Interlaken",28,4,null,80,"64b/67b",null,1000,28]
["OTU-4",27.952493400000002,4,null,80,"64b/66b",null,1000,27.952493400000002]
[null,{"$f":"ADDRESS(MATCH(GTY_PROTOCOL,GTY_PROTOCOLS,0)+ROW()+1,1)","v":"$A$85"}]
["10GBASE-KR","Rate","Channels","OpMode","Fabric","DataMode",null,"TX/OP","Rate list",null,null,null,null,null,null,"Clock","LUTs","FFs","SREG","SRAM","BRAM","CMAC","ILKN"]
["10GBASE-KR",10.3125,1,null,32,"64b/66b","Low Power",968,10.3125,null,null,null,null,null,null,null,2878,2747]
["10GBASE-R + MAC",10.3125,1,null,32,"64b/66b","Low Power",968,10.3125,null,null,null,null,null,null,null,6818,7107]
["100GbE MAC + CAUI-4",25.78125,4,null,80,"Raw","Low Power",968,25.78125,null,null,null,null,null,null,null,null,null,null,null,null,1]
["100GbE MAC + CAUI-10",10.3125,10,null,32,"Raw","Low Power",968,10.3125,null,null,null,null,null,null,null,null,null,null,null,null,1]
["Interlaken",12.5,12,null,64,"Raw","DFE",968,12.5,null,null,null,null,null,null,null,null,null,null,null,null,null,1]
[]
[]
[]
[]
[]
["12 Step"]
["Typical, Ambient=25C","Still Air"]
["Typical, Ambient=50C","250 LFM"]
["Typical, Ambient=75C","250 LFM (w/Heatsink)"]
["Maximum, Junction=85C"]
["Maximum, Junction=100C"]
["Maximum, Junction=125C"]
[]
[]
[]
[]
["User IP Section",null,null,null,null,null,"Ranges where this exists in the various sheets"]
["Module Name","IP Source","Power (W)","Scale",null,null,"CLOCK","LOGIC","IO","BRAM","DSP","PLL","MMCM","PHASER","PCIE","GTP","GTX","GTH","GTZ","PS"]

{"sheet":"Other","index":23,"n_rows":16,"n_cols":10,"rows_kept":16,"cut":false,"hidden":false,"merged":[[14,1,14,3],[15,1,15,3],[2,9,2,11],[0,1,0,11],[2,1,2,3],[12,9,12,11],[11,1,11,3],[9,1,9,3],[9,9,9,11],[6,1,6,3],[8,1,8,3],[12,1,12,3],[4,9,4,11]]}
[null,"        Other Block Power"]
[]
[null,"Power",null,null,null,null,null,null,null,"XPE User Guide"]
[null,"VCCINT",{"$f":"TEXT(VCCINT,\"0.000\")&\"V\"","v":"0.001V"},{"$f":"G10+G13","v":1.10656E-2}]
[null,"VCCAUX",{"$f":"TEXT(VCCAUX,\"#.000\")&\"V\"","v":"002V"},{"$f":"H13+F16","v":1.4400000000000001E-2},null,null,null,null,null,"Introduction to XPE (video)"]
[null,"VCCADC",{"$f":"TEXT(VCCADC,\"#.000\")&\"V\"","v":"002V"},{"$f":"H10","v":7.4692800000000018E-2},{"$f":"D6-(I10*VCCADC)","v":1.7280000000000073E-4}]
[null,{"$f":"TEXT((Other_INTPOWER+Other_AUXPOWER)/TOTAL_POWER,\"0%\")&\" of total on-chip power \"&TEXT(TOTAL_POWER,\"0.000\")&\"W\"","v":"0% of total on-chip power 0.084W"}]
[]
[null,"SYSMON",null,null,"Powered Down","Clock (MHz)","VCCINT (W)","VCCADC (W)"]
[null,null,null,null,"No",80,{"$f":"XADC_CLOCK*OFFSET(XADC_DATA,1,2)*(VCCINT/1000)*VCCINT_N*PL_POWERED","v":1.5656000000000001E-3},{"$f":"IF(E10=\"Yes\",0,(I10+(XADC_CLOCK*OFFSET(XADC_DATA,1,4)+OFFSET(XADC_DATA,IF(PROCESS=\"Maximum\",2,1),3))/1000)*VCCADC)","v":7.4692800000000018E-2},{"$f":"IF(E10=\"Yes\",0,NUM_DICE*(OFFSET(XADC_DATA,IF(PROCESS=\"Maximum\",2,1),5)/1000))","v":4.1400000000000006E-2},"SYSMON User Guide"]
[]
[null,"Config",null,null,"Readback CRC Clock (MHz)","Config Bank Voltage","VCCINT (W)","VCCAUX (W)"]
[null,null,null,null,80,"1.8V",{"$f":"CRC_CLOCK*(OFFSET(CFG_DATA,1,2)+OFFSET(CFG_DATA,2,2))*(VCCINT/1000)*VCCINT_N*PL_POWERED","v":9.4999999999999998E-3},{"$f":"IF(CRC_CLOCK>0,OFFSET(CFG_DATA,2,3)/1000*VCCAUX*PL_POWERED,0)","v":1.4400000000000001E-2},null,"Config User Guide"]
[]
[null,"eFUSE",null,null,"Programming","VCCAUX (W)"]
[null,null,null,null,"Off",{"$f":"IF(E16=\"On\",OFFSET(CFG_DATA,3,1),0)/1000*VCCAUX*PL_POWERED","v":0}]

{"sheet":"User","index":24,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":false,"merged":[[0,0,0,14]]}
["This sheet is intentionally blank and provided for the user to perform any calculations or add documentation."]

{"sheet":"Release","index":25,"n_rows":37,"n_cols":3,"rows_kept":37,"cut":false,"hidden":false,"merged":[[0,0,0,12],[1,2,1,12],[114,2,114,9],[118,2,118,9],[117,2,117,9],[115,2,115,9],[111,2,111,9],[112,2,112,9],[113,2,113,9]]}
[{"$f":"\"Revision History - \" & Summary!$E1","v":"Revision History -            Xilinx Power Estimator (XPE) - 2015,4"}]
["Date","Version","Release Notes"]
["2015-11-24",2015.4,"Production (Kintex UltraScale, Virtex UltraScale), Advance (-1H, KU085 -1L, KU115 -1L, VU065, VU125, VU440 -3)"]
[null,null,"Bug Fixes"]
["2015-09-30",2015.3,"Production (KU025, KU035, KU040, KU060, KU115 -1/-2, VU080, VU095), Advance (all other Kintex UltraScale, Virtex UltraScale)"]
[null,null,"Bug Fixes"]
["2015-08-05","2015.2.1","Production (KU035, KU040; KU060 -1/-2, KU115 -1/-2), Advance (-1L, Kintex UltraScale, Virtex UltraScale)"]
[null,null,"Bug Fixes"]
["2015-06-30",2015.2,"Production (KU035, KU040, KU060 -1/-2), Advance (Kintex UltraScale, Virtex UltraScale)"]
[null,null,"Bug Fixes"]
["2015-04-15",2015.1,"Production (KU035, KU040 -1/-2), Advance (Kintex UltraScale, Virtex UltraScale)"]
[null,null,"Bug Fixes"]
["2015-02-23","2014.4.1","Production (KU040 -1/-2), Advance (Kintex UltraScale, Virtex UltraScale)"]
[null,null,"Updated static and dynamic power"]
[null,null,"Bug Fixes"]
["2014-11-19",2014.4,"Advance (Kintex UltraScale, Virtex UltraScale)"]
[null,null,"Updated static and dynamic power"]
[null,null,"Enhanced Memory Interface and Transceiver Configuration wizards"]
[null,null,"Bug Fixes"]
["2014-10-08",2014.3,"Advance"]
[null,null,"Public (Kintex UltraScale and Virtex UltraScale)"]
["2014-06-04",2014.2,"Advance"]
[null,null,"Public (Kintex UltraScale and Virtex UltraScale)"]
["2014-04-16",2014.1,"Advance"]
[null,null,"Public (Kintex UltraScale)"]
["2014-01-17",2013.4,"Advance"]
[null,null,"Beta-4"]
["2013-10-23",2013.3,"Advance"]
[null,null,"Beta-3"]
["2013-06-28",2013.2,"Advance"]
[null,null,"Beta-2"]
["2013-03-27",2013.1,"Advance"]
[null,null,"Beta-1"]
["2012-11-20",14.3,"Advance"]
[null,null,"Beta-0"]
[]
["© Copyright 1994-2015 Xilinx, Inc. All Rights Reserved "]